Component: ARM Compiler 5.06 update 5 (build 528) Tool: armlink [4d35e2]

==============================================================================

Section Cross References

    gpioprocess.o(i.Pin_Trigger_handler_1) refers to printf5.o(i.__0printf$5) for __2printf
    gpioprocess.o(i.Pin_Trigger_handler_1) refers to gpioprocess.o(i.nrf_gpio_pin_toggle) for nrf_gpio_pin_toggle
    gpioprocess.o(i.Pin_Trigger_handler_1) refers to host.o(i.Action_Key1) for Action_Key1
    gpioprocess.o(i.Pin_Trigger_handler_1) refers to gpioprocess.o(.data) for KeyDebunseTick
    gpioprocess.o(i.Pin_Trigger_handler_2) refers to gpioprocess.o(i.nrf_gpio_pin_toggle) for nrf_gpio_pin_toggle
    gpioprocess.o(i.gpio_init) refers to nrfx_gpiote.o(i.nrfx_gpiote_init) for nrfx_gpiote_init
    gpioprocess.o(i.gpio_init) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    gpioprocess.o(i.gpio_init) refers to gpioprocess.o(i.nrf_gpio_cfg_output) for nrf_gpio_cfg_output
    gpioprocess.o(i.gpio_init) refers to gpioprocess.o(i.nrf_gpio_pin_clear) for nrf_gpio_pin_clear
    gpioprocess.o(i.gpio_init) refers to nrfx_gpiote.o(i.nrfx_gpiote_in_init) for nrfx_gpiote_in_init
    gpioprocess.o(i.gpio_init) refers to nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable) for nrfx_gpiote_in_event_enable
    gpioprocess.o(i.gpio_init) refers to gpioprocess.o(.constdata) for .constdata
    gpioprocess.o(i.gpio_init) refers to gpioprocess.o(i.Pin_Trigger_handler_1) for Pin_Trigger_handler_1
    gpioprocess.o(i.gpio_init) refers to gpioprocess.o(i.Pin_Trigger_handler_2) for Pin_Trigger_handler_2
    host.o(i.Action_Key1) refers to host.o(i.PacketSend) for PacketSend
    host.o(i.PacketSend) refers to esbprocess.o(i.EebTxRxSwitch) for EebTxRxSwitch
    host.o(i.PacketSend) refers to nrf_esb.o(i.nrf_esb_write_payload) for nrf_esb_write_payload
    host.o(i.PacketSend) refers to esbprocess.o(.data) for tx_payload
    host.o(i.Timer_1S) refers to printf5.o(i.__0printf$5) for __2printf
    host.o(i.Timer_1S) refers to host.o(.data) for PacketReceiveNGCnt
    host.o(i.esb_send_packet_timer_callback) refers to host.o(i.PacketSend) for PacketSend
    host.o(i.main) refers to host.o(i.clocks_start) for clocks_start
    host.o(i.main) refers to gpioprocess.o(i.gpio_init) for gpio_init
    host.o(i.main) refers to uartprocess.o(i.UART_Init) for UART_Init
    host.o(i.main) refers to printf5.o(i.__0printf$5) for __2printf
    host.o(i.main) refers to host.o(i.timers_init) for timers_init
    host.o(i.main) refers to esbprocess.o(i.esb_init) for esb_init
    host.o(i.main) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    host.o(i.main) refers to nrf_esb.o(i.nrf_esb_start_rx) for nrf_esb_start_rx
    host.o(i.main) refers to host.o(i.timers_start) for timers_start
    host.o(i.nrf_delay_ms) refers to host.o(.constdata) for delay_bytecode
    host.o(i.nrf_esb_event_handler) refers to esbprocess.o(i.EebTxRxSwitch) for EebTxRxSwitch
    host.o(i.nrf_esb_event_handler) refers to nrf_esb.o(i.nrf_esb_flush_tx) for nrf_esb_flush_tx
    host.o(i.nrf_esb_event_handler) refers to nrf_esb.o(i.nrf_esb_start_tx) for nrf_esb_start_tx
    host.o(i.nrf_esb_event_handler) refers to host.o(i.nrf_delay_ms) for nrf_delay_ms
    host.o(i.nrf_esb_event_handler) refers to host.o(i.PacketSend) for PacketSend
    host.o(i.nrf_esb_event_handler) refers to printf5.o(i.__0printf$5) for __2printf
    host.o(i.nrf_esb_event_handler) refers to memcpya.o(.text) for __aeabi_memcpy
    host.o(i.nrf_esb_event_handler) refers to nrf_esb.o(i.nrf_esb_read_rx_payload) for nrf_esb_read_rx_payload
    host.o(i.nrf_esb_event_handler) refers to host.o(.data) for PacketSendOKCnt
    host.o(i.nrf_esb_event_handler) refers to esbprocess.o(.data) for tx_payload
    host.o(i.nrf_esb_event_handler) refers to esbprocess.o(.bss) for rx_payload
    host.o(i.timers_init) refers to app_timer.o(i.app_timer_init) for app_timer_init
    host.o(i.timers_init) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    host.o(i.timers_init) refers to app_timer.o(i.app_timer_create) for app_timer_create
    host.o(i.timers_init) refers to host.o(i.esb_send_packet_timer_callback) for esb_send_packet_timer_callback
    host.o(i.timers_init) refers to host.o(.constdata) for m_esb_tx_timer_id
    host.o(i.timers_init) refers to host.o(i.Timer_1S) for Timer_1S
    host.o(i.timers_start) refers to app_timer.o(i.app_timer_start) for app_timer_start
    host.o(i.timers_start) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    host.o(i.timers_start) refers to host.o(.constdata) for Timer_1S_timer_id
    host.o(.constdata) refers to host.o(.bss) for m_esb_tx_timer_id_data
    esbprocess.o(i.EebTxRxSwitch) refers to nrf_esb.o(i.nrf_esb_disable) for nrf_esb_disable
    esbprocess.o(i.EebTxRxSwitch) refers to nrf_esb.o(i.nrf_esb_init) for nrf_esb_init
    esbprocess.o(i.EebTxRxSwitch) refers to nrf_esb.o(i.nrf_esb_start_rx) for nrf_esb_start_rx
    esbprocess.o(i.EebTxRxSwitch) refers to nrf_esb.o(i.nrf_esb_stop_rx) for nrf_esb_stop_rx
    esbprocess.o(i.EebTxRxSwitch) refers to nrf_esb.o(i.nrf_esb_start_tx) for nrf_esb_start_tx
    esbprocess.o(i.EebTxRxSwitch) refers to esbprocess.o(.data) for nrf_esb_config
    esbprocess.o(i.esb_init) refers to nrf_esb.o(i.nrf_esb_init) for nrf_esb_init
    esbprocess.o(i.esb_init) refers to nrf_esb.o(i.nrf_esb_set_base_address_0) for nrf_esb_set_base_address_0
    esbprocess.o(i.esb_init) refers to nrf_esb.o(i.nrf_esb_set_base_address_1) for nrf_esb_set_base_address_1
    esbprocess.o(i.esb_init) refers to nrf_esb.o(i.nrf_esb_set_prefixes) for nrf_esb_set_prefixes
    esbprocess.o(i.esb_init) refers to esbprocess.o(.data) for nrf_esb_config
    esbprocess.o(i.esb_init) refers to host.o(i.nrf_esb_event_handler) for nrf_esb_event_handler
    boards.o(i.bsp_board_button_idx_to_pin) refers to boards.o(.constdata) for m_board_btn_list
    boards.o(i.bsp_board_button_state_get) refers to boards.o(.constdata) for m_board_btn_list
    boards.o(i.bsp_board_buttons_init) refers to boards.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    boards.o(i.bsp_board_buttons_init) refers to boards.o(.constdata) for m_board_btn_list
    boards.o(i.bsp_board_init) refers to boards.o(i.bsp_board_leds_init) for bsp_board_leds_init
    boards.o(i.bsp_board_init) refers to boards.o(i.bsp_board_buttons_init) for bsp_board_buttons_init
    boards.o(i.bsp_board_led_idx_to_pin) refers to boards.o(.constdata) for m_board_led_list
    boards.o(i.bsp_board_led_invert) refers to boards.o(.constdata) for m_board_led_list
    boards.o(i.bsp_board_led_off) refers to boards.o(i.nrf_gpio_pin_write) for nrf_gpio_pin_write
    boards.o(i.bsp_board_led_off) refers to boards.o(.constdata) for m_board_led_list
    boards.o(i.bsp_board_led_on) refers to boards.o(i.nrf_gpio_pin_write) for nrf_gpio_pin_write
    boards.o(i.bsp_board_led_on) refers to boards.o(.constdata) for m_board_led_list
    boards.o(i.bsp_board_led_state_get) refers to boards.o(.constdata) for m_board_led_list
    boards.o(i.bsp_board_leds_init) refers to boards.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    boards.o(i.bsp_board_leds_init) refers to boards.o(i.bsp_board_leds_off) for bsp_board_leds_off
    boards.o(i.bsp_board_leds_init) refers to boards.o(.constdata) for m_board_led_list
    boards.o(i.bsp_board_leds_off) refers to boards.o(i.bsp_board_led_off) for bsp_board_led_off
    boards.o(i.bsp_board_leds_on) refers to boards.o(i.bsp_board_led_on) for bsp_board_led_on
    boards.o(i.bsp_board_pin_to_button_idx) refers to boards.o(.constdata) for m_board_btn_list
    boards.o(i.bsp_board_pin_to_led_idx) refers to boards.o(.constdata) for m_board_led_list
    nrf_drv_uart.o(i.nrf_drv_uart_init) refers to memcpya.o(.text) for __aeabi_memcpy4
    nrf_drv_uart.o(i.nrf_drv_uart_init) refers to nrfx_uarte.o(i.nrfx_uarte_init) for nrfx_uarte_init
    nrf_drv_uart.o(i.nrf_drv_uart_init) refers to nrfx_uart.o(i.nrfx_uart_init) for nrfx_uart_init
    nrf_drv_uart.o(i.nrf_drv_uart_init) refers to nrf_drv_uart.o(.data) for m_handlers
    nrf_drv_uart.o(i.nrf_drv_uart_init) refers to nrf_drv_uart.o(i.uarte_evt_handler) for uarte_evt_handler
    nrf_drv_uart.o(i.nrf_drv_uart_init) refers to nrf_drv_uart.o(i.uart_evt_handler) for uart_evt_handler
    nrf_drv_uart.o(i.uart_evt_handler) refers to nrf_drv_uart.o(.data) for m_contexts
    nrf_drv_uart.o(i.uarte_evt_handler) refers to nrf_drv_uart.o(.data) for m_contexts
    nrfx_prs.o(i.UARTE0_UART0_IRQHandler) refers to nrfx_prs.o(.data) for m_prs_box_4
    nrfx_prs.o(i.nrfx_prs_acquire) refers to nrfx_prs.o(i.prs_box_get) for prs_box_get
    nrfx_prs.o(i.nrfx_prs_acquire) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrfx_prs.o(i.nrfx_prs_acquire) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrfx_prs.o(i.nrfx_prs_release) refers to nrfx_prs.o(i.prs_box_get) for prs_box_get
    nrfx_prs.o(i.prs_box_get) refers to nrfx_prs.o(.data) for m_prs_box_4
    nrfx_uart.o(i.apply_config) refers to nrfx_uart.o(i.nrf_gpio_pin_set) for nrf_gpio_pin_set
    nrfx_uart.o(i.apply_config) refers to nrfx_uart.o(i.nrf_gpio_cfg_output) for nrf_gpio_cfg_output
    nrfx_uart.o(i.apply_config) refers to nrfx_uart.o(i.nrf_gpio_cfg_input) for nrf_gpio_cfg_input
    nrfx_uart.o(i.apply_config) refers to nrfx_uart.o(i.nrf_uart_txrx_pins_set) for nrf_uart_txrx_pins_set
    nrfx_uart.o(i.apply_config) refers to nrfx_uart.o(i.nrf_uart_hwfc_pins_set) for nrf_uart_hwfc_pins_set
    nrfx_uart.o(i.interrupts_disable) refers to nrfx_uart.o(i.nrf_uart_int_disable) for nrf_uart_int_disable
    nrfx_uart.o(i.interrupts_disable) refers to nrfx_uart.o(i.nrfx_get_irq_number) for nrfx_get_irq_number
    nrfx_uart.o(i.interrupts_enable) refers to nrfx_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrfx_uart.o(i.interrupts_enable) refers to nrfx_uart.o(i.nrf_uart_int_enable) for nrf_uart_int_enable
    nrfx_uart.o(i.interrupts_enable) refers to nrfx_uart.o(i.nrfx_get_irq_number) for nrfx_get_irq_number
    nrfx_uart.o(i.nrf_gpio_cfg_default) refers to nrfx_uart.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_uart.o(i.nrf_gpio_cfg_input) refers to nrfx_uart.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_uart.o(i.nrf_gpio_cfg_output) refers to nrfx_uart.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_uart.o(i.nrfx_uart_0_irq_handler) refers to nrfx_uart.o(i.uart_irq_handler) for uart_irq_handler
    nrfx_uart.o(i.nrfx_uart_0_irq_handler) refers to nrfx_uart.o(.bss) for m_cb
    nrfx_uart.o(i.nrfx_uart_errorsrc_get) refers to nrfx_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrfx_uart.o(i.nrfx_uart_errorsrc_get) refers to nrfx_uart.o(i.nrf_uart_errorsrc_get_and_clear) for nrf_uart_errorsrc_get_and_clear
    nrfx_uart.o(i.nrfx_uart_init) refers to nrfx_prs.o(i.nrfx_prs_acquire) for nrfx_prs_acquire
    nrfx_uart.o(i.nrfx_uart_init) refers to nrfx_uart.o(i.apply_config) for apply_config
    nrfx_uart.o(i.nrfx_uart_init) refers to nrfx_uart.o(i.interrupts_enable) for interrupts_enable
    nrfx_uart.o(i.nrfx_uart_init) refers to nrfx_uart.o(.bss) for m_cb
    nrfx_uart.o(i.nrfx_uart_init) refers to nrfx_uart.o(.constdata) for irq_handlers
    nrfx_uart.o(i.nrfx_uart_rx) refers to nrfx_uart.o(i.nrf_uart_int_disable) for nrf_uart_int_disable
    nrfx_uart.o(i.nrfx_uart_rx) refers to nrfx_uart.o(i.nrf_uart_int_enable) for nrf_uart_int_enable
    nrfx_uart.o(i.nrfx_uart_rx) refers to nrfx_uart.o(i.rx_enable) for rx_enable
    nrfx_uart.o(i.nrfx_uart_rx) refers to nrfx_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrfx_uart.o(i.nrfx_uart_rx) refers to nrfx_uart.o(i.nrf_uart_event_check) for nrf_uart_event_check
    nrfx_uart.o(i.nrfx_uart_rx) refers to nrfx_uart.o(i.rx_byte) for rx_byte
    nrfx_uart.o(i.nrfx_uart_rx) refers to nrfx_uart.o(i.nrf_uart_task_trigger) for nrf_uart_task_trigger
    nrfx_uart.o(i.nrfx_uart_rx) refers to nrfx_uart.o(.bss) for m_cb
    nrfx_uart.o(i.nrfx_uart_rx_abort) refers to nrfx_uart.o(i.nrf_uart_int_disable) for nrf_uart_int_disable
    nrfx_uart.o(i.nrfx_uart_rx_abort) refers to nrfx_uart.o(i.nrf_uart_task_trigger) for nrf_uart_task_trigger
    nrfx_uart.o(i.nrfx_uart_rx_disable) refers to nrfx_uart.o(i.nrf_uart_task_trigger) for nrf_uart_task_trigger
    nrfx_uart.o(i.nrfx_uart_rx_disable) refers to nrfx_uart.o(.bss) for m_cb
    nrfx_uart.o(i.nrfx_uart_rx_enable) refers to nrfx_uart.o(i.rx_enable) for rx_enable
    nrfx_uart.o(i.nrfx_uart_rx_enable) refers to nrfx_uart.o(.bss) for m_cb
    nrfx_uart.o(i.nrfx_uart_rx_ready) refers to nrfx_uart.o(i.nrf_uart_event_check) for nrf_uart_event_check
    nrfx_uart.o(i.nrfx_uart_tx) refers to nrfx_uart.o(i.nrfx_uart_tx_in_progress) for nrfx_uart_tx_in_progress
    nrfx_uart.o(i.nrfx_uart_tx) refers to nrfx_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrfx_uart.o(i.nrfx_uart_tx) refers to nrfx_uart.o(i.nrf_uart_task_trigger) for nrf_uart_task_trigger
    nrfx_uart.o(i.nrfx_uart_tx) refers to nrfx_uart.o(i.tx_byte) for tx_byte
    nrfx_uart.o(i.nrfx_uart_tx) refers to nrfx_uart.o(i.tx_blocking) for tx_blocking
    nrfx_uart.o(i.nrfx_uart_tx) refers to nrfx_uart.o(i.nrf_uart_event_check) for nrf_uart_event_check
    nrfx_uart.o(i.nrfx_uart_tx) refers to nrfx_uart.o(.bss) for m_cb
    nrfx_uart.o(i.nrfx_uart_tx_abort) refers to nrfx_uart.o(i.nrf_uart_task_trigger) for nrf_uart_task_trigger
    nrfx_uart.o(i.nrfx_uart_tx_abort) refers to nrfx_uart.o(i.tx_done_event) for tx_done_event
    nrfx_uart.o(i.nrfx_uart_tx_abort) refers to nrfx_uart.o(.bss) for m_cb
    nrfx_uart.o(i.nrfx_uart_tx_in_progress) refers to nrfx_uart.o(.bss) for m_cb
    nrfx_uart.o(i.nrfx_uart_uninit) refers to nrfx_uart.o(i.interrupts_disable) for interrupts_disable
    nrfx_uart.o(i.nrfx_uart_uninit) refers to nrfx_uart.o(i.pins_to_default) for pins_to_default
    nrfx_uart.o(i.nrfx_uart_uninit) refers to nrfx_prs.o(i.nrfx_prs_release) for nrfx_prs_release
    nrfx_uart.o(i.nrfx_uart_uninit) refers to nrfx_uart.o(.bss) for m_cb
    nrfx_uart.o(i.pins_to_default) refers to nrfx_uart.o(i.nrf_uart_txrx_pins_set) for nrf_uart_txrx_pins_set
    nrfx_uart.o(i.pins_to_default) refers to nrfx_uart.o(i.nrf_uart_hwfc_pins_set) for nrf_uart_hwfc_pins_set
    nrfx_uart.o(i.pins_to_default) refers to nrfx_uart.o(i.nrf_gpio_cfg_default) for nrf_gpio_cfg_default
    nrfx_uart.o(i.rx_byte) refers to nrfx_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrfx_uart.o(i.rx_enable) refers to nrfx_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrfx_uart.o(i.rx_enable) refers to nrfx_uart.o(i.nrf_uart_task_trigger) for nrf_uart_task_trigger
    nrfx_uart.o(i.tx_blocking) refers to nrfx_uart.o(i.nrf_uart_event_check) for nrf_uart_event_check
    nrfx_uart.o(i.tx_blocking) refers to nrfx_uart.o(i.tx_byte) for tx_byte
    nrfx_uart.o(i.tx_byte) refers to nrfx_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrfx_uart.o(i.uart_irq_handler) refers to nrfx_uart.o(i.nrf_uart_int_enable_check) for nrf_uart_int_enable_check
    nrfx_uart.o(i.uart_irq_handler) refers to nrfx_uart.o(i.nrf_uart_event_check) for nrf_uart_event_check
    nrfx_uart.o(i.uart_irq_handler) refers to nrfx_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrfx_uart.o(i.uart_irq_handler) refers to nrfx_uart.o(i.nrf_uart_int_disable) for nrf_uart_int_disable
    nrfx_uart.o(i.uart_irq_handler) refers to nrfx_uart.o(i.nrf_uart_task_trigger) for nrf_uart_task_trigger
    nrfx_uart.o(i.uart_irq_handler) refers to nrfx_uart.o(i.nrf_uart_errorsrc_get_and_clear) for nrf_uart_errorsrc_get_and_clear
    nrfx_uart.o(i.uart_irq_handler) refers to nrfx_uart.o(i.rx_byte) for rx_byte
    nrfx_uart.o(i.uart_irq_handler) refers to nrfx_uart.o(i.rx_done_event) for rx_done_event
    nrfx_uart.o(i.uart_irq_handler) refers to nrfx_uart.o(i.tx_byte) for tx_byte
    nrfx_uart.o(i.uart_irq_handler) refers to nrfx_uart.o(i.tx_done_event) for tx_done_event
    nrfx_uart.o(.constdata) refers to nrfx_uart.o(i.nrfx_uart_0_irq_handler) for nrfx_uart_0_irq_handler
    nrfx_uarte.o(i.apply_config) refers to nrfx_uarte.o(i.nrf_gpio_pin_set) for nrf_gpio_pin_set
    nrfx_uarte.o(i.apply_config) refers to nrfx_uarte.o(i.nrf_gpio_cfg_output) for nrf_gpio_cfg_output
    nrfx_uarte.o(i.apply_config) refers to nrfx_uarte.o(i.nrf_gpio_cfg_input) for nrf_gpio_cfg_input
    nrfx_uarte.o(i.apply_config) refers to nrfx_uarte.o(i.nrf_uarte_txrx_pins_set) for nrf_uarte_txrx_pins_set
    nrfx_uarte.o(i.apply_config) refers to nrfx_uarte.o(i.nrf_uarte_hwfc_pins_set) for nrf_uarte_hwfc_pins_set
    nrfx_uarte.o(i.interrupts_disable) refers to nrfx_uarte.o(i.nrf_uarte_int_disable) for nrf_uarte_int_disable
    nrfx_uarte.o(i.interrupts_disable) refers to nrfx_uarte.o(i.nrfx_get_irq_number) for nrfx_get_irq_number
    nrfx_uarte.o(i.interrupts_enable) refers to nrfx_uarte.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrfx_uarte.o(i.interrupts_enable) refers to nrfx_uarte.o(i.nrf_uarte_int_enable) for nrf_uarte_int_enable
    nrfx_uarte.o(i.interrupts_enable) refers to nrfx_uarte.o(i.nrfx_get_irq_number) for nrfx_get_irq_number
    nrfx_uarte.o(i.nrf_gpio_cfg_default) refers to nrfx_uarte.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_uarte.o(i.nrf_gpio_cfg_input) refers to nrfx_uarte.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_uarte.o(i.nrf_gpio_cfg_output) refers to nrfx_uarte.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_uarte.o(i.nrfx_uarte_0_irq_handler) refers to nrfx_uarte.o(i.uarte_irq_handler) for uarte_irq_handler
    nrfx_uarte.o(i.nrfx_uarte_0_irq_handler) refers to nrfx_uarte.o(.bss) for m_cb
    nrfx_uarte.o(i.nrfx_uarte_errorsrc_get) refers to nrfx_uarte.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrfx_uarte.o(i.nrfx_uarte_errorsrc_get) refers to nrfx_uarte.o(i.nrf_uarte_errorsrc_get_and_clear) for nrf_uarte_errorsrc_get_and_clear
    nrfx_uarte.o(i.nrfx_uarte_init) refers to nrfx_prs.o(i.nrfx_prs_acquire) for nrfx_prs_acquire
    nrfx_uarte.o(i.nrfx_uarte_init) refers to nrfx_uarte.o(i.apply_config) for apply_config
    nrfx_uarte.o(i.nrfx_uarte_init) refers to nrfx_uarte.o(i.interrupts_enable) for interrupts_enable
    nrfx_uarte.o(i.nrfx_uarte_init) refers to nrfx_uarte.o(.bss) for m_cb
    nrfx_uarte.o(i.nrfx_uarte_init) refers to nrfx_uarte.o(.constdata) for irq_handlers
    nrfx_uarte.o(i.nrfx_uarte_rx) refers to nrfx_uarte.o(i.nrfx_is_in_ram) for nrfx_is_in_ram
    nrfx_uarte.o(i.nrfx_uarte_rx) refers to nrfx_uarte.o(i.nrf_uarte_int_disable) for nrf_uarte_int_disable
    nrfx_uarte.o(i.nrfx_uarte_rx) refers to nrfx_uarte.o(i.nrf_uarte_int_enable) for nrf_uarte_int_enable
    nrfx_uarte.o(i.nrfx_uarte_rx) refers to nrfx_uarte.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrfx_uarte.o(i.nrfx_uarte_rx) refers to nrfx_uarte.o(i.nrf_uarte_task_trigger) for nrf_uarte_task_trigger
    nrfx_uarte.o(i.nrfx_uarte_rx) refers to nrfx_uarte.o(i.nrf_uarte_event_check) for nrf_uarte_event_check
    nrfx_uarte.o(i.nrfx_uarte_rx) refers to nrfx_uarte.o(.bss) for m_cb
    nrfx_uarte.o(i.nrfx_uarte_rx_abort) refers to nrfx_uarte.o(i.nrf_uarte_task_trigger) for nrf_uarte_task_trigger
    nrfx_uarte.o(i.nrfx_uarte_rx_ready) refers to nrfx_uarte.o(i.nrf_uarte_event_check) for nrf_uarte_event_check
    nrfx_uarte.o(i.nrfx_uarte_tx) refers to nrfx_uarte.o(i.nrfx_is_in_ram) for nrfx_is_in_ram
    nrfx_uarte.o(i.nrfx_uarte_tx) refers to nrfx_uarte.o(i.nrfx_uarte_tx_in_progress) for nrfx_uarte_tx_in_progress
    nrfx_uarte.o(i.nrfx_uarte_tx) refers to nrfx_uarte.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrfx_uarte.o(i.nrfx_uarte_tx) refers to nrfx_uarte.o(i.nrf_uarte_task_trigger) for nrf_uarte_task_trigger
    nrfx_uarte.o(i.nrfx_uarte_tx) refers to nrfx_uarte.o(i.nrf_uarte_event_check) for nrf_uarte_event_check
    nrfx_uarte.o(i.nrfx_uarte_tx) refers to nrfx_uarte.o(.bss) for m_cb
    nrfx_uarte.o(i.nrfx_uarte_tx_abort) refers to nrfx_uarte.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrfx_uarte.o(i.nrfx_uarte_tx_abort) refers to nrfx_uarte.o(i.nrf_uarte_task_trigger) for nrf_uarte_task_trigger
    nrfx_uarte.o(i.nrfx_uarte_tx_abort) refers to nrfx_uarte.o(i.nrf_uarte_event_check) for nrf_uarte_event_check
    nrfx_uarte.o(i.nrfx_uarte_tx_abort) refers to nrfx_uarte.o(.bss) for m_cb
    nrfx_uarte.o(i.nrfx_uarte_tx_in_progress) refers to nrfx_uarte.o(.bss) for m_cb
    nrfx_uarte.o(i.nrfx_uarte_uninit) refers to nrfx_uarte.o(i.interrupts_disable) for interrupts_disable
    nrfx_uarte.o(i.nrfx_uarte_uninit) refers to nrfx_uarte.o(i.pins_to_default) for pins_to_default
    nrfx_uarte.o(i.nrfx_uarte_uninit) refers to nrfx_prs.o(i.nrfx_prs_release) for nrfx_prs_release
    nrfx_uarte.o(i.nrfx_uarte_uninit) refers to nrfx_uarte.o(.bss) for m_cb
    nrfx_uarte.o(i.pins_to_default) refers to nrfx_uarte.o(i.nrf_uarte_txrx_pins_set) for nrf_uarte_txrx_pins_set
    nrfx_uarte.o(i.pins_to_default) refers to nrfx_uarte.o(i.nrf_uarte_hwfc_pins_set) for nrf_uarte_hwfc_pins_set
    nrfx_uarte.o(i.pins_to_default) refers to nrfx_uarte.o(i.nrf_gpio_cfg_default) for nrf_gpio_cfg_default
    nrfx_uarte.o(i.uarte_irq_handler) refers to nrfx_uarte.o(i.nrf_uarte_event_check) for nrf_uarte_event_check
    nrfx_uarte.o(i.uarte_irq_handler) refers to nrfx_uarte.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrfx_uarte.o(i.uarte_irq_handler) refers to nrfx_uarte.o(i.nrf_uarte_errorsrc_get_and_clear) for nrf_uarte_errorsrc_get_and_clear
    nrfx_uarte.o(i.uarte_irq_handler) refers to nrfx_uarte.o(i.nrf_uarte_rx_amount_get) for nrf_uarte_rx_amount_get
    nrfx_uarte.o(i.uarte_irq_handler) refers to nrfx_uarte.o(i.rx_done_event) for rx_done_event
    nrfx_uarte.o(i.uarte_irq_handler) refers to nrfx_uarte.o(i.tx_done_event) for tx_done_event
    nrfx_uarte.o(.constdata) refers to nrfx_uarte.o(i.nrfx_uarte_0_irq_handler) for nrfx_uarte_0_irq_handler
    nrfx_gpiote.o(i.GPIOTE_IRQHandler) refers to nrfx_gpiote.o(i.nrf_gpiote_event_is_set) for nrf_gpiote_event_is_set
    nrfx_gpiote.o(i.GPIOTE_IRQHandler) refers to nrfx_gpiote.o(i.nrf_gpiote_event_clear) for nrf_gpiote_event_clear
    nrfx_gpiote.o(i.GPIOTE_IRQHandler) refers to nrfx_gpiote.o(i.nrf_gpio_ports_read) for nrf_gpio_ports_read
    nrfx_gpiote.o(i.GPIOTE_IRQHandler) refers to nrfx_gpiote.o(i.channel_handler_get) for channel_handler_get
    nrfx_gpiote.o(i.GPIOTE_IRQHandler) refers to nrfx_gpiote.o(i.nrf_bitmask_bit_is_set) for nrf_bitmask_bit_is_set
    nrfx_gpiote.o(i.GPIOTE_IRQHandler) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.GPIOTE_IRQHandler) refers to nrfx_gpiote.o(i.nrf_bitmask_bit_set) for nrf_bitmask_bit_set
    nrfx_gpiote.o(i.GPIOTE_IRQHandler) refers to nrfx_gpiote.o(i.nrf_gpio_cfg_sense_set) for nrf_gpio_cfg_sense_set
    nrfx_gpiote.o(i.GPIOTE_IRQHandler) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.channel_free) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.channel_handler_get) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.channel_port_alloc) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.channel_port_get) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.nrf_gpio_cfg_default) refers to nrfx_gpiote.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_gpiote.o(i.nrf_gpio_ports_read) refers to nrfx_gpiote.o(.constdata) for .constdata
    nrfx_gpiote.o(i.nrf_gpiote_event_clear) refers to nrfx_gpiote.o(i.nrf_gpiote_event_addr_get) for nrf_gpiote_event_addr_get
    nrfx_gpiote.o(i.nrf_gpiote_event_is_set) refers to nrfx_gpiote.o(i.nrf_gpiote_event_addr_get) for nrf_gpiote_event_addr_get
    nrfx_gpiote.o(i.nrfx_gpiote_clr_task_addr_get) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_clr_task_addr_get) refers to nrfx_gpiote.o(i.nrf_gpiote_task_addr_get) for nrf_gpiote_task_addr_get
    nrfx_gpiote.o(i.nrfx_gpiote_clr_task_trigger) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_addr_get) refers to nrfx_gpiote.o(i.pin_in_use_by_te) for pin_in_use_by_te
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_addr_get) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_addr_get) refers to nrfx_gpiote.o(i.nrf_gpiote_event_addr_get) for nrf_gpiote_event_addr_get
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_disable) refers to nrfx_gpiote.o(i.pin_in_use_by_port) for pin_in_use_by_port
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_disable) refers to nrfx_gpiote.o(i.nrf_gpio_cfg_sense_set) for nrf_gpio_cfg_sense_set
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_disable) refers to nrfx_gpiote.o(i.pin_in_use_by_te) for pin_in_use_by_te
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_disable) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable) refers to nrfx_gpiote.o(i.pin_in_use_by_port) for pin_in_use_by_port
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable) refers to nrfx_gpiote.o(i.nrf_gpio_pin_read) for nrf_gpio_pin_read
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable) refers to nrfx_gpiote.o(i.nrf_gpio_cfg_sense_set) for nrf_gpio_cfg_sense_set
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable) refers to nrfx_gpiote.o(i.pin_in_use_by_te) for pin_in_use_by_te
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable) refers to nrfx_gpiote.o(i.nrf_gpiote_event_clear) for nrf_gpiote_event_clear
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable) refers to nrfx_gpiote.o(i.channel_handler_get) for channel_handler_get
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable) refers to nrfx_gpiote.o(i.nrf_gpiote_int_enable) for nrf_gpiote_int_enable
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.nrfx_gpiote_in_init) refers to nrfx_gpiote.o(i.pin_in_use_by_gpiote) for pin_in_use_by_gpiote
    nrfx_gpiote.o(i.nrfx_gpiote_in_init) refers to nrfx_gpiote.o(i.channel_port_alloc) for channel_port_alloc
    nrfx_gpiote.o(i.nrfx_gpiote_in_init) refers to nrfx_gpiote.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_gpiote.o(i.nrfx_gpiote_in_init) refers to nrfx_gpiote.o(i.pin_configured_set) for pin_configured_set
    nrfx_gpiote.o(i.nrfx_gpiote_in_init) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.nrfx_gpiote_in_is_set) refers to nrfx_gpiote.o(i.nrf_gpio_pin_read) for nrf_gpio_pin_read
    nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) refers to nrfx_gpiote.o(i.nrfx_gpiote_in_event_disable) for nrfx_gpiote_in_event_disable
    nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) refers to nrfx_gpiote.o(i.pin_in_use_by_te) for pin_in_use_by_te
    nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) refers to nrfx_gpiote.o(i.nrf_gpiote_te_default) for nrf_gpiote_te_default
    nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) refers to nrfx_gpiote.o(i.pin_configured_check) for pin_configured_check
    nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) refers to nrfx_gpiote.o(i.nrf_gpio_cfg_default) for nrf_gpio_cfg_default
    nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) refers to nrfx_gpiote.o(i.pin_configured_clear) for pin_configured_clear
    nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) refers to nrfx_gpiote.o(i.channel_free) for channel_free
    nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) refers to nrfx_gpiote.o(i.pin_in_use_clear) for pin_in_use_clear
    nrfx_gpiote.o(i.nrfx_gpiote_init) refers to nrfx_gpiote.o(i.pin_in_use_clear) for pin_in_use_clear
    nrfx_gpiote.o(i.nrfx_gpiote_init) refers to nrfx_gpiote.o(i.channel_free) for channel_free
    nrfx_gpiote.o(i.nrfx_gpiote_init) refers to nrfx_gpiote.o(i.nrf_gpiote_event_clear) for nrf_gpiote_event_clear
    nrfx_gpiote.o(i.nrfx_gpiote_init) refers to nrfx_gpiote.o(i.nrf_gpiote_int_enable) for nrf_gpiote_int_enable
    nrfx_gpiote.o(i.nrfx_gpiote_init) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.nrfx_gpiote_is_init) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.nrfx_gpiote_out_clear) refers to nrfx_gpiote.o(i.nrf_gpio_pin_clear) for nrf_gpio_pin_clear
    nrfx_gpiote.o(i.nrfx_gpiote_out_init) refers to nrfx_gpiote.o(i.channel_port_alloc) for channel_port_alloc
    nrfx_gpiote.o(i.nrfx_gpiote_out_init) refers to nrfx_gpiote.o(i.nrf_gpio_pin_set) for nrf_gpio_pin_set
    nrfx_gpiote.o(i.nrfx_gpiote_out_init) refers to nrfx_gpiote.o(i.nrf_gpio_pin_clear) for nrf_gpio_pin_clear
    nrfx_gpiote.o(i.nrfx_gpiote_out_init) refers to nrfx_gpiote.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_gpiote.o(i.nrfx_gpiote_out_init) refers to nrfx_gpiote.o(i.pin_configured_set) for pin_configured_set
    nrfx_gpiote.o(i.nrfx_gpiote_out_init) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.nrfx_gpiote_out_set) refers to nrfx_gpiote.o(i.nrf_gpio_pin_set) for nrf_gpio_pin_set
    nrfx_gpiote.o(i.nrfx_gpiote_out_task_addr_get) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_out_task_addr_get) refers to nrfx_gpiote.o(i.nrf_gpiote_task_addr_get) for nrf_gpiote_task_addr_get
    nrfx_gpiote.o(i.nrfx_gpiote_out_task_disable) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.nrfx_gpiote_out_task_enable) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.nrfx_gpiote_out_task_force) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.nrfx_gpiote_out_task_trigger) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_out_uninit) refers to nrfx_gpiote.o(i.pin_in_use_by_te) for pin_in_use_by_te
    nrfx_gpiote.o(i.nrfx_gpiote_out_uninit) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_out_uninit) refers to nrfx_gpiote.o(i.channel_free) for channel_free
    nrfx_gpiote.o(i.nrfx_gpiote_out_uninit) refers to nrfx_gpiote.o(i.nrf_gpiote_te_default) for nrf_gpiote_te_default
    nrfx_gpiote.o(i.nrfx_gpiote_out_uninit) refers to nrfx_gpiote.o(i.pin_in_use_clear) for pin_in_use_clear
    nrfx_gpiote.o(i.nrfx_gpiote_out_uninit) refers to nrfx_gpiote.o(i.pin_configured_check) for pin_configured_check
    nrfx_gpiote.o(i.nrfx_gpiote_out_uninit) refers to nrfx_gpiote.o(i.nrf_gpio_cfg_default) for nrf_gpio_cfg_default
    nrfx_gpiote.o(i.nrfx_gpiote_out_uninit) refers to nrfx_gpiote.o(i.pin_configured_clear) for pin_configured_clear
    nrfx_gpiote.o(i.nrfx_gpiote_set_task_addr_get) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_set_task_addr_get) refers to nrfx_gpiote.o(i.nrf_gpiote_task_addr_get) for nrf_gpiote_task_addr_get
    nrfx_gpiote.o(i.nrfx_gpiote_set_task_trigger) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_uninit) refers to nrfx_gpiote.o(i.nrfx_gpiote_out_uninit) for nrfx_gpiote_out_uninit
    nrfx_gpiote.o(i.nrfx_gpiote_uninit) refers to nrfx_gpiote.o(i.pin_in_use_by_gpiote) for pin_in_use_by_gpiote
    nrfx_gpiote.o(i.nrfx_gpiote_uninit) refers to nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) for nrfx_gpiote_in_uninit
    nrfx_gpiote.o(i.nrfx_gpiote_uninit) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.pin_configured_check) refers to nrfx_gpiote.o(i.nrf_bitmask_bit_is_set) for nrf_bitmask_bit_is_set
    nrfx_gpiote.o(i.pin_configured_check) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.pin_configured_clear) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.pin_configured_set) refers to nrfx_gpiote.o(i.nrf_bitmask_bit_set) for nrf_bitmask_bit_set
    nrfx_gpiote.o(i.pin_configured_set) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.pin_in_use_by_gpiote) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.pin_in_use_by_port) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.pin_in_use_by_te) refers to nrfx_gpiote.o(.bss) for m_cb
    nrfx_gpiote.o(i.pin_in_use_clear) refers to nrfx_gpiote.o(.bss) for m_cb
    app_error.o(i.app_error_handler_bare) refers to app_error_weak.o(i.app_error_fault_handler) for app_error_fault_handler
    app_error.o(i.app_error_save_and_stop) refers to app_error.o(.bss) for m_error_data
    app_error_handler_keil.o(.emb_text) refers to app_error_weak.o(i.app_error_fault_handler) for app_error_fault_handler
    app_fifo.o(i.app_fifo_get) refers to app_fifo.o(i.fifo_length) for fifo_length
    app_fifo.o(i.app_fifo_get) refers to app_fifo.o(i.fifo_get) for fifo_get
    app_fifo.o(i.app_fifo_peek) refers to app_fifo.o(i.fifo_length) for fifo_length
    app_fifo.o(i.app_fifo_peek) refers to app_fifo.o(i.fifo_peek) for fifo_peek
    app_fifo.o(i.app_fifo_put) refers to app_fifo.o(i.fifo_length) for fifo_length
    app_fifo.o(i.app_fifo_put) refers to app_fifo.o(i.fifo_put) for fifo_put
    app_fifo.o(i.app_fifo_read) refers to app_fifo.o(i.fifo_length) for fifo_length
    app_fifo.o(i.app_fifo_read) refers to app_fifo.o(i.fifo_get) for fifo_get
    app_fifo.o(i.app_fifo_write) refers to app_fifo.o(i.fifo_length) for fifo_length
    app_fifo.o(i.app_fifo_write) refers to app_fifo.o(i.fifo_put) for fifo_put
    app_fifo.o(i.fifo_get) refers to app_fifo.o(i.fifo_peek) for fifo_peek
    app_uart_fifo.o(i.app_uart_close) refers to nrfx_uarte.o(i.nrfx_uarte_uninit) for nrfx_uarte_uninit
    app_uart_fifo.o(i.app_uart_close) refers to nrfx_uart.o(i.nrfx_uart_uninit) for nrfx_uart_uninit
    app_uart_fifo.o(i.app_uart_close) refers to app_uart_fifo.o(.data) for app_uart_inst
    app_uart_fifo.o(i.app_uart_close) refers to nrf_drv_uart.o(.data) for nrf_drv_uart_use_easy_dma
    app_uart_fifo.o(i.app_uart_flush) refers to app_fifo.o(i.app_fifo_flush) for app_fifo_flush
    app_uart_fifo.o(i.app_uart_flush) refers to app_uart_fifo.o(.bss) for m_rx_fifo
    app_uart_fifo.o(i.app_uart_get) refers to app_fifo.o(i.app_fifo_get) for app_fifo_get
    app_uart_fifo.o(i.app_uart_get) refers to app_uart_fifo.o(i.nrf_drv_uart_rx) for nrf_drv_uart_rx
    app_uart_fifo.o(i.app_uart_get) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    app_uart_fifo.o(i.app_uart_get) refers to app_uart_fifo.o(.data) for m_rx_ovf
    app_uart_fifo.o(i.app_uart_get) refers to app_uart_fifo.o(.bss) for m_rx_fifo
    app_uart_fifo.o(i.app_uart_init) refers to app_fifo.o(i.app_fifo_init) for app_fifo_init
    app_uart_fifo.o(i.app_uart_init) refers to memcpya.o(.text) for __aeabi_memcpy4
    app_uart_fifo.o(i.app_uart_init) refers to nrf_drv_uart.o(i.nrf_drv_uart_init) for nrf_drv_uart_init
    app_uart_fifo.o(i.app_uart_init) refers to app_uart_fifo.o(i.nrf_drv_uart_rx) for nrf_drv_uart_rx
    app_uart_fifo.o(i.app_uart_init) refers to app_uart_fifo.o(.data) for m_event_handler
    app_uart_fifo.o(i.app_uart_init) refers to app_uart_fifo.o(.bss) for m_rx_fifo
    app_uart_fifo.o(i.app_uart_init) refers to app_uart_fifo.o(.constdata) for .constdata
    app_uart_fifo.o(i.app_uart_init) refers to app_uart_fifo.o(i.uart_event_handler) for uart_event_handler
    app_uart_fifo.o(i.app_uart_put) refers to app_fifo.o(i.app_fifo_put) for app_fifo_put
    app_uart_fifo.o(i.app_uart_put) refers to nrfx_uarte.o(i.nrfx_uarte_tx_in_progress) for nrfx_uarte_tx_in_progress
    app_uart_fifo.o(i.app_uart_put) refers to nrfx_uart.o(i.nrfx_uart_tx_in_progress) for nrfx_uart_tx_in_progress
    app_uart_fifo.o(i.app_uart_put) refers to app_fifo.o(i.app_fifo_get) for app_fifo_get
    app_uart_fifo.o(i.app_uart_put) refers to app_uart_fifo.o(i.nrf_drv_uart_tx) for nrf_drv_uart_tx
    app_uart_fifo.o(i.app_uart_put) refers to app_uart_fifo.o(.bss) for m_tx_fifo
    app_uart_fifo.o(i.app_uart_put) refers to app_uart_fifo.o(.data) for app_uart_inst
    app_uart_fifo.o(i.app_uart_put) refers to nrf_drv_uart.o(.data) for nrf_drv_uart_use_easy_dma
    app_uart_fifo.o(i.nrf_drv_uart_rx) refers to nrfx_uarte.o(i.nrfx_uarte_rx) for nrfx_uarte_rx
    app_uart_fifo.o(i.nrf_drv_uart_rx) refers to nrfx_uart.o(i.nrfx_uart_rx) for nrfx_uart_rx
    app_uart_fifo.o(i.nrf_drv_uart_rx) refers to nrf_drv_uart.o(.data) for nrf_drv_uart_use_easy_dma
    app_uart_fifo.o(i.nrf_drv_uart_tx) refers to nrfx_uarte.o(i.nrfx_uarte_tx) for nrfx_uarte_tx
    app_uart_fifo.o(i.nrf_drv_uart_tx) refers to nrfx_uart.o(i.nrfx_uart_tx) for nrfx_uart_tx
    app_uart_fifo.o(i.nrf_drv_uart_tx) refers to nrf_drv_uart.o(.data) for nrf_drv_uart_use_easy_dma
    app_uart_fifo.o(i.uart_event_handler) refers to app_fifo.o(i.app_fifo_put) for app_fifo_put
    app_uart_fifo.o(i.uart_event_handler) refers to app_uart_fifo.o(i.fifo_length) for fifo_length
    app_uart_fifo.o(i.uart_event_handler) refers to app_uart_fifo.o(i.nrf_drv_uart_rx) for nrf_drv_uart_rx
    app_uart_fifo.o(i.uart_event_handler) refers to app_fifo.o(i.app_fifo_get) for app_fifo_get
    app_uart_fifo.o(i.uart_event_handler) refers to app_uart_fifo.o(i.nrf_drv_uart_tx) for nrf_drv_uart_tx
    app_uart_fifo.o(i.uart_event_handler) refers to app_uart_fifo.o(.bss) for m_rx_fifo
    app_uart_fifo.o(i.uart_event_handler) refers to app_uart_fifo.o(.data) for m_event_handler
    app_util_platform.o(i.app_util_critical_region_enter) refers to app_util_platform.o(i.app_util_disable_irq) for app_util_disable_irq
    app_util_platform.o(i.app_util_critical_region_exit) refers to app_util_platform.o(i.app_util_enable_irq) for app_util_enable_irq
    app_util_platform.o(i.app_util_disable_irq) refers to app_util_platform.o(.data) for m_in_critical_region
    app_util_platform.o(i.app_util_enable_irq) refers to app_util_platform.o(.data) for m_in_critical_region
    nrf_assert.o(i.assert_nrf_callback) refers to app_error_weak.o(i.app_error_fault_handler) for app_error_fault_handler
    nrf_atomic.o(i.nrf_atomic_flag_clear) refers to nrf_atomic.o(i.nrf_atomic_u32_and) for nrf_atomic_u32_and
    nrf_atomic.o(i.nrf_atomic_flag_clear_fetch) refers to nrf_atomic.o(i.nrf_atomic_u32_fetch_and) for nrf_atomic_u32_fetch_and
    nrf_atomic.o(i.nrf_atomic_flag_set) refers to nrf_atomic.o(i.nrf_atomic_u32_or) for nrf_atomic_u32_or
    nrf_atomic.o(i.nrf_atomic_flag_set_fetch) refers to nrf_atomic.o(i.nrf_atomic_u32_fetch_or) for nrf_atomic_u32_fetch_or
    nrf_atomic.o(i.nrf_atomic_u32_add) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_add
    nrf_atomic.o(i.nrf_atomic_u32_and) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_and
    nrf_atomic.o(i.nrf_atomic_u32_cmp_exch) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_cmp_exch
    nrf_atomic.o(i.nrf_atomic_u32_fetch_add) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_add
    nrf_atomic.o(i.nrf_atomic_u32_fetch_and) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_and
    nrf_atomic.o(i.nrf_atomic_u32_fetch_or) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_orr
    nrf_atomic.o(i.nrf_atomic_u32_fetch_store) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_mov
    nrf_atomic.o(i.nrf_atomic_u32_fetch_sub) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_sub
    nrf_atomic.o(i.nrf_atomic_u32_fetch_sub_hs) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_sub_hs
    nrf_atomic.o(i.nrf_atomic_u32_fetch_xor) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_eor
    nrf_atomic.o(i.nrf_atomic_u32_or) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_orr
    nrf_atomic.o(i.nrf_atomic_u32_store) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_mov
    nrf_atomic.o(i.nrf_atomic_u32_sub) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_sub
    nrf_atomic.o(i.nrf_atomic_u32_sub_hs) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_sub_hs
    nrf_atomic.o(i.nrf_atomic_u32_xor) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_eor
    nrf_balloc.o(i.nrf_balloc_alloc) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_balloc.o(i.nrf_balloc_alloc) refers to nrf_balloc.o(i.nrf_balloc_idx2block) for nrf_balloc_idx2block
    nrf_balloc.o(i.nrf_balloc_alloc) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_balloc.o(i.nrf_balloc_free) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_balloc.o(i.nrf_balloc_free) refers to nrf_balloc.o(i.nrf_balloc_block2idx) for nrf_balloc_block2idx
    nrf_balloc.o(i.nrf_balloc_free) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_fprintf.o(i.nrf_fprintf) refers to nrf_fprintf_format.o(i.nrf_fprintf_fmt) for nrf_fprintf_fmt
    nrf_fprintf_format.o(i.buffer_add) refers to nrf_fprintf.o(i.nrf_fprintf_buffer_flush) for nrf_fprintf_buffer_flush
    nrf_fprintf_format.o(i.int_print) refers to nrf_fprintf_format.o(i.buffer_add) for buffer_add
    nrf_fprintf_format.o(i.int_print) refers to nrf_fprintf_format.o(i.unsigned_print) for unsigned_print
    nrf_fprintf_format.o(i.nrf_fprintf_fmt) refers to nrf_fprintf_format.o(i.buffer_add) for buffer_add
    nrf_fprintf_format.o(i.nrf_fprintf_fmt) refers to nrf_fprintf_format.o(i.int_print) for int_print
    nrf_fprintf_format.o(i.nrf_fprintf_fmt) refers to nrf_fprintf_format.o(i.unsigned_print) for unsigned_print
    nrf_fprintf_format.o(i.nrf_fprintf_fmt) refers to nrf_fprintf_format.o(i.string_print) for string_print
    nrf_fprintf_format.o(i.nrf_fprintf_fmt) refers to nrf_fprintf.o(i.nrf_fprintf_buffer_flush) for nrf_fprintf_buffer_flush
    nrf_fprintf_format.o(i.string_print) refers to nrf_fprintf_format.o(i.buffer_add) for buffer_add
    nrf_fprintf_format.o(i.string_print) refers to strlen.o(.text) for strlen
    nrf_fprintf_format.o(i.unsigned_print) refers to nrf_fprintf_format.o(i.buffer_add) for buffer_add
    nrf_fprintf_format.o(i.unsigned_print) refers to nrf_fprintf_format.o(.constdata) for _aV2C
    nrf_memobj.o(i.memobj_op) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_memobj.o(i.nrf_memobj_alloc) refers to nrf_balloc.o(i.nrf_balloc_alloc) for nrf_balloc_alloc
    nrf_memobj.o(i.nrf_memobj_alloc) refers to nrf_memobj.o(i.nrf_memobj_free) for nrf_memobj_free
    nrf_memobj.o(i.nrf_memobj_free) refers to nrf_balloc.o(i.nrf_balloc_free) for nrf_balloc_free
    nrf_memobj.o(i.nrf_memobj_get) refers to nrf_atomic.o(i.nrf_atomic_u32_add) for nrf_atomic_u32_add
    nrf_memobj.o(i.nrf_memobj_pool_init) refers to nrf_balloc.o(i.nrf_balloc_init) for nrf_balloc_init
    nrf_memobj.o(i.nrf_memobj_put) refers to nrf_atomic.o(i.nrf_atomic_u32_sub) for nrf_atomic_u32_sub
    nrf_memobj.o(i.nrf_memobj_put) refers to nrf_memobj.o(i.nrf_memobj_free) for nrf_memobj_free
    nrf_memobj.o(i.nrf_memobj_read) refers to nrf_memobj.o(i.memobj_op) for memobj_op
    nrf_memobj.o(i.nrf_memobj_write) refers to nrf_memobj.o(i.memobj_op) for memobj_op
    nrf_ringbuf.o(i.nrf_ringbuf_alloc) refers to nrf_atomic.o(i.nrf_atomic_flag_set_fetch) for nrf_atomic_flag_set_fetch
    nrf_ringbuf.o(i.nrf_ringbuf_alloc) refers to nrf_atomic.o(i.nrf_atomic_flag_clear) for nrf_atomic_flag_clear
    nrf_ringbuf.o(i.nrf_ringbuf_cpy_get) refers to nrf_atomic.o(i.nrf_atomic_flag_set_fetch) for nrf_atomic_flag_set_fetch
    nrf_ringbuf.o(i.nrf_ringbuf_cpy_get) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_ringbuf.o(i.nrf_ringbuf_cpy_get) refers to nrf_atomic.o(i.nrf_atomic_flag_clear) for nrf_atomic_flag_clear
    nrf_ringbuf.o(i.nrf_ringbuf_cpy_put) refers to nrf_atomic.o(i.nrf_atomic_flag_set_fetch) for nrf_atomic_flag_set_fetch
    nrf_ringbuf.o(i.nrf_ringbuf_cpy_put) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_ringbuf.o(i.nrf_ringbuf_cpy_put) refers to nrf_atomic.o(i.nrf_atomic_flag_clear) for nrf_atomic_flag_clear
    nrf_ringbuf.o(i.nrf_ringbuf_free) refers to nrf_atomic.o(i.nrf_atomic_flag_clear) for nrf_atomic_flag_clear
    nrf_ringbuf.o(i.nrf_ringbuf_get) refers to nrf_atomic.o(i.nrf_atomic_flag_set_fetch) for nrf_atomic_flag_set_fetch
    nrf_ringbuf.o(i.nrf_ringbuf_get) refers to nrf_atomic.o(i.nrf_atomic_flag_clear) for nrf_atomic_flag_clear
    nrf_ringbuf.o(i.nrf_ringbuf_put) refers to nrf_atomic.o(i.nrf_atomic_flag_clear_fetch) for nrf_atomic_flag_clear_fetch
    nrf_strerror.o(i.nrf_strerror_find) refers to nrf_strerror.o(.constdata) for nrf_strerror_array
    nrf_strerror.o(i.nrf_strerror_get) refers to nrf_strerror.o(i.nrf_strerror_find) for nrf_strerror_find
    nrf_strerror.o(i.nrf_strerror_get) refers to nrf_strerror.o(.constdata) for m_unknown_str
    nrf_strerror.o(.constdata) refers to nrf_strerror.o(.conststring) for .conststring
    app_timer.o(i.RTC1_IRQHandler) refers to app_timer.o(i.timer_timeouts_check) for timer_timeouts_check
    app_timer.o(i.SWI1_EGU1_IRQHandler) refers to app_timer.o(i.timer_list_handler) for timer_list_handler
    app_timer.o(i.app_timer_cnt_diff_compute) refers to app_timer.o(i.ticks_diff_get) for ticks_diff_get
    app_timer.o(i.app_timer_cnt_get) refers to app_timer.o(i.rtc1_counter_get) for rtc1_counter_get
    app_timer.o(i.app_timer_create) refers to app_timer.o(.bss) for m_op_queue
    app_timer.o(i.app_timer_init) refers to app_timer.o(i.rtc1_stop) for rtc1_stop
    app_timer.o(i.app_timer_init) refers to app_timer.o(i.NVIC_ClearPendingIRQ) for NVIC_ClearPendingIRQ
    app_timer.o(i.app_timer_init) refers to app_timer.o(i.NVIC_SetPriority) for NVIC_SetPriority
    app_timer.o(i.app_timer_init) refers to app_timer.o(i.NVIC_EnableIRQ) for NVIC_EnableIRQ
    app_timer.o(i.app_timer_init) refers to app_timer.o(i.rtc1_init) for rtc1_init
    app_timer.o(i.app_timer_init) refers to app_timer.o(i.rtc1_counter_get) for rtc1_counter_get
    app_timer.o(i.app_timer_init) refers to app_timer.o(.bss) for m_op_queue
    app_timer.o(i.app_timer_init) refers to app_timer.o(.data) for mp_timer_id_head
    app_timer.o(i.app_timer_start) refers to app_timer.o(i.timer_start_op_schedule) for timer_start_op_schedule
    app_timer.o(i.app_timer_start) refers to app_timer.o(.bss) for m_op_queue
    app_timer.o(i.app_timer_stop) refers to app_timer.o(i.timer_stop_op_schedule) for timer_stop_op_schedule
    app_timer.o(i.app_timer_stop) refers to app_timer.o(.bss) for m_op_queue
    app_timer.o(i.app_timer_stop_all) refers to app_timer.o(i.timer_stop_op_schedule) for timer_stop_op_schedule
    app_timer.o(i.app_timer_stop_all) refers to app_timer.o(.bss) for m_op_queue
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.rtc1_counter_get) for rtc1_counter_get
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.ticks_diff_get) for ticks_diff_get
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.rtc1_start) for rtc1_start
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.rtc1_compare0_set) for rtc1_compare0_set
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.nrfx_coredep_delay_us) for nrfx_coredep_delay_us
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.timer_timeouts_check_sched) for timer_timeouts_check_sched
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.rtc1_stop) for rtc1_stop
    app_timer.o(i.compare_reg_update) refers to app_timer.o(.data) for mp_timer_id_head
    app_timer.o(i.elapsed_ticks_acquire) refers to app_timer.o(.data) for m_ticks_elapsed_q_read_ind
    app_timer.o(i.expired_timers_handler) refers to app_timer.o(.data) for mp_timer_id_head
    app_timer.o(i.list_insertions_handler) refers to app_timer.o(i.timer_list_remove) for timer_list_remove
    app_timer.o(i.list_insertions_handler) refers to app_timer.o(i.ticks_diff_get) for ticks_diff_get
    app_timer.o(i.list_insertions_handler) refers to app_timer.o(i.timer_list_insert) for timer_list_insert
    app_timer.o(i.list_insertions_handler) refers to app_timer.o(.data) for mp_timer_id_head
    app_timer.o(i.list_insertions_handler) refers to app_timer.o(.bss) for m_op_queue
    app_timer.o(i.nrfx_coredep_delay_us) refers to app_timer.o(.constdata) for delay_bytecode
    app_timer.o(i.rtc1_init) refers to app_timer.o(i.NVIC_SetPriority) for NVIC_SetPriority
    app_timer.o(i.rtc1_start) refers to app_timer.o(i.NVIC_ClearPendingIRQ) for NVIC_ClearPendingIRQ
    app_timer.o(i.rtc1_start) refers to app_timer.o(i.NVIC_EnableIRQ) for NVIC_EnableIRQ
    app_timer.o(i.rtc1_start) refers to app_timer.o(i.nrfx_coredep_delay_us) for nrfx_coredep_delay_us
    app_timer.o(i.rtc1_start) refers to app_timer.o(.data) for m_rtc1_running
    app_timer.o(i.rtc1_stop) refers to app_timer.o(i.nrfx_coredep_delay_us) for nrfx_coredep_delay_us
    app_timer.o(i.rtc1_stop) refers to app_timer.o(.data) for m_ticks_latest
    app_timer.o(i.timer_list_handler) refers to app_timer.o(i.elapsed_ticks_acquire) for elapsed_ticks_acquire
    app_timer.o(i.timer_list_handler) refers to app_timer.o(i.expired_timers_handler) for expired_timers_handler
    app_timer.o(i.timer_list_handler) refers to app_timer.o(i.list_insertions_handler) for list_insertions_handler
    app_timer.o(i.timer_list_handler) refers to app_timer.o(i.compare_reg_update) for compare_reg_update
    app_timer.o(i.timer_list_handler) refers to app_timer.o(.data) for m_ticks_latest
    app_timer.o(i.timer_list_handler_sched) refers to app_timer.o(i.NVIC_SetPendingIRQ) for NVIC_SetPendingIRQ
    app_timer.o(i.timer_list_insert) refers to app_timer.o(.data) for mp_timer_id_head
    app_timer.o(i.timer_list_remove) refers to app_timer.o(i.nrfx_coredep_delay_us) for nrfx_coredep_delay_us
    app_timer.o(i.timer_list_remove) refers to app_timer.o(.data) for mp_timer_id_head
    app_timer.o(i.timer_start_op_schedule) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    app_timer.o(i.timer_start_op_schedule) refers to app_timer.o(i.user_op_alloc) for user_op_alloc
    app_timer.o(i.timer_start_op_schedule) refers to app_timer.o(i.rtc1_counter_get) for rtc1_counter_get
    app_timer.o(i.timer_start_op_schedule) refers to app_timer.o(i.user_op_enque) for user_op_enque
    app_timer.o(i.timer_start_op_schedule) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    app_timer.o(i.timer_start_op_schedule) refers to app_timer.o(i.timer_list_handler_sched) for timer_list_handler_sched
    app_timer.o(i.timer_stop_op_schedule) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    app_timer.o(i.timer_stop_op_schedule) refers to app_timer.o(i.user_op_alloc) for user_op_alloc
    app_timer.o(i.timer_stop_op_schedule) refers to app_timer.o(i.user_op_enque) for user_op_enque
    app_timer.o(i.timer_stop_op_schedule) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    app_timer.o(i.timer_stop_op_schedule) refers to app_timer.o(i.timer_list_handler_sched) for timer_list_handler_sched
    app_timer.o(i.timer_timeouts_check) refers to app_timer.o(i.rtc1_counter_get) for rtc1_counter_get
    app_timer.o(i.timer_timeouts_check) refers to app_timer.o(i.ticks_diff_get) for ticks_diff_get
    app_timer.o(i.timer_timeouts_check) refers to app_timer.o(i.timeout_handler_exec) for timeout_handler_exec
    app_timer.o(i.timer_timeouts_check) refers to app_timer.o(i.timer_list_handler_sched) for timer_list_handler_sched
    app_timer.o(i.timer_timeouts_check) refers to app_timer.o(.data) for mp_timer_id_head
    app_timer.o(i.timer_timeouts_check_sched) refers to app_timer.o(i.NVIC_SetPendingIRQ) for NVIC_SetPendingIRQ
    app_timer.o(i.user_op_alloc) refers to app_timer.o(.bss) for m_op_queue
    app_timer.o(i.user_op_enque) refers to app_timer.o(.bss) for m_op_queue
    retarget.o(i.fgetc) refers to app_uart_fifo.o(i.app_uart_get) for app_uart_get
    retarget.o(i.fputc) refers to app_uart_fifo.o(i.app_uart_put) for app_uart_put
    nrf_esb.o(i.RADIO_IRQHandler) refers to nrf_esb.o(.data) for on_radio_end
    nrf_esb.o(i.SWI0_EGU0_IRQHandler) refers to nrf_esb.o(i.nrf_esb_get_clear_interrupts) for nrf_esb_get_clear_interrupts
    nrf_esb.o(i.SWI0_EGU0_IRQHandler) refers to nrf_esb.o(.data) for m_last_tx_attempts
    nrf_esb.o(i.TIMER3_IRQHandler) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.addr_conv) refers to nrf_esb.o(i.bytewise_bit_swap) for bytewise_bit_swap
    nrf_esb.o(i.apply_address_workarounds) refers to nrf_esb.o(.data) for m_esb_addr
    nrf_esb.o(i.clear_events_restart_rx) refers to nrf_esb.o(.data) for m_radio_shorts_common
    nrf_esb.o(i.clear_events_restart_rx) refers to nrf_esb.o(.bss) for m_config_local
    nrf_esb.o(i.initialize_fifos) refers to nrf_esb.o(i.reset_fifos) for reset_fifos
    nrf_esb.o(i.initialize_fifos) refers to nrf_esb.o(.bss) for m_tx_fifo_payload
    nrf_esb.o(i.nrf_esb_disable) refers to nrf_esb.o(i.reset_fifos) for reset_fifos
    nrf_esb.o(i.nrf_esb_disable) refers to memseta.o(.text) for __aeabi_memclr
    nrf_esb.o(i.nrf_esb_disable) refers to nrf_esb.o(i.NVIC_DisableIRQ) for NVIC_DisableIRQ
    nrf_esb.o(i.nrf_esb_disable) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_disable) refers to nrf_esb.o(.bss) for m_rx_pipe_info
    nrf_esb.o(i.nrf_esb_enable_pipes) refers to nrf_esb.o(i.apply_address_workarounds) for apply_address_workarounds
    nrf_esb.o(i.nrf_esb_enable_pipes) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_flush_rx) refers to nrf_esb.o(i.NVIC_DisableIRQ) for NVIC_DisableIRQ
    nrf_esb.o(i.nrf_esb_flush_rx) refers to memseta.o(.text) for __aeabi_memclr
    nrf_esb.o(i.nrf_esb_flush_rx) refers to nrf_esb.o(i.NVIC_EnableIRQ) for NVIC_EnableIRQ
    nrf_esb.o(i.nrf_esb_flush_rx) refers to nrf_esb.o(.data) for m_esb_initialized
    nrf_esb.o(i.nrf_esb_flush_rx) refers to nrf_esb.o(.bss) for m_rx_fifo
    nrf_esb.o(i.nrf_esb_flush_tx) refers to nrf_esb.o(i.NVIC_DisableIRQ) for NVIC_DisableIRQ
    nrf_esb.o(i.nrf_esb_flush_tx) refers to nrf_esb.o(i.NVIC_EnableIRQ) for NVIC_EnableIRQ
    nrf_esb.o(i.nrf_esb_flush_tx) refers to nrf_esb.o(.data) for m_esb_initialized
    nrf_esb.o(i.nrf_esb_flush_tx) refers to nrf_esb.o(.bss) for m_tx_fifo
    nrf_esb.o(i.nrf_esb_get_clear_interrupts) refers to nrf_esb.o(i.NVIC_DisableIRQ) for NVIC_DisableIRQ
    nrf_esb.o(i.nrf_esb_get_clear_interrupts) refers to nrf_esb.o(i.NVIC_EnableIRQ) for NVIC_EnableIRQ
    nrf_esb.o(i.nrf_esb_get_clear_interrupts) refers to nrf_esb.o(.data) for m_esb_initialized
    nrf_esb.o(i.nrf_esb_get_rf_channel) refers to nrf_esb.o(.data) for m_esb_addr
    nrf_esb.o(i.nrf_esb_init) refers to nrf_esb.o(i.nrf_esb_disable) for nrf_esb_disable
    nrf_esb.o(i.nrf_esb_init) refers to memcpya.o(.text) for __aeabi_memcpy4
    nrf_esb.o(i.nrf_esb_init) refers to memseta.o(.text) for __aeabi_memclr
    nrf_esb.o(i.nrf_esb_init) refers to nrf_esb.o(i.update_radio_parameters) for update_radio_parameters
    nrf_esb.o(i.nrf_esb_init) refers to nrf_esb.o(i.initialize_fifos) for initialize_fifos
    nrf_esb.o(i.nrf_esb_init) refers to nrf_esb.o(i.sys_timer_init) for sys_timer_init
    nrf_esb.o(i.nrf_esb_init) refers to nrf_esb.o(i.ppi_init) for ppi_init
    nrf_esb.o(i.nrf_esb_init) refers to nrf_esb.o(i.NVIC_SetPriority) for NVIC_SetPriority
    nrf_esb.o(i.nrf_esb_init) refers to nrf_esb.o(i.NVIC_EnableIRQ) for NVIC_EnableIRQ
    nrf_esb.o(i.nrf_esb_init) refers to nrf_esb.o(.data) for m_esb_initialized
    nrf_esb.o(i.nrf_esb_init) refers to nrf_esb.o(.bss) for m_config_local
    nrf_esb.o(i.nrf_esb_is_idle) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_pop_tx) refers to nrf_esb.o(i.NVIC_DisableIRQ) for NVIC_DisableIRQ
    nrf_esb.o(i.nrf_esb_pop_tx) refers to nrf_esb.o(i.NVIC_EnableIRQ) for NVIC_EnableIRQ
    nrf_esb.o(i.nrf_esb_pop_tx) refers to nrf_esb.o(.data) for m_esb_initialized
    nrf_esb.o(i.nrf_esb_pop_tx) refers to nrf_esb.o(.bss) for m_tx_fifo
    nrf_esb.o(i.nrf_esb_read_rx_payload) refers to nrf_esb.o(i.NVIC_DisableIRQ) for NVIC_DisableIRQ
    nrf_esb.o(i.nrf_esb_read_rx_payload) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_esb.o(i.nrf_esb_read_rx_payload) refers to nrf_esb.o(i.NVIC_EnableIRQ) for NVIC_EnableIRQ
    nrf_esb.o(i.nrf_esb_read_rx_payload) refers to nrf_esb.o(.data) for m_esb_initialized
    nrf_esb.o(i.nrf_esb_read_rx_payload) refers to nrf_esb.o(.bss) for m_rx_fifo
    nrf_esb.o(i.nrf_esb_reuse_pid) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_set_address_length) refers to nrf_esb.o(i.apply_address_workarounds) for apply_address_workarounds
    nrf_esb.o(i.nrf_esb_set_address_length) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_set_address_length) refers to nrf_esb.o(.bss) for m_config_local
    nrf_esb.o(i.nrf_esb_set_base_address_0) refers to nrf_esb.o(i.addr_conv) for addr_conv
    nrf_esb.o(i.nrf_esb_set_base_address_0) refers to nrf_esb.o(i.update_radio_addresses) for update_radio_addresses
    nrf_esb.o(i.nrf_esb_set_base_address_0) refers to nrf_esb.o(i.apply_address_workarounds) for apply_address_workarounds
    nrf_esb.o(i.nrf_esb_set_base_address_0) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_set_base_address_1) refers to nrf_esb.o(i.addr_conv) for addr_conv
    nrf_esb.o(i.nrf_esb_set_base_address_1) refers to nrf_esb.o(i.update_radio_addresses) for update_radio_addresses
    nrf_esb.o(i.nrf_esb_set_base_address_1) refers to nrf_esb.o(i.apply_address_workarounds) for apply_address_workarounds
    nrf_esb.o(i.nrf_esb_set_base_address_1) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_set_bitrate) refers to nrf_esb.o(i.update_radio_bitrate) for update_radio_bitrate
    nrf_esb.o(i.nrf_esb_set_bitrate) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_set_bitrate) refers to nrf_esb.o(.bss) for m_config_local
    nrf_esb.o(i.nrf_esb_set_prefixes) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_esb.o(i.nrf_esb_set_prefixes) refers to nrf_esb.o(i.update_radio_addresses) for update_radio_addresses
    nrf_esb.o(i.nrf_esb_set_prefixes) refers to nrf_esb.o(i.apply_address_workarounds) for apply_address_workarounds
    nrf_esb.o(i.nrf_esb_set_prefixes) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_set_retransmit_count) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_set_retransmit_count) refers to nrf_esb.o(.bss) for m_config_local
    nrf_esb.o(i.nrf_esb_set_retransmit_delay) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_set_retransmit_delay) refers to nrf_esb.o(.bss) for m_config_local
    nrf_esb.o(i.nrf_esb_set_rf_channel) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_set_tx_power) refers to nrf_esb.o(i.update_radio_tx_power) for update_radio_tx_power
    nrf_esb.o(i.nrf_esb_set_tx_power) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_set_tx_power) refers to nrf_esb.o(.bss) for m_config_local
    nrf_esb.o(i.nrf_esb_skip_tx) refers to nrf_esb.o(i.NVIC_DisableIRQ) for NVIC_DisableIRQ
    nrf_esb.o(i.nrf_esb_skip_tx) refers to nrf_esb.o(i.NVIC_EnableIRQ) for NVIC_EnableIRQ
    nrf_esb.o(i.nrf_esb_skip_tx) refers to nrf_esb.o(.data) for m_esb_initialized
    nrf_esb.o(i.nrf_esb_skip_tx) refers to nrf_esb.o(.bss) for m_tx_fifo
    nrf_esb.o(i.nrf_esb_start_rx) refers to nrf_esb.o(i.NVIC_ClearPendingIRQ) for NVIC_ClearPendingIRQ
    nrf_esb.o(i.nrf_esb_start_rx) refers to nrf_esb.o(i.NVIC_EnableIRQ) for NVIC_EnableIRQ
    nrf_esb.o(i.nrf_esb_start_rx) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_start_rx) refers to nrf_esb.o(i.on_radio_disabled_rx) for on_radio_disabled_rx
    nrf_esb.o(i.nrf_esb_start_rx) refers to nrf_esb.o(.bss) for m_rx_payload_buffer
    nrf_esb.o(i.nrf_esb_start_tx) refers to nrf_esb.o(i.start_tx_transaction) for start_tx_transaction
    nrf_esb.o(i.nrf_esb_start_tx) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_start_tx) refers to nrf_esb.o(.bss) for m_tx_fifo
    nrf_esb.o(i.nrf_esb_stop_rx) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_suspend) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_update_prefix) refers to nrf_esb.o(i.update_radio_addresses) for update_radio_addresses
    nrf_esb.o(i.nrf_esb_update_prefix) refers to nrf_esb.o(i.apply_address_workarounds) for apply_address_workarounds
    nrf_esb.o(i.nrf_esb_update_prefix) refers to nrf_esb.o(.data) for m_nrf_esb_mainstate
    nrf_esb.o(i.nrf_esb_write_payload) refers to nrf_esb.o(i.NVIC_DisableIRQ) for NVIC_DisableIRQ
    nrf_esb.o(i.nrf_esb_write_payload) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_esb.o(i.nrf_esb_write_payload) refers to nrf_esb.o(i.NVIC_EnableIRQ) for NVIC_EnableIRQ
    nrf_esb.o(i.nrf_esb_write_payload) refers to nrf_esb.o(i.start_tx_transaction) for start_tx_transaction
    nrf_esb.o(i.nrf_esb_write_payload) refers to nrf_esb.o(.data) for m_esb_initialized
    nrf_esb.o(i.nrf_esb_write_payload) refers to nrf_esb.o(.bss) for m_config_local
    nrf_esb.o(i.on_radio_disabled_rx) refers to nrf_esb.o(i.clear_events_restart_rx) for clear_events_restart_rx
    nrf_esb.o(i.on_radio_disabled_rx) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_esb.o(i.on_radio_disabled_rx) refers to nrf_esb.o(i.rx_fifo_push_rfbuf) for rx_fifo_push_rfbuf
    nrf_esb.o(i.on_radio_disabled_rx) refers to nrf_esb.o(i.NVIC_SetPendingIRQ) for NVIC_SetPendingIRQ
    nrf_esb.o(i.on_radio_disabled_rx) refers to nrf_esb.o(.bss) for m_rx_fifo
    nrf_esb.o(i.on_radio_disabled_rx) refers to nrf_esb.o(.data) for m_radio_shorts_common
    nrf_esb.o(i.on_radio_disabled_rx) refers to nrf_esb.o(i.on_radio_disabled_rx_ack) for on_radio_disabled_rx_ack
    nrf_esb.o(i.on_radio_disabled_rx_ack) refers to nrf_esb.o(.data) for m_radio_shorts_common
    nrf_esb.o(i.on_radio_disabled_rx_ack) refers to nrf_esb.o(.bss) for m_config_local
    nrf_esb.o(i.on_radio_disabled_rx_ack) refers to nrf_esb.o(i.on_radio_disabled_rx) for on_radio_disabled_rx
    nrf_esb.o(i.on_radio_disabled_tx) refers to nrf_esb.o(.data) for m_radio_shorts_common
    nrf_esb.o(i.on_radio_disabled_tx) refers to nrf_esb.o(.bss) for m_config_local
    nrf_esb.o(i.on_radio_disabled_tx) refers to nrf_esb.o(i.on_radio_disabled_tx_wait_for_ack) for on_radio_disabled_tx_wait_for_ack
    nrf_esb.o(i.on_radio_disabled_tx_noack) refers to nrf_esb.o(i.nrf_esb_skip_tx) for nrf_esb_skip_tx
    nrf_esb.o(i.on_radio_disabled_tx_noack) refers to nrf_esb.o(i.NVIC_SetPendingIRQ) for NVIC_SetPendingIRQ
    nrf_esb.o(i.on_radio_disabled_tx_noack) refers to nrf_esb.o(i.start_tx_transaction) for start_tx_transaction
    nrf_esb.o(i.on_radio_disabled_tx_noack) refers to nrf_esb.o(.data) for m_interrupt_flags
    nrf_esb.o(i.on_radio_disabled_tx_noack) refers to nrf_esb.o(.bss) for m_tx_fifo
    nrf_esb.o(i.on_radio_disabled_tx_wait_for_ack) refers to nrf_esb.o(i.nrf_esb_skip_tx) for nrf_esb_skip_tx
    nrf_esb.o(i.on_radio_disabled_tx_wait_for_ack) refers to nrf_esb.o(i.rx_fifo_push_rfbuf) for rx_fifo_push_rfbuf
    nrf_esb.o(i.on_radio_disabled_tx_wait_for_ack) refers to nrf_esb.o(i.NVIC_SetPendingIRQ) for NVIC_SetPendingIRQ
    nrf_esb.o(i.on_radio_disabled_tx_wait_for_ack) refers to nrf_esb.o(i.start_tx_transaction) for start_tx_transaction
    nrf_esb.o(i.on_radio_disabled_tx_wait_for_ack) refers to nrf_esb.o(.data) for m_interrupt_flags
    nrf_esb.o(i.on_radio_disabled_tx_wait_for_ack) refers to nrf_esb.o(.bss) for m_config_local
    nrf_esb.o(i.on_radio_disabled_tx_wait_for_ack) refers to nrf_esb.o(i.on_radio_disabled_tx) for on_radio_disabled_tx
    nrf_esb.o(i.reset_fifos) refers to nrf_esb.o(.bss) for m_tx_fifo
    nrf_esb.o(i.rx_fifo_push_rfbuf) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_esb.o(i.rx_fifo_push_rfbuf) refers to nrf_esb.o(.bss) for m_rx_fifo
    nrf_esb.o(i.start_tx_transaction) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_esb.o(i.start_tx_transaction) refers to nrf_esb.o(i.NVIC_ClearPendingIRQ) for NVIC_ClearPendingIRQ
    nrf_esb.o(i.start_tx_transaction) refers to nrf_esb.o(i.NVIC_EnableIRQ) for NVIC_EnableIRQ
    nrf_esb.o(i.start_tx_transaction) refers to nrf_esb.o(.data) for m_last_tx_attempts
    nrf_esb.o(i.start_tx_transaction) refers to nrf_esb.o(.bss) for m_tx_fifo
    nrf_esb.o(i.start_tx_transaction) refers to nrf_esb.o(i.on_radio_disabled_tx) for on_radio_disabled_tx
    nrf_esb.o(i.start_tx_transaction) refers to nrf_esb.o(i.on_radio_disabled_tx_noack) for on_radio_disabled_tx_noack
    nrf_esb.o(i.update_radio_addresses) refers to nrf_esb.o(i.addr_conv) for addr_conv
    nrf_esb.o(i.update_radio_addresses) refers to nrf_esb.o(i.bytewise_bit_swap) for bytewise_bit_swap
    nrf_esb.o(i.update_radio_addresses) refers to nrf_esb.o(.data) for m_esb_addr
    nrf_esb.o(i.update_radio_bitrate) refers to nrf_esb.o(.bss) for m_config_local
    nrf_esb.o(i.update_radio_bitrate) refers to nrf_esb.o(.data) for m_wait_for_ack_timeout_us
    nrf_esb.o(i.update_radio_crc) refers to nrf_esb.o(.bss) for m_config_local
    nrf_esb.o(i.update_radio_parameters) refers to nrf_esb.o(i.update_radio_tx_power) for update_radio_tx_power
    nrf_esb.o(i.update_radio_parameters) refers to nrf_esb.o(i.update_radio_bitrate) for update_radio_bitrate
    nrf_esb.o(i.update_radio_parameters) refers to nrf_esb.o(i.update_radio_protocol) for update_radio_protocol
    nrf_esb.o(i.update_radio_parameters) refers to nrf_esb.o(i.update_radio_crc) for update_radio_crc
    nrf_esb.o(i.update_radio_parameters) refers to nrf_esb.o(.bss) for m_config_local
    nrf_esb.o(i.update_radio_parameters) refers to nrf_esb.o(.data) for update_rf_payload_format
    nrf_esb.o(i.update_radio_protocol) refers to nrf_esb.o(.bss) for m_config_local
    nrf_esb.o(i.update_radio_protocol) refers to nrf_esb.o(i.update_rf_payload_format_esb_dpl) for update_rf_payload_format_esb_dpl
    nrf_esb.o(i.update_radio_protocol) refers to nrf_esb.o(.data) for update_rf_payload_format
    nrf_esb.o(i.update_radio_protocol) refers to nrf_esb.o(i.update_rf_payload_format_esb) for update_rf_payload_format_esb
    nrf_esb.o(i.update_radio_tx_power) refers to nrf_esb.o(.bss) for m_config_local
    nrf_esb.o(i.update_rf_payload_format_esb) refers to nrf_esb.o(.data) for m_esb_addr
    nrf_esb.o(i.update_rf_payload_format_esb_dpl) refers to nrf_esb.o(.data) for m_esb_addr
    uartprocess.o(i.UART_Init) refers to memcpya.o(.text) for __aeabi_memcpy4
    uartprocess.o(i.UART_Init) refers to app_uart_fifo.o(i.app_uart_init) for app_uart_init
    uartprocess.o(i.UART_Init) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    uartprocess.o(i.UART_Init) refers to uartprocess.o(.constdata) for .constdata
    uartprocess.o(i.UART_Init) refers to uartprocess.o(.bss) for rx_buf
    uartprocess.o(i.UART_Init) refers to uartprocess.o(i.uart_event_handle) for uart_event_handle
    uartprocess.o(i.uart_event_handle) refers to app_uart_fifo.o(i.app_uart_get) for app_uart_get
    uartprocess.o(i.uart_event_handle) refers to memcmp.o(.text) for memcmp
    uartprocess.o(i.uart_event_handle) refers to printf5.o(i.__0printf$5) for __2printf
    uartprocess.o(i.uart_event_handle) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    uartprocess.o(i.uart_event_handle) refers to uartprocess.o(.bss) for data_array
    uartprocess.o(i.uart_event_handle) refers to uartprocess.o(.data) for index
    uartprocess.o(i.uart_event_handle) refers to uartprocess.o(.constdata) for delay_bytecode
    arm_startup_nrf52.o(RESET) refers to arm_startup_nrf52.o(STACK) for __initial_sp
    arm_startup_nrf52.o(RESET) refers to arm_startup_nrf52.o(.text) for Reset_Handler
    arm_startup_nrf52.o(RESET) refers to nrf_esb.o(i.RADIO_IRQHandler) for RADIO_IRQHandler
    arm_startup_nrf52.o(RESET) refers to nrfx_prs.o(i.UARTE0_UART0_IRQHandler) for UARTE0_UART0_IRQHandler
    arm_startup_nrf52.o(RESET) refers to nrfx_gpiote.o(i.GPIOTE_IRQHandler) for GPIOTE_IRQHandler
    arm_startup_nrf52.o(RESET) refers to app_timer.o(i.RTC1_IRQHandler) for RTC1_IRQHandler
    arm_startup_nrf52.o(RESET) refers to nrf_esb.o(i.SWI0_EGU0_IRQHandler) for SWI0_EGU0_IRQHandler
    arm_startup_nrf52.o(RESET) refers to app_timer.o(i.SWI1_EGU1_IRQHandler) for SWI1_EGU1_IRQHandler
    arm_startup_nrf52.o(RESET) refers to nrf_esb.o(i.TIMER3_IRQHandler) for TIMER3_IRQHandler
    arm_startup_nrf52.o(.text) refers to system_nrf52.o(i.SystemInit) for SystemInit
    arm_startup_nrf52.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    system_nrf52.o(i.SystemCoreClockUpdate) refers to system_nrf52.o(.data) for SystemCoreClock
    system_nrf52.o(i.SystemInit) refers to system_nrf52.o(i.errata_12) for errata_12
    system_nrf52.o(i.SystemInit) refers to system_nrf52.o(i.errata_16) for errata_16
    system_nrf52.o(i.SystemInit) refers to system_nrf52.o(i.errata_31) for errata_31
    system_nrf52.o(i.SystemInit) refers to system_nrf52.o(i.errata_32) for errata_32
    system_nrf52.o(i.SystemInit) refers to system_nrf52.o(i.errata_36) for errata_36
    system_nrf52.o(i.SystemInit) refers to system_nrf52.o(i.errata_37) for errata_37
    system_nrf52.o(i.SystemInit) refers to system_nrf52.o(i.errata_57) for errata_57
    system_nrf52.o(i.SystemInit) refers to system_nrf52.o(i.errata_66) for errata_66
    system_nrf52.o(i.SystemInit) refers to system_nrf52.o(i.errata_108) for errata_108
    system_nrf52.o(i.SystemInit) refers to system_nrf52.o(i.errata_136) for errata_136
    system_nrf52.o(i.SystemInit) refers to system_nrf52.o(i.errata_182) for errata_182
    system_nrf52.o(i.SystemInit) refers to system_nrf52.o(i.SystemCoreClockUpdate) for SystemCoreClockUpdate
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to retarget.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to retarget.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to retarget.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to retarget.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to retarget.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to retarget.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to retarget.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to retarget.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to retarget.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to retarget.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to retarget.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to retarget.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to retarget.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to retarget.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to retarget.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to retarget.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to retarget.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to retarget.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to retarget.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to retarget.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to retarget.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to retarget.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to retarget.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to retarget.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to retarget.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to retarget.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to retarget.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to retarget.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to retarget.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to retarget.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to retarget.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to retarget.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to retarget.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to retarget.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to retarget.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to retarget.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to retarget.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to retarget.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to retarget.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to retarget.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to retarget.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to retarget.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to retarget.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to retarget.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to retarget.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to retarget.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to retarget.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to retarget.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to retarget.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to retarget.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to retarget.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to retarget.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to retarget.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to retarget.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to retarget.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to retarget.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to retarget.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to retarget.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to retarget.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to retarget.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to retarget.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to retarget.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to retarget.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to retarget.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to retarget.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to retarget.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to arm_startup_nrf52.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to arm_startup_nrf52.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to host.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to host.o(i.main) for main
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr


==============================================================================

Removing Unused input sections from the image.

    Removing gpioprocess.o(.rev16_text), (4 bytes).
    Removing gpioprocess.o(.revsh_text), (4 bytes).
    Removing gpioprocess.o(.rrx_text), (6 bytes).
    Removing host.o(.rev16_text), (4 bytes).
    Removing host.o(.revsh_text), (4 bytes).
    Removing host.o(.rrx_text), (6 bytes).
    Removing esbprocess.o(.rev16_text), (4 bytes).
    Removing esbprocess.o(.revsh_text), (4 bytes).
    Removing esbprocess.o(.rrx_text), (6 bytes).
    Removing boards.o(.rev16_text), (4 bytes).
    Removing boards.o(.revsh_text), (4 bytes).
    Removing boards.o(.rrx_text), (6 bytes).
    Removing boards.o(i.bsp_board_button_idx_to_pin), (12 bytes).
    Removing boards.o(i.bsp_board_button_state_get), (48 bytes).
    Removing boards.o(i.bsp_board_buttons_init), (44 bytes).
    Removing boards.o(i.bsp_board_init), (26 bytes).
    Removing boards.o(i.bsp_board_led_idx_to_pin), (12 bytes).
    Removing boards.o(i.bsp_board_led_invert), (48 bytes).
    Removing boards.o(i.bsp_board_led_off), (20 bytes).
    Removing boards.o(i.bsp_board_led_on), (20 bytes).
    Removing boards.o(i.bsp_board_led_state_get), (48 bytes).
    Removing boards.o(i.bsp_board_leds_init), (48 bytes).
    Removing boards.o(i.bsp_board_leds_off), (20 bytes).
    Removing boards.o(i.bsp_board_leds_on), (20 bytes).
    Removing boards.o(i.bsp_board_pin_to_button_idx), (36 bytes).
    Removing boards.o(i.bsp_board_pin_to_led_idx), (36 bytes).
    Removing boards.o(i.nrf_gpio_cfg), (40 bytes).
    Removing boards.o(i.nrf_gpio_pin_write), (58 bytes).
    Removing boards.o(.constdata), (8 bytes).
    Removing nrf_drv_uart.o(.rev16_text), (4 bytes).
    Removing nrf_drv_uart.o(.revsh_text), (4 bytes).
    Removing nrf_drv_uart.o(.rrx_text), (6 bytes).
    Removing nrfx_prs.o(.rev16_text), (4 bytes).
    Removing nrfx_prs.o(.revsh_text), (4 bytes).
    Removing nrfx_prs.o(.rrx_text), (6 bytes).
    Removing nrfx_prs.o(i.nrfx_prs_release), (22 bytes).
    Removing nrfx_prs.o(.constdata), (17 bytes).
    Removing nrfx_uart.o(.rev16_text), (4 bytes).
    Removing nrfx_uart.o(.revsh_text), (4 bytes).
    Removing nrfx_uart.o(.rrx_text), (6 bytes).
    Removing nrfx_uart.o(i.interrupts_disable), (52 bytes).
    Removing nrfx_uart.o(i.nrf_gpio_cfg_default), (24 bytes).
    Removing nrfx_uart.o(i.nrfx_uart_errorsrc_get), (22 bytes).
    Removing nrfx_uart.o(i.nrfx_uart_rx_abort), (24 bytes).
    Removing nrfx_uart.o(i.nrfx_uart_rx_disable), (40 bytes).
    Removing nrfx_uart.o(i.nrfx_uart_rx_enable), (60 bytes).
    Removing nrfx_uart.o(i.nrfx_uart_rx_ready), (16 bytes).
    Removing nrfx_uart.o(i.nrfx_uart_tx_abort), (52 bytes).
    Removing nrfx_uart.o(i.nrfx_uart_uninit), (68 bytes).
    Removing nrfx_uart.o(i.pins_to_default), (120 bytes).
    Removing nrfx_uarte.o(.rev16_text), (4 bytes).
    Removing nrfx_uarte.o(.revsh_text), (4 bytes).
    Removing nrfx_uarte.o(.rrx_text), (6 bytes).
    Removing nrfx_uarte.o(i.interrupts_disable), (52 bytes).
    Removing nrfx_uarte.o(i.nrf_gpio_cfg_default), (24 bytes).
    Removing nrfx_uarte.o(i.nrfx_uarte_errorsrc_get), (22 bytes).
    Removing nrfx_uarte.o(i.nrfx_uarte_rx_abort), (14 bytes).
    Removing nrfx_uarte.o(i.nrfx_uarte_rx_ready), (16 bytes).
    Removing nrfx_uarte.o(i.nrfx_uarte_tx_abort), (60 bytes).
    Removing nrfx_uarte.o(i.nrfx_uarte_uninit), (64 bytes).
    Removing nrfx_uarte.o(i.pins_to_default), (126 bytes).
    Removing nrfx_gpiote.o(.rev16_text), (4 bytes).
    Removing nrfx_gpiote.o(.revsh_text), (4 bytes).
    Removing nrfx_gpiote.o(.rrx_text), (6 bytes).
    Removing nrfx_gpiote.o(i.nrf_gpio_cfg_default), (24 bytes).
    Removing nrfx_gpiote.o(i.nrf_gpio_pin_clear), (22 bytes).
    Removing nrfx_gpiote.o(i.nrf_gpio_pin_set), (22 bytes).
    Removing nrfx_gpiote.o(i.nrf_gpiote_task_addr_get), (12 bytes).
    Removing nrfx_gpiote.o(i.nrf_gpiote_te_default), (16 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_clr_task_addr_get), (24 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_clr_task_trigger), (32 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_in_event_addr_get), (38 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_in_event_disable), (84 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_in_is_set), (20 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_in_uninit), (72 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_is_init), (20 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_clear), (12 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_init), (208 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_set), (12 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_task_addr_get), (22 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_task_disable), (36 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_task_enable), (44 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_task_force), (48 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_task_trigger), (32 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_toggle), (38 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_uninit), (66 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_set_task_addr_get), (24 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_set_task_trigger), (32 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_uninit), (68 bytes).
    Removing nrfx_gpiote.o(i.pin_configured_check), (28 bytes).
    Removing nrfx_gpiote.o(i.pin_configured_clear), (32 bytes).
    Removing app_error.o(.rev16_text), (4 bytes).
    Removing app_error.o(.revsh_text), (4 bytes).
    Removing app_error.o(.rrx_text), (6 bytes).
    Removing app_error.o(i.app_error_save_and_stop), (136 bytes).
    Removing app_error.o(.bss), (32 bytes).
    Removing app_error_handler_keil.o(.rev16_text), (4 bytes).
    Removing app_error_handler_keil.o(.revsh_text), (4 bytes).
    Removing app_error_handler_keil.o(.rrx_text), (6 bytes).
    Removing app_error_handler_keil.o(.emb_text), (26 bytes).
    Removing app_error_weak.o(.rev16_text), (4 bytes).
    Removing app_error_weak.o(.revsh_text), (4 bytes).
    Removing app_error_weak.o(.rrx_text), (6 bytes).
    Removing app_fifo.o(.rev16_text), (4 bytes).
    Removing app_fifo.o(.revsh_text), (4 bytes).
    Removing app_fifo.o(.rrx_text), (6 bytes).
    Removing app_fifo.o(i.app_fifo_flush), (10 bytes).
    Removing app_fifo.o(i.app_fifo_peek), (36 bytes).
    Removing app_fifo.o(i.app_fifo_read), (102 bytes).
    Removing app_fifo.o(i.app_fifo_write), (106 bytes).
    Removing app_uart_fifo.o(.rev16_text), (4 bytes).
    Removing app_uart_fifo.o(.revsh_text), (4 bytes).
    Removing app_uart_fifo.o(.rrx_text), (6 bytes).
    Removing app_uart_fifo.o(i.app_uart_close), (52 bytes).
    Removing app_uart_fifo.o(i.app_uart_flush), (52 bytes).
    Removing app_util_platform.o(.rev16_text), (4 bytes).
    Removing app_util_platform.o(.revsh_text), (4 bytes).
    Removing app_util_platform.o(.rrx_text), (6 bytes).
    Removing app_util_platform.o(i.current_int_priority_get), (60 bytes).
    Removing app_util_platform.o(i.privilege_level_get), (34 bytes).
    Removing nrf_assert.o(.rev16_text), (4 bytes).
    Removing nrf_assert.o(.revsh_text), (4 bytes).
    Removing nrf_assert.o(.rrx_text), (6 bytes).
    Removing nrf_assert.o(i.assert_nrf_callback), (26 bytes).
    Removing nrf_atomic.o(.rev16_text), (4 bytes).
    Removing nrf_atomic.o(.revsh_text), (4 bytes).
    Removing nrf_atomic.o(.rrx_text), (6 bytes).
    Removing nrf_atomic.o(.emb_text), (226 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_flag_clear), (14 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_flag_clear_fetch), (14 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_flag_set), (14 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_flag_set_fetch), (14 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_add), (22 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_and), (22 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_cmp_exch), (20 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_fetch_add), (22 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_fetch_and), (22 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_fetch_or), (22 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_fetch_store), (22 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_fetch_sub), (22 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_fetch_sub_hs), (22 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_fetch_xor), (22 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_or), (22 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_store), (22 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_sub), (22 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_sub_hs), (22 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_xor), (22 bytes).
    Removing nrf_balloc.o(.rev16_text), (4 bytes).
    Removing nrf_balloc.o(.revsh_text), (4 bytes).
    Removing nrf_balloc.o(.rrx_text), (6 bytes).
    Removing nrf_balloc.o(i.nrf_balloc_alloc), (76 bytes).
    Removing nrf_balloc.o(i.nrf_balloc_block2idx), (16 bytes).
    Removing nrf_balloc.o(i.nrf_balloc_free), (42 bytes).
    Removing nrf_balloc.o(i.nrf_balloc_idx2block), (12 bytes).
    Removing nrf_balloc.o(i.nrf_balloc_init), (60 bytes).
    Removing nrf_fprintf.o(.rev16_text), (4 bytes).
    Removing nrf_fprintf.o(.revsh_text), (4 bytes).
    Removing nrf_fprintf.o(.rrx_text), (6 bytes).
    Removing nrf_fprintf.o(i.nrf_fprintf), (42 bytes).
    Removing nrf_fprintf.o(i.nrf_fprintf_buffer_flush), (28 bytes).
    Removing nrf_fprintf_format.o(.rev16_text), (4 bytes).
    Removing nrf_fprintf_format.o(.revsh_text), (4 bytes).
    Removing nrf_fprintf_format.o(.rrx_text), (6 bytes).
    Removing nrf_fprintf_format.o(i.buffer_add), (32 bytes).
    Removing nrf_fprintf_format.o(i.int_print), (190 bytes).
    Removing nrf_fprintf_format.o(i.nrf_fprintf_fmt), (496 bytes).
    Removing nrf_fprintf_format.o(i.string_print), (116 bytes).
    Removing nrf_fprintf_format.o(i.unsigned_print), (184 bytes).
    Removing nrf_fprintf_format.o(.constdata), (16 bytes).
    Removing nrf_memobj.o(.rev16_text), (4 bytes).
    Removing nrf_memobj.o(.revsh_text), (4 bytes).
    Removing nrf_memobj.o(.rrx_text), (6 bytes).
    Removing nrf_memobj.o(i.memobj_op), (202 bytes).
    Removing nrf_memobj.o(i.nrf_memobj_alloc), (122 bytes).
    Removing nrf_memobj.o(i.nrf_memobj_free), (64 bytes).
    Removing nrf_memobj.o(i.nrf_memobj_get), (16 bytes).
    Removing nrf_memobj.o(i.nrf_memobj_pool_init), (12 bytes).
    Removing nrf_memobj.o(i.nrf_memobj_put), (30 bytes).
    Removing nrf_memobj.o(i.nrf_memobj_read), (34 bytes).
    Removing nrf_memobj.o(i.nrf_memobj_write), (34 bytes).
    Removing nrf_ringbuf.o(.rev16_text), (4 bytes).
    Removing nrf_ringbuf.o(.revsh_text), (4 bytes).
    Removing nrf_ringbuf.o(.rrx_text), (6 bytes).
    Removing nrf_ringbuf.o(i.nrf_ringbuf_alloc), (150 bytes).
    Removing nrf_ringbuf.o(i.nrf_ringbuf_cpy_get), (152 bytes).
    Removing nrf_ringbuf.o(i.nrf_ringbuf_cpy_put), (138 bytes).
    Removing nrf_ringbuf.o(i.nrf_ringbuf_free), (54 bytes).
    Removing nrf_ringbuf.o(i.nrf_ringbuf_get), (146 bytes).
    Removing nrf_ringbuf.o(i.nrf_ringbuf_init), (28 bytes).
    Removing nrf_ringbuf.o(i.nrf_ringbuf_put), (64 bytes).
    Removing nrf_strerror.o(.rev16_text), (4 bytes).
    Removing nrf_strerror.o(.revsh_text), (4 bytes).
    Removing nrf_strerror.o(.rrx_text), (6 bytes).
    Removing nrf_strerror.o(i.nrf_strerror_find), (64 bytes).
    Removing nrf_strerror.o(i.nrf_strerror_get), (28 bytes).
    Removing nrf_strerror.o(.constdata), (300 bytes).
    Removing nrf_strerror.o(.conststring), (957 bytes).
    Removing app_timer.o(.rev16_text), (4 bytes).
    Removing app_timer.o(.revsh_text), (4 bytes).
    Removing app_timer.o(.rrx_text), (6 bytes).
    Removing app_timer.o(i.app_timer_cnt_diff_compute), (16 bytes).
    Removing app_timer.o(i.app_timer_cnt_get), (8 bytes).
    Removing app_timer.o(i.app_timer_pause), (12 bytes).
    Removing app_timer.o(i.app_timer_resume), (12 bytes).
    Removing app_timer.o(i.app_timer_stop), (48 bytes).
    Removing app_timer.o(i.app_timer_stop_all), (32 bytes).
    Removing app_timer.o(i.timer_stop_op_schedule), (56 bytes).
    Removing retarget.o(.rev16_text), (4 bytes).
    Removing retarget.o(.revsh_text), (4 bytes).
    Removing retarget.o(.rrx_text), (6 bytes).
    Removing retarget.o(i.fgetc), (22 bytes).
    Removing nrf_log_frontend.o(.rev16_text), (4 bytes).
    Removing nrf_log_frontend.o(.revsh_text), (4 bytes).
    Removing nrf_log_frontend.o(.rrx_text), (6 bytes).
    Removing nrf_log_str_formatter.o(.rev16_text), (4 bytes).
    Removing nrf_log_str_formatter.o(.revsh_text), (4 bytes).
    Removing nrf_log_str_formatter.o(.rrx_text), (6 bytes).
    Removing nrf_esb.o(.rev16_text), (4 bytes).
    Removing nrf_esb.o(.revsh_text), (4 bytes).
    Removing nrf_esb.o(.rrx_text), (6 bytes).
    Removing nrf_esb.o(i.nrf_esb_enable_pipes), (52 bytes).
    Removing nrf_esb.o(i.nrf_esb_flush_rx), (64 bytes).
    Removing nrf_esb.o(i.nrf_esb_get_rf_channel), (28 bytes).
    Removing nrf_esb.o(i.nrf_esb_is_idle), (20 bytes).
    Removing nrf_esb.o(i.nrf_esb_pop_tx), (84 bytes).
    Removing nrf_esb.o(i.nrf_esb_reuse_pid), (64 bytes).
    Removing nrf_esb.o(i.nrf_esb_set_address_length), (248 bytes).
    Removing nrf_esb.o(i.nrf_esb_set_bitrate), (44 bytes).
    Removing nrf_esb.o(i.nrf_esb_set_retransmit_count), (32 bytes).
    Removing nrf_esb.o(i.nrf_esb_set_retransmit_delay), (44 bytes).
    Removing nrf_esb.o(i.nrf_esb_set_rf_channel), (44 bytes).
    Removing nrf_esb.o(i.nrf_esb_set_tx_power), (48 bytes).
    Removing nrf_esb.o(i.nrf_esb_suspend), (40 bytes).
    Removing nrf_esb.o(i.nrf_esb_update_prefix), (136 bytes).
    Removing uartprocess.o(.rev16_text), (4 bytes).
    Removing uartprocess.o(.revsh_text), (4 bytes).
    Removing uartprocess.o(.rrx_text), (6 bytes).
    Removing arm_startup_nrf52.o(HEAP), (8192 bytes).
    Removing system_nrf52.o(.rev16_text), (4 bytes).
    Removing system_nrf52.o(.revsh_text), (4 bytes).
    Removing system_nrf52.o(.rrx_text), (6 bytes).
    Removing dadd.o(.text), (334 bytes).
    Removing dmul.o(.text), (228 bytes).
    Removing ddiv.o(.text), (222 bytes).
    Removing dfixul.o(.text), (48 bytes).
    Removing cdrcmple.o(.text), (48 bytes).
    Removing depilogue.o(.text), (186 bytes).

247 unused section(s) (total 18546 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    RESET                                    0x00000000   Section      512  arm_startup_nrf52.o(RESET)
    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/string/memcmp.c         0x00000000   Number         0  memcmp.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/string/strlen.c         0x00000000   Number         0  strlen.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ..\..\..\..\..\..\components\boards\boards.c 0x00000000   Number         0  boards.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\atomic\nrf_atomic.c 0x00000000   Number         0  nrf_atomic.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\balloc\nrf_balloc.c 0x00000000   Number         0  nrf_balloc.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\fifo\app_fifo.c 0x00000000   Number         0  app_fifo.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\log\src\nrf_log_frontend.c 0x00000000   Number         0  nrf_log_frontend.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\log\src\nrf_log_str_formatter.c 0x00000000   Number         0  nrf_log_str_formatter.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\memobj\nrf_memobj.c 0x00000000   Number         0  nrf_memobj.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\ringbuf\nrf_ringbuf.c 0x00000000   Number         0  nrf_ringbuf.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\strerror\nrf_strerror.c 0x00000000   Number         0  nrf_strerror.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\timer\app_timer.c 0x00000000   Number         0  app_timer.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\uart\app_uart_fifo.c 0x00000000   Number         0  app_uart_fifo.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\uart\retarget.c 0x00000000   Number         0  retarget.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\util\app_error.c 0x00000000   Number         0  app_error.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\util\app_error_handler_keil.c 0x00000000   Number         0  app_error_handler_keil.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\util\app_error_weak.c 0x00000000   Number         0  app_error_weak.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\util\app_util_platform.c 0x00000000   Number         0  app_util_platform.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\util\nrf_assert.c 0x00000000   Number         0  nrf_assert.o ABSOLUTE
    ..\..\..\..\..\..\components\proprietary_rf\esb\nrf_esb.c 0x00000000   Number         0  nrf_esb.o ABSOLUTE
    ..\..\..\..\..\..\external\fprintf\nrf_fprintf.c 0x00000000   Number         0  nrf_fprintf.o ABSOLUTE
    ..\..\..\..\..\..\external\fprintf\nrf_fprintf_format.c 0x00000000   Number         0  nrf_fprintf_format.o ABSOLUTE
    ..\..\..\..\..\..\integration\nrfx\legacy\nrf_drv_uart.c 0x00000000   Number         0  nrf_drv_uart.o ABSOLUTE
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_gpiote.c 0x00000000   Number         0  nrfx_gpiote.o ABSOLUTE
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_uart.c 0x00000000   Number         0  nrfx_uart.o ABSOLUTE
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_uarte.c 0x00000000   Number         0  nrfx_uarte.o ABSOLUTE
    ..\..\..\..\..\..\modules\nrfx\drivers\src\prs\nrfx_prs.c 0x00000000   Number         0  nrfx_prs.o ABSOLUTE
    ..\..\..\Driver\EsbProcess.c             0x00000000   Number         0  esbprocess.o ABSOLUTE
    ..\..\..\Driver\GpioProcess.c            0x00000000   Number         0  gpioprocess.o ABSOLUTE
    ..\..\..\Driver\UartProcess.c            0x00000000   Number         0  uartprocess.o ABSOLUTE
    ..\..\..\Host.c                          0x00000000   Number         0  host.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\boards\\boards.c 0x00000000   Number         0  boards.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\atomic\\nrf_atomic.c 0x00000000   Number         0  nrf_atomic.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\balloc\\nrf_balloc.c 0x00000000   Number         0  nrf_balloc.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\fifo\\app_fifo.c 0x00000000   Number         0  app_fifo.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\log\\src\\nrf_log_frontend.c 0x00000000   Number         0  nrf_log_frontend.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\log\\src\\nrf_log_str_formatter.c 0x00000000   Number         0  nrf_log_str_formatter.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\memobj\\nrf_memobj.c 0x00000000   Number         0  nrf_memobj.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\ringbuf\\nrf_ringbuf.c 0x00000000   Number         0  nrf_ringbuf.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\strerror\\nrf_strerror.c 0x00000000   Number         0  nrf_strerror.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\timer\\app_timer.c 0x00000000   Number         0  app_timer.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\uart\\app_uart_fifo.c 0x00000000   Number         0  app_uart_fifo.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\uart\\retarget.c 0x00000000   Number         0  retarget.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\util\\app_error.c 0x00000000   Number         0  app_error.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\util\\app_error_handler_keil.c 0x00000000   Number         0  app_error_handler_keil.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\util\\app_error_weak.c 0x00000000   Number         0  app_error_weak.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\util\\app_util_platform.c 0x00000000   Number         0  app_util_platform.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\util\\nrf_assert.c 0x00000000   Number         0  nrf_assert.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\proprietary_rf\\esb\\nrf_esb.c 0x00000000   Number         0  nrf_esb.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\external\\fprintf\\nrf_fprintf.c 0x00000000   Number         0  nrf_fprintf.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\external\\fprintf\\nrf_fprintf_format.c 0x00000000   Number         0  nrf_fprintf_format.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\integration\\nrfx\\legacy\\nrf_drv_uart.c 0x00000000   Number         0  nrf_drv_uart.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\modules\\nrfx\\drivers\\src\\nrfx_gpiote.c 0x00000000   Number         0  nrfx_gpiote.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\modules\\nrfx\\drivers\\src\\nrfx_uart.c 0x00000000   Number         0  nrfx_uart.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\modules\\nrfx\\drivers\\src\\nrfx_uarte.c 0x00000000   Number         0  nrfx_uarte.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\modules\\nrfx\\drivers\\src\\prs\\nrfx_prs.c 0x00000000   Number         0  nrfx_prs.o ABSOLUTE
    ..\\..\\..\\Driver\\EsbProcess.c         0x00000000   Number         0  esbprocess.o ABSOLUTE
    ..\\..\\..\\Driver\\GpioProcess.c        0x00000000   Number         0  gpioprocess.o ABSOLUTE
    ..\\..\\..\\Driver\\UartProcess.c        0x00000000   Number         0  uartprocess.o ABSOLUTE
    ..\\..\\..\\Host.c                       0x00000000   Number         0  host.o ABSOLUTE
    RTE\Device\nRF52832_xxAA\arm_startup_nrf52.s 0x00000000   Number         0  arm_startup_nrf52.o ABSOLUTE
    RTE\Device\nRF52832_xxAA\system_nrf52.c  0x00000000   Number         0  system_nrf52.o ABSOLUTE
    RTE\\Device\\nRF52832_xxAA\\system_nrf52.c 0x00000000   Number         0  system_nrf52.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    .ARM.Collect$$$$00000000                 0x00000200   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x00000200   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x00000204   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x00000208   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x00000208   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x00000208   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x00000210   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x00000210   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x00000210   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x00000210   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .text                                    0x00000214   Section       36  arm_startup_nrf52.o(.text)
    $v0                                      0x00000214   Number         0  arm_startup_nrf52.o(.text)
    .text                                    0x00000238   Section        0  memcpya.o(.text)
    .text                                    0x0000025c   Section        0  memseta.o(.text)
    .text                                    0x00000280   Section        0  memcmp.o(.text)
    .text                                    0x0000029a   Section        0  uldiv.o(.text)
    .text                                    0x000002fc   Section       36  init.o(.text)
    .text                                    0x00000320   Section        0  llshl.o(.text)
    .text                                    0x0000033e   Section        0  llushr.o(.text)
    .text                                    0x0000035e   Section        0  __dczerorl2.o(.text)
    i.Action_Key1                            0x000003b4   Section        0  host.o(i.Action_Key1)
    i.EebTxRxSwitch                          0x000003bc   Section        0  esbprocess.o(i.EebTxRxSwitch)
    i.GPIOTE_IRQHandler                      0x00000400   Section        0  nrfx_gpiote.o(i.GPIOTE_IRQHandler)
    i.NVIC_ClearPendingIRQ                   0x0000061c   Section        0  app_timer.o(i.NVIC_ClearPendingIRQ)
    NVIC_ClearPendingIRQ                     0x0000061d   Thumb Code    18  app_timer.o(i.NVIC_ClearPendingIRQ)
    i.NVIC_ClearPendingIRQ                   0x00000634   Section        0  nrf_esb.o(i.NVIC_ClearPendingIRQ)
    NVIC_ClearPendingIRQ                     0x00000635   Thumb Code    18  nrf_esb.o(i.NVIC_ClearPendingIRQ)
    i.NVIC_DisableIRQ                        0x0000064c   Section        0  nrf_esb.o(i.NVIC_DisableIRQ)
    NVIC_DisableIRQ                          0x0000064d   Thumb Code    18  nrf_esb.o(i.NVIC_DisableIRQ)
    i.NVIC_EnableIRQ                         0x00000664   Section        0  app_timer.o(i.NVIC_EnableIRQ)
    NVIC_EnableIRQ                           0x00000665   Thumb Code    22  app_timer.o(i.NVIC_EnableIRQ)
    i.NVIC_EnableIRQ                         0x0000067a   Section        0  nrf_esb.o(i.NVIC_EnableIRQ)
    NVIC_EnableIRQ                           0x0000067b   Thumb Code    22  nrf_esb.o(i.NVIC_EnableIRQ)
    i.NVIC_SetPendingIRQ                     0x00000690   Section        0  app_timer.o(i.NVIC_SetPendingIRQ)
    NVIC_SetPendingIRQ                       0x00000691   Thumb Code    18  app_timer.o(i.NVIC_SetPendingIRQ)
    i.NVIC_SetPendingIRQ                     0x000006a8   Section        0  nrf_esb.o(i.NVIC_SetPendingIRQ)
    NVIC_SetPendingIRQ                       0x000006a9   Thumb Code    18  nrf_esb.o(i.NVIC_SetPendingIRQ)
    i.NVIC_SetPriority                       0x000006c0   Section        0  app_timer.o(i.NVIC_SetPriority)
    NVIC_SetPriority                         0x000006c1   Thumb Code    32  app_timer.o(i.NVIC_SetPriority)
    i.NVIC_SetPriority                       0x000006e8   Section        0  nrf_esb.o(i.NVIC_SetPriority)
    NVIC_SetPriority                         0x000006e9   Thumb Code    32  nrf_esb.o(i.NVIC_SetPriority)
    i.PacketSend                             0x00000710   Section        0  host.o(i.PacketSend)
    i.Pin_Trigger_handler_1                  0x00000758   Section        0  gpioprocess.o(i.Pin_Trigger_handler_1)
    i.Pin_Trigger_handler_2                  0x00000790   Section        0  gpioprocess.o(i.Pin_Trigger_handler_2)
    i.RADIO_IRQHandler                       0x000007a0   Section        0  nrf_esb.o(i.RADIO_IRQHandler)
    i.RTC1_IRQHandler                        0x00000818   Section        0  app_timer.o(i.RTC1_IRQHandler)
    i.SWI0_EGU0_IRQHandler                   0x0000084c   Section        0  nrf_esb.o(i.SWI0_EGU0_IRQHandler)
    i.SWI1_EGU1_IRQHandler                   0x000008b0   Section        0  app_timer.o(i.SWI1_EGU1_IRQHandler)
    i.SystemCoreClockUpdate                  0x000008b8   Section        0  system_nrf52.o(i.SystemCoreClockUpdate)
    i.SystemInit                             0x000008c8   Section        0  system_nrf52.o(i.SystemInit)
    i.TIMER3_IRQHandler                      0x00000b60   Section        0  nrf_esb.o(i.TIMER3_IRQHandler)
    i.Timer_1S                               0x00000b88   Section        0  host.o(i.Timer_1S)
    i.UARTE0_UART0_IRQHandler                0x00000c18   Section        0  nrfx_prs.o(i.UARTE0_UART0_IRQHandler)
    i.UART_Init                              0x00000c28   Section        0  uartprocess.o(i.UART_Init)
    i.__0printf$5                            0x00000c84   Section        0  printf5.o(i.__0printf$5)
    i.__scatterload_copy                     0x00000ca4   Section       14  handlers.o(i.__scatterload_copy)
    i.__scatterload_null                     0x00000cb2   Section        2  handlers.o(i.__scatterload_null)
    i.__scatterload_zeroinit                 0x00000cb4   Section       14  handlers.o(i.__scatterload_zeroinit)
    i._printf_core                           0x00000cc4   Section        0  printf5.o(i._printf_core)
    _printf_core                             0x00000cc5   Thumb Code   658  printf5.o(i._printf_core)
    i.addr_conv                              0x00000f84   Section        0  nrf_esb.o(i.addr_conv)
    addr_conv                                0x00000f85   Thumb Code    14  nrf_esb.o(i.addr_conv)
    i.app_error_fault_handler                0x00000f94   Section        0  app_error_weak.o(i.app_error_fault_handler)
    i.app_error_handler_bare                 0x00000ff0   Section        0  app_error.o(i.app_error_handler_bare)
    i.app_fifo_get                           0x0000100c   Section        0  app_fifo.o(i.app_fifo_get)
    i.app_fifo_init                          0x0000102a   Section        0  app_fifo.o(i.app_fifo_init)
    i.app_fifo_put                           0x0000104e   Section        0  app_fifo.o(i.app_fifo_put)
    i.app_timer_create                       0x00001070   Section        0  app_timer.o(i.app_timer_create)
    i.app_timer_init                         0x000010ac   Section        0  app_timer.o(i.app_timer_init)
    i.app_timer_start                        0x00001108   Section        0  app_timer.o(i.app_timer_start)
    i.app_uart_get                           0x0000115c   Section        0  app_uart_fifo.o(i.app_uart_get)
    i.app_uart_init                          0x000011b0   Section        0  app_uart_fifo.o(i.app_uart_init)
    i.app_uart_put                           0x0000128c   Section        0  app_uart_fifo.o(i.app_uart_put)
    i.app_util_critical_region_enter         0x000012f8   Section        0  app_util_platform.o(i.app_util_critical_region_enter)
    i.app_util_critical_region_exit          0x00001302   Section        0  app_util_platform.o(i.app_util_critical_region_exit)
    i.app_util_disable_irq                   0x0000130c   Section        0  app_util_platform.o(i.app_util_disable_irq)
    i.app_util_enable_irq                    0x00001320   Section        0  app_util_platform.o(i.app_util_enable_irq)
    i.apply_address_workarounds              0x00001338   Section        0  nrf_esb.o(i.apply_address_workarounds)
    apply_address_workarounds                0x00001339   Thumb Code   290  nrf_esb.o(i.apply_address_workarounds)
    i.apply_config                           0x00001474   Section        0  nrfx_uart.o(i.apply_config)
    apply_config                             0x00001475   Thumb Code   124  nrfx_uart.o(i.apply_config)
    i.apply_config                           0x000014f0   Section        0  nrfx_uarte.o(i.apply_config)
    apply_config                             0x000014f1   Thumb Code   124  nrfx_uarte.o(i.apply_config)
    i.bytewise_bit_swap                      0x0000156c   Section        0  nrf_esb.o(i.bytewise_bit_swap)
    bytewise_bit_swap                        0x0000156d   Thumb Code    12  nrf_esb.o(i.bytewise_bit_swap)
    i.channel_free                           0x00001578   Section        0  nrfx_gpiote.o(i.channel_free)
    channel_free                             0x00001579   Thumb Code    26  nrfx_gpiote.o(i.channel_free)
    i.channel_handler_get                    0x00001598   Section        0  nrfx_gpiote.o(i.channel_handler_get)
    channel_handler_get                      0x00001599   Thumb Code    10  nrfx_gpiote.o(i.channel_handler_get)
    i.channel_port_alloc                     0x000015a8   Section        0  nrfx_gpiote.o(i.channel_port_alloc)
    channel_port_alloc                       0x000015a9   Thumb Code   122  nrfx_gpiote.o(i.channel_port_alloc)
    i.channel_port_get                       0x00001628   Section        0  nrfx_gpiote.o(i.channel_port_get)
    channel_port_get                         0x00001629   Thumb Code     8  nrfx_gpiote.o(i.channel_port_get)
    i.clear_events_restart_rx                0x00001634   Section        0  nrf_esb.o(i.clear_events_restart_rx)
    clear_events_restart_rx                  0x00001635   Thumb Code    78  nrf_esb.o(i.clear_events_restart_rx)
    i.clocks_start                           0x000016a0   Section        0  host.o(i.clocks_start)
    i.compare_reg_update                     0x000016bc   Section        0  app_timer.o(i.compare_reg_update)
    compare_reg_update                       0x000016bd   Thumb Code   132  app_timer.o(i.compare_reg_update)
    i.elapsed_ticks_acquire                  0x0000174c   Section        0  app_timer.o(i.elapsed_ticks_acquire)
    elapsed_ticks_acquire                    0x0000174d   Thumb Code    82  app_timer.o(i.elapsed_ticks_acquire)
    i.errata_108                             0x000017b0   Section        0  system_nrf52.o(i.errata_108)
    errata_108                               0x000017b1   Thumb Code    78  system_nrf52.o(i.errata_108)
    i.errata_12                              0x00001804   Section        0  system_nrf52.o(i.errata_12)
    errata_12                                0x00001805   Thumb Code    78  system_nrf52.o(i.errata_12)
    i.errata_136                             0x00001858   Section        0  system_nrf52.o(i.errata_136)
    errata_136                               0x00001859   Thumb Code    78  system_nrf52.o(i.errata_136)
    i.errata_16                              0x000018ac   Section        0  system_nrf52.o(i.errata_16)
    errata_16                                0x000018ad   Thumb Code    42  system_nrf52.o(i.errata_16)
    i.errata_182                             0x000018dc   Section        0  system_nrf52.o(i.errata_182)
    errata_182                               0x000018dd   Thumb Code    26  system_nrf52.o(i.errata_182)
    i.errata_31                              0x000018fc   Section        0  system_nrf52.o(i.errata_31)
    errata_31                                0x000018fd   Thumb Code    78  system_nrf52.o(i.errata_31)
    i.errata_32                              0x00001950   Section        0  system_nrf52.o(i.errata_32)
    errata_32                                0x00001951   Thumb Code    42  system_nrf52.o(i.errata_32)
    i.errata_36                              0x00001980   Section        0  system_nrf52.o(i.errata_36)
    errata_36                                0x00001981   Thumb Code    78  system_nrf52.o(i.errata_36)
    i.errata_37                              0x000019d4   Section        0  system_nrf52.o(i.errata_37)
    errata_37                                0x000019d5   Thumb Code    42  system_nrf52.o(i.errata_37)
    i.errata_57                              0x00001a04   Section        0  system_nrf52.o(i.errata_57)
    errata_57                                0x00001a05   Thumb Code    42  system_nrf52.o(i.errata_57)
    i.errata_66                              0x00001a34   Section        0  system_nrf52.o(i.errata_66)
    errata_66                                0x00001a35   Thumb Code    42  system_nrf52.o(i.errata_66)
    i.esb_init                               0x00001a64   Section        0  esbprocess.o(i.esb_init)
    i.esb_send_packet_timer_callback         0x00001b18   Section        0  host.o(i.esb_send_packet_timer_callback)
    i.expired_timers_handler                 0x00001b24   Section        0  app_timer.o(i.expired_timers_handler)
    expired_timers_handler                   0x00001b25   Thumb Code    84  app_timer.o(i.expired_timers_handler)
    i.fifo_get                               0x00001b7c   Section        0  app_fifo.o(i.fifo_get)
    fifo_get                                 0x00001b7d   Thumb Code    24  app_fifo.o(i.fifo_get)
    i.fifo_length                            0x00001b94   Section        0  app_fifo.o(i.fifo_length)
    fifo_length                              0x00001b95   Thumb Code    10  app_fifo.o(i.fifo_length)
    i.fifo_length                            0x00001b9e   Section        0  app_uart_fifo.o(i.fifo_length)
    fifo_length                              0x00001b9f   Thumb Code    10  app_uart_fifo.o(i.fifo_length)
    i.fifo_peek                              0x00001ba8   Section        0  app_fifo.o(i.fifo_peek)
    fifo_peek                                0x00001ba9   Thumb Code    18  app_fifo.o(i.fifo_peek)
    i.fifo_put                               0x00001bba   Section        0  app_fifo.o(i.fifo_put)
    fifo_put                                 0x00001bbb   Thumb Code    18  app_fifo.o(i.fifo_put)
    i.fputc                                  0x00001bcc   Section        0  retarget.o(i.fputc)
    i.gpio_init                              0x00001bdc   Section        0  gpioprocess.o(i.gpio_init)
    i.initialize_fifos                       0x00001c8c   Section        0  nrf_esb.o(i.initialize_fifos)
    initialize_fifos                         0x00001c8d   Thumb Code    60  nrf_esb.o(i.initialize_fifos)
    i.interrupts_enable                      0x00001cd8   Section        0  nrfx_uart.o(i.interrupts_enable)
    interrupts_enable                        0x00001cd9   Thumb Code   144  nrfx_uart.o(i.interrupts_enable)
    i.interrupts_enable                      0x00001d78   Section        0  nrfx_uarte.o(i.interrupts_enable)
    interrupts_enable                        0x00001d79   Thumb Code   164  nrfx_uarte.o(i.interrupts_enable)
    i.list_insertions_handler                0x00001e2c   Section        0  app_timer.o(i.list_insertions_handler)
    list_insertions_handler                  0x00001e2d   Thumb Code   294  app_timer.o(i.list_insertions_handler)
    i.main                                   0x00001f68   Section        0  host.o(i.main)
    i.nrf_bitmask_bit_is_set                 0x00001fd4   Section        0  nrfx_gpiote.o(i.nrf_bitmask_bit_is_set)
    nrf_bitmask_bit_is_set                   0x00001fd5   Thumb Code    22  nrfx_gpiote.o(i.nrf_bitmask_bit_is_set)
    i.nrf_bitmask_bit_set                    0x00001fea   Section        0  nrfx_gpiote.o(i.nrf_bitmask_bit_set)
    nrf_bitmask_bit_set                      0x00001feb   Thumb Code    22  nrfx_gpiote.o(i.nrf_bitmask_bit_set)
    i.nrf_delay_ms                           0x00002000   Section        0  host.o(i.nrf_delay_ms)
    nrf_delay_ms                             0x00002001   Thumb Code    42  host.o(i.nrf_delay_ms)
    i.nrf_drv_uart_init                      0x00002030   Section        0  nrf_drv_uart.o(i.nrf_drv_uart_init)
    i.nrf_drv_uart_rx                        0x000020bc   Section        0  app_uart_fifo.o(i.nrf_drv_uart_rx)
    nrf_drv_uart_rx                          0x000020bd   Thumb Code    62  app_uart_fifo.o(i.nrf_drv_uart_rx)
    i.nrf_drv_uart_tx                        0x00002100   Section        0  app_uart_fifo.o(i.nrf_drv_uart_tx)
    nrf_drv_uart_tx                          0x00002101   Thumb Code    62  app_uart_fifo.o(i.nrf_drv_uart_tx)
    i.nrf_esb_disable                        0x00002144   Section        0  nrf_esb.o(i.nrf_esb_disable)
    i.nrf_esb_event_handler                  0x00002194   Section        0  host.o(i.nrf_esb_event_handler)
    i.nrf_esb_flush_tx                       0x000022cc   Section        0  nrf_esb.o(i.nrf_esb_flush_tx)
    i.nrf_esb_get_clear_interrupts           0x00002300   Section        0  nrf_esb.o(i.nrf_esb_get_clear_interrupts)
    nrf_esb_get_clear_interrupts             0x00002301   Thumb Code    56  nrf_esb.o(i.nrf_esb_get_clear_interrupts)
    i.nrf_esb_init                           0x00002340   Section        0  nrf_esb.o(i.nrf_esb_init)
    i.nrf_esb_read_rx_payload                0x00002438   Section        0  nrf_esb.o(i.nrf_esb_read_rx_payload)
    i.nrf_esb_set_base_address_0             0x000024e4   Section        0  nrf_esb.o(i.nrf_esb_set_base_address_0)
    i.nrf_esb_set_base_address_1             0x00002560   Section        0  nrf_esb.o(i.nrf_esb_set_base_address_1)
    i.nrf_esb_set_prefixes                   0x00002620   Section        0  nrf_esb.o(i.nrf_esb_set_prefixes)
    i.nrf_esb_skip_tx                        0x000026dc   Section        0  nrf_esb.o(i.nrf_esb_skip_tx)
    i.nrf_esb_start_rx                       0x00002730   Section        0  nrf_esb.o(i.nrf_esb_start_rx)
    i.nrf_esb_start_tx                       0x000027d8   Section        0  nrf_esb.o(i.nrf_esb_start_tx)
    i.nrf_esb_stop_rx                        0x00002804   Section        0  nrf_esb.o(i.nrf_esb_stop_rx)
    i.nrf_esb_write_payload                  0x00002858   Section        0  nrf_esb.o(i.nrf_esb_write_payload)
    i.nrf_gpio_cfg                           0x00002948   Section        0  nrfx_uart.o(i.nrf_gpio_cfg)
    nrf_gpio_cfg                             0x00002949   Thumb Code    40  nrfx_uart.o(i.nrf_gpio_cfg)
    i.nrf_gpio_cfg                           0x00002970   Section        0  nrfx_uarte.o(i.nrf_gpio_cfg)
    nrf_gpio_cfg                             0x00002971   Thumb Code    40  nrfx_uarte.o(i.nrf_gpio_cfg)
    i.nrf_gpio_cfg                           0x00002998   Section        0  nrfx_gpiote.o(i.nrf_gpio_cfg)
    nrf_gpio_cfg                             0x00002999   Thumb Code    40  nrfx_gpiote.o(i.nrf_gpio_cfg)
    i.nrf_gpio_cfg_input                     0x000029c0   Section        0  nrfx_uart.o(i.nrf_gpio_cfg_input)
    nrf_gpio_cfg_input                       0x000029c1   Thumb Code    26  nrfx_uart.o(i.nrf_gpio_cfg_input)
    i.nrf_gpio_cfg_input                     0x000029da   Section        0  nrfx_uarte.o(i.nrf_gpio_cfg_input)
    nrf_gpio_cfg_input                       0x000029db   Thumb Code    26  nrfx_uarte.o(i.nrf_gpio_cfg_input)
    i.nrf_gpio_cfg_output                    0x000029f4   Section        0  gpioprocess.o(i.nrf_gpio_cfg_output)
    nrf_gpio_cfg_output                      0x000029f5   Thumb Code    48  gpioprocess.o(i.nrf_gpio_cfg_output)
    i.nrf_gpio_cfg_output                    0x00002a24   Section        0  nrfx_uart.o(i.nrf_gpio_cfg_output)
    nrf_gpio_cfg_output                      0x00002a25   Thumb Code    24  nrfx_uart.o(i.nrf_gpio_cfg_output)
    i.nrf_gpio_cfg_output                    0x00002a3c   Section        0  nrfx_uarte.o(i.nrf_gpio_cfg_output)
    nrf_gpio_cfg_output                      0x00002a3d   Thumb Code    24  nrfx_uarte.o(i.nrf_gpio_cfg_output)
    i.nrf_gpio_cfg_sense_set                 0x00002a54   Section        0  nrfx_gpiote.o(i.nrf_gpio_cfg_sense_set)
    nrf_gpio_cfg_sense_set                   0x00002a55   Thumb Code    50  nrfx_gpiote.o(i.nrf_gpio_cfg_sense_set)
    i.nrf_gpio_pin_clear                     0x00002a86   Section        0  gpioprocess.o(i.nrf_gpio_pin_clear)
    nrf_gpio_pin_clear                       0x00002a87   Thumb Code    22  gpioprocess.o(i.nrf_gpio_pin_clear)
    i.nrf_gpio_pin_read                      0x00002a9c   Section        0  nrfx_gpiote.o(i.nrf_gpio_pin_read)
    nrf_gpio_pin_read                        0x00002a9d   Thumb Code    24  nrfx_gpiote.o(i.nrf_gpio_pin_read)
    i.nrf_gpio_pin_set                       0x00002ab4   Section        0  nrfx_uart.o(i.nrf_gpio_pin_set)
    nrf_gpio_pin_set                         0x00002ab5   Thumb Code    22  nrfx_uart.o(i.nrf_gpio_pin_set)
    i.nrf_gpio_pin_set                       0x00002aca   Section        0  nrfx_uarte.o(i.nrf_gpio_pin_set)
    nrf_gpio_pin_set                         0x00002acb   Thumb Code    22  nrfx_uarte.o(i.nrf_gpio_pin_set)
    i.nrf_gpio_pin_toggle                    0x00002ae0   Section        0  gpioprocess.o(i.nrf_gpio_pin_toggle)
    nrf_gpio_pin_toggle                      0x00002ae1   Thumb Code    34  gpioprocess.o(i.nrf_gpio_pin_toggle)
    i.nrf_gpio_ports_read                    0x00002b04   Section        0  nrfx_gpiote.o(i.nrf_gpio_ports_read)
    nrf_gpio_ports_read                      0x00002b05   Thumb Code    36  nrfx_gpiote.o(i.nrf_gpio_ports_read)
    i.nrf_gpiote_event_addr_get              0x00002b2c   Section        0  nrfx_gpiote.o(i.nrf_gpiote_event_addr_get)
    nrf_gpiote_event_addr_get                0x00002b2d   Thumb Code     8  nrfx_gpiote.o(i.nrf_gpiote_event_addr_get)
    i.nrf_gpiote_event_clear                 0x00002b38   Section        0  nrfx_gpiote.o(i.nrf_gpiote_event_clear)
    nrf_gpiote_event_clear                   0x00002b39   Thumb Code    28  nrfx_gpiote.o(i.nrf_gpiote_event_clear)
    i.nrf_gpiote_event_is_set                0x00002b54   Section        0  nrfx_gpiote.o(i.nrf_gpiote_event_is_set)
    nrf_gpiote_event_is_set                  0x00002b55   Thumb Code    22  nrfx_gpiote.o(i.nrf_gpiote_event_is_set)
    i.nrf_gpiote_int_enable                  0x00002b6c   Section        0  nrfx_gpiote.o(i.nrf_gpiote_int_enable)
    nrf_gpiote_int_enable                    0x00002b6d   Thumb Code     6  nrfx_gpiote.o(i.nrf_gpiote_int_enable)
    i.nrf_uart_errorsrc_get_and_clear        0x00002b78   Section        0  nrfx_uart.o(i.nrf_uart_errorsrc_get_and_clear)
    nrf_uart_errorsrc_get_and_clear          0x00002b79   Thumb Code    12  nrfx_uart.o(i.nrf_uart_errorsrc_get_and_clear)
    i.nrf_uart_event_check                   0x00002b84   Section        0  nrfx_uart.o(i.nrf_uart_event_check)
    nrf_uart_event_check                     0x00002b85   Thumb Code    14  nrfx_uart.o(i.nrf_uart_event_check)
    i.nrf_uart_event_clear                   0x00002b92   Section        0  nrfx_uart.o(i.nrf_uart_event_clear)
    nrf_uart_event_clear                     0x00002b93   Thumb Code    14  nrfx_uart.o(i.nrf_uart_event_clear)
    i.nrf_uart_hwfc_pins_set                 0x00002ba0   Section        0  nrfx_uart.o(i.nrf_uart_hwfc_pins_set)
    nrf_uart_hwfc_pins_set                   0x00002ba1   Thumb Code    10  nrfx_uart.o(i.nrf_uart_hwfc_pins_set)
    i.nrf_uart_int_disable                   0x00002baa   Section        0  nrfx_uart.o(i.nrf_uart_int_disable)
    nrf_uart_int_disable                     0x00002bab   Thumb Code     6  nrfx_uart.o(i.nrf_uart_int_disable)
    i.nrf_uart_int_enable                    0x00002bb0   Section        0  nrfx_uart.o(i.nrf_uart_int_enable)
    nrf_uart_int_enable                      0x00002bb1   Thumb Code     6  nrfx_uart.o(i.nrf_uart_int_enable)
    i.nrf_uart_int_enable_check              0x00002bb6   Section        0  nrfx_uart.o(i.nrf_uart_int_enable_check)
    nrf_uart_int_enable_check                0x00002bb7   Thumb Code    18  nrfx_uart.o(i.nrf_uart_int_enable_check)
    i.nrf_uart_task_trigger                  0x00002bc8   Section        0  nrfx_uart.o(i.nrf_uart_task_trigger)
    nrf_uart_task_trigger                    0x00002bc9   Thumb Code     6  nrfx_uart.o(i.nrf_uart_task_trigger)
    i.nrf_uart_txrx_pins_set                 0x00002bce   Section        0  nrfx_uart.o(i.nrf_uart_txrx_pins_set)
    nrf_uart_txrx_pins_set                   0x00002bcf   Thumb Code    10  nrfx_uart.o(i.nrf_uart_txrx_pins_set)
    i.nrf_uarte_errorsrc_get_and_clear       0x00002bd8   Section        0  nrfx_uarte.o(i.nrf_uarte_errorsrc_get_and_clear)
    nrf_uarte_errorsrc_get_and_clear         0x00002bd9   Thumb Code    12  nrfx_uarte.o(i.nrf_uarte_errorsrc_get_and_clear)
    i.nrf_uarte_event_check                  0x00002be4   Section        0  nrfx_uarte.o(i.nrf_uarte_event_check)
    nrf_uarte_event_check                    0x00002be5   Thumb Code    14  nrfx_uarte.o(i.nrf_uarte_event_check)
    i.nrf_uarte_event_clear                  0x00002bf2   Section        0  nrfx_uarte.o(i.nrf_uarte_event_clear)
    nrf_uarte_event_clear                    0x00002bf3   Thumb Code    14  nrfx_uarte.o(i.nrf_uarte_event_clear)
    i.nrf_uarte_hwfc_pins_set                0x00002c00   Section        0  nrfx_uarte.o(i.nrf_uarte_hwfc_pins_set)
    nrf_uarte_hwfc_pins_set                  0x00002c01   Thumb Code    12  nrfx_uarte.o(i.nrf_uarte_hwfc_pins_set)
    i.nrf_uarte_int_disable                  0x00002c0c   Section        0  nrfx_uarte.o(i.nrf_uarte_int_disable)
    nrf_uarte_int_disable                    0x00002c0d   Thumb Code     6  nrfx_uarte.o(i.nrf_uarte_int_disable)
    i.nrf_uarte_int_enable                   0x00002c12   Section        0  nrfx_uarte.o(i.nrf_uarte_int_enable)
    nrf_uarte_int_enable                     0x00002c13   Thumb Code     6  nrfx_uarte.o(i.nrf_uarte_int_enable)
    i.nrf_uarte_rx_amount_get                0x00002c18   Section        0  nrfx_uarte.o(i.nrf_uarte_rx_amount_get)
    nrf_uarte_rx_amount_get                  0x00002c19   Thumb Code    10  nrfx_uarte.o(i.nrf_uarte_rx_amount_get)
    i.nrf_uarte_task_trigger                 0x00002c22   Section        0  nrfx_uarte.o(i.nrf_uarte_task_trigger)
    nrf_uarte_task_trigger                   0x00002c23   Thumb Code     6  nrfx_uarte.o(i.nrf_uarte_task_trigger)
    i.nrf_uarte_txrx_pins_set                0x00002c28   Section        0  nrfx_uarte.o(i.nrf_uarte_txrx_pins_set)
    nrf_uarte_txrx_pins_set                  0x00002c29   Thumb Code    14  nrfx_uarte.o(i.nrf_uarte_txrx_pins_set)
    i.nrfx_coredep_delay_us                  0x00002c38   Section        0  app_timer.o(i.nrfx_coredep_delay_us)
    nrfx_coredep_delay_us                    0x00002c39   Thumb Code    20  app_timer.o(i.nrfx_coredep_delay_us)
    i.nrfx_get_irq_number                    0x00002c50   Section        0  nrfx_uart.o(i.nrfx_get_irq_number)
    nrfx_get_irq_number                      0x00002c51   Thumb Code     8  nrfx_uart.o(i.nrfx_get_irq_number)
    i.nrfx_get_irq_number                    0x00002c58   Section        0  nrfx_uarte.o(i.nrfx_get_irq_number)
    nrfx_get_irq_number                      0x00002c59   Thumb Code     8  nrfx_uarte.o(i.nrfx_get_irq_number)
    i.nrfx_gpiote_in_event_enable            0x00002c60   Section        0  nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable)
    i.nrfx_gpiote_in_init                    0x00002d0c   Section        0  nrfx_gpiote.o(i.nrfx_gpiote_in_init)
    i.nrfx_gpiote_init                       0x00002e00   Section        0  nrfx_gpiote.o(i.nrfx_gpiote_init)
    i.nrfx_is_in_ram                         0x00002ec4   Section        0  nrfx_uarte.o(i.nrfx_is_in_ram)
    nrfx_is_in_ram                           0x00002ec5   Thumb Code    20  nrfx_uarte.o(i.nrfx_is_in_ram)
    i.nrfx_prs_acquire                       0x00002ed8   Section        0  nrfx_prs.o(i.nrfx_prs_acquire)
    i.nrfx_uart_0_irq_handler                0x00002f20   Section        0  nrfx_uart.o(i.nrfx_uart_0_irq_handler)
    i.nrfx_uart_init                         0x00002f34   Section        0  nrfx_uart.o(i.nrfx_uart_init)
    i.nrfx_uart_rx                           0x00002fbc   Section        0  nrfx_uart.o(i.nrfx_uart_rx)
    i.nrfx_uart_tx                           0x000030e0   Section        0  nrfx_uart.o(i.nrfx_uart_tx)
    i.nrfx_uart_tx_in_progress               0x0000316c   Section        0  nrfx_uart.o(i.nrfx_uart_tx_in_progress)
    i.nrfx_uarte_0_irq_handler               0x00003190   Section        0  nrfx_uarte.o(i.nrfx_uarte_0_irq_handler)
    i.nrfx_uarte_init                        0x000031a4   Section        0  nrfx_uarte.o(i.nrfx_uarte_init)
    i.nrfx_uarte_rx                          0x00003224   Section        0  nrfx_uarte.o(i.nrfx_uarte_rx)
    i.nrfx_uarte_tx                          0x0000335c   Section        0  nrfx_uarte.o(i.nrfx_uarte_tx)
    i.nrfx_uarte_tx_in_progress              0x00003404   Section        0  nrfx_uarte.o(i.nrfx_uarte_tx_in_progress)
    i.on_radio_disabled_rx                   0x00003424   Section        0  nrf_esb.o(i.on_radio_disabled_rx)
    on_radio_disabled_rx                     0x00003425   Thumb Code   408  nrf_esb.o(i.on_radio_disabled_rx)
    i.on_radio_disabled_rx_ack               0x000035fc   Section        0  nrf_esb.o(i.on_radio_disabled_rx_ack)
    on_radio_disabled_rx_ack                 0x000035fd   Thumb Code    44  nrf_esb.o(i.on_radio_disabled_rx_ack)
    i.on_radio_disabled_tx                   0x0000364c   Section        0  nrf_esb.o(i.on_radio_disabled_tx)
    on_radio_disabled_tx                     0x0000364d   Thumb Code   102  nrf_esb.o(i.on_radio_disabled_tx)
    i.on_radio_disabled_tx_noack             0x000036f0   Section        0  nrf_esb.o(i.on_radio_disabled_tx_noack)
    on_radio_disabled_tx_noack               0x000036f1   Thumb Code    50  nrf_esb.o(i.on_radio_disabled_tx_noack)
    i.on_radio_disabled_tx_wait_for_ack      0x00003730   Section        0  nrf_esb.o(i.on_radio_disabled_tx_wait_for_ack)
    on_radio_disabled_tx_wait_for_ack        0x00003731   Thumb Code   290  nrf_esb.o(i.on_radio_disabled_tx_wait_for_ack)
    i.pin_configured_set                     0x000038a0   Section        0  nrfx_gpiote.o(i.pin_configured_set)
    pin_configured_set                       0x000038a1   Thumb Code    14  nrfx_gpiote.o(i.pin_configured_set)
    i.pin_in_use_by_gpiote                   0x000038b4   Section        0  nrfx_gpiote.o(i.pin_in_use_by_gpiote)
    pin_in_use_by_gpiote                     0x000038b5   Thumb Code    22  nrfx_gpiote.o(i.pin_in_use_by_gpiote)
    i.pin_in_use_by_port                     0x000038d0   Section        0  nrfx_gpiote.o(i.pin_in_use_by_port)
    pin_in_use_by_port                       0x000038d1   Thumb Code    18  nrfx_gpiote.o(i.pin_in_use_by_port)
    i.pin_in_use_by_te                       0x000038e8   Section        0  nrfx_gpiote.o(i.pin_in_use_by_te)
    pin_in_use_by_te                         0x000038e9   Thumb Code    26  nrfx_gpiote.o(i.pin_in_use_by_te)
    i.pin_in_use_clear                       0x00003908   Section        0  nrfx_gpiote.o(i.pin_in_use_clear)
    pin_in_use_clear                         0x00003909   Thumb Code     8  nrfx_gpiote.o(i.pin_in_use_clear)
    i.ppi_init                               0x00003914   Section        0  nrf_esb.o(i.ppi_init)
    ppi_init                                 0x00003915   Thumb Code    58  nrf_esb.o(i.ppi_init)
    i.prs_box_get                            0x00003964   Section        0  nrfx_prs.o(i.prs_box_get)
    prs_box_get                              0x00003965   Thumb Code    16  nrfx_prs.o(i.prs_box_get)
    i.reset_fifos                            0x0000397c   Section        0  nrf_esb.o(i.reset_fifos)
    reset_fifos                              0x0000397d   Thumb Code    20  nrf_esb.o(i.reset_fifos)
    i.rtc1_compare0_set                      0x00003998   Section        0  app_timer.o(i.rtc1_compare0_set)
    rtc1_compare0_set                        0x00003999   Thumb Code     6  app_timer.o(i.rtc1_compare0_set)
    i.rtc1_counter_get                       0x000039a4   Section        0  app_timer.o(i.rtc1_counter_get)
    rtc1_counter_get                         0x000039a5   Thumb Code     6  app_timer.o(i.rtc1_counter_get)
    i.rtc1_init                              0x000039b0   Section        0  app_timer.o(i.rtc1_init)
    rtc1_init                                0x000039b1   Thumb Code    18  app_timer.o(i.rtc1_init)
    i.rtc1_start                             0x000039c8   Section        0  app_timer.o(i.rtc1_start)
    rtc1_start                               0x000039c9   Thumb Code    48  app_timer.o(i.rtc1_start)
    i.rtc1_stop                              0x00003a04   Section        0  app_timer.o(i.rtc1_stop)
    rtc1_stop                                0x00003a05   Thumb Code    68  app_timer.o(i.rtc1_stop)
    i.rx_byte                                0x00003a5c   Section        0  nrfx_uart.o(i.rx_byte)
    rx_byte                                  0x00003a5d   Thumb Code    62  nrfx_uart.o(i.rx_byte)
    i.rx_done_event                          0x00003a9a   Section        0  nrfx_uart.o(i.rx_done_event)
    rx_done_event                            0x00003a9b   Thumb Code    28  nrfx_uart.o(i.rx_done_event)
    i.rx_done_event                          0x00003ab6   Section        0  nrfx_uarte.o(i.rx_done_event)
    rx_done_event                            0x00003ab7   Thumb Code    32  nrfx_uarte.o(i.rx_done_event)
    i.rx_enable                              0x00003ad6   Section        0  nrfx_uart.o(i.rx_enable)
    rx_enable                                0x00003ad7   Thumb Code    34  nrfx_uart.o(i.rx_enable)
    i.rx_fifo_push_rfbuf                     0x00003af8   Section        0  nrf_esb.o(i.rx_fifo_push_rfbuf)
    rx_fifo_push_rfbuf                       0x00003af9   Thumb Code   216  nrf_esb.o(i.rx_fifo_push_rfbuf)
    i.start_tx_transaction                   0x00003be0   Section        0  nrf_esb.o(i.start_tx_transaction)
    start_tx_transaction                     0x00003be1   Thumb Code   372  nrf_esb.o(i.start_tx_transaction)
    i.sys_timer_init                         0x00003d94   Section        0  nrf_esb.o(i.sys_timer_init)
    sys_timer_init                           0x00003d95   Thumb Code    24  nrf_esb.o(i.sys_timer_init)
    i.ticks_diff_get                         0x00003db4   Section        0  app_timer.o(i.ticks_diff_get)
    ticks_diff_get                           0x00003db5   Thumb Code    10  app_timer.o(i.ticks_diff_get)
    i.timeout_handler_exec                   0x00003dbe   Section        0  app_timer.o(i.timeout_handler_exec)
    timeout_handler_exec                     0x00003dbf   Thumb Code    12  app_timer.o(i.timeout_handler_exec)
    i.timer_list_handler                     0x00003dcc   Section        0  app_timer.o(i.timer_list_handler)
    timer_list_handler                       0x00003dcd   Thumb Code    68  app_timer.o(i.timer_list_handler)
    i.timer_list_handler_sched               0x00003e1c   Section        0  app_timer.o(i.timer_list_handler_sched)
    timer_list_handler_sched                 0x00003e1d   Thumb Code    10  app_timer.o(i.timer_list_handler_sched)
    i.timer_list_insert                      0x00003e28   Section        0  app_timer.o(i.timer_list_insert)
    timer_list_insert                        0x00003e29   Thumb Code    98  app_timer.o(i.timer_list_insert)
    i.timer_list_remove                      0x00003e90   Section        0  app_timer.o(i.timer_list_remove)
    timer_list_remove                        0x00003e91   Thumb Code   118  app_timer.o(i.timer_list_remove)
    i.timer_start_op_schedule                0x00003f18   Section        0  app_timer.o(i.timer_start_op_schedule)
    timer_start_op_schedule                  0x00003f19   Thumb Code    88  app_timer.o(i.timer_start_op_schedule)
    i.timer_timeouts_check                   0x00003f70   Section        0  app_timer.o(i.timer_timeouts_check)
    timer_timeouts_check                     0x00003f71   Thumb Code   130  app_timer.o(i.timer_timeouts_check)
    i.timer_timeouts_check_sched             0x00004008   Section        0  app_timer.o(i.timer_timeouts_check_sched)
    timer_timeouts_check_sched               0x00004009   Thumb Code    10  app_timer.o(i.timer_timeouts_check_sched)
    i.timers_init                            0x00004014   Section        0  host.o(i.timers_init)
    timers_init                              0x00004015   Thumb Code    94  host.o(i.timers_init)
    i.timers_start                           0x00004084   Section        0  host.o(i.timers_start)
    timers_start                             0x00004085   Thumb Code    38  host.o(i.timers_start)
    i.tx_blocking                            0x000040b0   Section        0  nrfx_uart.o(i.tx_blocking)
    tx_blocking                              0x000040b1   Thumb Code    54  nrfx_uart.o(i.tx_blocking)
    i.tx_byte                                0x000040e6   Section        0  nrfx_uart.o(i.tx_byte)
    tx_byte                                  0x000040e7   Thumb Code    38  nrfx_uart.o(i.tx_byte)
    i.tx_done_event                          0x0000410c   Section        0  nrfx_uart.o(i.tx_done_event)
    tx_done_event                            0x0000410d   Thumb Code    32  nrfx_uart.o(i.tx_done_event)
    i.tx_done_event                          0x0000412c   Section        0  nrfx_uarte.o(i.tx_done_event)
    tx_done_event                            0x0000412d   Thumb Code    36  nrfx_uarte.o(i.tx_done_event)
    i.uart_event_handle                      0x00004150   Section        0  uartprocess.o(i.uart_event_handle)
    i.uart_event_handler                     0x000042e4   Section        0  app_uart_fifo.o(i.uart_event_handler)
    uart_event_handler                       0x000042e5   Thumb Code   184  app_uart_fifo.o(i.uart_event_handler)
    i.uart_evt_handler                       0x000043b8   Section        0  nrf_drv_uart.o(i.uart_evt_handler)
    uart_evt_handler                         0x000043b9   Thumb Code    46  nrf_drv_uart.o(i.uart_evt_handler)
    i.uart_irq_handler                       0x000043f0   Section        0  nrfx_uart.o(i.uart_irq_handler)
    uart_irq_handler                         0x000043f1   Thumb Code   332  nrfx_uart.o(i.uart_irq_handler)
    i.uarte_evt_handler                      0x0000453c   Section        0  nrf_drv_uart.o(i.uarte_evt_handler)
    uarte_evt_handler                        0x0000453d   Thumb Code    46  nrf_drv_uart.o(i.uarte_evt_handler)
    i.uarte_irq_handler                      0x00004574   Section        0  nrfx_uarte.o(i.uarte_irq_handler)
    uarte_irq_handler                        0x00004575   Thumb Code   268  nrfx_uarte.o(i.uarte_irq_handler)
    i.update_radio_addresses                 0x00004680   Section        0  nrf_esb.o(i.update_radio_addresses)
    update_radio_addresses                   0x00004681   Thumb Code    76  nrf_esb.o(i.update_radio_addresses)
    i.update_radio_bitrate                   0x000046d4   Section        0  nrf_esb.o(i.update_radio_bitrate)
    update_radio_bitrate                     0x000046d5   Thumb Code    64  nrf_esb.o(i.update_radio_bitrate)
    i.update_radio_crc                       0x00004720   Section        0  nrf_esb.o(i.update_radio_crc)
    update_radio_crc                         0x00004721   Thumb Code    68  nrf_esb.o(i.update_radio_crc)
    i.update_radio_parameters                0x00004770   Section        0  nrf_esb.o(i.update_radio_parameters)
    update_radio_parameters                  0x00004771   Thumb Code    56  nrf_esb.o(i.update_radio_parameters)
    i.update_radio_protocol                  0x000047b0   Section        0  nrf_esb.o(i.update_radio_protocol)
    update_radio_protocol                    0x000047b1   Thumb Code    36  nrf_esb.o(i.update_radio_protocol)
    i.update_radio_tx_power                  0x000047e4   Section        0  nrf_esb.o(i.update_radio_tx_power)
    update_radio_tx_power                    0x000047e5   Thumb Code    10  nrf_esb.o(i.update_radio_tx_power)
    i.update_rf_payload_format_esb           0x000047f8   Section        0  nrf_esb.o(i.update_rf_payload_format_esb)
    update_rf_payload_format_esb             0x000047f9   Thumb Code    34  nrf_esb.o(i.update_rf_payload_format_esb)
    i.update_rf_payload_format_esb_dpl       0x00004828   Section        0  nrf_esb.o(i.update_rf_payload_format_esb_dpl)
    update_rf_payload_format_esb_dpl         0x00004829   Thumb Code    32  nrf_esb.o(i.update_rf_payload_format_esb_dpl)
    i.user_op_alloc                          0x00004854   Section        0  app_timer.o(i.user_op_alloc)
    user_op_alloc                            0x00004855   Thumb Code    56  app_timer.o(i.user_op_alloc)
    i.user_op_enque                          0x00004890   Section        0  app_timer.o(i.user_op_enque)
    user_op_enque                            0x00004891   Thumb Code     6  app_timer.o(i.user_op_enque)
    .constdata                               0x0000489c   Section        3  gpioprocess.o(.constdata)
    .constdata                               0x000048a0   Section       22  host.o(.constdata)
    m_esb_tx_timer_id                        0x000048a0   Data           4  host.o(.constdata)
    Timer_1S_timer_id                        0x000048a4   Data           4  host.o(.constdata)
    delay_bytecode                           0x000048b0   Data           6  host.o(.constdata)
    .constdata                               0x000048b8   Section       46  nrfx_uart.o(.constdata)
    __func__                                 0x000048b8   Data          15  nrfx_uart.o(.constdata)
    irq_handlers                             0x000048c8   Data           4  nrfx_uart.o(.constdata)
    __func__                                 0x000048cc   Data          13  nrfx_uart.o(.constdata)
    __func__                                 0x000048d9   Data          13  nrfx_uart.o(.constdata)
    .constdata                               0x000048e8   Section       48  nrfx_uarte.o(.constdata)
    __func__                                 0x000048e8   Data          16  nrfx_uarte.o(.constdata)
    irq_handlers                             0x000048f8   Data           4  nrfx_uarte.o(.constdata)
    __func__                                 0x000048fc   Data          14  nrfx_uarte.o(.constdata)
    __func__                                 0x0000490a   Data          14  nrfx_uarte.o(.constdata)
    .constdata                               0x00004918   Section       62  nrfx_gpiote.o(.constdata)
    __func__                                 0x0000491c   Data          17  nrfx_gpiote.o(.constdata)
    __func__                                 0x0000492d   Data          21  nrfx_gpiote.o(.constdata)
    __func__                                 0x00004942   Data          20  nrfx_gpiote.o(.constdata)
    .constdata                               0x00004958   Section       32  app_uart_fifo.o(.constdata)
    .constdata                               0x00004980   Section        6  app_timer.o(.constdata)
    delay_bytecode                           0x00004980   Data           6  app_timer.o(.constdata)
    .constdata                               0x00004990   Section       32  uartprocess.o(.constdata)
    delay_bytecode                           0x00004990   Data           6  uartprocess.o(.constdata)
    .ARM.__AT_0x1000120C                     0x1000120c   Section        4  gpioprocess.o(.ARM.__AT_0x1000120C)
    __tagsym$$used                           0x1000120c   Number         0  gpioprocess.o(.ARM.__AT_0x1000120C)
    .data                                    0x20000000   Section        1  gpioprocess.o(.data)
    .data                                    0x20000004   Section       44  host.o(.data)
    sPacketSendOKCnt                         0x20000020   Data           4  host.o(.data)
    sPacketSentNGCnt                         0x20000024   Data           4  host.o(.data)
    sPacketReceiveOKCnt                      0x20000028   Data           4  host.o(.data)
    sPacketReceiveNGCnt                      0x2000002c   Data           4  host.o(.data)
    .data                                    0x20000030   Section       92  esbprocess.o(.data)
    .data                                    0x2000008c   Section        9  nrf_drv_uart.o(.data)
    m_handlers                               0x2000008c   Data           4  nrf_drv_uart.o(.data)
    m_contexts                               0x20000090   Data           4  nrf_drv_uart.o(.data)
    .data                                    0x20000098   Section        8  nrfx_prs.o(.data)
    m_prs_box_4                              0x20000098   Data           8  nrfx_prs.o(.data)
    .data                                    0x200000a0   Section       27  app_uart_fifo.o(.data)
    app_uart_inst                            0x200000a0   Data          20  app_uart_fifo.o(.data)
    m_event_handler                          0x200000b4   Data           4  app_uart_fifo.o(.data)
    tx_buffer                                0x200000b8   Data           1  app_uart_fifo.o(.data)
    rx_buffer                                0x200000b9   Data           1  app_uart_fifo.o(.data)
    m_rx_ovf                                 0x200000ba   Data           1  app_uart_fifo.o(.data)
    .data                                    0x200000bc   Section        4  app_util_platform.o(.data)
    m_in_critical_region                     0x200000bc   Data           4  app_util_platform.o(.data)
    .data                                    0x200000c0   Section       20  app_timer.o(.data)
    mp_timer_id_head                         0x200000c0   Data           4  app_timer.o(.data)
    m_ticks_latest                           0x200000c4   Data           4  app_timer.o(.data)
    m_ticks_elapsed                          0x200000c8   Data           8  app_timer.o(.data)
    m_ticks_elapsed_q_read_ind               0x200000d0   Data           1  app_timer.o(.data)
    m_ticks_elapsed_q_write_ind              0x200000d1   Data           1  app_timer.o(.data)
    m_rtc1_running                           0x200000d2   Data           1  app_timer.o(.data)
    m_rtc1_reset                             0x200000d3   Data           1  app_timer.o(.data)
    .data                                    0x200000d4   Section        8  retarget.o(.data)
    .data                                    0x200000dc   Section       72  nrf_esb.o(.data)
    m_esb_initialized                        0x200000dc   Data           1  nrf_esb.o(.data)
    m_nrf_esb_mainstate                      0x200000dd   Data           1  nrf_esb.o(.data)
    mp_current_payload                       0x200000e0   Data           4  nrf_esb.o(.data)
    m_event_handler                          0x200000e4   Data           4  nrf_esb.o(.data)
    m_esb_addr                               0x200000e8   Data          20  nrf_esb.o(.data)
    m_interrupt_flags                        0x200000fc   Data           4  nrf_esb.o(.data)
    m_pids                                   0x20000100   Data           8  nrf_esb.o(.data)
    m_retransmits_remaining                  0x20000108   Data           4  nrf_esb.o(.data)
    m_last_tx_attempts                       0x2000010c   Data           4  nrf_esb.o(.data)
    m_wait_for_ack_timeout_us                0x20000110   Data           4  nrf_esb.o(.data)
    m_radio_shorts_common                    0x20000114   Data           4  nrf_esb.o(.data)
    on_radio_disabled                        0x20000118   Data           4  nrf_esb.o(.data)
    on_radio_end                             0x2000011c   Data           4  nrf_esb.o(.data)
    update_rf_payload_format                 0x20000120   Data           4  nrf_esb.o(.data)
    .data                                    0x20000124   Section        1  uartprocess.o(.data)
    index                                    0x20000124   Data           1  uartprocess.o(.data)
    .data                                    0x20000128   Section        4  system_nrf52.o(.data)
    __tagsym$$used                           0x20000128   Number         0  system_nrf52.o(.data)
    .bss                                     0x2000012c   Section       64  host.o(.bss)
    m_esb_tx_timer_id_data                   0x2000012c   Data          32  host.o(.bss)
    Timer_1S_timer_id_data                   0x2000014c   Data          32  host.o(.bss)
    .bss                                     0x2000016c   Section       68  esbprocess.o(.bss)
    .bss                                     0x200001b0   Section       44  nrfx_uart.o(.bss)
    m_cb                                     0x200001b0   Data          44  nrfx_uart.o(.bss)
    .bss                                     0x200001dc   Section       36  nrfx_uarte.o(.bss)
    m_cb                                     0x200001dc   Data          36  nrfx_uarte.o(.bss)
    .bss                                     0x20000200   Section       76  nrfx_gpiote.o(.bss)
    m_cb                                     0x20000200   Data          76  nrfx_gpiote.o(.bss)
    .bss                                     0x2000024c   Section       32  app_uart_fifo.o(.bss)
    m_rx_fifo                                0x2000024c   Data          16  app_uart_fifo.o(.bss)
    m_tx_fifo                                0x2000025c   Data          16  app_uart_fifo.o(.bss)
    .bss                                     0x2000026c   Section      268  app_timer.o(.bss)
    m_op_queue                               0x2000026c   Data         268  app_timer.o(.bss)
    .bss                                     0x20000378   Section     1362  nrf_esb.o(.bss)
    m_config_local                           0x20000378   Data          24  nrf_esb.o(.bss)
    m_tx_fifo_payload                        0x20000390   Data         544  nrf_esb.o(.bss)
    m_tx_fifo                                0x200005b0   Data          44  nrf_esb.o(.bss)
    m_rx_fifo_payload                        0x200005dc   Data         544  nrf_esb.o(.bss)
    m_rx_fifo                                0x200007fc   Data          44  nrf_esb.o(.bss)
    m_tx_payload_buffer                      0x20000828   Data          65  nrf_esb.o(.bss)
    m_rx_payload_buffer                      0x20000869   Data          65  nrf_esb.o(.bss)
    m_rx_pipe_info                           0x200008aa   Data          32  nrf_esb.o(.bss)
    .bss                                     0x200008ca   Section     2064  uartprocess.o(.bss)
    data_array                               0x200008ca   Data          16  uartprocess.o(.bss)
    rx_buf                                   0x200008da   Data        1024  uartprocess.o(.bss)
    tx_buf                                   0x20000cda   Data        1024  uartprocess.o(.bss)
    STACK                                    0x200010e0   Section     8192  arm_startup_nrf52.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv4$E$P$D$K$B$S$7EM$VFPi3$EXTD16$VFPS$VFMA$PE$A:L22UL41UL21$X:L11$S22US41US21$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OSPACE$ROPI$EBA8$MICROLIB$REQ8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  host.o ABSOLUTE
    __Vectors                                0x00000000   Data           4  arm_startup_nrf52.o(RESET)
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    __Vectors_End                            0x00000200   Data           0  arm_startup_nrf52.o(RESET)
    __Vectors_Size                           0x00000200   Number         0  arm_startup_nrf52.o ABSOLUTE
    __main                                   0x00000201   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x00000201   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x00000205   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x00000209   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x00000209   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x00000209   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x00000209   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x00000211   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x00000211   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    Reset_Handler                            0x00000215   Thumb Code     8  arm_startup_nrf52.o(.text)
    NMI_Handler                              0x0000021d   Thumb Code     2  arm_startup_nrf52.o(.text)
    HardFault_Handler                        0x0000021f   Thumb Code     2  arm_startup_nrf52.o(.text)
    MemoryManagement_Handler                 0x00000221   Thumb Code     2  arm_startup_nrf52.o(.text)
    BusFault_Handler                         0x00000223   Thumb Code     2  arm_startup_nrf52.o(.text)
    UsageFault_Handler                       0x00000225   Thumb Code     2  arm_startup_nrf52.o(.text)
    SVC_Handler                              0x00000227   Thumb Code     2  arm_startup_nrf52.o(.text)
    DebugMon_Handler                         0x00000229   Thumb Code     2  arm_startup_nrf52.o(.text)
    PendSV_Handler                           0x0000022b   Thumb Code     2  arm_startup_nrf52.o(.text)
    SysTick_Handler                          0x0000022d   Thumb Code     2  arm_startup_nrf52.o(.text)
    CCM_AAR_IRQHandler                       0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    COMP_LPCOMP_IRQHandler                   0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    ECB_IRQHandler                           0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    FPU_IRQHandler                           0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    I2S_IRQHandler                           0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    MWU_IRQHandler                           0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    NFCT_IRQHandler                          0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    PDM_IRQHandler                           0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    POWER_CLOCK_IRQHandler                   0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    PWM0_IRQHandler                          0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    PWM1_IRQHandler                          0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    PWM2_IRQHandler                          0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    QDEC_IRQHandler                          0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    RNG_IRQHandler                           0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    RTC0_IRQHandler                          0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    RTC2_IRQHandler                          0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    SAADC_IRQHandler                         0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler 0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    SPIM1_SPIS1_TWIM1_TWIS1_SPI1_TWI1_IRQHandler 0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    SPIM2_SPIS2_SPI2_IRQHandler              0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    SWI2_EGU2_IRQHandler                     0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    SWI3_EGU3_IRQHandler                     0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    SWI4_EGU4_IRQHandler                     0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    SWI5_EGU5_IRQHandler                     0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    TEMP_IRQHandler                          0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    TIMER0_IRQHandler                        0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    TIMER1_IRQHandler                        0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    TIMER2_IRQHandler                        0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    TIMER4_IRQHandler                        0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    WDT_IRQHandler                           0x0000022f   Thumb Code     0  arm_startup_nrf52.o(.text)
    __aeabi_memcpy                           0x00000239   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x00000239   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x00000239   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x0000025d   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x0000025d   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x0000025d   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x0000026b   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x0000026b   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x0000026b   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x0000026f   Thumb Code    18  memseta.o(.text)
    memcmp                                   0x00000281   Thumb Code    26  memcmp.o(.text)
    __aeabi_uldivmod                         0x0000029b   Thumb Code    98  uldiv.o(.text)
    __scatterload                            0x000002fd   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x000002fd   Thumb Code     0  init.o(.text)
    __aeabi_llsl                             0x00000321   Thumb Code    30  llshl.o(.text)
    _ll_shift_l                              0x00000321   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x0000033f   Thumb Code    32  llushr.o(.text)
    _ll_ushift_r                             0x0000033f   Thumb Code     0  llushr.o(.text)
    __decompress                             0x0000035f   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x0000035f   Thumb Code    86  __dczerorl2.o(.text)
    Action_Key1                              0x000003b5   Thumb Code     8  host.o(i.Action_Key1)
    EebTxRxSwitch                            0x000003bd   Thumb Code    64  esbprocess.o(i.EebTxRxSwitch)
    GPIOTE_IRQHandler                        0x00000401   Thumb Code   528  nrfx_gpiote.o(i.GPIOTE_IRQHandler)
    PacketSend                               0x00000711   Thumb Code    68  host.o(i.PacketSend)
    Pin_Trigger_handler_1                    0x00000759   Thumb Code    36  gpioprocess.o(i.Pin_Trigger_handler_1)
    Pin_Trigger_handler_2                    0x00000791   Thumb Code    14  gpioprocess.o(i.Pin_Trigger_handler_2)
    RADIO_IRQHandler                         0x000007a1   Thumb Code   102  nrf_esb.o(i.RADIO_IRQHandler)
    RTC1_IRQHandler                          0x00000819   Thumb Code    44  app_timer.o(i.RTC1_IRQHandler)
    SWI0_EGU0_IRQHandler                     0x0000084d   Thumb Code    92  nrf_esb.o(i.SWI0_EGU0_IRQHandler)
    SWI1_EGU1_IRQHandler                     0x000008b1   Thumb Code     8  app_timer.o(i.SWI1_EGU1_IRQHandler)
    SystemCoreClockUpdate                    0x000008b9   Thumb Code     8  system_nrf52.o(i.SystemCoreClockUpdate)
    SystemInit                               0x000008c9   Thumb Code   596  system_nrf52.o(i.SystemInit)
    TIMER3_IRQHandler                        0x00000b61   Thumb Code    28  nrf_esb.o(i.TIMER3_IRQHandler)
    Timer_1S                                 0x00000b89   Thumb Code    86  host.o(i.Timer_1S)
    UARTE0_UART0_IRQHandler                  0x00000c19   Thumb Code    10  nrfx_prs.o(i.UARTE0_UART0_IRQHandler)
    UART_Init                                0x00000c29   Thumb Code    74  uartprocess.o(i.UART_Init)
    __0printf$5                              0x00000c85   Thumb Code    22  printf5.o(i.__0printf$5)
    __1printf$5                              0x00000c85   Thumb Code     0  printf5.o(i.__0printf$5)
    __2printf                                0x00000c85   Thumb Code     0  printf5.o(i.__0printf$5)
    __scatterload_copy                       0x00000ca5   Thumb Code    14  handlers.o(i.__scatterload_copy)
    __scatterload_null                       0x00000cb3   Thumb Code     2  handlers.o(i.__scatterload_null)
    __scatterload_zeroinit                   0x00000cb5   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    app_error_fault_handler                  0x00000f95   Thumb Code    82  app_error_weak.o(i.app_error_fault_handler)
    app_error_handler_bare                   0x00000ff1   Thumb Code    28  app_error.o(i.app_error_handler_bare)
    app_fifo_get                             0x0000100d   Thumb Code    30  app_fifo.o(i.app_fifo_get)
    app_fifo_init                            0x0000102b   Thumb Code    36  app_fifo.o(i.app_fifo_init)
    app_fifo_put                             0x0000104f   Thumb Code    34  app_fifo.o(i.app_fifo_put)
    app_timer_create                         0x00001071   Thumb Code    56  app_timer.o(i.app_timer_create)
    app_timer_init                           0x000010ad   Thumb Code    70  app_timer.o(i.app_timer_init)
    app_timer_start                          0x00001109   Thumb Code    78  app_timer.o(i.app_timer_start)
    app_uart_get                             0x0000115d   Thumb Code    66  app_uart_fifo.o(i.app_uart_get)
    app_uart_init                            0x000011b1   Thumb Code   188  app_uart_fifo.o(i.app_uart_init)
    app_uart_put                             0x0000128d   Thumb Code    90  app_uart_fifo.o(i.app_uart_put)
    app_util_critical_region_enter           0x000012f9   Thumb Code    10  app_util_platform.o(i.app_util_critical_region_enter)
    app_util_critical_region_exit            0x00001303   Thumb Code    10  app_util_platform.o(i.app_util_critical_region_exit)
    app_util_disable_irq                     0x0000130d   Thumb Code    14  app_util_platform.o(i.app_util_disable_irq)
    app_util_enable_irq                      0x00001321   Thumb Code    20  app_util_platform.o(i.app_util_enable_irq)
    clocks_start                             0x000016a1   Thumb Code    24  host.o(i.clocks_start)
    esb_init                                 0x00001a65   Thumb Code   156  esbprocess.o(i.esb_init)
    esb_send_packet_timer_callback           0x00001b19   Thumb Code    10  host.o(i.esb_send_packet_timer_callback)
    fputc                                    0x00001bcd   Thumb Code    16  retarget.o(i.fputc)
    gpio_init                                0x00001bdd   Thumb Code   164  gpioprocess.o(i.gpio_init)
    main                                     0x00001f69   Thumb Code    82  host.o(i.main)
    nrf_drv_uart_init                        0x00002031   Thumb Code   118  nrf_drv_uart.o(i.nrf_drv_uart_init)
    nrf_esb_disable                          0x00002145   Thumb Code    56  nrf_esb.o(i.nrf_esb_disable)
    nrf_esb_event_handler                    0x00002195   Thumb Code   256  host.o(i.nrf_esb_event_handler)
    nrf_esb_flush_tx                         0x000022cd   Thumb Code    42  nrf_esb.o(i.nrf_esb_flush_tx)
    nrf_esb_init                             0x00002341   Thumb Code   200  nrf_esb.o(i.nrf_esb_init)
    nrf_esb_read_rx_payload                  0x00002439   Thumb Code   164  nrf_esb.o(i.nrf_esb_read_rx_payload)
    nrf_esb_set_base_address_0               0x000024e5   Thumb Code   102  nrf_esb.o(i.nrf_esb_set_base_address_0)
    nrf_esb_set_base_address_1               0x00002561   Thumb Code   170  nrf_esb.o(i.nrf_esb_set_base_address_1)
    nrf_esb_set_prefixes                     0x00002621   Thumb Code   166  nrf_esb.o(i.nrf_esb_set_prefixes)
    nrf_esb_skip_tx                          0x000026dd   Thumb Code    74  nrf_esb.o(i.nrf_esb_skip_tx)
    nrf_esb_start_rx                         0x00002731   Thumb Code   128  nrf_esb.o(i.nrf_esb_start_rx)
    nrf_esb_start_tx                         0x000027d9   Thumb Code    36  nrf_esb.o(i.nrf_esb_start_tx)
    nrf_esb_stop_rx                          0x00002805   Thumb Code    66  nrf_esb.o(i.nrf_esb_stop_rx)
    nrf_esb_write_payload                    0x00002859   Thumb Code   220  nrf_esb.o(i.nrf_esb_write_payload)
    nrfx_gpiote_in_event_enable              0x00002c61   Thumb Code   164  nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable)
    nrfx_gpiote_in_init                      0x00002d0d   Thumb Code   232  nrfx_gpiote.o(i.nrfx_gpiote_in_init)
    nrfx_gpiote_init                         0x00002e01   Thumb Code   178  nrfx_gpiote.o(i.nrfx_gpiote_init)
    nrfx_prs_acquire                         0x00002ed9   Thumb Code    72  nrfx_prs.o(i.nrfx_prs_acquire)
    nrfx_uart_0_irq_handler                  0x00002f21   Thumb Code    12  nrfx_uart.o(i.nrfx_uart_0_irq_handler)
    nrfx_uart_init                           0x00002f35   Thumb Code   128  nrfx_uart.o(i.nrfx_uart_init)
    nrfx_uart_rx                             0x00002fbd   Thumb Code   286  nrfx_uart.o(i.nrfx_uart_rx)
    nrfx_uart_tx                             0x000030e1   Thumb Code   134  nrfx_uart.o(i.nrfx_uart_tx)
    nrfx_uart_tx_in_progress                 0x0000316d   Thumb Code    30  nrfx_uart.o(i.nrfx_uart_tx_in_progress)
    nrfx_uarte_0_irq_handler                 0x00003191   Thumb Code    12  nrfx_uarte.o(i.nrfx_uarte_0_irq_handler)
    nrfx_uarte_init                          0x000031a5   Thumb Code   120  nrfx_uarte.o(i.nrfx_uarte_init)
    nrfx_uarte_rx                            0x00003225   Thumb Code   306  nrfx_uarte.o(i.nrfx_uarte_rx)
    nrfx_uarte_tx                            0x0000335d   Thumb Code   162  nrfx_uarte.o(i.nrfx_uarte_tx)
    nrfx_uarte_tx_in_progress                0x00003405   Thumb Code    26  nrfx_uarte.o(i.nrfx_uarte_tx_in_progress)
    uart_event_handle                        0x00004151   Thumb Code   284  uartprocess.o(i.uart_event_handle)
    Region$$Table$$Base                      0x000049b0   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x000049d0   Number         0  anon$$obj.o(Region$$Table)
    UICR_ADDR_0x20C                          0x1000120c   Data           4  gpioprocess.o(.ARM.__AT_0x1000120C)
    KeyDebunseTick                           0x20000000   Data           1  gpioprocess.o(.data)
    PacketSendCnt                            0x20000004   Data           4  host.o(.data)
    PacketSendOKCnt                          0x20000008   Data           4  host.o(.data)
    PacketSentNGCnt                          0x2000000c   Data           4  host.o(.data)
    PacketReceiveOKCnt                       0x20000010   Data           4  host.o(.data)
    PacketReceiveNGCnt                       0x20000014   Data           4  host.o(.data)
    RxLedFlashCnt                            0x20000018   Data           4  host.o(.data)
    TriggerPressed                           0x2000001c   Data           1  host.o(.data)
    TriggerPressedFlag                       0x2000001d   Data           1  host.o(.data)
    tx_payload                               0x20000030   Data          68  esbprocess.o(.data)
    nrf_esb_config                           0x20000074   Data          24  esbprocess.o(.data)
    nrf_drv_uart_use_easy_dma                0x20000094   Data           1  nrf_drv_uart.o(.data)
    __stdout                                 0x200000d4   Data           4  retarget.o(.data)
    __stdin                                  0x200000d8   Data           4  retarget.o(.data)
    SystemCoreClock                          0x20000128   Data           4  system_nrf52.o(.data)
    rx_payload                               0x2000016c   Data          68  esbprocess.o(.bss)
    __initial_sp                             0x200030e0   Data           0  arm_startup_nrf52.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x00000201

  Load Region LR_IROM1 (Base: 0x00000000, Size: 0x00004afc, Max: 0x00080000, ABSOLUTE, COMPRESSED[0x00004a48])

    Execution Region ER_IROM1 (Exec base: 0x00000000, Load base: 0x00000000, Size: 0x000049d0, Max: 0x00080000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00000000   0x00000000   0x00000200   Data   RO         2947    RESET               arm_startup_nrf52.o
    0x00000200   0x00000200   0x00000000   Code   RO         3043  * .ARM.Collect$$$$00000000  mc_w.l(entry.o)
    0x00000200   0x00000200   0x00000004   Code   RO         3317    .ARM.Collect$$$$00000001  mc_w.l(entry2.o)
    0x00000204   0x00000204   0x00000004   Code   RO         3320    .ARM.Collect$$$$00000004  mc_w.l(entry5.o)
    0x00000208   0x00000208   0x00000000   Code   RO         3322    .ARM.Collect$$$$00000008  mc_w.l(entry7b.o)
    0x00000208   0x00000208   0x00000000   Code   RO         3324    .ARM.Collect$$$$0000000A  mc_w.l(entry8b.o)
    0x00000208   0x00000208   0x00000008   Code   RO         3325    .ARM.Collect$$$$0000000B  mc_w.l(entry9a.o)
    0x00000210   0x00000210   0x00000000   Code   RO         3327    .ARM.Collect$$$$0000000D  mc_w.l(entry10a.o)
    0x00000210   0x00000210   0x00000000   Code   RO         3329    .ARM.Collect$$$$0000000F  mc_w.l(entry11a.o)
    0x00000210   0x00000210   0x00000004   Code   RO         3318    .ARM.Collect$$$$00002712  mc_w.l(entry2.o)
    0x00000214   0x00000214   0x00000024   Code   RO         2948    .text               arm_startup_nrf52.o
    0x00000238   0x00000238   0x00000024   Code   RO         3046    .text               mc_w.l(memcpya.o)
    0x0000025c   0x0000025c   0x00000024   Code   RO         3048    .text               mc_w.l(memseta.o)
    0x00000280   0x00000280   0x0000001a   Code   RO         3052    .text               mc_w.l(memcmp.o)
    0x0000029a   0x0000029a   0x00000062   Code   RO         3333    .text               mc_w.l(uldiv.o)
    0x000002fc   0x000002fc   0x00000024   Code   RO         3346    .text               mc_w.l(init.o)
    0x00000320   0x00000320   0x0000001e   Code   RO         3348    .text               mc_w.l(llshl.o)
    0x0000033e   0x0000033e   0x00000020   Code   RO         3350    .text               mc_w.l(llushr.o)
    0x0000035e   0x0000035e   0x00000056   Code   RO         3364    .text               mc_w.l(__dczerorl2.o)
    0x000003b4   0x000003b4   0x00000008   Code   RO          227    i.Action_Key1       host.o
    0x000003bc   0x000003bc   0x00000044   Code   RO          369    i.EebTxRxSwitch     esbprocess.o
    0x00000400   0x00000400   0x0000021c   Code   RO         1129    i.GPIOTE_IRQHandler  nrfx_gpiote.o
    0x0000061c   0x0000061c   0x00000018   Code   RO         2261    i.NVIC_ClearPendingIRQ  app_timer.o
    0x00000634   0x00000634   0x00000018   Code   RO         2562    i.NVIC_ClearPendingIRQ  nrf_esb.o
    0x0000064c   0x0000064c   0x00000018   Code   RO         2563    i.NVIC_DisableIRQ   nrf_esb.o
    0x00000664   0x00000664   0x00000016   Code   RO         2262    i.NVIC_EnableIRQ    app_timer.o
    0x0000067a   0x0000067a   0x00000016   Code   RO         2564    i.NVIC_EnableIRQ    nrf_esb.o
    0x00000690   0x00000690   0x00000018   Code   RO         2263    i.NVIC_SetPendingIRQ  app_timer.o
    0x000006a8   0x000006a8   0x00000018   Code   RO         2565    i.NVIC_SetPendingIRQ  nrf_esb.o
    0x000006c0   0x000006c0   0x00000028   Code   RO         2264    i.NVIC_SetPriority  app_timer.o
    0x000006e8   0x000006e8   0x00000028   Code   RO         2566    i.NVIC_SetPriority  nrf_esb.o
    0x00000710   0x00000710   0x00000048   Code   RO          228    i.PacketSend        host.o
    0x00000758   0x00000758   0x00000038   Code   RO            4    i.Pin_Trigger_handler_1  gpioprocess.o
    0x00000790   0x00000790   0x0000000e   Code   RO            5    i.Pin_Trigger_handler_2  gpioprocess.o
    0x0000079e   0x0000079e   0x00000002   PAD
    0x000007a0   0x000007a0   0x00000078   Code   RO         2567    i.RADIO_IRQHandler  nrf_esb.o
    0x00000818   0x00000818   0x00000034   Code   RO         2265    i.RTC1_IRQHandler   app_timer.o
    0x0000084c   0x0000084c   0x00000064   Code   RO         2568    i.SWI0_EGU0_IRQHandler  nrf_esb.o
    0x000008b0   0x000008b0   0x00000008   Code   RO         2266    i.SWI1_EGU1_IRQHandler  app_timer.o
    0x000008b8   0x000008b8   0x00000010   Code   RO         2955    i.SystemCoreClockUpdate  system_nrf52.o
    0x000008c8   0x000008c8   0x00000298   Code   RO         2956    i.SystemInit        system_nrf52.o
    0x00000b60   0x00000b60   0x00000028   Code   RO         2569    i.TIMER3_IRQHandler  nrf_esb.o
    0x00000b88   0x00000b88   0x00000090   Code   RO          229    i.Timer_1S          host.o
    0x00000c18   0x00000c18   0x00000010   Code   RO          611    i.UARTE0_UART0_IRQHandler  nrfx_prs.o
    0x00000c28   0x00000c28   0x0000005c   Code   RO         2905    i.UART_Init         uartprocess.o
    0x00000c84   0x00000c84   0x00000020   Code   RO         3189    i.__0printf$5       mc_w.l(printf5.o)
    0x00000ca4   0x00000ca4   0x0000000e   Code   RO         3358    i.__scatterload_copy  mc_w.l(handlers.o)
    0x00000cb2   0x00000cb2   0x00000002   Code   RO         3359    i.__scatterload_null  mc_w.l(handlers.o)
    0x00000cb4   0x00000cb4   0x0000000e   Code   RO         3360    i.__scatterload_zeroinit  mc_w.l(handlers.o)
    0x00000cc2   0x00000cc2   0x00000002   PAD
    0x00000cc4   0x00000cc4   0x000002c0   Code   RO         3196    i._printf_core      mc_w.l(printf5.o)
    0x00000f84   0x00000f84   0x0000000e   Code   RO         2570    i.addr_conv         nrf_esb.o
    0x00000f92   0x00000f92   0x00000002   PAD
    0x00000f94   0x00000f94   0x0000005c   Code   RO         1507    i.app_error_fault_handler  app_error_weak.o
    0x00000ff0   0x00000ff0   0x0000001c   Code   RO         1447    i.app_error_handler_bare  app_error.o
    0x0000100c   0x0000100c   0x0000001e   Code   RO         1545    i.app_fifo_get      app_fifo.o
    0x0000102a   0x0000102a   0x00000024   Code   RO         1546    i.app_fifo_init     app_fifo.o
    0x0000104e   0x0000104e   0x00000022   Code   RO         1548    i.app_fifo_put      app_fifo.o
    0x00001070   0x00001070   0x0000003c   Code   RO         2269    i.app_timer_create  app_timer.o
    0x000010ac   0x000010ac   0x0000005c   Code   RO         2270    i.app_timer_init    app_timer.o
    0x00001108   0x00001108   0x00000054   Code   RO         2273    i.app_timer_start   app_timer.o
    0x0000115c   0x0000115c   0x00000054   Code   RO         1632    i.app_uart_get      app_uart_fifo.o
    0x000011b0   0x000011b0   0x000000dc   Code   RO         1633    i.app_uart_init     app_uart_fifo.o
    0x0000128c   0x0000128c   0x0000006c   Code   RO         1634    i.app_uart_put      app_uart_fifo.o
    0x000012f8   0x000012f8   0x0000000a   Code   RO         1718    i.app_util_critical_region_enter  app_util_platform.o
    0x00001302   0x00001302   0x0000000a   Code   RO         1719    i.app_util_critical_region_exit  app_util_platform.o
    0x0000130c   0x0000130c   0x00000014   Code   RO         1720    i.app_util_disable_irq  app_util_platform.o
    0x00001320   0x00001320   0x00000018   Code   RO         1721    i.app_util_enable_irq  app_util_platform.o
    0x00001338   0x00001338   0x0000013c   Code   RO         2571    i.apply_address_workarounds  nrf_esb.o
    0x00001474   0x00001474   0x0000007c   Code   RO          671    i.apply_config      nrfx_uart.o
    0x000014f0   0x000014f0   0x0000007c   Code   RO          920    i.apply_config      nrfx_uarte.o
    0x0000156c   0x0000156c   0x0000000c   Code   RO         2572    i.bytewise_bit_swap  nrf_esb.o
    0x00001578   0x00001578   0x00000020   Code   RO         1130    i.channel_free      nrfx_gpiote.o
    0x00001598   0x00001598   0x00000010   Code   RO         1131    i.channel_handler_get  nrfx_gpiote.o
    0x000015a8   0x000015a8   0x00000080   Code   RO         1132    i.channel_port_alloc  nrfx_gpiote.o
    0x00001628   0x00001628   0x0000000c   Code   RO         1133    i.channel_port_get  nrfx_gpiote.o
    0x00001634   0x00001634   0x0000006c   Code   RO         2573    i.clear_events_restart_rx  nrf_esb.o
    0x000016a0   0x000016a0   0x0000001c   Code   RO          230    i.clocks_start      host.o
    0x000016bc   0x000016bc   0x00000090   Code   RO         2276    i.compare_reg_update  app_timer.o
    0x0000174c   0x0000174c   0x00000064   Code   RO         2277    i.elapsed_ticks_acquire  app_timer.o
    0x000017b0   0x000017b0   0x00000054   Code   RO         2957    i.errata_108        system_nrf52.o
    0x00001804   0x00001804   0x00000054   Code   RO         2958    i.errata_12         system_nrf52.o
    0x00001858   0x00001858   0x00000054   Code   RO         2959    i.errata_136        system_nrf52.o
    0x000018ac   0x000018ac   0x00000030   Code   RO         2960    i.errata_16         system_nrf52.o
    0x000018dc   0x000018dc   0x00000020   Code   RO         2961    i.errata_182        system_nrf52.o
    0x000018fc   0x000018fc   0x00000054   Code   RO         2962    i.errata_31         system_nrf52.o
    0x00001950   0x00001950   0x00000030   Code   RO         2963    i.errata_32         system_nrf52.o
    0x00001980   0x00001980   0x00000054   Code   RO         2964    i.errata_36         system_nrf52.o
    0x000019d4   0x000019d4   0x00000030   Code   RO         2965    i.errata_37         system_nrf52.o
    0x00001a04   0x00001a04   0x00000030   Code   RO         2966    i.errata_57         system_nrf52.o
    0x00001a34   0x00001a34   0x00000030   Code   RO         2967    i.errata_66         system_nrf52.o
    0x00001a64   0x00001a64   0x000000b4   Code   RO          370    i.esb_init          esbprocess.o
    0x00001b18   0x00001b18   0x0000000a   Code   RO          231    i.esb_send_packet_timer_callback  host.o
    0x00001b22   0x00001b22   0x00000002   PAD
    0x00001b24   0x00001b24   0x00000058   Code   RO         2278    i.expired_timers_handler  app_timer.o
    0x00001b7c   0x00001b7c   0x00000018   Code   RO         1551    i.fifo_get          app_fifo.o
    0x00001b94   0x00001b94   0x0000000a   Code   RO         1552    i.fifo_length       app_fifo.o
    0x00001b9e   0x00001b9e   0x0000000a   Code   RO         1635    i.fifo_length       app_uart_fifo.o
    0x00001ba8   0x00001ba8   0x00000012   Code   RO         1553    i.fifo_peek         app_fifo.o
    0x00001bba   0x00001bba   0x00000012   Code   RO         1554    i.fifo_put          app_fifo.o
    0x00001bcc   0x00001bcc   0x00000010   Code   RO         2490    i.fputc             retarget.o
    0x00001bdc   0x00001bdc   0x000000b0   Code   RO            6    i.gpio_init         gpioprocess.o
    0x00001c8c   0x00001c8c   0x0000004c   Code   RO         2574    i.initialize_fifos  nrf_esb.o
    0x00001cd8   0x00001cd8   0x000000a0   Code   RO          673    i.interrupts_enable  nrfx_uart.o
    0x00001d78   0x00001d78   0x000000b4   Code   RO          922    i.interrupts_enable  nrfx_uarte.o
    0x00001e2c   0x00001e2c   0x0000013c   Code   RO         2279    i.list_insertions_handler  app_timer.o
    0x00001f68   0x00001f68   0x0000006c   Code   RO          232    i.main              host.o
    0x00001fd4   0x00001fd4   0x00000016   Code   RO         1134    i.nrf_bitmask_bit_is_set  nrfx_gpiote.o
    0x00001fea   0x00001fea   0x00000016   Code   RO         1135    i.nrf_bitmask_bit_set  nrfx_gpiote.o
    0x00002000   0x00002000   0x00000030   Code   RO          233    i.nrf_delay_ms      host.o
    0x00002030   0x00002030   0x0000008c   Code   RO          559    i.nrf_drv_uart_init  nrf_drv_uart.o
    0x000020bc   0x000020bc   0x00000044   Code   RO         1636    i.nrf_drv_uart_rx   app_uart_fifo.o
    0x00002100   0x00002100   0x00000044   Code   RO         1637    i.nrf_drv_uart_tx   app_uart_fifo.o
    0x00002144   0x00002144   0x00000050   Code   RO         2575    i.nrf_esb_disable   nrf_esb.o
    0x00002194   0x00002194   0x00000138   Code   RO          234    i.nrf_esb_event_handler  host.o
    0x000022cc   0x000022cc   0x00000034   Code   RO         2578    i.nrf_esb_flush_tx  nrf_esb.o
    0x00002300   0x00002300   0x00000040   Code   RO         2579    i.nrf_esb_get_clear_interrupts  nrf_esb.o
    0x00002340   0x00002340   0x000000f8   Code   RO         2581    i.nrf_esb_init      nrf_esb.o
    0x00002438   0x00002438   0x000000ac   Code   RO         2584    i.nrf_esb_read_rx_payload  nrf_esb.o
    0x000024e4   0x000024e4   0x0000007c   Code   RO         2587    i.nrf_esb_set_base_address_0  nrf_esb.o
    0x00002560   0x00002560   0x000000c0   Code   RO         2588    i.nrf_esb_set_base_address_1  nrf_esb.o
    0x00002620   0x00002620   0x000000bc   Code   RO         2590    i.nrf_esb_set_prefixes  nrf_esb.o
    0x000026dc   0x000026dc   0x00000054   Code   RO         2595    i.nrf_esb_skip_tx   nrf_esb.o
    0x00002730   0x00002730   0x000000a8   Code   RO         2596    i.nrf_esb_start_rx  nrf_esb.o
    0x000027d8   0x000027d8   0x0000002c   Code   RO         2597    i.nrf_esb_start_tx  nrf_esb.o
    0x00002804   0x00002804   0x00000054   Code   RO         2598    i.nrf_esb_stop_rx   nrf_esb.o
    0x00002858   0x00002858   0x000000f0   Code   RO         2601    i.nrf_esb_write_payload  nrf_esb.o
    0x00002948   0x00002948   0x00000028   Code   RO          674    i.nrf_gpio_cfg      nrfx_uart.o
    0x00002970   0x00002970   0x00000028   Code   RO          923    i.nrf_gpio_cfg      nrfx_uarte.o
    0x00002998   0x00002998   0x00000028   Code   RO         1136    i.nrf_gpio_cfg      nrfx_gpiote.o
    0x000029c0   0x000029c0   0x0000001a   Code   RO          676    i.nrf_gpio_cfg_input  nrfx_uart.o
    0x000029da   0x000029da   0x0000001a   Code   RO          925    i.nrf_gpio_cfg_input  nrfx_uarte.o
    0x000029f4   0x000029f4   0x00000030   Code   RO            7    i.nrf_gpio_cfg_output  gpioprocess.o
    0x00002a24   0x00002a24   0x00000018   Code   RO          677    i.nrf_gpio_cfg_output  nrfx_uart.o
    0x00002a3c   0x00002a3c   0x00000018   Code   RO          926    i.nrf_gpio_cfg_output  nrfx_uarte.o
    0x00002a54   0x00002a54   0x00000032   Code   RO         1138    i.nrf_gpio_cfg_sense_set  nrfx_gpiote.o
    0x00002a86   0x00002a86   0x00000016   Code   RO            8    i.nrf_gpio_pin_clear  gpioprocess.o
    0x00002a9c   0x00002a9c   0x00000018   Code   RO         1140    i.nrf_gpio_pin_read  nrfx_gpiote.o
    0x00002ab4   0x00002ab4   0x00000016   Code   RO          678    i.nrf_gpio_pin_set  nrfx_uart.o
    0x00002aca   0x00002aca   0x00000016   Code   RO          927    i.nrf_gpio_pin_set  nrfx_uarte.o
    0x00002ae0   0x00002ae0   0x00000022   Code   RO            9    i.nrf_gpio_pin_toggle  gpioprocess.o
    0x00002b02   0x00002b02   0x00000002   PAD
    0x00002b04   0x00002b04   0x00000028   Code   RO         1142    i.nrf_gpio_ports_read  nrfx_gpiote.o
    0x00002b2c   0x00002b2c   0x0000000c   Code   RO         1143    i.nrf_gpiote_event_addr_get  nrfx_gpiote.o
    0x00002b38   0x00002b38   0x0000001c   Code   RO         1144    i.nrf_gpiote_event_clear  nrfx_gpiote.o
    0x00002b54   0x00002b54   0x00000016   Code   RO         1145    i.nrf_gpiote_event_is_set  nrfx_gpiote.o
    0x00002b6a   0x00002b6a   0x00000002   PAD
    0x00002b6c   0x00002b6c   0x0000000c   Code   RO         1146    i.nrf_gpiote_int_enable  nrfx_gpiote.o
    0x00002b78   0x00002b78   0x0000000c   Code   RO          679    i.nrf_uart_errorsrc_get_and_clear  nrfx_uart.o
    0x00002b84   0x00002b84   0x0000000e   Code   RO          680    i.nrf_uart_event_check  nrfx_uart.o
    0x00002b92   0x00002b92   0x0000000e   Code   RO          681    i.nrf_uart_event_clear  nrfx_uart.o
    0x00002ba0   0x00002ba0   0x0000000a   Code   RO          682    i.nrf_uart_hwfc_pins_set  nrfx_uart.o
    0x00002baa   0x00002baa   0x00000006   Code   RO          683    i.nrf_uart_int_disable  nrfx_uart.o
    0x00002bb0   0x00002bb0   0x00000006   Code   RO          684    i.nrf_uart_int_enable  nrfx_uart.o
    0x00002bb6   0x00002bb6   0x00000012   Code   RO          685    i.nrf_uart_int_enable_check  nrfx_uart.o
    0x00002bc8   0x00002bc8   0x00000006   Code   RO          686    i.nrf_uart_task_trigger  nrfx_uart.o
    0x00002bce   0x00002bce   0x0000000a   Code   RO          687    i.nrf_uart_txrx_pins_set  nrfx_uart.o
    0x00002bd8   0x00002bd8   0x0000000c   Code   RO          928    i.nrf_uarte_errorsrc_get_and_clear  nrfx_uarte.o
    0x00002be4   0x00002be4   0x0000000e   Code   RO          929    i.nrf_uarte_event_check  nrfx_uarte.o
    0x00002bf2   0x00002bf2   0x0000000e   Code   RO          930    i.nrf_uarte_event_clear  nrfx_uarte.o
    0x00002c00   0x00002c00   0x0000000c   Code   RO          931    i.nrf_uarte_hwfc_pins_set  nrfx_uarte.o
    0x00002c0c   0x00002c0c   0x00000006   Code   RO          932    i.nrf_uarte_int_disable  nrfx_uarte.o
    0x00002c12   0x00002c12   0x00000006   Code   RO          933    i.nrf_uarte_int_enable  nrfx_uarte.o
    0x00002c18   0x00002c18   0x0000000a   Code   RO          934    i.nrf_uarte_rx_amount_get  nrfx_uarte.o
    0x00002c22   0x00002c22   0x00000006   Code   RO          935    i.nrf_uarte_task_trigger  nrfx_uarte.o
    0x00002c28   0x00002c28   0x0000000e   Code   RO          936    i.nrf_uarte_txrx_pins_set  nrfx_uarte.o
    0x00002c36   0x00002c36   0x00000002   PAD
    0x00002c38   0x00002c38   0x00000018   Code   RO         2280    i.nrfx_coredep_delay_us  app_timer.o
    0x00002c50   0x00002c50   0x00000008   Code   RO          688    i.nrfx_get_irq_number  nrfx_uart.o
    0x00002c58   0x00002c58   0x00000008   Code   RO          937    i.nrfx_get_irq_number  nrfx_uarte.o
    0x00002c60   0x00002c60   0x000000ac   Code   RO         1153    i.nrfx_gpiote_in_event_enable  nrfx_gpiote.o
    0x00002d0c   0x00002d0c   0x000000f4   Code   RO         1154    i.nrfx_gpiote_in_init  nrfx_gpiote.o
    0x00002e00   0x00002e00   0x000000c4   Code   RO         1157    i.nrfx_gpiote_init  nrfx_gpiote.o
    0x00002ec4   0x00002ec4   0x00000014   Code   RO          938    i.nrfx_is_in_ram    nrfx_uarte.o
    0x00002ed8   0x00002ed8   0x00000048   Code   RO          612    i.nrfx_prs_acquire  nrfx_prs.o
    0x00002f20   0x00002f20   0x00000014   Code   RO          689    i.nrfx_uart_0_irq_handler  nrfx_uart.o
    0x00002f34   0x00002f34   0x00000088   Code   RO          691    i.nrfx_uart_init    nrfx_uart.o
    0x00002fbc   0x00002fbc   0x00000124   Code   RO          692    i.nrfx_uart_rx      nrfx_uart.o
    0x000030e0   0x000030e0   0x0000008c   Code   RO          697    i.nrfx_uart_tx      nrfx_uart.o
    0x0000316c   0x0000316c   0x00000024   Code   RO          699    i.nrfx_uart_tx_in_progress  nrfx_uart.o
    0x00003190   0x00003190   0x00000014   Code   RO          939    i.nrfx_uarte_0_irq_handler  nrfx_uarte.o
    0x000031a4   0x000031a4   0x00000080   Code   RO          941    i.nrfx_uarte_init   nrfx_uarte.o
    0x00003224   0x00003224   0x00000138   Code   RO          942    i.nrfx_uarte_rx     nrfx_uarte.o
    0x0000335c   0x0000335c   0x000000a8   Code   RO          945    i.nrfx_uarte_tx     nrfx_uarte.o
    0x00003404   0x00003404   0x00000020   Code   RO          947    i.nrfx_uarte_tx_in_progress  nrfx_uarte.o
    0x00003424   0x00003424   0x000001d8   Code   RO         2602    i.on_radio_disabled_rx  nrf_esb.o
    0x000035fc   0x000035fc   0x00000050   Code   RO         2603    i.on_radio_disabled_rx_ack  nrf_esb.o
    0x0000364c   0x0000364c   0x000000a4   Code   RO         2604    i.on_radio_disabled_tx  nrf_esb.o
    0x000036f0   0x000036f0   0x00000040   Code   RO         2605    i.on_radio_disabled_tx_noack  nrf_esb.o
    0x00003730   0x00003730   0x00000170   Code   RO         2606    i.on_radio_disabled_tx_wait_for_ack  nrf_esb.o
    0x000038a0   0x000038a0   0x00000014   Code   RO         1174    i.pin_configured_set  nrfx_gpiote.o
    0x000038b4   0x000038b4   0x0000001c   Code   RO         1175    i.pin_in_use_by_gpiote  nrfx_gpiote.o
    0x000038d0   0x000038d0   0x00000018   Code   RO         1176    i.pin_in_use_by_port  nrfx_gpiote.o
    0x000038e8   0x000038e8   0x00000020   Code   RO         1177    i.pin_in_use_by_te  nrfx_gpiote.o
    0x00003908   0x00003908   0x0000000c   Code   RO         1178    i.pin_in_use_clear  nrfx_gpiote.o
    0x00003914   0x00003914   0x00000050   Code   RO         2607    i.ppi_init          nrf_esb.o
    0x00003964   0x00003964   0x00000018   Code   RO          614    i.prs_box_get       nrfx_prs.o
    0x0000397c   0x0000397c   0x0000001c   Code   RO         2608    i.reset_fifos       nrf_esb.o
    0x00003998   0x00003998   0x0000000c   Code   RO         2281    i.rtc1_compare0_set  app_timer.o
    0x000039a4   0x000039a4   0x0000000c   Code   RO         2282    i.rtc1_counter_get  app_timer.o
    0x000039b0   0x000039b0   0x00000018   Code   RO         2283    i.rtc1_init         app_timer.o
    0x000039c8   0x000039c8   0x0000003c   Code   RO         2284    i.rtc1_start        app_timer.o
    0x00003a04   0x00003a04   0x00000058   Code   RO         2285    i.rtc1_stop         app_timer.o
    0x00003a5c   0x00003a5c   0x0000003e   Code   RO          702    i.rx_byte           nrfx_uart.o
    0x00003a9a   0x00003a9a   0x0000001c   Code   RO          703    i.rx_done_event     nrfx_uart.o
    0x00003ab6   0x00003ab6   0x00000020   Code   RO          950    i.rx_done_event     nrfx_uarte.o
    0x00003ad6   0x00003ad6   0x00000022   Code   RO          704    i.rx_enable         nrfx_uart.o
    0x00003af8   0x00003af8   0x000000e8   Code   RO         2609    i.rx_fifo_push_rfbuf  nrf_esb.o
    0x00003be0   0x00003be0   0x000001b4   Code   RO         2610    i.start_tx_transaction  nrf_esb.o
    0x00003d94   0x00003d94   0x00000020   Code   RO         2611    i.sys_timer_init    nrf_esb.o
    0x00003db4   0x00003db4   0x0000000a   Code   RO         2286    i.ticks_diff_get    app_timer.o
    0x00003dbe   0x00003dbe   0x0000000c   Code   RO         2287    i.timeout_handler_exec  app_timer.o
    0x00003dca   0x00003dca   0x00000002   PAD
    0x00003dcc   0x00003dcc   0x00000050   Code   RO         2288    i.timer_list_handler  app_timer.o
    0x00003e1c   0x00003e1c   0x0000000a   Code   RO         2289    i.timer_list_handler_sched  app_timer.o
    0x00003e26   0x00003e26   0x00000002   PAD
    0x00003e28   0x00003e28   0x00000068   Code   RO         2290    i.timer_list_insert  app_timer.o
    0x00003e90   0x00003e90   0x00000088   Code   RO         2291    i.timer_list_remove  app_timer.o
    0x00003f18   0x00003f18   0x00000058   Code   RO         2292    i.timer_start_op_schedule  app_timer.o
    0x00003f70   0x00003f70   0x00000098   Code   RO         2294    i.timer_timeouts_check  app_timer.o
    0x00004008   0x00004008   0x0000000a   Code   RO         2295    i.timer_timeouts_check_sched  app_timer.o
    0x00004012   0x00004012   0x00000002   PAD
    0x00004014   0x00004014   0x00000070   Code   RO          235    i.timers_init       host.o
    0x00004084   0x00004084   0x0000002c   Code   RO          236    i.timers_start      host.o
    0x000040b0   0x000040b0   0x00000036   Code   RO          705    i.tx_blocking       nrfx_uart.o
    0x000040e6   0x000040e6   0x00000026   Code   RO          706    i.tx_byte           nrfx_uart.o
    0x0000410c   0x0000410c   0x00000020   Code   RO          707    i.tx_done_event     nrfx_uart.o
    0x0000412c   0x0000412c   0x00000024   Code   RO          951    i.tx_done_event     nrfx_uarte.o
    0x00004150   0x00004150   0x00000194   Code   RO         2906    i.uart_event_handle  uartprocess.o
    0x000042e4   0x000042e4   0x000000d4   Code   RO         1638    i.uart_event_handler  app_uart_fifo.o
    0x000043b8   0x000043b8   0x00000038   Code   RO          560    i.uart_evt_handler  nrf_drv_uart.o
    0x000043f0   0x000043f0   0x0000014c   Code   RO          708    i.uart_irq_handler  nrfx_uart.o
    0x0000453c   0x0000453c   0x00000038   Code   RO          561    i.uarte_evt_handler  nrf_drv_uart.o
    0x00004574   0x00004574   0x0000010c   Code   RO          952    i.uarte_irq_handler  nrfx_uarte.o
    0x00004680   0x00004680   0x00000054   Code   RO         2612    i.update_radio_addresses  nrf_esb.o
    0x000046d4   0x000046d4   0x0000004c   Code   RO         2613    i.update_radio_bitrate  nrf_esb.o
    0x00004720   0x00004720   0x00000050   Code   RO         2614    i.update_radio_crc  nrf_esb.o
    0x00004770   0x00004770   0x00000040   Code   RO         2615    i.update_radio_parameters  nrf_esb.o
    0x000047b0   0x000047b0   0x00000034   Code   RO         2616    i.update_radio_protocol  nrf_esb.o
    0x000047e4   0x000047e4   0x00000014   Code   RO         2617    i.update_radio_tx_power  nrf_esb.o
    0x000047f8   0x000047f8   0x00000030   Code   RO         2618    i.update_rf_payload_format_esb  nrf_esb.o
    0x00004828   0x00004828   0x0000002c   Code   RO         2619    i.update_rf_payload_format_esb_dpl  nrf_esb.o
    0x00004854   0x00004854   0x0000003c   Code   RO         2296    i.user_op_alloc     app_timer.o
    0x00004890   0x00004890   0x0000000c   Code   RO         2297    i.user_op_enque     app_timer.o
    0x0000489c   0x0000489c   0x00000003   Data   RO           11    .constdata          gpioprocess.o
    0x0000489f   0x0000489f   0x00000001   PAD
    0x000048a0   0x000048a0   0x00000016   Data   RO          238    .constdata          host.o
    0x000048b6   0x000048b6   0x00000002   PAD
    0x000048b8   0x000048b8   0x0000002e   Data   RO          710    .constdata          nrfx_uart.o
    0x000048e6   0x000048e6   0x00000002   PAD
    0x000048e8   0x000048e8   0x00000030   Data   RO          954    .constdata          nrfx_uarte.o
    0x00004918   0x00004918   0x0000003e   Data   RO         1180    .constdata          nrfx_gpiote.o
    0x00004956   0x00004956   0x00000002   PAD
    0x00004958   0x00004958   0x00000020   Data   RO         1640    .constdata          app_uart_fifo.o
    0x00004978   0x00004978   0x00000008   PAD
    0x00004980   0x00004980   0x00000006   Data   RO         2299    .constdata          app_timer.o
    0x00004986   0x00004986   0x0000000a   PAD
    0x00004990   0x00004990   0x00000020   Data   RO         2908    .constdata          uartprocess.o
    0x000049b0   0x000049b0   0x00000020   Data   RO         3356    Region$$Table       anon$$obj.o


    Execution Region RW_IRAM1 (Exec base: 0x20000000, Load base: 0x000049d0, Size: 0x000030e0, Max: 0x00010000, ABSOLUTE, COMPRESSED[0x00000078])

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x20000000   COMPRESSED   0x00000001   Data   RW           12    .data               gpioprocess.o
    0x20000001   COMPRESSED   0x00000003   PAD
    0x20000004   COMPRESSED   0x0000002c   Data   RW          239    .data               host.o
    0x20000030   COMPRESSED   0x0000005c   Data   RW          372    .data               esbprocess.o
    0x2000008c   COMPRESSED   0x00000009   Data   RW          562    .data               nrf_drv_uart.o
    0x20000095   COMPRESSED   0x00000003   PAD
    0x20000098   COMPRESSED   0x00000008   Data   RW          616    .data               nrfx_prs.o
    0x200000a0   COMPRESSED   0x0000001b   Data   RW         1641    .data               app_uart_fifo.o
    0x200000bb   COMPRESSED   0x00000001   PAD
    0x200000bc   COMPRESSED   0x00000004   Data   RW         1724    .data               app_util_platform.o
    0x200000c0   COMPRESSED   0x00000014   Data   RW         2300    .data               app_timer.o
    0x200000d4   COMPRESSED   0x00000008   Data   RW         2491    .data               retarget.o
    0x200000dc   COMPRESSED   0x00000048   Data   RW         2621    .data               nrf_esb.o
    0x20000124   COMPRESSED   0x00000001   Data   RW         2909    .data               uartprocess.o
    0x20000125   COMPRESSED   0x00000003   PAD
    0x20000128   COMPRESSED   0x00000004   Data   RW         2968    .data               system_nrf52.o
    0x2000012c        -       0x00000040   Zero   RW          237    .bss                host.o
    0x2000016c        -       0x00000044   Zero   RW          371    .bss                esbprocess.o
    0x200001b0        -       0x0000002c   Zero   RW          709    .bss                nrfx_uart.o
    0x200001dc        -       0x00000024   Zero   RW          953    .bss                nrfx_uarte.o
    0x20000200        -       0x0000004c   Zero   RW         1179    .bss                nrfx_gpiote.o
    0x2000024c        -       0x00000020   Zero   RW         1639    .bss                app_uart_fifo.o
    0x2000026c        -       0x0000010c   Zero   RW         2298    .bss                app_timer.o
    0x20000378        -       0x00000552   Zero   RW         2620    .bss                nrf_esb.o
    0x200008ca        -       0x00000810   Zero   RW         2907    .bss                uartprocess.o
    0x200010da   COMPRESSED   0x00000006   PAD
    0x200010e0        -       0x00002000   Zero   RW         2945    STACK               arm_startup_nrf52.o



  Load Region LR$$.ARM.__AT_0x1000120C (Base: 0x1000120c, Size: 0x00000004, Max: 0x00000004, ABSOLUTE)

    Execution Region ER$$.ARM.__AT_0x1000120C (Exec base: 0x1000120c, Load base: 0x1000120c, Size: 0x00000004, Max: 0x00000004, ABSOLUTE, UNINIT)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x1000120c   0x1000120c   0x00000004   Data   RO           10    .ARM.__AT_0x1000120C  gpioprocess.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

        28          0          0          0          0       2485   app_error.o
        92         10          0          0          0      27465   app_error_weak.o
       170          0          0          0          0       6194   app_fifo.o
      1948        238          6         20        268      52358   app_timer.o
       770        108         32         27         32      21810   app_uart_fifo.o
        64         10          0          4          0       3482   app_util_platform.o
        36          8        512          0       8192        932   arm_startup_nrf52.o
         0          0          0          0          0      34412   boards.o
       248         28          0         92         68       2142   esbprocess.o
       350         32          7          1          0      57097   gpioprocess.o
       886        178         22         44         64      18876   host.o
       252         42          0          9          0      17924   nrf_drv_uart.o
      5084        860          0         72       1362      35287   nrf_esb.o
      1728        114         62          0         76      62593   nrfx_gpiote.o
       112         14          0          8          0       3741   nrfx_prs.o
      1704         50         46          0         44      62927   nrfx_uart.o
      1534         50         48          0         36      29573   nrfx_uarte.o
        16          0          0          8          0       2926   retarget.o
      1372        142          0          4          0       8643   system_nrf52.o
       496        138         32          1       2064      30391   uartprocess.o

    ----------------------------------------------------------------------
     16908       2022        824        300      12212     481258   Object Totals
         0          0         32          0          0          0   (incl. Generated)
        18          0         25         10          6          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

        86          0          0          0          0          0   __dczerorl2.o
         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        30          0          0          0          0          0   handlers.o
        36          8          0          0          0         68   init.o
        30          0          0          0          0         68   llshl.o
        32          0          0          0          0         68   llushr.o
        26          0          0          0          0         80   memcmp.o
        36          0          0          0          0         68   memcpya.o
        36          0          0          0          0        108   memseta.o
       736         56          0          0          0        184   printf5.o
        98          0          0          0          0         92   uldiv.o

    ----------------------------------------------------------------------
      1168         72          0          0          0        736   Library Totals
         2          0          0          0          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

      1166         72          0          0          0        736   mc_w.l

    ----------------------------------------------------------------------
      1168         72          0          0          0        736   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     18076       2094        824        300      12212     461366   Grand Totals
     18076       2094        824        120      12212     461366   ELF Image Totals (compressed)
     18076       2094        824        120          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                18900 (  18.46kB)
    Total RW  Size (RW Data + ZI Data)             12512 (  12.22kB)
    Total ROM Size (Code + RO Data + RW Data)      19020 (  18.57kB)

==============================================================================

