Archive member included to satisfy reference by file (symbol)

C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                              Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o (isprint)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
                              Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o (memcpy)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
                              (__vfprintf_long)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
                              (__vfscanf_long)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
                              C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o) (__heap_lock)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
                              C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o) (__aeabi_uldivmod)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
                              Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o (debug_fopen)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(do_nv_debug_operation.o)
                              C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o) (__do_nvdebug_operation)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
                              (__do_debug_operation_mempoll)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
                              C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o) (__aeabi_dadd)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
                              C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o) (frexp)

Discarded input sections

 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__aeabi_read_tp
                0x0000000000000000        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.abort    0x0000000000000000        0x2 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__assert
                0x0000000000000000        0x2 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__assert_func
                0x0000000000000000        0x2 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__aeabi_assert
                0x0000000000000000        0x2 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__sync_synchronize
                0x0000000000000000        0x2 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__getchar
                0x0000000000000000        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__putchar
                0x0000000000000000        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__open   0x0000000000000000        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__close  0x0000000000000000        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__write  0x0000000000000000        0xa Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__read   0x0000000000000000        0xa Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__seek   0x0000000000000000       0x1a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.remove   0x0000000000000000        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.rename   0x0000000000000000        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .bss.__user_locale_name_buffer
                0x0000000000000000        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .stack         0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .stack_process
                0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .heap          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x31 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x98 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000      0x185 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_info    0x0000000000000000       0x6f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_abbrev  0x0000000000000000       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_pubnames
                0x0000000000000000       0x12 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_pubtypes
                0x0000000000000000       0xc5 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_aranges
                0x0000000000000000       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0x13a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_line    0x0000000000000000      0x344 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_str     0x0000000000000000    0x7e7f7 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .comment       0x0000000000000000       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .ARM.attributes
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x31 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x98 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0x185 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.higher_lvl_get
                0x0000000000000000       0x4e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_module_filter_set
                0x0000000000000000       0x12 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_module_init_filter_get
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_module_filter_get
                0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_push
                0x0000000000000000       0xa4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_frontend_std_3
                0x0000000000000000       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_frontend_std_4
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_frontend_std_6
                0x0000000000000000       0x38 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_frontend_hexdump
                0x0000000000000000      0x144 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_backend_remove
                0x0000000000000000       0x54 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x31 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0x185 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .bss.m_freq    0x0000000000000000        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .bss.m_timestamp_div
                0x0000000000000000        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .text.nrf_log_str_formatter_timestamp_freq_set
                0x0000000000000000       0x3c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x31 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x98 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0x185 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .rodata        0x0000000000000000       0x77 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.nrf_gpio_pin_port_decode
                0x0000000000000000       0x44 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.nrf_gpio_cfg
                0x0000000000000000       0x62 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.nrf_gpio_cfg_output
                0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.nrf_gpio_cfg_input
                0x0000000000000000       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.nrf_gpio_pin_set
                0x0000000000000000       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.nrf_gpio_pin_clear
                0x0000000000000000       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.nrf_gpio_pin_toggle
                0x0000000000000000       0x44 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.nrf_gpio_pin_write
                0x0000000000000000       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.nrf_gpio_pin_read
                0x0000000000000000       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.nrf_gpio_pin_out_read
                0x0000000000000000       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.nrf_gpio_port_in_read
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.nrf_gpio_port_out_read
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.nrf_gpio_port_out_set
                0x0000000000000000       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.nrf_gpio_port_out_clear
                0x0000000000000000       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .rodata.m_board_led_list
                0x0000000000000000        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .rodata.m_board_btn_list
                0x0000000000000000        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_led_state_get
                0x0000000000000000       0x5c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_led_on
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_led_off
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_leds_off
                0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_leds_on
                0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_led_invert
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_leds_init
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_led_idx_to_pin
                0x0000000000000000       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_pin_to_led_idx
                0x0000000000000000       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_button_state_get
                0x0000000000000000       0x5c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_buttons_init
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_pin_to_button_idx
                0x0000000000000000       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_button_idx_to_pin
                0x0000000000000000       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_init
                0x0000000000000000       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_frame   0x0000000000000000      0x440 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_info    0x0000000000000000      0x8c3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_abbrev  0x0000000000000000      0x24d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_pubnames
                0x0000000000000000      0x4bd Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_pubtypes
                0x0000000000000000      0x181 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_aranges
                0x0000000000000000       0xf8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_ranges  0x0000000000000000       0xe8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x225 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x430 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x59 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x25d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x3f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x19 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x35 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x7b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x208 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_line    0x0000000000000000      0x99a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_str     0x0000000000000000    0x835ae Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .comment       0x0000000000000000       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .ARM.attributes
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .text.app_error_handler_bare
                0x0000000000000000       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x78 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x31 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0x185 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x9a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x98 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .text.NVIC_GetPriority
                0x0000000000000000       0x48 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .text.current_int_priority_get
                0x0000000000000000       0x38 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x78 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x78 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_internal_cmp_exch
                0x0000000000000000       0x5e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_store
                0x0000000000000000       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_fetch_or
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_and
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_fetch_xor
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_xor
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_fetch_add
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_fetch_sub
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_cmp_exch
                0x0000000000000000       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_fetch_sub_hs
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_sub_hs
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_flag_set_fetch
                0x0000000000000000       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_flag_clear
                0x0000000000000000       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x31 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x98 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0x185 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x9a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x31 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x98 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .text.NVIC_SystemReset
                0x0000000000000000       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .text.nrf_section_iter_get
                0x0000000000000000       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .text.nrf_mtx_trylock
                0x0000000000000000       0x3c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .text.nrf_mtx_unlock
                0x0000000000000000       0x3c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .text.nrf_power_system_off
                0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .bss.m_pwr_mgmt_evt
                0x0000000000000000        0x1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .text.nrf_pwr_mgmt_feed
                0x0000000000000000        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .text.shutdown_process
                0x0000000000000000       0x70 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .text.nrf_pwr_mgmt_shutdown
                0x0000000000000000       0x78 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x31 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0x430 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x59 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0x25d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x19 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0xac Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x98 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x9a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .rodata        0x0000000000000000       0x57 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .text.nrf_ringbuf_alloc
                0x0000000000000000      0x100 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .text.nrf_ringbuf_put
                0x0000000000000000       0x66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .text.nrf_ringbuf_cpy_put
                0x0000000000000000       0xec Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .text.nrf_ringbuf_get
                0x0000000000000000      0x104 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .text.nrf_ringbuf_cpy_get
                0x0000000000000000      0x108 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .text.nrf_ringbuf_free
                0x0000000000000000       0x56 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .text.nrf_section_iter_next
                0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x31 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x11 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.NVIC_SetPriority
                0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.rtc1_init
                0x0000000000000000       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.user_op_enque
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.user_op_alloc
                0x0000000000000000       0x5c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.timer_start_op_schedule
                0x0000000000000000       0x7a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.timer_stop_op_schedule
                0x0000000000000000       0x60 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.app_timer_init
                0x0000000000000000       0x68 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.app_timer_create
                0x0000000000000000       0x60 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.app_timer_start
                0x0000000000000000       0x6c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.app_timer_stop
                0x0000000000000000       0x44 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.app_timer_stop_all
                0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.app_timer_cnt_get
                0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.app_timer_cnt_diff_compute
                0x0000000000000000       0x1a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.app_timer_pause
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.app_timer_resume
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000      0x430 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000      0x25d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x45 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x19 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x35 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x7b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .bss.m_drv_state
                0x0000000000000000        0x1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .text.nrf_drv_ppi_init
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .text.nrf_drv_ppi_uninit
                0x0000000000000000       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_frame   0x0000000000000000       0x3c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_info    0x0000000000000000       0xfa Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_abbrev  0x0000000000000000       0xa4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_pubnames
                0x0000000000000000       0xbc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_pubtypes
                0x0000000000000000       0xf6 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_aranges
                0x0000000000000000       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_ranges  0x0000000000000000       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0x226 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0x430 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x59 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0x25d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x3f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x19 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x35 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x7b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x88 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_line    0x0000000000000000      0x5ae Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_str     0x0000000000000000    0x82478 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .comment       0x0000000000000000       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .ARM.attributes
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .bss.m_handlers
                0x0000000000000000        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .bss.m_contexts
                0x0000000000000000        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .bss.nrf_drv_uart_use_easy_dma
                0x0000000000000000        0x2 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .text.uarte_evt_handler
                0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .text.uart_evt_handler
                0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .rodata        0x0000000000000000       0x53 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .text.nrf_drv_uart_init
                0x0000000000000000       0xdc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_frame   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_info    0x0000000000000000     0x1105 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_abbrev  0x0000000000000000      0x1ee Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_pubnames
                0x0000000000000000       0xcb Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_pubtypes
                0x0000000000000000      0x3d8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_aranges
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_ranges  0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0x24e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0x430 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x59 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0x25d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x3f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x19 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x35 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x7b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x3f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_line    0x0000000000000000      0x68d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_str     0x0000000000000000    0x83204 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .comment       0x0000000000000000       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .ARM.attributes
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_internal_cmp_exch
                0x0000000000000000       0x5a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_fetch_store
                0x0000000000000000       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_store
                0x0000000000000000       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_fetch_or
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_or
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_fetch_and
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_and
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_fetch_xor
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_xor
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_fetch_add
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_add
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_fetch_sub
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_sub
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_cmp_exch
                0x0000000000000000       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_fetch_sub_hs
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_sub_hs
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_flag_set_fetch
                0x0000000000000000       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_flag_set
                0x0000000000000000       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_flag_clear_fetch
                0x0000000000000000       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_flag_clear
                0x0000000000000000       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_frame   0x0000000000000000      0x3b0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_info    0x0000000000000000      0x86f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_abbrev  0x0000000000000000      0x121 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_pubnames
                0x0000000000000000      0x247 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_pubtypes
                0x0000000000000000      0x109 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_aranges
                0x0000000000000000       0xb8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_ranges  0x0000000000000000       0xa8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0x213 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0x430 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x59 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0x25d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x3f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x19 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x35 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x7b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x42 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_line    0x0000000000000000      0x74f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_str     0x0000000000000000    0x824ec Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .comment       0x0000000000000000       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .ARM.attributes
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrf_ppi_channel_disable
                0x0000000000000000       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrf_ppi_channels_disable
                0x0000000000000000       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrf_ppi_fork_endpoint_setup
                0x0000000000000000       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrf_ppi_channels_include_in_group
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrf_ppi_channels_remove_from_group
                0x0000000000000000       0x38 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrf_ppi_channel_group_clear
                0x0000000000000000       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrf_ppi_group_enable
                0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrf_ppi_group_disable
                0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .bss.m_groups_allocated
                0x0000000000000000        0x1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.group_to_mask
                0x0000000000000000       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.is_app_group
                0x0000000000000000       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.channel_allocated_clr
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.channel_allocated_clr_all
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.is_allocated_group
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.group_allocated_set
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.group_allocated_clr
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.group_allocated_clr_all
                0x0000000000000000       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_free_all
                0x0000000000000000       0x6a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_channel_free
                0x0000000000000000       0x54 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_channel_fork_assign
                0x0000000000000000       0x42 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_channel_disable
                0x0000000000000000       0x6e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_group_alloc
                0x0000000000000000       0x9e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_group_free
                0x0000000000000000       0x6e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_group_enable
                0x0000000000000000       0x5a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_group_disable
                0x0000000000000000       0x3e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_channels_remove_from_group
                0x0000000000000000       0x82 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_channels_include_in_group
                0x0000000000000000       0x82 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0x430 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x59 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0x25d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x3f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x19 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x35 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x7b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x5b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0x17f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x9a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .text.prs_box_get
                0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .text.nrfx_prs_acquire
                0x0000000000000000       0x74 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .text.nrfx_prs_release
                0x0000000000000000       0x3c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0x430 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x59 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0x25d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x3f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x19 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x35 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x7b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x5b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x37 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0x17f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x9a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x42 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.NVIC_DisableIRQ
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text._NRFX_IRQ_DISABLE
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrfx_coredep_delay_us
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrf_saadc_channel_limits_set
                0x0000000000000000       0x3c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrf_saadc_limit_int_get
                0x0000000000000000       0x4c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrf_saadc_disable
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrfx_saadc_uninit
                0x0000000000000000       0xd4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrfx_saadc_channel_uninit
                0x0000000000000000       0xbc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrfx_saadc_sample_convert
                0x0000000000000000      0x158 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrfx_saadc_sample
                0x0000000000000000       0x58 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrfx_saadc_calibrate_offset
                0x0000000000000000       0x5c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrfx_saadc_is_busy
                0x0000000000000000       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrfx_saadc_abort
                0x0000000000000000       0x98 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrfx_saadc_limits_set
                0x0000000000000000      0x154 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .rodata.delay_machine_code.0
                0x0000000000000000        0x6 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0x430 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x59 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0x25d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x3f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x19 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x35 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x7b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x5b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x37 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0x17f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x9a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x42 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.NVIC_EnableIRQ
                0x0000000000000000       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.NVIC_DisableIRQ
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.NVIC_SetPriority
                0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_get_irq_number
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text._NRFX_IRQ_PRIORITY_SET
                0x0000000000000000       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text._NRFX_IRQ_ENABLE
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text._NRFX_IRQ_DISABLE
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrf_timer_task_trigger
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrf_timer_shorts_enable
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrf_timer_shorts_disable
                0x0000000000000000       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrf_timer_int_enable
                0x0000000000000000       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrf_timer_int_disable
                0x0000000000000000       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrf_timer_mode_set
                0x0000000000000000       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrf_timer_mode_get
                0x0000000000000000       0x12 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrf_timer_bit_width_set
                0x0000000000000000       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrf_timer_frequency_set
                0x0000000000000000       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrf_timer_cc_write
                0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrf_timer_cc_read
                0x0000000000000000       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrf_timer_capture_task_get
                0x0000000000000000       0x12 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_init
                0x0000000000000000      0x1f8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_uninit
                0x0000000000000000       0x60 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_enable
                0x0000000000000000       0x5c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_disable
                0x0000000000000000       0x5c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_is_enabled
                0x0000000000000000       0x58 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_resume
                0x0000000000000000       0x44 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_pause
                0x0000000000000000       0x44 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_clear
                0x0000000000000000       0x44 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_increment
                0x0000000000000000       0x5c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_capture
                0x0000000000000000       0x7c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_compare
                0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_extended_compare
                0x0000000000000000       0x5e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_compare_int_enable
                0x0000000000000000       0x74 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_compare_int_disable
                0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0x430 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x59 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0x25d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x3f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x19 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x35 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x7b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x5b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x37 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0x17f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x9a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x42 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.NVIC_EnableIRQ
                0x0000000000000000       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.NVIC_DisableIRQ
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.NVIC_SetPriority
                0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_get_irq_number
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text._NRFX_IRQ_PRIORITY_SET
                0x0000000000000000       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text._NRFX_IRQ_ENABLE
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text._NRFX_IRQ_DISABLE
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_event_clear
                0x0000000000000000       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_event_check
                0x0000000000000000       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_int_enable
                0x0000000000000000       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_int_enable_check
                0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_int_disable
                0x0000000000000000       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_errorsrc_get_and_clear
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_enable
                0x0000000000000000       0x12 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_disable
                0x0000000000000000       0x12 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_txrx_pins_set
                0x0000000000000000       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_txrx_pins_disconnect
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_tx_pin_get
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_rx_pin_get
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_rts_pin_get
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_cts_pin_get
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_hwfc_pins_set
                0x0000000000000000       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_hwfc_pins_disconnect
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_rxd_get
                0x0000000000000000       0x12 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_txd_set
                0x0000000000000000       0x1a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_task_trigger
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_configure
                0x0000000000000000       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_uart_baudrate_set
                0x0000000000000000       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_gpio_pin_port_decode
                0x0000000000000000       0x44 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_gpio_cfg
                0x0000000000000000       0x62 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_gpio_cfg_output
                0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_gpio_cfg_input
                0x0000000000000000       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_gpio_cfg_default
                0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_gpio_pin_set
                0x0000000000000000       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrf_gpio_port_out_set
                0x0000000000000000       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .bss.m_cb      0x0000000000000000       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.apply_config
                0x0000000000000000       0xc6 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.interrupts_enable
                0x0000000000000000       0x6c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.interrupts_disable
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.pins_to_default
                0x0000000000000000       0x8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_init
                0x0000000000000000       0xd4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_uninit
                0x0000000000000000       0x5c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.tx_byte  0x0000000000000000       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.tx_blocking
                0x0000000000000000       0x52 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_tx
                0x0000000000000000      0x110 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_tx_in_progress
                0x0000000000000000       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.rx_enable
                0x0000000000000000       0x36 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.rx_byte  0x0000000000000000       0x4e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_rx
                0x0000000000000000      0x21c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_rx_ready
                0x0000000000000000       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_rx_enable
                0x0000000000000000       0x4c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_rx_disable
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_errorsrc_get
                0x0000000000000000       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.rx_done_event
                0x0000000000000000       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.tx_done_event
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_tx_abort
                0x0000000000000000       0x4c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_rx_abort
                0x0000000000000000       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.uart_irq_handler
                0x0000000000000000      0x1de Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_0_irq_handler
                0x0000000000000000       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .rodata.irq_handlers.0
                0x0000000000000000        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0x430 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x59 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0x25d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x3f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x19 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x35 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x7b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x5b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x37 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0x17f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x9a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x42 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.NVIC_EnableIRQ
                0x0000000000000000       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.NVIC_DisableIRQ
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.NVIC_SetPriority
                0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_is_in_ram
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_get_irq_number
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text._NRFX_IRQ_PRIORITY_SET
                0x0000000000000000       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text._NRFX_IRQ_ENABLE
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text._NRFX_IRQ_DISABLE
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_event_clear
                0x0000000000000000       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_event_check
                0x0000000000000000       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_shorts_enable
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_shorts_disable
                0x0000000000000000       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_int_enable
                0x0000000000000000       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_int_disable
                0x0000000000000000       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_errorsrc_get_and_clear
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_enable
                0x0000000000000000       0x12 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_disable
                0x0000000000000000       0x12 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_txrx_pins_set
                0x0000000000000000       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_txrx_pins_disconnect
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_tx_pin_get
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_rx_pin_get
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_rts_pin_get
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_cts_pin_get
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_hwfc_pins_set
                0x0000000000000000       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_hwfc_pins_disconnect
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_task_trigger
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_configure
                0x0000000000000000       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_baudrate_set
                0x0000000000000000       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_tx_buffer_set
                0x0000000000000000       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_tx_amount_get
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_rx_buffer_set
                0x0000000000000000       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_uarte_rx_amount_get
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_gpio_pin_port_decode
                0x0000000000000000       0x44 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_gpio_cfg
                0x0000000000000000       0x62 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_gpio_cfg_output
                0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_gpio_cfg_input
                0x0000000000000000       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_gpio_cfg_default
                0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_gpio_pin_set
                0x0000000000000000       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrf_gpio_port_out_set
                0x0000000000000000       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .bss.m_cb      0x0000000000000000       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.apply_config
                0x0000000000000000       0xc6 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.interrupts_enable
                0x0000000000000000       0x98 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.interrupts_disable
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.pins_to_default
                0x0000000000000000       0x8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_uarte_init
                0x0000000000000000       0xcc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_uarte_uninit
                0x0000000000000000       0xac Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_uarte_tx
                0x0000000000000000      0x180 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_uarte_tx_in_progress
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_uarte_rx
                0x0000000000000000      0x23c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_uarte_rx_ready
                0x0000000000000000       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_uarte_errorsrc_get
                0x0000000000000000       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.rx_done_event
                0x0000000000000000       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.tx_done_event
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_uarte_tx_abort
                0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_uarte_rx_abort
                0x0000000000000000       0x48 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.uarte_irq_handler
                0x0000000000000000      0x18c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_uarte_0_irq_handler
                0x0000000000000000       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .rodata.irq_handlers.0
                0x0000000000000000        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0x430 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x59 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0x25d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x3f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x19 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x35 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x7b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x5b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x37 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0x17f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x9a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x42 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.NVIC_DisableIRQ
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text._NRFX_IRQ_DISABLE
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrf_clock_lf_is_running
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrf_clock_hf_is_running
                0x0000000000000000       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_disable
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_uninit
                0x0000000000000000       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_lfclk_stop
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_hfclk_start
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_hfclk_stop
                0x0000000000000000       0x3c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_calibration_start
                0x0000000000000000        0xe Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_is_calibrating
                0x0000000000000000        0x6 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_calibration_timer_start
                0x0000000000000000        0xe Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_calibration_timer_stop
                0x0000000000000000        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0x430 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x59 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0x25d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x3f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x19 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x35 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x7b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x5b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x37 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0x17f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x9a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x42 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.NVIC_DisableIRQ
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text._NRFX_IRQ_DISABLE
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_uninit
                0x0000000000000000       0x80 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_disable
                0x0000000000000000       0x54 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_cc_disable
                0x0000000000000000       0xc4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_tick_enable
                0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_tick_disable
                0x0000000000000000       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_overflow_enable
                0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_overflow_disable
                0x0000000000000000       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_max_ticks_get
                0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0x430 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x59 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0x25d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x3f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x19 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x35 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x7b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x5b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x37 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0x17f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x9a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x42 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_clock_lf_is_running
                0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_clock_hf_is_running
                0x0000000000000000       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrfx_clock_hfclk_is_running
                0x0000000000000000        0xe Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrfx_clock_lfclk_is_running
                0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.lfclk_stop
                0x0000000000000000       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.hfclk_start
                0x0000000000000000        0xa Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.hfclk_stop
                0x0000000000000000       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_init_check
                0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_uninit
                0x0000000000000000       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_lfclk_release
                0x0000000000000000       0x54 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_lfclk_is_running
                0x0000000000000000       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_hfclk_request
                0x0000000000000000       0xa0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_hfclk_release
                0x0000000000000000       0x54 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_hfclk_is_running
                0x0000000000000000       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_calibration_start
                0x0000000000000000       0x1a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_calibration_abort
                0x0000000000000000       0x12 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_is_calibrating
                0x0000000000000000       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0x430 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x59 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0x25d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x3f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x19 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x35 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x7b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x5b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x37 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0x17f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x9a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .bss.m_notifications_timer_data
                0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .rodata.m_notifications_timer
                0x0000000000000000        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x78 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x3c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x430 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x59 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x25d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x5a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x35 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x7b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x208 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x37 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x11 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x5b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x185 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x9a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x9e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .data._aTerminalId
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .bss._ActiveTerminal
                0x0000000000000000        0x1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text._PostTerminalSwitch
                0x0000000000000000       0x38 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_ReadNoLock
                0x0000000000000000      0x100 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_Read
                0x0000000000000000       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_WriteWithOverwriteNoLock
                0x0000000000000000      0x118 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_WriteSkipNoLock
                0x0000000000000000      0x120 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_Write
                0x0000000000000000       0x3c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_WriteString
                0x0000000000000000       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_PutCharSkipNoLock
                0x0000000000000000       0x68 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_PutCharSkip
                0x0000000000000000       0x84 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_PutChar
                0x0000000000000000       0x98 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_GetKey
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_WaitKey
                0x0000000000000000       0x1a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_HasKey
                0x0000000000000000       0x38 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_HasData
                0x0000000000000000       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_AllocDownBuffer
                0x0000000000000000       0xec Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_AllocUpBuffer
                0x0000000000000000       0xf0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_ConfigUpBuffer
                0x0000000000000000       0xcc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_ConfigDownBuffer
                0x0000000000000000       0xc8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_SetNameUpBuffer
                0x0000000000000000       0x5c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_SetNameDownBuffer
                0x0000000000000000       0x5c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_SetFlagsUpBuffer
                0x0000000000000000       0x5c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_SetFlagsDownBuffer
                0x0000000000000000       0x5c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_SetTerminal
                0x0000000000000000       0xb4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_TerminalOut
                0x0000000000000000      0x124 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x78 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000      0x115 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .text.printf   0x0000000000000000       0x4c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .text.puts     0x0000000000000000       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .text.__putchar
                0x0000000000000000       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .text.__getchar
                0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_frame   0x0000000000000000       0xc8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_info    0x0000000000000000      0x207 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_abbrev  0x0000000000000000      0x155 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_pubnames
                0x0000000000000000       0x42 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_pubtypes
                0x0000000000000000      0x10e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_aranges
                0x0000000000000000       0x38 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_ranges  0x0000000000000000       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0x18a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x78 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x47 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0x115 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x86 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0xa6 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0xc8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_line    0x0000000000000000      0x41c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_str     0x0000000000000000    0x78486 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .comment       0x0000000000000000       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .ARM.attributes
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .text._StoreChar
                0x0000000000000000       0x7e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .text._PrintUnsigned
                0x0000000000000000      0x15c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .text._PrintInt
                0x0000000000000000      0x14c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .text.SEGGER_RTT_vprintf
                0x0000000000000000      0x390 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .text.SEGGER_RTT_printf
                0x0000000000000000       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .rodata._aV2C.0
                0x0000000000000000       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_frame   0x0000000000000000       0xf8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_info    0x0000000000000000      0x415 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_abbrev  0x0000000000000000      0x193 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_pubnames
                0x0000000000000000       0x6f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_pubtypes
                0x0000000000000000       0xf8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_aranges
                0x0000000000000000       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_ranges  0x0000000000000000       0x48 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0x174 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x78 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x47 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0x115 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_line    0x0000000000000000      0x6e4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_str     0x0000000000000000    0x77b1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .comment       0x0000000000000000       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .ARM.attributes
                0x0000000000000000       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .text          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .data          0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .bss           0x0000000000000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .text          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .data          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss           0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__stdin_ungetc
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ungetc_fn
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.put_twodigit
                0x0000000000000000       0x5c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_utf8_mbtowc
                0x0000000000000000       0x94 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_1_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_2_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_3_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_4_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_5_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_6_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_7_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_8_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_9_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_10_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_11_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_13_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_14_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_15_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_16_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1250_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1251_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1252_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1253_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1254_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1255_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1256_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1257_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1258_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_map_range_search
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_map_singleton_search
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_set_bmp_singleton_search
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_set_nonbmp_singleton_search
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_set_bmp_range_search
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_set_nonbmp_range_search
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.getchar
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.put_twodigits_leading_blank
                0x0000000000000000       0x50 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_utf8_wctomb
                0x0000000000000000       0x88 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.put_twodigit_optional_zero_suppress
                0x0000000000000000       0x78 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__getc
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_pow10
                0x0000000000000000       0x58 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_pow10f
                0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__putc
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_print_padding
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_pre_padding
                0x0000000000000000       0x64 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__xlltoa
                0x0000000000000000       0x7c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__xtoa
                0x0000000000000000       0x58 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__xltoa
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.abs
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.asctime_r
                0x0000000000000000      0x13c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.asctime
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.atexit
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc._execute_at_exit_fns
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.bsearch
                0x0000000000000000       0x5c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_towupper
                0x0000000000000000       0x7c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_toupper
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_towlower
                0x0000000000000000       0x7c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_tolower
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_1_wctomb
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_11_wctomb
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_13_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_2_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_3_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_4_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_9_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_10_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_5_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_6_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_7_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_8_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1255_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1256_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1257_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1258_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_14_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_15_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_16_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1250_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1251_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1252_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1253_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1254_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ctl_is_exact_power_of_two
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ctl_round_power_of_two
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ctl_count_leading_zeroes
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ctl_ilogb
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.buddy_alloc
                0x0000000000000000      0x124 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.buddy_heap_init
                0x0000000000000000       0x88 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_isctype
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_isctype_l
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isalpha
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isupper
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.islower
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isdigit
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__digit
                0x0000000000000000       0x44 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isxdigit
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isspace
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ispunct
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isalnum
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isgraph
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iscntrl
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isblank
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.tolower
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.toupper
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isalpha_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isupper_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.islower_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isdigit_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isxdigit_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isspace_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ispunct_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isalnum_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isprint_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isgraph_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iscntrl_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isblank_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.tolower_l
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.toupper_l
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isascii
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.div
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__aeabi_errno_addr
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.buddy_free
                0x0000000000000000       0xb4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__strtoul
                0x0000000000000000       0xd4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__strtoull
                0x0000000000000000      0x10c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fopen
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.vfprintf
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fprintf
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.vfscanf
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fscanf
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fgetpos
                0x0000000000000000       0x64 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ftell
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ungetc
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fileno
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.feof
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ferror
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fstat
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.gets
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.itoa
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.labs
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ldiv
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.linked_heap_init
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.linked_heap_alloc
                0x0000000000000000       0x9c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.linked_heap_free
                0x0000000000000000       0xb4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.linked_heap_realloc
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.llabs
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.lldiv
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.lltoa
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_global_locale_category
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_locale_category
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.localeconv_l
                0x0000000000000000       0xb0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.localeconv
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_compare_locale_name
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ltoa
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.malloc
                0x0000000000000000       0x8c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.getBuf
                0x0000000000000000       0x5c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fflush
                0x0000000000000000       0x44 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fseek
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fsetpos
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.rewind
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.output_fn
                0x0000000000000000       0x88 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fputc
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fputs
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fwrite
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.putc
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.getc_fn
                0x0000000000000000       0xcc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fgetc
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fread
                0x0000000000000000       0x84 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fgets
                0x0000000000000000       0x7c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.getc
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.calloc
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.free
                0x0000000000000000       0xa4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.setbuf
                0x0000000000000000       0x5c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.setvbuf
                0x0000000000000000       0x50 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fclose
                0x0000000000000000       0x44 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.realloc
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.aligned_alloc
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.memccpy
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mempcpy
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.memchr
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.memcmp
                0x0000000000000000       0x74 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__aeabi_uread4
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__aeabi_uwrite4
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__aeabi_uread8
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__aeabi_uwrite8
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.memmove
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.printf
                0x0000000000000000       0x44 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.putchar
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.puts
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.qsort
                0x0000000000000000      0x218 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.rand
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.scanf
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.snprintf
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.sprintf
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.srand
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.sscanf
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strcasecmp
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strcasestr
                0x0000000000000000       0x5c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_decode_error.str1.4
                0x0000000000000000       0x7a C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_decode_error
                0x0000000000000000       0x7c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strerror
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_register_error_decoder
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strcat
                0x0000000000000000       0x84 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_encode_locale.str1.4
                0x0000000000000000        0x2 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_encode_locale
                0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strchr
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strcoll
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strcspn
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strdup
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_string_list_encode
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_string_list_decode
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strncasecmp
                0x0000000000000000       0x64 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strncasestr
                0x0000000000000000       0x60 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strncat
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strlcat
                0x0000000000000000       0x60 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strnchr
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strncmp
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strncpy
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strlcpy
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strnlen
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strndup
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strnstr
                0x0000000000000000       0x50 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strpbrk
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strrchr
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strsep
                0x0000000000000000       0x44 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strspn
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strstr
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtod
                0x0000000000000000      0x1cc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtold
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtof
                0x0000000000000000      0x1a4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtok
                0x0000000000000000       0x6c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtok_r
                0x0000000000000000       0x58 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtol
                0x0000000000000000       0xb8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.atoi
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.atof
                0x0000000000000000      0x150 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.atol
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtoll
                0x0000000000000000       0xbc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.atoll
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtoul
                0x0000000000000000       0x90 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtoull
                0x0000000000000000       0x9c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strxfrm
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.stpcpy
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.localtime_r
                0x0000000000000000      0x144 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.difftime
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.checktm
                0x0000000000000000      0x1f0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mktime
                0x0000000000000000      0x158 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ctime
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ctime_r
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.gmtime
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.gmtime_r
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.localtime
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.gettimeofday
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.settimeofday
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.time
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ulltoa
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ultoa
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.utoa
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.vprintf
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.vscanf
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.vsnprintf
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.vsprintf
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.vasprintf
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.vsscanf
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcscat
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcschr
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcscmp
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcscoll
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcscpy
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcscspn
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcslen
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsdup
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsncat
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsnchr
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsncmp
                0x0000000000000000       0x50 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsncpy
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsnlen
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsnstr
                0x0000000000000000       0x50 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcspbrk
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsrchr
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcssep
                0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsspn
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsstr
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcstok
                0x0000000000000000       0x6c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcstok_r
                0x0000000000000000       0x58 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wmemcpy
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wmemccpy
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wmempcpy
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wmemmove
                0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wmemcmp
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wmemchr
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wmemset
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsxfrm
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.tmpnam
                0x0000000000000000       0x5c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.duplocale
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.uselocale
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.freelocale
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__user_find_locale
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_find_locale
                0x0000000000000000       0x84 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_set_locale.part.0
                0x0000000000000000       0x60 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.newlocale
                0x0000000000000000       0x4c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.setlocale
                0x0000000000000000       0x94 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbsinit
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wctob_l
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wctob
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.btowc_l
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.btowc
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mblen_l
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mblen
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbrlen_l
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbrlen
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wctomb_l
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wctomb
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.put_formatted.str1.4
                0x0000000000000000       0x63 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.put_formatted
                0x0000000000000000      0x6cc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strftime_l
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strftime
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcrtomb_l
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcrtomb
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbtowc_l
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbtowc
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.mbrtowc_l.str1.4
                0x0000000000000000        0x1 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbrtowc_l
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbrtowc
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbstowcs_l
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbstowcs
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbsrtowcs_l
                0x0000000000000000       0xa8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbsrtowcs
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbsnrtowcs
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcstombs_l
                0x0000000000000000       0xc4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcstombs
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsrtombs_l
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsrtombs
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsnrtombs
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_init_mbstate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_mb_max
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_1_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_1
                0x0000000000000000       0x4c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_1_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_1_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_2_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_2
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_2_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_2_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_3_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_3
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_3_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_3_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_4_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_4
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_4_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_4_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_5_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_5
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_5_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_5_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_6_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_6
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_6_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_6_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_7_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_7
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_7_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_7_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_8_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_8
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_8_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_8_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_9_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_9
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_9_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_9_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_10_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_10
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_10_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_10_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_11_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_11
                0x0000000000000000       0x4c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_11_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_11_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_13_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_13
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_13_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_13_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_14_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_14
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_14_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_14_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_15_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_15
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_15_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_15_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_16_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_16
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_16_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_16_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1250_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1250
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1250_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1250_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1251_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1251
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1251_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1251_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1252_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1252
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1252_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1252_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1253_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1253
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1253_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1253_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1254_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1254
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1254_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1254_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1255_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1255
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1255_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1255_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1256_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1256
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1256_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1256_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1257_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1257
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1257_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1257_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1258_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1258
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1258_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1258_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wctrans
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wctrans_l
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.towlower
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.towupper
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.towlower_l
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.towupper_l
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.towctrans
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.towctrans_l
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswalpha
                0x0000000000000000       0x84 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswprint
                0x0000000000000000       0x84 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswblank
                0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswcntrl
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswdigit
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswspace
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswxdigit
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswalnum
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswlower
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswupper
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswgraph
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswpunct
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswctype
                0x0000000000000000       0xf4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_isctype
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_1_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_2_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_3_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_4_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_5_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_6_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_7_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_8_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_9_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_10_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_11_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_13_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_14_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_15_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_16_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1250_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1251_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1252_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1253_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1254_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1255_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1256_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1257_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1258_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wctype
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iswctype
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iswctype_l
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswalpha
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswupper
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswlower
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswdigit
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswxdigit
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswspace
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswpunct
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswalnum
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswprint
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswgraph
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswcntrl
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswblank
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswalpha_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswupper_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswlower_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswdigit_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswxdigit_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswspace_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswpunct_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswalnum_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswprint_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswgraph_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswcntrl_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswblank_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__RAL_asctime_buf
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__RAL_error_decoder_head
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__RAL_lconv_data
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__RAL_tmpnam_buf
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__RAL_tmpnam_fileno
                0x0000000000000000        0x2 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__atexitfns
                0x0000000000000000       0x80 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__user_format_extender
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__user_get_time_of_day
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__user_set_time_of_day
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc._tm  0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.atexitfn_count
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.iod  0x0000000000000000       0x80 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.iod2
                0x0000000000000000       0x60 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.stdin
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .data.libc.__RAL_rand_next
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .data.libc.__ungot
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .data.libc.heap
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .data.libc.stderr
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .data.libc.stdout
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .data.libc.streams
                0x0000000000000000       0xc0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1250
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1251
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1252
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1253
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1254
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1255
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1256
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1257
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1258
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_10
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_11
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_13
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_14
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_15
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_16
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_3
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_4
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_5
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_6
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_7
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_8
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_9
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_utf8
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1250_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1251_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1252_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1253_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1254_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1255_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1256_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1257_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1258_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_data_utf8_comma
                0x0000000000000000        0x2 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_data_utf8_minus
                0x0000000000000000        0x2 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_data_utf8_plus
                0x0000000000000000        0x2 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_data_utf8_space
                0x0000000000000000        0x2 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_hex_lc
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_hex_uc
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_10_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_11_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_13_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_14_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_15_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_16_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_1_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_2_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_3_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_4_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_5_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_6_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_7_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_8_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_9_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_mon_lengths
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_tmpnam_template
                0x0000000000000000       0x11 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_isalpha_range
                0x0000000000000000      0x46c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_isalpha_singleton
                0x0000000000000000       0xac C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_isprint_range
                0x0000000000000000      0x534 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_isprint_singleton
                0x0000000000000000       0x52 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_tolower_range1_map
                0x0000000000000000       0xde C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_tolower_range2_map
                0x0000000000000000       0xde C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_tolower_singleton_map
                0x0000000000000000      0x13c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_toupper_range1_map
                0x0000000000000000       0xde C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_toupper_range2_map
                0x0000000000000000       0xd2 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_toupper_singleton_map
                0x0000000000000000      0x168 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_nonbmp_isalpha_range
                0x0000000000000000      0x2d0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_nonbmp_isalpha_singleton
                0x0000000000000000       0x74 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_nonbmp_isprint_range
                0x0000000000000000      0x470 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_nonbmp_isprint_singleton
                0x0000000000000000       0x88 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1250_range_map
                0x0000000000000000       0x6c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1250_singleton_map
                0x0000000000000000      0x140 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1251_range_map
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1251_singleton_map
                0x0000000000000000       0xa8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1252_range_map
                0x0000000000000000       0x1e C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1252_singleton_map
                0x0000000000000000       0x4c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1253_range_map
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1253_singleton_map
                0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1254_range_map
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1254_singleton_map
                0x0000000000000000       0x60 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1255_range_map
                0x0000000000000000       0x4e C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1255_singleton_map
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1256_range_map
                0x0000000000000000       0x72 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1256_singleton_map
                0x0000000000000000       0x98 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1257_range_map
                0x0000000000000000       0x4e C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1257_singleton_map
                0x0000000000000000      0x134 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1258_range_map
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1258_singleton_map
                0x0000000000000000       0x80 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_10_range_map
                0x0000000000000000       0x36 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_10_singleton_map
                0x0000000000000000       0xe0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_11_range_map
                0x0000000000000000       0x12 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_13_range_map
                0x0000000000000000       0x42 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_13_singleton_map
                0x0000000000000000      0x104 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_14_range_map
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_14_singleton_map
                0x0000000000000000       0x60 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_15_range_map
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_15_singleton_map
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_16_range_map
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_16_singleton_map
                0x0000000000000000       0xb0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_1_range_map
                0x0000000000000000        0x6 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_2_range_map
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_2_singleton_map
                0x0000000000000000      0x124 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_3_range_map
                0x0000000000000000       0x5a C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_3_singleton_map
                0x0000000000000000       0x84 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_4_range_map
                0x0000000000000000       0x42 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_4_singleton_map
                0x0000000000000000       0xec C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_5_range_map
                0x0000000000000000       0x1e C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_5_singleton_map
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_6_range_map
                0x0000000000000000       0x12 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_6_singleton_map
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_7_range_map
                0x0000000000000000       0x36 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_7_singleton_map
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_8_range_map
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_8_singleton_map
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_9_range_map
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_9_singleton_map
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unknown_string
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_wctrans_name_list
                0x0000000000000000       0x11 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_wctype_class_name_list
                0x0000000000000000       0x4a C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_year_lengths
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__aeabi_EDOM
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__aeabi_EILSEQ
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__aeabi_ERANGE
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.power
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.powerf
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_mbrlen_mbstate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_mbrtowc_mbstate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_mbsrtowcs_mbstate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_mbtowc_mbstate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_strtok_state
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_wcrtomb_mbstate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_wcsrtombs_mbstate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_wcstok_state
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_wctomb_mbstate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.errno_val
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .data.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .bss.libc      0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text.libc.longjmp
                0x0000000000000000       0x16 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text.libc.memcpy_fast
                0x0000000000000000      0x3ac C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text.libc.memcpy_small
                0x0000000000000000       0x1a C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text.libc.memset
                0x0000000000000000       0x66 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text.libc.__aeabi_memset
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text.libc.setjmp
                0x0000000000000000        0xe C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text.libc.strcpy
                0x0000000000000000       0x44 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text.libc.strcmp
                0x0000000000000000       0x4e C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .data          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .bss           0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .rodata.libc.__vfprintf_int.str1.4
                0x0000000000000000        0x7 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_int
                0x0000000000000000      0x5e8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_int_nwp
                0x0000000000000000      0x5a0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_long
                0x0000000000000000      0x5fc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_long_nwp
                0x0000000000000000      0x5bc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_long_long
                0x0000000000000000      0x6b8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_long_long_nwp
                0x0000000000000000      0x710 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .rodata.libc.__vfprintf_float_long.str1.4
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_float_long
                0x0000000000000000     0x1100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_float_long_long
                0x0000000000000000     0x1100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_short_float_long
                0x0000000000000000      0xe68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_short_float_long_long
                0x0000000000000000      0xf48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__RAL_compute_wide_metrics
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__RAL_print_wide_string
                0x0000000000000000       0x4c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_int_wchar
                0x0000000000000000      0x6c4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_int_nwp_wchar
                0x0000000000000000      0x5e0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_long_wchar
                0x0000000000000000      0x6d4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_long_nwp_wchar
                0x0000000000000000      0x5e8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_long_long_wchar
                0x0000000000000000      0x790 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_long_long_nwp_wchar
                0x0000000000000000      0x738 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_float_long_wchar
                0x0000000000000000     0x11ac C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_float_long_long_wchar
                0x0000000000000000     0x11ac C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_short_float_long_wchar
                0x0000000000000000      0xef8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_short_float_long_long_wchar
                0x0000000000000000     0x1010 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .rodata.libc.ipow10
                0x0000000000000000       0xa0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .comment       0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .ARM.attributes
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .data          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .bss           0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.rd_string_map
                0x0000000000000000       0xb4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.rd_string
                0x0000000000000000       0xa8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.rd_int
                0x0000000000000000      0x188 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.rd_int_long_long
                0x0000000000000000      0x1a8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.rd_real
                0x0000000000000000      0x2ec C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_int
                0x0000000000000000      0x3e4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_int_cc
                0x0000000000000000      0x464 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_long
                0x0000000000000000      0x3f8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_long_cc
                0x0000000000000000      0x474 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_long_long
                0x0000000000000000      0x418 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_long_long_cc
                0x0000000000000000      0x498 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_float_long
                0x0000000000000000      0x408 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_float_long_cc
                0x0000000000000000      0x484 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_float_long_long
                0x0000000000000000      0x428 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_float_long_long_cc
                0x0000000000000000      0x4a0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .comment       0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .ARM.attributes
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .data          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .bss           0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.ctl_count_leading_zeros_64
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.ctl_count_trailing_zeros_16
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.ctl_count_trailing_zeros_32
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.ctl_count_trailing_zeros_64
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__popcountsi2
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__popcountdi2
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__paritysi2
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__paritydi2
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__bswapsi2
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__bswapdi2
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_lock
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_unlock
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_add_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_sub_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_or_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_and_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_xor_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_nand_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_add_and_fetch_1
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_sub_and_fetch_1
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_or_and_fetch_1
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_and_and_fetch_1
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_xor_and_fetch_1
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_nand_and_fetch_1
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_bool_compare_and_swap_1
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_val_compare_and_swap_1
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_lock_test_and_set_1
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_lock_release_1
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_add_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_sub_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_or_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_and_2
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_xor_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_nand_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_add_and_fetch_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_sub_and_fetch_2
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_or_and_fetch_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_and_and_fetch_2
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_xor_and_fetch_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_nand_and_fetch_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_bool_compare_and_swap_2
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_val_compare_and_swap_2
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_lock_test_and_set_2
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_lock_release_2
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_add_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_sub_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_or_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_and_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_xor_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_nand_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_add_and_fetch_4
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_sub_and_fetch_4
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_or_and_fetch_4
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_and_and_fetch_4
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_xor_and_fetch_4
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_nand_and_fetch_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_bool_compare_and_swap_4
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_val_compare_and_swap_4
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_lock_test_and_set_4
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_lock_release_4
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_add_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_sub_8
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_or_8
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_and_8
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_xor_8
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_nand_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_add_and_fetch_8
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_sub_and_fetch_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_or_and_fetch_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_and_and_fetch_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_xor_and_fetch_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_nand_and_fetch_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_bool_compare_and_swap_8
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_val_compare_and_swap_8
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_lock_test_and_set_8
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_lock_release_8
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_load_1
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_store_1
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_exchange_1
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_compare_exchange_1
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_add_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_sub_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_or_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_and_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_xor_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_nand_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_load_2
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_store_2
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_exchange_2
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_compare_exchange_2
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_add_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_sub_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_or_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_and_2
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_xor_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_nand_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_load_4
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_store_4
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_exchange_4
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_compare_exchange_4
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_add_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_sub_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_or_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_and_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_xor_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_nand_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_load_8
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_store_8
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_exchange_8
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_compare_exchange_8
                0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_add_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_sub_8
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_or_8
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_and_8
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_xor_8
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_nand_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_load
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_store
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_is_lock_free
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__heap_lock
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__heap_unlock
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__printf_lock
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__printf_unlock
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__scanf_lock
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__scanf_unlock
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .comment       0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .ARM.attributes
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .data.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .bss.libc      0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_umod
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_asr
                0x0000000000000000       0x26 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_div
                0x0000000000000000       0x44 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_lsl
                0x0000000000000000       0x26 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_lsr
                0x0000000000000000       0x26 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_mod
                0x0000000000000000       0x46 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_udivmod
                0x0000000000000000       0xce C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__aeabi_ldivmod
                0x0000000000000000       0x58 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_cmp
                0x0000000000000000       0x1a C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_ucmp
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.muldi3
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int32_umod
                0x0000000000000000        0xa C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int32_div
                0x0000000000000000      0x216 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .rodata.libc.__aeabi_idiv
                0x0000000000000000        0xa C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__uint32_div
                0x0000000000000000       0xf6 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .rodata.libc.__aeabi_uidiv
                0x0000000000000000       0x46 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int32_mod
                0x0000000000000000        0xa C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__aeabi_uidivmod
                0x0000000000000000       0x2a C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__aeabi_idivmod
                0x0000000000000000       0x4a C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.ctl_count_leading_zeros_32
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.ctl_count_leading_zeros_16
                0x0000000000000000       0x32 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__gnu_thumb1_case_shi
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__gnu_thumb1_case_si
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__gnu_thumb1_case_sqi
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__gnu_thumb1_case_uhi
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__gnu_thumb1_case_uqi
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .ARM.attributes
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .data          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .bss           0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio
                0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_abort
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fopen
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fgets
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fputc
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fputs
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fread
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fwrite
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fseek
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_ftell
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_gets
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fflush
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fclose
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fgetc
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getchar
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_putchar
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_puts
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_rewind
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_clearerr
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_feof
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_ferror
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getch
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_time
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_vprintf
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_vfprintf
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_ungetc
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fgetpos
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fsetpos
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_freopen
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_perror
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_remove
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_rename
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_tmpfile
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_tmpnam
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getenv
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_system
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_vfscanf
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_vscanf
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_exit
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_enabled
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_kbhit
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_ioctl
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_runtime_error
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_break
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getargs
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_geti
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getu
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getl
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getul
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getf
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getd
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getll
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getull
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_filesize
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_accept
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_bind
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_listen
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_shutdown
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_socket
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_htons
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_htonl
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_loadsymbols
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_unloadsymbols
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_evaluate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.__debug_io_lock
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.__debug_io_unlock
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .bss.libdebugio.__dbgEnabled
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .bss.libdebugio.getenv_buffer
                0x0000000000000000      0x400 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .bss.libdebugio.tmpnam_buffer
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .comment       0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .ARM.attributes
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(do_nv_debug_operation.o)
 .data          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(do_nv_debug_operation.o)
 .bss           0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(do_nv_debug_operation.o)
 .text.libdebugio
                0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(do_nv_debug_operation.o)
 .text.libdebugio.__do_nvdebug_operation
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(do_nv_debug_operation.o)
 .comment       0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(do_nv_debug_operation.o)
 .ARM.attributes
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(do_nv_debug_operation.o)
 .text          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .data          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .bss           0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .text.libdebugio
                0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .text.libdebugio.__do_debug_operation_mempoll
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .bss.libdebugio.dbgCntrlWord_mempoll
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .bss.libdebugio.dbgCommWord
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .comment       0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .ARM.attributes
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .text.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .data.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .bss.libc      0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .rodata.__aeabi_fdiv_reciprocal_table
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .rodata.__aeabi_ddiv_reciprocal_table
                0x0000000000000000      0x180 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fadd
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dadd
                0x0000000000000000      0x244 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fsub
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dsub
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_frsub
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_drsub
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fmul
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dmul
                0x0000000000000000      0x138 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fdiv
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_ddiv
                0x0000000000000000      0x1cc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fcmple
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dcmple
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fcmpeq
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dcmpeq
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fcmpge
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dcmpge
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fcmpgt
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dcmpgt
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fcmplt
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dcmplt
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fcmpun
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dcmpun
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_cfcmpeq
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_cdcmpeq
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_cfcmple
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_cdcmple
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_cfrcmple
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_cdrcmple
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__cmpdf2
                0x0000000000000000       0x64 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_f2iz
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_d2iz
                0x0000000000000000       0x4c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_f2lz
                0x0000000000000000       0x74 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_d2lz
                0x0000000000000000       0x84 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_f2uiz
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_d2uiz
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_f2ulz
                0x0000000000000000       0x44 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_d2ulz
                0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_i2f
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_i2d
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_l2f
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_l2d
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_ui2f
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_ui2d
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_ul2f
                0x0000000000000000       0x58 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_ul2d
                0x0000000000000000       0x5c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_f2d
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_d2f
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float32_isfinite
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float64_isfinite
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float32_isinf
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float64_isinf
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float32_isnan
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float64_isnan
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float32_isnormal
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float64_isnormal
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float32_signbit
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float64_signbit
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float32_classify
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float64_classify
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.fabs     0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.fabsf    0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.ceilf    0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.floorf   0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.frexpf   0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.ldexpf   0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .ARM.attributes
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .data          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .bss           0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.__RAL_asinacosf
                0x0000000000000000      0x174 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.__RAL_poly1_eval
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.__RAL_poly1_evalf
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.__RAL_poly_eval
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.__RAL_poly_evalf
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.__RAL_sincos
                0x0000000000000000      0x224 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.__RAL_sincosf
                0x0000000000000000       0xf8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.acosf
                0x0000000000000000      0x150 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.asinf
                0x0000000000000000      0x12c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.atan
                0x0000000000000000      0x290 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.atan2
                0x0000000000000000      0x14c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.atanf
                0x0000000000000000      0x12c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.atan2f
                0x0000000000000000       0xcc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.ceil
                0x0000000000000000       0xa8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.cos
                0x0000000000000000      0x1c8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.cosf
                0x0000000000000000      0x17c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.expf
                0x0000000000000000      0x16c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.coshf
                0x0000000000000000       0xa8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.fma
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.fmax
                0x0000000000000000       0x50 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.fmaxf
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.fmin
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.fminf
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.frexp
                0x0000000000000000       0x50 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.hypotf
                0x0000000000000000       0xec C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.ldexp
                0x0000000000000000       0x7c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.exp
                0x0000000000000000      0x200 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.cosh
                0x0000000000000000      0x128 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.log
                0x0000000000000000      0x230 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.atanh
                0x0000000000000000      0x160 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.log10
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.logf
                0x0000000000000000      0x114 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.acoshf
                0x0000000000000000       0xc0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.asinhf
                0x0000000000000000       0xa8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.atanhf
                0x0000000000000000       0xd4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.log10f
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.modf
                0x0000000000000000       0x94 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.modff
                0x0000000000000000       0x5c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.pow
                0x0000000000000000      0x168 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.exp2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.powf
                0x0000000000000000       0xcc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.exp2f
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.scalbn
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.scalbnf
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.sin
                0x0000000000000000      0x1bc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.sinf
                0x0000000000000000      0x164 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.sinh
                0x0000000000000000      0x250 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.sinhf
                0x0000000000000000       0xc8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.tan
                0x0000000000000000      0x23c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.tanf
                0x0000000000000000      0x15c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.tanh
                0x0000000000000000      0x1ec C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.tanhf
                0x0000000000000000       0xe0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.sqrt
                0x0000000000000000      0x134 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.__RAL_asinacos
                0x0000000000000000      0x2dc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.acosh
                0x0000000000000000      0x138 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.asinh
                0x0000000000000000      0x124 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.hypot
                0x0000000000000000      0x204 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.asin
                0x0000000000000000      0x27c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.acos
                0x0000000000000000      0x284 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.cbrtf
                0x0000000000000000       0xe4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.cbrt
                0x0000000000000000      0x1fc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.floor
                0x0000000000000000       0xa8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.fmodf
                0x0000000000000000       0xfc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.fmod
                0x0000000000000000      0x1a4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .rodata.libc.__asinacos_a
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .rodata.libc.__asinacos_b
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .rodata.libc.__asinacosf_a
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .rodata.libc.__asinacosf_b
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .rodata.libc.atanf_a
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .rodata.libc.expf_twojby8
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .comment       0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .ARM.attributes
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)

Memory Configuration

Name             Origin             Length             Attributes
UNPLACED_SECTIONS 0x0000000100000000 0x0000000000000000 xw
RAM              0x0000000020000000 0x0000000000040000 xw
FLASH            0x0000000000000000 0x0000000000100000 xw
*default*        0x0000000000000000 0xffffffffffffffff

Linker script and memory map

                0x0000000000000000                __do_debug_operation = __do_debug_operation_mempoll
                0x0000000000000000                __vfprintf = __vfprintf_long
                0x0000000000000000                __vfscanf = __vfscanf_long
                0x0000000020000000                __RAM_segment_start__ = 0x20000000
                0x0000000020040000                __RAM_segment_end__ = 0x20040000
                0x0000000000040000                __RAM_segment_size__ = 0x40000
                0x0000000000000000                __FLASH_segment_start__ = 0x0
                0x0000000000100000                __FLASH_segment_end__ = 0x100000
                0x0000000000100000                __FLASH_segment_size__ = 0x100000
                0x0000000000002000                __HEAPSIZE__ = 0x2000
                0x0000000000000000                __STACKSIZE_PROCESS__ = 0x0
                0x0000000000002000                __STACKSIZE__ = 0x2000
                0x0000000020000000                __vectors_ram_load_start__ = 0x20000000

.vectors_ram    0x0000000020000000        0x0
                0x0000000020000000                __vectors_ram_start__ = .
                0x0000000020000000                __app_ram_start__ = __vectors_ram_start__
 *(.vectors_ram .vectors_ram.*)
                0x0000000020000000                __vectors_ram_end__ = (__vectors_ram_start__ + SIZEOF (.vectors_ram))
                0x0000000000000000                __vectors_ram_size__ = SIZEOF (.vectors_ram)
                0x0000000020000000                __vectors_ram_load_end__ = __vectors_ram_end__
                0x0000000000000001                . = ASSERT (((__vectors_ram_start__ == __vectors_ram_end__) || ((__vectors_ram_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .vectors_ram is too large to fit in RAM memory segment)
                0x0000000020000000                __nrf_sections_run_load_start__ = ALIGN (__vectors_ram_end__, 0x4)

.nrf_sections_run
                0x0000000020000000        0x0
                0x0000000020000000                __nrf_sections_run_start__ = .
                0x0000000020000000                __start_nrf_sections_run = __nrf_sections_run_start__
 *(.nrf_sections_run .nrf_sections_run.*)
                0x0000000020000000                __nrf_sections_run_end__ = (__nrf_sections_run_start__ + SIZEOF (.nrf_sections_run))
                0x0000000000000000                __nrf_sections_run_size__ = SIZEOF (.nrf_sections_run)
                0x0000000020000000                __nrf_sections_run_load_end__ = __nrf_sections_run_end__
                0x0000000000000001                . = ASSERT (((__nrf_sections_run_start__ == __nrf_sections_run_end__) || ((__nrf_sections_run_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .nrf_sections_run is too large to fit in RAM memory segment)
                0x0000000000000000                __vectors_load_start__ = 0x0

.vectors        0x0000000000000000      0x200
                0x0000000000000000                __vectors_start__ = .
 *(.vectors .vectors.*)
 .vectors       0x0000000000000000      0x200 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
                0x0000000000000000                _vectors
                0x0000000000000200                __vectors_end__ = (__vectors_start__ + SIZEOF (.vectors))
                0x0000000000000200                __vectors_size__ = SIZEOF (.vectors)
                0x0000000000000200                __vectors_load_end__ = __vectors_end__
                0x0000000000000001                . = ASSERT (((__vectors_start__ == __vectors_end__) || ((__vectors_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .vectors is too large to fit in FLASH memory segment)
                0x0000000000000200                __init_load_start__ = ALIGN (__vectors_end__, 0x4)

.init           0x0000000000000200      0x1d0
                0x0000000000000200                __init_start__ = .
 *(.init .init.*)
 .init          0x0000000000000200      0x15c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
                0x0000000000000200                _start
                0x00000000000002b4                exit
 .init          0x000000000000035c       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
                0x000000000000035c                NMI_Handler
                0x000000000000035e                HardFault_Handler
                0x0000000000000360                MemoryManagement_Handler
                0x0000000000000362                BusFault_Handler
                0x0000000000000364                UsageFault_Handler
                0x0000000000000366                SVC_Handler
                0x0000000000000368                DebugMon_Handler
                0x000000000000036a                PendSV_Handler
                0x000000000000036c                SysTick_Handler
                0x000000000000036e                RTC0_IRQHandler
                0x000000000000036e                RADIO_IRQHandler
                0x000000000000036e                PDM_IRQHandler
                0x000000000000036e                PWM1_IRQHandler
                0x000000000000036e                GPIOTE_IRQHandler
                0x000000000000036e                QDEC_IRQHandler
                0x000000000000036e                TIMER3_IRQHandler
                0x000000000000036e                PWM3_IRQHandler
                0x000000000000036e                FPU_IRQHandler
                0x000000000000036e                USBD_IRQHandler
                0x000000000000036e                SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler
                0x000000000000036e                SWI2_EGU2_IRQHandler
                0x000000000000036e                TEMP_IRQHandler
                0x000000000000036e                CRYPTOCELL_IRQHandler
                0x000000000000036e                I2S_IRQHandler
                0x000000000000036e                SWI4_EGU4_IRQHandler
                0x000000000000036e                UARTE1_IRQHandler
                0x000000000000036e                Dummy_Handler
                0x000000000000036e                TIMER1_IRQHandler
                0x000000000000036e                SPIM3_IRQHandler
                0x000000000000036e                PWM2_IRQHandler
                0x000000000000036e                ECB_IRQHandler
                0x000000000000036e                SPIM1_SPIS1_TWIM1_TWIS1_SPI1_TWI1_IRQHandler
                0x000000000000036e                CCM_AAR_IRQHandler
                0x000000000000036e                WDT_IRQHandler
                0x000000000000036e                QSPI_IRQHandler
                0x000000000000036e                SWI5_EGU5_IRQHandler
                0x000000000000036e                RNG_IRQHandler
                0x000000000000036e                PWM0_IRQHandler
                0x000000000000036e                SWI3_EGU3_IRQHandler
                0x000000000000036e                SWI1_EGU1_IRQHandler
                0x000000000000036e                SPIM2_SPIS2_SPI2_IRQHandler
                0x000000000000036e                NFCT_IRQHandler
                0x000000000000036e                TIMER4_IRQHandler
                0x000000000000036e                MWU_IRQHandler
                0x000000000000036e                TIMER2_IRQHandler
                0x000000000000036e                COMP_LPCOMP_IRQHandler
                0x0000000000000370                nRFInitialize
 .init          0x0000000000000374       0x5c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
                0x0000000000000374                Reset_Handler
                0x0000000000000378                afterInitialize
                0x000000000000039c                InitializeUserMemorySections
                0x00000000000003d0                __init_end__ = (__init_start__ + SIZEOF (.init))
                0x00000000000001d0                __init_size__ = SIZEOF (.init)
                0x00000000000003d0                __init_load_end__ = __init_end__
                0x0000000000000001                . = ASSERT (((__init_start__ == __init_end__) || ((__init_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .init is too large to fit in FLASH memory segment)
                0x00000000000003d0                __init_rodata_load_start__ = ALIGN (__init_end__, 0x4)

.init_rodata    0x00000000000003d0        0x0
                0x00000000000003d0                __init_rodata_start__ = .
 *(.init_rodata .init_rodata.*)
                0x00000000000003d0                __init_rodata_end__ = (__init_rodata_start__ + SIZEOF (.init_rodata))
                0x0000000000000000                __init_rodata_size__ = SIZEOF (.init_rodata)
                0x00000000000003d0                __init_rodata_load_end__ = __init_rodata_end__
                0x0000000000000001                . = ASSERT (((__init_rodata_start__ == __init_rodata_end__) || ((__init_rodata_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .init_rodata is too large to fit in FLASH memory segment)
                0x00000000000003d0                __text_load_start__ = ALIGN (__init_rodata_end__, 0x4)

.text           0x00000000000003d0     0x50f2
                0x00000000000003d0                __text_start__ = .
 *(.text .text.* .glue_7t .glue_7 .gnu.linkonce.t.* .gcc_except_table .ARM.extab* .gnu.linkonce.armextab.*)
 .glue_7        0x00000000000003d0        0x0 linker stubs
 .glue_7t       0x00000000000003d0        0x0 linker stubs
 .text.nrfx_coredep_delay_us
                0x00000000000003d0       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .text.nrf_delay_ms
                0x0000000000000400       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .text.nrf_log_backend_rtt_init
                0x000000000000042a        0xa Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
                0x000000000000042a                nrf_log_backend_rtt_init
 .text.serial_tx
                0x0000000000000434       0x84 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .text.nrf_log_backend_rtt_put
                0x00000000000004b8       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .text.nrf_log_backend_rtt_flush
                0x00000000000004e0        0xa Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .text.nrf_log_backend_rtt_panic_set
                0x00000000000004ea        0xa Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .text.nrf_log_backend_serial_put
                0x00000000000004f4      0x124 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
                0x00000000000004f4                nrf_log_backend_serial_put
 .text.nrf_log_backend_enable
                0x0000000000000618       0x12 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 *fill*         0x000000000000062a        0x2 
 .text.nrf_log_default_backends_init
                0x000000000000062c       0x3c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
                0x000000000000062c                nrf_log_default_backends_init
 .text.nrf_log_backend_put
                0x0000000000000668       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_backend_panic_set
                0x0000000000000684       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_backend_flush
                0x000000000000069c       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_backend_id_set
                0x00000000000006b4       0x1a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_backend_id_get
                0x00000000000006ce       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_backend_enable
                0x00000000000006de       0x12 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_backend_is_enabled
                0x00000000000006f0       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_init
                0x0000000000000700       0x74 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000000700                nrf_log_init
 .text.nrf_log_module_cnt_get
                0x0000000000000774       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000000774                nrf_log_module_cnt_get
 .text.module_idx_get
                0x0000000000000788       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_module_name_get
                0x00000000000007ec       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x00000000000007ec                nrf_log_module_name_get
 .text.nrf_log_color_id_get
                0x000000000000082c       0x70 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x000000000000082c                nrf_log_color_id_get
 .text.invalid_packets_omit
                0x000000000000089c       0x6e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 *fill*         0x000000000000090a        0x2 
 .text.log_skip
                0x000000000000090c      0x114 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.dropped_sat16_get
                0x0000000000000a20       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.std_header_set
                0x0000000000000a48       0xb4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.buf_prealloc
                0x0000000000000afc      0x124 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.std_n    0x0000000000000c20       0x90 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_frontend_std_0
                0x0000000000000cb0       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000000cb0                nrf_log_frontend_std_0
 .text.nrf_log_frontend_std_1
                0x0000000000000ccc       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000000ccc                nrf_log_frontend_std_1
 .text.nrf_log_frontend_std_2
                0x0000000000000cee       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000000cee                nrf_log_frontend_std_2
 .text.nrf_log_frontend_std_5
                0x0000000000000d16       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000000d16                nrf_log_frontend_std_5
 *fill*         0x0000000000000d4a        0x2 
 .text.buffer_is_empty
                0x0000000000000d4c       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000000d4c                buffer_is_empty
 .text.nrf_log_frontend_dequeue
                0x0000000000000d68      0x39c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000000d68                nrf_log_frontend_dequeue
 .text.backend_id_assign
                0x0000000000001104       0x68 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_backend_add
                0x000000000000116c       0x70 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x000000000000116c                nrf_log_backend_add
 .text.nrf_log_panic
                0x00000000000011dc       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x00000000000011dc                nrf_log_panic
 .text.timestamp_print
                0x000000000000121c        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .text.prefix_process
                0x0000000000001228       0xb0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .text.postfix_process
                0x00000000000012d8       0x60 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .text.nrf_log_std_entry_process
                0x0000000000001338      0x144 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
                0x0000000000001338                nrf_log_std_entry_process
 .text.nrf_log_hexdump_entry_process
                0x000000000000147c       0xf0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
                0x000000000000147c                nrf_log_hexdump_entry_process
 .text.app_error_save_and_stop
                0x000000000000156c       0x9c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
                0x000000000000156c                app_error_save_and_stop
 .text.app_error_handler
                0x0000000000001608       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
                0x0000000000001608                app_error_handler
 .text.app_error_fault_handler
                0x0000000000001624      0x104 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
                0x0000000000001624                app_error_fault_handler
 .text.app_util_disable_irq
                0x0000000000001728       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
                0x0000000000001728                app_util_disable_irq
 .text.app_util_enable_irq
                0x0000000000001740       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
                0x0000000000001740                app_util_enable_irq
 .text.app_util_critical_region_enter
                0x0000000000001760       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
                0x0000000000001760                app_util_critical_region_enter
 .text.app_util_critical_region_exit
                0x0000000000001788       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
                0x0000000000001788                app_util_critical_region_exit
 .text.privilege_level_get
                0x00000000000017b4       0x3a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
                0x00000000000017b4                privilege_level_get
 .text.assert_nrf_callback
                0x00000000000017ee       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
                0x00000000000017ee                assert_nrf_callback
 .text.nrf_atomic_u32_fetch_store
                0x000000000000181c       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
                0x000000000000181c                nrf_atomic_u32_fetch_store
 .text.nrf_atomic_u32_or
                0x000000000000184a       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
                0x000000000000184a                nrf_atomic_u32_or
 .text.nrf_atomic_u32_fetch_and
                0x000000000000187a       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
                0x000000000000187a                nrf_atomic_u32_fetch_and
 .text.nrf_atomic_u32_add
                0x00000000000018aa       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
                0x00000000000018aa                nrf_atomic_u32_add
 .text.nrf_atomic_u32_sub
                0x00000000000018da       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
                0x00000000000018da                nrf_atomic_u32_sub
 .text.nrf_atomic_flag_set
                0x000000000000190a       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
                0x000000000000190a                nrf_atomic_flag_set
 .text.nrf_atomic_flag_clear_fetch
                0x0000000000001922       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
                0x0000000000001922                nrf_atomic_flag_clear_fetch
 *fill*         0x000000000000193a        0x2 
 .text.nrf_balloc_idx2block
                0x000000000000193c       0x38 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .text.nrf_balloc_block2idx
                0x0000000000001974       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .text.nrf_balloc_init
                0x00000000000019a8       0xb8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
                0x00000000000019a8                nrf_balloc_init
 .text.nrf_balloc_alloc
                0x0000000000001a60       0x84 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
                0x0000000000001a60                nrf_balloc_alloc
 .text.nrf_balloc_free
                0x0000000000001ae4       0x58 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
                0x0000000000001ae4                nrf_balloc_free
 .text.nrf_fprintf_buffer_flush
                0x0000000000001b3c       0x44 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
                0x0000000000001b3c                nrf_fprintf_buffer_flush
 .text.nrf_fprintf
                0x0000000000001b80       0x74 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
                0x0000000000001b80                nrf_fprintf
 .text.buffer_add
                0x0000000000001bf4       0x4c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .text.string_print
                0x0000000000001c40       0xc2 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 *fill*         0x0000000000001d02        0x2 
 .text.unsigned_print
                0x0000000000001d04      0x130 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .text.int_print
                0x0000000000001e34      0x11c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .text.nrf_fprintf_fmt
                0x0000000000001f50      0x388 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
                0x0000000000001f50                nrf_fprintf_fmt
 .text.nrf_memobj_pool_init
                0x00000000000022d8       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
                0x00000000000022d8                nrf_memobj_pool_init
 .text.nrf_memobj_alloc
                0x00000000000022ee       0xae Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
                0x00000000000022ee                nrf_memobj_alloc
 .text.nrf_memobj_free
                0x000000000000239c       0x74 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
                0x000000000000239c                nrf_memobj_free
 .text.nrf_memobj_get
                0x0000000000002410       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
                0x0000000000002410                nrf_memobj_get
 .text.nrf_memobj_put
                0x000000000000242e       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
                0x000000000000242e                nrf_memobj_put
 *fill*         0x0000000000002462        0x2 
 .text.memobj_op
                0x0000000000002464      0x124 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .text.nrf_memobj_write
                0x0000000000002588       0x3c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
                0x0000000000002588                nrf_memobj_write
 .text.nrf_memobj_read
                0x00000000000025c4       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
                0x00000000000025c4                nrf_memobj_read
 .text.NVIC_ClearPendingIRQ
                0x0000000000002604       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .text.nrf_mtx_init
                0x0000000000002634       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .text.pwr_mgmt_fpu_sleep_prepare
                0x0000000000002660       0x54 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .text.nrf_pwr_mgmt_init
                0x00000000000026b4       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
                0x00000000000026b4                nrf_pwr_mgmt_init
 .text.nrf_pwr_mgmt_run
                0x00000000000026e0       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
                0x00000000000026e0                nrf_pwr_mgmt_run
 .text.nrf_ringbuf_init
                0x00000000000026f6       0x3a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
                0x00000000000026f6                nrf_ringbuf_init
 .text.nrf_section_iter_init
                0x0000000000002730       0x54 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
                0x0000000000002730                nrf_section_iter_init
 .text.nrf_strerror_get
                0x0000000000002784       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
                0x0000000000002784                nrf_strerror_get
 .text.nrf_strerror_find
                0x00000000000027ac       0x68 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
                0x00000000000027ac                nrf_strerror_find
 .text.NVIC_EnableIRQ
                0x0000000000002814       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.NVIC_DisableIRQ
                0x0000000000002840       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.NVIC_SetPendingIRQ
                0x0000000000002870       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.NVIC_ClearPendingIRQ
                0x00000000000028a0       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.nrfx_coredep_delay_us
                0x00000000000028d0       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.rtc1_start
                0x0000000000002900       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.rtc1_stop
                0x0000000000002940       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.rtc1_counter_get
                0x0000000000002990       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.ticks_diff_get
                0x00000000000029a0       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 *fill*         0x00000000000029b6        0x2 
 .text.rtc1_compare0_set
                0x00000000000029b8       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.timer_list_insert
                0x00000000000029d0       0xac Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.timer_list_remove
                0x0000000000002a7c       0xc0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.timer_timeouts_check_sched
                0x0000000000002b3c        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.timer_list_handler_sched
                0x0000000000002b48        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.timeout_handler_exec
                0x0000000000002b54       0x1a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 *fill*         0x0000000000002b6e        0x2 
 .text.timer_timeouts_check
                0x0000000000002b70       0xc8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.elapsed_ticks_acquire
                0x0000000000002c38       0x78 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.expired_timers_handler
                0x0000000000002cb0       0x94 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.list_insertions_handler
                0x0000000000002d44      0x1bc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.compare_reg_update
                0x0000000000002f00       0xb0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.timer_list_handler
                0x0000000000002fb0       0x80 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .text.RTC1_IRQHandler
                0x0000000000003030       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
                0x0000000000003030                RTC1_IRQHandler
 .text.SWI0_EGU0_IRQHandler
                0x0000000000003070        0xa Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
                0x0000000000003070                SWI0_EGU0_IRQHandler
 *fill*         0x000000000000307a        0x2 
 .text.nrf_ppi_channel_enable
                0x000000000000307c       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrf_ppi_channel_endpoint_setup
                0x00000000000030a0       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_channel_to_mask
                0x00000000000030d4       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.is_programmable_app_channel
                0x00000000000030ec       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.are_app_channels
                0x0000000000003118        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.is_app_channel
                0x0000000000003124       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 *fill*         0x000000000000314a        0x2 
 .text.is_allocated_channel
                0x000000000000314c       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.channel_allocated_set
                0x0000000000003180       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_channel_alloc
                0x00000000000031ac       0xa8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
                0x00000000000031ac                nrfx_ppi_channel_alloc
 .text.nrfx_ppi_channel_assign
                0x0000000000003254       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
                0x0000000000003254                nrfx_ppi_channel_assign
 .text.nrfx_ppi_channel_enable
                0x00000000000032c6       0x6a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
                0x00000000000032c6                nrfx_ppi_channel_enable
 .text.UARTE0_UART0_IRQHandler
                0x0000000000003330       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
                0x0000000000003330                UARTE0_UART0_IRQHandler
 .text.NVIC_EnableIRQ
                0x0000000000003354       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.NVIC_SetPriority
                0x0000000000003380       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text._NRFX_IRQ_PRIORITY_SET
                0x00000000000033d0       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text._NRFX_IRQ_ENABLE
                0x0000000000003410       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrf_saadc_task_trigger
                0x000000000000342c       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrf_saadc_task_address_get
                0x000000000000344a       0x1a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrf_saadc_event_check
                0x0000000000003464       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrf_saadc_event_clear
                0x000000000000348a       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 *fill*         0x00000000000034ba        0x2 
 .text.nrf_saadc_channel_input_set
                0x00000000000034bc       0x44 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrf_saadc_int_enable
                0x0000000000003500       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrf_saadc_int_disable
                0x0000000000003518       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrf_saadc_enable
                0x0000000000003530       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrf_saadc_buffer_init
                0x0000000000003540       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrf_saadc_resolution_set
                0x0000000000003560       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrf_saadc_oversample_set
                0x000000000000357c       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrf_saadc_oversample_get
                0x0000000000003598       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrf_saadc_channel_init
                0x00000000000035a8       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.SAADC_IRQHandler
                0x0000000000003634      0x250 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
                0x0000000000003634                SAADC_IRQHandler
 .text.nrfx_saadc_init
                0x0000000000003884       0xe0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
                0x0000000000003884                nrfx_saadc_init
 .text.nrfx_saadc_channel_init
                0x0000000000003964       0xfc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
                0x0000000000003964                nrfx_saadc_channel_init
 .text.nrfx_saadc_sample_task_get
                0x0000000000003a60       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
                0x0000000000003a60                nrfx_saadc_sample_task_get
 .text.nrfx_saadc_buffer_convert
                0x0000000000003a84      0x148 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
                0x0000000000003a84                nrfx_saadc_buffer_convert
 .text.nrf_timer_event_clear
                0x0000000000003bcc       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrf_timer_event_check
                0x0000000000003bf6       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrf_timer_int_enable_check
                0x0000000000003c1a       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrf_timer_compare_event_get
                0x0000000000003c3a       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrf_timer_compare_int_get
                0x0000000000003c4e       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.irq_handler
                0x0000000000003c62       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.TIMER0_IRQHandler
                0x0000000000003cf0       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
                0x0000000000003cf0                TIMER0_IRQHandler
 .text.NVIC_EnableIRQ
                0x0000000000003d08       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.NVIC_SetPriority
                0x0000000000003d34       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_get_irq_number
                0x0000000000003d84       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text._NRFX_IRQ_PRIORITY_SET
                0x0000000000003d94       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text._NRFX_IRQ_ENABLE
                0x0000000000003dd4       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text._NRFX_IRQ_IS_ENABLED
                0x0000000000003df0       0x4c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrf_clock_int_enable
                0x0000000000003e3c       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrf_clock_int_disable
                0x0000000000003e50       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrf_clock_task_trigger
                0x0000000000003e64       0x1a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrf_clock_event_clear
                0x0000000000003e7e       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrf_clock_event_check
                0x0000000000003ea6       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrf_clock_lf_src_set
                0x0000000000003ec8       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_power_clock_irq_init
                0x0000000000003edc       0x56 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 *fill*         0x0000000000003f32        0x2 
 .text.nrfx_clock_init
                0x0000000000003f34       0x4c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
                0x0000000000003f34                nrfx_clock_init
 .text.nrfx_clock_enable
                0x0000000000003f80       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
                0x0000000000003f80                nrfx_clock_enable
 .text.nrfx_clock_lfclk_start
                0x0000000000003fa8       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
                0x0000000000003fa8                nrfx_clock_lfclk_start
 .text.POWER_CLOCK_IRQHandler
                0x0000000000003fdc       0x68 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
                0x0000000000003fdc                POWER_CLOCK_IRQHandler
 .text.NVIC_EnableIRQ
                0x0000000000004044       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.NVIC_SetPriority
                0x0000000000004070       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text._NRFX_IRQ_PRIORITY_SET
                0x00000000000040c0       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text._NRFX_IRQ_ENABLE
                0x0000000000004100       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrf_rtc_cc_set
                0x000000000000411c       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrf_rtc_int_enable
                0x0000000000004138       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrf_rtc_int_disable
                0x000000000000414c       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrf_rtc_int_is_enabled
                0x0000000000004160       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrf_rtc_event_pending
                0x0000000000004176       0x1a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrf_rtc_event_clear
                0x0000000000004190       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrf_rtc_counter_get
                0x00000000000041ba       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 *fill*         0x00000000000041ca        0x2 
 .text.nrf_rtc_prescaler_set
                0x00000000000041cc       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrf_rtc_task_trigger
                0x00000000000041fc       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrf_rtc_event_enable
                0x000000000000421a       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrf_rtc_event_disable
                0x000000000000422e       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 *fill*         0x0000000000004242        0x2 
 .text.nrfx_rtc_init
                0x0000000000004244       0xe4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
                0x0000000000004244                nrfx_rtc_init
 .text.nrfx_rtc_enable
                0x0000000000004328       0x54 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
                0x0000000000004328                nrfx_rtc_enable
 .text.nrfx_rtc_cc_set
                0x000000000000437c      0x140 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
                0x000000000000437c                nrfx_rtc_cc_set
 .text.irq_handler
                0x00000000000044bc      0x114 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.RTC2_IRQHandler
                0x00000000000045d0       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
                0x00000000000045d0                RTC2_IRQHandler
 .text.nrf_drv_clock_init
                0x00000000000045e4       0x54 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
                0x00000000000045e4                nrf_drv_clock_init
 .text.item_enqueue
                0x0000000000004638       0x38 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.item_dequeue
                0x0000000000004670       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_lfclk_request
                0x0000000000004690       0x9c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
                0x0000000000004690                nrf_drv_clock_lfclk_request
 .text.clock_clk_started_notify
                0x000000000000472c       0x4c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.clock_irq_handler
                0x0000000000004778       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_rtc_event_address_get
                0x00000000000047b8       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .text.nrf_rtc_task_trigger
                0x00000000000047d0       0x1e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .text.nrfx_rtc_counter_clear
                0x00000000000047ee       0x1a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .text.nrfx_rtc_event_address_get
                0x0000000000004808       0x26 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .text.nrf_saadc_task_address_get
                0x000000000000482e       0x1a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .text.nrf_saadc_event_address_get
                0x0000000000004848       0x1a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 *fill*         0x0000000000004862        0x2 
 .text.ppi_init
                0x0000000000004864      0x100 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .text.rtc_handler
                0x0000000000004964       0x6c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .text.rtc_config
                0x00000000000049d0       0x7c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .text.saadc_callback
                0x0000000000004a4c       0xd8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
                0x0000000000004a4c                saadc_callback
 .text.saadc_init
                0x0000000000004b24       0xa8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
                0x0000000000004b24                saadc_init
 .text.lfclk_config
                0x0000000000004bcc       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .text.log_init
                0x0000000000004bfc       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .text.pwr_mgmt_init
                0x0000000000004c30       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .text.main     0x0000000000004c5c       0x58 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
                0x0000000000004c5c                main
 .text._DoInit  0x0000000000004cb4       0x9c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text._WriteBlocking
                0x0000000000004d50       0xb2 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text._WriteNoCheck
                0x0000000000004e02       0x7e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text._GetAvailWriteSpace
                0x0000000000004e80       0x3c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_WriteNoLock
                0x0000000000004ebc       0xa0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
                0x0000000000004ebc                SEGGER_RTT_WriteNoLock
 .text.SEGGER_RTT_Init
                0x0000000000004f5c        0xa Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
                0x0000000000004f5c                SEGGER_RTT_Init
 *fill*         0x0000000000004f66        0x2 
 .text.NVIC_SystemReset
                0x0000000000004f68       0x2c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .text.SystemCoreClockUpdate
                0x0000000000004f94       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
                0x0000000000004f94                SystemCoreClockUpdate
 .text.SystemInit
                0x0000000000004fa8      0x254 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
                0x0000000000004fa8                SystemInit
 .text.errata_36
                0x00000000000051fc       0x48 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .text.errata_66
                0x0000000000005244       0x48 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .text.errata_98
                0x000000000000528c       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .text.errata_103
                0x00000000000052b0       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .text.errata_115
                0x00000000000052d4       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .text.errata_120
                0x00000000000052f8       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .text.errata_136
                0x000000000000531c       0x48 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .text.libc.__RAL_ascii_isctype
                0x0000000000005364       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_ascii_toupper
                0x0000000000005380        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_ascii_tolower
                0x000000000000538c        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_ascii_wctomb
                0x0000000000005398       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000005398                __RAL_ascii_wctomb
 .text.libc.__RAL_ascii_mbtowc
                0x00000000000053a8       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x00000000000053a8                __RAL_ascii_mbtowc
 .text.libc.__RAL_ascii_towupper
                0x00000000000053cc        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_ascii_towlower
                0x00000000000053d8        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_ascii_iswctype
                0x00000000000053e4       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isprint
                0x0000000000005400       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000005400                isprint
 .text.libc.memcpy
                0x0000000000005410       0x52 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
                0x0000000000005410                __aeabi_memcpy
                0x0000000000005410                memcpy
                0x000000000000541c                __aeabi_memcpy8
                0x000000000000541c                __aeabi_memcpy4
 .text.libc.strlen
                0x0000000000005462       0x60 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
                0x0000000000005462                strlen
                0x00000000000054c2                __text_end__ = (__text_start__ + SIZEOF (.text))
                0x00000000000050f2                __text_size__ = SIZEOF (.text)
                0x00000000000054c2                __text_load_end__ = __text_end__

.vfp11_veneer   0x0000000100000000        0x0
 .vfp11_veneer  0x0000000100000000        0x0 linker stubs

.v4_bx          0x0000000100000000        0x0
 .v4_bx         0x0000000100000000        0x0 linker stubs

.iplt           0x0000000100000000        0x0
 .iplt          0x0000000100000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
                0x0000000000000001                . = ASSERT (((__text_start__ == __text_end__) || ((__text_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .text is too large to fit in FLASH memory segment)
                0x00000000000054c4                __pwr_mgmt_data_load_start__ = ALIGN (__text_end__, 0x4)

.pwr_mgmt_data  0x00000000000054c4        0x0
                0x00000000000054c4                __pwr_mgmt_data_start__ = .
                0x00000000000054c4                __start_pwr_mgmt_data = __pwr_mgmt_data_start__
 *(SORT_BY_NAME(.pwr_mgmt_data*))
                0x00000000000054c4                __pwr_mgmt_data_end__ = (__pwr_mgmt_data_start__ + SIZEOF (.pwr_mgmt_data))
                0x0000000000000000                __pwr_mgmt_data_size__ = SIZEOF (.pwr_mgmt_data)
                0x00000000000054c4                __stop_pwr_mgmt_data = __pwr_mgmt_data_end__
                0x00000000000054c4                __pwr_mgmt_data_load_end__ = __pwr_mgmt_data_end__
                0x0000000000000001                . = ASSERT (((__pwr_mgmt_data_start__ == __pwr_mgmt_data_end__) || ((__pwr_mgmt_data_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .pwr_mgmt_data is too large to fit in FLASH memory segment)
                0x00000000000054c4                __log_const_data_load_start__ = ALIGN (__pwr_mgmt_data_end__, 0x4)

.log_const_data
                0x00000000000054c4       0x58
                0x00000000000054c4                __log_const_data_start__ = .
                0x00000000000054c4                __start_log_const_data = __log_const_data_start__
 *(SORT_BY_NAME(.log_const_data*))
 .log_const_data_CLOCK
                0x00000000000054c4        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
                0x00000000000054c4                m_nrf_log_CLOCK_logs_data_const
 .log_const_data_PPI
                0x00000000000054cc        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
                0x00000000000054cc                m_nrf_log_PPI_logs_data_const
 .log_const_data_PRS
                0x00000000000054d4        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
                0x00000000000054d4                m_nrf_log_PRS_logs_data_const
 .log_const_data_RTC
                0x00000000000054dc        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
                0x00000000000054dc                m_nrf_log_RTC_logs_data_const
 .log_const_data_SAADC
                0x00000000000054e4        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
                0x00000000000054e4                m_nrf_log_SAADC_logs_data_const
 .log_const_data_TIMER
                0x00000000000054ec        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
                0x00000000000054ec                m_nrf_log_TIMER_logs_data_const
 .log_const_data_UART
                0x00000000000054f4        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
                0x00000000000054f4                m_nrf_log_UART_logs_data_const
 .log_const_data_UARTE
                0x00000000000054fc        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
                0x00000000000054fc                m_nrf_log_UARTE_logs_data_const
 .log_const_data_app
                0x0000000000005504        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000005504                m_nrf_log_app_logs_data_const
 .log_const_data_clock
                0x000000000000550c        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
                0x000000000000550c                m_nrf_log_clock_logs_data_const
 .log_const_data_pwr_mgmt
                0x0000000000005514        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
                0x0000000000005514                m_nrf_log_pwr_mgmt_logs_data_const
                0x000000000000551c                __log_const_data_end__ = (__log_const_data_start__ + SIZEOF (.log_const_data))
                0x0000000000000058                __log_const_data_size__ = SIZEOF (.log_const_data)
                0x000000000000551c                __stop_log_const_data = __log_const_data_end__
                0x000000000000551c                __log_const_data_load_end__ = __log_const_data_end__
                0x0000000000000001                . = ASSERT (((__log_const_data_start__ == __log_const_data_end__) || ((__log_const_data_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .log_const_data is too large to fit in FLASH memory segment)
                0x000000000000551c                __log_backends_load_start__ = ALIGN (__log_const_data_end__, 0x4)

.log_backends   0x000000000000551c       0x10
                0x000000000000551c                __log_backends_start__ = .
                0x000000000000551c                __start_log_backends = __log_backends_start__
 *(SORT_BY_NAME(.log_backends*))
 .log_backends  0x000000000000551c       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
                0x000000000000552c                __log_backends_end__ = (__log_backends_start__ + SIZEOF (.log_backends))
                0x0000000000000010                __log_backends_size__ = SIZEOF (.log_backends)
                0x000000000000552c                __stop_log_backends = __log_backends_end__
                0x000000000000552c                __log_backends_load_end__ = __log_backends_end__
                0x0000000000000001                . = ASSERT (((__log_backends_start__ == __log_backends_end__) || ((__log_backends_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .log_backends is too large to fit in FLASH memory segment)
                0x000000000000552c                __nrf_balloc_load_start__ = ALIGN (__log_backends_end__, 0x4)

.nrf_balloc     0x000000000000552c       0x14
                0x000000000000552c                __nrf_balloc_start__ = .
                0x000000000000552c                __start_nrf_balloc = __nrf_balloc_start__
 *(.nrf_balloc*)
 .nrf_balloc    0x000000000000552c       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x000000000000552c                log_mempool
                0x0000000000005540                __nrf_balloc_end__ = (__nrf_balloc_start__ + SIZEOF (.nrf_balloc))
                0x0000000000000014                __nrf_balloc_size__ = SIZEOF (.nrf_balloc)
                0x0000000000005540                __stop_nrf_balloc = __nrf_balloc_end__
                0x0000000000005540                __nrf_balloc_load_end__ = __nrf_balloc_end__
                0x0000000000000001                . = ASSERT (((__nrf_balloc_start__ == __nrf_balloc_end__) || ((__nrf_balloc_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .nrf_balloc is too large to fit in FLASH memory segment)
                0x0000000000005540                __nrf_sections_load_start__ = ALIGN (__nrf_balloc_end__, 0x4)

.nrf_sections   0x0000000000005540        0x0
                0x0000000000005540                __nrf_sections_start__ = .
                0x0000000000005540                __start_nrf_sections = __nrf_sections_start__
 *(.nrf_sections .nrf_sections.*)
                0x0000000000005540                __nrf_sections_end__ = (__nrf_sections_start__ + SIZEOF (.nrf_sections))
                0x0000000000000000                __nrf_sections_size__ = SIZEOF (.nrf_sections)
                0x0000000000005540                __nrf_sections_load_end__ = __nrf_sections_end__
                0x0000000000000001                . = ASSERT (((__nrf_sections_start__ == __nrf_sections_end__) || ((__nrf_sections_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .nrf_sections is too large to fit in FLASH memory segment)
                0x0000000000005540                __log_dynamic_data_load_start__ = ALIGN (__nrf_sections_end__, 0x4)

.log_dynamic_data
                0x0000000020000000        0x0 load address 0x0000000000005540
                0x0000000020000000                __log_dynamic_data_start__ = .
 *(SORT_BY_NAME(.log_dynamic_data*))
                0x0000000020000000                __log_dynamic_data_end__ = (__log_dynamic_data_start__ + SIZEOF (.log_dynamic_data))
                0x0000000000000000                __log_dynamic_data_size__ = SIZEOF (.log_dynamic_data)
                0x0000000000005540                __log_dynamic_data_load_end__ = (__log_dynamic_data_load_start__ + SIZEOF (.log_dynamic_data))
                0x0000000000000001                . = ASSERT (((__log_dynamic_data_load_start__ == __log_dynamic_data_load_end__) || ((__log_dynamic_data_load_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .log_dynamic_data is too large to fit in FLASH memory segment)

.log_dynamic_data_run
                0x0000000020000000        0x0
                0x0000000020000000                __log_dynamic_data_run_start__ = .
                0x0000000020000000                __start_log_dynamic_data = __log_dynamic_data_run_start__
                0x0000000020000000                __log_dynamic_data_run_end__ = (__log_dynamic_data_run_start__ + SIZEOF (.log_dynamic_data))
                0x0000000000000000                __log_dynamic_data_run_size__ = (__log_dynamic_data_run_end__ - __log_dynamic_data_run_start__)
                0x0000000020000000                __stop_log_dynamic_data = __log_dynamic_data_run_end__
                0x0000000020000000                __log_dynamic_data_run_load_end__ = __log_dynamic_data_run_end__
                0x0000000000000001                . = ASSERT (((__log_dynamic_data_run_start__ == __log_dynamic_data_run_end__) || ((__log_dynamic_data_run_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .log_dynamic_data_run is too large to fit in RAM memory segment)
                0x0000000000005540                __log_filter_data_load_start__ = ALIGN ((__log_dynamic_data_load_start__ + SIZEOF (.log_dynamic_data)), 0x4)

.log_filter_data
                0x0000000020000000        0x0 load address 0x0000000000005540
                0x0000000020000000                __log_filter_data_start__ = .
 *(SORT_BY_NAME(.log_filter_data*))
                0x0000000020000000                __log_filter_data_end__ = (__log_filter_data_start__ + SIZEOF (.log_filter_data))
                0x0000000000000000                __log_filter_data_size__ = SIZEOF (.log_filter_data)
                0x0000000000005540                __log_filter_data_load_end__ = (__log_filter_data_load_start__ + SIZEOF (.log_filter_data))
                0x0000000000000001                . = ASSERT (((__log_filter_data_load_start__ == __log_filter_data_load_end__) || ((__log_filter_data_load_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .log_filter_data is too large to fit in FLASH memory segment)

.log_filter_data_run
                0x0000000020000000        0x0
                0x0000000020000000                __log_filter_data_run_start__ = .
                0x0000000020000000                __start_log_filter_data = __log_filter_data_run_start__
                0x0000000020000000                __log_filter_data_run_end__ = (__log_filter_data_run_start__ + SIZEOF (.log_filter_data))
                0x0000000000000000                __log_filter_data_run_size__ = (__log_filter_data_run_end__ - __log_filter_data_run_start__)
                0x0000000020000000                __stop_log_filter_data = __log_filter_data_run_end__
                0x0000000020000000                __log_filter_data_run_load_end__ = __log_filter_data_run_end__
                0x0000000000000001                . = ASSERT (((__log_filter_data_run_start__ == __log_filter_data_run_end__) || ((__log_filter_data_run_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .log_filter_data_run is too large to fit in RAM memory segment)
                0x0000000020000000                __nrf_sections_run_end_load_start__ = ALIGN (__log_filter_data_run_end__, 0x4)

.nrf_sections_run_end
                0x0000000020000000        0x0
                0x0000000020000000                __nrf_sections_run_end_start__ = .
                0x0000000020000000                __end_nrf_sections_run = __nrf_sections_run_end_start__
 *(.nrf_sections_run_end .nrf_sections_run_end.*)
                0x0000000020000000                __nrf_sections_run_end_end__ = (__nrf_sections_run_end_start__ + SIZEOF (.nrf_sections_run_end))
                0x0000000000000000                __nrf_sections_run_end_size__ = SIZEOF (.nrf_sections_run_end)
                0x0000000020000000                __nrf_sections_run_end_load_end__ = __nrf_sections_run_end_end__
                0x0000000000000001                . = ASSERT (((__nrf_sections_run_end_start__ == __nrf_sections_run_end_end__) || ((__nrf_sections_run_end_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .nrf_sections_run_end is too large to fit in RAM memory segment)
                0x0000000000005540                __dtors_load_start__ = ALIGN ((__log_filter_data_load_start__ + SIZEOF (.log_filter_data)), 0x4)

.dtors          0x0000000000005540        0x0
                0x0000000000005540                __dtors_start__ = .
 *(SORT_BY_NAME(.dtors.*))
 *(.dtors)
 *(.fini_array)
 *(SORT_BY_NAME(.fini_array.*))
                0x0000000000005540                __dtors_end__ = (__dtors_start__ + SIZEOF (.dtors))
                0x0000000000000000                __dtors_size__ = SIZEOF (.dtors)
                0x0000000000005540                __dtors_load_end__ = __dtors_end__
                0x0000000000000001                . = ASSERT (((__dtors_start__ == __dtors_end__) || ((__dtors_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .dtors is too large to fit in FLASH memory segment)
                0x0000000000005540                __ctors_load_start__ = ALIGN (__dtors_end__, 0x4)

.ctors          0x0000000000005540        0x0
                0x0000000000005540                __ctors_start__ = .
 *(SORT_BY_NAME(.ctors.*))
 *(.ctors)
 *(.init_array)
 *(SORT_BY_NAME(.init_array.*))
                0x0000000000005540                __ctors_end__ = (__ctors_start__ + SIZEOF (.ctors))
                0x0000000000000000                __ctors_size__ = SIZEOF (.ctors)
                0x0000000000005540                __ctors_load_end__ = __ctors_end__
                0x0000000000000001                . = ASSERT (((__ctors_start__ == __ctors_end__) || ((__ctors_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .ctors is too large to fit in FLASH memory segment)
                0x0000000000005540                __rodata_load_start__ = ALIGN (__ctors_end__, 0x4)

.rodata         0x0000000000005540     0x1222
                0x0000000000005540                __rodata_start__ = .
 *(.rodata .rodata.* .gnu.linkonce.r.*)
 .rodata.nrf_log_backend_rtt_api
                0x0000000000005540        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
                0x0000000000005540                nrf_log_backend_rtt_api
 *fill*         0x000000000000554c        0x4 
 .rodata.delay_machine_code.0
                0x0000000000005550        0x6 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 *fill*         0x0000000000005556        0x2 
 .rodata        0x0000000000005558       0x74 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .rodata.m_log_push_ringbuf
                0x00000000000055cc        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .rodata        0x00000000000055d8       0x71 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 *fill*         0x0000000000005649        0x3 
 .rodata        0x000000000000564c       0xaa Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 *fill*         0x00000000000056f6        0x2 
 .rodata        0x00000000000056f8       0x70 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .rodata        0x0000000000005768       0x5a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 *fill*         0x00000000000057c2        0x2 
 .rodata        0x00000000000057c4       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 *fill*         0x0000000000005819        0x3 
 .rodata        0x000000000000581c       0x4b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 *fill*         0x0000000000005867        0x1 
 .rodata        0x0000000000005868       0x52 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 *fill*         0x00000000000058ba        0x2 
 .rodata._aV2C.0
                0x00000000000058bc       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .rodata        0x00000000000058cc       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 *fill*         0x0000000000005921        0x3 
 .rodata        0x0000000000005924       0xf1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 *fill*         0x0000000000005a15        0x3 
 .rodata.pwr_mgmt_data
                0x0000000000005a18        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .rodata        0x0000000000005a24       0x6e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 *fill*         0x0000000000005a92        0x2 
 .rodata.m_unknown_str
                0x0000000000005a94       0x13 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 *fill*         0x0000000000005aa7        0x1 
 .rodata        0x0000000000005aa8      0x3bd Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 *fill*         0x0000000000005e65        0x3 
 .rodata.nrf_strerror_array
                0x0000000000005e68      0x118 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .rodata.delay_machine_code.0
                0x0000000000005f80        0x6 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 *fill*         0x0000000000005f86        0x2 
 .rodata        0x0000000000005f88        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .rodata        0x0000000000005f8c       0x58 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .rodata        0x0000000000005fe4       0xba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 *fill*         0x000000000000609e        0x2 
 .rodata        0x00000000000060a0       0x8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 *fill*         0x000000000000612a        0x2 
 .rodata        0x000000000000612c       0xb9 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 *fill*         0x00000000000061e5        0x3 
 .rodata        0x00000000000061e8       0xba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 *fill*         0x00000000000062a2        0x2 
 .rodata        0x00000000000062a4       0x8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 *fill*         0x000000000000632e        0x2 
 .rodata        0x0000000000006330       0xb4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .rodata        0x00000000000063e4       0x5c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .rodata.rtc    0x0000000000006440        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
                0x0000000000006440                rtc
 .rodata        0x0000000000006448       0xbe Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 *fill*         0x0000000000006506        0x2 
 .rodata.default_config.0
                0x0000000000006508        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .rodata        0x000000000000650c       0x17 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 *fill*         0x0000000000006523        0x1 
 .rodata.libc.__RAL_find_locale.str1.4
                0x0000000000006524        0xa C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 *fill*         0x000000000000652e        0x2 
 .rodata.libc.__RAL_ascii_ctype_map
                0x0000000000006530       0x80 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000006530                __RAL_ascii_ctype_map
 .rodata.libc.__RAL_ascii_ctype_mask
                0x00000000000065b0        0xd C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 *fill*         0x00000000000065bd        0x3 
 .rodata.libc.__RAL_c_locale
                0x00000000000065c0        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x00000000000065c0                __RAL_c_locale
 .rodata.libc.__RAL_c_locale_abbrev_day_names
                0x00000000000065cc       0x1d C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x00000000000065cc                __RAL_c_locale_abbrev_day_names
 *fill*         0x00000000000065e9        0x3 
 .rodata.libc.__RAL_c_locale_abbrev_month_names
                0x00000000000065ec       0x31 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x00000000000065ec                __RAL_c_locale_abbrev_month_names
 *fill*         0x000000000000661d        0x3 
 .rodata.libc.__RAL_c_locale_am_pm_indicator
                0x0000000000006620        0x7 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000006620                __RAL_c_locale_am_pm_indicator
 *fill*         0x0000000000006627        0x1 
 .rodata.libc.__RAL_c_locale_data
                0x0000000000006628       0x58 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000006628                __RAL_c_locale_data
 .rodata.libc.__RAL_c_locale_date_format
                0x0000000000006680        0x9 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000006680                __RAL_c_locale_date_format
 *fill*         0x0000000000006689        0x3 
 .rodata.libc.__RAL_c_locale_date_time_format
                0x000000000000668c        0xf C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x000000000000668c                __RAL_c_locale_date_time_format
 *fill*         0x000000000000669b        0x1 
 .rodata.libc.__RAL_c_locale_day_names
                0x000000000000669c       0x3a C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x000000000000669c                __RAL_c_locale_day_names
 *fill*         0x00000000000066d6        0x2 
 .rodata.libc.__RAL_c_locale_month_names
                0x00000000000066d8       0x57 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x00000000000066d8                __RAL_c_locale_month_names
 *fill*         0x000000000000672f        0x1 
 .rodata.libc.__RAL_c_locale_time_format
                0x0000000000006730        0x9 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000006730                __RAL_c_locale_time_format
 *fill*         0x0000000000006739        0x3 
 .rodata.libc.__RAL_codeset_ascii
                0x000000000000673c       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x000000000000673c                __RAL_codeset_ascii
 .rodata.libc.__RAL_data_empty_string
                0x000000000000675c        0x1 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x000000000000675c                __RAL_data_empty_string
 *fill*         0x000000000000675d        0x3 
 .rodata.libc.__RAL_data_utf8_period
                0x0000000000006760        0x2 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000006760                __RAL_data_utf8_period
                0x0000000000006762                __rodata_end__ = (__rodata_start__ + SIZEOF (.rodata))
                0x0000000000001222                __rodata_size__ = SIZEOF (.rodata)
                0x0000000000006762                __rodata_load_end__ = __rodata_end__

.rel.dyn        0x0000000000006764        0x0
 .rel.iplt      0x0000000000006764        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
                0x0000000000000001                . = ASSERT (((__rodata_start__ == __rodata_end__) || ((__rodata_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .rodata is too large to fit in FLASH memory segment)
                0x0000000000006764                __ARM.exidx_load_start__ = ALIGN (__rodata_end__, 0x4)

.ARM.exidx      0x0000000000006764        0x0
                0x0000000000006764                __ARM.exidx_start__ = .
                0x0000000000006764                __exidx_start = __ARM.exidx_start__
 *(.ARM.exidx .ARM.exidx.*)
                0x0000000000006764                __ARM.exidx_end__ = (__ARM.exidx_start__ + SIZEOF (.ARM.exidx))
                0x0000000000000000                __ARM.exidx_size__ = SIZEOF (.ARM.exidx)
                0x0000000000006764                __exidx_end = __ARM.exidx_end__
                0x0000000000006764                __ARM.exidx_load_end__ = __ARM.exidx_end__
                0x0000000000000001                . = ASSERT (((__ARM.exidx_start__ == __ARM.exidx_end__) || ((__ARM.exidx_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .ARM.exidx is too large to fit in FLASH memory segment)
                0x0000000000006764                __fast_load_start__ = ALIGN (__ARM.exidx_end__, 0x4)

.fast           0x0000000020000000        0x0 load address 0x0000000000006764
                0x0000000020000000                __fast_start__ = .
 *(.fast .fast.*)
                0x0000000020000000                __fast_end__ = (__fast_start__ + SIZEOF (.fast))
                0x0000000000000000                __fast_size__ = SIZEOF (.fast)
                0x0000000000006764                __fast_load_end__ = (__fast_load_start__ + SIZEOF (.fast))
                0x0000000000000001                . = ASSERT (((__fast_load_start__ == __fast_load_end__) || ((__fast_load_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .fast is too large to fit in FLASH memory segment)

.fast_run       0x0000000020000000        0x0
                0x0000000020000000                __fast_run_start__ = .
                0x0000000020000000                __fast_run_end__ = (__fast_run_start__ + SIZEOF (.fast))
                0x0000000000000000                __fast_run_size__ = (__fast_run_end__ - __fast_run_start__)
                0x0000000020000000                __fast_run_load_end__ = __fast_run_end__
                0x0000000000000001                . = ASSERT (((__fast_run_start__ == __fast_run_end__) || ((__fast_run_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .fast_run is too large to fit in RAM memory segment)
                0x0000000000006764                __data_load_start__ = ALIGN ((__fast_load_start__ + SIZEOF (.fast)), 0x4)

.data           0x0000000020000000       0x58 load address 0x0000000000006764
                0x0000000020000000                __data_start__ = .
 *(.data .data.* .gnu.linkonce.d.*)
 .data.log_backend_cb_rtt_log_backend
                0x0000000020000000        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .data.severity_names
                0x0000000020000008       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .data.m_colors
                0x000000002000001c       0x24 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .data.SystemCoreClock
                0x0000000020000040        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
                0x0000000020000040                SystemCoreClock
 .data.libc.__RAL_global_locale
                0x0000000020000044       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000020000044                __RAL_global_locale
                0x0000000020000058                __data_end__ = (__data_start__ + SIZEOF (.data))
                0x0000000000000058                __data_size__ = SIZEOF (.data)
                0x00000000000067bc                __data_load_end__ = (__data_load_start__ + SIZEOF (.data))

.igot.plt       0x0000000100000000        0x0
 .igot.plt      0x0000000100000000        0x0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
                0x0000000000000001                . = ASSERT (((__data_load_start__ == __data_load_end__) || ((__data_load_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .data is too large to fit in FLASH memory segment)

.data_run       0x0000000020000000        0x0
                0x0000000020000000                __data_run_start__ = .
                0x0000000020000058                __data_run_end__ = (__data_run_start__ + SIZEOF (.data))
                0x0000000000000058                __data_run_size__ = (__data_run_end__ - __data_run_start__)
                0x0000000020000058                __data_run_load_end__ = __data_run_end__
                0x0000000000000001                . = ASSERT (((__data_run_start__ == __data_run_end__) || ((__data_run_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .data_run is too large to fit in RAM memory segment)
                0x00000000000067bc                __tdata_load_start__ = ALIGN ((__data_load_start__ + SIZEOF (.data)), 0x4)

.tdata          0x0000000020000058        0x0 load address 0x00000000000067bc
                0x0000000020000058                __tdata_start__ = .
 *(.tdata .tdata.*)
                0x0000000020000058                __tdata_end__ = (__tdata_start__ + SIZEOF (.tdata))
                0x0000000000000000                __tdata_size__ = SIZEOF (.tdata)
                0x00000000000067bc                __tdata_load_end__ = (__tdata_load_start__ + SIZEOF (.tdata))
                0x00000000000067bc                __FLASH_segment_used_end__ = (ALIGN ((__data_load_start__ + SIZEOF (.data)), 0x4) + SIZEOF (.tdata))
                0x00000000000067bc                __FLASH_segment_used_size__ = (__FLASH_segment_used_end__ - __FLASH_segment_start__)
                0x0000000000000001                . = ASSERT (((__tdata_load_start__ == __tdata_load_end__) || ((__tdata_load_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .tdata is too large to fit in FLASH memory segment)

.tdata_run      0x0000000020000058        0x0
                0x0000000020000058                __tdata_run_start__ = .
                0x0000000020000058                __tdata_run_end__ = (__tdata_run_start__ + SIZEOF (.tdata))
                0x0000000000000000                __tdata_run_size__ = (__tdata_run_end__ - __tdata_run_start__)
                0x0000000020000058                __tdata_run_load_end__ = __tdata_run_end__
                0x0000000000000001                . = ASSERT (((__tdata_run_start__ == __tdata_run_end__) || ((__tdata_run_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .tdata_run is too large to fit in RAM memory segment)
                0x0000000020000058                __bss_load_start__ = ALIGN (__tdata_run_end__, 0x4)

.bss            0x0000000020000058      0xa24
                0x0000000020000058                __bss_start__ = .
 *(.bss .bss.* .gnu.linkonce.b.*)
 .bss.m_host_present
                0x0000000020000058        0x1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 *fill*         0x0000000020000059        0x3 
 .bss.m_string_buff
                0x000000002000005c       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .bss.log_mempool_nrf_balloc_pool_stack
                0x000000002000009c        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .bss.log_mempool_nrf_balloc_pool_mem
                0x00000000200000a4       0xc0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .bss.log_mempool_nrf_balloc_cb
                0x0000000020000164        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .bss.m_log_push_ringbuf_buf
                0x000000002000016c       0x80 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .bss.m_log_push_ringbuf_cb
                0x00000000200001ec       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .bss.m_log_data
                0x0000000020000204      0x424 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .bss.m_error_data.0
                0x0000000020000628       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .bss.m_in_critical_region
                0x0000000020000648        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .bss.m_sysoff_mtx
                0x000000002000064c        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .bss.m_shutdown_started
                0x0000000020000650        0x1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 *fill*         0x0000000020000651        0x3 
 .bss.m_handlers_iter
                0x0000000020000654        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .bss.m_op_queue
                0x000000002000065c      0x10c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .bss.mp_timer_id_head
                0x0000000020000768        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .bss.m_ticks_latest
                0x000000002000076c        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .bss.m_ticks_elapsed
                0x0000000020000770        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .bss.m_ticks_elapsed_q_read_ind
                0x0000000020000778        0x1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .bss.m_ticks_elapsed_q_write_ind
                0x0000000020000779        0x1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .bss.m_rtc1_running
                0x000000002000077a        0x1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .bss.m_rtc1_reset
                0x000000002000077b        0x1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .bss.m_channels_allocated
                0x000000002000077c        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .bss.m_prs_box_4
                0x0000000020000780        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .bss.m_cb      0x0000000020000788       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .bss.m_cb      0x00000000200007b8        0xc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .bss.m_clock_cb
                0x00000000200007c4        0x8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .bss.m_handlers
                0x00000000200007cc        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .bss.m_cb      0x00000000200007d0        0x3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 *fill*         0x00000000200007d3        0x1 
 .bss.m_clock_cb
                0x00000000200007d4       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .bss.m_ppi_channel
                0x00000000200007e8        0x1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .bss.m_start_SAADC_ppi_channel
                0x00000000200007e9        0x1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 *fill*         0x00000000200007ea        0x2 
 .bss.m_buffer_pool
                0x00000000200007ec        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .bss.m_adc_evt_counter
                0x00000000200007f0        0x4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .bss._SEGGER_RTT
                0x00000000200007f4       0x78 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
                0x00000000200007f4                _SEGGER_RTT
 .bss._acUpBuffer
                0x000000002000086c      0x200 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .bss._acDownBuffer
                0x0000000020000a6c       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 *(COMMON)
                0x0000000020000a7c                __bss_end__ = (__bss_start__ + SIZEOF (.bss))
                0x0000000000000a24                __bss_size__ = SIZEOF (.bss)
                0x0000000020000a7c                __bss_load_end__ = __bss_end__
                0x0000000000000001                . = ASSERT (((__bss_start__ == __bss_end__) || ((__bss_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .bss is too large to fit in RAM memory segment)
                0x0000000020000a7c                __tbss_load_start__ = ALIGN (__bss_end__, 0x4)

.tbss           0x0000000020000a7c        0x0
                0x0000000020000a7c                __tbss_start__ = .
 *(.tbss .tbss.*)
                0x0000000020000a7c                __tbss_end__ = (__tbss_start__ + SIZEOF (.tbss))
                0x0000000000000000                __tbss_size__ = SIZEOF (.tbss)
                0x0000000020000a7c                __tbss_load_end__ = __tbss_end__
                0x0000000000000001                . = ASSERT (((__tbss_start__ == __tbss_end__) || ((__tbss_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .tbss is too large to fit in RAM memory segment)
                0x0000000020000a7c                __non_init_load_start__ = ALIGN (__tbss_end__, 0x4)

.non_init       0x0000000020000a7c        0x0
                0x0000000020000a7c                __non_init_start__ = .
 *(.non_init .non_init.*)
                0x0000000020000a7c                __non_init_end__ = (__non_init_start__ + SIZEOF (.non_init))
                0x0000000000000000                __non_init_size__ = SIZEOF (.non_init)
                0x0000000020000a7c                __non_init_load_end__ = __non_init_end__
                0x0000000000000001                . = ASSERT (((__non_init_start__ == __non_init_end__) || ((__non_init_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .non_init is too large to fit in RAM memory segment)
                0x0000000020000a7c                __heap_load_start__ = ALIGN (__non_init_end__, 0x4)

.heap           0x0000000020000a7c     0x2000
                0x0000000020000a7c                __heap_start__ = .
 *(.heap .heap.*)
                0x0000000020002a7c                . = ALIGN (MAX ((__heap_start__ + __HEAPSIZE__), .), 0x4)
 *fill*         0x0000000020000a7c     0x2000 
                0x0000000020002a7c                __heap_end__ = (__heap_start__ + SIZEOF (.heap))
                0x0000000000002000                __heap_size__ = SIZEOF (.heap)
                0x0000000020002a7c                __heap_load_end__ = __heap_end__
                0x0000000000000001                . = ASSERT (((__heap_start__ == __heap_end__) || ((__heap_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .heap is too large to fit in RAM memory segment)
                0x000000002003e000                __stack_load_start__ = (__RAM_segment_start__ + (__RAM_segment_size__ - 0x2000))

.stack          0x000000002003e000     0x2000
                0x000000002003e000                __stack_start__ = .
                0x000000002003e000                __StackLimit = __stack_start__
 *(.stack .stack.*)
                0x0000000020040000                . = ALIGN (MAX ((__stack_start__ + __STACKSIZE__), .), 0x8)
 *fill*         0x000000002003e000     0x2000 
                0x0000000020040000                __stack_end__ = (__stack_start__ + SIZEOF (.stack))
                0x0000000000002000                __stack_size__ = SIZEOF (.stack)
                0x0000000020040000                __StackTop = __stack_end__
                0x0000000020040000                __stack_load_end__ = __stack_end__
                0x0000000000000001                . = ASSERT (((__stack_start__ == __stack_end__) || ((__stack_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .stack is too large to fit in RAM memory segment)
                0x0000000000000001                . = ASSERT ((__heap_end__ <= __stack_start__), error: section .heap overlaps absolute placed section .stack)
                0x0000000020040000                __stack_process_load_start__ = ALIGN (__stack_end__, 0x8)

.stack_process  0x0000000020040000        0x0
                0x0000000020040000                __stack_process_start__ = .
 *(.stack_process .stack_process.*)
                0x0000000020040000                . = ALIGN (MAX ((__stack_process_start__ + __STACKSIZE_PROCESS__), .), 0x8)
                0x0000000020040000                __stack_process_end__ = (__stack_process_start__ + SIZEOF (.stack_process))
                0x0000000000000000                __stack_process_size__ = SIZEOF (.stack_process)
                0x0000000020040000                __stack_process_load_end__ = __stack_process_end__
                0x0000000020040000                __RAM_segment_used_end__ = (ALIGN (__stack_end__, 0x8) + SIZEOF (.stack_process))
                0x0000000000040000                __RAM_segment_used_size__ = (__RAM_segment_used_end__ - __RAM_segment_start__)
                0x0000000000000001                . = ASSERT (((__stack_process_start__ == __stack_process_end__) || ((__stack_process_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .stack_process is too large to fit in RAM memory segment)
START GROUP
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/boards.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
LOAD Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
LOAD C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a
LOAD C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a
LOAD C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a
END GROUP
OUTPUT(Output/Debug/Exe/SAADC_RTC_PPI_pca10056.elf elf32-littlearm)
LOAD linker stubs

.ARM.attributes
                0x0000000000000000       0x30
 .ARM.attributes
                0x0000000000000000       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .ARM.attributes
                0x0000000000000020       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .ARM.attributes
                0x0000000000000054       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .ARM.attributes
                0x0000000000000088       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .ARM.attributes
                0x00000000000000bc       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .ARM.attributes
                0x00000000000000f0       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .ARM.attributes
                0x0000000000000124       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .ARM.attributes
                0x0000000000000158       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .ARM.attributes
                0x000000000000018c       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .ARM.attributes
                0x00000000000001c0       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .ARM.attributes
                0x00000000000001f4       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .ARM.attributes
                0x0000000000000228       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .ARM.attributes
                0x000000000000025c       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .ARM.attributes
                0x0000000000000290       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .ARM.attributes
                0x00000000000002c4       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .ARM.attributes
                0x00000000000002f8       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .ARM.attributes
                0x000000000000032c       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .ARM.attributes
                0x0000000000000360       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .ARM.attributes
                0x0000000000000394       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .ARM.attributes
                0x00000000000003c8       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .ARM.attributes
                0x00000000000003fc       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .ARM.attributes
                0x0000000000000430       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .ARM.attributes
                0x0000000000000464       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .ARM.attributes
                0x0000000000000498       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .ARM.attributes
                0x00000000000004cc       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .ARM.attributes
                0x0000000000000500       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .ARM.attributes
                0x0000000000000534       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .ARM.attributes
                0x0000000000000568       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .ARM.attributes
                0x000000000000059c       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .ARM.attributes
                0x00000000000005d0       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .ARM.attributes
                0x0000000000000604       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .ARM.attributes
                0x0000000000000638       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .ARM.attributes
                0x000000000000066c       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
 .ARM.attributes
                0x000000000000068c       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
 .ARM.attributes
                0x00000000000006ac       0x34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .ARM.attributes
                0x00000000000006e0       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .ARM.attributes
                0x0000000000000714       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)

.comment        0x0000000000000000       0x3f
 .comment       0x0000000000000000       0x3f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
                                         0x40 (size before relaxing)
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .comment       0x000000000000003f       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .comment       0x000000000000003f       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)

.debug_line     0x0000000000000000    0x12055
 .debug_line    0x0000000000000000      0x21e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .debug_line    0x000000000000021e      0x8ff Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_line    0x0000000000000b1d      0x652 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_line    0x000000000000116f      0x5ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_line    0x0000000000001739     0x1051 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_line    0x000000000000278a      0x77a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_line    0x0000000000002f04      0x367 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_line    0x000000000000326b      0x35d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_line    0x00000000000035c8      0x62e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_line    0x0000000000003bf6      0x42b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_line    0x0000000000004021      0x2e7 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_line    0x0000000000004308      0x5a7 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_line    0x00000000000048af      0x662 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_line    0x0000000000004f11      0x3fe Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_line    0x000000000000530f      0x6f1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_line    0x0000000000005a00      0x6e8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_line    0x00000000000060e8      0xaef Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_line    0x0000000000006bd7      0x7e3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_line    0x00000000000073ba      0x41b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_line    0x00000000000077d5      0x3be Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_line    0x0000000000007b93      0xe38 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_line    0x00000000000089cb      0xd68 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_line    0x0000000000009733      0x72c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_line    0x0000000000009e5f     0x1090 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_line    0x000000000000aeef      0xd7b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_line    0x000000000000bc6a     0x11b4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_line    0x000000000000ce1e     0x1136 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_line    0x000000000000df54      0xb49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_line    0x000000000000ea9d      0xc2f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_line    0x000000000000f6cc      0xae0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_line    0x00000000000101ac      0xc71 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_line    0x0000000000010e1d      0xb34 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_line    0x0000000000011951       0x92 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
 .debug_line    0x00000000000119e3       0xb1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
 .debug_line    0x0000000000011a94      0x5c1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o

.debug_info     0x0000000000000000    0x160b6
 .debug_info    0x0000000000000000       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .debug_info    0x0000000000000022      0x3fd Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_info    0x000000000000041f      0x62f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_info    0x0000000000000a4e      0x282 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_info    0x0000000000000cd0     0x183f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_info    0x000000000000250f      0x48e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_info    0x000000000000299d      0x270 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_info    0x0000000000002c0d       0xe3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_info    0x0000000000002cf0      0x2d5 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_info    0x0000000000002fc5      0x744 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_info    0x0000000000003709      0x10f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_info    0x0000000000003818      0x878 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_info    0x0000000000004090      0x2d2 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_info    0x0000000000004362      0x1fb Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_info    0x000000000000455d      0x481 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_info    0x00000000000049de      0x695 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_info    0x0000000000005073      0xf7c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_info    0x0000000000005fef      0x484 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_info    0x0000000000006473      0x195 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_info    0x0000000000006608      0x1c8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_info    0x00000000000067d0     0x133b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_info    0x0000000000007b0b      0xd5f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_info    0x000000000000886a      0x740 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_info    0x0000000000008faa     0x19d6 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_info    0x000000000000a980     0x144c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_info    0x000000000000bdcc     0x1e03 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_info    0x000000000000dbcf     0x1f14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_info    0x000000000000fae3      0xed8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_info    0x00000000000109bb     0x11f3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_info    0x0000000000011bae      0x9a1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_info    0x000000000001254f     0x18e9 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_info    0x0000000000013e38      0xdc3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_info    0x0000000000014bfb       0x23 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
 .debug_info    0x0000000000014c1e       0x23 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
 .debug_info    0x0000000000014c41     0x1475 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o

.debug_abbrev   0x0000000000000000     0x432f
 .debug_abbrev  0x0000000000000000       0x12 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .debug_abbrev  0x0000000000000012      0x195 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_abbrev  0x00000000000001a7      0x1be Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_abbrev  0x0000000000000365      0x12d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_abbrev  0x0000000000000492      0x46b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_abbrev  0x00000000000008fd      0x18c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_abbrev  0x0000000000000a89      0x114 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_abbrev  0x0000000000000b9d       0x7a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_abbrev  0x0000000000000c17      0x163 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_abbrev  0x0000000000000d7a      0x235 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_abbrev  0x0000000000000faf       0xab Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_abbrev  0x000000000000105a      0x121 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_abbrev  0x000000000000117b      0x183 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_abbrev  0x00000000000012fe      0x106 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_abbrev  0x0000000000001404      0x1bf Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_abbrev  0x00000000000015c3      0x17b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_abbrev  0x000000000000173e      0x32b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_abbrev  0x0000000000001a69       0xd9 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_abbrev  0x0000000000001b42       0xbd Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_abbrev  0x0000000000001bff       0xe6 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_abbrev  0x0000000000001ce5      0x3a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_abbrev  0x0000000000002088      0x2aa Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_abbrev  0x0000000000002332      0x1e9 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_abbrev  0x000000000000251b      0x3af Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_abbrev  0x00000000000028ca      0x2e3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_abbrev  0x0000000000002bad      0x398 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_abbrev  0x0000000000002f45      0x360 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_abbrev  0x00000000000032a5      0x31f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_abbrev  0x00000000000035c4      0x328 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_abbrev  0x00000000000038ec      0x326 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_abbrev  0x0000000000003c12      0x2e8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_abbrev  0x0000000000003efa      0x203 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_abbrev  0x00000000000040fd       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
 .debug_abbrev  0x0000000000004111       0x14 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
 .debug_abbrev  0x0000000000004125      0x20a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o

.debug_aranges  0x0000000000000000     0x1498
 .debug_aranges
                0x0000000000000000       0x98 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .debug_aranges
                0x0000000000000098       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_aranges
                0x00000000000000e8       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_aranges
                0x0000000000000108       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_aranges
                0x0000000000000130      0x140 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_aranges
                0x0000000000000270       0x48 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_aranges
                0x00000000000002b8       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_aranges
                0x00000000000002e0       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_aranges
                0x0000000000000300       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_aranges
                0x0000000000000320       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_aranges
                0x0000000000000370       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_aranges
                0x0000000000000390       0xb8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_aranges
                0x0000000000000448       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_aranges
                0x0000000000000488       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_aranges
                0x00000000000004b0       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_aranges
                0x00000000000004f0       0x58 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_aranges
                0x0000000000000548       0x80 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_aranges
                0x00000000000005c8       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_aranges
                0x0000000000000618       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_aranges
                0x0000000000000640       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_aranges
                0x0000000000000668      0x148 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_aranges
                0x00000000000007b0      0x140 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_aranges
                0x00000000000008f0       0x38 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_aranges
                0x0000000000000928      0x138 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_aranges
                0x0000000000000a60      0x158 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_aranges
                0x0000000000000bb8      0x1e8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_aranges
                0x0000000000000da0      0x1d8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_aranges
                0x0000000000000f78      0x108 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_aranges
                0x0000000000001080      0x108 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_aranges
                0x0000000000001188       0xd0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_aranges
                0x0000000000001258       0x90 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_aranges
                0x00000000000012e8      0x108 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_aranges
                0x00000000000013f0       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
 .debug_aranges
                0x0000000000001410       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
 .debug_aranges
                0x0000000000001430       0x68 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o

.debug_str      0x0000000000000000    0x934b5
 .debug_str     0x0000000000000000       0xc8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .debug_str     0x00000000000000c8    0x84da7 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
                                      0x861c4 (size before relaxing)
 .debug_str     0x0000000000084e6f      0x287 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
                                      0x82864 (size before relaxing)
 .debug_str     0x00000000000850f6      0x121 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
                                      0x82639 (size before relaxing)
 .debug_str     0x0000000000085217     0x13df Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                                      0x83b51 (size before relaxing)
 .debug_str     0x00000000000865f6      0x2fe Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
                                      0x82920 (size before relaxing)
 .debug_str     0x00000000000868f4      0x10d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
                                      0x741b0 (size before relaxing)
 .debug_str     0x0000000000086a01       0x70 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
                                      0x7ecf8 (size before relaxing)
 .debug_str     0x0000000000086a71       0x9d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
                                      0x82cc3 (size before relaxing)
 .debug_str     0x0000000000086b0e      0x4e9 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
                                      0x74a22 (size before relaxing)
 .debug_str     0x0000000000086ff7       0x67 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
                                      0x741bb (size before relaxing)
 .debug_str     0x000000000008705e      0x731 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
                                      0x7ef17 (size before relaxing)
 .debug_str     0x000000000008778f      0x159 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
                                      0x82652 (size before relaxing)
 .debug_str     0x00000000000878e8      0x131 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
                                      0x7ea98 (size before relaxing)
 .debug_str     0x0000000000087a19      0x53b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
                                      0x7ef82 (size before relaxing)
 .debug_str     0x0000000000087f54      0x22b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
                                      0x8099c (size before relaxing)
 .debug_str     0x000000000008817f      0xfa9 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
                                      0x87214 (size before relaxing)
 .debug_str     0x0000000000089128      0x13a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
                                      0x7f2ad (size before relaxing)
 .debug_str     0x0000000000089262       0x9a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
                                      0x7ed21 (size before relaxing)
 .debug_str     0x00000000000892fc      0x107 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
                                      0x7e8dc (size before relaxing)
 .debug_str     0x0000000000089403      0xb76 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
                                      0x83380 (size before relaxing)
 .debug_str     0x0000000000089f79      0xb9b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
                                      0x856b9 (size before relaxing)
 .debug_str     0x000000000008ab14      0x486 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
                                      0x8534b (size before relaxing)
 .debug_str     0x000000000008af9a     0x19a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
                                      0x86cc0 (size before relaxing)
 .debug_str     0x000000000008c93d     0x1028 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
                                      0x864de (size before relaxing)
 .debug_str     0x000000000008d965     0x105c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
                                      0x86551 (size before relaxing)
 .debug_str     0x000000000008e9c1      0xf6d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
                                      0x869e4 (size before relaxing)
 .debug_str     0x000000000008f92e      0x996 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
                                      0x85c53 (size before relaxing)
 .debug_str     0x00000000000902c4      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
                                      0x85e3d (size before relaxing)
 .debug_str     0x0000000000090d25      0x45d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
                                      0x8549a (size before relaxing)
 .debug_str     0x0000000000091182     0x1920 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
                                      0x8a3cc (size before relaxing)
 .debug_str     0x0000000000092aa2      0x5ed Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
                                      0x77e1a (size before relaxing)
 .debug_str     0x000000000009308f       0x54 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
                                         0xcc (size before relaxing)
 .debug_str     0x00000000000930e3       0x56 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
                                         0xce (size before relaxing)
 .debug_str     0x0000000000093139      0x37c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
                                      0x7314a (size before relaxing)

.debug_ranges   0x0000000000000000     0x1298
 .debug_ranges  0x0000000000000000       0x90 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .debug_ranges  0x0000000000000090       0x58 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_ranges  0x00000000000000e8       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_ranges  0x00000000000000f8       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_ranges  0x0000000000000110      0x130 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_ranges  0x0000000000000240       0x38 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_ranges  0x0000000000000278       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_ranges  0x0000000000000290       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_ranges  0x00000000000002a0       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_ranges  0x00000000000002b0       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_ranges  0x00000000000002f0       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_ranges  0x0000000000000300       0xa8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_ranges  0x00000000000003a8       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_ranges  0x00000000000003d8       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_ranges  0x00000000000003f0       0x30 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_ranges  0x0000000000000420       0x48 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_ranges  0x0000000000000468       0x88 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_ranges  0x00000000000004f0       0x40 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_ranges  0x0000000000000530       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_ranges  0x0000000000000548       0x18 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_ranges  0x0000000000000560      0x138 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_ranges  0x0000000000000698      0x130 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_ranges  0x00000000000007c8       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_ranges  0x00000000000007f0      0x128 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_ranges  0x0000000000000918      0x148 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_ranges  0x0000000000000a60      0x1d8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_ranges  0x0000000000000c38      0x1c8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_ranges  0x0000000000000e00       0xf8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_ranges  0x0000000000000ef8       0xf8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_ranges  0x0000000000000ff0       0xd8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_ranges  0x00000000000010c8       0x80 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_ranges  0x0000000000001148       0xf8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_ranges  0x0000000000001240       0x58 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o

.debug_frame    0x0000000000000000     0x4c40
 .debug_frame   0x0000000000000000      0x10c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_frame   0x000000000000010c       0x38 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_frame   0x0000000000000144       0x58 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_frame   0x000000000000019c      0x558 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_frame   0x00000000000006f4       0xf8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_frame   0x00000000000007ec       0x58 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_frame   0x0000000000000844       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_frame   0x0000000000000864       0x3c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_frame   0x00000000000008a0       0xe8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_frame   0x0000000000000988       0x38 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_frame   0x00000000000009c0      0x3b0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_frame   0x0000000000000d70       0xdc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_frame   0x0000000000000e4c       0x80 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_frame   0x0000000000000ecc       0xd8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_frame   0x0000000000000fa4      0x150 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_frame   0x00000000000010f4      0x1b0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_frame   0x00000000000012a4      0x120 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_frame   0x00000000000013c4       0x60 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_frame   0x0000000000001424       0x58 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_frame   0x000000000000147c      0x4e8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_frame   0x0000000000001964      0x544 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_frame   0x0000000000001ea8       0x9c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_frame   0x0000000000001f44      0x4d4 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_frame   0x0000000000002418      0x5b0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_frame   0x00000000000029c8      0x850 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_frame   0x0000000000003218      0x7dc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_frame   0x00000000000039f4      0x3a8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_frame   0x0000000000003d9c      0x444 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_frame   0x00000000000041e0      0x2d0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_frame   0x00000000000044b0      0x240 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_frame   0x00000000000046f0      0x494 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_frame   0x0000000000004b84       0xbc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o

.debug_pubnames
                0x0000000000000000     0x8a83
 .debug_pubnames
                0x0000000000000000      0x12a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_pubnames
                0x000000000000012a       0x31 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_pubnames
                0x000000000000015b      0x12b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_pubnames
                0x0000000000000286      0x5e9 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_pubnames
                0x000000000000086f      0x1bd Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_pubnames
                0x0000000000000a2c       0x6c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_pubnames
                0x0000000000000a98       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_pubnames
                0x0000000000000ac0       0xe5 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_pubnames
                0x0000000000000ba5      0x221 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_pubnames
                0x0000000000000dc6       0x2a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_pubnames
                0x0000000000000df0      0x233 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_pubnames
                0x0000000000001023      0x126 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_pubnames
                0x0000000000001149       0x3f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_pubnames
                0x0000000000001188       0x67 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_pubnames
                0x00000000000011ef       0xb1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_pubnames
                0x00000000000012a0      0xcc8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_pubnames
                0x0000000000001f68       0xaa Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_pubnames
                0x0000000000002012       0x46 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_pubnames
                0x0000000000002058       0x66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_pubnames
                0x00000000000020be      0x91a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_pubnames
                0x00000000000029d8      0x894 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_pubnames
                0x000000000000326c      0x13f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_pubnames
                0x00000000000033ab     0x10eb Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_pubnames
                0x0000000000004496      0x813 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_pubnames
                0x0000000000004ca9      0xaae Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_pubnames
                0x0000000000005757      0xc5f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_pubnames
                0x00000000000063b6      0x6ee Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_pubnames
                0x0000000000006aa4      0x6a0 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_pubnames
                0x0000000000007144      0x4b2 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_pubnames
                0x00000000000075f6      0xfe2 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_pubnames
                0x00000000000085d8      0x3c3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_pubnames
                0x000000000000899b       0xe8 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o

.debug_pubtypes
                0x0000000000000000     0x3dcf
 .debug_pubtypes
                0x0000000000000000      0x184 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_pubtypes
                0x0000000000000184      0x287 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_pubtypes
                0x000000000000040b      0x178 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_pubtypes
                0x0000000000000583      0x33e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_pubtypes
                0x00000000000008c1      0x181 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_pubtypes
                0x0000000000000a42      0x117 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_pubtypes
                0x0000000000000b59       0xed Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_pubtypes
                0x0000000000000c46      0x162 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_pubtypes
                0x0000000000000da8      0x110 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_pubtypes
                0x0000000000000eb8       0xed Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_pubtypes
                0x0000000000000fa5      0x107 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_pubtypes
                0x00000000000010ac      0x12a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_pubtypes
                0x00000000000011d6      0x15c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_pubtypes
                0x0000000000001332      0x175 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_pubtypes
                0x00000000000014a7      0x1f3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_pubtypes
                0x000000000000169a      0x25a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_pubtypes
                0x00000000000018f4      0x14c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_pubtypes
                0x0000000000001a40      0x128 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_pubtypes
                0x0000000000001b68       0xf9 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_pubtypes
                0x0000000000001c61      0x21f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_pubtypes
                0x0000000000001e80      0x1b9 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_pubtypes
                0x0000000000002039      0x1bc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_pubtypes
                0x00000000000021f5      0x420 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_pubtypes
                0x0000000000002615      0x2d7 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_pubtypes
                0x00000000000028ec      0x392 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_pubtypes
                0x0000000000002c7e      0x3c7 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_pubtypes
                0x0000000000003045      0x236 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_pubtypes
                0x000000000000327b      0x232 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_pubtypes
                0x00000000000034ad      0x216 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_pubtypes
                0x00000000000036c3      0x456 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_pubtypes
                0x0000000000003b19       0xfb Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_pubtypes
                0x0000000000003c14      0x1bb Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o

.debug_macro    0x0000000000000000    0x1aaf0
 .debug_macro   0x0000000000000000      0x304 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000304      0xaba Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000dbe      0x1a3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000f61       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000f83       0x89 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x000000000000100c       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x000000000000101c      0xa61 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000001a7d      0x16d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000001bea       0x32 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000001c1c       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000001c3e       0x8e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000001ccc       0xad Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000001d79       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000001d8f       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000001db1       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000001dec       0x3b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000001e27       0x50 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000001e77      0xe66 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000002cdd      0x402 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x00000000000030df    0x10c8a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000013d69      0xa65 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x00000000000147ce       0x96 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000014864      0x7ca Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x000000000001502e       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000015044       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000015099       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x00000000000150bb       0x72 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x000000000001512d       0x49 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000015176       0x8c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000015202       0x31 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000015233       0x55 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000015288       0x98 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000015320       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000015330       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x000000000001534d       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x000000000001535d       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x000000000001538b       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x00000000000153a7      0x185 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x000000000001552c      0x430 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x000000000001595c       0x59 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x00000000000159b5      0x25d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000015c12      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000015d60       0x5a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000015dba       0x1d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000015dd7       0xac Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000015e83       0x64 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000015ee7       0x20 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000015f07       0x4d Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000015f54      0x115 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000016069      0x225 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x000000000001628e      0x221 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x00000000000164af       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x00000000000164bf      0x297 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000016756       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x000000000001676c       0x9a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000016806       0x9e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x00000000000168a4      0x274 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000016b18      0x109 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000016c21       0x35 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000016c56       0x78 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000016cce      0x15c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000016e2a      0x233 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x000000000001705d      0x11f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x000000000001717c      0x112 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x000000000001728e       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x000000000001729e      0x159 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x00000000000173f7       0x42 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000017439      0x207 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000017640       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000017650      0x15a Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x00000000000177aa       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x00000000000177cc      0x1cc Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000017998      0x1cf Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000017b67       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000017b95       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000017ba5       0x5b Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000017c00      0x39c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000017f9c       0x11 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000017fad       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000017fbd       0x45 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000018002       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x000000000001802a      0x17f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x00000000000181a9      0x199 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000018342      0x164 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x00000000000184a6      0x14e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x00000000000185f4      0x2a5 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000018899       0x3c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x00000000000188d5       0x5f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/app_timer.o
 .debug_macro   0x0000000000018934      0x2ac Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000018be0       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000018bfc       0x37 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000018c33       0x42 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000018c75      0x2ae Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000018f23       0x28 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000018f4b      0x2d5 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000019220       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000019230       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000019252      0x2b9 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x000000000001950b       0x22 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x000000000001952d       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x000000000001953d      0x2c9 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000019806       0x1c Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000019822      0x2e7 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000019b09      0x2c1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000019dca       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000019de0       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000019df0      0x2b1 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x000000000001a0a1       0x2e Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x000000000001a0cf       0x16 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x000000000001a0e5      0x2e3 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x000000000001a3c8      0x3d7 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x000000000001a79f       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x000000000001a7af       0x94 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x000000000001a843       0x10 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x000000000001a853      0x19f Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x000000000001a9f2       0x47 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x000000000001aa39       0xb7 Output/Debug/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
