Archive member included to satisfy reference by file (symbol)

C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                              Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o (isprint)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
                              Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o (memcpy)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
                              (__vfprintf_long)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
                              (__vfscanf_long)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
                              C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o) (__heap_lock)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
                              C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o) (__aeabi_uldivmod)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
                              Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o (debug_fopen)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(do_nv_debug_operation.o)
                              C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o) (__do_nvdebug_operation)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
                              (__do_debug_operation_mempoll)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
                              C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o) (__aeabi_dadd)
C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
                              C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o) (frexp)

Discarded input sections

 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__aeabi_read_tp
                0x0000000000000000        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.abort    0x0000000000000000        0x2 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__assert
                0x0000000000000000        0x2 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__assert_func
                0x0000000000000000        0x2 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__aeabi_assert
                0x0000000000000000        0x2 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__sync_synchronize
                0x0000000000000000        0x2 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__getchar
                0x0000000000000000        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__putchar
                0x0000000000000000        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__open   0x0000000000000000        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__close  0x0000000000000000        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__write  0x0000000000000000        0xa Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__read   0x0000000000000000        0xa Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.__seek   0x0000000000000000       0x1a Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.remove   0x0000000000000000        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .text.rename   0x0000000000000000        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .bss.__user_locale_name_buffer
                0x0000000000000000        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .stack         0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .stack_process
                0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .heap          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_info    0x0000000000000000       0x6f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_abbrev  0x0000000000000000       0x2c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_pubnames
                0x0000000000000000       0x12 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_pubtypes
                0x0000000000000000       0xc5 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_aranges
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000      0x13a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_line    0x0000000000000000      0x343 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .debug_str     0x0000000000000000    0x7e834 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .comment       0x0000000000000000       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .ARM.attributes
                0x0000000000000000       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x31 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x98 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000000      0x185 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x2e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x31 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x98 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x0000000000000000      0x185 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_module_cnt_get
                0x0000000000000000       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_module_filter_set
                0x0000000000000000        0x2 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_module_filter_get
                0x0000000000000000       0x3c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_push
                0x0000000000000000       0x60 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_frontend_std_2
                0x0000000000000000       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_frontend_std_3
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_frontend_std_4
                0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_frontend_std_5
                0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_frontend_std_6
                0x0000000000000000       0x24 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_frontend_hexdump
                0x0000000000000000       0xbc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_backend_remove
                0x0000000000000000       0x30 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x31 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000      0x185 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x2e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .text.nrf_log_str_formatter_timestamp_freq_set
                0x0000000000000000       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .bss.m_timestamp_div
                0x0000000000000000        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x2e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x31 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x98 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000000000      0x185 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_led_state_get
                0x0000000000000000       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_led_on
                0x0000000000000000       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_led_off
                0x0000000000000000       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_leds_off
                0x0000000000000000       0x1e Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_leds_on
                0x0000000000000000       0x1e Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_led_invert
                0x0000000000000000       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_led_idx_to_pin
                0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_pin_to_led_idx
                0x0000000000000000       0x24 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_button_state_get
                0x0000000000000000       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_pin_to_button_idx
                0x0000000000000000       0x24 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_button_idx_to_pin
                0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .text.bsp_board_init
                0x0000000000000000       0x3e Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .rodata.m_board_btn_list
                0x0000000000000000        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .rodata.m_board_led_list
                0x0000000000000000        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_frame   0x0000000000000000      0x104 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_info    0x0000000000000000      0xcf8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_abbrev  0x0000000000000000      0x313 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_loc     0x0000000000000000      0x93c Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_pubnames
                0x0000000000000000      0x4bd Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_pubtypes
                0x0000000000000000      0x181 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_aranges
                0x0000000000000000       0x78 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_ranges  0x0000000000000000      0x2c8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x225 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x430 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x59 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x3c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x14e Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x19 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x35 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x7b Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x208 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_line    0x0000000000000000      0xb1f Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .debug_str     0x0000000000000000    0x83d63 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .comment       0x0000000000000000       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .ARM.attributes
                0x0000000000000000       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .text.app_error_save_and_stop
                0x0000000000000000       0x58 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .bss.m_error_data.0
                0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .text.app_error_handler
                0x0000000000000000       0x1a Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_frame   0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_info    0x0000000000000000       0xf5 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_abbrev  0x0000000000000000       0x7d Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_loc     0x0000000000000000       0x6f Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_pubnames
                0x0000000000000000       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_pubtypes
                0x0000000000000000       0xed Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_aranges
                0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_ranges  0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000      0x15c Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_line    0x0000000000000000      0x35c Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .debug_str     0x0000000000000000    0x7ed1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .comment       0x0000000000000000       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .ARM.attributes
                0x0000000000000000       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x78 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x31 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000      0x185 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x9a Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x2e Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x98 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .text.privilege_level_get
                0x0000000000000000       0x1a Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .text.current_int_priority_get
                0x0000000000000000       0x38 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x78 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .text.assert_nrf_callback
                0x0000000000000000       0x1a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_frame   0x0000000000000000       0x30 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_info    0x0000000000000000      0x145 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_abbrev  0x0000000000000000       0xda Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_loc     0x0000000000000000       0x66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_pubnames
                0x0000000000000000       0x2a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_pubtypes
                0x0000000000000000       0xed Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_aranges
                0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_ranges  0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000      0x112 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x78 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_line    0x0000000000000000      0x2f5 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .debug_str     0x0000000000000000    0x741c5 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .comment       0x0000000000000000       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .ARM.attributes
                0x0000000000000000       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_store
                0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_fetch_or
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_and
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_fetch_xor
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_xor
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_fetch_add
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_fetch_sub
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_cmp_exch
                0x0000000000000000       0x2a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_fetch_sub_hs
                0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_u32_sub_hs
                0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_flag_set_fetch
                0x0000000000000000        0x6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .text.nrf_atomic_flag_clear
                0x0000000000000000        0x6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x31 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x98 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000      0x185 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x0000000000000000       0x9a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x31 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x98 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .text.nrf_pwr_mgmt_feed
                0x0000000000000000        0x2 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .text.nrf_pwr_mgmt_shutdown
                0x0000000000000000       0xa4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .bss.m_pwr_mgmt_evt
                0x0000000000000000        0x1 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x31 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0x430 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x59 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0x3c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000      0x14e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x19 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0xac Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x2e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x98 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000000000       0x9a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .text.nrf_ringbuf_alloc
                0x0000000000000000       0x70 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .text.nrf_ringbuf_put
                0x0000000000000000       0x2e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .text.nrf_ringbuf_cpy_put
                0x0000000000000000       0x7c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .text.nrf_ringbuf_get
                0x0000000000000000       0x6e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .text.nrf_ringbuf_cpy_get
                0x0000000000000000       0x7e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .text.nrf_ringbuf_free
                0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .text.nrf_section_iter_next
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x31 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x0000000000000000       0x11 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .text.nrf_strerror_find
                0x0000000000000000       0x3c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .text.nrf_strerror_get
                0x0000000000000000       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .rodata.str1.1
                0x0000000000000000      0x391 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .rodata.m_unknown_str
                0x0000000000000000       0x13 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .rodata.nrf_strerror_array
                0x0000000000000000      0x118 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_frame   0x0000000000000000       0x48 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_info    0x0000000000000000      0x1f8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_abbrev  0x0000000000000000      0x112 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_loc     0x0000000000000000      0x11b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_pubnames
                0x0000000000000000       0x66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_pubtypes
                0x0000000000000000       0xf9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_aranges
                0x0000000000000000       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_ranges  0x0000000000000000       0x30 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000      0x14e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_line    0x0000000000000000      0x3e1 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .debug_str     0x0000000000000000    0x7e91a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .comment       0x0000000000000000       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .ARM.attributes
                0x0000000000000000       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .text.nrf_drv_ppi_uninit
                0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0x430 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x59 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0x3c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0x14e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x19 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x35 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x7b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0x430 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x59 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0x3c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0x14e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x19 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x35 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x7b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000000000       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_fetch_store
                0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_store
                0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_fetch_or
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_or
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_fetch_and
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_and
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_fetch_xor
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_xor
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_fetch_add
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_add
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_fetch_sub
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_sub
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_cmp_exch
                0x0000000000000000       0x2a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_fetch_sub_hs
                0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_u32_sub_hs
                0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_flag_set_fetch
                0x0000000000000000        0x6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_flag_set
                0x0000000000000000        0x6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_flag_clear_fetch
                0x0000000000000000        0x6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .text.nrfx_atomic_flag_clear
                0x0000000000000000        0x6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_frame   0x0000000000000000      0x1f8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_info    0x0000000000000000      0x922 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_abbrev  0x0000000000000000      0x1a0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_loc     0x0000000000000000      0x449 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_pubnames
                0x0000000000000000      0x247 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_pubtypes
                0x0000000000000000      0x109 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_aranges
                0x0000000000000000       0xb0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_ranges  0x0000000000000000      0x208 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0x213 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0x430 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x59 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0x3c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0x14e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x19 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x35 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x7b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_macro   0x0000000000000000       0x42 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_line    0x0000000000000000      0x848 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .debug_str     0x0000000000000000    0x82ca1 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .comment       0x0000000000000000       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .ARM.attributes
                0x0000000000000000       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_free_all
                0x0000000000000000       0x4c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_channel_free
                0x0000000000000000       0x3c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_channel_fork_assign
                0x0000000000000000       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_channel_disable
                0x0000000000000000       0x2c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_group_alloc
                0x0000000000000000       0x58 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_group_free
                0x0000000000000000       0x48 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_group_enable
                0x0000000000000000       0x2c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_group_disable
                0x0000000000000000       0x1e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_channels_remove_from_group
                0x0000000000000000       0x48 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .text.nrfx_ppi_channels_include_in_group
                0x0000000000000000       0x48 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .bss.m_groups_allocated
                0x0000000000000000        0x1 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0x430 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x59 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0x3c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0x14e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x19 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x35 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x7b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x5b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000      0x17f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000000000       0x9a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0x430 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x59 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0x3c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0x14e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x19 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x35 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x7b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x5b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x37 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000      0x17f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x9a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000000000       0x42 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrfx_saadc_sample_convert
                0x0000000000000000       0xd4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrfx_saadc_sample
                0x0000000000000000       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrfx_saadc_calibrate_offset
                0x0000000000000000       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrfx_saadc_is_busy
                0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrfx_saadc_abort
                0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrfx_saadc_limits_set
                0x0000000000000000       0x7c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrfx_saadc_channel_uninit
                0x0000000000000000       0x54 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.nrfx_saadc_uninit
                0x0000000000000000       0x58 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0x430 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x59 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0x3c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0x14e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x19 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x35 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x7b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x5b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x37 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000      0x17f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x9a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x0000000000000000       0x42 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_disable
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_uninit
                0x0000000000000000       0x48 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_is_enabled
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_resume
                0x0000000000000000        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_pause
                0x0000000000000000        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_clear
                0x0000000000000000        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_increment
                0x0000000000000000        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_capture
                0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_compare_int_enable
                0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .text.nrfx_timer_compare_int_disable
                0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0x430 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x59 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0x3c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0x14e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x19 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x35 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x7b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x5b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x37 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000      0x17f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x9a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000000000       0x42 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.rx_enable
                0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_rx
                0x0000000000000000       0xf4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_rx_ready
                0x0000000000000000        0xe Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_rx_enable
                0x0000000000000000       0x2c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_rx_disable
                0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_errorsrc_get
                0x0000000000000000       0x1a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_tx_abort
                0x0000000000000000       0x3c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_rx_abort
                0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0x430 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x59 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0x3c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0x14e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x19 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x35 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x7b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x5b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x37 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000      0x17f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x9a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000000000       0x42 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_uarte_rx
                0x0000000000000000       0xd8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_uarte_rx_ready
                0x0000000000000000        0xe Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_uarte_errorsrc_get
                0x0000000000000000       0x1a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_uarte_tx_abort
                0x0000000000000000       0x30 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_uarte_rx_abort
                0x0000000000000000       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0x430 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x59 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0x3c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0x14e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x19 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x35 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x7b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x5b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x37 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000      0x17f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x9a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000000000       0x42 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_disable
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_lfclk_stop
                0x0000000000000000       0x12 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_hfclk_start
                0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_hfclk_stop
                0x0000000000000000       0x24 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_uninit
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_calibration_start
                0x0000000000000000        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_is_calibrating
                0x0000000000000000        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_calibration_timer_start
                0x0000000000000000        0x2 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .text.nrfx_clock_calibration_timer_stop
                0x0000000000000000        0x2 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0x430 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x59 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0x3c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0x14e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x19 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x35 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x7b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x5b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x37 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000      0x17f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x9a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000000000       0x42 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_init
                0x0000000000000000       0x84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_uninit
                0x0000000000000000       0x44 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_enable
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_disable
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_cc_disable
                0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_cc_set
                0x0000000000000000       0x84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_tick_enable
                0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_tick_disable
                0x0000000000000000        0xe Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_overflow_enable
                0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_overflow_disable
                0x0000000000000000        0xe Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.nrfx_rtc_max_ticks_get
                0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .bss.m_cb      0x0000000000000000        0x3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0x430 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x59 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0x3c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0x14e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x19 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x35 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x7b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x5b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x37 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000      0x17f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x9a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x0000000000000000       0x42 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_init_check
                0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_uninit
                0x0000000000000000       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_lfclk_release
                0x0000000000000000       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_lfclk_is_running
                0x0000000000000000        0xe Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_hfclk_request
                0x0000000000000000       0x54 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_hfclk_release
                0x0000000000000000       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_hfclk_is_running
                0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_calibration_start
                0x0000000000000000        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_calibration_abort
                0x0000000000000000        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_is_calibrating
                0x0000000000000000        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0x430 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x59 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0x3c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0x14e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0x7ca Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x19 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x35 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x7b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x5b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x37 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000      0x17f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x0000000000000000       0x9a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .data.state    0x0000000000000000        0x1 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x78 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x430 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x59 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x3c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x14e Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x19 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x35 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x7b Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x208 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x88 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x37 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x11 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x2e Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x5b Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000      0x185 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x9a Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x2e Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x9e Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text._GetAvailWriteSpace
                0x0000000000000000       0x12 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text._WriteNoCheck
                0x0000000000000000       0x38 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text._WriteBlocking
                0x0000000000000000       0x52 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .rodata._DoInit.str1.1
                0x0000000000000000       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text._DoInit  0x0000000000000000       0x60 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text._PostTerminalSwitch.constprop.0
                0x0000000000000000       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_ReadNoLock
                0x0000000000000000       0x88 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_Read
                0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_WriteWithOverwriteNoLock
                0x0000000000000000       0xb8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_WriteSkipNoLock
                0x0000000000000000       0x90 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_WriteNoLock
                0x0000000000000000       0x60 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_Write
                0x0000000000000000       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_WriteString
                0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_PutCharSkipNoLock
                0x0000000000000000       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_PutCharSkip
                0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_PutChar
                0x0000000000000000       0x60 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_GetKey
                0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_WaitKey
                0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_HasKey
                0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_HasData
                0x0000000000000000       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_AllocDownBuffer
                0x0000000000000000       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_AllocUpBuffer
                0x0000000000000000       0x70 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_ConfigUpBuffer
                0x0000000000000000       0x60 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_ConfigDownBuffer
                0x0000000000000000       0x58 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_SetNameUpBuffer
                0x0000000000000000       0x38 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_SetNameDownBuffer
                0x0000000000000000       0x38 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_SetFlagsUpBuffer
                0x0000000000000000       0x38 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_SetFlagsDownBuffer
                0x0000000000000000       0x38 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_Init
                0x0000000000000000        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_SetTerminal
                0x0000000000000000       0x80 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .text.SEGGER_RTT_TerminalOut
                0x0000000000000000       0x98 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .bss._ActiveTerminal
                0x0000000000000000        0x1 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .bss._SEGGER_RTT
                0x0000000000000000       0x78 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .bss._acDownBuffer
                0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .bss._acUpBuffer
                0x0000000000000000      0x200 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .rodata._aTerminalId
                0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_frame   0x0000000000000000      0x42c Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_info    0x0000000000000000     0x15fd Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_abbrev  0x0000000000000000      0x2d4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_loc     0x0000000000000000     0x1743 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_pubnames
                0x0000000000000000      0x3c3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_pubtypes
                0x0000000000000000       0xfb Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_aranges
                0x0000000000000000      0x108 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_ranges  0x0000000000000000       0xf8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000      0x19f Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x78 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000       0x47 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_macro   0x0000000000000000      0x115 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_line    0x0000000000000000     0x1288 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .debug_str     0x0000000000000000    0x77ea1 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .comment       0x0000000000000000       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .ARM.attributes
                0x0000000000000000       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .text.printf   0x0000000000000000       0x3a Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .text.puts     0x0000000000000000        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .text.__putchar
                0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .text.__getchar
                0x0000000000000000        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_frame   0x0000000000000000       0xa4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_info    0x0000000000000000      0x2cb Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_abbrev  0x0000000000000000      0x1a5 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_loc     0x0000000000000000       0xa9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_pubnames
                0x0000000000000000       0x42 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_pubtypes
                0x0000000000000000      0x10e Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_aranges
                0x0000000000000000       0x38 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_ranges  0x0000000000000000       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0x18a Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x78 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x47 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000      0x115 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0x86 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0xa6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_macro   0x0000000000000000       0xc8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_line    0x0000000000000000      0x460 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .debug_str     0x0000000000000000    0x784ef Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .comment       0x0000000000000000       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .ARM.attributes
                0x0000000000000000       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .text._StoreChar
                0x0000000000000000       0x3c Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .text._PrintUnsigned
                0x0000000000000000       0xd0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .text.SEGGER_RTT_vprintf
                0x0000000000000000      0x25c Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .text.SEGGER_RTT_printf
                0x0000000000000000       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .rodata._aV2C.0
                0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_frame   0x0000000000000000       0xd8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_info    0x0000000000000000      0x617 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_abbrev  0x0000000000000000      0x273 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_loc     0x0000000000000000      0x97b Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_pubnames
                0x0000000000000000       0x6f Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_pubtypes
                0x0000000000000000       0xf8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_aranges
                0x0000000000000000       0x38 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_ranges  0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0x174 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0x16d Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x89 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x78 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x8e Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0xad Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0xa84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x47 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000      0x115 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_line    0x0000000000000000      0x87f Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .debug_str     0x0000000000000000    0x77b53 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .comment       0x0000000000000000       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .ARM.attributes
                0x0000000000000000       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .group         0x0000000000000000        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .text          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .data          0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .bss           0x0000000000000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .text.SystemCoreClockUpdate
                0x0000000000000000       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000      0xaba Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000      0x1a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000       0x3b Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000      0xe66 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000      0x402 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000    0x10c8a Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000      0xa65 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000       0x96 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .debug_macro   0x0000000000000000       0x26 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .text          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .data          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss           0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__stdin_ungetc
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ungetc_fn
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.put_twodigit
                0x0000000000000000       0x5c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_utf8_mbtowc
                0x0000000000000000       0x94 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_1_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_2_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_3_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_4_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_5_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_6_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_7_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_8_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_9_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_10_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_11_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_13_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_14_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_15_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_16_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1250_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1251_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1252_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1253_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1254_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1255_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1256_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1257_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1258_mbtowc
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_map_range_search
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_map_singleton_search
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_set_bmp_singleton_search
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_set_nonbmp_singleton_search
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_set_bmp_range_search
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_set_nonbmp_range_search
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.getchar
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.put_twodigits_leading_blank
                0x0000000000000000       0x50 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_utf8_wctomb
                0x0000000000000000       0x88 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.put_twodigit_optional_zero_suppress
                0x0000000000000000       0x78 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__getc
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_pow10
                0x0000000000000000       0x58 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_pow10f
                0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__putc
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_print_padding
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_pre_padding
                0x0000000000000000       0x64 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__xlltoa
                0x0000000000000000       0x7c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__xtoa
                0x0000000000000000       0x58 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__xltoa
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.abs
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.asctime_r
                0x0000000000000000      0x13c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.asctime
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.atexit
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc._execute_at_exit_fns
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.bsearch
                0x0000000000000000       0x5c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_towupper
                0x0000000000000000       0x7c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_toupper
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_towlower
                0x0000000000000000       0x7c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_tolower
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_1_wctomb
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_11_wctomb
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_13_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_2_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_3_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_4_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_9_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_10_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_5_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_6_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_7_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_8_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1255_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1256_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1257_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1258_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_14_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_15_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_16_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1250_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1251_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1252_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1253_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1254_wctomb
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ctl_is_exact_power_of_two
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ctl_round_power_of_two
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ctl_count_leading_zeroes
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ctl_ilogb
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.buddy_alloc
                0x0000000000000000      0x124 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.buddy_heap_init
                0x0000000000000000       0x88 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_isctype
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_isctype_l
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isalpha
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isupper
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.islower
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isdigit
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__digit
                0x0000000000000000       0x44 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isxdigit
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isspace
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ispunct
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isalnum
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isgraph
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iscntrl
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isblank
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.tolower
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.toupper
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isalpha_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isupper_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.islower_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isdigit_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isxdigit_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isspace_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ispunct_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isalnum_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isprint_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isgraph_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iscntrl_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isblank_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.tolower_l
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.toupper_l
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isascii
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.div
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__aeabi_errno_addr
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.buddy_free
                0x0000000000000000       0xb4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__strtoul
                0x0000000000000000       0xd4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__strtoull
                0x0000000000000000      0x10c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fopen
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.vfprintf
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fprintf
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.vfscanf
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fscanf
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fgetpos
                0x0000000000000000       0x64 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ftell
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ungetc
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fileno
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.feof
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ferror
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fstat
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.gets
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.itoa
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.labs
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ldiv
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.linked_heap_init
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.linked_heap_alloc
                0x0000000000000000       0x9c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.linked_heap_free
                0x0000000000000000       0xb4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.linked_heap_realloc
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.llabs
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.lldiv
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.lltoa
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_global_locale_category
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_locale_category
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.localeconv_l
                0x0000000000000000       0xb0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.localeconv
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_compare_locale_name
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ltoa
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.malloc
                0x0000000000000000       0x8c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.getBuf
                0x0000000000000000       0x5c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fflush
                0x0000000000000000       0x44 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fseek
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fsetpos
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.rewind
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.output_fn
                0x0000000000000000       0x88 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fputc
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fputs
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fwrite
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.putc
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.getc_fn
                0x0000000000000000       0xcc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fgetc
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fread
                0x0000000000000000       0x84 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fgets
                0x0000000000000000       0x7c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.getc
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.calloc
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.free
                0x0000000000000000       0xa4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.setbuf
                0x0000000000000000       0x5c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.setvbuf
                0x0000000000000000       0x50 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.fclose
                0x0000000000000000       0x44 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.realloc
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.aligned_alloc
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.memccpy
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mempcpy
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.memchr
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.memcmp
                0x0000000000000000       0x74 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__aeabi_uread4
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__aeabi_uwrite4
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__aeabi_uread8
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__aeabi_uwrite8
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.memmove
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.printf
                0x0000000000000000       0x44 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.putchar
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.puts
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.qsort
                0x0000000000000000      0x218 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.rand
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.scanf
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.snprintf
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.sprintf
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.srand
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.sscanf
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strcasecmp
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strcasestr
                0x0000000000000000       0x5c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_decode_error.str1.4
                0x0000000000000000       0x7a C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_decode_error
                0x0000000000000000       0x7c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strerror
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_register_error_decoder
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strcat
                0x0000000000000000       0x84 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_encode_locale.str1.4
                0x0000000000000000        0x2 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_encode_locale
                0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strchr
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strcoll
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strcspn
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strdup
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_string_list_encode
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_string_list_decode
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strncasecmp
                0x0000000000000000       0x64 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strncasestr
                0x0000000000000000       0x60 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strncat
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strlcat
                0x0000000000000000       0x60 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strnchr
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strncmp
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strncpy
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strlcpy
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strnlen
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strndup
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strnstr
                0x0000000000000000       0x50 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strpbrk
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strrchr
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strsep
                0x0000000000000000       0x44 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strspn
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strstr
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtod
                0x0000000000000000      0x1cc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtold
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtof
                0x0000000000000000      0x1a4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtok
                0x0000000000000000       0x6c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtok_r
                0x0000000000000000       0x58 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtol
                0x0000000000000000       0xb8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.atoi
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.atof
                0x0000000000000000      0x150 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.atol
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtoll
                0x0000000000000000       0xbc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.atoll
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtoul
                0x0000000000000000       0x90 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strtoull
                0x0000000000000000       0x9c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strxfrm
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.stpcpy
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.localtime_r
                0x0000000000000000      0x144 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.difftime
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.checktm
                0x0000000000000000      0x1f0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mktime
                0x0000000000000000      0x158 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ctime
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ctime_r
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.gmtime
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.gmtime_r
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.localtime
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.gettimeofday
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.settimeofday
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.time
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ulltoa
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.ultoa
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.utoa
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.vprintf
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.vscanf
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.vsnprintf
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.vsprintf
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.vasprintf
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.vsscanf
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcscat
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcschr
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcscmp
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcscoll
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcscpy
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcscspn
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcslen
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsdup
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsncat
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsnchr
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsncmp
                0x0000000000000000       0x50 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsncpy
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsnlen
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsnstr
                0x0000000000000000       0x50 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcspbrk
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsrchr
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcssep
                0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsspn
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsstr
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcstok
                0x0000000000000000       0x6c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcstok_r
                0x0000000000000000       0x58 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wmemcpy
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wmemccpy
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wmempcpy
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wmemmove
                0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wmemcmp
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wmemchr
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wmemset
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsxfrm
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.tmpnam
                0x0000000000000000       0x5c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.duplocale
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.uselocale
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.freelocale
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__user_find_locale
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_find_locale
                0x0000000000000000       0x84 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_set_locale.part.0
                0x0000000000000000       0x60 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.newlocale
                0x0000000000000000       0x4c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.setlocale
                0x0000000000000000       0x94 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbsinit
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wctob_l
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wctob
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.btowc_l
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.btowc
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mblen_l
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mblen
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbrlen_l
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbrlen
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wctomb_l
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wctomb
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.put_formatted.str1.4
                0x0000000000000000       0x63 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.put_formatted
                0x0000000000000000      0x6cc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strftime_l
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.strftime
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcrtomb_l
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcrtomb
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbtowc_l
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbtowc
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.mbrtowc_l.str1.4
                0x0000000000000000        0x1 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbrtowc_l
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbrtowc
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbstowcs_l
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbstowcs
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbsrtowcs_l
                0x0000000000000000       0xa8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbsrtowcs
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.mbsnrtowcs
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcstombs_l
                0x0000000000000000       0xc4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcstombs
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsrtombs_l
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsrtombs
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wcsnrtombs
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_init_mbstate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_mb_max
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_1_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_1
                0x0000000000000000       0x4c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_1_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_1_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_2_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_2
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_2_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_2_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_3_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_3
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_3_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_3_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_4_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_4
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_4_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_4_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_5_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_5
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_5_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_5_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_6_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_6
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_6_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_6_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_7_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_7
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_7_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_7_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_8_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_8
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_8_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_8_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_9_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_9
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_9_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_9_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_10_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_10
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_10_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_10_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_11_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_11
                0x0000000000000000       0x4c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_11_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_11_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_13_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_13
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_13_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_13_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_14_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_14
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_14_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_14_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_15_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_15
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_15_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_15_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_16_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_iso8859_16
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_16_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_16_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1250_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1250
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1250_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1250_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1251_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1251
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1251_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1251_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1252_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1252
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1252_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1252_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1253_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1253
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1253_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1253_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1254_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1254
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1254_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1254_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1255_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1255
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1255_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1255_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1256_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1256
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1256_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1256_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1257_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1257
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1257_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1257_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1258_to_unicode
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_to_cp1258
                0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1258_toupper
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1258_tolower
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wctrans
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wctrans_l
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.towlower
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.towupper
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.towlower_l
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.towupper_l
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.towctrans
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.towctrans_l
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswalpha
                0x0000000000000000       0x84 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswprint
                0x0000000000000000       0x84 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswblank
                0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswcntrl
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswdigit
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswspace
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswxdigit
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswalnum
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswlower
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswupper
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswgraph
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswpunct
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_iswctype
                0x0000000000000000       0xf4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_unicode_isctype
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_1_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_2_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_3_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_4_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_5_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_6_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_7_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_8_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_9_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_10_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_11_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_13_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_14_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_15_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iso8859_16_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1250_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1251_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1252_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1253_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1254_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1255_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1256_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1257_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_cp1258_isctype
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.wctype
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iswctype
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_iswctype_l
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswalpha
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswupper
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswlower
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswdigit
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswxdigit
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswspace
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswpunct
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswalnum
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswprint
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswgraph
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswcntrl
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswblank
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswalpha_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswupper_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswlower_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswdigit_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswxdigit_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswspace_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswpunct_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswalnum_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswprint_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswgraph_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswcntrl_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.iswblank_l
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__RAL_asctime_buf
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__RAL_error_decoder_head
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__RAL_lconv_data
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__RAL_tmpnam_buf
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__RAL_tmpnam_fileno
                0x0000000000000000        0x2 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__atexitfns
                0x0000000000000000       0x80 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__user_format_extender
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__user_get_time_of_day
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.__user_set_time_of_day
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc._tm  0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.atexitfn_count
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.iod  0x0000000000000000       0x80 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.iod2
                0x0000000000000000       0x60 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .bss.libc.stdin
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .data.libc.__RAL_rand_next
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .data.libc.__ungot
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .data.libc.heap
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .data.libc.stderr
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .data.libc.stdout
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .data.libc.streams
                0x0000000000000000       0xc0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1250
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1251
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1252
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1253
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1254
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1255
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1256
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1257
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_cp1258
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_10
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_11
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_13
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_14
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_15
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_16
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_3
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_4
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_5
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_6
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_7
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_8
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_iso8859_9
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_codeset_utf8
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1250_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1251_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1252_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1253_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1254_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1255_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1256_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1257_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_cp1258_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_data_utf8_comma
                0x0000000000000000        0x2 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_data_utf8_minus
                0x0000000000000000        0x2 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_data_utf8_plus
                0x0000000000000000        0x2 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_data_utf8_space
                0x0000000000000000        0x2 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_hex_lc
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_hex_uc
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_10_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_11_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_13_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_14_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_15_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_16_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_1_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_2_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_3_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_4_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_5_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_6_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_7_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_8_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_iso8859_9_to_unicode_map
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_mon_lengths
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_tmpnam_template
                0x0000000000000000       0x11 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_isalpha_range
                0x0000000000000000      0x46c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_isalpha_singleton
                0x0000000000000000       0xac C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_isprint_range
                0x0000000000000000      0x534 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_isprint_singleton
                0x0000000000000000       0x52 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_tolower_range1_map
                0x0000000000000000       0xde C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_tolower_range2_map
                0x0000000000000000       0xde C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_tolower_singleton_map
                0x0000000000000000      0x13c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_toupper_range1_map
                0x0000000000000000       0xde C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_toupper_range2_map
                0x0000000000000000       0xd2 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_bmp_toupper_singleton_map
                0x0000000000000000      0x168 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_nonbmp_isalpha_range
                0x0000000000000000      0x2d0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_nonbmp_isalpha_singleton
                0x0000000000000000       0x74 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_nonbmp_isprint_range
                0x0000000000000000      0x470 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_nonbmp_isprint_singleton
                0x0000000000000000       0x88 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1250_range_map
                0x0000000000000000       0x6c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1250_singleton_map
                0x0000000000000000      0x140 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1251_range_map
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1251_singleton_map
                0x0000000000000000       0xa8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1252_range_map
                0x0000000000000000       0x1e C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1252_singleton_map
                0x0000000000000000       0x4c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1253_range_map
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1253_singleton_map
                0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1254_range_map
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1254_singleton_map
                0x0000000000000000       0x60 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1255_range_map
                0x0000000000000000       0x4e C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1255_singleton_map
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1256_range_map
                0x0000000000000000       0x72 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1256_singleton_map
                0x0000000000000000       0x98 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1257_range_map
                0x0000000000000000       0x4e C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1257_singleton_map
                0x0000000000000000      0x134 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1258_range_map
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_cp1258_singleton_map
                0x0000000000000000       0x80 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_10_range_map
                0x0000000000000000       0x36 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_10_singleton_map
                0x0000000000000000       0xe0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_11_range_map
                0x0000000000000000       0x12 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_13_range_map
                0x0000000000000000       0x42 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_13_singleton_map
                0x0000000000000000      0x104 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_14_range_map
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_14_singleton_map
                0x0000000000000000       0x60 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_15_range_map
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_15_singleton_map
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_16_range_map
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_16_singleton_map
                0x0000000000000000       0xb0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_1_range_map
                0x0000000000000000        0x6 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_2_range_map
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_2_singleton_map
                0x0000000000000000      0x124 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_3_range_map
                0x0000000000000000       0x5a C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_3_singleton_map
                0x0000000000000000       0x84 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_4_range_map
                0x0000000000000000       0x42 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_4_singleton_map
                0x0000000000000000       0xec C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_5_range_map
                0x0000000000000000       0x1e C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_5_singleton_map
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_6_range_map
                0x0000000000000000       0x12 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_6_singleton_map
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_7_range_map
                0x0000000000000000       0x36 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_7_singleton_map
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_8_range_map
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_8_singleton_map
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_9_range_map
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unicode_to_iso8859_9_singleton_map
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_unknown_string
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_wctrans_name_list
                0x0000000000000000       0x11 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_wctype_class_name_list
                0x0000000000000000       0x4a C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__RAL_year_lengths
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__aeabi_EDOM
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__aeabi_EILSEQ
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.__aeabi_ERANGE
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.power
                0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .rodata.libc.powerf
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_mbrlen_mbstate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_mbrtowc_mbstate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_mbsrtowcs_mbstate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_mbtowc_mbstate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_strtok_state
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_wcrtomb_mbstate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_wcsrtombs_mbstate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_wcstok_state
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.__RAL_wctomb_mbstate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .tbss.errno_val
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .data.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .bss.libc      0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text.libc.longjmp
                0x0000000000000000       0x16 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text.libc.memcpy_fast
                0x0000000000000000      0x3ac C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text.libc.memcpy_small
                0x0000000000000000       0x1a C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text.libc.memset
                0x0000000000000000       0x66 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text.libc.__aeabi_memset
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text.libc.setjmp
                0x0000000000000000        0xe C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text.libc.strcpy
                0x0000000000000000       0x44 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text.libc.strcmp
                0x0000000000000000       0x4e C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
 .text          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .data          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .bss           0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .rodata.libc.__vfprintf_int.str1.4
                0x0000000000000000        0x7 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_int
                0x0000000000000000      0x5e8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_int_nwp
                0x0000000000000000      0x5a0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_long
                0x0000000000000000      0x5fc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_long_nwp
                0x0000000000000000      0x5bc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_long_long
                0x0000000000000000      0x6b8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_long_long_nwp
                0x0000000000000000      0x710 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .rodata.libc.__vfprintf_float_long.str1.4
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_float_long
                0x0000000000000000     0x1100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_float_long_long
                0x0000000000000000     0x1100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_short_float_long
                0x0000000000000000      0xe68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_short_float_long_long
                0x0000000000000000      0xf48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__RAL_compute_wide_metrics
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__RAL_print_wide_string
                0x0000000000000000       0x4c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_int_wchar
                0x0000000000000000      0x6c4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_int_nwp_wchar
                0x0000000000000000      0x5e0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_long_wchar
                0x0000000000000000      0x6d4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_long_nwp_wchar
                0x0000000000000000      0x5e8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_long_long_wchar
                0x0000000000000000      0x790 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_long_long_nwp_wchar
                0x0000000000000000      0x738 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_float_long_wchar
                0x0000000000000000     0x11ac C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_float_long_long_wchar
                0x0000000000000000     0x11ac C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_short_float_long_wchar
                0x0000000000000000      0xef8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text.libc.__vfprintf_short_float_long_long_wchar
                0x0000000000000000     0x1010 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .rodata.libc.ipow10
                0x0000000000000000       0xa0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .comment       0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .ARM.attributes
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfprintf.o)
 .text          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .data          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .bss           0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.rd_string_map
                0x0000000000000000       0xb4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.rd_string
                0x0000000000000000       0xa8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.rd_int
                0x0000000000000000      0x188 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.rd_int_long_long
                0x0000000000000000      0x1a8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.rd_real
                0x0000000000000000      0x2ec C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_int
                0x0000000000000000      0x3e4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_int_cc
                0x0000000000000000      0x464 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_long
                0x0000000000000000      0x3f8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_long_cc
                0x0000000000000000      0x474 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_long_long
                0x0000000000000000      0x418 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_long_long_cc
                0x0000000000000000      0x498 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_float_long
                0x0000000000000000      0x408 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_float_long_cc
                0x0000000000000000      0x484 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_float_long_long
                0x0000000000000000      0x428 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text.libc.__vfscanf_float_long_long_cc
                0x0000000000000000      0x4a0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .comment       0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .ARM.attributes
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libvfscanf.o)
 .text          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .data          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .bss           0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.ctl_count_leading_zeros_64
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.ctl_count_trailing_zeros_16
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.ctl_count_trailing_zeros_32
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.ctl_count_trailing_zeros_64
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__popcountsi2
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__popcountdi2
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__paritysi2
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__paritydi2
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__bswapsi2
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__bswapdi2
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_lock
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_unlock
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_add_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_sub_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_or_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_and_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_xor_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_nand_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_add_and_fetch_1
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_sub_and_fetch_1
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_or_and_fetch_1
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_and_and_fetch_1
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_xor_and_fetch_1
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_nand_and_fetch_1
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_bool_compare_and_swap_1
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_val_compare_and_swap_1
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_lock_test_and_set_1
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_lock_release_1
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_add_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_sub_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_or_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_and_2
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_xor_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_nand_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_add_and_fetch_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_sub_and_fetch_2
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_or_and_fetch_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_and_and_fetch_2
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_xor_and_fetch_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_nand_and_fetch_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_bool_compare_and_swap_2
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_val_compare_and_swap_2
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_lock_test_and_set_2
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_lock_release_2
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_add_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_sub_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_or_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_and_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_xor_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_nand_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_add_and_fetch_4
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_sub_and_fetch_4
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_or_and_fetch_4
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_and_and_fetch_4
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_xor_and_fetch_4
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_nand_and_fetch_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_bool_compare_and_swap_4
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_val_compare_and_swap_4
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_lock_test_and_set_4
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_lock_release_4
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_add_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_sub_8
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_or_8
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_and_8
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_xor_8
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_fetch_and_nand_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_add_and_fetch_8
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_sub_and_fetch_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_or_and_fetch_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_and_and_fetch_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_xor_and_fetch_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_nand_and_fetch_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_bool_compare_and_swap_8
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_val_compare_and_swap_8
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_lock_test_and_set_8
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__sync_lock_release_8
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_load_1
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_store_1
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_exchange_1
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_compare_exchange_1
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_add_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_sub_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_or_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_and_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_xor_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_nand_1
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_load_2
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_store_2
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_exchange_2
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_compare_exchange_2
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_add_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_sub_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_or_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_and_2
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_xor_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_nand_2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_load_4
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_store_4
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_exchange_4
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_compare_exchange_4
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_add_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_sub_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_or_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_and_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_xor_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_nand_4
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_load_8
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_store_8
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_exchange_8
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_compare_exchange_8
                0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_add_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_sub_8
                0x0000000000000000       0x30 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_or_8
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_and_8
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_xor_8
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_fetch_nand_8
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_load
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_store
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__atomic_is_lock_free
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__heap_lock
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__heap_unlock
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__printf_lock
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__printf_unlock
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__scanf_lock
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc.__scanf_unlock
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .comment       0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .ARM.attributes
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc.o)
 .text.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .data.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .bss.libc      0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_umod
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_asr
                0x0000000000000000       0x26 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_div
                0x0000000000000000       0x44 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_lsl
                0x0000000000000000       0x26 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_lsr
                0x0000000000000000       0x26 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_mod
                0x0000000000000000       0x46 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_udivmod
                0x0000000000000000       0xce C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__aeabi_ldivmod
                0x0000000000000000       0x58 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_cmp
                0x0000000000000000       0x1a C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int64_ucmp
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.muldi3
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int32_umod
                0x0000000000000000        0xa C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int32_div
                0x0000000000000000      0x216 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .rodata.libc.__aeabi_idiv
                0x0000000000000000        0xa C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__uint32_div
                0x0000000000000000       0xf6 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .rodata.libc.__aeabi_uidiv
                0x0000000000000000       0x46 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__int32_mod
                0x0000000000000000        0xa C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__aeabi_uidivmod
                0x0000000000000000       0x2a C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__aeabi_idivmod
                0x0000000000000000       0x4a C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.ctl_count_leading_zeros_32
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.ctl_count_leading_zeros_16
                0x0000000000000000       0x32 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__gnu_thumb1_case_shi
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__gnu_thumb1_case_si
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__gnu_thumb1_case_sqi
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__gnu_thumb1_case_uhi
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text.libc.__gnu_thumb1_case_uqi
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .ARM.attributes
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc_asm.o)
 .text          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .data          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .bss           0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio
                0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_abort
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fopen
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fgets
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fputc
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fputs
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fread
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fwrite
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fseek
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_ftell
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_gets
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fflush
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fclose
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fgetc
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getchar
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_putchar
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_puts
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_rewind
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_clearerr
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_feof
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_ferror
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getch
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_time
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_vprintf
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_vfprintf
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_ungetc
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fgetpos
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_fsetpos
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_freopen
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_perror
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_remove
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_rename
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_tmpfile
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_tmpnam
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getenv
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_system
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_vfscanf
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_vscanf
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_exit
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_enabled
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_kbhit
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_ioctl
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_runtime_error
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_break
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getargs
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_geti
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getu
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getl
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getul
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getf
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getd
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getll
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_getull
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_filesize
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_accept
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_bind
                0x0000000000000000       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_listen
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_shutdown
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_socket
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_htons
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_htonl
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_loadsymbols
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_unloadsymbols
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.debug_evaluate
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.__debug_io_lock
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text.libdebugio.__debug_io_unlock
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .bss.libdebugio.__dbgEnabled
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .bss.libdebugio.getenv_buffer
                0x0000000000000000      0x400 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .bss.libdebugio.tmpnam_buffer
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .comment       0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .ARM.attributes
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libdebugio.o)
 .text          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(do_nv_debug_operation.o)
 .data          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(do_nv_debug_operation.o)
 .bss           0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(do_nv_debug_operation.o)
 .text.libdebugio
                0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(do_nv_debug_operation.o)
 .text.libdebugio.__do_nvdebug_operation
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(do_nv_debug_operation.o)
 .comment       0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(do_nv_debug_operation.o)
 .ARM.attributes
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(do_nv_debug_operation.o)
 .text          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .data          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .bss           0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .text.libdebugio
                0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .text.libdebugio.__do_debug_operation_mempoll
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .bss.libdebugio.dbgCntrlWord_mempoll
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .bss.libdebugio.dbgCommWord
                0x0000000000000000        0x4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .comment       0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .ARM.attributes
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a(mempoll_debug_operations.o)
 .text.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .data.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .bss.libc      0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .rodata.__aeabi_fdiv_reciprocal_table
                0x0000000000000000      0x100 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .rodata.__aeabi_ddiv_reciprocal_table
                0x0000000000000000      0x180 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fadd
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dadd
                0x0000000000000000      0x244 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fsub
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dsub
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_frsub
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_drsub
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fmul
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dmul
                0x0000000000000000      0x138 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fdiv
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_ddiv
                0x0000000000000000      0x1cc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fcmple
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dcmple
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fcmpeq
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dcmpeq
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fcmpge
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dcmpge
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fcmpgt
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dcmpgt
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fcmplt
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dcmplt
                0x0000000000000000       0x38 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_fcmpun
                0x0000000000000000       0x18 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_dcmpun
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_cfcmpeq
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_cdcmpeq
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_cfcmple
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_cdcmple
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_cfrcmple
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_cdrcmple
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__cmpdf2
                0x0000000000000000       0x64 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_f2iz
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_d2iz
                0x0000000000000000       0x4c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_f2lz
                0x0000000000000000       0x74 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_d2lz
                0x0000000000000000       0x84 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_f2uiz
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_d2uiz
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_f2ulz
                0x0000000000000000       0x44 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_d2ulz
                0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_i2f
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_i2d
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_l2f
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_l2d
                0x0000000000000000       0x68 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_ui2f
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_ui2d
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_ul2f
                0x0000000000000000       0x58 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_ul2d
                0x0000000000000000       0x5c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_f2d
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__aeabi_d2f
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float32_isfinite
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float64_isfinite
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float32_isinf
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float64_isinf
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float32_isnan
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float64_isnan
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float32_isnormal
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float64_isnormal
                0x0000000000000000       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float32_signbit
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float64_signbit
                0x0000000000000000        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float32_classify
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.__float64_classify
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.fabs     0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.fabsf    0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.ceilf    0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.floorf   0x0000000000000000       0x70 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.frexpf   0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text.ldexpf   0x0000000000000000       0x48 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .ARM.attributes
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm_asm.o)
 .text          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .data          0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .bss           0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc     0x0000000000000000        0x0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.__RAL_asinacosf
                0x0000000000000000      0x174 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.__RAL_poly1_eval
                0x0000000000000000       0x54 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.__RAL_poly1_evalf
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.__RAL_poly_eval
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.__RAL_poly_evalf
                0x0000000000000000       0x2c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.__RAL_sincos
                0x0000000000000000      0x224 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.__RAL_sincosf
                0x0000000000000000       0xf8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.acosf
                0x0000000000000000      0x150 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.asinf
                0x0000000000000000      0x12c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.atan
                0x0000000000000000      0x290 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.atan2
                0x0000000000000000      0x14c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.atanf
                0x0000000000000000      0x12c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.atan2f
                0x0000000000000000       0xcc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.ceil
                0x0000000000000000       0xa8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.cos
                0x0000000000000000      0x1c8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.cosf
                0x0000000000000000      0x17c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.expf
                0x0000000000000000      0x16c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.coshf
                0x0000000000000000       0xa8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.fma
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.fmax
                0x0000000000000000       0x50 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.fmaxf
                0x0000000000000000       0x3c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.fmin
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.fminf
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.frexp
                0x0000000000000000       0x50 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.hypotf
                0x0000000000000000       0xec C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.ldexp
                0x0000000000000000       0x7c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.exp
                0x0000000000000000      0x200 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.cosh
                0x0000000000000000      0x128 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.log
                0x0000000000000000      0x230 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.atanh
                0x0000000000000000      0x160 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.log10
                0x0000000000000000       0x28 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.logf
                0x0000000000000000      0x114 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.acoshf
                0x0000000000000000       0xc0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.asinhf
                0x0000000000000000       0xa8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.atanhf
                0x0000000000000000       0xd4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.log10f
                0x0000000000000000       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.modf
                0x0000000000000000       0x94 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.modff
                0x0000000000000000       0x5c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.pow
                0x0000000000000000      0x168 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.exp2
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.powf
                0x0000000000000000       0xcc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.exp2f
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.scalbn
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.scalbnf
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.sin
                0x0000000000000000      0x1bc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.sinf
                0x0000000000000000      0x164 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.sinh
                0x0000000000000000      0x250 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.sinhf
                0x0000000000000000       0xc8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.tan
                0x0000000000000000      0x23c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.tanf
                0x0000000000000000      0x15c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.tanh
                0x0000000000000000      0x1ec C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.tanhf
                0x0000000000000000       0xe0 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.sqrt
                0x0000000000000000      0x134 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.__RAL_asinacos
                0x0000000000000000      0x2dc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.acosh
                0x0000000000000000      0x138 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.asinh
                0x0000000000000000      0x124 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.hypot
                0x0000000000000000      0x204 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.asin
                0x0000000000000000      0x27c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.acos
                0x0000000000000000      0x284 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.cbrtf
                0x0000000000000000       0xe4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.cbrt
                0x0000000000000000      0x1fc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.floor
                0x0000000000000000       0xa8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.fmodf
                0x0000000000000000       0xfc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .text.libc.fmod
                0x0000000000000000      0x1a4 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .rodata.libc.__asinacos_a
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .rodata.libc.__asinacos_b
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .rodata.libc.__asinacosf_a
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .rodata.libc.__asinacosf_b
                0x0000000000000000        0x8 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .rodata.libc.atanf_a
                0x0000000000000000       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .rodata.libc.expf_twojby8
                0x0000000000000000       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .comment       0x0000000000000000       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)
 .ARM.attributes
                0x0000000000000000       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libm2.o)

Memory Configuration

Name             Origin             Length             Attributes
UNPLACED_SECTIONS 0x0000000100000000 0x0000000000000000 xw
RAM              0x0000000020000000 0x0000000000040000 xw
FLASH            0x0000000000000000 0x0000000000100000 xw
*default*        0x0000000000000000 0xffffffffffffffff

Linker script and memory map

                0x0000000000000000                __do_debug_operation = __do_debug_operation_mempoll
                0x0000000000000000                __vfprintf = __vfprintf_long
                0x0000000000000000                __vfscanf = __vfscanf_long
                0x0000000020000000                __RAM_segment_start__ = 0x20000000
                0x0000000020040000                __RAM_segment_end__ = 0x20040000
                0x0000000000040000                __RAM_segment_size__ = 0x40000
                0x0000000000000000                __FLASH_segment_start__ = 0x0
                0x0000000000100000                __FLASH_segment_end__ = 0x100000
                0x0000000000100000                __FLASH_segment_size__ = 0x100000
                0x0000000000002000                __HEAPSIZE__ = 0x2000
                0x0000000000000000                __STACKSIZE_PROCESS__ = 0x0
                0x0000000000002000                __STACKSIZE__ = 0x2000
                0x0000000020000000                __vectors_ram_load_start__ = 0x20000000

.vectors_ram    0x0000000020000000        0x0
                0x0000000020000000                __vectors_ram_start__ = .
                0x0000000020000000                __app_ram_start__ = __vectors_ram_start__
 *(.vectors_ram .vectors_ram.*)
                0x0000000020000000                __vectors_ram_end__ = (__vectors_ram_start__ + SIZEOF (.vectors_ram))
                0x0000000000000000                __vectors_ram_size__ = SIZEOF (.vectors_ram)
                0x0000000020000000                __vectors_ram_load_end__ = __vectors_ram_end__
                0x0000000000000001                . = ASSERT (((__vectors_ram_start__ == __vectors_ram_end__) || ((__vectors_ram_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .vectors_ram is too large to fit in RAM memory segment)
                0x0000000020000000                __nrf_sections_run_load_start__ = ALIGN (__vectors_ram_end__, 0x4)

.nrf_sections_run
                0x0000000020000000        0x0
                0x0000000020000000                __nrf_sections_run_start__ = .
                0x0000000020000000                __start_nrf_sections_run = __nrf_sections_run_start__
 *(.nrf_sections_run .nrf_sections_run.*)
                0x0000000020000000                __nrf_sections_run_end__ = (__nrf_sections_run_start__ + SIZEOF (.nrf_sections_run))
                0x0000000000000000                __nrf_sections_run_size__ = SIZEOF (.nrf_sections_run)
                0x0000000020000000                __nrf_sections_run_load_end__ = __nrf_sections_run_end__
                0x0000000000000001                . = ASSERT (((__nrf_sections_run_start__ == __nrf_sections_run_end__) || ((__nrf_sections_run_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .nrf_sections_run is too large to fit in RAM memory segment)
                0x0000000000000000                __vectors_load_start__ = 0x0

.vectors        0x0000000000000000      0x200
                0x0000000000000000                __vectors_start__ = .
 *(.vectors .vectors.*)
 .vectors       0x0000000000000000      0x200 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
                0x0000000000000000                _vectors
                0x0000000000000200                __vectors_end__ = (__vectors_start__ + SIZEOF (.vectors))
                0x0000000000000200                __vectors_size__ = SIZEOF (.vectors)
                0x0000000000000200                __vectors_load_end__ = __vectors_end__
                0x0000000000000001                . = ASSERT (((__vectors_start__ == __vectors_end__) || ((__vectors_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .vectors is too large to fit in FLASH memory segment)
                0x0000000000000200                __init_load_start__ = ALIGN (__vectors_end__, 0x4)

.init           0x0000000000000200      0x1d0
                0x0000000000000200                __init_start__ = .
 *(.init .init.*)
 .init          0x0000000000000200      0x15c Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
                0x0000000000000200                _start
                0x00000000000002b4                exit
 .init          0x000000000000035c       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
                0x000000000000035c                NMI_Handler
                0x000000000000035e                HardFault_Handler
                0x0000000000000360                MemoryManagement_Handler
                0x0000000000000362                BusFault_Handler
                0x0000000000000364                UsageFault_Handler
                0x0000000000000366                SVC_Handler
                0x0000000000000368                DebugMon_Handler
                0x000000000000036a                PendSV_Handler
                0x000000000000036c                SysTick_Handler
                0x000000000000036e                SWI0_EGU0_IRQHandler
                0x000000000000036e                RADIO_IRQHandler
                0x000000000000036e                PDM_IRQHandler
                0x000000000000036e                PWM1_IRQHandler
                0x000000000000036e                GPIOTE_IRQHandler
                0x000000000000036e                QDEC_IRQHandler
                0x000000000000036e                TIMER3_IRQHandler
                0x000000000000036e                PWM3_IRQHandler
                0x000000000000036e                FPU_IRQHandler
                0x000000000000036e                USBD_IRQHandler
                0x000000000000036e                SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler
                0x000000000000036e                SWI2_EGU2_IRQHandler
                0x000000000000036e                TIMER4_IRQHandler
                0x000000000000036e                TEMP_IRQHandler
                0x000000000000036e                I2S_IRQHandler
                0x000000000000036e                SWI4_EGU4_IRQHandler
                0x000000000000036e                UARTE1_IRQHandler
                0x000000000000036e                Dummy_Handler
                0x000000000000036e                TIMER1_IRQHandler
                0x000000000000036e                SPIM3_IRQHandler
                0x000000000000036e                PWM2_IRQHandler
                0x000000000000036e                ECB_IRQHandler
                0x000000000000036e                SPIM1_SPIS1_TWIM1_TWIS1_SPI1_TWI1_IRQHandler
                0x000000000000036e                CCM_AAR_IRQHandler
                0x000000000000036e                WDT_IRQHandler
                0x000000000000036e                QSPI_IRQHandler
                0x000000000000036e                SWI5_EGU5_IRQHandler
                0x000000000000036e                RNG_IRQHandler
                0x000000000000036e                RTC2_IRQHandler
                0x000000000000036e                PWM0_IRQHandler
                0x000000000000036e                SWI3_EGU3_IRQHandler
                0x000000000000036e                RTC1_IRQHandler
                0x000000000000036e                SWI1_EGU1_IRQHandler
                0x000000000000036e                SPIM2_SPIS2_SPI2_IRQHandler
                0x000000000000036e                NFCT_IRQHandler
                0x000000000000036e                CRYPTOCELL_IRQHandler
                0x000000000000036e                MWU_IRQHandler
                0x000000000000036e                TIMER2_IRQHandler
                0x000000000000036e                COMP_LPCOMP_IRQHandler
                0x0000000000000370                nRFInitialize
 .init          0x0000000000000374       0x5c Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
                0x0000000000000374                Reset_Handler
                0x0000000000000378                afterInitialize
                0x000000000000039c                InitializeUserMemorySections
                0x00000000000003d0                __init_end__ = (__init_start__ + SIZEOF (.init))
                0x00000000000001d0                __init_size__ = SIZEOF (.init)
                0x00000000000003d0                __init_load_end__ = __init_end__
                0x0000000000000001                . = ASSERT (((__init_start__ == __init_end__) || ((__init_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .init is too large to fit in FLASH memory segment)
                0x00000000000003d0                __init_rodata_load_start__ = ALIGN (__init_end__, 0x4)

.init_rodata    0x00000000000003d0        0x0
                0x00000000000003d0                __init_rodata_start__ = .
 *(.init_rodata .init_rodata.*)
                0x00000000000003d0                __init_rodata_end__ = (__init_rodata_start__ + SIZEOF (.init_rodata))
                0x0000000000000000                __init_rodata_size__ = SIZEOF (.init_rodata)
                0x00000000000003d0                __init_rodata_load_end__ = __init_rodata_end__
                0x0000000000000001                . = ASSERT (((__init_rodata_start__ == __init_rodata_end__) || ((__init_rodata_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .init_rodata is too large to fit in FLASH memory segment)
                0x00000000000003d0                __text_load_start__ = ALIGN (__init_rodata_end__, 0x4)

.text           0x00000000000003d0     0x28b6
                0x00000000000003d0                __text_start__ = .
 *(.text .text.* .glue_7t .glue_7 .gnu.linkonce.t.* .gcc_except_table .ARM.extab* .gnu.linkonce.armextab.*)
 .glue_7        0x00000000000003d0        0x0 linker stubs
 .glue_7t       0x00000000000003d0        0x0 linker stubs
 .text.nrf_log_backend_serial_put
                0x00000000000003d0       0xc2 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
                0x00000000000003d0                nrf_log_backend_serial_put
 *fill*         0x0000000000000492        0x2 
 .text.uart_evt_handler
                0x0000000000000494        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .text.nrf_log_backend_uart_flush
                0x00000000000004a0        0x2 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 *fill*         0x00000000000004a2        0x2 
 .text.uart_init
                0x00000000000004a4       0x4c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .text.nrf_log_backend_uart_put
                0x00000000000004f0       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .text.serial_tx
                0x000000000000050c       0x48 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .text.nrf_log_backend_uart_panic_set
                0x0000000000000554       0x2c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .text.nrf_log_backend_uart_init
                0x0000000000000580        0x6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
                0x0000000000000580                nrf_log_backend_uart_init
 *fill*         0x0000000000000586        0x2 
 .text.nrf_log_default_backends_init
                0x0000000000000588       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
                0x0000000000000588                nrf_log_default_backends_init
 .text.invalid_packets_omit
                0x00000000000005a8       0x3a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 *fill*         0x00000000000005e2        0x2 
 .text.buf_prealloc
                0x00000000000005e4      0x130 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_init
                0x0000000000000714       0x3c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000000714                nrf_log_init
 .text.nrf_log_module_name_get
                0x0000000000000750       0x38 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000000750                nrf_log_module_name_get
 .text.nrf_log_color_id_get
                0x0000000000000788       0x2c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000000788                nrf_log_color_id_get
 .text.buffer_is_empty
                0x00000000000007b4       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x00000000000007b4                buffer_is_empty
 .text.nrf_log_frontend_dequeue
                0x00000000000007c8      0x224 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x00000000000007c8                nrf_log_frontend_dequeue
 .text.std_n    0x00000000000009ec       0x98 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .text.nrf_log_frontend_std_0
                0x0000000000000a84        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000000a84                nrf_log_frontend_std_0
 .text.nrf_log_frontend_std_1
                0x0000000000000a8c       0x12 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000000a8c                nrf_log_frontend_std_1
 *fill*         0x0000000000000a9e        0x2 
 .text.nrf_log_backend_add
                0x0000000000000aa0       0x44 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000000aa0                nrf_log_backend_add
 .text.nrf_log_panic
                0x0000000000000ae4       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000000ae4                nrf_log_panic
 .text.prefix_process
                0x0000000000000b0c       0x7c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .text.postfix_process
                0x0000000000000b88       0x44 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .text.nrf_log_std_entry_process
                0x0000000000000bcc       0xc8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
                0x0000000000000bcc                nrf_log_std_entry_process
 .text.nrf_log_hexdump_entry_process
                0x0000000000000c94       0xc0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
                0x0000000000000c94                nrf_log_hexdump_entry_process
 .text.app_error_handler_bare
                0x0000000000000d54       0x1a Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
                0x0000000000000d54                app_error_handler_bare
 *fill*         0x0000000000000d6e        0x2 
 .text.app_error_fault_handler
                0x0000000000000d70       0x6c Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
                0x0000000000000d70                app_error_fault_handler
 .text.app_util_disable_irq
                0x0000000000000ddc       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
                0x0000000000000ddc                app_util_disable_irq
 .text.app_util_enable_irq
                0x0000000000000dec       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
                0x0000000000000dec                app_util_enable_irq
 .text.app_util_critical_region_enter
                0x0000000000000e00        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
                0x0000000000000e00                app_util_critical_region_enter
 .text.app_util_critical_region_exit
                0x0000000000000e04        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
                0x0000000000000e04                app_util_critical_region_exit
 .text.nrf_atomic_u32_fetch_store
                0x0000000000000e08       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
                0x0000000000000e08                nrf_atomic_u32_fetch_store
 .text.nrf_atomic_u32_or
                0x0000000000000e1e       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
                0x0000000000000e1e                nrf_atomic_u32_or
 .text.nrf_atomic_u32_fetch_and
                0x0000000000000e36       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
                0x0000000000000e36                nrf_atomic_u32_fetch_and
 .text.nrf_atomic_u32_add
                0x0000000000000e4e       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
                0x0000000000000e4e                nrf_atomic_u32_add
 .text.nrf_atomic_u32_sub
                0x0000000000000e66       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
                0x0000000000000e66                nrf_atomic_u32_sub
 .text.nrf_atomic_flag_set
                0x0000000000000e7e        0x6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
                0x0000000000000e7e                nrf_atomic_flag_set
 .text.nrf_atomic_flag_clear_fetch
                0x0000000000000e84        0x6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
                0x0000000000000e84                nrf_atomic_flag_clear_fetch
 .text.nrf_balloc_init
                0x0000000000000e8a       0x2e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
                0x0000000000000e8a                nrf_balloc_init
 .text.nrf_balloc_alloc
                0x0000000000000eb8       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
                0x0000000000000eb8                nrf_balloc_alloc
 .text.nrf_balloc_free
                0x0000000000000ef8       0x2a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
                0x0000000000000ef8                nrf_balloc_free
 .text.nrf_fprintf_buffer_flush
                0x0000000000000f22       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
                0x0000000000000f22                nrf_fprintf_buffer_flush
 .text.nrf_fprintf
                0x0000000000000f38       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
                0x0000000000000f38                nrf_fprintf
 .text.buffer_add
                0x0000000000000f54       0x2e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 *fill*         0x0000000000000f82        0x2 
 .text.unsigned_print
                0x0000000000000f84       0xb4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .text.nrf_fprintf_fmt
                0x0000000000001038      0x294 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
                0x0000000000001038                nrf_fprintf_fmt
 .text.memobj_op
                0x00000000000012cc       0x86 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .text.nrf_memobj_pool_init
                0x0000000000001352        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
                0x0000000000001352                nrf_memobj_pool_init
 .text.nrf_memobj_free
                0x0000000000001356       0x2c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
                0x0000000000001356                nrf_memobj_free
 .text.nrf_memobj_alloc
                0x0000000000001382       0x5e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
                0x0000000000001382                nrf_memobj_alloc
 .text.nrf_memobj_get
                0x00000000000013e0        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
                0x00000000000013e0                nrf_memobj_get
 .text.nrf_memobj_put
                0x00000000000013e8       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
                0x00000000000013e8                nrf_memobj_put
 .text.nrf_memobj_write
                0x0000000000001404       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
                0x0000000000001404                nrf_memobj_write
 .text.nrf_memobj_read
                0x0000000000001418       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
                0x0000000000001418                nrf_memobj_read
 .text.nrf_pwr_mgmt_init
                0x000000000000142c       0x2c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
                0x000000000000142c                nrf_pwr_mgmt_init
 .text.nrf_pwr_mgmt_run
                0x0000000000001458       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
                0x0000000000001458                nrf_pwr_mgmt_run
 .text.nrf_ringbuf_init
                0x000000000000148c       0x12 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
                0x000000000000148c                nrf_ringbuf_init
 .text.nrf_section_iter_init
                0x000000000000149e       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
                0x000000000000149e                nrf_section_iter_init
 *fill*         0x00000000000014b2        0x2 
 .text.nrf_drv_ppi_init
                0x00000000000014b4       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
                0x00000000000014b4                nrf_drv_ppi_init
 .text.uarte_evt_handler
                0x00000000000014c8       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .text.uart_evt_handler
                0x00000000000014fc       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .text.nrf_drv_uart_init
                0x0000000000001530       0x7c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
                0x0000000000001530                nrf_drv_uart_init
 .text.nrfx_ppi_channel_alloc
                0x00000000000015ac       0x5c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
                0x00000000000015ac                nrfx_ppi_channel_alloc
 .text.nrfx_ppi_channel_assign
                0x0000000000001608       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
                0x0000000000001608                nrfx_ppi_channel_assign
 .text.nrfx_ppi_channel_enable
                0x0000000000001648       0x2c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
                0x0000000000001648                nrfx_ppi_channel_enable
 .text.UARTE0_UART0_IRQHandler
                0x0000000000001674        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
                0x0000000000001674                UARTE0_UART0_IRQHandler
 .text.nrfx_prs_acquire
                0x0000000000001680       0x38 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
                0x0000000000001680                nrfx_prs_acquire
 .text.nrfx_prs_release
                0x00000000000016b8       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
                0x00000000000016b8                nrfx_prs_release
 .text.nrf_saadc_event_clear
                0x00000000000016d0       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .text.SAADC_IRQHandler
                0x00000000000016e8      0x154 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
                0x00000000000016e8                SAADC_IRQHandler
 .text.nrfx_saadc_init
                0x000000000000183c       0x88 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
                0x000000000000183c                nrfx_saadc_init
 .text.nrfx_saadc_channel_init
                0x00000000000018c4       0x90 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
                0x00000000000018c4                nrfx_saadc_channel_init
 .text.nrfx_saadc_sample_task_get
                0x0000000000001954       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
                0x0000000000001954                nrfx_saadc_sample_task_get
 .text.nrfx_saadc_buffer_convert
                0x0000000000001970       0xa4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
                0x0000000000001970                nrfx_saadc_buffer_convert
 .text.nrfx_timer_init
                0x0000000000001a14       0xd0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
                0x0000000000001a14                nrfx_timer_init
 .text.nrfx_timer_enable
                0x0000000000001ae4       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
                0x0000000000001ae4                nrfx_timer_enable
 .text.nrfx_timer_compare
                0x0000000000001b00       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
                0x0000000000001b00                nrfx_timer_compare
 .text.nrfx_timer_extended_compare
                0x0000000000001b32       0x2a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
                0x0000000000001b32                nrfx_timer_extended_compare
 .text.TIMER0_IRQHandler
                0x0000000000001b5c       0x54 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
                0x0000000000001b5c                TIMER0_IRQHandler
 .text.nrf_uart_event_clear
                0x0000000000001bb0       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.tx_byte  0x0000000000001bc0       0x1e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.rx_byte  0x0000000000001bde       0x2c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 *fill*         0x0000000000001c0a        0x2 
 .text.rx_done_event.constprop.0
                0x0000000000001c0c       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_0_irq_handler
                0x0000000000001c2c      0x140 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
                0x0000000000001c2c                nrfx_uart_0_irq_handler
 .text.nrf_gpio_cfg_default
                0x0000000000001d6c       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .text.nrfx_uart_init
                0x0000000000001d8c      0x1a8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
                0x0000000000001d8c                nrfx_uart_init
 .text.nrfx_uart_uninit
                0x0000000000001f34       0xa8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
                0x0000000000001f34                nrfx_uart_uninit
 .text.nrfx_uart_tx_in_progress
                0x0000000000001fdc       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
                0x0000000000001fdc                nrfx_uart_tx_in_progress
 .text.nrfx_uart_tx
                0x0000000000001ff4       0xa0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
                0x0000000000001ff4                nrfx_uart_tx
 .text.nrf_uarte_event_clear
                0x0000000000002094       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.rx_done_event.constprop.0
                0x00000000000020a4       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_uarte_0_irq_handler
                0x00000000000020c4      0x118 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
                0x00000000000020c4                nrfx_uarte_0_irq_handler
 .text.nrf_gpio_cfg_default
                0x00000000000021dc       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .text.nrfx_uarte_init
                0x00000000000021fc      0x1c4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
                0x00000000000021fc                nrfx_uarte_init
 .text.nrfx_uarte_uninit
                0x00000000000023c0       0xcc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
                0x00000000000023c0                nrfx_uarte_uninit
 .text.nrfx_uarte_tx_in_progress
                0x000000000000248c       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
                0x000000000000248c                nrfx_uarte_tx_in_progress
 .text.nrfx_uarte_tx
                0x00000000000024a4       0x9c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
                0x00000000000024a4                nrfx_uarte_tx
 .text.nrfx_clock_init
                0x0000000000002540       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
                0x0000000000002540                nrfx_clock_init
 .text.nrfx_clock_enable
                0x0000000000002558       0x24 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
                0x0000000000002558                nrfx_clock_enable
 .text.nrfx_clock_lfclk_start
                0x000000000000257c       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
                0x000000000000257c                nrfx_clock_lfclk_start
 *fill*         0x000000000000259e        0x2 
 .text.POWER_CLOCK_IRQHandler
                0x00000000000025a0       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
                0x00000000000025a0                POWER_CLOCK_IRQHandler
 .text.nrf_rtc_event_clear
                0x0000000000002604       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .text.RTC0_IRQHandler
                0x0000000000002614       0x9c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
                0x0000000000002614                RTC0_IRQHandler
 .text.clock_clk_started_notify
                0x00000000000026b0       0x24 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.clock_irq_handler
                0x00000000000026d4       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .text.nrf_drv_clock_init
                0x00000000000026f0       0x30 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
                0x00000000000026f0                nrf_drv_clock_init
 .text.nrf_drv_clock_lfclk_request
                0x0000000000002720       0x54 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
                0x0000000000002720                nrf_drv_clock_lfclk_request
 .text.timer_handler
                0x0000000000002774        0x2 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
                0x0000000000002774                timer_handler
 *fill*         0x0000000000002776        0x2 
 .text.saadc_callback
                0x0000000000002778       0x68 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
                0x0000000000002778                saadc_callback
 .text.saadc_sampling_event_init
                0x00000000000027e0       0x88 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
                0x00000000000027e0                saadc_sampling_event_init
 .text.saadc_sampling_event_enable
                0x0000000000002868       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
                0x0000000000002868                saadc_sampling_event_enable
 .text.saadc_init
                0x0000000000002884       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
                0x0000000000002884                saadc_init
 .text.startup.main
                0x00000000000028e8       0x68 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
                0x00000000000028e8                main
 .text.errata_98
                0x0000000000002950       0x1a Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 *fill*         0x000000000000296a        0x2 
 .text.SystemInit
                0x000000000000296c      0x1bc Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
                0x000000000000296c                SystemInit
 .text.libc.__RAL_ascii_isctype
                0x0000000000002b28       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_ascii_toupper
                0x0000000000002b44        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_ascii_tolower
                0x0000000000002b50        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_ascii_wctomb
                0x0000000000002b5c       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000002b5c                __RAL_ascii_wctomb
 .text.libc.__RAL_ascii_mbtowc
                0x0000000000002b6c       0x24 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000002b6c                __RAL_ascii_mbtowc
 .text.libc.__RAL_ascii_towupper
                0x0000000000002b90        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_ascii_towlower
                0x0000000000002b9c        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.__RAL_ascii_iswctype
                0x0000000000002ba8       0x1c C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .text.libc.isprint
                0x0000000000002bc4       0x10 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000002bc4                isprint
 .text.libc.memcpy
                0x0000000000002bd4       0x52 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
                0x0000000000002bd4                __aeabi_memcpy
                0x0000000000002bd4                memcpy
                0x0000000000002be0                __aeabi_memcpy8
                0x0000000000002be0                __aeabi_memcpy4
 .text.libc.strlen
                0x0000000000002c26       0x60 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)
                0x0000000000002c26                strlen
                0x0000000000002c86                __text_end__ = (__text_start__ + SIZEOF (.text))
                0x00000000000028b6                __text_size__ = SIZEOF (.text)
                0x0000000000002c86                __text_load_end__ = __text_end__

.vfp11_veneer   0x0000000100000000        0x0
 .vfp11_veneer  0x0000000100000000        0x0 linker stubs

.v4_bx          0x0000000100000000        0x0
 .v4_bx         0x0000000100000000        0x0 linker stubs

.iplt           0x0000000100000000        0x0
 .iplt          0x0000000100000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
                0x0000000000000001                . = ASSERT (((__text_start__ == __text_end__) || ((__text_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .text is too large to fit in FLASH memory segment)
                0x0000000000002c88                __pwr_mgmt_data_load_start__ = ALIGN (__text_end__, 0x4)

.pwr_mgmt_data  0x0000000000002c88        0x0
                0x0000000000002c88                __pwr_mgmt_data_start__ = .
                0x0000000000002c88                __start_pwr_mgmt_data = __pwr_mgmt_data_start__
 *(SORT_BY_NAME(.pwr_mgmt_data*))
                0x0000000000002c88                __pwr_mgmt_data_end__ = (__pwr_mgmt_data_start__ + SIZEOF (.pwr_mgmt_data))
                0x0000000000000000                __pwr_mgmt_data_size__ = SIZEOF (.pwr_mgmt_data)
                0x0000000000002c88                __stop_pwr_mgmt_data = __pwr_mgmt_data_end__
                0x0000000000002c88                __pwr_mgmt_data_load_end__ = __pwr_mgmt_data_end__
                0x0000000000000001                . = ASSERT (((__pwr_mgmt_data_start__ == __pwr_mgmt_data_end__) || ((__pwr_mgmt_data_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .pwr_mgmt_data is too large to fit in FLASH memory segment)
                0x0000000000002c88                __log_const_data_load_start__ = ALIGN (__pwr_mgmt_data_end__, 0x4)

.log_const_data
                0x0000000000002c88       0x58
                0x0000000000002c88                __log_const_data_start__ = .
                0x0000000000002c88                __start_log_const_data = __log_const_data_start__
 *(SORT_BY_NAME(.log_const_data*))
 .log_const_data_CLOCK
                0x0000000000002c88        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
                0x0000000000002c88                m_nrf_log_CLOCK_logs_data_const
 .log_const_data_PPI
                0x0000000000002c90        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
                0x0000000000002c90                m_nrf_log_PPI_logs_data_const
 .log_const_data_PRS
                0x0000000000002c98        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
                0x0000000000002c98                m_nrf_log_PRS_logs_data_const
 .log_const_data_RTC
                0x0000000000002ca0        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
                0x0000000000002ca0                m_nrf_log_RTC_logs_data_const
 .log_const_data_SAADC
                0x0000000000002ca8        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
                0x0000000000002ca8                m_nrf_log_SAADC_logs_data_const
 .log_const_data_TIMER
                0x0000000000002cb0        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
                0x0000000000002cb0                m_nrf_log_TIMER_logs_data_const
 .log_const_data_UART
                0x0000000000002cb8        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
                0x0000000000002cb8                m_nrf_log_UART_logs_data_const
 .log_const_data_UARTE
                0x0000000000002cc0        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
                0x0000000000002cc0                m_nrf_log_UARTE_logs_data_const
 .log_const_data_app
                0x0000000000002cc8        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000002cc8                m_nrf_log_app_logs_data_const
 .log_const_data_clock
                0x0000000000002cd0        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
                0x0000000000002cd0                m_nrf_log_clock_logs_data_const
 .log_const_data_pwr_mgmt
                0x0000000000002cd8        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
                0x0000000000002cd8                m_nrf_log_pwr_mgmt_logs_data_const
                0x0000000000002ce0                __log_const_data_end__ = (__log_const_data_start__ + SIZEOF (.log_const_data))
                0x0000000000000058                __log_const_data_size__ = SIZEOF (.log_const_data)
                0x0000000000002ce0                __stop_log_const_data = __log_const_data_end__
                0x0000000000002ce0                __log_const_data_load_end__ = __log_const_data_end__
                0x0000000000000001                . = ASSERT (((__log_const_data_start__ == __log_const_data_end__) || ((__log_const_data_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .log_const_data is too large to fit in FLASH memory segment)
                0x0000000000002ce0                __log_backends_load_start__ = ALIGN (__log_const_data_end__, 0x4)

.log_backends   0x0000000000002ce0       0x10
                0x0000000000002ce0                __log_backends_start__ = .
                0x0000000000002ce0                __start_log_backends = __log_backends_start__
 *(SORT_BY_NAME(.log_backends*))
 .log_backends  0x0000000000002ce0       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
                0x0000000000002cf0                __log_backends_end__ = (__log_backends_start__ + SIZEOF (.log_backends))
                0x0000000000000010                __log_backends_size__ = SIZEOF (.log_backends)
                0x0000000000002cf0                __stop_log_backends = __log_backends_end__
                0x0000000000002cf0                __log_backends_load_end__ = __log_backends_end__
                0x0000000000000001                . = ASSERT (((__log_backends_start__ == __log_backends_end__) || ((__log_backends_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .log_backends is too large to fit in FLASH memory segment)
                0x0000000000002cf0                __nrf_balloc_load_start__ = ALIGN (__log_backends_end__, 0x4)

.nrf_balloc     0x0000000000002cf0       0x14
                0x0000000000002cf0                __nrf_balloc_start__ = .
                0x0000000000002cf0                __start_nrf_balloc = __nrf_balloc_start__
 *(.nrf_balloc*)
 .nrf_balloc    0x0000000000002cf0       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                0x0000000000002cf0                log_mempool
                0x0000000000002d04                __nrf_balloc_end__ = (__nrf_balloc_start__ + SIZEOF (.nrf_balloc))
                0x0000000000000014                __nrf_balloc_size__ = SIZEOF (.nrf_balloc)
                0x0000000000002d04                __stop_nrf_balloc = __nrf_balloc_end__
                0x0000000000002d04                __nrf_balloc_load_end__ = __nrf_balloc_end__
                0x0000000000000001                . = ASSERT (((__nrf_balloc_start__ == __nrf_balloc_end__) || ((__nrf_balloc_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .nrf_balloc is too large to fit in FLASH memory segment)
                0x0000000000002d04                __nrf_sections_load_start__ = ALIGN (__nrf_balloc_end__, 0x4)

.nrf_sections   0x0000000000002d04        0x0
                0x0000000000002d04                __nrf_sections_start__ = .
                0x0000000000002d04                __start_nrf_sections = __nrf_sections_start__
 *(.nrf_sections .nrf_sections.*)
                0x0000000000002d04                __nrf_sections_end__ = (__nrf_sections_start__ + SIZEOF (.nrf_sections))
                0x0000000000000000                __nrf_sections_size__ = SIZEOF (.nrf_sections)
                0x0000000000002d04                __nrf_sections_load_end__ = __nrf_sections_end__
                0x0000000000000001                . = ASSERT (((__nrf_sections_start__ == __nrf_sections_end__) || ((__nrf_sections_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .nrf_sections is too large to fit in FLASH memory segment)
                0x0000000000002d04                __log_dynamic_data_load_start__ = ALIGN (__nrf_sections_end__, 0x4)

.log_dynamic_data
                0x0000000020000000        0x0 load address 0x0000000000002d04
                0x0000000020000000                __log_dynamic_data_start__ = .
 *(SORT_BY_NAME(.log_dynamic_data*))
                0x0000000020000000                __log_dynamic_data_end__ = (__log_dynamic_data_start__ + SIZEOF (.log_dynamic_data))
                0x0000000000000000                __log_dynamic_data_size__ = SIZEOF (.log_dynamic_data)
                0x0000000000002d04                __log_dynamic_data_load_end__ = (__log_dynamic_data_load_start__ + SIZEOF (.log_dynamic_data))
                0x0000000000000001                . = ASSERT (((__log_dynamic_data_load_start__ == __log_dynamic_data_load_end__) || ((__log_dynamic_data_load_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .log_dynamic_data is too large to fit in FLASH memory segment)

.log_dynamic_data_run
                0x0000000020000000        0x0
                0x0000000020000000                __log_dynamic_data_run_start__ = .
                0x0000000020000000                __start_log_dynamic_data = __log_dynamic_data_run_start__
                0x0000000020000000                __log_dynamic_data_run_end__ = (__log_dynamic_data_run_start__ + SIZEOF (.log_dynamic_data))
                0x0000000000000000                __log_dynamic_data_run_size__ = (__log_dynamic_data_run_end__ - __log_dynamic_data_run_start__)
                0x0000000020000000                __stop_log_dynamic_data = __log_dynamic_data_run_end__
                0x0000000020000000                __log_dynamic_data_run_load_end__ = __log_dynamic_data_run_end__
                0x0000000000000001                . = ASSERT (((__log_dynamic_data_run_start__ == __log_dynamic_data_run_end__) || ((__log_dynamic_data_run_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .log_dynamic_data_run is too large to fit in RAM memory segment)
                0x0000000000002d04                __log_filter_data_load_start__ = ALIGN ((__log_dynamic_data_load_start__ + SIZEOF (.log_dynamic_data)), 0x4)

.log_filter_data
                0x0000000020000000        0x0 load address 0x0000000000002d04
                0x0000000020000000                __log_filter_data_start__ = .
 *(SORT_BY_NAME(.log_filter_data*))
                0x0000000020000000                __log_filter_data_end__ = (__log_filter_data_start__ + SIZEOF (.log_filter_data))
                0x0000000000000000                __log_filter_data_size__ = SIZEOF (.log_filter_data)
                0x0000000000002d04                __log_filter_data_load_end__ = (__log_filter_data_load_start__ + SIZEOF (.log_filter_data))
                0x0000000000000001                . = ASSERT (((__log_filter_data_load_start__ == __log_filter_data_load_end__) || ((__log_filter_data_load_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .log_filter_data is too large to fit in FLASH memory segment)

.log_filter_data_run
                0x0000000020000000        0x0
                0x0000000020000000                __log_filter_data_run_start__ = .
                0x0000000020000000                __start_log_filter_data = __log_filter_data_run_start__
                0x0000000020000000                __log_filter_data_run_end__ = (__log_filter_data_run_start__ + SIZEOF (.log_filter_data))
                0x0000000000000000                __log_filter_data_run_size__ = (__log_filter_data_run_end__ - __log_filter_data_run_start__)
                0x0000000020000000                __stop_log_filter_data = __log_filter_data_run_end__
                0x0000000020000000                __log_filter_data_run_load_end__ = __log_filter_data_run_end__
                0x0000000000000001                . = ASSERT (((__log_filter_data_run_start__ == __log_filter_data_run_end__) || ((__log_filter_data_run_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .log_filter_data_run is too large to fit in RAM memory segment)
                0x0000000020000000                __nrf_sections_run_end_load_start__ = ALIGN (__log_filter_data_run_end__, 0x4)

.nrf_sections_run_end
                0x0000000020000000        0x0
                0x0000000020000000                __nrf_sections_run_end_start__ = .
                0x0000000020000000                __end_nrf_sections_run = __nrf_sections_run_end_start__
 *(.nrf_sections_run_end .nrf_sections_run_end.*)
                0x0000000020000000                __nrf_sections_run_end_end__ = (__nrf_sections_run_end_start__ + SIZEOF (.nrf_sections_run_end))
                0x0000000000000000                __nrf_sections_run_end_size__ = SIZEOF (.nrf_sections_run_end)
                0x0000000020000000                __nrf_sections_run_end_load_end__ = __nrf_sections_run_end_end__
                0x0000000000000001                . = ASSERT (((__nrf_sections_run_end_start__ == __nrf_sections_run_end_end__) || ((__nrf_sections_run_end_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .nrf_sections_run_end is too large to fit in RAM memory segment)
                0x0000000000002d04                __dtors_load_start__ = ALIGN ((__log_filter_data_load_start__ + SIZEOF (.log_filter_data)), 0x4)

.dtors          0x0000000000002d04        0x0
                0x0000000000002d04                __dtors_start__ = .
 *(SORT_BY_NAME(.dtors.*))
 *(.dtors)
 *(.fini_array)
 *(SORT_BY_NAME(.fini_array.*))
                0x0000000000002d04                __dtors_end__ = (__dtors_start__ + SIZEOF (.dtors))
                0x0000000000000000                __dtors_size__ = SIZEOF (.dtors)
                0x0000000000002d04                __dtors_load_end__ = __dtors_end__
                0x0000000000000001                . = ASSERT (((__dtors_start__ == __dtors_end__) || ((__dtors_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .dtors is too large to fit in FLASH memory segment)
                0x0000000000002d04                __ctors_load_start__ = ALIGN (__dtors_end__, 0x4)

.ctors          0x0000000000002d04        0x0
                0x0000000000002d04                __ctors_start__ = .
 *(SORT_BY_NAME(.ctors.*))
 *(.ctors)
 *(.init_array)
 *(SORT_BY_NAME(.init_array.*))
                0x0000000000002d04                __ctors_end__ = (__ctors_start__ + SIZEOF (.ctors))
                0x0000000000000000                __ctors_size__ = SIZEOF (.ctors)
                0x0000000000002d04                __ctors_load_end__ = __ctors_end__
                0x0000000000000001                . = ASSERT (((__ctors_start__ == __ctors_end__) || ((__ctors_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .ctors is too large to fit in FLASH memory segment)
                0x0000000000002d04                __rodata_load_start__ = ALIGN (__ctors_end__, 0x4)

.rodata         0x0000000000002d04      0x41e
                0x0000000000002d04                __rodata_start__ = .
 *(.rodata .rodata.* .gnu.linkonce.r.*)
 .rodata        0x0000000000002d04       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .rodata.nrf_log_backend_uart_api
                0x0000000000002d24        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
                0x0000000000002d24                nrf_log_backend_uart_api
 .rodata.str1.1
                0x0000000000002d30       0x11 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .rodata.nrf_log_frontend_dequeue.str1.1
                0x0000000000002d41       0x11 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .rodata.str1.1
                0x0000000000002d52        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 *fill*         0x0000000000002d56        0x2 
 .rodata.m_log_push_ringbuf
                0x0000000000002d58        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .rodata.prefix_process.str1.1
                0x0000000000002d64       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .rodata.postfix_process.str1.1
                0x0000000000002d96       0x32 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
                                          0x3 (size before relaxing)
 .rodata.nrf_log_hexdump_entry_process.str1.1
                0x0000000000002d96        0xf Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
                                         0x11 (size before relaxing)
 .rodata.str1.1
                0x0000000000002da5       0x4b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
                                         0x51 (size before relaxing)
 .rodata.m_colors
                0x0000000000002df0       0x24 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .rodata.severity_names
                0x0000000000002e14       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .rodata.app_error_fault_handler.str1.1
                0x0000000000002e28       0x19 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .rodata._aV2C.0
                0x0000000000002e41       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .rodata.str1.1
                0x0000000000002e51        0x9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 *fill*         0x0000000000002e5a        0x2 
 .rodata.pwr_mgmt_data
                0x0000000000002e5c        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .rodata.str1.1
                0x0000000000002e68        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .rodata.str1.1
                0x0000000000002e6c        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .rodata.str1.1
                0x0000000000002e70        0x6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .rodata.str1.1
                0x0000000000002e76        0x6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .rodata.str1.1
                0x0000000000002e7c        0x5 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .rodata.str1.1
                0x0000000000002e81        0x6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .rodata.str1.1
                0x0000000000002e87        0x6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .rodata.str1.1
                0x0000000000002e8d        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .rodata.str1.1
                0x0000000000002e91        0x6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .rodata.saadc_callback.str1.1
                0x0000000000002e97       0x15 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
                                         0x18 (size before relaxing)
 .rodata.main.str1.1
                0x0000000000002eac       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .rodata        0x0000000000002ece        0x9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .rodata.default_config.0
                0x0000000000002ed7        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 *fill*         0x0000000000002edb        0x1 
 .rodata.m_timer
                0x0000000000002edc        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .rodata.libc.__RAL_find_locale.str1.4
                0x0000000000002ee4        0xa C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 *fill*         0x0000000000002eee        0x2 
 .rodata.libc.__RAL_ascii_ctype_map
                0x0000000000002ef0       0x80 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000002ef0                __RAL_ascii_ctype_map
 .rodata.libc.__RAL_ascii_ctype_mask
                0x0000000000002f70        0xd C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 *fill*         0x0000000000002f7d        0x3 
 .rodata.libc.__RAL_c_locale
                0x0000000000002f80        0xc C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000002f80                __RAL_c_locale
 .rodata.libc.__RAL_c_locale_abbrev_day_names
                0x0000000000002f8c       0x1d C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000002f8c                __RAL_c_locale_abbrev_day_names
 *fill*         0x0000000000002fa9        0x3 
 .rodata.libc.__RAL_c_locale_abbrev_month_names
                0x0000000000002fac       0x31 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000002fac                __RAL_c_locale_abbrev_month_names
 *fill*         0x0000000000002fdd        0x3 
 .rodata.libc.__RAL_c_locale_am_pm_indicator
                0x0000000000002fe0        0x7 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000002fe0                __RAL_c_locale_am_pm_indicator
 *fill*         0x0000000000002fe7        0x1 
 .rodata.libc.__RAL_c_locale_data
                0x0000000000002fe8       0x58 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000002fe8                __RAL_c_locale_data
 .rodata.libc.__RAL_c_locale_date_format
                0x0000000000003040        0x9 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000003040                __RAL_c_locale_date_format
 *fill*         0x0000000000003049        0x3 
 .rodata.libc.__RAL_c_locale_date_time_format
                0x000000000000304c        0xf C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x000000000000304c                __RAL_c_locale_date_time_format
 *fill*         0x000000000000305b        0x1 
 .rodata.libc.__RAL_c_locale_day_names
                0x000000000000305c       0x3a C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x000000000000305c                __RAL_c_locale_day_names
 *fill*         0x0000000000003096        0x2 
 .rodata.libc.__RAL_c_locale_month_names
                0x0000000000003098       0x57 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000003098                __RAL_c_locale_month_names
 *fill*         0x00000000000030ef        0x1 
 .rodata.libc.__RAL_c_locale_time_format
                0x00000000000030f0        0x9 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x00000000000030f0                __RAL_c_locale_time_format
 *fill*         0x00000000000030f9        0x3 
 .rodata.libc.__RAL_codeset_ascii
                0x00000000000030fc       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x00000000000030fc                __RAL_codeset_ascii
 .rodata.libc.__RAL_data_empty_string
                0x000000000000311c        0x1 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x000000000000311c                __RAL_data_empty_string
 *fill*         0x000000000000311d        0x3 
 .rodata.libc.__RAL_data_utf8_period
                0x0000000000003120        0x2 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000000003120                __RAL_data_utf8_period
                0x0000000000003122                __rodata_end__ = (__rodata_start__ + SIZEOF (.rodata))
                0x000000000000041e                __rodata_size__ = SIZEOF (.rodata)
                0x0000000000003122                __rodata_load_end__ = __rodata_end__

.rel.dyn        0x0000000000003124        0x0
 .rel.iplt      0x0000000000003124        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
                0x0000000000000001                . = ASSERT (((__rodata_start__ == __rodata_end__) || ((__rodata_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .rodata is too large to fit in FLASH memory segment)
                0x0000000000003124                __ARM.exidx_load_start__ = ALIGN (__rodata_end__, 0x4)

.ARM.exidx      0x0000000000003124        0x0
                0x0000000000003124                __ARM.exidx_start__ = .
                0x0000000000003124                __exidx_start = __ARM.exidx_start__
 *(.ARM.exidx .ARM.exidx.*)
                0x0000000000003124                __ARM.exidx_end__ = (__ARM.exidx_start__ + SIZEOF (.ARM.exidx))
                0x0000000000000000                __ARM.exidx_size__ = SIZEOF (.ARM.exidx)
                0x0000000000003124                __exidx_end = __ARM.exidx_end__
                0x0000000000003124                __ARM.exidx_load_end__ = __ARM.exidx_end__
                0x0000000000000001                . = ASSERT (((__ARM.exidx_start__ == __ARM.exidx_end__) || ((__ARM.exidx_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .ARM.exidx is too large to fit in FLASH memory segment)
                0x0000000000003124                __fast_load_start__ = ALIGN (__ARM.exidx_end__, 0x4)

.fast           0x0000000020000000        0x0 load address 0x0000000000003124
                0x0000000020000000                __fast_start__ = .
 *(.fast .fast.*)
                0x0000000020000000                __fast_end__ = (__fast_start__ + SIZEOF (.fast))
                0x0000000000000000                __fast_size__ = SIZEOF (.fast)
                0x0000000000003124                __fast_load_end__ = (__fast_load_start__ + SIZEOF (.fast))
                0x0000000000000001                . = ASSERT (((__fast_load_start__ == __fast_load_end__) || ((__fast_load_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .fast is too large to fit in FLASH memory segment)

.fast_run       0x0000000020000000        0x0
                0x0000000020000000                __fast_run_start__ = .
                0x0000000020000000                __fast_run_end__ = (__fast_run_start__ + SIZEOF (.fast))
                0x0000000000000000                __fast_run_size__ = (__fast_run_end__ - __fast_run_start__)
                0x0000000020000000                __fast_run_load_end__ = __fast_run_end__
                0x0000000000000001                . = ASSERT (((__fast_run_start__ == __fast_run_end__) || ((__fast_run_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .fast_run is too large to fit in RAM memory segment)
                0x0000000000003124                __data_load_start__ = ALIGN ((__fast_load_start__ + SIZEOF (.fast)), 0x4)

.data           0x0000000020000000       0x34 load address 0x0000000000003124
                0x0000000020000000                __data_start__ = .
 *(.data .data.* .gnu.linkonce.d.*)
 .data.m_uart   0x0000000020000000       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
                0x0000000020000000                m_uart
 .data.log_backend_cb_uart_log_backend
                0x0000000020000014        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .data.SystemCoreClock
                0x000000002000001c        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
                0x000000002000001c                SystemCoreClock
 .data.libc.__RAL_global_locale
                0x0000000020000020       0x14 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
                0x0000000020000020                __RAL_global_locale
                0x0000000020000034                __data_end__ = (__data_start__ + SIZEOF (.data))
                0x0000000000000034                __data_size__ = SIZEOF (.data)
                0x0000000000003158                __data_load_end__ = (__data_load_start__ + SIZEOF (.data))

.igot.plt       0x0000000100000000        0x0
 .igot.plt      0x0000000100000000        0x0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
                0x0000000000000001                . = ASSERT (((__data_load_start__ == __data_load_end__) || ((__data_load_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .data is too large to fit in FLASH memory segment)

.data_run       0x0000000020000000        0x0
                0x0000000020000000                __data_run_start__ = .
                0x0000000020000034                __data_run_end__ = (__data_run_start__ + SIZEOF (.data))
                0x0000000000000034                __data_run_size__ = (__data_run_end__ - __data_run_start__)
                0x0000000020000034                __data_run_load_end__ = __data_run_end__
                0x0000000000000001                . = ASSERT (((__data_run_start__ == __data_run_end__) || ((__data_run_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .data_run is too large to fit in RAM memory segment)
                0x0000000000003158                __tdata_load_start__ = ALIGN ((__data_load_start__ + SIZEOF (.data)), 0x4)

.tdata          0x0000000020000034        0x0 load address 0x0000000000003158
                0x0000000020000034                __tdata_start__ = .
 *(.tdata .tdata.*)
                0x0000000020000034                __tdata_end__ = (__tdata_start__ + SIZEOF (.tdata))
                0x0000000000000000                __tdata_size__ = SIZEOF (.tdata)
                0x0000000000003158                __tdata_load_end__ = (__tdata_load_start__ + SIZEOF (.tdata))
                0x0000000000003158                __FLASH_segment_used_end__ = (ALIGN ((__data_load_start__ + SIZEOF (.data)), 0x4) + SIZEOF (.tdata))
                0x0000000000003158                __FLASH_segment_used_size__ = (__FLASH_segment_used_end__ - __FLASH_segment_start__)
                0x0000000000000001                . = ASSERT (((__tdata_load_start__ == __tdata_load_end__) || ((__tdata_load_end__ - __FLASH_segment_start__) <= __FLASH_segment_size__)), error: .tdata is too large to fit in FLASH memory segment)

.tdata_run      0x0000000020000034        0x0
                0x0000000020000034                __tdata_run_start__ = .
                0x0000000020000034                __tdata_run_end__ = (__tdata_run_start__ + SIZEOF (.tdata))
                0x0000000000000000                __tdata_run_size__ = (__tdata_run_end__ - __tdata_run_start__)
                0x0000000020000034                __tdata_run_load_end__ = __tdata_run_end__
                0x0000000000000001                . = ASSERT (((__tdata_run_start__ == __tdata_run_end__) || ((__tdata_run_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .tdata_run is too large to fit in RAM memory segment)
                0x0000000020000034                __bss_load_start__ = ALIGN (__tdata_run_end__, 0x4)

.bss            0x0000000020000034      0x6cd
                0x0000000020000034                __bss_start__ = .
 *(.bss .bss.* .gnu.linkonce.b.*)
 .bss.m_async_mode
                0x0000000020000034        0x1 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .bss.m_string_buff
                0x0000000020000035       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .bss.m_xfer_done
                0x0000000020000075        0x1 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 *fill*         0x0000000020000076        0x2 
 .bss.log_mempool_nrf_balloc_cb
                0x0000000020000078        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .bss.log_mempool_nrf_balloc_pool_mem
                0x0000000020000080       0xc0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .bss.log_mempool_nrf_balloc_pool_stack
                0x0000000020000140        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .bss.m_log_data
                0x0000000020000148      0x424 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .bss.m_log_push_ringbuf_buf
                0x000000002000056c       0x80 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .bss.m_log_push_ringbuf_cb
                0x00000000200005ec       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .bss.m_in_critical_region
                0x0000000020000604        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .bss.m_handlers_iter
                0x0000000020000608        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .bss.m_shutdown_started
                0x0000000020000610        0x1 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 *fill*         0x0000000020000611        0x3 
 .bss.m_sysoff_mtx
                0x0000000020000614        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .bss.m_drv_state
                0x0000000020000618        0x1 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 *fill*         0x0000000020000619        0x3 
 .bss.m_contexts
                0x000000002000061c        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .bss.m_handlers
                0x0000000020000624        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .bss.nrf_drv_uart_use_easy_dma
                0x000000002000062c        0x2 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
                0x000000002000062c                nrf_drv_uart_use_easy_dma
 *fill*         0x000000002000062e        0x2 
 .bss.m_channels_allocated
                0x0000000020000630        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .bss.m_prs_box_4
                0x0000000020000634        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .bss.m_cb      0x000000002000063c       0x30 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .bss.m_cb      0x000000002000066c        0xc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .bss.m_cb      0x0000000020000678       0x2c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .bss.m_cb      0x00000000200006a4       0x24 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .bss.m_clock_cb
                0x00000000200006c8        0x8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .bss.m_handlers
                0x00000000200006d0        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .bss.m_clock_cb
                0x00000000200006d4       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .bss.m_adc_evt_counter
                0x00000000200006e8        0x4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .bss.m_buffer_pool
                0x00000000200006ec       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .bss.m_ppi_channel
                0x0000000020000700        0x1 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 *(COMMON)
                0x0000000020000701                __bss_end__ = (__bss_start__ + SIZEOF (.bss))
                0x00000000000006cd                __bss_size__ = SIZEOF (.bss)
                0x0000000020000701                __bss_load_end__ = __bss_end__
                0x0000000000000001                . = ASSERT (((__bss_start__ == __bss_end__) || ((__bss_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .bss is too large to fit in RAM memory segment)
                0x0000000020000704                __tbss_load_start__ = ALIGN (__bss_end__, 0x4)

.tbss           0x0000000020000704        0x0
                0x0000000020000704                __tbss_start__ = .
 *(.tbss .tbss.*)
                0x0000000020000704                __tbss_end__ = (__tbss_start__ + SIZEOF (.tbss))
                0x0000000000000000                __tbss_size__ = SIZEOF (.tbss)
                0x0000000020000704                __tbss_load_end__ = __tbss_end__
                0x0000000000000001                . = ASSERT (((__tbss_start__ == __tbss_end__) || ((__tbss_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .tbss is too large to fit in RAM memory segment)
                0x0000000020000704                __non_init_load_start__ = ALIGN (__tbss_end__, 0x4)

.non_init       0x0000000020000704        0x0
                0x0000000020000704                __non_init_start__ = .
 *(.non_init .non_init.*)
                0x0000000020000704                __non_init_end__ = (__non_init_start__ + SIZEOF (.non_init))
                0x0000000000000000                __non_init_size__ = SIZEOF (.non_init)
                0x0000000020000704                __non_init_load_end__ = __non_init_end__
                0x0000000000000001                . = ASSERT (((__non_init_start__ == __non_init_end__) || ((__non_init_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .non_init is too large to fit in RAM memory segment)
                0x0000000020000704                __heap_load_start__ = ALIGN (__non_init_end__, 0x4)

.heap           0x0000000020000704     0x2000
                0x0000000020000704                __heap_start__ = .
 *(.heap .heap.*)
                0x0000000020002704                . = ALIGN (MAX ((__heap_start__ + __HEAPSIZE__), .), 0x4)
 *fill*         0x0000000020000704     0x2000 
                0x0000000020002704                __heap_end__ = (__heap_start__ + SIZEOF (.heap))
                0x0000000000002000                __heap_size__ = SIZEOF (.heap)
                0x0000000020002704                __heap_load_end__ = __heap_end__
                0x0000000000000001                . = ASSERT (((__heap_start__ == __heap_end__) || ((__heap_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .heap is too large to fit in RAM memory segment)
                0x000000002003e000                __stack_load_start__ = (__RAM_segment_start__ + (__RAM_segment_size__ - 0x2000))

.stack          0x000000002003e000     0x2000
                0x000000002003e000                __stack_start__ = .
                0x000000002003e000                __StackLimit = __stack_start__
 *(.stack .stack.*)
                0x0000000020040000                . = ALIGN (MAX ((__stack_start__ + __STACKSIZE__), .), 0x8)
 *fill*         0x000000002003e000     0x2000 
                0x0000000020040000                __stack_end__ = (__stack_start__ + SIZEOF (.stack))
                0x0000000000002000                __stack_size__ = SIZEOF (.stack)
                0x0000000020040000                __StackTop = __stack_end__
                0x0000000020040000                __stack_load_end__ = __stack_end__
                0x0000000000000001                . = ASSERT (((__stack_start__ == __stack_end__) || ((__stack_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .stack is too large to fit in RAM memory segment)
                0x0000000000000001                . = ASSERT ((__heap_end__ <= __stack_start__), error: section .heap overlaps absolute placed section .stack)
                0x0000000020040000                __stack_process_load_start__ = ALIGN (__stack_end__, 0x8)

.stack_process  0x0000000020040000        0x0
                0x0000000020040000                __stack_process_start__ = .
 *(.stack_process .stack_process.*)
                0x0000000020040000                . = ALIGN (MAX ((__stack_process_start__ + __STACKSIZE_PROCESS__), .), 0x8)
                0x0000000020040000                __stack_process_end__ = (__stack_process_start__ + SIZEOF (.stack_process))
                0x0000000000000000                __stack_process_size__ = SIZEOF (.stack_process)
                0x0000000020040000                __stack_process_load_end__ = __stack_process_end__
                0x0000000020040000                __RAM_segment_used_end__ = (ALIGN (__stack_end__, 0x8) + SIZEOF (.stack_process))
                0x0000000000040000                __RAM_segment_used_size__ = (__RAM_segment_used_end__ - __RAM_segment_start__)
                0x0000000000000001                . = ASSERT (((__stack_process_start__ == __stack_process_end__) || ((__stack_process_end__ - __RAM_segment_start__) <= __RAM_segment_size__)), error: .stack_process is too large to fit in RAM memory segment)
START GROUP
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_rtt.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/boards.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_handler_gcc.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_assert.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_strerror.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_atomic.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_Syscalls_SES.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/SEGGER_RTT_printf.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
LOAD Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
LOAD C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libm_v7em_fpv4_sp_d16_hard_t_le_eabi.a
LOAD C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a
LOAD C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libdebugio_v7em_fpv4_sp_d16_hard_t_le_eabi.a
END GROUP
OUTPUT(Output/Release/Exe/SAADC_RTC_PPI_pca10056.elf elf32-littlearm)
LOAD linker stubs

.ARM.attributes
                0x0000000000000000       0x30
 .ARM.attributes
                0x0000000000000000       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .ARM.attributes
                0x0000000000000020       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .ARM.attributes
                0x0000000000000054       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .ARM.attributes
                0x0000000000000088       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .ARM.attributes
                0x00000000000000bc       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .ARM.attributes
                0x00000000000000f0       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .ARM.attributes
                0x0000000000000124       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .ARM.attributes
                0x0000000000000158       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .ARM.attributes
                0x000000000000018c       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .ARM.attributes
                0x00000000000001c0       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .ARM.attributes
                0x00000000000001f4       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .ARM.attributes
                0x0000000000000228       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .ARM.attributes
                0x000000000000025c       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .ARM.attributes
                0x0000000000000290       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .ARM.attributes
                0x00000000000002c4       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .ARM.attributes
                0x00000000000002f8       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .ARM.attributes
                0x000000000000032c       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .ARM.attributes
                0x0000000000000360       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .ARM.attributes
                0x0000000000000394       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .ARM.attributes
                0x00000000000003c8       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .ARM.attributes
                0x00000000000003fc       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .ARM.attributes
                0x0000000000000430       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .ARM.attributes
                0x0000000000000464       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .ARM.attributes
                0x0000000000000498       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .ARM.attributes
                0x00000000000004cc       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .ARM.attributes
                0x0000000000000500       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .ARM.attributes
                0x0000000000000534       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .ARM.attributes
                0x0000000000000568       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .ARM.attributes
                0x000000000000059c       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .ARM.attributes
                0x00000000000005d0       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
 .ARM.attributes
                0x00000000000005f0       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
 .ARM.attributes
                0x0000000000000610       0x34 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .ARM.attributes
                0x0000000000000644       0x34 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)
 .ARM.attributes
                0x0000000000000678       0x20 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2_asm.o)

.comment        0x0000000000000000       0x3f
 .comment       0x0000000000000000       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
                                         0x40 (size before relaxing)
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .comment       0x000000000000003f       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
 .comment       0x000000000000003f       0x40 C:/Program Files/SEGGER/SEGGER Embedded Studio for ARM 5.66/lib/libc_v7em_fpv4_sp_d16_hard_t_le_eabi.a(libc2.o)

.debug_line     0x0000000000000000    0x12dc1
 .debug_line    0x0000000000000000      0x21e Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .debug_line    0x000000000000021e      0x6d7 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_line    0x00000000000008f5      0x984 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_line    0x0000000000001279      0x5cf Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_line    0x0000000000001848     0x12da Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_line    0x0000000000002b22      0x7de Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_line    0x0000000000003300      0x3c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_line    0x00000000000036c9      0x706 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_line    0x0000000000003dcf      0x447 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_line    0x0000000000004216      0x6af Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_line    0x00000000000048c5      0x6c0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_line    0x0000000000004f85      0x3eb Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_line    0x0000000000005370      0x857 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_line    0x0000000000005bc7      0x816 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_line    0x00000000000063dd      0xba8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_line    0x0000000000006f85      0x786 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_line    0x000000000000770b      0x40d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_line    0x0000000000007b18      0x5cd Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_line    0x00000000000080e5      0x696 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_line    0x000000000000877b      0xfb5 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_line    0x0000000000009730      0x746 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_line    0x0000000000009e76     0x1781 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_line    0x000000000000b5f7      0xf13 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_line    0x000000000000c50a     0x1786 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_line    0x000000000000dc90     0x16dc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_line    0x000000000000f36c      0xbee Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_line    0x000000000000ff5a      0xe84 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_line    0x0000000000010dde      0xb52 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_line    0x0000000000011930      0xe37 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_line    0x0000000000012767       0x92 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
 .debug_line    0x00000000000127f9       0xb1 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
 .debug_line    0x00000000000128aa      0x517 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o

.debug_info     0x0000000000000000    0x1c3a6
 .debug_info    0x0000000000000000       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .debug_info    0x0000000000000022      0x77b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_info    0x000000000000079d     0x1161 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_info    0x00000000000018fe      0x2df Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_info    0x0000000000001bdd     0x2382 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_info    0x0000000000003f5f      0x7a5 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_info    0x0000000000004704      0x2b0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_info    0x00000000000049b4      0x4c1 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_info    0x0000000000004e75      0x7a7 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_info    0x000000000000561c      0x933 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_info    0x0000000000005f4f      0x3a6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_info    0x00000000000062f5      0x233 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_info    0x0000000000006528      0x72d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_info    0x0000000000006c55      0x8bb Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_info    0x0000000000007510     0x1183 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_info    0x0000000000008693      0x622 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_info    0x0000000000008cb5      0x192 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_info    0x0000000000008e47      0x114 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_info    0x0000000000008f5b     0x11c7 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_info    0x000000000000a122     0x14aa Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_info    0x000000000000b5cc      0x7c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_info    0x000000000000bd95     0x24e9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_info    0x000000000000e27e     0x1b41 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_info    0x000000000000fdbf     0x30da Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_info    0x0000000000012e99     0x3230 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_info    0x00000000000160c9     0x124c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_info    0x0000000000017315     0x19b4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_info    0x0000000000018cc9      0xcd4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_info    0x000000000001999d     0x1523 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_info    0x000000000001aec0       0x23 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
 .debug_info    0x000000000001aee3       0x23 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
 .debug_info    0x000000000001af06     0x14a0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o

.debug_abbrev   0x0000000000000000     0x537b
 .debug_abbrev  0x0000000000000000       0x12 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .debug_abbrev  0x0000000000000012      0x214 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_abbrev  0x0000000000000226      0x356 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_abbrev  0x000000000000057c      0x193 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_abbrev  0x000000000000070f      0x5e7 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_abbrev  0x0000000000000cf6      0x1f2 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_abbrev  0x0000000000000ee8      0x13e Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_abbrev  0x0000000000001026      0x207 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_abbrev  0x000000000000122d      0x22d Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_abbrev  0x000000000000145a      0x199 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_abbrev  0x00000000000015f3      0x1fc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_abbrev  0x00000000000017ef      0x146 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_abbrev  0x0000000000001935      0x2e2 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_abbrev  0x0000000000001c17      0x1ff Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_abbrev  0x0000000000001e16      0x3da Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_abbrev  0x00000000000021f0      0x15e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_abbrev  0x000000000000234e       0xbd Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_abbrev  0x000000000000240b       0xc4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_abbrev  0x00000000000024cf      0x22d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_abbrev  0x00000000000026fc      0x3a6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_abbrev  0x0000000000002aa2      0x294 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_abbrev  0x0000000000002d36      0x4cd Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_abbrev  0x0000000000003203      0x3fe Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_abbrev  0x0000000000003601      0x553 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_abbrev  0x0000000000003b54      0x4c0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_abbrev  0x0000000000004014      0x424 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_abbrev  0x0000000000004438      0x4bd Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_abbrev  0x00000000000048f5      0x446 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_abbrev  0x0000000000004d3b      0x3c4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_abbrev  0x00000000000050ff       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
 .debug_abbrev  0x0000000000005113       0x14 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
 .debug_abbrev  0x0000000000005127      0x254 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o

.debug_aranges  0x0000000000000000      0xa88
 .debug_aranges
                0x0000000000000000       0x98 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .debug_aranges
                0x0000000000000098       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_aranges
                0x00000000000000b8       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_aranges
                0x0000000000000108       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_aranges
                0x0000000000000128       0xd0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_aranges
                0x00000000000001f8       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_aranges
                0x0000000000000238       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_aranges
                0x0000000000000260       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_aranges
                0x0000000000000280       0x48 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_aranges
                0x00000000000002c8       0xb0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_aranges
                0x0000000000000378       0x30 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_aranges
                0x00000000000003a8       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_aranges
                0x00000000000003d0       0x30 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_aranges
                0x0000000000000400       0x58 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_aranges
                0x0000000000000458       0x38 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_aranges
                0x0000000000000490       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_aranges
                0x00000000000004e0       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_aranges
                0x0000000000000508       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_aranges
                0x0000000000000530       0x30 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_aranges
                0x0000000000000560       0x80 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_aranges
                0x00000000000005e0       0x30 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_aranges
                0x0000000000000610       0x88 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_aranges
                0x0000000000000698       0x90 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_aranges
                0x0000000000000728       0xa8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_aranges
                0x00000000000007d0       0x80 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_aranges
                0x0000000000000850       0x78 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_aranges
                0x00000000000008c8       0x80 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_aranges
                0x0000000000000948       0x88 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_aranges
                0x00000000000009d0       0x48 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_aranges
                0x0000000000000a18       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
 .debug_aranges
                0x0000000000000a38       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
 .debug_aranges
                0x0000000000000a58       0x30 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o

.debug_str      0x0000000000000000    0x931e8
 .debug_str     0x0000000000000000       0xc8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .debug_str     0x00000000000000c8    0x812e8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
                                      0x82883 (size before relaxing)
 .debug_str     0x00000000000813b0     0x4c78 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
                                      0x86f77 (size before relaxing)
 .debug_str     0x0000000000086028      0x136 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
                                      0x82626 (size before relaxing)
 .debug_str     0x000000000008615e     0x14a7 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
                                      0x83c1a (size before relaxing)
 .debug_str     0x0000000000087605      0x2f3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
                                      0x82933 (size before relaxing)
 .debug_str     0x00000000000878f8      0x10e Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
                                      0x741ba (size before relaxing)
 .debug_str     0x0000000000087a06       0xf3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
                                      0x82cec (size before relaxing)
 .debug_str     0x0000000000087af9      0x41f Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
                                      0x74a14 (size before relaxing)
 .debug_str     0x0000000000087f18      0x6d3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
                                      0x7ef55 (size before relaxing)
 .debug_str     0x00000000000885eb      0x159 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
                                      0x826b3 (size before relaxing)
 .debug_str     0x0000000000088744      0x11c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
                                      0x7eae6 (size before relaxing)
 .debug_str     0x0000000000088860      0x52b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
                                      0x7efe0 (size before relaxing)
 .debug_str     0x0000000000088d8b      0x1c6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
                                      0x80a2f (size before relaxing)
 .debug_str     0x0000000000088f51      0xf45 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
                                      0x87a09 (size before relaxing)
 .debug_str     0x0000000000089e96       0xf6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
                                      0x7f335 (size before relaxing)
 .debug_str     0x0000000000089f8c       0x6e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
                                      0x7ed5f (size before relaxing)
 .debug_str     0x0000000000089ffa      0x716 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
                                      0x82c3f (size before relaxing)
 .debug_str     0x000000000008a710      0x48a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
                                      0x839d8 (size before relaxing)
 .debug_str     0x000000000008ab9a      0x926 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
                                      0x85eab (size before relaxing)
 .debug_str     0x000000000008b4c0      0x33b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
                                      0x85b3d (size before relaxing)
 .debug_str     0x000000000008b7fb     0x17d2 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
                                      0x8745c (size before relaxing)
 .debug_str     0x000000000008cfcd     0x1029 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
                                      0x86c80 (size before relaxing)
 .debug_str     0x000000000008dff6      0xa01 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
                                      0x86d28 (size before relaxing)
 .debug_str     0x000000000008e9f7      0x962 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
                                      0x871bb (size before relaxing)
 .debug_str     0x000000000008f359      0x99f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
                                      0x86408 (size before relaxing)
 .debug_str     0x000000000008fcf8      0x931 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
                                      0x865f2 (size before relaxing)
 .debug_str     0x0000000000090629      0x45d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
                                      0x85d2d (size before relaxing)
 .debug_str     0x0000000000090a86     0x233c Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
                                      0x8b4ac (size before relaxing)
 .debug_str     0x0000000000092dc2       0x54 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf52840.o
                                         0xcc (size before relaxing)
 .debug_str     0x0000000000092e16       0x56 Output/Release/Obj/SAADC_RTC_PPI_pca10056/ses_startup_nrf_common.o
                                         0xce (size before relaxing)
 .debug_str     0x0000000000092e6c      0x37c Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
                                      0x73156 (size before relaxing)

.debug_ranges   0x0000000000000000     0x1fa0
 .debug_ranges  0x0000000000000000       0x90 Output/Release/Obj/SAADC_RTC_PPI_pca10056/thumb_crt0.o
 .debug_ranges  0x0000000000000090       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_ranges  0x00000000000000b8       0x88 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_ranges  0x0000000000000140       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_ranges  0x0000000000000150      0x2f8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_ranges  0x0000000000000448       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_ranges  0x0000000000000498       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_ranges  0x00000000000004b0       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_ranges  0x00000000000004d8       0x38 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_ranges  0x0000000000000510      0x208 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_ranges  0x0000000000000718       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_ranges  0x0000000000000738       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_ranges  0x0000000000000750       0x60 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_ranges  0x00000000000007b0       0x48 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_ranges  0x00000000000007f8       0xd8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_ranges  0x00000000000008d0       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_ranges  0x0000000000000910       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_ranges  0x0000000000000928       0x18 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_ranges  0x0000000000000940       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_ranges  0x0000000000000960      0x390 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_ranges  0x0000000000000cf0       0x40 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_ranges  0x0000000000000d30      0x3b0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_ranges  0x00000000000010e0      0x250 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_ranges  0x0000000000001330      0x418 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_ranges  0x0000000000001748      0x3c0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_ranges  0x0000000000001b08      0x118 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_ranges  0x0000000000001c20      0x1a8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_ranges  0x0000000000001dc8       0xf0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_ranges  0x0000000000001eb8       0xc8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_ranges  0x0000000000001f80       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o

.debug_frame    0x0000000000000000     0x1b98
 .debug_frame   0x0000000000000000       0x48 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_frame   0x0000000000000048       0xdc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_frame   0x0000000000000124       0x2c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_frame   0x0000000000000150      0x300 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_frame   0x0000000000000450      0x114 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_frame   0x0000000000000564       0x58 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_frame   0x00000000000005bc       0x30 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_frame   0x00000000000005ec       0x70 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_frame   0x000000000000065c      0x1f8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_frame   0x0000000000000854       0x78 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_frame   0x00000000000008cc       0x6c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_frame   0x0000000000000938       0xc0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_frame   0x00000000000009f8      0x114 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_frame   0x0000000000000b0c       0x78 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_frame   0x0000000000000b84       0xf4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_frame   0x0000000000000c78       0x30 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_frame   0x0000000000000ca8       0x3c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_frame   0x0000000000000ce4       0x88 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_frame   0x0000000000000d6c      0x170 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_frame   0x0000000000000edc       0x50 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_frame   0x0000000000000f2c      0x1b0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_frame   0x00000000000010dc      0x190 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_frame   0x000000000000126c      0x240 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_frame   0x00000000000014ac      0x190 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_frame   0x000000000000163c      0x134 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_frame   0x0000000000001770      0x170 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_frame   0x00000000000018e0      0x19c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_frame   0x0000000000001a7c       0xd0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_frame   0x0000000000001b4c       0x4c Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o

.debug_loc      0x0000000000000000     0xab93
 .debug_loc     0x0000000000000000      0x186 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_loc     0x0000000000000186      0x2a6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_loc     0x000000000000042c       0x31 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_loc     0x000000000000045d     0x17d4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_loc     0x0000000000001c31      0x372 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_loc     0x0000000000001fa3       0xcd Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_loc     0x0000000000002070       0x6f Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_loc     0x00000000000020df       0xda Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_loc     0x00000000000021b9      0x45f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_loc     0x0000000000002618      0x1c4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_loc     0x00000000000027dc       0x47 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_loc     0x0000000000002823      0xa67 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_loc     0x000000000000328a      0x8b3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_loc     0x0000000000003b3d      0x131 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_loc     0x0000000000003c6e      0x6b9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_loc     0x0000000000004327      0x1b6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_loc     0x00000000000044dd      0xb45 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_loc     0x0000000000005022       0xff Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_loc     0x0000000000005121      0xcba Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_loc     0x0000000000005ddb      0xb1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_loc     0x00000000000068f8     0x15ad Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_loc     0x0000000000007ea5     0x16b8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_loc     0x000000000000955d      0x2b0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_loc     0x000000000000980d      0xc77 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_loc     0x000000000000a484      0x36c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_loc     0x000000000000a7f0      0x3a3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o

.debug_pubnames
                0x0000000000000000     0x7944
 .debug_pubnames
                0x0000000000000000       0x31 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_pubnames
                0x0000000000000031      0x1e4 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_pubnames
                0x0000000000000215      0x12d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_pubnames
                0x0000000000000342      0x5b3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_pubnames
                0x00000000000008f5      0x1bd Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_pubnames
                0x0000000000000ab2       0x6c Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_pubnames
                0x0000000000000b1e      0x10e Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_pubnames
                0x0000000000000c2c      0x221 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_pubnames
                0x0000000000000e4d      0x233 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_pubnames
                0x0000000000001080      0x126 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_pubnames
                0x00000000000011a6       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_pubnames
                0x00000000000011e5       0x67 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_pubnames
                0x000000000000124c       0xb1 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_pubnames
                0x00000000000012fd      0xcc8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_pubnames
                0x0000000000001fc5       0xaa Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_pubnames
                0x000000000000206f       0x46 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_pubnames
                0x00000000000020b5       0xbc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_pubnames
                0x0000000000002171       0xcb Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_pubnames
                0x000000000000223c      0x894 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_pubnames
                0x0000000000002ad0      0x13f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_pubnames
                0x0000000000002c0f     0x10ce Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_pubnames
                0x0000000000003cdd      0x7fc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_pubnames
                0x00000000000044d9      0xaae Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_pubnames
                0x0000000000004f87      0xc5f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_pubnames
                0x0000000000005be6      0x6ee Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_pubnames
                0x00000000000062d4      0x6a0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_pubnames
                0x0000000000006974      0x4b2 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_pubnames
                0x0000000000006e26      0xa36 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_pubnames
                0x000000000000785c       0xe8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o

.debug_pubtypes
                0x0000000000000000     0x3dc0
 .debug_pubtypes
                0x0000000000000000      0x287 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_pubtypes
                0x0000000000000287      0x2f6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_pubtypes
                0x000000000000057d      0x178 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_pubtypes
                0x00000000000006f5      0x33e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_pubtypes
                0x0000000000000a33      0x181 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_pubtypes
                0x0000000000000bb4      0x117 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_pubtypes
                0x0000000000000ccb      0x13f Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_pubtypes
                0x0000000000000e0a      0x110 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_pubtypes
                0x0000000000000f1a      0x107 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_pubtypes
                0x0000000000001021      0x12a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_pubtypes
                0x000000000000114b      0x15c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_pubtypes
                0x00000000000012a7      0x175 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_pubtypes
                0x000000000000141c      0x1f3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_pubtypes
                0x000000000000160f      0x25a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_pubtypes
                0x0000000000001869      0x14c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_pubtypes
                0x00000000000019b5      0x128 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_pubtypes
                0x0000000000001add       0xf6 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_pubtypes
                0x0000000000001bd3      0x3d8 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_pubtypes
                0x0000000000001fab      0x1b9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_pubtypes
                0x0000000000002164      0x1bc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_pubtypes
                0x0000000000002320      0x420 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_pubtypes
                0x0000000000002740      0x2d7 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_pubtypes
                0x0000000000002a17      0x392 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_pubtypes
                0x0000000000002da9      0x3c7 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_pubtypes
                0x0000000000003170      0x236 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_pubtypes
                0x00000000000033a6      0x232 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_pubtypes
                0x00000000000035d8      0x216 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_pubtypes
                0x00000000000037ee      0x417 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_pubtypes
                0x0000000000003c05      0x1bb Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o

.debug_macro    0x0000000000000000     0x6336
 .debug_macro   0x0000000000000000      0x225 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000225       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000247       0x72 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x00000000000002b9       0x49 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000302       0x8c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x000000000000038e       0x31 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x00000000000003bf       0x55 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000414       0x98 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x00000000000004ac       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x00000000000004bc       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x00000000000004d9       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x00000000000004e9       0x2e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000517       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x0000000000000533      0x185 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_serial.o
 .debug_macro   0x00000000000006b8      0x304 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x00000000000009bc      0x430 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000dec       0x59 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000000e45      0x3c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x000000000000120e      0x14e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x000000000000135c       0x5a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x00000000000013b6       0x1d Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x00000000000013d3       0xac Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x000000000000147f       0x64 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x00000000000014e3       0x20 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000001503       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000001513       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000001523       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000001533       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000001543       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000001553       0x3f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_backend_uart.o
 .debug_macro   0x0000000000001592      0x221 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x00000000000017b3       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_default_backends.o
 .debug_macro   0x00000000000017c3      0x297 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000001a5a       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000001a70       0x9a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000001b0a       0x9e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_frontend.o
 .debug_macro   0x0000000000001ba8      0x274 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_log_str_formatter.o
 .debug_macro   0x0000000000001e1c      0x109 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000001f25       0x35 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000001f5a       0x78 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error.o
 .debug_macro   0x0000000000001fd2      0x233 Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_error_weak.o
 .debug_macro   0x0000000000002205      0x11f Output/Release/Obj/SAADC_RTC_PPI_pca10056/app_util_platform.o
 .debug_macro   0x0000000000002324      0x159 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x000000000000247d       0x42 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_atomic.o
 .debug_macro   0x00000000000024bf      0x207 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x00000000000026c6       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_balloc.o
 .debug_macro   0x00000000000026d6      0x15a Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000002830       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf.o
 .debug_macro   0x0000000000002852      0x1cc Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_fprintf_format.o
 .debug_macro   0x0000000000002a1e      0x1cf Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000002bed       0x2e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000002c1b       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000002c2b       0x5b Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_memobj.o
 .debug_macro   0x0000000000002c86      0x39c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000003022       0x11 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000003033       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000003043       0x45 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x0000000000003088       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x00000000000030b0      0x17f Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_pwr_mgmt.o
 .debug_macro   0x000000000000322f      0x199 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_ringbuf.o
 .debug_macro   0x00000000000033c8      0x164 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_section_iter.o
 .debug_macro   0x000000000000352c      0x226 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000003752       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x0000000000003768       0x88 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_ppi.o
 .debug_macro   0x00000000000037f0      0x24e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_uart.o
 .debug_macro   0x0000000000003a3e      0x2ac Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000003cea       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000003d06       0x37 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000003d3d       0x42 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_ppi.o
 .debug_macro   0x0000000000003d7f      0x2ae Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x000000000000402d       0x28 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_prs.o
 .debug_macro   0x0000000000004055      0x2d5 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x000000000000432a       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x000000000000433a       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_saadc.o
 .debug_macro   0x000000000000435c      0x2b9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000004615       0x22 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000004637       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_timer.o
 .debug_macro   0x0000000000004647      0x2c9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x0000000000004910       0x1c Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uart.o
 .debug_macro   0x000000000000492c      0x2e7 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_uarte.o
 .debug_macro   0x0000000000004c13      0x2c1 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000004ed4       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000004eea       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_clock.o
 .debug_macro   0x0000000000004efa      0x2b1 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x00000000000051ab       0x2e Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x00000000000051d9       0x16 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrfx_rtc.o
 .debug_macro   0x00000000000051ef      0x2e3 Output/Release/Obj/SAADC_RTC_PPI_pca10056/nrf_drv_clock.o
 .debug_macro   0x00000000000054d2      0x3e9 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x00000000000058bb      0x7d0 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x000000000000608b       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x000000000000609b       0x94 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x000000000000612f       0x94 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x00000000000061c3       0xac Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x000000000000626f       0x10 Output/Release/Obj/SAADC_RTC_PPI_pca10056/main.o
 .debug_macro   0x000000000000627f       0xb7 Output/Release/Obj/SAADC_RTC_PPI_pca10056/system_nrf52840.o
