# Create a span for the RAM to be configured as SECURE by the spm.
sram_secure:
  region: sram_primary
  span:
    - pcd_sram
sram_nonsecure:
  region: sram_primary
  span:
    - sram_primary
    - rpmsg_nrf53_sram
