#

##

##

##

    µVision Build Log
    Tool Versions:
    IDE-Version: µVision V5.12.0.0
    Copyright (C) 2014 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: John Microsoft, Microsoft, LIC=SDAUH-W2HUU-00UN9-4PAZI-SN409-GPAGJ

    Tool Versions:
    Toolchain:       MDK-ARM Standard  Version:
    Toolchain Path:  C:\Keil_v5\ARM\ARMCC\bin\
    C Compiler:      Armcc.exe V5.05 (build 41)
    Assembler:       Armasm.exe V5.05 (build 41)
    Linker/Locator:  ArmLink.exe V5.05 (build 41)
    Library Manager: ArmAr.exe V5.05 (build 41)
    Hex Converter:   FromElf.exe V5.05 (build 41)
    CPU DLL:
    Dialog DLL:
        Target DLL: Segger\JL2CM3.dll
    Dialog DLL:      TCM.DLL

    Project:
    F:\BLE Mesh Official\My Software\Experimental\Provisionee or Server node, modified based on above project\pca10056\blank\arm5_no_packs\Official BLE Mesh, built from template project of pack nRF5_SDK_13.1.0_7ca7556.uvprojx
    Project File Date:  08/17/2017

    Output:
    Load "F:\\BLE Mesh Official\\My Software\\Experimental\\Provisionee or Server node, modified based on above project\\pca10056\\blank\\arm5_no_packs\\_build\\nrf52840_xxaa.axf"
    Set JLink Project File to "F:\BLE Mesh Official\My Software\Experimental\Provisionee or Server node, modified based on above project\pca10056\blank\arm5_no_packs\JLinkSettings.ini"
    * JLink Info: Device "NRF52840_XXAA" selected.

    JLink info:
    ------------
    DLL: V6.12a, compiled Dec  2 2016 16:44:26
    Firmware: J-Link OB-SAM3U128-V2-NordicSemi compiled Nov 14 2016 16:58:29
    Hardware: V1.00
    S/N : 683925172

    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: Found SWD-DP with ID 0x2BA01477
    * JLink Info: AP-IDR: 0x24770011, Type: AHB-AP
    * JLink Info: Found Cortex-M4 r0p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: CoreSight components:
    * JLink Info: ROMTbl 0 @ E00FF000
    * JLink Info: ROMTbl 0 [0]: FFF0F000, CID: B105E00D, PID: 000BB00C SCS
    * JLink Info: ROMTbl 0 [1]: FFF02000, CID: B105E00D, PID: 003BB002 DWT
    * JLink Info: ROMTbl 0 [2]: FFF03000, CID: B105E00D, PID: 002BB003 FPB
    * JLink Info: ROMTbl 0 [3]: FFF01000, CID: B105E00D, PID: 003BB001 ITM
    * JLink Info: ROMTbl 0 [4]: FFF41000, CID: B105900D, PID: 000BB9A1 TPIU
    * JLink Info: ROMTbl 0 [5]: FFF42000, CID: B105900D, PID: 000BB925 ETM
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: nRF52840_xxAA
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 1000 kHz

    Erase Done.
    Programming Done.
    Verify OK.