<!DOCTYPE CrossStudio_Project_File>
<solution cmakelists_end_section="# NORDIC SDK APP END" cmakelists_file_name="D:/hng/projects/CyCollector/working/GPS_LTE_June20/CMakeLists.txt" cmakelists_project="GPS_LTE_June20;build;app/libapp.a" target="8" version="2" source_directory="D:/hng/projects/CyCollector/ncs/zephyr" board_directory="D:/hng/projects/CyCollector/ncs/zephyr/boards/arm/nrf9160_pca10090" board_name="nrf9160_pca10090ns" dts_compiled_file_name="D:/hng/projects/CyCollector/working/GPS_LTE_June20/build_nrf9160_pca10090ns/zephyr/nrf9160_pca10090ns.dts_compiled" build_directory="D:/hng/projects/CyCollector/working/GPS_LTE_June20/build_nrf9160_pca10090ns" dts_overlay_file_name="D:/hng/projects/CyCollector/working/GPS_LTE_June20/nrf9160_pca10090ns.overlay" load_command_environment="ZEPHYR_BASE=D:/hng/projects/CyCollector/ncs/zephyr" cmakelists_start_section="# NORDIC SDK APP START" Name="GPS_LTE_June20" load_command="&quot;cmake&quot; -GNinja -DBOARD=nrf9160_pca10090ns -DBOARD_DIR=D:/hng/projects/CyCollector/ncs/zephyr/boards/arm/nrf9160_pca10090 -DZEPHYR_TOOLCHAIN_VARIANT=gnuarmemb -DGNUARMEMB_TOOLCHAIN_PATH=&quot;C:/gnuarmemb/gcc-arm-none-eabi-7-2018-q2-update-win32&quot; -B&quot;D:/hng/projects/CyCollector/working/GPS_LTE_June20/build_nrf9160_pca10090ns&quot; -H&quot;D:/hng/projects/CyCollector/working/GPS_LTE_June20&quot; -DEXTRA_KCONFIG_TARGETS=menuconfig_ses -DEXTRA_KCONFIG_TARGET_COMMAND_FOR_menuconfig_ses=&quot;D:/hng/softs/EmbeddedStudio_ARM_Nordic_v416_win_x86/arm_segger_embedded_studio_v416_win_x86_nordic/html/configure_nordic_project_menuconfig.py&quot; &amp;&amp; $(StudioDir)/bin/ninja_import all -hide zephyr/zephyr_prebuilt.elf -show zephyr/merged.hex" dts_folder="dts files">
  <configuration properties_filter="Debug" arm_target_device_name="nRF9160" debug_target_connection="J-Link" debug_register_definition_file="$(PackagesDir)/nRF/Device/Registers/nrf9160.svd" arm_architecture="v8M_Mainline" external_link_command="&quot;$(ToolChainDir)/arm-none-eabi-gcc&quot; $(Objects) $(LinkOptions) -o &quot;$(RelTargetPath)&quot;" arm_core_type="Cortex-M33" external_assemble_command="&quot;$(ToolChainDir)/arm-none-eabi-gcc&quot; $(AsmOptions) -MD -MF &quot;$(RelDependencyPath)&quot; -o &quot;$(RelTargetPath)&quot; -c &quot;$(RelInputPath)&quot;" Name="Common" external_c_compile_command="&quot;$(ToolChainDir)/arm-none-eabi-gcc&quot; $(COptions) -MD -MF &quot;$(RelDependencyPath)&quot; -fno-diagnostics-show-caret -o &quot;$(RelTargetPath)&quot; -c &quot;$(RelInputPath)&quot;" arm_fpu_type="FPv5-SP-D16" external_archive_command="&quot;$(ToolChainDir)/arm-none-eabi-ar&quot; -rcs &quot;$(RelTargetPath)&quot; $(Objects)" linker_section_placements_segments="FLASH RX 0x00000000 0x00100000;RAM RWX 0x20000000 0x00040000" source_code_control_directory="D:/hng/projects/CyCollector/ncs/zephyr" build_toolchain_directory="C:/gnuarmemb/gcc-arm-none-eabi-7-2018-q2-update-win32/bin" debug_start_from_entry_point_symbol="No" arm_target_interface_type="SWD"/>
  <folder path="D:/hng/projects/CyCollector/working/GPS_LTE_June20" filter="nrf9160_pca10090ns.overlay" Name="dts files">
    <configuration Name="Common" c_user_include_directories="D:/hng/projects/CyCollector/ncs/zephyr/dts/common" c_system_include_directories="D:/hng/projects/CyCollector/ncs/zephyr/include;D:/hng/projects/CyCollector/ncs/zephyr/dts/arm;D:/hng/projects/CyCollector/ncs/zephyr/dts"/>
    <file file_name="D:/hng/projects/CyCollector/ncs/zephyr/boards/arm/nrf9160_pca10090/nrf9160_pca10090ns.dts"/>
    <file file_name="D:/hng/projects/CyCollector/ncs/zephyr/boards/arm/nrf9160_pca10090/nrf9160_pca10090ns.yaml"/>
    <file file_name="D:/hng/projects/CyCollector/ncs/zephyr/dts/common/common.dts"/>
    <file file_name="D:/hng/projects/CyCollector/working/GPS_LTE_June20/build_nrf9160_pca10090ns/zephyr/nrf9160_pca10090ns.dts_compiled"/>
  </folder>
  <import can_modify_solution="No" file_name="build.emProject"/>
</solution>
