#

##

##

##

##

##

##

    µVision Build Log
    Tool Versions:
    IDE-Version: µVision V5.17.0.0
    Copyright (C) 2015 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: Christian Ellingsen, Circle Consult, LIC=----

    Tool Versions:
    Toolchain:       MDK-Lite  Version: 5.17
    Toolchain Path:  C:\Keil_v5\ARM\ARMCC\Bin
    C Compiler:      Armcc.exe V5.06 update 1 (build 61)
    Assembler:       Armasm.exe V5.06 update 1 (build 61)
    Linker/Locator:  ArmLink.exe V5.06 update 1 (build 61)
    Library Manager: ArmAr.exe V5.06 update 1 (build 61)
    Hex Converter:   FromElf.exe V5.06 update 1 (build 61)
    CPU DLL:
    Dialog DLL:
    Target DLL:      Segger\JL2CM3.dll V2.99.16.0
    Dialog DLL:      TARMCM1.DLL V1.9.0.0

    Project:
    T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\ble_app_multilink_central_s120_pca10028.uvprojx
    Project File Date:  12/03/2015

    Output:
    *** Using Compiler 'V5.06 update 1 (build 61)', folder: 'C:\Keil_v5\ARM\ARMCC\Bin'
    Rebuild target 'nrf51422_xxac_s120'
    compiling acc_lis2.c...
    compiling client_handling.c...
    ..\..\..\client_handling.h(50): warning:  #1295-D: Deprecated declaration read_acc_other_device - give arg types
      uint8_t read_acc_other_device();
    ..\..\..\client_handling.h(51): warning:  #1295-D: Deprecated declaration print_client_data - give arg types
      void print_client_data();
    ..\..\..\client_handling.c(111): warning:  #177-D: variable "buffer" was declared but never referenced
      		char buffer[20];
    ..\..\..\client_handling.c(137): warning:  #177-D: variable "buffer" was declared but never referenced
      		char buffer[20];
    ..\..\..\client_handling.c(394): warning:  #177-D: variable "buffer" was declared but never referenced
      	  char buffer[10];
    ..\..\..\client_handling.c: 5 warnings, 0 errors
    compiling debug_util.c...
    compiling main.c...
    ..\..\..\client_handling.h(50): warning:  #1295-D: Deprecated declaration read_acc_other_device - give arg types
      uint8_t read_acc_other_device();
    ..\..\..\client_handling.h(51): warning:  #1295-D: Deprecated declaration print_client_data - give arg types
      void print_client_data();
    ..\..\..\main.c(361): warning:  #177-D: variable "leds" was declared but never referenced
      					  uint8_t leds[] = LEDS_LIST;
    ..\..\..\main.c(591): warning:  #177-D: variable "value" was declared but never referenced
        uint32_t value;
    ..\..\..\main.c: 4 warnings, 0 errors
    compiling simple_uart.c...
    compiling firfilter.c...
    assembling arm_startup_nrf51.s...
    compiling spi_master.c...
    compiling ble_advdata.c...
    compiling system_nrf51.c...
    compiling ble_srv_common.c...
    compiling ble_db_discovery.c...
    compiling pstorage.c...
    compiling app_uart_fifo.c...
    compiling device_manager_central.c...
    compiling nrf_drv_common.c...
    compiling nrf_delay.c...
    compiling nrf_drv_gpiote.c...
    compiling app_error.c...
    compiling nrf_drv_ppi.c...
    compiling nrf_drv_timer.c...
    compiling app_trace.c...
    compiling app_fifo.c...
    compiling nrf_assert.c...
    compiling retarget.c...
    compiling app_pwm.c...
    compiling softdevice_handler.c...
    linking...
    Program Size: Code=19052 RO-data=428 RW-data=144 ZI-data=4048
    FromELF: creating hex file...
    ".\_build\nrf51422_xxac_s120.axf" - 0 Error(s), 9 Warning(s).

    Software Packages used:

    Package Vendor: ARM
                    http://www.keil.com/pack/ARM.CMSIS.4.5.0.pack
                    ARM::CMSIS:CORE:4.3.0
                    CMSIS (Cortex Microcontroller Software Interface Standard)
       * Component: CORE Version: 4.3.0

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_BLE/NordicSemiconductor.nRF_BLE.3.0.1.pack
                    NordicSemiconductor::nRF_BLE:BLE_Modules:ble_service_common:3.0.1
                    Bluetooth Low Energy (Bluetooth Smart) services and software modules for Nordic Semiconductor nRF family.
       * Component: ble_service_common Version: 3.0.1
       * Component: ble_db_discovery Version: 3.0.1
       * Component: device_manager Variant: Central Version: 3.0.1
       * Component: ble_advdata Version: 3.0.1

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_DeviceFamilyPack/NordicSemiconductor.nRF_DeviceFamilyPack.8.2.0.pack
                    NordicSemiconductor::Device:Startup:8.2.0
                    Nordic Semiconductor nRF ARM devices Device Family Pack.
       * Component: Startup Version: 8.2.0

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_Drivers/NordicSemiconductor.nRF_Drivers.3.0.1.pack
                    NordicSemiconductor::nRF_Drivers:nrf_delay:3.0.1
                    Drivers for Nordic Semiconductor nRF family.
       * Component: nrf_delay Version: 3.0.1
       * Component: nrf_gpio Version: 3.0.1
       * Component: nrf_ppi Version: 3.0.1
       * Component: nrf_gpiote Version: 3.0.1
       * Component: nrf_error Variant: default Version: 3.0.1
       * Component: nrf_timer Version: 3.0.1
       * Component: pstorage Variant: default Version: 3.0.1
       * Component: nrf_drv_timer Version: 3.0.1
       * Component: nrf_soc Variant: default Version: 3.0.1
       * Component: nrf_drv_gpiote Version: 3.0.1
       * Component: nrf_drv_common Version: 3.0.1
       * Component: nrf_drv_ppi Version: 3.0.1
       * Component: app_uart Variant: Fifo Version: 3.0.1

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_Examples/NordicSemiconductor.nRF_Examples.9.0.0.pack
                    NordicSemiconductor::Board Support:bsp:Defines:9.0.0
                    Examples and BSP for Nordic Semiconductor nRF family.
       * Component: bsp Variant: Defines Version: 9.0.0

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_Libraries/NordicSemiconductor.nRF_Libraries.3.0.1.pack
                    NordicSemiconductor::nRF_Libraries:app_error:3.0.1
                    Software modules for Nordic Semiconductor nRF family.
       * Component: app_error Version: 3.0.1
       * Component: retarget Version: 3.0.1
       * Component: app_fifo Version: 3.0.1
       * Component: app_pwm Version: 3.0.1
       * Component: app_trace Variant: default Version: 3.0.1
       * Component: nrf_assert Version: 3.0.1
       * Component: nordic_common Version: 3.0.1
       * Component: app_util Variant: default Version: 3.0.1

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_SoftDevice_Common/NordicSemiconductor.nRF_SoftDevice_Common.1.1.4.pack
                    NordicSemiconductor::nRF_SoftDevice:Internal:sd_common:default:1.1.4
                    Common components for Nordic Semiconductor nRF family SoftDevices.
       * Component: sd_common Variant: default Version: 1.1.4
       * Component: softdevice_present Version: 1.1.4
       * Component: softdevice_hex Variant: S120 Version: 1.1.4

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_SoftDevice_S120/NordicSemiconductor.nRF_SoftDevice_S120.2.1.0.pack
                    NordicSemiconductor::nRF_SoftDevice:s120_hex:2.1.0
                    Components for Bluetooth Low Energy (Bluetooth Smart) S120 SoftDevice for Nordic Semiconductor nRF family.
       * Component: s120_hex Version: 2.1.0
       * Component: s120 Variant: default Version: 2.1.0

    Collection of Component include folders:
      T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE
      T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC
      T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC
      T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC
      C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

    Collection of Component Files used:

       * Component: ARM::CMSIS:CORE:4.3.0

       * Component: NordicSemiconductor::nRF_BLE:BLE_Modules:ble_service_common:3.0.1
          Source file:   common\ble_srv_common.c
          Include file:  common\ble_srv_common.h

       * Component: NordicSemiconductor::nRF_BLE:BLE_Modules:ble_db_discovery:3.0.1
          Source file:   ble_db_discovery\ble_db_discovery.c
          Include file:  ble_db_discovery\ble_db_discovery.h

       * Component: NordicSemiconductor::nRF_BLE:BLE_Modules:device_manager:Central:3.0.1
          Source file:   device_manager\device_manager_central.c
          Include file:  device_manager\config\device_manager_cnfg.h
          Include file:  device_manager\device_manager.h

       * Component: NordicSemiconductor::nRF_BLE:BLE_Modules:ble_advdata:3.0.1
          Source file:   common\ble_advdata.c
          Include file:  common\ble_advdata.h

       * Component: NordicSemiconductor::Device:Startup:8.2.0
          Source file:   Device\Source\arm\arm_startup_nrf51.s
          Source file:   Device\Source\system_nrf51.c
          Include file:  Device\Include\system_nrf51.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_delay:3.0.1
          Source file:   hal\nrf_delay.c
          Include file:  hal\nrf_delay.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_gpio:3.0.1
          Include file:  hal\nrf_gpio.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_ppi:3.0.1
          Include file:  hal\nrf_ppi.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_gpiote:3.0.1
          Include file:  hal\nrf_gpiote.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_error:default:3.0.1

       * Component: NordicSemiconductor::nRF_Drivers:nrf_timer:3.0.1
          Include file:  hal\nrf_timer.h

       * Component: NordicSemiconductor::nRF_Drivers:pstorage:default:3.0.1
          Source file:   pstorage\pstorage.c
          Include file:  pstorage\pstorage.h
          Include file:  pstorage\config\pstorage_platform.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_drv_timer:3.0.1
          Source file:   timer\nrf_drv_timer.c
          Include file:  timer\nrf_drv_timer.h
          Include file:  config\nrf_drv_config.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_soc:default:3.0.1

       * Component: NordicSemiconductor::nRF_Drivers:nrf_drv_gpiote:3.0.1
          Source file:   gpiote\nrf_drv_gpiote.c
          Include file:  gpiote\nrf_drv_gpiote.h
          Include file:  config\nrf_drv_config.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_drv_common:3.0.1
          Source file:   common\nrf_drv_common.c
          Include file:  common\nrf_drv_common.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_drv_ppi:3.0.1
          Source file:   ppi\nrf_drv_ppi.c
          Include file:  ppi\nrf_drv_ppi.h

       * Component: NordicSemiconductor::nRF_Drivers:app_uart:Fifo:3.0.1
          Source file:   uart\app_uart_fifo.c
          Include file:  uart\app_uart.h

       * Component: NordicSemiconductor::Board Support:bsp:Defines:9.0.0

       * Component: NordicSemiconductor::nRF_Libraries:app_error:3.0.1
          Source file:   util\app_error.c
          Include file:  util\app_error.h

       * Component: NordicSemiconductor::nRF_Libraries:retarget:3.0.1
          Source file:   uart\retarget.c

       * Component: NordicSemiconductor::nRF_Libraries:app_fifo:3.0.1
          Source file:   fifo\app_fifo.c
          Include file:  fifo\app_fifo.h

       * Component: NordicSemiconductor::nRF_Libraries:app_pwm:3.0.1
          Source file:   pwm\app_pwm.c
          Include file:  pwm\app_pwm.h

       * Component: NordicSemiconductor::nRF_Libraries:app_trace:default:3.0.1
          Source file:   trace\app_trace.c
          Include file:  trace\app_trace.h

       * Component: NordicSemiconductor::nRF_Libraries:nrf_assert:3.0.1
          Source file:   util\nrf_assert.c
          Include file:  util\nrf_assert.h

       * Component: NordicSemiconductor::nRF_Libraries:nordic_common:3.0.1

       * Component: NordicSemiconductor::nRF_Libraries:app_util:default:3.0.1

       * Component: NordicSemiconductor::nRF_SoftDevice:Internal:sd_common:default:1.1.4
          Source file:   softdevice_handler\softdevice_handler.c

       * Component: NordicSemiconductor::nRF_SoftDevice:Internal:softdevice_present:1.1.4

       * Component: NordicSemiconductor::nRF_SoftDevice:softdevice_hex:S120:1.1.4

       * Component: NordicSemiconductor::nRF_SoftDevice:s120_hex:2.1.0

       * Component: NordicSemiconductor::nRF_SoftDevice:s120:default:2.1.0
          Include file:  headers\ble.h
          Include file:  headers\ble_gatt.h
          Include file:  headers\ble_hci.h
          Include file:  headers\ble_types.h
          Include file:  headers\nrf_error_soc.h
          Include file:  headers\nrf_soc.h
          Include file:  headers\ble_err.h
          Include file:  headers\ble_gattc.h
          Include file:  headers\ble_l2cap.h
          Include file:  headers\nrf_error.h
          Include file:  headers\nrf_mbr.h
          Include file:  headers\nrf_svc.h
          Include file:  headers\ble_gap.h
          Include file:  headers\ble_gatts.h
          Include file:  headers\ble_ranges.h
          Include file:  headers\nrf_error_sdm.h
          Include file:  headers\nrf_sdm.h
          Include file:  headers\softdevice_assert.h
          Include file:  headers\nrf_sd_def.h
    Build Time Elapsed:  00:00:21