Dependencies for Project 'ble_app_multilink_central_s120_pca10028', Target 'nrf51422_xxac_s120': (DO NOT MODIFY !)
F (..\..\..\client_handling.c)(0x56655E06)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\client_handling.o --omf_browse .\_build\client_handling.crf --depend .\_build\client_handling.d)
I (..\..\..\client_handling.h)(0x565EBD9A)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_ranges.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_types.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gap.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_svc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_l2cap.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_err.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gatt.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gattc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gatts.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager\device_manager.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\sdk_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x55DB7FD8)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\nordic_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\sdk_os.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\sdk_errors.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC\device_manager_cnfg.h)(0x559EF43E)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC\ble_db_discovery.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common\ble_srv_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_deprecated.h)(0x5626150A)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\app_error.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_gpio.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\app_trace.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp\boards.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp\pca10028.h)(0x565C1A5E)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\debug_util.h)(0x5639EA20)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_delay.h)(0x559EF3D4)
F (..\..\..\main.c)(0x56655E06)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\main.o --omf_browse .\_build\main.crf --depend .\_build\main.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x55DB7FD8)
I (C:\Keil_v5\ARM\ARMCC\include\stdlib.h)(0x55DB7FD8)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\nordic_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_sdm.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_svc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error_sdm.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_ranges.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_types.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gap.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_l2cap.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_err.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gatt.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gattc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gatts.h)(0x559EF3D6)
I (..\..\..\client_handling.h)(0x565EBD9A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager\device_manager.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\sdk_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\sdk_os.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\sdk_errors.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC\device_manager_cnfg.h)(0x559EF43E)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC\ble_db_discovery.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common\ble_srv_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler\softdevice_handler.h)(0x559EF3D6)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\app_error.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler\ble_stack_handler_types.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler\ant_stack_handler_types.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp\boards.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_gpio.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp\pca10028.h)(0x565C1A5E)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC\pstorage.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC\pstorage_platform.h)(0x559EF43E)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_deprecated.h)(0x5626150A)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\app_trace.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\simple_uart.h)(0x5639EA1A)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\debug_util.h)(0x5639EA20)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\acc_lis2.h)(0x558014BD)
I (..\..\..\configuration.h)(0x564EE846)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_delay.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\app_pwm.h)(0x565F18BF)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer\nrf_drv_timer.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC\nrf_drv_config.h)(0x565EFA7C)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_timer.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x55DB7FDE)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common\nrf_drv_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi\nrf_drv_ppi.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC\nrf_ppi.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\sdk_resources.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_sd_def.h)(0x559EF3D6)
F (..\..\..\Abstract.txt)(0x559EF3E8)()
F (..\..\..\license.txt)(0x559EF3E8)()
F (.\RTE\Accelerometer\acc_lis2.c)(0x56582ED3)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\acc_lis2.o --omf_browse .\_build\acc_lis2.crf --depend .\_build\acc_lis2.d)
I (RTE\Accelerometer\nrf_delay.h)(0x556D588E)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_deprecated.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_gpio.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC\spi_master.h)(0x564F2928)
I (C:\Keil_v5\ARM\ARMCC\include\stdlib.h)(0x55DB7FD8)
I (RTE\Accelerometer\acc_lis2.h)(0x564F3177)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\nordic_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util_platform.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_svc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_error.h)(0x559EF3D4)
F (.\RTE\nRF_Libraries\nRF51422_xxAC\simple_uart.c)(0x5639EA20)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\simple_uart.o --omf_browse .\_build\simple_uart.crf --depend .\_build\simple_uart.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_deprecated.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (RTE\nRF_Libraries\nRF51422_xxAC\simple_uart.h)(0x5639EA1A)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_delay.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_gpio.h)(0x559EF3D4)
F (.\RTE\nRF_Libraries\nRF51422_xxAC\debug_util.c)(0x564DD290)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\debug_util.o --omf_browse .\_build\debug_util.crf --depend .\_build\debug_util.d)
I (RTE\nRF_Libraries\nRF51422_xxAC\debug_util.h)(0x5639EA20)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\ARMCC\include\stdarg.h)(0x55DB7FDE)
I (RTE\nRF_Libraries\nRF51422_xxAC\simple_uart.h)(0x5639EA1A)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
F (.\RTE\nRF_Libraries\nRF51422_xxAC\spi_master.c)(0x557553FF)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\spi_master.o --omf_browse .\_build\spi_master.crf --depend .\_build\spi_master.d)
I (RTE\nRF_Libraries\nRF51422_xxAC\app_error.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_gpio.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_svc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error_soc.h)(0x559EF3D6)
I (RTE\nRF_Libraries\nRF51422_xxAC\spi_master.h)(0x564DEBC5)
I (C:\Keil_v5\ARM\ARMCC\include\stdlib.h)(0x55DB7FD8)
F (.\RTE\nRF_Libraries\nRF51422_xxAC\firfilter.c)(0x556D588E)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\firfilter.o --omf_browse .\_build\firfilter.crf --depend .\_build\firfilter.d)
I (RTE\nRF_Libraries\nRF51422_xxAC\firfilter.h)(0x556D588E)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
F (..\..\..\configuration.h)(0x564EE846)()
F (RTE\Device\nRF51422_xxAC\arm_startup_nrf51.s)(0x557E91C8)(--cpu Cortex-M0 --pd "__EVAL SETA 1" -g --apcs=interwork --pd "__MICROLIB SETA 1"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

--pd "__UVISION_VERSION SETA 517" --pd "_RTE_ SETA 1" --pd "NRF51 SETA 1" --pd "__HEAP_SIZE SETA 0" --pd "BLE_STACK_SUPPORT_REQD SETA 1" --pd "S120 SETA 1" --pd "BOARD_PCA10028 SETA 1" --pd "BSP_DEFINES_ONLY SETA 1" --pd "NRF51 SETA 1" --pd "SOFTDEVICE_PRESENT SETA 1"

--list .\_build\arm_startup_nrf51.lst --xref -o .\_build\arm_startup_nrf51.o --depend .\_build\arm_startup_nrf51.d)
F (RTE\Device\nRF51422_xxAC\system_nrf51.c)(0x557E91C8)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\system_nrf51.o --omf_browse .\_build\system_nrf51.crf --depend .\_build\system_nrf51.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_deprecated.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
F (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.1.0\common\ble_srv_common.c)(0x56407686)()
F (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.1.0\device_manager\device_manager_central.c)(0x56407686)()
F (RTE\nRF_BLE\nRF51422_xxAC\ble_advdata.c)(0x559EF3D4)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\ble_advdata.o --omf_browse .\_build\ble_advdata.crf --depend .\_build\ble_advdata.d)
I (RTE\nRF_BLE\nRF51422_xxAC\ble_advdata.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x55DB7FD8)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_ranges.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_types.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gap.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_svc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_l2cap.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_err.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gatt.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gattc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gatts.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\nordic_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common\ble_srv_common.h)(0x559EF3D4)
F (RTE\nRF_BLE\nRF51422_xxAC\ble_advdata.h)(0x559EF3D4)()
F (RTE\nRF_BLE\nRF51422_xxAC\ble_db_discovery.c)(0x559EF3D4)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\ble_db_discovery.o --omf_browse .\_build\ble_db_discovery.crf --depend .\_build\ble_db_discovery.d)
I (RTE\nRF_BLE\nRF51422_xxAC\ble_db_discovery.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gattc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gatt.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_types.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_ranges.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_svc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gap.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_l2cap.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_err.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gatts.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common\ble_srv_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (C:\Keil_v5\ARM\ARMCC\include\stdlib.h)(0x55DB7FD8)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x55DB7FD8)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\app_trace.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\nordic_common.h)(0x559EF3D4)
F (RTE\nRF_BLE\nRF51422_xxAC\ble_db_discovery.h)(0x559EF3D4)()
F (RTE\nRF_BLE\nRF51422_xxAC\device_manager_cnfg.h)(0x559EF43E)()
F (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common\ble_srv_common.c)(0x559EF3D4)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\ble_srv_common.o --omf_browse .\_build\ble_srv_common.crf --depend .\_build\ble_srv_common.d)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common\ble_srv_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_types.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_ranges.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gap.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_svc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_l2cap.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_err.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gatt.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gattc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gatts.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x55DB7FD8)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\nordic_common.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\app_error.h)(0x559EF3D4)
F (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager\device_manager_central.c)(0x559EF3D4)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\device_manager_central.o --omf_browse .\_build\device_manager_central.crf --depend .\_build\device_manager_central.d)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager\device_manager.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\sdk_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x55DB7FD8)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\nordic_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\sdk_os.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\sdk_errors.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_ranges.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_types.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gap.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_svc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_l2cap.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_err.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gatt.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gattc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gatts.h)(0x559EF3D6)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC\device_manager_cnfg.h)(0x559EF43E)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\app_trace.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x55DB7FD6)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC\ble_advdata.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC\pstorage.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC\pstorage_platform.h)(0x559EF43E)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_deprecated.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_hci.h)(0x559EF3D6)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\app_error.h)(0x559EF3D4)
F (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.1.0\common\nrf_drv_common.c)(0x56407686)()
F (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.1.0\delay\nrf_delay.c)(0x56407686)()
F (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.1.0\gpiote\nrf_drv_gpiote.c)(0x56407686)()
F (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.1.0\ppi\nrf_drv_ppi.c)(0x56407686)()
F (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.1.0\timer\nrf_drv_timer.c)(0x56407686)()
F (RTE\nRF_Drivers\nRF51422_xxAC\app_uart.h)(0x559EF3D4)()
F (RTE\nRF_Drivers\nRF51422_xxAC\app_uart_fifo.c)(0x559EF3D4)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\app_uart_fifo.o --omf_browse .\_build\app_uart_fifo.crf --depend .\_build\app_uart_fifo.d)
I (RTE\nRF_Drivers\nRF51422_xxAC\app_uart.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util_platform.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_svc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_error.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\app_fifo.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdlib.h)(0x55DB7FD8)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_deprecated.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote\nrf_drv_gpiote.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_gpiote.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x55DB7FDE)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_gpio.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC\nrf_drv_config.h)(0x565EFA7C)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\sdk_errors.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\app_error.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util.h)(0x559EF3D4)
F (RTE\nRF_Drivers\nRF51422_xxAC\nrf_drv_config.h)(0x565EFA7C)()
F (RTE\nRF_Drivers\nRF51422_xxAC\nrf_ppi.h)(0x559EF3D4)()
F (RTE\nRF_Drivers\nRF51422_xxAC\pstorage.c)(0x559EF3D4)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\pstorage.o --omf_browse .\_build\pstorage.crf --depend .\_build\pstorage.d)
I (RTE\nRF_Drivers\nRF51422_xxAC\pstorage.h)(0x559EF3D4)
I (RTE\nRF_Drivers\nRF51422_xxAC\pstorage_platform.h)(0x559EF43E)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_deprecated.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (C:\Keil_v5\ARM\ARMCC\include\stdlib.h)(0x55DB7FD8)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x55DB7FD8)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\nordic_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\nrf_assert.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_svc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\app_error.h)(0x559EF3D4)
F (RTE\nRF_Drivers\nRF51422_xxAC\pstorage.h)(0x559EF3D4)()
F (RTE\nRF_Drivers\nRF51422_xxAC\pstorage_platform.h)(0x559EF43E)()
F (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common\nrf_drv_common.c)(0x559EF3D4)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\nrf_drv_common.o --omf_browse .\_build\nrf_drv_common.crf --depend .\_build\nrf_drv_common.d)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common\nrf_drv_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_deprecated.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\nrf_assert.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_svc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error_soc.h)(0x559EF3D6)
F (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote\nrf_drv_gpiote.c)(0x559EF3D4)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\nrf_drv_gpiote.o --omf_browse .\_build\nrf_drv_gpiote.crf --depend .\_build\nrf_drv_gpiote.d)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote\nrf_drv_gpiote.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_gpiote.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_deprecated.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x55DB7FDE)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_gpio.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC\nrf_drv_config.h)(0x565EFA7C)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\sdk_errors.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common\nrf_drv_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util_platform.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_svc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_error.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\nrf_assert.h)(0x559EF3D4)
F (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_delay.c)(0x559EF3D4)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\nrf_delay.o --omf_browse .\_build\nrf_delay.crf --depend .\_build\nrf_delay.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_deprecated.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_delay.h)(0x559EF3D4)
F (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi\nrf_drv_ppi.c)(0x559EF3D4)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\nrf_drv_ppi.o --omf_browse .\_build\nrf_drv_ppi.crf --depend .\_build\nrf_drv_ppi.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\ARMCC\include\stdlib.h)(0x55DB7FD8)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_deprecated.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi\nrf_drv_ppi.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\sdk_errors.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC\nrf_ppi.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x55DB7FDE)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\sdk_resources.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_sd_def.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common\nrf_drv_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util_platform.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_svc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_error.h)(0x559EF3D4)
F (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer\nrf_drv_timer.c)(0x559EF3D4)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\nrf_drv_timer.o --omf_browse .\_build\nrf_drv_timer.crf --depend .\_build\nrf_drv_timer.d)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer\nrf_drv_timer.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC\nrf_drv_config.h)(0x565EFA7C)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_timer.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x55DB7FDE)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_deprecated.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\sdk_errors.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\nrf_assert.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\nordic_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common\nrf_drv_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util_platform.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_svc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_error.h)(0x559EF3D4)
F (RTE\nRF_Libraries\nRF51422_xxAC\app_error.c)(0x559EF3D4)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\app_error.o --omf_browse .\_build\app_error.crf --depend .\_build\app_error.d)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_deprecated.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (RTE\nRF_Libraries\nRF51422_xxAC\app_error.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\nordic_common.h)(0x559EF3D4)
F (RTE\nRF_Libraries\nRF51422_xxAC\app_error.h)(0x559EF3D4)()
F (RTE\nRF_Libraries\nRF51422_xxAC\app_fifo.c)(0x559EF3D4)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\app_fifo.o --omf_browse .\_build\app_fifo.crf --depend .\_build\app_fifo.d)
I (RTE\nRF_Libraries\nRF51422_xxAC\app_fifo.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\ARMCC\include\stdlib.h)(0x55DB7FD8)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
F (RTE\nRF_Libraries\nRF51422_xxAC\app_fifo.h)(0x559EF3D4)()
F (RTE\nRF_Libraries\nRF51422_xxAC\app_pwm.c)(0x565F18C1)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\app_pwm.o --omf_browse .\_build\app_pwm.crf --depend .\_build\app_pwm.d)
I (RTE\nRF_Libraries\nRF51422_xxAC\app_pwm.h)(0x565F18BF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\sdk_errors.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer\nrf_drv_timer.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC\nrf_drv_config.h)(0x565EFA7C)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_timer.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x55DB7FDE)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_deprecated.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common\nrf_drv_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi\nrf_drv_ppi.h)(0x559EF3D4)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC\nrf_ppi.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\sdk_resources.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_sd_def.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote\nrf_drv_gpiote.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_gpiote.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal\nrf_gpio.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util_platform.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_svc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_error.h)(0x559EF3D4)
I (RTE\nRF_Libraries\nRF51422_xxAC\nrf_assert.h)(0x559EF3D4)
F (RTE\nRF_Libraries\nRF51422_xxAC\app_pwm.h)(0x565F18BF)()
F (RTE\nRF_Libraries\nRF51422_xxAC\app_trace.c)(0x559EF3D4)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\app_trace.o --omf_browse .\_build\app_trace.crf --depend .\_build\app_trace.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x55DB7FD8)
I (C:\Keil_v5\ARM\ARMCC\include\stdarg.h)(0x55DB7FDE)
F (RTE\nRF_Libraries\nRF51422_xxAC\app_trace.h)(0x559EF3D4)()
F (RTE\nRF_Libraries\nRF51422_xxAC\nrf_assert.c)(0x559EF3D4)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\nrf_assert.o --omf_browse .\_build\nrf_assert.crf --depend .\_build\nrf_assert.d)
I (RTE\nRF_Libraries\nRF51422_xxAC\nrf_assert.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
F (RTE\nRF_Libraries\nRF51422_xxAC\nrf_assert.h)(0x559EF3D4)()
F (RTE\nRF_Libraries\nRF51422_xxAC\retarget.c)(0x559EF3D4)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\retarget.o --omf_browse .\_build\retarget.crf --depend .\_build\retarget.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC\app_uart.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util_platform.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_svc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_error.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\nordic_common.h)(0x559EF3D4)
F (RTE\nRF_SoftDevice\nRF51422_xxAC\s120_nrf51822_2.0.0_licence_agreement.txt)(0x559EF3D6)()
F (RTE\nRF_SoftDevice\nRF51422_xxAC\s120_nrf51_2.1.0_readme.txt)(0x555EE306)()
F (RTE\nRF_SoftDevice\nRF51422_xxAC\s120_nrf51_2.1.0_softdevice.hex)(0x555EE306)()
F (RTE\nRF_SoftDevice\nRF51422_xxAC\s120_softdevice.hex)(0x555EF116)()
F (RTE\nRF_SoftDevice\nRF51422_xxAC\softdevice_handler.c)(0x559EF3D6)(-c --cpu Cortex-M0 -D__EVAL -D__MICROLIB -g -O3 --apcs=interwork --split_sections --c99

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_BLE\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Drivers\nRF51422_xxAC"

-I "T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC"

-I C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ppi

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\timer

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\fifo

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\pwm

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler

-I C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

-D__UVISION_VERSION="517" -D_RTE_ -DNRF51 -D__HEAP_SIZE="0" -DBLE_STACK_SUPPORT_REQD -DS120 -DBOARD_PCA10028 -DBSP_DEFINES_ONLY -DNRF51 -DSOFTDEVICE_PRESENT -DSPI_MASTER_0_ENABLE

-o .\_build\softdevice_handler.o --omf_browse .\_build\softdevice_handler.crf --depend .\_build\softdevice_handler.d)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler\softdevice_handler.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\ARMCC\include\stdlib.h)(0x55DB7FD8)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\nordic_common.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_sdm.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_svc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51.h)(0x56261506)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cm0.h)(0x56260B6C)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x55DB7FE0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmInstr.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\cmsis_armcc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include\core_cmFunc.h)(0x5625F7B0)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\system_nrf51.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x55DB7FD6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\nrf51_bitfields.h)(0x56261508)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error_soc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\nrf_error_sdm.h)(0x559EF3D6)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\app_error.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util\app_util.h)(0x559EF3D4)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.2.0\Device\Include\compiler_abstraction.h)(0x5626150A)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler\ble_stack_handler_types.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_ranges.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_types.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gap.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_l2cap.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_err.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gatt.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gattc.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers\ble_gatts.h)(0x559EF3D6)
I (C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler\ant_stack_handler_types.h)(0x559EF3D6)
I (T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\s120\arm5\RTE\nRF_Libraries\nRF51422_xxAC\nrf_assert.h)(0x559EF3D4)
