#

##

##

##

##

##

##

    µVision Build Log
    Tool Versions:
    IDE-Version: µVision V5.17.0.0
    Copyright (C) 2015 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: Christian Ellingsen, Circle Consult, LIC=----

    Tool Versions:
    Toolchain:       MDK-Lite  Version: 5.17
    Toolchain Path:  C:\Keil_v5\ARM\ARMCC\Bin
    C Compiler:      Armcc.exe V5.06 update 1 (build 61)
    Assembler:       Armasm.exe V5.06 update 1 (build 61)
    Linker/Locator:  ArmLink.exe V5.06 update 1 (build 61)
    Library Manager: ArmAr.exe V5.06 update 1 (build 61)
    Hex Converter:   FromElf.exe V5.06 update 1 (build 61)
    CPU DLL:
    Dialog DLL:
    Target DLL:      Segger\JL2CM3.dll V2.99.16.0
    Dialog DLL:      TARMCM1.DLL V1.9.0.0

    Project:
    T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\ser_s120_spi\arm5\ble_app_multilink_central_s120_spi_pca10028.uvprojx
    Project File Date:  11/19/2015

    Output:
    *** Using Compiler 'V5.06 update 1 (build 61)', folder: 'C:\Keil_v5\ARM\ARMCC\Bin'
    Rebuild target 'nrf51422_xxac_s120'
    compiling main.c...
    ..\..\..\main.c(33): error:  #5: cannot open source input file "simple_uart.h": No such file or directory
      #include "simple_uart.h"
    ..\..\..\main.c: 0 warnings, 1 error
    compiling acc_lis2.c...
    ..\..\s120\arm5\RTE\Accelerometer\acc_lis2.c(85): warning:  #223-D: function "nrf_gpio_cfg_output" declared implicitly
      	nrf_gpio_cfg_output(VCCA);
    ..\..\s120\arm5\RTE\Accelerometer\acc_lis2.c(86): warning:  #223-D: function "nrf_gpio_pin_clear" declared implicitly
      	nrf_gpio_pin_clear(VCCA);
    ..\..\s120\arm5\RTE\Accelerometer\acc_lis2.c(87): warning:  #223-D: function "nrf_gpio_cfg_input" declared implicitly
          nrf_gpio_cfg_input(AINT_PIN, NRF_GPIO_PIN_PULLDOWN);
    ..\..\s120\arm5\RTE\Accelerometer\acc_lis2.c(87): error:  #20: identifier "NRF_GPIO_PIN_PULLDOWN" is undefined
          nrf_gpio_cfg_input(
    INT_PIN, NRF_GPIO_PIN_PULLDOWN);
    ..\..\s120\arm5\RTE\Accelerometer\acc_lis2.c(105): error:  #20: identifier "NRF_APP_PRIORITY_HIGH" is undefined
              spi_instance.SPI_PriorityIRQ = NRF_APP_PRIORITY_HIGH;	//with softdevice enabled.
    ..\..\s120\arm5\RTE\Accelerometer\acc_lis2.c(124): warning:  #223-D: function "nrf_gpio_pin_set" declared implicitly
      	nrf_gpio_pin_set(VCCA);
    ..\..\s120\arm5\RTE\Accelerometer\acc_lis2.c(136): error:  #20: identifier "NRF_SUCCESS" is undefined
      	if (err_code != NRF_SUCCESS)
    ..\..\s120\arm5\RTE\Accelerometer\acc_lis2.c: 4 warnings, 3 errors
    assembling arm_startup_nrf51.s...
    compiling ble_srv_common.c...
    compiling client_handling.c...
    compiling system_nrf51.c...
    compiling ble_advdata.c...
    compiling ble_db_discovery.c...
    compiling device_manager_central.c...
    compiling nrf_drv_common.c...
    compiling nrf_delay.c...
    compiling nrf_drv_gpiote.c...
    compiling app_uart.c...
    compiling nrf_soc.c...
    compiling ble_flash.c...
    compiling pstorage_nosd.c...
    compiling spi_master.c...
    compiling app_error.c...
    compiling app_trace.c...
    compiling nrf_assert.c...
    compiling app_util_platform.c...
    compiling app_scheduler.c...
    compiling retarget.c...
    compiling app_mw_ble_gattc.c...
    compiling app_mw_ble_gap.c...
    compiling app_mw_ble.c...
    compiling app_mw_ble_gatts.c...
    compiling app_mw_ble_l2cap.c...
    compiling app_ble_gap_sec_keys.c...
    compiling ble_enable.c...
    compiling app_mw_nrf_soc.c...
    compiling app_ble_user_mem.c...
    compiling ble_event.c...
    compiling ble_evt_tx_complete.c...
    compiling ble_evt_user_mem_request.c...
    compiling ble_gap_address_get.c...
    compiling ble_gap_address_set.c...
    compiling ble_gap_adv_data_set.c...
    compiling ble_evt_user_mem_release.c...
    compiling ble_gap_adv_stop.c...
    compiling ble_gap_adv_start.c...
    compiling ble_gap_appearance_get.c...
    compiling ble_gap_appearance_set.c...
    compiling ble_gap_auth_key_reply.c...
    compiling ble_gap_authenticate.c...
    compiling ble_gap_conn_param_update.c...
    compiling ble_gap_conn_sec_get.c...
    compiling ble_gap_connect.c...
    compiling ble_gap_connect_cancel.c...
    compiling ble_gap_device_name_get.c...
    compiling ble_gap_device_name_set.c...
    compiling ble_gap_disconnect.c...
    compiling ble_gap_encrypt.c...
    compiling ble_gap_evt_adv_report.c...
    compiling ble_gap_evt_auth_key_request.c...
    compiling ble_gap_evt_conn_param_update.c...
    compiling ble_gap_evt_auth_status.c...
    compiling ble_gap_evt_conn_param_update_request.c...
    compiling ble_gap_evt_conn_sec_update.c...
    compiling ble_gap_evt_connected.c...
    compiling ble_gap_evt_disconnected.c...
    compiling ble_gap_evt_passkey_display.c...
    compiling ble_gap_evt_rssi_changed.c...
    compiling ble_gap_evt_scan_req_report.c...
    compiling ble_gap_evt_sec_info_request.c...
    compiling ble_gap_evt_sec_params_request.c...
    compiling ble_gap_evt_sec_request.c...
    compiling ble_gap_evt_timeout.c...
    compiling ble_gap_ppcp_get.c...
    compiling ble_gap_ppcp_set.c...
    compiling ble_gap_rssi_get.c...
    compiling ble_gap_rssi_start.c...
    compiling ble_gap_rssi_stop.c...
    compiling ble_gap_scan_stop.c...
    compiling ble_gap_scan_start.c...
    compiling ble_gap_sec_info_reply.c...
    compiling ble_gap_tx_power_set.c...
    compiling ble_gap_sec_params_reply.c...
    compiling ble_gattc_char_value_by_uuid_read.c...
    compiling ble_gattc_characteristics_discover.c...
    compiling ble_gattc_char_values_read.c...
    compiling ble_gattc_descriptors_discover.c...
    compiling ble_gattc_evt_char_disc_rsp.c...
    compiling ble_gattc_evt_char_val_by_uuid_read_rsp.c...
    compiling ble_gattc_evt_char_vals_read_rsp.c...
    compiling ble_gattc_evt_desc_disc_rsp.c...
    compiling ble_gattc_evt_hvx.c...
    compiling ble_gattc_evt_prim_srvc_disc_rsp.c...
    compiling ble_gattc_evt_read_rsp.c...
    compiling ble_gattc_evt_rel_disc_rsp.c...
    compiling ble_gattc_evt_timeout.c...
    compiling ble_gattc_evt_write_rsp.c...
    compiling ble_gattc_hv_confirm.c...
    compiling ble_gattc_primary_services_discover.c...
    compiling ble_gattc_read.c...
    compiling ble_gattc_relationships_discover.c...
    compiling ble_gattc_write.c...
    compiling ble_gatts_characteristic_add.c...
    compiling ble_gatts_descriptor_add.c...
    compiling ble_gatts_evt_hvc.c...
    compiling ble_gatts_evt_sc_confirm.c...
    compiling ble_gatts_evt_sys_attr_missing.c...
    compiling ble_gatts_evt_timeout.c...
    compiling ble_gatts_evt_rw_authorize_request.c...
    compiling ble_gatts_hvx.c...
    compiling ble_gatts_include_add.c...
    compiling ble_gatts_evt_write.c...
    compiling ble_gatts_rw_authorize_reply.c...
    compiling ble_gatts_service_add.c...
    compiling ble_gatts_service_changed.c...
    compiling ble_gatts_sys_attr_get.c...
    compiling ble_gatts_sys_attr_set.c...
    compiling ble_gatts_value_set.c...
    compiling ble_gatts_value_get.c...
    compiling ble_l2cap_cid_register.c...
    compiling ble_l2cap_cid_unregister.c...
    compiling ble_l2cap_evt_rx.c...
    compiling ble_l2cap_tx.c...
    compiling ble_opt_get.c...
    compiling ble_opt_set.c...
    compiling ble_tx_buffer_count_get.c...
    compiling ble_user_mem_reply.c...
    compiling ble_uuid_decode.c...
    compiling ble_uuid_encode.c...
    compiling ble_version_get.c...
    compiling ble_uuid_vs_add.c...
    compiling power_system_off.c...
    compiling app_mailbox.c...
    compiling ser_sd_transport.c...
    compiling temp_get.c...
    compiling ble_serialization.c...
    compiling cond_field_serialization.c...
    compiling ble_gattc_struct_serialization.c...
    compiling ble_gap_struct_serialization.c...
    compiling ser_softdevice_handler.c...
    compiling ble_gatts_struct_serialization.c...
    compiling ble_struct_serialization.c...
    compiling ser_hal_transport.c...
    compiling ser_app_hal_nrf51.c...
    compiling ser_phy_nrf51_spi_master.c...
    compiling ser_app_power_system_off.c...
    compiling softdevice_handler.c...
    ".\_build\nrf51422_xxac_s120.axf" - 4 Error(s), 4 Warning(s).

    Software Packages used:

    Package Vendor: ARM
                    http://www.keil.com/pack/ARM.CMSIS.4.5.0.pack
                    ARM::CMSIS:CORE:4.3.0
                    CMSIS (Cortex Microcontroller Software Interface Standard)
       * Component: CORE Version: 4.3.0

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_BLE/NordicSemiconductor.nRF_BLE.3.0.1.pack
                    NordicSemiconductor::nRF_BLE:BLE_Modules:ble_service_common:3.0.1
                    Bluetooth Low Energy (Bluetooth Smart) services and software modules for Nordic Semiconductor nRF family.
       * Component: ble_service_common Version: 3.0.1
       * Component: ble_db_discovery Version: 3.0.1
       * Component: device_manager Variant: Central Version: 3.0.1
       * Component: ble_advdata Version: 3.0.1

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_DeviceFamilyPack/NordicSemiconductor.nRF_DeviceFamilyPack.8.0.3.pack
                    NordicSemiconductor::Device:Startup:8.0.3
                    Nordic Semiconductor nRF ARM devices Device Family Pack.
       * Component: Startup Version: 8.0.3

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_Drivers/NordicSemiconductor.nRF_Drivers.3.0.1.pack
                    NordicSemiconductor::nRF_Drivers:nrf_delay:3.0.1
                    Drivers for Nordic Semiconductor nRF family.
       * Component: nrf_delay Version: 3.0.1
       * Component: nrf_gpio Version: 3.0.1
       * Component: ble_flash Version: 3.0.1
       * Component: spi_master Version: 3.0.1
       * Component: nrf_gpiote Version: 3.0.1
       * Component: nrf_error Variant: default Version: 3.0.1
       * Component: pstorage Variant: No_softdevice Version: 3.0.1
       * Component: nrf_soc Variant: Serialized Version: 3.0.1
       * Component: nrf_drv_gpiote Version: 3.0.1
       * Component: nrf_drv_common Version: 3.0.1
       * Component: app_uart Variant: default Version: 3.0.1

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_Examples/NordicSemiconductor.nRF_Examples.9.0.0.pack
                    NordicSemiconductor::Board Support:bsp:Defines:9.0.0
                    Examples and BSP for Nordic Semiconductor nRF family.
       * Component: bsp Variant: Defines Version: 9.0.0

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_Libraries/NordicSemiconductor.nRF_Libraries.3.0.1.pack
                    NordicSemiconductor::nRF_Libraries:app_error:3.0.1
                    Software modules for Nordic Semiconductor nRF family.
       * Component: app_error Version: 3.0.1
       * Component: app_scheduler Variant: default Version: 3.0.1
       * Component: retarget Version: 3.0.1
       * Component: app_trace Variant: default Version: 3.0.1
       * Component: nrf_assert Version: 3.0.1
       * Component: app_util Variant: No_softdevice Version: 3.0.1

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_Serialization/NordicSemiconductor.nRF_Serialization.2.0.1.pack
                    NordicSemiconductor::nRF_Serialization:Internal:serapp_codecs_s120_ble_gattc_evt:2.0.1
                    Serialization for Nordic Semiconductor nRF family Bluetooth Low Energy (Bluetooth Smart) SoftDevices.
       * Component: serapp_codecs_s120_ble_gattc_evt Version: 2.0.1
       * Component: ser_phy Variant: Spi_master Version: 2.0.1
       * Component: serapp_codecs_s120_ble_gap_evt Version: 2.0.1
       * Component: ser_codecs_common Version: 2.0.1
       * Component: serapp_codecs_s120_ble_gatts_evt Version: 2.0.1
       * Component: cond_field_serialization Version: 2.0.1
       * Component: serapp_codecs_s120_ble_l2cap Version: 2.0.1
       * Component: serapp_mw_s120 Version: 2.0.1
       * Component: serapp_codecs_s120_ble_l2cap_evt Version: 2.0.1
       * Component: ser_codecs_s120_ble_gattc_struct Version: 2.0.1
       * Component: ser_codecs_s120_ble_gatts_struct Version: 2.0.1
       * Component: ser_sd_transport Version: 2.0.1
       * Component: serapp_s120 Version: 2.0.1
       * Component: ser_app_hal Version: 2.0.1
       * Component: ser_codecs_s120_ble_gap_struct Version: 2.0.1
       * Component: serapp_codecs_s120_nrf_soc Version: 2.0.1
       * Component: serapp_codecs_s120_ble_gap Version: 2.0.1
       * Component: serapp_codecs_s120_ble_gattc Version: 2.0.1
       * Component: serapp_codecs_s120_ble_evt_mux Version: 2.0.1
       * Component: ser_hal_transport Version: 2.0.1
       * Component: serapp_codecs_s120_ble_gatts Version: 2.0.1
       * Component: app_mailbox Version: 2.0.1
       * Component: ser_softdevice_handler Version: 2.0.1
       * Component: serapp_codecs_s120_ble Version: 2.0.1
       * Component: serapp_hal_power_system_off Version: 2.0.1
       * Component: ser_codecs_s120_ble_struct Version: 2.0.1

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_SoftDevice_Common/NordicSemiconductor.nRF_SoftDevice_Common.1.1.4.pack
                    NordicSemiconductor::nRF_SoftDevice:Internal:sd_common:default:1.1.4
                    Common components for Nordic Semiconductor nRF family SoftDevices.
       * Component: sd_common Variant: default Version: 1.1.4

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_SoftDevice_S120/NordicSemiconductor.nRF_SoftDevice_S120.2.1.0.pack
                    NordicSemiconductor::nRF_SoftDevice:s120:Serialized:2.1.0
                    Components for Bluetooth Low Energy (Bluetooth Smart) S120 SoftDevice for Nordic Semiconductor nRF family.
       * Component: s120 Variant: Serialized Version: 2.1.0

    Collection of Component include folders:
      T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\ser_s120_spi\arm5\RTE
      T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\ser_s120_spi\arm5\RTE\nRF_BLE\nRF51422_xxAC
      T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\ser_s120_spi\arm5\RTE\nRF_Drivers\nRF51422_xxAC
      T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\ser_s120_spi\arm5\RTE\nRF_Libraries\nRF51422_xxAC
      T:\E0000 Personal folders\ce\Projects\Helm alert\example_multilink_c\ble_central\ble_app_multilink_central\pca10028\ser_s120_spi\arm5\RTE\nRF_Serialization\nRF51422_xxAC
      C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\ble_db_discovery
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\common
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.1\device_manager
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.0.3\Device\Include
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\ble_flash
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\common
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\config
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\gpiote
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\hal
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\pstorage
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\spi_master
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.1\uart
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\9.0.0\bsp
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\scheduler
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\trace
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.1\util
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Serialization\2.0.1\application\codecs\s120\serializers
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Serialization\2.0.1\application\hal
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Serialization\2.0.1\application\transport
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Serialization\2.0.1\common
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Serialization\2.0.1\common\struct_ser\s120
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Serialization\2.0.1\common\transport
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Serialization\2.0.1\common\transport\ser_phy
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Serialization\2.0.1\common\transport\ser_phy\config
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_Common\1.1.4\softdevice_handler
      C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S120\2.1.0\headers

    Collection of Component Files used:

       * Component: ARM::CMSIS:CORE:4.3.0

       * Component: NordicSemiconductor::nRF_BLE:BLE_Modules:ble_service_common:3.0.1
          Source file:   common\ble_srv_common.c
          Include file:  common\ble_srv_common.h

       * Component: NordicSemiconductor::nRF_BLE:BLE_Modules:ble_db_discovery:3.0.1
          Source file:   ble_db_discovery\ble_db_discovery.c
          Include file:  ble_db_discovery\ble_db_discovery.h

       * Component: NordicSemiconductor::nRF_BLE:BLE_Modules:device_manager:Central:3.0.1
          Source file:   device_manager\device_manager_central.c
          Include file:  device_manager\config\device_manager_cnfg.h
          Include file:  device_manager\device_manager.h

       * Component: NordicSemiconductor::nRF_BLE:BLE_Modules:ble_advdata:3.0.1
          Source file:   common\ble_advdata.c
          Include file:  common\ble_advdata.h

       * Component: NordicSemiconductor::Device:Startup:8.0.3
          Source file:   Device\Source\arm\arm_startup_nrf51.s
          Source file:   Device\Source\system_nrf51.c
          Include file:  Device\Include\system_nrf51.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_delay:3.0.1
          Source file:   hal\nrf_delay.c
          Include file:  hal\nrf_delay.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_gpio:3.0.1
          Include file:  hal\nrf_gpio.h

       * Component: NordicSemiconductor::nRF_Drivers:ble_flash:3.0.1
          Source file:   ble_flash\ble_flash.c

       * Component: NordicSemiconductor::nRF_Drivers:spi_master:3.0.1
          Source file:   spi_master\spi_master.c
          Include file:  spi_master\spi_master.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_gpiote:3.0.1
          Include file:  hal\nrf_gpiote.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_error:default:3.0.1

       * Component: NordicSemiconductor::nRF_Drivers:pstorage:No_softdevice:3.0.1
          Source file:   pstorage\pstorage_nosd.c
          Include file:  pstorage\pstorage.h
          Include file:  pstorage\config\pstorage_platform.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_soc:Serialized:3.0.1
          Source file:   nrf_soc_nosd\nrf_soc.c

       * Component: NordicSemiconductor::nRF_Drivers:nrf_drv_gpiote:3.0.1
          Source file:   gpiote\nrf_drv_gpiote.c
          Include file:  gpiote\nrf_drv_gpiote.h
          Include file:  config\nrf_drv_config.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_drv_common:3.0.1
          Source file:   common\nrf_drv_common.c
          Include file:  common\nrf_drv_common.h

       * Component: NordicSemiconductor::nRF_Drivers:app_uart:default:3.0.1
          Source file:   uart\app_uart.c
          Include file:  uart\app_uart.h

       * Component: NordicSemiconductor::Board Support:bsp:Defines:9.0.0

       * Component: NordicSemiconductor::nRF_Libraries:app_error:3.0.1
          Source file:   util\app_error.c
          Include file:  util\app_error.h

       * Component: NordicSemiconductor::nRF_Libraries:app_scheduler:default:3.0.1
          Source file:   scheduler\app_scheduler.c
          Include file:  scheduler\app_scheduler.h

       * Component: NordicSemiconductor::nRF_Libraries:retarget:3.0.1
          Source file:   uart\retarget.c

       * Component: NordicSemiconductor::nRF_Libraries:app_trace:default:3.0.1
          Source file:   trace\app_trace.c
          Include file:  trace\app_trace.h

       * Component: NordicSemiconductor::nRF_Libraries:nrf_assert:3.0.1
          Source file:   util\nrf_assert.c
          Include file:  util\nrf_assert.h

       * Component: NordicSemiconductor::nRF_Libraries:app_util:No_softdevice:3.0.1
          Source file:   util\app_util_platform.c

       * Component: NordicSemiconductor::nRF_Serialization:Internal:serapp_codecs_s120_ble_gattc_evt:2.0.1
          Source file:   application\codecs\s120\serializers\ble_gattc_evt_char_disc_rsp.c
          Source file:   application\codecs\s120\serializers\ble_gattc_evt_char_val_by_uuid_read_rsp.c
          Source file:   application\codecs\s120\serializers\ble_gattc_evt_char_vals_read_rsp.c
          Source file:   application\codecs\s120\serializers\ble_gattc_evt_desc_disc_rsp.c
          Source file:   application\codecs\s120\serializers\ble_gattc_evt_hvx.c
          Source file:   application\codecs\s120\serializers\ble_gattc_evt_prim_srvc_disc_rsp.c
          Source file:   application\codecs\s120\serializers\ble_gattc_evt_read_rsp.c
          Source file:   application\codecs\s120\serializers\ble_gattc_evt_rel_disc_rsp.c
          Source file:   application\codecs\s120\serializers\ble_gattc_evt_timeout.c
          Source file:   application\codecs\s120\serializers\ble_gattc_evt_write_rsp.c

       * Component: NordicSemiconductor::nRF_Serialization:ser_phy:Spi_master:2.0.1
          Source file:   common\transport\ser_phy\ser_phy_nrf51_spi_master.c
          Include file:  common\transport\ser_phy\ser_phy.h
          Include file:  common\transport\ser_phy\config\ser_phy_config_app_nrf51.h

       * Component: NordicSemiconductor::nRF_Serialization:Internal:serapp_codecs_s120_ble_gap_evt:2.0.1
          Source file:   application\codecs\s120\serializers\ble_gap_evt_adv_report.c
          Source file:   application\codecs\s120\serializers\ble_gap_evt_auth_key_request.c
          Source file:   application\codecs\s120\serializers\ble_gap_evt_auth_status.c
          Source file:   application\codecs\s120\serializers\ble_gap_evt_conn_param_update.c
          Source file:   application\codecs\s120\serializers\ble_gap_evt_conn_param_update_request.c
          Source file:   application\codecs\s120\serializers\ble_gap_evt_conn_sec_update.c
          Source file:   application\codecs\s120\serializers\ble_gap_evt_connected.c
          Source file:   application\codecs\s120\serializers\ble_gap_evt_disconnected.c
          Source file:   application\codecs\s120\serializers\ble_gap_evt_passkey_display.c
          Source file:   application\codecs\s120\serializers\ble_gap_evt_rssi_changed.c
          Source file:   application\codecs\s120\serializers\ble_gap_evt_sec_info_request.c
          Source file:   application\codecs\s120\serializers\ble_gap_evt_sec_params_request.c
          Source file:   application\codecs\s120\serializers\ble_gap_evt_sec_request.c
          Source file:   application\codecs\s120\serializers\ble_gap_evt_timeout.c
          Source file:   application\codecs\s120\serializers\ble_gap_evt_scan_req_report.c

       * Component: NordicSemiconductor::nRF_Serialization:Internal:ser_codecs_common:2.0.1
          Source file:   common\ble_serialization.c
          Include file:  common\ble_serialization.h

       * Component: NordicSemiconductor::nRF_Serialization:Internal:serapp_codecs_s120_ble_gatts_evt:2.0.1
          Source file:   application\codecs\s120\serializers\ble_gatts_evt_hvc.c
          Source file:   application\codecs\s120\serializers\ble_gatts_evt_rw_authorize_request.c
          Source file:   application\codecs\s120\serializers\ble_gatts_evt_sc_confirm.c
          Source file:   application\codecs\s120\serializers\ble_gatts_evt_sys_attr_missing.c
          Source file:   application\codecs\s120\serializers\ble_gatts_evt_timeout.c
          Source file:   application\codecs\s120\serializers\ble_gatts_evt_write.c

       * Component: NordicSemiconductor::nRF_Serialization:Internal:cond_field_serialization:2.0.1
          Source file:   common\cond_field_serialization.c
          Source file:   common\cond_field_serialization.c

       * Component: NordicSemiconductor::nRF_Serialization:Internal:serapp_codecs_s120_ble_l2cap:2.0.1
          Source file:   application\codecs\s120\serializers\ble_l2cap_cid_register.c
          Source file:   application\codecs\s120\serializers\ble_l2cap_cid_unregister.c
          Source file:   application\codecs\s120\serializers\ble_l2cap_tx.c
          Include file:  application\codecs\s120\serializers\ble_l2cap_app.h

       * Component: NordicSemiconductor::nRF_Serialization:Internal:serapp_mw_s120:2.0.1
          Source file:   application\codecs\s120\middleware\app_mw_nrf_soc.c
          Source file:   application\codecs\s120\middleware\app_mw_ble_l2cap.c
          Source file:   application\codecs\s120\middleware\app_mw_ble.c
          Source file:   application\codecs\s120\middleware\app_mw_ble_gap.c
          Source file:   application\codecs\s120\middleware\app_mw_ble_gattc.c
          Source file:   application\codecs\s120\middleware\app_mw_ble_gatts.c

       * Component: NordicSemiconductor::nRF_Serialization:Internal:serapp_codecs_s120_ble_l2cap_evt:2.0.1
          Source file:   application\codecs\s120\serializers\ble_l2cap_evt_rx.c

       * Component: NordicSemiconductor::nRF_Serialization:Internal:ser_codecs_s120_ble_gattc_struct:2.0.1
          Source file:   common\struct_ser\s120\ble_gattc_struct_serialization.c
          Include file:  common\struct_ser\s120\ble_gattc_struct_serialization.h

       * Component: NordicSemiconductor::nRF_Serialization:Internal:ser_codecs_s120_ble_gatts_struct:2.0.1
          Source file:   common\struct_ser\s120\ble_gatts_struct_serialization.c
          Include file:  common\struct_ser\s120\ble_gatts_struct_serialization.h

       * Component: NordicSemiconductor::nRF_Serialization:Internal:ser_sd_transport:2.0.1
          Source file:   application\transport\ser_sd_transport.c
          Include file:  application\transport\ser_sd_transport.h

       * Component: NordicSemiconductor::nRF_Serialization:Internal:serapp_s120:2.0.1

       * Component: NordicSemiconductor::nRF_Serialization:Internal:ser_app_hal:2.0.1
          Source file:   application\hal\ser_app_hal_nrf51.c
          Include file:  application\hal\ser_app_hal.h

       * Component: NordicSemiconductor::nRF_Serialization:Internal:ser_codecs_s120_ble_gap_struct:2.0.1
          Source file:   common\struct_ser\s120\ble_gap_struct_serialization.c
          Include file:  common\struct_ser\s120\ble_gap_struct_serialization.h

       * Component: NordicSemiconductor::nRF_Serialization:Internal:serapp_codecs_s120_nrf_soc:2.0.1
          Source file:   application\codecs\s120\serializers\power_system_off.c
          Source file:   application\codecs\s120\serializers\temp_get.c
          Include file:  application\codecs\s120\serializers\nrf_soc_app.h

       * Component: NordicSemiconductor::nRF_Serialization:Internal:serapp_codecs_s120_ble_gap:2.0.1
          Source file:   application\codecs\s120\serializers\ble_gap_address_get.c
          Source file:   application\codecs\s120\serializers\ble_gap_address_set.c
          Source file:   application\codecs\s120\serializers\ble_gap_adv_data_set.c
          Source file:   application\codecs\s120\serializers\ble_gap_adv_start.c
          Source file:   application\codecs\s120\serializers\ble_gap_adv_stop.c
          Source file:   application\codecs\s120\serializers\ble_gap_appearance_get.c
          Source file:   application\codecs\s120\serializers\ble_gap_appearance_set.c
          Source file:   application\codecs\s120\serializers\ble_gap_auth_key_reply.c
          Source file:   application\codecs\s120\serializers\ble_gap_authenticate.c
          Source file:   application\codecs\s120\serializers\ble_gap_conn_param_update.c
          Source file:   application\codecs\s120\serializers\ble_gap_conn_sec_get.c
          Source file:   application\codecs\s120\serializers\ble_gap_connect.c
          Source file:   application\codecs\s120\serializers\ble_gap_connect_cancel.c
          Source file:   application\codecs\s120\serializers\ble_gap_device_name_get.c
          Source file:   application\codecs\s120\serializers\ble_gap_device_name_set.c
          Source file:   application\codecs\s120\serializers\ble_gap_disconnect.c
          Source file:   application\codecs\s120\serializers\ble_gap_encrypt.c
          Source file:   application\codecs\s120\serializers\ble_gap_ppcp_get.c
          Source file:   application\codecs\s120\serializers\ble_gap_ppcp_set.c
          Source file:   application\codecs\s120\serializers\ble_gap_rssi_start.c
          Source file:   application\codecs\s120\serializers\ble_gap_rssi_stop.c
          Source file:   application\codecs\s120\serializers\ble_gap_rssi_get.c
          Source file:   application\codecs\s120\serializers\ble_gap_scan_start.c
          Source file:   application\codecs\s120\serializers\ble_gap_scan_stop.c
          Source file:   application\codecs\s120\serializers\ble_gap_sec_info_reply.c
          Source file:   application\codecs\s120\serializers\ble_gap_sec_params_reply.c
          Source file:   application\codecs\s120\serializers\ble_gap_tx_power_set.c
          Source file:   application\codecs\s120\serializers\app_ble_gap_sec_keys.c
          Include file:  application\codecs\s120\serializers\ble_gap_app.h

       * Component: NordicSemiconductor::nRF_Serialization:Internal:serapp_codecs_s120_ble_gattc:2.0.1
          Source file:   application\codecs\s120\serializers\ble_gattc_char_value_by_uuid_read.c
          Source file:   application\codecs\s120\serializers\ble_gattc_char_values_read.c
          Source file:   application\codecs\s120\serializers\ble_gattc_characteristics_discover.c
          Source file:   application\codecs\s120\serializers\ble_gattc_descriptors_discover.c
          Source file:   application\codecs\s120\serializers\ble_gattc_hv_confirm.c
          Source file:   application\codecs\s120\serializers\ble_gattc_primary_services_discover.c
          Source file:   application\codecs\s120\serializers\ble_gattc_read.c
          Source file:   application\codecs\s120\serializers\ble_gattc_relationships_discover.c
          Source file:   application\codecs\s120\serializers\ble_gattc_write.c
          Include file:  application\codecs\s120\serializers\ble_gattc_app.h

       * Component: NordicSemiconductor::nRF_Serialization:Internal:serapp_codecs_s120_ble_evt_mux:2.0.1
          Source file:   application\codecs\s120\serializers\ble_event.c
          Source file:   application\codecs\s120\serializers\ble_evt_tx_complete.c
          Source file:   application\codecs\s120\serializers\ble_evt_user_mem_release.c
          Source file:   application\codecs\s120\serializers\ble_evt_user_mem_request.c

       * Component: NordicSemiconductor::nRF_Serialization:Internal:ser_hal_transport:2.0.1
          Source file:   common\transport\ser_hal_transport.c
          Include file:  common\transport\ser_hal_transport.h

       * Component: NordicSemiconductor::nRF_Serialization:Internal:serapp_codecs_s120_ble_gatts:2.0.1
          Source file:   application\codecs\s120\serializers\ble_gatts_characteristic_add.c
          Source file:   application\codecs\s120\serializers\ble_gatts_descriptor_add.c
          Source file:   application\codecs\s120\serializers\ble_gatts_hvx.c
          Source file:   application\codecs\s120\serializers\ble_gatts_include_add.c
          Source file:   application\codecs\s120\serializers\ble_gatts_rw_authorize_reply.c
          Source file:   application\codecs\s120\serializers\ble_gatts_service_add.c
          Source file:   application\codecs\s120\serializers\ble_gatts_service_changed.c
          Source file:   application\codecs\s120\serializers\ble_gatts_sys_attr_get.c
          Source file:   application\codecs\s120\serializers\ble_gatts_sys_attr_set.c
          Source file:   application\codecs\s120\serializers\ble_gatts_value_get.c
          Source file:   application\codecs\s120\serializers\ble_gatts_value_set.c
          Include file:  application\codecs\s120\serializers\ble_gatts_app.h

       * Component: NordicSemiconductor::nRF_Serialization:Internal:app_mailbox:2.0.1
          Source file:   application\transport\app_mailbox.c
          Include file:  application\transport\app_mailbox.h

       * Component: NordicSemiconductor::nRF_Serialization:Internal:ser_softdevice_handler:2.0.1
          Source file:   application\transport\ser_softdevice_handler.c
          Include file:  application\transport\ser_softdevice_handler.h

       * Component: NordicSemiconductor::nRF_Serialization:Internal:serapp_codecs_s120_ble:2.0.1
          Source file:   application\codecs\s120\serializers\ble_opt_get.c
          Source file:   application\codecs\s120\serializers\ble_opt_set.c
          Source file:   application\codecs\s120\serializers\ble_tx_buffer_count_get.c
          Source file:   application\codecs\s120\serializers\ble_uuid_decode.c
          Source file:   application\codecs\s120\serializers\ble_uuid_encode.c
          Source file:   application\codecs\s120\serializers\ble_uuid_vs_add.c
          Source file:   application\codecs\s120\serializers\ble_version_get.c
          Source file:   application\codecs\s120\serializers\ble_enable.c
          Source file:   application\codecs\s120\serializers\ble_user_mem_reply.c
          Source file:   application\codecs\s120\serializers\app_ble_user_mem.c
          Include file:  application\codecs\s120\serializers\ble_app.h

       * Component: NordicSemiconductor::nRF_Serialization:Internal:serapp_hal_power_system_off:2.0.1
          Source file:   application\hal\ser_app_power_system_off.c
          Include file:  application\hal\ser_app_power_system_off.h

       * Component: NordicSemiconductor::nRF_Serialization:Internal:ser_codecs_s120_ble_struct:2.0.1
          Source file:   common\struct_ser\s120\ble_struct_serialization.c
          Include file:  common\struct_ser\s120\ble_struct_serialization.h

       * Component: NordicSemiconductor::nRF_SoftDevice:Internal:sd_common:default:1.1.4
          Source file:   softdevice_handler\softdevice_handler.c

       * Component: NordicSemiconductor::nRF_SoftDevice:s120:Serialized:2.1.0
          Include file:  headers\ble.h
          Include file:  headers\ble_gatt.h
          Include file:  headers\ble_hci.h
          Include file:  headers\ble_types.h
          Include file:  headers\nrf_error_soc.h
          Include file:  headers\nrf_soc.h
          Include file:  headers\ble_err.h
          Include file:  headers\ble_gattc.h
          Include file:  headers\ble_l2cap.h
          Include file:  headers\nrf_error.h
          Include file:  headers\nrf_mbr.h
          Include file:  headers\nrf_svc.h
          Include file:  headers\ble_gap.h
          Include file:  headers\ble_gatts.h
          Include file:  headers\ble_ranges.h
          Include file:  headers\nrf_error_sdm.h
          Include file:  headers\nrf_sdm.h
          Include file:  headers\softdevice_assert.h
          Include file:  headers\nrf_sd_def.h
    Target not created.
    Build Time Elapsed:  00:01:26