----- timezone:Asia/Seoul
09-29 16:20:05.411575   690   690 I terservice: [terserver] service not enabled. exit.
09-29 16:20:05.514185   696   696 I NVRAM   : MD1 set status: vendor.mtk.md1.status=init 
09-29 16:20:05.515181   696   696 I NVRAM   : MD0 set status: mtk.md0.status=init 
09-29 16:20:05.527533   696   696 I NVRAM   : MD1 set status: vendor.mtk.md1.status=reset 
09-29 16:20:05.536909   696   696 I NVRAM   : MD1 set status: mtk.md1.status=reset 
09-29 16:20:06.622732   696   696 I NVRAM   : MD1 set status: vendor.mtk.md1.status=bootup 
09-29 16:20:06.624004   696   696 I NVRAM   : MD1 set status: mtk.md1.status=bootup 
09-29 16:20:07.888787   696   696 I NVRAM   : MD1 set status: vendor.mtk.md1.status=ready 
09-29 16:20:07.890178   696   696 I NVRAM   : MD1 set status: mtk.md1.status=ready 
09-29 16:20:07.972370  1055  1055 E RILMUXD : 4081:main(): Enter
09-29 16:20:07.975744  1055  1055 I RILMUXD : 4125:main(): ccci_get_node_name=/dev/ttyC0
09-29 16:20:07.976721  1055  1055 E RILMUXD : 4361:getSimCount(): getSimCount ro.boot.opt_sim_count = 0
09-29 16:20:07.976851  1055  1055 E RILMUXD : 4365:getSimCount(): getSimCount prop = ss
09-29 16:20:07.976948  1055  1055 E RILMUXD : 4263:main(): /vendor/bin/gsm0710muxd $Rev: 1 $ starting
09-29 16:20:07.978412  1055  1055 I RILMUXD : 3378:open_serial_device(): Opened serial port,serial->fd=0
09-29 16:20:07.978481  1055  1055 I RILMUXD : 3448:open_serial_device(): Configured serial device
09-29 16:20:07.978499  1055  1055 I RILMUXD : 3713:watchdog(): Watchdog started
09-29 16:20:07.978509  1055  1055 I RILMUXD : 3520:start_muxer(): Configuring modem
09-29 16:20:07.978546  1055  1055 I RILMUXD : 2119:poll_modem_ready(): gsm0710muxd: wait for modem boot up
09-29 16:20:08.172533  1055  1055 I RILMUXD : 2138:poll_modem_ready(): Selected 1
09-29 16:20:08.172659  1055  1055 I RILMUXD : 2143:poll_modem_ready(): Read 13 bytes from serial device
09-29 16:20:08.172712  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  0d 0a 2b 45 49 4e 44 3a 20 36 34 0d 0a 
09-29 16:20:08.172736  1055  1055 I RILMUXD : 2146:poll_modem_ready(): serial device buff: 
09-29 16:20:08.172736  1055  1055 I RILMUXD : +EIND: 64
09-29 16:20:09.192776  1055  1055 I RILMUXD : 2138:poll_modem_ready(): Selected 1
09-29 16:20:09.192905  1055  1055 I RILMUXD : 2143:poll_modem_ready(): Read 14 bytes from serial device
09-29 16:20:09.192964  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  0d 0a 2b 45 49 4e 44 3a 20 31 32 38 0d 0a 
09-29 16:20:09.192990  1055  1055 I RILMUXD : 2146:poll_modem_ready(): serial device buff: 
09-29 16:20:09.192990  1055  1055 I RILMUXD : +EIND: 64
09-29 16:20:09.192990  1055  1055 I RILMUXD : 
09-29 16:20:09.192990  1055  1055 I RILMUXD : +EIND: 128
09-29 16:20:09.193003  1055  1055 I RILMUXD : 2149:poll_modem_ready(): Received +EIND: 128
09-29 16:20:09.193138  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  0d 0a 2b 45 49 4e 44 3a 20 31 32 38 0d 0a 
09-29 16:20:09.193643  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  41 
09-29 16:20:09.193743  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  54 
09-29 16:20:09.193798  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  0d 
09-29 16:20:09.194517  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  0d 0a 4f 4b 0d 0a 
09-29 16:20:09.195413  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  41 
09-29 16:20:09.195572  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  54 
09-29 16:20:09.195632  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  5a 
09-29 16:20:09.195865  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  0d 
09-29 16:20:09.196701  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  0d 0a 4f 4b 0d 0a 
09-29 16:20:09.197505  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  41 
09-29 16:20:09.197751  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  54 
09-29 16:20:09.197869  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  45 
09-29 16:20:09.197956  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  30 
09-29 16:20:09.198040  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  0d 
09-29 16:20:09.198619  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  0d 0a 4f 4b 0d 0a 
09-29 16:20:09.198838  1055  1055 I RILMUXD : 3573:start_muxer(): Starting mux mode
09-29 16:20:09.200843  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  2b 43 4d 55 58 3a 20 52 45 41 44 59 
09-29 16:20:09.201088  1055  1055 E RILMUXD : 746:syslogdumpLv(): <sw  4f 4b 
09-29 16:20:09.202485  1055  1055 I RILMUXD : 3791:watchdog(): Init control channel
09-29 16:20:09.227086  1055  1160 I RILMUXD : 2941:extract_frames(): Finish MUX Channel Setup Procedure
09-29 16:20:09.231825  1055  1055 I RILMUXD : 3824:watchdog(): ril-daemon stopped!
09-29 16:20:09.236808  1055  1055 I RILMUXD : 3828:watchdog(): ril-daemon-mtk started!
09-29 16:20:09.237011  1055  1055 I RILMUXD : 3832:watchdog(): muxd switch to user radio
09-29 16:20:09.561113  1176  1176 D RilClientQueue: construct head message
09-29 16:20:09.587003  1176  1176 I RilOpProxy: initOpLibrary, init non mipc path
09-29 16:20:09.587536  1176  1176 I RilOpProxy: [initOpLibrary] dlopen failed error: dlopen failed: library "libmtk-rilop.so" not found
09-29 16:20:09.588722  1176  1176 I RILC    : FUSION RIL getSimCount: 1
09-29 16:20:09.589053  1176  1179 I RIL-Fusion: entering mainLoop()
09-29 16:20:09.590714  1176  1176 E RILC    : RIL_register: RIL version 15
09-29 16:20:09.590802  1176  1176 I RILC    : s_registerCalled flag set, 1
09-29 16:20:09.591649  1176  1179 E RfxOpUtils: [initOpLibrary] return, sDlOpHandler = 0x0
09-29 16:20:09.592054  1176  1179 I RfxGwsdUtils: [initHandler] (null)
09-29 16:20:09.592383  1176  1179 D RatConfigC: getMaxRat: initial Lf/Lt/W/G
09-29 16:20:09.592422  1176  1179 I RfxViaUtils: [initViaHandler] not support C2K
09-29 16:20:09.592815  1176  1179 I RfxVsimUtils: VSIM is not supported.
09-29 16:20:09.593106  1176  1176 I RILC    : register service start
09-29 16:20:09.595178  1176  1180 E SchedPolicy: open of /dev/cpuctl/bg_non_interactive/tasks failed: No such file or directory
09-29 16:20:09.595876  1176  1180 D RfxVersionMgr: init
09-29 16:20:09.596364  1176  1180 I RfxChannelMgr: /dev/radio/pttyims TTY channel exists!
09-29 16:20:09.599630  1176  1176 I RILC    : radio::registerService IRadio slot1 status: 0
09-29 16:20:09.603169  1176  1176 I RILC    : radio::registerService IMtkRadioEx mtkSlot1 status: 0
09-29 16:20:09.607490  1176  1176 I RILC    : radio::registerService IRadio imsAospSlot1 status: 0
09-29 16:20:09.608251  1176  1180 E RfxChannelMgr: init urc first
09-29 16:20:09.609125  1176  1185 D RmcImsRttCtlUrcHdl: [0] RmcImsRttControlUrcHandler constructor
09-29 16:20:09.609337  1176  1176 I RILC    : radio::registerService IMtkRadioEx imsSlot1 status:0
09-29 16:20:09.609432  1176  1185 D RmcImsProvisioningUrcHandler: [0] RmcImsProvisioningUrcHandler constructor
09-29 16:20:09.609533  1176  1185 D RmcImsVideoRingtoneUrcHandler: [0] RmcImsVideoRingtoneUrcHandler constructor
09-29 16:20:09.610062  1176  1185 D RmcDcUrcHandler: [0]Notify ImsRegHandler URC registration is done
09-29 16:20:09.611644  1176  1176 I RILC    : radio::registerService se1 status: 0
09-29 16:20:09.612237  1176  1184 I AT      : [0] threadLoop. RfxReader RIL_URC_READER init, channel id = 0, fd = 9
09-29 16:20:09.613593  1176  1176 I RILC    : radio::registerService IMtkRadioEx mtkSe1 status:0
09-29 16:20:09.613719  1176  1184 I AT      : [0] AT< +EIND: 128 (RIL_URC_READER, tid:493447834880)
09-29 16:20:09.615738  1176  1176 I RILC    : radio::registerService IRadio em1 status: 0
09-29 16:20:09.617743  1176  1176 I RILC    : radio::registerService IMtkRadioEx mtkEm1 status:0
09-29 16:20:09.619237  1176  1176 I RILC    : radio::registerService IMtkRadioEx mtkAssist1 status:0
09-29 16:20:09.621167  1176  1176 I RILC    : radio::registerService IMtkRadioEx mtkRcs1 status: 0
09-29 16:20:09.621634  1176  1182 I RfxMainThread: initControllers start
09-29 16:20:09.622134  1176  1182 I RfxOpUtils: [getPreNonSlotOpCtlerList] return, sDlOpHandler == NULL
09-29 16:20:09.623806  1176  1182 D RtcSuppServQueue: Init RtcSuppServQueue's singleton instance!
09-29 16:20:09.624934  1176  1182 D RtcSuppServController: [-1] RtcSuppServController onInit!
09-29 16:20:09.625312  1176  1185 I RmcVsim : [0] RmcVsimUrcHandler init slot: 0, ch id 0
09-29 16:20:09.625383  1176  1185 I VT RIL URC: RmcVtUrcHandler constructor
09-29 16:20:09.626059  1176  1185 D RmcOemUrcHandler: [0] initRFCableStatusReader
09-29 16:20:09.627058  1176  1176 I RILC    : radio::registerService IMtkRadioEx mtkCap1 status: 0
09-29 16:20:09.628256  1176  1185 D RmcNwHdlr: [0] Default nr_display_rule=1, jp_mode_timer1_delay_timer=20, jp_mode_timer2_delay_timer=20
09-29 16:20:09.628477  1176  1185 D RmcNwHdlr: [0] prop nr_display_rule=-1, jp_mode_timer1_delay_timer=-1, jp_mode_timer2_delay_timer=-1
09-29 16:20:09.629293  1176  1176 I RILC    : radio::registerService IMtkRadioEx mtkSmartRatSwitch1 status: 0
09-29 16:20:09.629347  1176  1185 I RmcCapa : [0] constructor slot_id = 0, channel_id = 0
09-29 16:20:09.629512  1176  1185 E AT      : [0] threadLoop. Urc init done
09-29 16:20:09.629608  1176  1185 E RfxChannelMgr: urcRegisterDone
09-29 16:20:09.629659  1176  1185 E RfxChannelMgr: init other channel
09-29 16:20:09.629937  1176  1182 D RtcEccNumberController: [0] [initEmergencyNumberSource] XML file exist, init XML source
09-29 16:20:09.630097  1176  1182 D EccNumberSource: [XML][0][XmlEccNumberSource] START
09-29 16:20:09.632552  1176  1176 I RILC    : radio::registerService IMtkRadioEx mtkRsu1 status: 0
09-29 16:20:09.632587  1176  1176 I RILC    : RILHIDL called registerService
09-29 16:20:09.632608  1176  1176 I RilOpProxy: [registerOpService] dlopen failed error: (null)
09-29 16:20:09.632620  1176  1176 I RILC    : RILOP HIDL called registerOpService
09-29 16:20:09.634345  1176  1176 D RadioConfig_service: radioConfig::registerService status: 0
09-29 16:20:09.634373  1176  1176 I RILC    : radioConfig called register radio config Service
09-29 16:20:09.634485  1176  1176 I RILC    : RIL_register_socket: calling registerService
09-29 16:20:09.634509  1176  1176 D RIL_SAP : registerService: starting ISap slot1 for slotId 0
09-29 16:20:09.635984  1176  1190 I RmcOemUrcHandler: [0] rfCableStatusReaderLoop - RFCable status working thread
09-29 16:20:09.636536  1176  1190 I RmcOemUrcHandler: [0] [RmcOemUrcHandler] rfCableStatusReaderLoop: fd = 34
09-29 16:20:09.636619  1176  1176 D RIL_SAP : registerService: started ISap slot1 status 0
09-29 16:20:09.636781  1176  1191 I AT      : [0] threadLoop. RfxReader RIL_CMD_READER_1 init, channel id = 1, fd = 13
09-29 16:20:09.637480  1176  1192 I AT      : [0] AT> AT+EMDVER? (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.638125  1176  1193 I AT      : [0] threadLoop. RfxReader RIL_CMD_READER_2 init, channel id = 2, fd = 14
09-29 16:20:09.638706  1176  1194 D RmcImsVideoRingToneReqHdl: [0] RmcImsVideoRingtoneRequestHandler constructor
09-29 16:20:09.639107  1176  1194 I VT RIL CMN RMC: [RMC VT REQ HDLR] RmcVtCommonReqHandler create (slot_id = 0)
09-29 16:20:09.639341  1176  1194 I AT      : [0] AT> AT+ECFGSET="disable_cs_call","0" (RIL_CMD_READER_2 tid:493437472000)
09-29 16:20:09.639751  1176  1195 I AT      : [0] threadLoop. RfxReader RIL_CMD_READER_3 init, channel id = 3, fd = 15
09-29 16:20:09.640532  1176  1196 D RmcImsRttCtlReqHdl: [0] RmcImsRttControlRequestHandler constructor
09-29 16:20:09.640957  1176  1196 D RmcImsProvisioningRequestHandler: [0] RmcImsProvisioningRequestHandler constructor
09-29 16:20:09.641244  1176  1196 I AT      : [0] AT> AT+CIREG=2 (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:09.641624  1176  1197 I AT      : [0] threadLoop. RfxReader RIL_CMD_READER_4 init, channel id = 4, fd = 16
09-29 16:20:09.642334  1176  1198 D RmcDcMsimReqHandler: Single SIM project, send EDALLOW=1 at boot time
09-29 16:20:09.642737  1176  1198 I AT      : [0] AT> AT+EDALLOW=1 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:09.643141  1176  1199 I AT      : [0] threadLoop. RfxReader RIL_ATCI_READER init, channel id = 5, fd = 17
09-29 16:20:09.644101  1176  1200 D RmcSSHandler: [0] startUtInterface(): libutinterface_md.so
09-29 16:20:09.644237  1176  1191 I AT      : [0] AT< +EMDVER: "LWCTG one MD","1" (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.644293  1176  1191 I AT      : [0] AT< +EMDVER: "DSS_NO_RESET","1" (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.644311  1176  1191 I AT      : [0] AT< +EMDVER: "REG_REPORT_MODE","5" (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.644326  1176  1191 I AT      : [0] AT< +EMDVER: "IMS_TEST_MODE","1" (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.644341  1176  1191 I AT      : [0] AT< +EMDVER: "ESIMIND_IMPI_SUPPORT","1" (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.644355  1176  1191 I AT      : [0] AT< +EMDVER: "SWITCH_OFF_SIM","1" (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.644369  1176  1191 I AT      : [0] AT< +EMDVER: "ECFGRESET Supported","1" (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.644384  1176  1191 I AT      : [0] AT< +EMDVER: "STK_USSD_OVER_IMS","1" (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.644398  1176  1191 I AT      : [0] AT< +EMDVER: "STK_CALL_OVER_IMS","1" (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.644413  1176  1191 I AT      : [0] AT< +EMDVER: "MD_MSM","0" (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.644428  1176  1191 I AT      : [0] AT< +EMDVER: "SAT_ADDITIONAL_LOCK","0" (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.644442  1176  1191 I AT      : [0] AT< +EMDVER: "SIM_SWITCH_DURING_SIMLOCK","1" (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.644456  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.644851  1176  1193 I AT      : [0] AT< ERROR (RIL_CMD_READER_2, tid:493438508288)
09-29 16:20:09.645818  1176  1201 I AT      : [0] threadLoop. RfxReader RIL_CMD_RT_7 init, channel id = 6, fd = 18
09-29 16:20:09.645848  1176  1184 I AT      : [0] AT< +CIREGU: 0 (RIL_URC_READER, tid:493447834880)
09-29 16:20:09.648093  1176  1203 I AT      : [0] threadLoop. RfxReader RIL_CMD_NRT_8 init, channel id = 7, fd = 19
09-29 16:20:09.648849  1176  1194 D RfxVersionMgr: waitLooper() begin
09-29 16:20:09.648917  1176  1194 D RfxVersionMgr: waitLooper() end
09-29 16:20:09.648950  1176  1194 D RmcCCReqHandler: [0] queryEmciSupport, EMCI=0
09-29 16:20:09.649110  1176  1204 I AT      : [0] AT> AT+COPS=3,3 (RIL_CMD_NRT_8 tid:493337836800)
09-29 16:20:09.649331  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:09.649531  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:09.649596  1176  1182 D EccNumberSource: [XML][0][XmlEccNumberSource] END
09-29 16:20:09.649804  1176  1198 D RmcDcMsimReqHandler: [updateDataAllowStatus] SIM[0]: 0 , allowed = 0
09-29 16:20:09.649840  1176  1198 D RmcDcMsimReqHandler: [0] isMdSelfEdallow = 0
09-29 16:20:09.650458  1176  1205 I AT      : [0] threadLoop. RfxReader RIL_CMD_RADIO_9 init, channel id = 8, fd = 20
09-29 16:20:09.651344  1176  1192 I AT      : [0] AT> AT+EINFO=1074 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.651381  1176  1206 I AT      : [0] AT> AT+ES3G? (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:09.652088  1176  1207 I AT      : [0] threadLoop. RfxReader RIL_CMD_DATA2_10 init, channel id = 9, fd = 22
09-29 16:20:09.653257  1176  1211 I AT      : [0] threadLoop. RfxReader RIL_CMD_IMS init, channel id = 11, fd = 24
09-29 16:20:09.653380  1176  1203 I AT      : [0] AT< OK (RIL_CMD_NRT_8, tid:493338873088)
09-29 16:20:09.653749  1176  1196 I AT      : [0] AT> AT+EMULTIIMS? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:09.653886  1176  1182 D EccNumberPreference: [0][update] for PLMN:  GSM only: , GSM prefer: , CDMA prefer: 
09-29 16:20:09.654733  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.655097  1176  1192 I AT      : [0] AT> AT+EINFO=1082,401,0 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.655872  1176  1209 I AT      : [0] threadLoop. RfxReader RIL_CMD_SIM2_11 init, channel id = 10, fd = 23
09-29 16:20:09.655901  1176  1205 I AT      : [0] AT< +ES3G: 1 (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:09.656650  1176  1212 I VT RIL RMC: [RMC VT REQ HDLR] RmcVtReqHandler create (slot_id = 0)
09-29 16:20:09.656648  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:09.657104  1176  1206 I RmcRadioReq: [0] slot_id = 0, main_sim = 1, 1, 1
09-29 16:20:09.657726  1176  1210 D RmcVsim : [0] RmmVsimHandler construct,slot:0, channel:10(10), support:0
09-29 16:20:09.661004  1176  1206 I AT      : [0] AT> ATE0Q0V1 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:09.661167  1176  1185 D RmcDcUrcHandler: [0]Notify ImsRegHandler URC registration is done
09-29 16:20:09.661365  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.661395  1176  1208 D RmcDcImsDc2ReqHandler: [0][onRegisterUrcDone], send AT+EIMSPDN= "onoff", 1
09-29 16:20:09.661445  1176  1208 I AT      : [0] AT> AT+EIMSPDN= "onoff", 1 (RIL_CMD_DATA2_10 tid:493333691648)
09-29 16:20:09.661762  1176  1194 I AT      : [0] AT> AT+EGMC=1,"stk_call_over_ims",1 (RIL_CMD_READER_2 tid:493437472000)
09-29 16:20:09.662090  1176  1192 I AT      : [0] AT> AT+CGSN (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.663025  1176  1198 I AT      : [0] AT> AT+EEPDG=1 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:09.663749  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:09.664145  1176  1182 D RpOemCtlr: [0] init()
09-29 16:20:09.664283  1176  1182 D RtcCC   : [0] create ecc controller
09-29 16:20:09.664324  1176  1182 D RtcEcc  : [0] onInit !! (bsp)
09-29 16:20:09.664378  1176  1182 D RtcRedialController: [0] onInit !!
09-29 16:20:09.664418  1176  1182 D RtcCC   : [0] createRedialController set ecc controller
09-29 16:20:09.664846  1176  1182 D RtcImsVideoRingtoneHandler: RtcImsVideoRingtoneHandler()
09-29 16:20:09.664988  1176  1206 I AT      : [0] AT> AT+CMEE=1 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:09.665048  1176  1182 D RtcMwi  : [0] [onInit]
09-29 16:20:09.665041  1176  1184 I AT      : [0] AT< +EIMSPDN: "init" (RIL_URC_READER, tid:493447834880)
09-29 16:20:09.665105  1176  1207 I AT      : [0] AT< OK (RIL_CMD_DATA2_10, tid:493334727936)
09-29 16:20:09.665586  1176  1213 I VT RIL THD: [VT RIL THD] Start
09-29 16:20:09.665651  1176  1208 I RmcDcImsDc2ReqHandler: [0][handleImsBearerNotify] urc=+EIMSPDN: "init"
09-29 16:20:09.665663  1176  1213 I VT RIL THD: [VT RIL THD] socket fd: 31
09-29 16:20:09.665680  1176  1208 D RmcDcImsDc2ReqHandler: [0][handleImsBearerNotify] IMS notification phone=0 bearer initial...
09-29 16:20:09.665682  1176  1213 I VT RIL THD: [VT RIL THD] start readerLooper
09-29 16:20:09.666137  1176  1212 I RCS RIL RMC: RmcRcsReqHandler create (slot_id = 0)
09-29 16:20:09.666168  1176  1214 I VT RIL THD: [RIL IMCB THD] Start
09-29 16:20:09.666167  1176  1193 I AT      : [0] AT< +EGMC: "stk_call_over_ims",1 (RIL_CMD_READER_2, tid:493438508288)
09-29 16:20:09.666214  1176  1212 I RCS RIL RMC: isImsSubmarineSupport, IMS SUBMARINE = 0
09-29 16:20:09.666661  1176  1193 I AT      : [0] AT< OK (RIL_CMD_READER_2, tid:493438508288)
09-29 16:20:09.666799  1176  1194 I AT      : [0] AT> AT+EGMC=1,"ecc_redial_notify",1 (RIL_CMD_READER_2 tid:493437472000)
09-29 16:20:09.668137  1176  1191 I AT      : [0] AT< *** (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.668185  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:09.668392  1176  1198 I AT      : [0] AT> AT+EIWLPLEN =1 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:09.668898  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.669098  1176  1192 I AT      : [0] AT> AT+EGMR=*** (RIL_CMD_READER_1, tid:493439544576)
09-29 16:20:09.669660  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:09.669828  1176  1206 I AT      : [0] AT> AT+CMER=1,0,0,2,0 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:09.670878  1176  1193 I AT      : [0] AT< +EGMC: "ecc_redial_notify",1 (RIL_CMD_READER_2, tid:493438508288)
09-29 16:20:09.671282  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:09.671411  1176  1198 D RmcDcMiscImpl: [syncIwlanOperationModeToMd] enable IWLAN Priority List update
09-29 16:20:09.671595  1176  1193 I AT      : [0] AT< OK (RIL_CMD_READER_2, tid:493438508288)
09-29 16:20:09.671742  1176  1198 D Atch    : client connected, type = 6, fd = 51, fp = 0xb4000074a74eb4b8
09-29 16:20:09.671791  1176  1194 I AT      : [0] AT> AT+CMOD=0 (RIL_CMD_READER_2 tid:493437472000)
09-29 16:20:09.671843  1176  1198 D Atch    : client connected, type = 6, fd = 54, fp = 0xb4000074a74eb550
09-29 16:20:09.673123  1176  1198 I NetAgentService: [registerCbKernelAddressUpdated] action=0xb4000073a7501c50, slotId=0, simCount=1
09-29 16:20:09.673238  1176  1198 I AT      : [0] AT> AT+CGDCONT=? (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:09.674213  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:09.674414  1176  1206 I AT      : [0] AT> AT+ICCID=1 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:09.675125  1176  1191 I AT      : [0] AT< +EGMR: "01" (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.675412  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.675553  1176  1193 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_2, tid:493438508288)
09-29 16:20:09.675592  1176  1192 I AT      : [0] AT> AT+EPCT? (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.675748  1176  1194 I AT      : [0] AT> ATS0=0 (RIL_CMD_READER_2 tid:493437472000)
09-29 16:20:09.678721  1176  1197 I AT      : [0] AT< +CGDCONT:=*** (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:09.678810  1176  1197 I AT      : [0] AT< +CGDCONT:=*** (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:09.678832  1176  1197 I AT      : [0] AT< +CGDCONT:=*** (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:09.678853  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:09.678968  1176  1198 E RmcDcPdnManager: [0][getModemSupportPdnNumber] the MD support pdn range:(0-10)
09-29 16:20:09.678994  1176  1198 E RmcDcPdnManager: [0][getModemSupportPdnNumber] the 1's token is 0
09-29 16:20:09.679005  1176  1198 E RmcDcPdnManager: [0][getModemSupportPdnNumber] the 2's token is 10
09-29 16:20:09.679014  1176  1198 E RmcDcPdnManager: [0][getModemSupportPdnNumber] the MD support pdn range:(0-10)
09-29 16:20:09.679022  1176  1198 E RmcDcPdnManager: [0][getModemSupportPdnNumber] the 1's token is 0
09-29 16:20:09.679030  1176  1198 E RmcDcPdnManager: [0][getModemSupportPdnNumber] the 2's token is 10
09-29 16:20:09.679038  1176  1198 E RmcDcPdnManager: [0][getModemSupportPdnNumber] the MD support pdn range:(0-10)
09-29 16:20:09.679046  1176  1198 E RmcDcPdnManager: [0][getModemSupportPdnNumber] the 1's token is 0
09-29 16:20:09.679054  1176  1198 E RmcDcPdnManager: [0][getModemSupportPdnNumber] the 2's token is 10
09-29 16:20:09.679160  1176  1198 I AT      : [0] AT> AT+EIAREG=1 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:09.680001  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:09.680276  1176  1206 I AT      : [0] AT> AT+ESIMS=1 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:09.681127  1176  1191 I AT      : [0] AT< +EPCT: 0,0 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.681245  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.682262  1176  1192 I AT      : [0] AT> AT+EGMR=*** (RIL_CMD_READER_1, tid:493439544576)
09-29 16:20:09.682276  1176  1193 I AT      : [0] AT< OK (RIL_CMD_READER_2, tid:493438508288)
09-29 16:20:09.682419  1176  1194 I AT      : [0] AT> AT+CCWA=1 (RIL_CMD_READER_2 tid:493437472000)
09-29 16:20:09.683446  1176  1215 E Atapi   : Can't execute the at command, ret = 8, cmd = (AT+ENAPTRCONFIG=1)
09-29 16:20:09.683519  1176  1215 E NetAgent_IO: ret = 1
09-29 16:20:09.683536  1176  1215 E NetAgentService: [setNAPTRCapabilityToModem] fail
09-29 16:20:09.684602  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:09.684765  1176  1198 I AT      : [0] AT> AT+ECCAUSE=1 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:09.687912  1176  1193 I AT      : [0] AT< OK (RIL_CMD_READER_2, tid:493438508288)
09-29 16:20:09.687913  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:09.688028  1176  1191 I AT      : [0] AT< +EGMR: "XQ660_GH6601_MODEM" (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.688053  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.688072  1176  1194 I AT      : [0] AT> AT+CMUT=0 (RIL_CMD_READER_2 tid:493437472000)
09-29 16:20:09.688173  1176  1192 I AT      : [0] AT> AT+EGMR=*** (RIL_CMD_READER_1, tid:493439544576)
09-29 16:20:09.688179  1176  1206 I AT      : [0] AT> AT+ECFGSET="disable_sms", "0" (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:09.689284  1176  1215 E Atapi   : Can't execute the at command, ret = 8, cmd = (AT+EIPSPI?)
09-29 16:20:09.689313  1176  1215 E NetAgent_IO: ret = 1
09-29 16:20:09.689328  1176  1215 E NetAgentService: [setSpiQueryToModem] fail
09-29 16:20:09.690587  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:09.690782  1176  1198 I AT      : [0] AT> AT+EOSID=1,"97a498e3fc925c9489860333d06e4e47" (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:09.692244  1176  1191 I AT      : [0] AT< +EGMR: "LWCTG_8768A" (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.692333  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.692432  1176  1192 E RmcOemHandler: proj: XQ660_GH6601_MODEM, flavor: LWCTG_8768A
09-29 16:20:09.693179  1176  1192 I AT      : [0] AT> AT+EGMR=*** (RIL_CMD_READER_1, tid:493439544576)
09-29 16:20:09.693675  1176  1205 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:09.693712  1176  1193 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_2, tid:493438508288)
09-29 16:20:09.693843  1176  1194 I AT      : [0] AT> AT+ECPI=4294967295 (RIL_CMD_READER_2 tid:493437472000)
09-29 16:20:09.693943  1176  1206 I AT      : [0] AT> AT+ESBP=5,"SBP_ETWS_FOR_AOSP_DESIGN",1 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:09.695505  1176  1197 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:09.697475  1176  1200 D RmcSSHandler: [0] call fnstartUtInterface
09-29 16:20:09.697492  1176  1193 I AT      : [0] AT< OK (RIL_CMD_READER_2, tid:493438508288)
09-29 16:20:09.697689  1176  1194 I AT      : [0] AT> AT+EAIC=2 (RIL_CMD_READER_2 tid:493437472000)
09-29 16:20:09.698048  1176  1200 I UtInterface: startUtInterface (IMS Repo)
09-29 16:20:09.698355  1176  1200 D UtConfig: OsVersion: ro.vendor.md_prop_ver=1
09-29 16:20:09.698387  1176  1200 D UtConfig: custom_init
09-29 16:20:09.701193  1176  1182 I RtcEmbmsAt: [0] onInit:mSdkVersion:11001
09-29 16:20:09.701404  1176  1182 D RTC_EMBMS_CON_PROXY: [0] onInit to TK-AT: ctrl = 0xb4000074174e7190.
09-29 16:20:09.709925  1176  1182 D RtcAtciController: [-1] [onInit] enter
09-29 16:20:09.710137  1176  1182 D VT RIL RTC: [0] [RTC VT REQ HDLR] onInit
09-29 16:20:09.710202  1176  1182 D VT RIL RTC: [0] [updateOpId] m_slot_id: 0, operatorId: 0
09-29 16:20:09.710356  1176  1182 D VT RIL RTC: [0] [RTC VT REQ HDLR] send RFX_MSG_EVENT_VT_ENABLE_ANBR, enable
09-29 16:20:09.710392  1176  1182 D RtcPhbSimIo: [0] [onInit]
09-29 16:20:09.710426  1176  1182 D RtcPhbInModem: [0] [onInit]
09-29 16:20:09.710488  1176  1182 D RtcImsRtt: [0] onInit()
09-29 16:20:09.710567  1176  1182 D RtcGwsdCtrl: [0][onInit] enter
09-29 16:20:09.710606  1176  1182 D RtcWr   : [0] [onInit]
09-29 16:20:09.710642  1176  1182 D RtcVsim : [-1] RtcVsimController construct,slot:-1
09-29 16:20:09.710782  1176  1182 I RtcCapa : [-1] constructor entered
09-29 16:20:09.710832  1176  1182 I RtcCapa : constructor entered
09-29 16:20:09.710879  1176  1182 I RtcCapa : [-1] constructor entered
09-29 16:20:09.711297  1176  1200 I ServiceController: ~ServiceController: Constructor
09-29 16:20:09.711536  1176  1200 D UtInterface: startUtInterface exit
09-29 16:20:09.711586  1176  1200 D RmcSSHandler: [0] Check data only project, CONFIG_SS_MODE = 1
09-29 16:20:09.711614  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:09.711630  1176  1200 I AT      : [0] AT> AT+ECFGSET="disable_cs_ss","0" (RIL_ATCI_READER tid:493431254272)
09-29 16:20:09.711757  1176  1212 I VT RIL RMC: [Handle REQ] request = 59522
09-29 16:20:09.711772  1176  1212 I VT RIL RMC: set mSimOpIdTable[0] = 0
09-29 16:20:09.712028  1176  1206 I AT      : [0] AT> AT+ESBP=5,"SBP_TERMINAL_CAPABILITY_FLEX",1 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:09.712384  1176  1182 I RTC_DAC : [-1] resendAllowData, byPrefer=1, allowSlot=-1, simCount=1
09-29 16:20:09.712618  1176  1218 I UtInterface: mask the SIGPIPE for xcap thread success!
09-29 16:20:09.712657  1176  1218 D UtInterface: work
09-29 16:20:09.714009  1176  1218 D SS_CCCI : socket opened, fd = 62!!
09-29 16:20:09.714080  1176  1218 D SS_CCCI : sendMessage: SS_CCCI_MSG_TYPE_SS_INIT_REQ
09-29 16:20:09.714103  1176  1218 I SS_CCCI : sendMessage: data=****************************************
09-29 16:20:09.714128  1176  1218 D SS_CCCI : getModemCurrentStatus(): getModemCurrentStatus(), modem status=2
09-29 16:20:09.714406  1176  1218 D UtInterface: initMsgLoop
09-29 16:20:09.714464  1176  1218 D UtInterface: Loop: gCommandQueue.size=0
09-29 16:20:09.714511  1176  1191 I AT      : [0] AT< +EGMR: "4898137410072302   SF650A4LAWBA145                          10P" (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.714513  1176  1193 I AT      : [0] AT< OK (RIL_CMD_READER_2, tid:493438508288)
09-29 16:20:09.714554  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.714677  1176  1194 I AT      : [0] AT> AT+EVOCD=1 (RIL_CMD_READER_2 tid:493437472000)
09-29 16:20:09.715610  1176  1199 I AT      : [0] AT< +CME ERROR: 100 (RIL_ATCI_READER, tid:493432290560)
09-29 16:20:09.715885  1176  1200 D RmcSSHandler: [0] Create RmcSuppServUssdDomainSelector
09-29 16:20:09.715990  1176  1200 I AT      : [0] AT> AT+EIUSD=*** (RIL_ATCI_READER, tid:493431254272)
09-29 16:20:09.716533  1176  1220 I SS_CCCI : mask the SIGPIPE for ccci thread success!
09-29 16:20:09.716869  1176  1220 D SS_CCCI : CCCIThread(), pid: 1176, tid: 1220
09-29 16:20:09.718507  1176  1199 I AT      : [0] AT< OK (RIL_ATCI_READER, tid:493432290560)
09-29 16:20:09.718657  1176  1200 I AT      : [0] AT> AT+CSSN=1,1 (RIL_ATCI_READER tid:493431254272)
09-29 16:20:09.720820  1176  1182 D RpMDCtrl: [-1] Init()
09-29 16:20:09.720927  1176  1182 D RtcRilClientController: [-1] RtcRilClientController init()
09-29 16:20:09.720949  1176  1182 D RtcRilClientController: [-1] init client number: 6
09-29 16:20:09.721261  1176  1182 D RtcRilClientController: [-1] RtcRilClientController CLIENT_TYPE_OEM
09-29 16:20:09.721563  1176  1182 I RilOemClient: Init Oem client
09-29 16:20:09.721601  1176  1182 D RilClientQueue: construct client with client id 1001
09-29 16:20:09.721629  1176  1182 D RtcRilClientController: [-1] RtcRilClientController CLIENT_TYPE_ATCI
09-29 16:20:09.721709  1176  1223 I RilClient: start listen on fd: 30, socket name: rild-oem
09-29 16:20:09.721822  1176  1182 D RilClientQueue: construct client with client id 1006
09-29 16:20:09.721921  1176  1182 D RtcRadioConfig: [-1] RtcCommSimRadioConfigController::onInit
09-29 16:20:09.721953  1176  1182 W sms-ril : [RtcSmsThread]create
09-29 16:20:09.721969  1176  1182 V sms-ril : [RtcSmsThread]Construct 0x12970367424629017360
09-29 16:20:09.722190  1176  1182 V RtcNrSwCtrl: [-1] [onInit]
09-29 16:20:09.722280  1176  1182 I RfxMainThread: initControllers end
09-29 16:20:09.722293  1176  1182 I RfxMainThread: initControllers process async queue start
09-29 16:20:09.722308  1176  1182 I RfxMainThread: initControllers process async queue end
09-29 16:20:09.724052  1176  1225 D sms-ril : [RtcSmsThread]readyToRun
09-29 16:20:09.724284  1176  1224 I RilClient: start listen on fd: 32, socket name: rild-atci
09-29 16:20:09.726225  1176  1192 I AT      : [0] AT> AT+EAPC? (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.729595  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:09.729833  1176  1193 I AT      : [0] AT< OK (RIL_CMD_READER_2, tid:493438508288)
09-29 16:20:09.729999  1176  1206 I AT      : [0] AT> AT+ESIMS (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:09.730082  1176  1182 E RILC    : imsNetworkStateChangedInd: radioService[0]->mRadioIndication == NULL
09-29 16:20:09.730155  1176  1194 I AT      : [0] AT> AT+ECCP=1 (RIL_CMD_READER_2 tid:493437472000)
09-29 16:20:09.730689  1176  1182 I RTC_DAC : [-1] setAllowDataSlot allow=1 slot=0
09-29 16:20:09.733012  1176  1199 I AT      : [0] AT< OK (RIL_ATCI_READER, tid:493432290560)
09-29 16:20:09.733160  1176  1191 I AT      : [0] AT< +EAPC=*** (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.733185  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.733447  1176  1200 I AT      : [0] AT> AT+COLP=1 (RIL_ATCI_READER tid:493431254272)
09-29 16:20:09.734731  1176  1192 I AT      : [0] AT> AT+EREG=3 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.735107  1176  1198 D RmcDcMsimReqHandler: setDataAllowed: allowed= 1
09-29 16:20:09.735237  1176  1198 D RmcDcMsimReqHandler: [updatePreDataAllowStatus] SIM[0]: -2 , allowed = 1
09-29 16:20:09.735326  1176  1198 I AT      : [0] AT> AT+EDALLOW=1 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:09.735866  1176  1182 I RtcDC   : [0]onAllowedChanged: allowed = -2
09-29 16:20:09.736704  1176  1193 I AT      : [0] AT< OK (RIL_CMD_READER_2, tid:493438508288)
09-29 16:20:09.736904  1176  1194 I AT      : [0] AT> AT+EECCFC=1 (RIL_CMD_READER_2 tid:493437472000)
09-29 16:20:09.738352  1176  1184 I AT      : [0] AT< +EREG=*** (RIL_URC_READER, tid:493447834880)
09-29 16:20:09.738363  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.738574  1176  1192 I AT      : [0] AT> AT+EGREG=3,1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.739011  1176  1185 D RmcNwHdlr: [0] [handleCsNetworkStateChanged] mMdEreg n=0, stat=0, lac=**FF, ci=***FFFF, eAct=0, nwk_existence=0, roam_indicator=0, cause_type=0, reject_cause=0 mMdEcell act=0, cid=*, mcc=0, mnc=0, lacTac=*, pscPci=*, sig1=0, sig2=0, rsrp=0, rsrq=0, timingAdvance=0, rssnr=0, cqi=0, bsic=0, arfcn=0
09-29 16:20:09.739413  1176  1182 E RILC    : responseCsNetworkStateChangeInd: mtkRadioExService[0]->responseCsNetworkStateChangeInd == NULL
09-29 16:20:09.739568  1176  1182 E RILC    : networkStateChangedInd: radioService[0]->mRadioIndication == NULL
09-29 16:20:09.740030  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:09.740143  1176  1199 I AT      : [0] AT< OK (RIL_ATCI_READER, tid:493432290560)
09-29 16:20:09.740217  1176  1198 D RmcDcMsimReqHandler: [updateDataAllowStatus] SIM[0]: 1 , allowed = 1
09-29 16:20:09.740243  1176  1200 I AT      : [0] AT> AT+CUSD=1 (RIL_ATCI_READER tid:493431254272)
09-29 16:20:09.740391  1176  1182 I RtcDC   : [0]onAllowedChanged: allowed = 1
09-29 16:20:09.740495  1176  1182 E RILC    : onMdDataRetryCountReset: mtkRadioExService[0]->mRadioIndicationMtk == NULL
09-29 16:20:09.740634  1176  1182 E RILC    : RIL_onRequestComplete: invalid RIL_Token
09-29 16:20:09.741795  1176  1193 I AT      : [0] AT< OK (RIL_CMD_READER_2, tid:493438508288)
09-29 16:20:09.742524  1176  1191 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.742714  1176  1192 I AT      : [0] AT> AT+EGREG=3 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.743892  1176  1199 I AT      : [0] AT< OK (RIL_ATCI_READER, tid:493432290560)
09-29 16:20:09.744112  1176  1200 I AT      : [0] AT> AT+CLIP=1 (RIL_ATCI_READER tid:493431254272)
09-29 16:20:09.745061  1176  1184 I AT      : [0] AT< +EGREG=*** (RIL_URC_READER, tid:493447834880)
09-29 16:20:09.745767  1176  1185 D RmcNwHdlr: [0] [handlePsNetworkStateChanged] mMdEgreg n=0, stat=0, lac=**FF, ci=***FFFF, eAct=0, rac=255, nwk_existence=0, roam_indicator=0, cause_type=0, reject_cause=0, dcnr_restricted=0, endc_sib=0, endc_available=0.   mMdEcell act=0, cid=*, mcc=0, mnc=0, lacTac=*, pscPci=*, sig1=0, sig2=0, rsrp=0, rsrq=0, timingAdvance=0, rssnr=0, cqi=0, bsic=0, arfcn=0
09-29 16:20:09.745836  1176  1185 D RmcNwHdlr: [0] handleScgConnectionChange old=0, new=0
09-29 16:20:09.746098  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.746233  1176  1192 I AT      : [0] AT> AT+PSBEARER=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.746599  1176  1199 I AT      : [0] AT< OK (RIL_ATCI_READER, tid:493432290560)
09-29 16:20:09.746764  1176  1200 I AT      : [0] AT> AT+CNAP=1 (RIL_ATCI_READER tid:493431254272)
09-29 16:20:09.748554  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.749148  1176  1192 I AT      : [0] AT> AT+ECSQ=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.749642  1176  1199 I AT      : [0] AT< OK (RIL_ATCI_READER, tid:493432290560)
09-29 16:20:09.749812  1176  1200 I AT      : [0] AT> AT+ESSP=1 (RIL_ATCI_READER tid:493431254272)
09-29 16:20:09.751762  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.751961  1176  1192 I AT      : [0] AT> AT+CTZR=3 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.753060  1176  1199 I AT      : [0] AT< OK (RIL_ATCI_READER, tid:493432290560)
09-29 16:20:09.753258  1176  1200 I AT      : [0] AT> AT+CSCS="UCS2" (RIL_ATCI_READER tid:493431254272)
09-29 16:20:09.754931  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.755208  1176  1192 I AT      : [0] AT> AT+ECELL=4 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.757215  1176  1199 I AT      : [0] AT< OK (RIL_ATCI_READER, tid:493432290560)
09-29 16:20:09.757396  1176  1200 I AT      : [0] AT> AT+EXCAPCFGGET="version" (RIL_ATCI_READER tid:493431254272)
09-29 16:20:09.758674  1176  1213 I VT RIL THD: [VT RIL THD] accepted, sVtsFd: 1, sIsVtConnected: 49
09-29 16:20:09.759023  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.759202  1176  1192 I AT      : [0] AT> AT+ECELL=7,1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.763954  1176  1199 I AT      : [0] AT< +CME ERROR: 100 (RIL_ATCI_READER, tid:493432290560)
09-29 16:20:09.763943  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.764138  1176  1200 E RmcSSHandler: [0] requestGetModemVersion p_response->getIntermediates() == NULL
09-29 16:20:09.764448  1176  1192 I AT      : [0] AT> AT+EONS=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.765539  1176  1200 D RmcSSHandler: [0] syncCLIRToStatusManager, clir_n = 0
09-29 16:20:09.767879  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.768066  1176  1192 I AT      : [0] AT> AT+EOPS=3,2 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.770160  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.770382  1176  1192 I AT      : [0] AT> AT+ECAL? (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.772690  1176  1191 I AT      : [0] AT< +ECAL: 1 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.773314  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.773528  1176  1192 I AT      : [0] AT> AT+EMCCMNC=0 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.776575  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.776808  1176  1192 I AT      : [0] AT> AT+EIMSESS=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.780149  1176  1191 I AT      : [0] AT< +EIMSESS: 3,0 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.780374  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.780520  1176  1192 I AT      : [0] AT> AT+CSCON=3 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.780740  1176  1185 D RmcNwHdlr: [0] onImsEmergencySupportR9: 0
09-29 16:20:09.781200  1176  1182 E RILC    : networkStateChangedInd: radioService[0]->mRadioIndication == NULL
09-29 16:20:09.783579  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.783932  1176  1192 I AT      : [0] AT> AT+EOPS=6,1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.786703  1176  1191 I AT      : [0] AT< +CME ERROR: 3 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.786927  1176  1192 I AT      : [0] AT> AT+EOPS=3,2 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.790636  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.790848  1176  1192 I AT      : [0] AT> AT+ECAMPUI=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.793616  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.793995  1176  1192 I AT      : [0] AT> AT+ECAPABILITY=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.796558  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.797085  1176  1192 I AT      : [0] AT> AT+ECAPABILITY? (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.799226  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.799415  1176  1192 E RmcNwReqHdlr: [0] There is something wrong with AT+ECAPABILITY
09-29 16:20:09.799577  1176  1192 I AT      : [0] AT> AT+ENWSCN=? (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.801817  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.801986  1176  1192 I AT      : [0] AT> AT+E5GUW=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.814915  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.815146  1176  1192 I AT      : [0] AT> AT+E5GUC=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.817771  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.818050  1176  1192 I AT      : [0] AT> AT+EPHYCONFIG=2 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.820225  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.820596  1176  1192 I AT      : [0] AT> AT+EOPS? (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:09.822900  1176  1191 I AT      : [0] AT< +EOPS: 0,2,"",1 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.823085  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:09.857022  1176  1195 I AT      : [0] AT< +EMULTIIMS: 2 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:09.857123  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:09.858529  1176  1196 I AT      : [0] AT> AT+ECFGSET="report_eimsreginfo_urc","1" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:09.869648  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:09.869873  1176  1196 I AT      : [0] AT> AT+CIREP=1 (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:09.872270  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:09.872426  1176  1196 I AT      : [0] AT> AT+ECFGSET="mtk_ct_volte_support","2" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:09.884772  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:09.886762  1176  1196 I AT      : [0] AT> AT+ECGLA=? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:09.888803  1176  1195 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:09.895811  1176  1196 I AT      : [0] AT> AT+CSRA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:09.898190  1176  1195 I AT      : [0] AT< +CSRAC: 1,1,0,0,0,1,1 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:09.898404  1176  1195 I AT      : [0] AT< +CSRAA: 1,1,0,0,0,1,1 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:09.898432  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:09.899475  1176  1196 D RmcGwsdReqHdl: [0] RmcGwsdRequestHandler constructor
09-29 16:20:09.899883  1176  1196 D RmcCatComReqHandler: [0] query SUBMARINE support, IMS SUBMARINE=0
09-29 16:20:10.166482  1176  1214 D VT RIL THD: [RIL IMCB THD] id = 103003, size = 12
09-29 16:20:10.451457  1176  1205 I AT      : [0] AT< +ESIMS: 0 (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.451743  1176  1205 I AT      : [0] AT< +ECT=*** (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.451839  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.451974  1176  1206 I AT      : [0] AT> AT+CSCS="UCS2" (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:10.454202  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.454542  1176  1206 I AT      : [0] AT> AT+EGTP=1 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:10.456617  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.456847  1176  1206 I AT      : [0] AT> AT+EMPPCH=1 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:10.459409  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.459593  1176  1206 I AT      : [0] AT> AT+EDSDA=1 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:10.461668  1176  1205 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.462712  1176  1206 I AT      : [0] AT> AT+ESADM=1 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:10.464781  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.466667  1176  1206 I RmcRadioReq: [0] isNormalBootUp = 1, boot_reason = reboot,userrequested
09-29 16:20:10.466768  1176  1206 I AT      : [0] AT> AT+EBOOT=0 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:10.469830  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.470885  1176  1206 I AT      : [0] AT> AT+EDSBP=1 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:10.492778  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.492969  1176  1206 I AT      : [0] AT> AT+EPOC (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:10.500699  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.500912  1176  1206 I AT      : [0] AT> AT+EFUN=0 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:10.534052  1176  1184 I AT      : [0] AT< +ESIMS: 1,29 (RIL_URC_READER, tid:493447834880)
09-29 16:20:10.534806  1176  1182 I RtcPhb  : [0] [onSimPlugOut] newValue 29
09-29 16:20:10.534929  1176  1182 D RtcCatController: [0] onSimOnOffStateChanged  newState 0
09-29 16:20:10.534652  1176  1184 I AT      : [0] AT< +EUSIM: 2, 2, 2 (RIL_URC_READER, tid:493447834880)
09-29 16:20:10.535419  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.535566  1176  1184 I AT      : [0] AT< +ICCID=*** (RIL_URC_READER, tid:493447834880)
09-29 16:20:10.535831  1176  1184 I AT      : [0] AT< +ESIMS: 0,1 (RIL_URC_READER, tid:493447834880)
09-29 16:20:10.535931  1176  1184 I AT      : [0] AT< +ESIMIND: 1, 0, 0 (RIL_URC_READER, tid:493447834880)
09-29 16:20:10.538952  1176  1182 E RILC    : uiccApplicationsEnablementChanged(): radioService[0]->mRadioIndication == NULL
09-29 16:20:10.539838  1176  1182 D RtcEccNumberController: [0] [onCardTypeChanged], reset SIM/NW ECC due to No SIM
09-29 16:20:10.540744  1176  1180 I RfxMclMessenger: RFX_MSG_REQUEST_BOOT_TURN_ON_RADIO(56525) dispatchs to main protocol: 0
09-29 16:20:10.541070  1176  1196 I AT      : [0] AT> AT+ICCID? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:10.541526  1176  1182 D EccNumberSource: [XML][0][update] START for plmn: , isSimInsert: 0
09-29 16:20:10.542400  1176  1206 I AT      : [0] AT> AT+ESLOTSINFO=1 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:10.542599  1176  1237 I RmcRadioReq: [0] mdStatusReaderLoop - md status working thread
09-29 16:20:10.543925  1176  1182 D EccNumberPreference: [0][update] for PLMN:  GSM only: , GSM prefer: , CDMA prefer: 
09-29 16:20:10.544068  1176  1182 I RtcEccNumberController: [0] [updateEmergencyNumber] mIsFwkReady: 0, mIsPendingUpdate: 0, ecc list: 112,911,000,08,110,118,119,999
09-29 16:20:10.544435  1176  1237 I RmcRadioReq: [0] [RmcRadioRequestHandler] mdStatusReaderLoop: fd = 63
09-29 16:20:10.544593  1176  1237 I RmcRadioReq: [0] mdStatusReaderLoop: count: 56 modem id: 0, event type: 10, reason: ----
09-29 16:20:10.545463  1176  1195 I AT      : [0] AT< +CME ERROR: 10 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:10.545941  1176  1196 I AT      : [0] AT> AT+EPINC (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:10.546835  1176  1182 I RtcEccNumberController: [0] [updateEmergencyNumber] mIsFwkReady: 0, mIsPendingUpdate: 1, ecc list: 112,911,000,08,110,118,119,999
09-29 16:20:10.548612  1176  1182 D RtcCarrier: [0] [onCardTypeChanged]oldValue: -1, newValue: 0
09-29 16:20:10.548774  1176  1182 D VT RIL RTC: [0] [onCardTypeChanged]oldValue: -1, newValue: 0
09-29 16:20:10.548833  1176  1182 D VT RIL RTC: [0] [updateOpId] m_slot_id: 0, operatorId: 8
09-29 16:20:10.549025  1176  1182 D RtcPhbSimIo: [0] SIM plug out, clear store PBR file
09-29 16:20:10.549209  1176  1212 I VT RIL RMC: [Handle REQ] request = 59522
09-29 16:20:10.549254  1176  1182 D RtcSuppServController: [0] onSimIccidChanged: ICCID is not valid, return directly
09-29 16:20:10.549331  1176  1212 I VT RIL RMC: set mSimOpIdTable[0] = 8
09-29 16:20:10.549664  1176  1205 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.550707  1176  1206 D RmcModemRequestHandler: [0] RmcModemRequestHandler constructor
09-29 16:20:10.550877  1176  1206 D RmcRadioRelReqHandler: [0] RmcRadioRelatedRequestHandler constructor
09-29 16:20:10.551078  1176  1206 I AT      : [0] AT> AT+ES3G? (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:10.551076  1176  1195 I AT      : [0] AT< +CME ERROR: 10 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:10.551194  1176  1196 E RmcCommSimReq: [0] Fail to get PIN and PUK retry count!
09-29 16:20:10.551261  1176  1196 I AT      : [0] AT> AT+EXCGLA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:10.552648  1176  1184 I AT      : [0] AT< +EIND: 32 (RIL_URC_READER, tid:493447834880)
09-29 16:20:10.553165  1176  1185 I RmcPhbUrc: [0] onPhbStateChanged slot=0, isPhbReady=0, isTelephonyAddOnPolicy=1
09-29 16:20:10.553523  1176  1205 I AT      : [0] AT< +ES3G: 1 (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.553569  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.555150  1176  1195 I AT      : [0] AT< +EXCGLA: 0 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:10.555258  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:10.560597  1176  1182 I RtcRadioCont: [0] radio State: 1 -> 0, using google native API for urc
09-29 16:20:10.560880  1176  1182 I RIL-Fusion: getRadioState(): radioState=0
09-29 16:20:10.560990  1176  1182 E RILC    : radioStateChangedInd: radioService[0]->mRadioIndication == NULL
09-29 16:20:10.561033  1176  1196 I RmcCommSimReq: [0] querySimExtendedFormat temp_cap: 0, vendor.gsm.sim.extended.format1: 0
09-29 16:20:10.561052  1176  1182 E RILC    : radioStateChangedInd: radioService[4]->mRadioIndication == NULL
09-29 16:20:10.561068  1176  1182 I RILC    : Request UNSOL_RESPONSE_RADIO_STATE_CHANGED(0) already append into IMS pending ind list
09-29 16:20:10.561080  1176  1182 E RILC    : radioStateChangedInd: radioService[8]->mRadioIndication == NULL
09-29 16:20:10.561091  1176  1182 E RILC    : radioStateChangedInd: radioService[12]->mRadioIndication == NULL
09-29 16:20:10.561143  1176  1182 I RtcEccNumberController: [0] [onRadioStateChanged] radio off, clear network ECC list
09-29 16:20:10.561351  1176  1206 I AT      : [0] AT> AT+ESBP=7,"SBP_T_PLUS_W" (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:10.562898  1176  1182 I RtcEccNumberController: [0] [updateEmergencyNumber] mIsFwkReady: 0, mIsPendingUpdate: 1, ecc list: 112,911,000,08,110,118,119,999
09-29 16:20:10.564229  1176  1182 I RtcImsConfigController: [0] onRadioStateChanged, state = 0
09-29 16:20:10.564299  1176  1182 D RTC_EMBMS_CON_PROXY: [0] radioState 0
09-29 16:20:10.569679  1176  1205 I AT      : [0] AT< +ESBP: 1 (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.569784  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.570624  1176  1206 I AT      : [0] AT> AT+ESBP=7,"SBP_GEMINI_LG_WG_MODE" (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:10.573125  1176  1205 I AT      : [0] AT< +ESBP: 0 (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.573225  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.574686  1176  1206 I AT      : [0] AT> AT+EPSB? (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:10.581472  1176  1205 I AT      : [0] AT< +EPSB: 1023 (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.581580  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.582133  1176  1206 I RmcCapa : [0] sendEGRAT: raf=249358, rat=6
09-29 16:20:10.582223  1176  1206 I AT      : [0] AT> AT+EGRAT=6 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:10.582376  1176  1198 I AT      : [0] AT> AT+EFD=? (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:10.585231  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.585745  1176  1197 I AT      : [0] AT< +EFD: (0-3) (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:10.586329  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:10.586613  1176  1196 D RmcHdcHdr: [0] onHandleEvent: 52512
09-29 16:20:10.586651  1176  1196 D RmcHdcHdr: [0] sendHardwareConfigUrc: m_slot_id:0
09-29 16:20:10.586670  1176  1206 I RmcRadioReq: [0] bootupSetRadioPower, origin mode = 0
09-29 16:20:10.586694  1176  1206 I RmcRadioReq: [0] bootupSetRadioPower, target mode = 0
09-29 16:20:10.590103  1176  1198 I AT      : [0] AT> AT+EFD=2,0,50 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:10.590432  1176  1182 I RtcCapa : [-1] updateRadioCapability, no c2k, session=-1, capability[0] = 81930
09-29 16:20:10.590566  1176  1182 D RtcRatSwCtrl: [0] [calculateDefaultNetworkType] card_type: 0, card_state: 3, rat_mode: -1, isCt3GDualMode: false, ct3gStatus: 0.  slotCap: 81930, slotNwtype: 9, defaultRaf: 81930, defNwType: 9.
09-29 16:20:10.591841  1176  1182 D RtcRatSwCtrl: [0] [setPreferredNetworkType] rafFromRiljNetworkType: 642574, targetRaf: 642574, targetNetworkType: 9, mNwsMode: 1, mInRestrictedMode: 0
09-29 16:20:10.591985  1176  1182 D RtcRatSwCtrl: [0] [switchNwRat] ratSwitchCaller: INIT, mCurPreferedNetWorkType: -1, mDefaultNetworkType: -1, prefNwTypeFromRilj: 9, targetPrefNwType: 9, GsmOnlySim: 0
09-29 16:20:10.592139  1176  1182 I RtcCapa : getRafFromNetworkType, type=-1, raf=1
09-29 16:20:10.592299  1176  1182 D RtcCC   : [0] [onCsPhoneChanged], preCsPhone:0, newCsPhone:0
09-29 16:20:10.592365  1176  1182 D RtcCarrier: [0] [onNwsModeChanged] oldValue: -1, newValue: 1
09-29 16:20:10.592425  1176  1182 D RtcCarrier: [0] [onNwsModeChanged] mccmnc is empty
09-29 16:20:10.592563  1176  1206 I AT      : [0] AT> AT+ERAT=6,4 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:10.592697  1176  1182 E RILC    : RIL_onRequestComplete: invalid RIL_Token
09-29 16:20:10.595876  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:10.596047  1176  1198 I AT      : [0] AT> AT+EFD=2,2,50 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:10.597591  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:10.598338  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:10.599005  1176  1182 D RtcRatSwCtrl: [0] [updatePhoneMode] mPhoneMode: 1
09-29 16:20:10.599016  1176  1198 I AT      : [0] AT> AT+EFD=2,1,150 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:10.607436  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:10.607641  1176  1198 I AT      : [0] AT> AT+EFD=2,3,150 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:10.611521  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:10.611798  1176  1198 I AT      : [0] AT> AT+EFD=1 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:10.619416  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:10.619609  1176  1198 I AT      : [0] AT> AT+EEPDG=1 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:10.621804  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:10.621987  1176  1198 I AT      : [0] AT> AT+EIWLPLEN =1 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:10.624313  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:10.624471  1176  1198 D RmcDcMiscImpl: [syncIwlanOperationModeToMd] enable IWLAN Priority List update
09-29 16:20:10.632395  1176  1184 I AT      : [0] AT< +EIND: 1 (RIL_URC_READER, tid:493447834880)
09-29 16:20:10.633148  1176  1196 D RmcCommSmsReq: [0] notifySmsReady
09-29 16:20:10.633259  1176  1196 I AT      : [0] AT> AT+CMGF=0 (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:10.633421  1176  1182 D RtcGsmSmsCtrl: [0] SMS framework isn't ready yet. queue RFX_MSG_URC_SMS_READY_NOTIFICATION
09-29 16:20:10.639886  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:10.640074  1176  1196 I AT      : [0] AT> AT+CSMS=1 (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:10.647355  1176  1195 I AT      : [0] AT< +CME ERROR: 10 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:10.647525  1176  1196 I AT      : [0] AT> AT+CNMI=1,2,2,1,1 (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:10.655105  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:10.655280  1176  1196 I AT      : [0] AT> AT+CPMS="SM", "SM", "SM" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:10.662588  1176  1195 I AT      : [0] AT< ERROR (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:10.662789  1176  1196 I AT      : [0] AT> AT+EC2KCPMS="SM", "SM", "SM" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:10.669941  1176  1195 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:10.670128  1176  1196 I AT      : [0] AT> AT+EWAC=1 (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:10.677428  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:10.687413  1176  1196 D RmcCommSmsReq: [0] SIM card was removed!
09-29 16:20:10.711533  1176  1194 I VT RIL CMN RMC: [Handle REQ] request = 59527
09-29 16:20:10.711603  1176  1194 I VT RIL CMN RMC: [Handle REQ] RFX_MSG_REQUEST_ENABLE_ANBR
09-29 16:20:10.711616  1176  1194 I VT RIL CMN RMC: [handleEnableANBR] enable = 1
09-29 16:20:10.711712  1176  1194 I AT      : [0] AT> AT+EANBR=1 (RIL_CMD_READER_2 tid:493437472000)
09-29 16:20:10.719027  1176  1193 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_2, tid:493438508288)
09-29 16:20:10.719193  1176  1194 I VT RIL CMN RMC: [handleEnableANBR] response error
09-29 16:20:11.426965   622   622 D MtkSubscriptionInfoUpdater: initIccidStringForNoSim
09-29 16:20:12.741173  1176  1182 E RILC    : networkStateChangedInd: radioService[0]->mRadioIndication == NULL
09-29 16:20:15.744791  1176  1182 E RILC    : networkStateChangedInd: radioService[0]->mRadioIndication == NULL
09-29 16:20:18.219913  1251  1251 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=android listener=com.android.server.wifi.WifiCarrierInfoManager$SubscriptionChangeListener@608524d
09-29 16:20:18.221984  1251  1251 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:18.747517  1176  1182 E RILC    : networkStateChangedInd: radioService[0]->mRadioIndication == NULL
09-29 16:20:19.334734  1251  1251 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=android listener=com.mediatek.net.networkstats.MtkTestSimHandler$1@fee08d7
09-29 16:20:19.335127  1251  1251 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:19.415929   626   626 D MtkSubscriptionInfoUpdater: initIccidStringForNoSim
09-29 16:20:20.742884  1251  1361 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=android listener=com.android.server.net.NetworkStatsSubscriptionsMonitor@8b7f5fc
09-29 16:20:20.743189  1251  1361 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:20.863590  1251  1251 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=android listener=com.android.server.vcn.TelephonySubscriptionTracker$1@594668a
09-29 16:20:20.864121  1251  1251 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:21.043774  1251  1362 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=android listener=com.android.server.net.NetworkPolicyManagerService$3@ee19ba2
09-29 16:20:21.044151  1251  1362 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:21.117107  1251  1251 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=android listener=com.android.server.location.gnss.GnssNetworkConnectivityHandler$1@ac447d
09-29 16:20:21.117379  1251  1251 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:21.143061  1251  1272 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:21.200456  1251  1251 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=android listener=com.android.server.emergency.EmergencyAffordanceService$2@69bd8c
09-29 16:20:21.200792  1251  1251 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:21.245830  1519  1519 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.android.systemui listener=com.android.keyguard.KeyguardUpdateMonitor$5@ffbcd24
09-29 16:20:21.249199  1251  1547 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:21.271832  1251  1251 D TelephonyRegistry: systemRunning register for intents
09-29 16:20:21.464254  1251  1283 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=android listener=com.android.server.stats.pull.StatsPullAtomService$StatsSubscriptionsListener@fea7df
09-29 16:20:21.464643  1251  1283 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:21.749230  1176  1182 E RILC    : networkStateChangedInd: radioService[0]->mRadioIndication == NULL
09-29 16:20:22.024514  1669  1669 I MtkIccProvider: MtkIccProvider URL_MATCHER android.content.UriMatcher@a85749f
09-29 16:20:22.229900  1669  1669 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.android.phone listener=com.android.phone.SimPhonebookProvider$1@f73aea2
09-29 16:20:22.232138  1251  1557 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:22.342429  1669  1669 E TelephonyComponentFactory: getValidatedPaths: com.mediatek.internal.telephony.MtkTelephonyComponentFactory ,/system/framework/mediatek-telephony-common.jar
09-29 16:20:22.343459  1669  1669 E TelephonyComponentFactory: StructStatVfs: 4097 ,1
09-29 16:20:22.343558  1669  1669 D TelephonyComponentFactory: validated paths: /system/framework/mediatek-telephony-common.jar
09-29 16:20:22.398388  1519  1519 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:22.405671  1669  1669 E TelephonyComponentFactory: getValidatedPaths: com.mediatek.internal.telephony.MtkTelephonyComponentFactory ,/system/framework/mediatek-telephony-common.jar
09-29 16:20:22.405976  1669  1669 E TelephonyComponentFactory: StructStatVfs: 4097 ,1
09-29 16:20:22.406053  1669  1669 D TelephonyComponentFactory: Total components injected: 21
09-29 16:20:22.406260  1669  1669 D TDC     : class = class com.mediatek.internal.telephony.MtkTelephonyDevController
09-29 16:20:22.406395  1669  1669 D TDC     : constructor function = public com.mediatek.internal.telephony.MtkTelephonyDevController()
09-29 16:20:22.406621  1669  1669 D TDC     : updateOrInsert: inserting: Modem { uuid=modem, state=0, rilModel=0, rat={}, maxActiveVoiceCall=1, maxActiveDataCall=1, maxStandby=1 }
09-29 16:20:22.406682  1669  1669 D TDC     : updateOrInsert: inserting: Sim { uuid=sim, modemUuid=modem, state=0 }
09-29 16:20:22.406717  1669  1669 D TDC     : MtkTelephonyDevController constructor
09-29 16:20:22.425172  1669  1669 D MetricsCollector: registered
09-29 16:20:22.426999  1669  1669 D TelephonyComponentFactory: makeDefaultPhoneNotifier mtk
09-29 16:20:22.427322  1669  1669 D MtkTelephonyRegistryEx: publish: com.mediatek.internal.telephony.MtkTelephonyRegistryEx@f890452
09-29 16:20:22.429408  1669  1669 D CdmaSSM : subscriptionSource from settings: 0
09-29 16:20:22.429504  1669  1669 I PhoneFactory: Cdma Subscription set to 0
09-29 16:20:22.429705  1669  1669 I PhoneFactory: Network Mode set to 9
09-29 16:20:22.430129  1669  1669 D RILJ    : RIL: init allowedNetworkTypes=9 cdmaSubscription=0) [PHONEnull]
09-29 16:20:22.433825  1519  1608 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.android.systemui listener=com.android.systemui.statusbar.policy.NetworkControllerImpl$SubListener@1a0dbd9
09-29 16:20:22.434478  1251  1782 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:22.440652  1669  1669 I MtkRILJ : getRadioProxy wait for MtkRIL
09-29 16:20:22.440892  1669  1669 I MtkRILJ : getRadioProxy wait for MtkRIL
09-29 16:20:22.440964  1669  1669 D RILJ    : Radio HAL version: -1.-1 [PHONE0]
09-29 16:20:22.441043  1669  1669 D MtkRILJ : constructor: sub = 0
09-29 16:20:22.448689  1669  1669 E RILJ    : getRadioProxy: mRadioVersion 1.6 [PHONE0]
09-29 16:20:22.449726  1669  1669 D MtkRILJ : override response functions [SUB0]
09-29 16:20:22.450567  1176  1176 I RILC    : setResponseFunctions, slotId = 0
09-29 16:20:22.456789  1176  1176 I RIL-Fusion: getRadioState(): radioState=0
09-29 16:20:22.456880  1176  1176 E RILC    : radioStateChangedInd: radioService[4]->mRadioIndication == NULL
09-29 16:20:22.456899  1176  1176 E RILC    : radioStateChangedInd: radioService[8]->mRadioIndication == NULL
09-29 16:20:22.456911  1176  1176 E RILC    : radioStateChangedInd: radioService[12]->mRadioIndication == NULL
09-29 16:20:22.456942  1176  1176 I RILC    : RIL Daemon version: android reference-ril 1.0
09-29 16:20:22.457032  1176  1182 D RtcCC   : [0] No call, ignore hangup all: slot = 0
09-29 16:20:22.457891  1176  1176 I RILC    : onNewCommandConnect, slot 0, client 0
09-29 16:20:22.458183  1176  1178 I RILC    : sendPendedUrcCallback 0 0 0
09-29 16:20:22.458215  1176  1178 I RILC    : sendPendedUrcs RIL_SOCKET_1, UNSOL_RESPONSE_SIM_STATUS_CHANGED, client 0
09-29 16:20:22.458299  1176  1178 E RILC    : simStatusChangedInd: radioService[8]->mRadioIndication == NULL
09-29 16:20:22.458314  1176  1178 I RILC    : sendPendedUrcs RIL_SOCKET_1, UNSOL_RESPONSE_SIM_STATUS_CHANGED, client 0
09-29 16:20:22.458348  1176  1178 E RILC    : simStatusChangedInd: radioService[8]->mRadioIndication == NULL
09-29 16:20:22.458359  1176  1178 I RILC    : sendPendedUrcs RIL_SOCKET_1, UNSOL_RADIO_CAPABILITY, client 0
09-29 16:20:22.458407  1176  1178 I RILC    : sendPendedUrcs RIL_SOCKET_1, UNSOL_HARDWARE_CONFIG_CHANGED, client 0
09-29 16:20:22.458502  1176  1178 I RILC    : sendPendedUrcs RIL_SOCKET_1, UNSOL_VOICE_RADIO_TECH_CHANGED, client 0
09-29 16:20:22.458538  1176  1178 I RILC    : sendPendedUrcs RIL_SOCKET_1, UNSOL_RESPONSE_SIM_STATUS_CHANGED, client 0
09-29 16:20:22.458567  1176  1178 E RILC    : simStatusChangedInd: radioService[8]->mRadioIndication == NULL
09-29 16:20:22.459096  1176  1182 D RtcEccNumberController: [0] [onConnectionStateChanged] status: 1, mIsFwkReady: 0, mIsPendingUpdate: 1
09-29 16:20:22.459213  1176  1182 I RtcMwi  : [0] [0]onConnectionStateChanged: oldState = 0, newState = 1
09-29 16:20:22.459245  1176  1182 D RtcGsmSmsCtrl: [0] onHidlStateChanged (false, true, false) (slot 0)
09-29 16:20:22.460162  1176  1208 D RmcDcImsDc2ReqHandler: [0][handleResetImsConnection] imsConnState: 0, eimsConnState: 0
09-29 16:20:22.460576  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:22.460911  1669  1811 D RILJ    : [UNSL]< UNSOL_RIL_CONNECTED [PHONE0]
09-29 16:20:22.463434  1669  1669 D RILJ    : [0001]> GET_HARDWARE_CONFIG [PHONE0]
09-29 16:20:22.467045  1176  1196 D RmcHdcHdr: [0] onHandleRequest: 55517
09-29 16:20:22.467100  1176  1196 D RmcHdcHdr: [0] handleHardwareConfigRequest: m_slot_id:0
09-29 16:20:22.467247  1176  1196 D RmcHdcHdr: [0] sendHardwareConfigUrc: m_slot_id:0
09-29 16:20:22.472797  1669  1811 D RILJ    : [0002]> CDMA_SET_SUBSCRIPTION_SOURCE cdmaSubscription = 0 [PHONE0]
09-29 16:20:22.474541  1669  1811 D RILJ    : [0001]< GET_HARDWARE_CONFIG  [Modem { uuid=modem_sys1_ps0, state=0, rilModel=0, rat={0, 2, 13, 15}, maxActiveVoiceCall=1, maxActiveDataCall=1, maxStandby=1 }] [Sim { uuid=modem_sys1_ps0, modemUuid=modem_sys1_ps0, state=0 }]  [PHONE0]
09-29 16:20:22.474989  1176  1176 I RILC    : setResponseFunctionsMtk, slotId = 0
09-29 16:20:22.475104  1176  1178 I RILC    : sendPendedUrcCallback 0 0 1
09-29 16:20:22.475128  1176  1178 I RILC    : sendPendedUrcs RIL_SOCKET_1, UNSOL_RESPONSE_PS_NETWORK_STATE_CHANGED, client 1
09-29 16:20:22.475283  1176  1178 I RILC    : sendPendedUrcs RIL_SOCKET_1, RIL_UNSOL_PLMN_DATA, client 1
09-29 16:20:22.475372  1176  1178 I RILC    : sendPendedUrcs RIL_SOCKET_1, RIL_UNSOL_ICCID_CHANGED, client 1
09-29 16:20:22.475427  1176  1178 I RILC    : sendPendedUrcs RIL_SOCKET_1, RIL_UNSOL_ICCID_CHANGED, client 1
09-29 16:20:22.475477  1176  1178 I RILC    : sendPendedUrcs RIL_SOCKET_1, RIL_UNSOL_PHB_READY_NOTIFICATION, client 1
09-29 16:20:22.475524  1176  1178 I RILC    : sendPendedUrcs RIL_SOCKET_1, RIL_UNSOL_ICCID_CHANGED, client 1
09-29 16:20:22.475711  1176  1176 I RILC    : onNewCommandConnect, slot 0, client 1
09-29 16:20:22.476184  1669  1669 D MtkRILJ : queue size  0
09-29 16:20:22.476243  1669  1669 D MtkRILJ : getRilOp
09-29 16:20:22.476464  1669  1669 D MtkRILJ : mMtkRilOp init fail, because OM load
09-29 16:20:22.476553  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:22.476944  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_RADIO_STATE_CHANGED radioStateChanged: 0 [PHONE0]
09-29 16:20:22.477046  1669  1669 D RadioConfig: class = class com.mediatek.internal.telephony.MtkRadioConfig
09-29 16:20:22.477209  1669  1669 D RadioConfig: constructor function = public com.mediatek.internal.telephony.MtkRadioConfig(android.content.Context,com.android.internal.telephony.HalVersion)
09-29 16:20:22.479844  1176  1182 D RtcEccNumberController: [0] [onConnectionStateChanged] status: 1, mIsFwkReady: 0, mIsPendingUpdate: 1
09-29 16:20:22.479949  1176  1182 I RtcMwi  : [0] [0]onConnectionStateChanged: oldState = 1, newState = 1
09-29 16:20:22.479981  1176  1182 D RtcGsmSmsCtrl: [0] onHidlStateChanged (true, true, false) (slot 0)
09-29 16:20:22.480065  1176  1182 E RfxRoot : no RfxBaseData, send error to RILJ
09-29 16:20:22.481262  1669  1811 D RILJ    : Broadcast for RadioStateChanged: state=0 [PHONE0]
09-29 16:20:22.486331  1669  1669 D MtkImsManager [-1]: createMtkImsService binder is null
09-29 16:20:22.487315  1176  1176 D RadioConfig_service: radioConfig::setResponseFunctions
09-29 16:20:22.488735  1669  1669 D FeatureConnector: [InstanceManager, -1] imsFeatureRemoved: reason=3
09-29 16:20:22.490491  1669  1669 D SubscriptionManager: [getSubId]- fail
09-29 16:20:22.491304  1669  1669 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:22.491432  1669  1669 D SubscriptionManager: [getSubId]- fail
09-29 16:20:22.492126  1669  1669 D SubscriptionManager: [getSubId]- fail
09-29 16:20:22.492804  1669  1669 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:22.492932  1669  1669 D ImsManagerIM [-1]: getWfcMode - setting=2
09-29 16:20:22.493597  1669  1669 D MtkImsManager [0]: createMtkImsService binder is null
09-29 16:20:22.495063  1669  1816 D RadioConfig: [0005]> GET_HAL_DEVICE_CAPABILITIES
09-29 16:20:22.495213  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:22.495355  1669  1816 E RadioInterfaceCapabilityController: getRadioInterfaceCapabilities: Radio Capabilities not loaded in time
09-29 16:20:22.495404  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_PS_NETWORK_STATE_CHANGED [PHONE0]
09-29 16:20:22.496799  1669  1811 D RILJ    : [0002]< CDMA_SET_SUBSCRIPTION_SOURCE error 6 [PHONE0]
09-29 16:20:22.497771  1669  1811 D RilRequest: [0002]< CDMA_SET_SUBSCRIPTION_SOURCE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result=null
09-29 16:20:22.501138  1669  1669 D FeatureConnector: [InstanceManager, 0] imsFeatureRemoved: reason=3
09-29 16:20:22.501844  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:22.502079  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_SIM_STATUS_CHANGED [PHONE0]
09-29 16:20:22.502749  1669  1811 D RadioConfigResponse: Radio Hal Version = 1.6
09-29 16:20:22.502938  1669  1811 D RadioConfigResponse: CAPABILITY_USES_ALLOWED_NETWORK_TYPES_BITMASK
09-29 16:20:22.503012  1669  1811 D RadioConfigResponse: CAPABILITY_SECONDARY_LINK_BANDWIDTH_VISIBLE
09-29 16:20:22.503078  1669  1811 D RadioConfigResponse: CAPABILITY_NR_DUAL_CONNECTIVITY_CONFIGURATION_AVAILABLE
09-29 16:20:22.503131  1669  1811 D RadioConfigResponse: CAPABILITY_THERMAL_MITIGATION_DATA_THROTTLING
09-29 16:20:22.503209  1669  1811 D RadioConfigResponse: CAPABILITY_SLICING_CONFIG_SUPPORTED
09-29 16:20:22.503921  1669  1811 D RadioConfigResponse: CAPABILITY_PHYSICAL_CHANNEL_CONFIG_1_6_SUPPORTED
09-29 16:20:22.504092  1669  1811 D RadioConfigResponse: [0005]< GET_HAL_DEVICE_CAPABILITIES
09-29 16:20:22.504184  1669  1816 D RadioInterfaceCapabilityController: setupRadioInterfaceCapabilities: mRadioInterfaceCapabilities now setup
09-29 16:20:22.508585  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:22.517640  1669  1811 D RILJ    : [UNSL]< MTK: RIL_UNSOL_PLMN_DATA PlmnMvnoData(xxx) [PHONE0]
09-29 16:20:22.519579  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:22.519857  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_SIM_STATUS_CHANGED [PHONE0]
09-29 16:20:22.520915  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:22.522605  1669  1811 D RILJ    : [UNSL]< MTK: RIL_UNSOL_ICCID_CHANGED N/A [PHONE0]
09-29 16:20:22.523313  1251  1251 D TelephonyRegistry: notifyCellLocationForSubscriber: subId=2147483647 cellIdentity=null
09-29 16:20:22.524606  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:22.525040  1669  1811 D RILJ    : convertHalRadioCapability: session=-1, phase=3, rat=36869, logicModemUuid=modem_sys1_ps0, status=1, rcRil.raf=81930 [PHONE0]
09-29 16:20:22.525527  1669  1811 D RILJ    : [UNSL]< UNSOL_RADIO_CAPABILITY {mPhoneId = 0 mVersion=1 mSession=-1 mPhase=3 mRadioAccessFamily=36869 mLogicModemId=modem_sys1_ps0 mStatus=1} [PHONE0]
09-29 16:20:22.527158  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:22.527636  1669  1669 D ImsSwitchController: Initialize ImsSwitchController
09-29 16:20:22.530032  1669  1811 D RILJ    : [UNSL]< MTK: RIL_UNSOL_ICCID_CHANGED N/A [PHONE0]
09-29 16:20:22.531621  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:22.533277  1669  1811 D RILJ    : [UNSL]< UNSOL_HARDWARE_CONFIG_CHANGED [Modem { uuid=modem_sys1_ps0, state=0, rilModel=0, rat={0, 2, 13, 15}, maxActiveVoiceCall=1, maxActiveDataCall=1, maxStandby=1 }, Sim { uuid=modem_sys1_ps0, modemUuid=modem_sys1_ps0, state=0 }] [PHONE0]
09-29 16:20:22.537009  1669  1669 D MtkRILJ : [0012]> MTK: RIL_REQUEST_SET_VENDOR_SETTING [SUB0]
09-29 16:20:22.538331  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:22.539161  1669  1669 D RatConfig: getMaxRat: initial Lf/Lt/W/G 29
09-29 16:20:22.539523  1669  1669 D RatConfig: getActiveRatConfig: Lf/Lt/W/G
09-29 16:20:22.540833  1669  1822 I RadioManager: PowerIdleState: enter
09-29 16:20:22.541624  1669  1811 D RILJ    : [UNSL]< MTK: UNSOL_PHB_READY_NOTIFICATION phbReadyNotification: 0 [PHONE0]
09-29 16:20:22.543106  1669  1669 D TelephonyComponentFactory: makeUiccController mtk
09-29 16:20:22.543185  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:22.543438  1669  1811 D RILJ    : [UNSL]< UNSOL_VOICE_RADIO_TECH_CHANGED {1} [PHONE0]
09-29 16:20:22.546295  1669  1811 D RILJ    : [0012]< MTK: RIL_REQUEST_SET_VENDOR_SETTING  [PHONE0]
09-29 16:20:22.550640  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:22.552607  1669  1811 D RILJ    : [UNSL]< MTK: RIL_UNSOL_ICCID_CHANGED N/A [PHONE0]
09-29 16:20:22.553976  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:22.554180  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_SIM_STATUS_CHANGED [PHONE0]
09-29 16:20:22.555396  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:22.559052  1669  1811 D RILJ    : [UNSL]< MTK: RIL_UNSOL_ICCID_CHANGED N/A [PHONE0]
09-29 16:20:22.560553  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:22.560984  1669  1811 D RILJ    : [UNSL]< UNSOL_HARDWARE_CONFIG_CHANGED [Modem { uuid=modem_sys1_ps0, state=0, rilModel=0, rat={0, 2, 13, 15}, maxActiveVoiceCall=1, maxActiveDataCall=1, maxStandby=1 }, Sim { uuid=modem_sys1_ps0, modemUuid=modem_sys1_ps0, state=0 }] [PHONE0]
09-29 16:20:22.570778  1615  1725 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:22.573297  1615  1725 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:22.578281  1669  1669 D PinStorage: KeyStore: alias PinStorage_longTerm_always_key exists
09-29 16:20:22.578540  1669  1669 D PinStorage: onDeviceReady
09-29 16:20:22.585325  1669  1669 D PinStorage: KeyStore: alias PinStorage_shortTerm_key does not exist - Nothing to do
09-29 16:20:22.592865  1669  1669 I RsuSml  : [RSU-SIMLOCK] initialize RsuSml: [Lcom.android.internal.telephony.RIL;@69be150
09-29 16:20:22.597109  1669  1669 I PhoneFactory: Creating SubscriptionController
09-29 16:20:22.615134  1615  1725 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:22.616631  1615  1725 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:22.632451  1669  1669 D MtkSubscriptionControllerEx: [MtkSubscriptionControllerEx] init by Context, this = com.mediatek.internal.telephony.MtkSubscriptionControllerEx@365c27c
09-29 16:20:22.632636  1669  1669 D MtkSubscriptionControllerEx: [MtkSubscriptionControllerEx] init by Context
09-29 16:20:22.632704  1669  1669 D MtkSubscriptionControllerEx: [MtkSubscriptionControllerEx] sInstance = com.mediatek.internal.telephony.MtkSubscriptionControllerEx@365c27c
09-29 16:20:22.632821  1669  1669 D TelephonyComponentFactory: makeMultiSimSettingController mtk
09-29 16:20:22.640551  1669  1669 D MtkTelephonyManagerEx: simSwitchMode result = 3
09-29 16:20:22.641800  1669  1669 I PhoneFactory: Creating Phone with type = 1 phoneId = 0
09-29 16:20:22.642973  1669  1669 D TelephonyTester: register for intent action=com.mediatek.internal.telephony.action_detached
09-29 16:20:22.643177  1669  1669 D TelephonyTester: register for intent action=com.mediatek.internal.telephony.action_attached
09-29 16:20:22.643230  1669  1669 D TelephonyTester: register for intent action=com.android.internal.telephony.TestServiceState
09-29 16:20:22.643268  1669  1669 D TelephonyTester: register for intent action=com.android.internal.telephony.TestChangeNumber
09-29 16:20:22.668093  1669  1669 D GsmCdmaCallTkr: Reset mWaitForHoldToRedialRequest variables
09-29 16:20:22.668285  1669  1669 D GsmCdmaCallTkr: Reset mWaitForHoldToHangupRequest variables
09-29 16:20:22.668404  1669  1669 D TelephonyComponentFactory: makeIccPhoneBookInterfaceManager mtk
09-29 16:20:22.668983  1669  1669 D SmsDispatchersController: SmsDispatchersController created
09-29 16:20:22.672008  1669  1669 D SMSDispatcher: SMSDispatcher: ctor mSmsCapable=true format=unknown mSmsSendDisabled=false
09-29 16:20:22.672768  1669  1669 D MtkImsSmsDispacher: Created!
09-29 16:20:22.675586  1669  1669 D SMSDispatcher: SMSDispatcher: ctor mSmsCapable=true format=3gpp2 mSmsSendDisabled=false
09-29 16:20:22.675808  1669  1669 D CdmaSMSDispatcher: CdmaSMSDispatcher created
09-29 16:20:22.675882  1669  1669 D MtkCdmaSMSDispatcher: MtkCdmaSMSDispatcher created
09-29 16:20:22.678319  1669  1669 E WAP PUSH: bindService() for wappush manager failed
09-29 16:20:22.680737  1669  1669 D m.android.phon: created InboundSmsHandler
09-29 16:20:22.696422  1669  1669 D MtkGsmInboundSmsHandler-0: created InboundSmsHandler from MtkGsmInboundSmsHandler
09-29 16:20:22.696791  1669  1830 D MtkGsmInboundSmsHandler-0: StartupState.enter: entering StartupState
09-29 16:20:22.699188  1669  1669 E WAP PUSH: bindService() for wappush manager failed
09-29 16:20:22.701324  1669  1669 D m.android.phon: created InboundSmsHandler
09-29 16:20:22.707979  1669  1831 D MtkCdmaInboundSmsHandler-0: StartupState.enter: entering StartupState
09-29 16:20:22.709316  1669  1669 D SMSDispatcher: SMSDispatcher: ctor mSmsCapable=true format=3gpp mSmsSendDisabled=false
09-29 16:20:22.709579  1669  1669 D GsmSMSDispatcher: GsmSMSDispatcher created
09-29 16:20:22.709752  1669  1669 D MtkGsmSMSDispatcher: MtkGsmSMSDispatcher created
09-29 16:20:22.709854  1669  1669 D MtkSmsBroadcastUndelivered:  call initialize
09-29 16:20:22.711746  1669  1831 D MtkCdmaInboundSmsHandler-0: StartupState.processMessage: processing EVENT_START_ACCEPTING_SMS
09-29 16:20:22.711829  1669  1830 D MtkGsmInboundSmsHandler-0: StartupState.processMessage: processing EVENT_START_ACCEPTING_SMS
09-29 16:20:22.711855  1669  1831 D MtkCdmaInboundSmsHandler-0: IdleState.enter: entering IdleState
09-29 16:20:22.711874  1669  1830 D MtkGsmInboundSmsHandler-0: IdleState.enter: entering IdleState
09-29 16:20:22.711946  1669  1831 D MtkCdmaInboundSmsHandler-0: IdleState.processMessage: processing EVENT_RELEASE_WAKELOCK
09-29 16:20:22.711999  1669  1830 D MtkGsmInboundSmsHandler-0: IdleState.processMessage: processing EVENT_RELEASE_WAKELOCK
09-29 16:20:22.713016  1669  1831 D MtkCdmaInboundSmsHandler-0: IdleState.processMessage: EVENT_RELEASE_WAKELOCK: mWakeLock released
09-29 16:20:22.715188  1669  1669 D MtkSmsDispatchersController: MtkSmsDispatchersController created
09-29 16:20:22.716299  1669  1830 D MtkGsmInboundSmsHandler-0: IdleState.processMessage: EVENT_RELEASE_WAKELOCK: mWakeLock released
09-29 16:20:22.717749  1669  1669 D CdmaSSM : subscriptionSource from settings: 0
09-29 16:20:22.717954  1669  1669 D CdmaSSM : cdmaSSM constructor: 0
09-29 16:20:22.721252  1669  1669 D RILJ    : setPhoneType=1 old value=0 [PHONE0]
09-29 16:20:22.724633  1669  1669 D CarrierActionAgent: [0]Creating CarrierActionAgent
09-29 16:20:22.725555  1669  1669 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:22.727089  1669  1669 D TransportManager-0: operates in AP-assisted mode.
09-29 16:20:22.734878  1669  1669 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:22.735207  1669  1669 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.android.phone listener=com.android.internal.telephony.ServiceStateTracker$SstSubscriptionsChangedListener@6930ae3
09-29 16:20:22.736891  1251  1809 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:22.739299  1669  1669 D NRM-C-0 : registerForNetworkRegistrationInfoChanged
09-29 16:20:22.741548  1669  1669 D NRM-I-0 : registerForNetworkRegistrationInfoChanged
09-29 16:20:22.745788  1669  1669 D NewNitzStateMachineImpl: handleNetworkUnavailable(): mLatestNitzSignal was already null. Nothing to do.
09-29 16:20:22.750064  1669  1669 D RILJ    : [0020]> SIGNAL_STRENGTH [PHONE0]
09-29 16:20:22.750564  1669  1669 D MTKSST  : [GsmSST0] notifyVoiceRegStateRilRadioTechnologyChanged: vrs=1 rat=0
09-29 16:20:22.753679  1669  1669 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.android.phone listener=com.android.internal.telephony.CarrierServiceStateTracker$1@f84f35b
09-29 16:20:22.754592  1251  1809 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:22.755032  1669  1811 D RILJ    : [0020]< SIGNAL_STRENGTH SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=2147483647 ber=2147483647 rscp=2147483647 ecno=2147483647 level=0,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthLte} [PHONE0]
09-29 16:20:22.758409  1669  1669 D PlusCodeProcessor: makePlusCodeUtis Exception, return default DefaultPlusCodeUtilsjava.lang.ClassNotFoundException: Didn't find class "com.mediatek.internal.telephony.cdma.pluscode.CdmaPlusCodeUtils" on path: DexPathList[[],nativeLibraryDirectories=[/system/lib64, /system/system_ext/lib64]]
09-29 16:20:22.758731  1669  1669 D PlusCodeProcessor: getPlusCodeUtils sPlusCodeUtilsInstance=com.mediatek.internal.telephony.cdma.pluscode.DefaultPlusCodeUtils@12387f8
09-29 16:20:22.761885  1669  1833 D MTKSST  : [GsmSST0] MtkHandler: EVENT_RIL_READY
09-29 16:20:22.762237  1669  1833 D MTKSST  : [GsmSST0] MtkHandler: EVENT_NETWORK_STATE_CHANGED
09-29 16:20:22.764599  1669  1669 D NrMap-0 : SIM not ready, use default carrier config.
09-29 16:20:22.764856  1669  1833 D RILJ    : [0021]> OPERATOR [PHONE0]
09-29 16:20:22.764973  1669  1669 D NrMap-0 : gps.nfw_proxy_apps: com.mediatek.gnss.nonframeworklbs
09-29 16:20:22.765171  1669  1669 D NrMap-0 : mGnssProxyPackageName from carrierConfig: com.mediatek.gnss.nonframeworklbs
09-29 16:20:22.765331  1669  1669 D NrMap-0 : swtichNrMap=false listening=false
09-29 16:20:22.766112  1176  1202 I AT      : [0] AT> AT+EOPS? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:22.766736  1669  1833 D RILJ    : [0022]> DATA_REGISTRATION_STATE [PHONE0]
09-29 16:20:22.767212  1669  1833 D RILJ    : getDataRegistrationState: overrideHalVersion=null [PHONE0]
09-29 16:20:22.768694  1669  1833 D RILJ    : [0023]> VOICE_REGISTRATION_STATE [PHONE0]
09-29 16:20:22.768890  1669  1833 D RILJ    : getVoiceRegistrationState: overrideHalVersion=null [PHONE0]
09-29 16:20:22.770260  1669  1833 D RILJ    : [0024]> SIGNAL_STRENGTH [PHONE0]
09-29 16:20:22.772497  1669  1669 D NrMap-0 : loadCityFromXml.onPreExecute: system_ext/etc/nr-city.xml
09-29 16:20:22.772950  1669  1811 D RILJ    : [0024]< SIGNAL_STRENGTH SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=2147483647 ber=2147483647 rscp=2147483647 ecno=2147483647 level=0,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthLte} [PHONE0]
09-29 16:20:22.773325  1669  1669 D NrMap-0 : notify MD about NR city 2
09-29 16:20:22.773463  1669  1833 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:22.773868  1176  1201 I AT      : [0] AT< +EOPS: 0,2,"",1 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:22.773931  1176  1201 I AT      : [0] AT< OK (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:22.774308  1176  1202 I AT      : [0] AT> AT+E5GOPT? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:22.774508  1669  1833 D MTKSST  : [GsmSST0] notifyMtkSignalStrength level:0 raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=2147483647 ber=2147483647 rscp=2147483647 ecno=2147483647 level=0,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthLte}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null
09-29 16:20:22.774766  1669  1669 D MtkRILJ : [0025]> OEM_HOOK_RAW[41542B45474D433D312C2235675F617661696C61626C65222C32] [SUB0]
09-29 16:20:22.774995  1669  1811 D RILJ    : [0021]< OPERATOR {, , } [PHONE0]
09-29 16:20:22.776004  1176  1182 D RpOemCtlr: onHandleOemHookRaw, data = AT+EGMC=1,"5g_available",2
09-29 16:20:22.776459  1176  1192 I AT      : [0] AT> AT+EGMC=1,"5g_available",2 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:22.777189  1251  1270 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:22.778341  1669  1669 D NrMap-0 : proxyApp = com.mediatek.gnss.nonframeworklbs proxyAppLocationGranted = false
09-29 16:20:22.778510  1669  1669 D NrMap-0 : NrMap set=0 permission=false
09-29 16:20:22.779126  1669  1669 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:22.779311  1669  1835 D NrMap-0 : [0]Record(/Beijing/cn)
09-29 16:20:22.780780  1669  1835 D NrMap-0 : findByCityName Record[0] _id=1, mccmnc=, iso=cn, country_name=beijing
09-29 16:20:22.782065  1669  1669 D EmergencyNumberTracker:  asset emergency database is loaded. Ver: 2 Phone Id: 0
09-29 16:20:22.782272  1176  1201 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:22.783272  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:22.783425  1176  1192 E RmcOemHandler: [0] OEM_HOOK_RAW fail
09-29 16:20:22.783638  1176  1192 D RmcNwReqHdlr: [0] [currentPhysicalChannelConfigs] needNotifyEmpty and has notified empty list, return
09-29 16:20:22.784254  1669  1811 D RILJ    : [0022]< DATA_REGISTRATION_STATE {.regState = NOT_REG_MT_NOT_SEARCHING_OP, .rat = UNKNOWN, .reasonForDenial = NONE, .cellIdentity = {.noinit = {}}, .registeredPlmn = , .accessTechnologySpecificInfo = {.noinit = {}}} [PHONE0]
09-29 16:20:22.784767  1669  1669 E EmergencyNumberTracker: Cache ota emergency database IOException: java.io.FileNotFoundException: /data/misc/emergencynumberdb/emergency_number_db: open failed: ENOENT (No such file or directory)
09-29 16:20:22.784819  1669  1669 D EmergencyNumberTracker: Using Asset Emergency database. Version: 2
09-29 16:20:22.784901  1669  1811 D RILJ    : [0025]< OEM_HOOK_RAW error 2 [PHONE0]
09-29 16:20:22.785018  1669  1811 D RilRequest: [0025]< OEM_HOOK_RAW error: com.android.internal.telephony.CommandException: GENERIC_FAILURE ret= result={ when=-31s605ms what=101 target=com.mediatek.internal.telephony.NrMap$MtkHandler }
09-29 16:20:22.785172  1669  1669 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.android.phone listener=com.android.internal.telephony.dataconnection.DataEnabledSettings$1@f3b5e10
09-29 16:20:22.785644  1669  1811 D RILJ    : [0023]< VOICE_REGISTRATION_STATE {.regState = NOT_REG_MT_NOT_SEARCHING_OP, .rat = UNKNOWN, .reasonForDenial = NONE, .cellIdentity = {.noinit = {}}, .registeredPlmn = , .accessTechnologySpecificInfo = {.noinit = {}}} [PHONE0]
09-29 16:20:22.785940  1251  1809 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:22.797147  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:22.811612  1669  1669 D MtkDeviceStateMonitor: [phoneId0]Initialize MtkDeviceStateMonitor
09-29 16:20:22.811740  1669  1669 D MtkDeviceStateMonitor: [phoneId0]isLowDataExpected mIsScreenOn = true mIsCharging = true mIsTetheringOn = false
09-29 16:20:22.823818  1669  1669 D DcTesterDeacativateAll: register for intent action=com.android.internal.telephony.dataconnection.action_deactivate_all
09-29 16:20:22.823923  1669  1669 D DcTesterDeacativateAll: register for intent action=com.mediatek.internal.telephony.action_detached
09-29 16:20:22.825323  1669  1669 D DcTesterFailBrinupAll: register for intent action=com.android.internal.telephony.dataconnection.action_fail_bringup
09-29 16:20:22.825424  1669  1669 D DcTesterFailBrinupAll: register for intent action=com.mediatek.internal.telephony.action_detached
09-29 16:20:22.825459  1669  1669 D DcTesterFailBrinupAll: register for intent action=com.mediatek.internal.telephony.action_attached
09-29 16:20:22.828476  1669  1669 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:22.829056  1669  1669 W ApnConfigTypeRepository: carrier config is null
09-29 16:20:22.833443  1251  1269 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WWAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, xcap, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.836758  1251  1269 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WWAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, ia, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.839301  1251  1269 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WWAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, cbs, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.841861  1251  1269 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WWAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, mcx, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.844562  1251  1269 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WWAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, enterprise, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.848670  1251  1517 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WWAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, ims, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.851376  1251  1517 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WWAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, emergency, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.854061  1251  1809 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WWAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, rcs, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.856660  1251  1809 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WWAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, bip, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.859196  1251  1809 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WWAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, vsim, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.861402  1251  1809 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WWAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, mms, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.863906  1251  1517 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WWAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, supl, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.866496  1251  1517 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WWAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, dun, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.867839  1251  1517 D TelephonyRegistry: onDataConnectionStateChanged(DISCONNECTED, UNKNOWN) subId=-1, phoneId=0
09-29 16:20:22.868121  1251  1517 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:22.869776  1251  1517 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WWAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, hipri, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.873557  1251  1517 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WWAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, hipri | default, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.876197  1251  1809 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WWAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, fota, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.882289  1669  1669 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.android.phone listener=com.mediatek.internal.telephony.dataconnection.MtkDcTracker$DctOnSubscriptionsChangedListener@e13d6b3
09-29 16:20:22.883234  1251  1809 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:22.891852  1669  1669 D DcTesterDeacativateAll: register for intent action=com.android.internal.telephony.dataconnection.action_deactivate_all
09-29 16:20:22.891957  1669  1669 D DcTesterDeacativateAll: register for intent action=com.mediatek.internal.telephony.action_detached
09-29 16:20:22.893223  1669  1669 D DcTesterFailBrinupAll: register for intent action=com.android.internal.telephony.dataconnection.action_fail_bringup
09-29 16:20:22.893339  1669  1669 D DcTesterFailBrinupAll: register for intent action=com.mediatek.internal.telephony.action_detached
09-29 16:20:22.893374  1669  1669 D DcTesterFailBrinupAll: register for intent action=com.mediatek.internal.telephony.action_attached
09-29 16:20:22.896441  1669  1669 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:22.896886  1669  1669 W ApnConfigTypeRepository: carrier config is null
09-29 16:20:22.899315  1251  1809 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WLAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, xcap, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.902016  1251  1809 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WLAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, ia, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.904541  1251  1809 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WLAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, cbs, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.907216  1251  1517 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WLAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, mcx, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.909892  1251  1809 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WLAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, enterprise, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.913758  1251  1809 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WLAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, ims, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.916214  1251  1517 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WLAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, emergency, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.918705  1251  1269 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WLAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, rcs, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.921302  1251  1269 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WLAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, bip, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.923764  1251  1809 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WLAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, vsim, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.926173  1251  1809 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WLAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, mms, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.929116  1251  1809 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WLAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, supl, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.931742  1251  1809 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WLAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, dun, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.934539  1251  1269 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WLAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, hipri, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.938330  1251  1517 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WLAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, hipri | default, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.940922  1251  1517 D TelephonyRegistry: notifyDataConnectionForSubscriber: phoneId=0 subId=-1  state: DISCONNECTED, transport: WLAN, id: -1, network type: UNKNOWN, APN Setting: [ApnSettingV7] null, 0, null, null, null, null, null, null, null, 0, fota, null, null, false, 0, false, 0, 0, 0, 0, null, null, false, 0, 0, -1, -1, link properties: null, fail cause: NONE
09-29 16:20:22.945109  1669  1669 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.android.phone listener=com.mediatek.internal.telephony.dataconnection.MtkDcTracker$DctOnSubscriptionsChangedListener@9d61746
09-29 16:20:22.945817  1251  1269 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:22.946274  1669  1669 D CarrierResolver: Creating CarrierResolver[0]
09-29 16:20:22.949677  1669  1669 D MTKSST  : [GsmSST0] notifyVoiceRegStateRilRadioTechnologyChanged: vrs=1 rat=0
09-29 16:20:22.967754  1669  1669 I GsmCdmaPhone: [0] updateTtyMode ttyMode=0
09-29 16:20:22.970357  1669  1669 D RILJ    : [0026]> SET_TTY_MODE ttyMode = 0 [PHONE0]
09-29 16:20:22.972626  1176  1182 D RtcCC   : [0] updateRQ() : RQ   = 0
09-29 16:20:22.973060  1176  1194 D RmcCCReqHandler: [0] onHandleRequest: RFX_MSG_REQUEST_SET_TTY_MODE
09-29 16:20:22.973153  1176  1194 I AT      : [0] AT> AT+CTMCALL=0 (RIL_CMD_READER_2 tid:493437472000)
09-29 16:20:22.973350  1669  1669 I GsmCdmaPhone: [0] updateUiTtyMode ttyMode=0
09-29 16:20:22.973596  1669  1669 D CallManager: registerPhone(GSM Handler (com.mediatek.internal.telephony.MtkGsmCdmaPhone) {f245017})
09-29 16:20:22.973939  1669  1669 D MtkGsmCdmaPhone: constructor: sub = 0
09-29 16:20:22.974695  1669  1669 D FeatureConnector: [InstanceManager, 0] imsFeatureRemoved: reason=3
09-29 16:20:22.976191  1669  1669 D SelfActivationDefault: init
09-29 16:20:22.976899  1669  1669 D CpaDct  : [CpaDct]makeCpaDcTracker: X sCpaDcTracker=Handler (com.mediatek.internal.telephony.dataconnection.CpaDcTracker) {2cc61d2}
09-29 16:20:22.978327  1669  1669 D RILJ    : [0027]> VOICE_RADIO_TECH [PHONE0]
09-29 16:20:22.980570  1176  1193 I AT      : [0] AT< OK (RIL_CMD_READER_2, tid:493438508288)
09-29 16:20:22.981113  1669  1811 D RILJ    : [0027]< VOICE_RADIO_TECH {1} [PHONE0]
09-29 16:20:22.982771  1669  1811 D RILJ    : [0026]< SET_TTY_MODE  [PHONE0]
09-29 16:20:23.008648  1669  1669 I PhoneFactory: defaultSmsApplication: com.google.android.apps.messaging
09-29 16:20:23.016543  1669  1669 I PhoneFactory: Creating SubInfoRecordUpdater 
09-29 16:20:23.017641  1669  1669 D SubscriptionInfoUpdater: Constructor invoked
09-29 16:20:23.028888  1669  1669 D MtkSubscriptionInfoUpdater: MtkSubscriptionInfoUpdater created
09-29 16:20:23.031637  1669  1669 D SuppServManager: Create MtkSuppServManager singleton instance, phones.length = 1
09-29 16:20:23.031906  1669  1669 D SuppServManager: Initialize MtkSuppServManager!
09-29 16:20:23.034791  1669  1669 D MtkImsManager [0]: createMtkImsService binder is null
09-29 16:20:23.035513  1669  1669 D FeatureConnector: [MtkSuppServHelper, 0] imsFeatureRemoved: reason=3
09-29 16:20:23.036985  1669  1669 D MtkRILJ : call registerForCallForwardingInfo, Handler : Handler (com.mediatek.internal.telephony.MtkSuppServHelper) {d1decb8}
09-29 16:20:23.037777  1669  1844 D MtkSuppServHelper: [0]unSetImsCallback
09-29 16:20:23.039539  1669  1669 D MtkSuppServHelper: [0]MtkSuppServHelper init done.
09-29 16:20:23.039926  1669  1669 I SuppServConf: [0]MtkSuppServConf constructor.
09-29 16:20:23.040085  1669  1669 I SuppServConf: [0]MtkSuppServConf init.
09-29 16:20:23.040549  1669  1669 I SuppServConf: [0]initConfig start.
09-29 16:20:23.040694  1669  1669 I SuppServConf: [0]initConfig end.
09-29 16:20:23.042290  1669  1844 D SuppServConf: [0]handleMessage msg: EVENT_ICC_CHANGED
09-29 16:20:23.042487  1669  1669 D SmartDataSwitch:  is created
09-29 16:20:23.042692  1669  1669 D SmartDataSwitch: registerEvents
09-29 16:20:23.042997  1669  1844 D SuppServConf: [0]handleMessage msg: EVENT_INIT
09-29 16:20:23.043165  1669  1669 D SmartDataSwitchOpExt: init()
09-29 16:20:23.043290  1669  1669 D SmartDataSwitch: init done
09-29 16:20:23.043357  1669  1844 I SuppServConf: [0]resetConfig start.
09-29 16:20:23.043450  1669  1669 D SmartDataSwitch: makeSDSA: X sSDSA =Handler (com.mediatek.internal.telephony.datasub.SmartDataSwitchAssistant) {372b0a6}
09-29 16:20:23.043519  1669  1844 I SuppServConf: [0]resetConfig end.
09-29 16:20:23.043887  1669  1669 D DcHelper: makeMtkDcHelper: phones.length=1
09-29 16:20:23.044051  1669  1669 D DcHelper: registerEvents
09-29 16:20:23.044160  1669  1844 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:23.044282  1669  1844 D SuppServConf: [0]Config is null.
09-29 16:20:23.044374  1669  1844 I SuppServConf: [0]NEED_CHECK_DATA_ROAMING -> bValue: false, sValue: , iValue: -1
09-29 16:20:23.044441  1669  1844 I SuppServConf: [0]TBCLIR -> bValue: false, sValue: , iValue: -1
09-29 16:20:23.044491  1669  1844 I SuppServConf: [0]RE_REGISTER_FOR_CF -> bValue: false, sValue: , iValue: -1
09-29 16:20:23.044540  1669  1844 I SuppServConf: [0]SUPPORT_SAVE_CF_NUMBER -> bValue: false, sValue: , iValue: -1
09-29 16:20:23.044589  1669  1844 I SuppServConf: [0]TRANSFER_XCAP_404 -> bValue: false, sValue: , iValue: -1
09-29 16:20:23.044637  1669  1844 I SuppServConf: [0]NEED_CHECK_IMS_WHEN_ROAMING -> bValue: false, sValue: , iValue: -1
09-29 16:20:23.044686  1669  1844 I SuppServConf: [0]NOT_SUPPORT_XCAP -> bValue: false, sValue: , iValue: -1
09-29 16:20:23.044746  1669  1844 I SuppServConf: [0]NOT_SUPPORT_OCB -> bValue: false, sValue: , iValue: -1
09-29 16:20:23.044794  1669  1844 I SuppServConf: [0]GSM_UT_SUPPORT -> bValue: false, sValue: , iValue: -1
09-29 16:20:23.044841  1669  1844 I SuppServConf: [0]ENABLE_XCAP_HTTP_RESPONSE_409 -> bValue: false, sValue: , iValue: -1
09-29 16:20:23.044889  1669  1844 I SuppServConf: [0]QUERY_CFU_AGAIN_AFTER_SET -> bValue: false, sValue: , iValue: -1
09-29 16:20:23.044936  1669  1844 I SuppServConf: [0]NOT_SUPPORT_CALL_IDENTITY -> bValue: false, sValue: , iValue: -1
09-29 16:20:23.044983  1669  1844 I SuppServConf: [0]NEED_CHECK_DATA_ENABLE -> bValue: false, sValue: , iValue: -1
09-29 16:20:23.045040  1669  1844 I SuppServConf: [0]IMS_NW_CW -> bValue: false, sValue: , iValue: -1
09-29 16:20:23.045088  1669  1844 I SuppServConf: [0]NOT_SUPPORT_WFC_UT -> bValue: false, sValue: , iValue: -1
09-29 16:20:23.045427  1669  1669 D DcHelper: registered phone change event.
09-29 16:20:23.045593  1669  1669 D DcHelper: makesMtkDcHelper: X sMtkDcHelper =com.mediatek.internal.telephony.dataconnection.MtkDcHelper@e893132
09-29 16:20:23.047127  1669  1669 D TelephonyComponentFactory: not found VoData library
09-29 16:20:23.048216  1669  1669 D TelephonyTester: register for intent action=com.mediatek.internal.telephony.imsphone.action_detached
09-29 16:20:23.048480  1669  1669 D TelephonyTester: register for intent action=com.mediatek.internal.telephony.imsphone.action_attached
09-29 16:20:23.048571  1669  1669 D TelephonyTester: register for intent action=com.android.internal.telephony.TestConferenceEventPackage
09-29 16:20:23.048693  1669  1669 D TelephonyTester: register for intent action=com.android.internal.telephony.TestServiceState
09-29 16:20:23.048739  1669  1669 D TelephonyTester: register for intent action=com.android.internal.telephony.TestChangeNumber
09-29 16:20:23.067815  1669  1669 E ImsPhoneCallTracker: [0] cacheCarrierConfiguration: No carrier config service found or not active subId = -1
09-29 16:20:23.068830  1669  1669 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:23.069076  1669  1669 E ImsPhoneCallTracker: [0] updateCarrierConfiguration: Empty carrier config.
09-29 16:20:23.077059  1669  1669 D ImsPhoneCallTracker: [0] registerIndicationReceiver
09-29 16:20:23.083023  1669  1669 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.android.phone listener=com.mediatek.internal.telephony.imsphone.MtkImsPhoneCallTracker$1@7a88ef5
09-29 16:20:23.084033  1251  1517 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:23.084974  1669  1669 D RttEmcGuardTimerUtil: initRttEmcGuardTimer
09-29 16:20:23.087036  1669  1669 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:23.088646  1669  1669 D CallManager: registerPhone(MtkImsPhone Handler (com.mediatek.internal.telephony.imsphone.MtkImsPhone) {75d5800})
09-29 16:20:23.088971  1669  1669 D DcHelper: registerImsEvents, phoneId = 0
09-29 16:20:23.090661  1669  1669 D MtkPhoneSwitcher: MtkPhoneSwitcher mtkMake
09-29 16:20:23.093554  1669  1669 D FeatureConnector: [InstanceManager, 0] imsFeatureRemoved: reason=3
09-29 16:20:23.095647  1251  1809 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:23.102399  1669  1669 D MtkPhoneSwitcher: updateHalCommandToUse
09-29 16:20:23.102443  1669  1669 D PhoneSwitcher: PhoneSwitcher started
09-29 16:20:23.102591  1669  1669 D MtkPhoneSwitcher: getSimLockPolicy:0
09-29 16:20:23.107400  1669  1669 D MtkProxyController: Constructor - Enter, rild mode = 2
09-29 16:20:23.112116  1669  1669 D MtkProxyController: Constructor - Exit
09-29 16:20:23.118741  1669  1669 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.android.phone listener=com.android.internal.telephony.dataconnection.TelephonyNetworkFactory$1@b0a9cc4
09-29 16:20:23.119573  1251  1517 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:23.120081  1669  1669 D TelephonyNetworkFactory[0]: Registering NetworkFactory
09-29 16:20:23.121737  1669  1669 D TelephonyComponentFactory: Creating CarrierExpress
09-29 16:20:23.132997  1669  1669 W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
09-29 16:20:23.133549  1669  1669 D RcsProvisioningMonitor: RcsProvisioningMonitor created.
09-29 16:20:23.136130  1669  1669 D RcsProvisioningMonitor: init.
09-29 16:20:23.137969  1251  1809 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:23.158546  1669  1669 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.android.phone listener=com.android.phone.CallNotifier$1@170b719
09-29 16:20:23.159352  1251  1269 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:23.159913  1669  1669 D CallManager: registerForMmiComplete
09-29 16:20:23.161057  1669  1669 D NewNitzStateMachineImpl: handleAirplaneModeChanged(false): mLatestNitzSignal was already null. Nothing to do.
09-29 16:20:23.166388  1669  1669 D NewNitzStateMachineImpl: handleAirplaneModeChanged(false): mLatestNitzSignal was already null. Nothing to do.
09-29 16:20:23.180416  1669  1669 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.android.phone listener=com.android.services.telephony.TelecomAccountRegistry$1@c6b1178
09-29 16:20:23.181101  1251  1270 D TelephonyRegistry: listen oscl: mHasNotifySubscriptionInfoChangedOccurred==false no callback
09-29 16:20:23.192576  1669  1669 D TDC     : handleMessage: received EVENT_HARDWARE_CONFIG_CHANGED
09-29 16:20:23.192918  1669  1669 D TDC     : updateOrInsert: inserting: Modem { uuid=modem_sys1_ps0, state=0, rilModel=0, rat={}, maxActiveVoiceCall=1, maxActiveDataCall=1, maxStandby=1 }
09-29 16:20:23.193019  1669  1669 D TDC     : updateOrInsert: inserting: Sim { uuid=modem_sys1_ps0, modemUuid=modem_sys1_ps0, state=0 }
09-29 16:20:23.193745  1669  1669 I RadioManager: sendEvent: EVENT_RADIO_AVAILABLE
09-29 16:20:23.194193  1669  1822 I RadioManager: processMessage: EVENT_RADIO_AVAILABLE
09-29 16:20:23.197924  1669  1669 D RILJ    : [0028]> GET_SIM_STATUS [PHONE0]
09-29 16:20:23.198439  1669  1669 D RadioConfig: [0029]> GET_SLOT_STATUS
09-29 16:20:23.198980  1176  1176 D RadioConfig_service: radioConfig::getSimSlotsStatus 
09-29 16:20:23.199337  1176  1202 I AT      : [0] AT> AT+CPIN? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:23.199893  1176  1182 D RtcRadioConfig: [-1] onHandleRequest, slot id = 0
09-29 16:20:23.201900  1669  1669 D RILJ    : [0030]> GET_SIM_STATUS [PHONE0]
09-29 16:20:23.202392  1669  1669 D TDC     : handleMessage: received EVENT_HARDWARE_CONFIG_CHANGED
09-29 16:20:23.202704  1669  1669 D TDC     : updateOrInsert: removing: Modem { uuid=modem_sys1_ps0, state=0, rilModel=0, rat={}, maxActiveVoiceCall=1, maxActiveDataCall=1, maxStandby=1 }
09-29 16:20:23.202834  1669  1669 D TDC     : updateOrInsert: inserting: Modem { uuid=modem_sys1_ps0, state=0, rilModel=0, rat={}, maxActiveVoiceCall=1, maxActiveDataCall=1, maxStandby=1 }
09-29 16:20:23.202939  1669  1669 D TDC     : updateOrInsert: removing: Sim { uuid=modem_sys1_ps0, modemUuid=modem_sys1_ps0, state=0 }
09-29 16:20:23.202996  1669  1669 D TDC     : updateOrInsert: inserting: Sim { uuid=modem_sys1_ps0, modemUuid=modem_sys1_ps0, state=0 }
09-29 16:20:23.204912  1669  1669 D RILJ    : [0031]> GET_SIM_STATUS [PHONE0]
09-29 16:20:23.205385  1669  1669 D RadioConfig: [0032]> GET_SLOT_STATUS
09-29 16:20:23.205761  1176  1176 D RadioConfig_service: radioConfig::getSimSlotsStatus 
09-29 16:20:23.206221  1669  1669 D MtkGsmCdmaPhone: EVENT_ICC_CHANGED, phone id = 0, result = null
09-29 16:20:23.206646  1176  1182 D RtcRadioConfig: [-1] onHandleRequest, slot id = 0
09-29 16:20:23.206756  1669  1669 E GsmCdmaPhone: [0] reapplyUiccAppsEnablementIfNeeded(), slot is null ,mUiccApplicationsEnabled = null
09-29 16:20:23.207244  1176  1201 I AT      : [0] AT< +CME ERROR: 10 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:23.207496  1176  1202 I AT      : [0] AT> AT+ESLOTSINFO? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:23.207851  1669  1669 D MtkGsmCdmaPhone: isPhoneTypeCdmaLte:false, phoneId: 0 isCdmaWithoutLteCard: false mNewVoiceTech: -1
09-29 16:20:23.215753  1176  1201 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:23.229657  1176  1202 I AT      : [0] AT> AT+ESLOTSINFO? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:23.230345  1176  1182 I RtcImsConfigController: [0] onSimStateChanged, simState = 1
09-29 16:20:23.230663  1176  1182 I RtcImsConfigController: [0] DIMS setImsResourceCapability, volte:1, vilte:1, wfc:0, vonr:0, vinr:0
09-29 16:20:23.231360  1176  1182 E RILC    : imsCfgDynamicImsSwitchCompleteInd: mtkRadioExService[4]->mRadioIndicationIms == NULL
09-29 16:20:23.233778  1669  1811 D RILJ    : responseIccCardStatus: from HIDL: IccCardState {CARDSTATE_ABSENT,PINSTATE_UNKNOWN,num_apps=0,gsm_id=-1,cdma_id=-1,ims_id=-1,physical_slot_id=0,atr=,iccid=,eid=} [PHONE0]
09-29 16:20:23.234258  1669  1811 D RILJ    : [0028]< GET_SIM_STATUS IccCardState {CARDSTATE_ABSENT,PINSTATE_UNKNOWN,num_apps=0,gsm_id=-1,cdma_id=-1,ims_id=-1,physical_slot_id=0,atr=,iccid=,eid=} [PHONE0]
09-29 16:20:23.244694  1176  1201 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:23.245266  1176  1202 E RmcCommSimReq: [0] handleGetSlotStatus error!, pp_slot_status = 0x0
09-29 16:20:23.245684  1176  1202 I AT      : [0] AT> AT+CPIN? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:23.246285  1176  1182 D RadioConfig_service: getSimSlotsStatusResponse: response
09-29 16:20:23.246337  1176  1182 D RadioConfig_service: radioConfigService ->mRadioConfigResponseV1_2 != NULL
09-29 16:20:23.246347  1176  1182 E RadioConfig_service: getSimSlotsStatusResponse: Invalid response
09-29 16:20:23.247026  1669  1811 D RilRequest: [0029]< GET_SLOT_STATUS error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=[] result={ when=-32s67ms what=4 obj=0 target=com.mediatek.internal.telephony.uicc.MtkUiccController }
09-29 16:20:23.247219  1669  1811 E RadioConfigResponse: [0029]< GET_SLOT_STATUS error 6
09-29 16:20:23.253232  1176  1201 I AT      : [0] AT< +CME ERROR: 10 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:23.253442  1176  1202 I AT      : [0] AT> AT+ESLOTSINFO? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:23.260821  1176  1201 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:23.277440  1176  1202 I AT      : [0] AT> AT+CPIN? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:23.278107  1669  1811 D RILJ    : responseIccCardStatus: from HIDL: IccCardState {CARDSTATE_ABSENT,PINSTATE_UNKNOWN,num_apps=0,gsm_id=-1,cdma_id=-1,ims_id=-1,physical_slot_id=0,atr=,iccid=,eid=} [PHONE0]
09-29 16:20:23.278313  1669  1811 D RILJ    : [0030]< GET_SIM_STATUS IccCardState {CARDSTATE_ABSENT,PINSTATE_UNKNOWN,num_apps=0,gsm_id=-1,cdma_id=-1,ims_id=-1,physical_slot_id=0,atr=,iccid=,eid=} [PHONE0]
09-29 16:20:23.285563  1176  1201 I AT      : [0] AT< +CME ERROR: 10 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:23.285772  1176  1202 I AT      : [0] AT> AT+ESLOTSINFO? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:23.294283  1176  1201 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:23.314094  1176  1202 I AT      : [0] AT> AT+ESLOTSINFO? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:23.314769  1669  1811 D RILJ    : responseIccCardStatus: from HIDL: IccCardState {CARDSTATE_ABSENT,PINSTATE_UNKNOWN,num_apps=0,gsm_id=-1,cdma_id=-1,ims_id=-1,physical_slot_id=0,atr=,iccid=,eid=} [PHONE0]
09-29 16:20:23.314974  1669  1811 D RILJ    : [0031]< GET_SIM_STATUS IccCardState {CARDSTATE_ABSENT,PINSTATE_UNKNOWN,num_apps=0,gsm_id=-1,cdma_id=-1,ims_id=-1,physical_slot_id=0,atr=,iccid=,eid=} [PHONE0]
09-29 16:20:23.321597  1176  1201 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:23.321840  1176  1202 E RmcCommSimReq: [0] handleGetSlotStatus error!, pp_slot_status = 0x0
09-29 16:20:23.322161  1176  1182 D RadioConfig_service: getSimSlotsStatusResponse: response
09-29 16:20:23.322195  1176  1182 D RadioConfig_service: radioConfigService ->mRadioConfigResponseV1_2 != NULL
09-29 16:20:23.322206  1176  1182 E RadioConfig_service: getSimSlotsStatusResponse: Invalid response
09-29 16:20:23.322688  1669  1811 D RilRequest: [0032]< GET_SLOT_STATUS error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=[] result={ when=-32s142ms what=4 obj=0 target=com.mediatek.internal.telephony.uicc.MtkUiccController }
09-29 16:20:23.322951  1669  1811 E RadioConfigResponse: [0032]< GET_SLOT_STATUS error 6
09-29 16:20:23.375388  1669  1669 D GsmCdmaCallTkr: Receives EVENT_RADIO_OFF_OR_NOT_AVAILABLE
09-29 16:20:23.375576  1669  1669 D GsmCdmaCallTracker: [0] update phone state, old=IDLE new=IDLE
09-29 16:20:23.376689  1669  1669 D MtkImsManager [0]: createMtkImsService binder is null
09-29 16:20:23.380465  1669  1669 D MtkGsmSMSDispatcher: Wrong phone id event coming, PhoneId: -1
09-29 16:20:23.380755  1669  1669 D MtkGsmSMSDispatcher: Wrong phone id event coming, PhoneId: -1
09-29 16:20:23.384002  1669  1669 D RILJ    : [0033]> BASEBAND_VERSION [PHONE0]
09-29 16:20:23.385504  1176  1192 I AT      : [0] AT> AT+CGMR (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.385685  1669  1669 D RILJ    : [0034]> DEVICE_IDENTITY [PHONE0]
09-29 16:20:23.387378  1669  1669 D RILJ    : [0035]> GET_RADIO_CAPABILITY [PHONE0]
09-29 16:20:23.389161  1669  1669 D RILJ    : [0036]> GET_UICC_APPLICATIONS_ENABLEMENT [PHONE0]
09-29 16:20:23.389970  1669  1669 D MtkGsmCdmaPhone: EVENT_RADIO_OFF_OR_NOT_AVAILABLEreceived.
09-29 16:20:23.391086  1669  1811 D RILJ    : convertHalRadioCapability: session=-1, phase=3, rat=36869, logicModemUuid=modem_sys1_ps0, status=1, rcRil.raf=81930 [PHONE0]
09-29 16:20:23.391358  1669  1811 D RILJ    : [0035]< GET_RADIO_CAPABILITY {mPhoneId = 0 mVersion=1 mSession=-1 mPhase=3 mRadioAccessFamily=36869 mLogicModemId=modem_sys1_ps0 mStatus=1} [PHONE0]
09-29 16:20:23.391381  1669  1669 D GsmCdmaCallTkr: onRilConnected 0
09-29 16:20:23.392131  1176  1196 I AT      : [0] AT> AT+ESIMPOWER? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:23.394043  1669  1669 D ANM-0   : bind to com.android.phone
09-29 16:20:23.397470  1669  1669 D MTKSST  : [GsmSST0] EVENT_ICC_CHANGED: SIM absent
09-29 16:20:23.397652  1669  1669 D MTKSST  : [GsmSST0] cancelAllNotifications: mPrevSubId=-1
09-29 16:20:23.399961  1176  1191 I AT      : [0] AT< +CGMR: MOLY.LR12A.R3.MP.V223.P4, 2022/09/09 14:14 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.400045  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.400133  1176  1195 I AT      : [0] AT< +CME ERROR: 10 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:23.400337  1176  1192 I AT      : [0] AT> AT+CGSN (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.400998  1669  1811 D RILJ    : [0033]< BASEBAND_VERSION MOLY.LR12A.R3.MP.V223.P4 [PHONE0]
09-29 16:20:23.401451  1669  1811 D RILJ    : [0036]< GET_UICC_APPLICATIONS_ENABLEMENT error 11 [PHONE0]
09-29 16:20:23.401637  1669  1811 D RilRequest: [0036]< GET_UICC_APPLICATIONS_ENABLEMENT error: com.android.internal.telephony.CommandException: SIM_ABSENT ret=true result={ when=-32s221ms what=55 target=com.mediatek.internal.telephony.MtkGsmCdmaPhone }
09-29 16:20:23.404215  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: radio is on but out of service, set plmn='No service'
09-29 16:20:23.405218  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: rawSpn = 
09-29 16:20:23.407072  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: updateSpnDisplay: changed sending intent, rule=2, showPlmn='true', plmn='No service', showSpn='false', spn='null', dataSpn='', subId='-1'
09-29 16:20:23.407437  1669  1669 D SubscriptionManager: putPhoneIdAndSubIdExtra: no valid subs
09-29 16:20:23.412170  1669  1669 D NRM-C-0 : Trying to bind com.android.phone for transport WWAN
09-29 16:20:23.415082  1176  1191 I AT      : [0] AT< *** (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.415200  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.416827  1669  1811 D RILJ    : [0034]< DEVICE_IDENTITY {[v2iLqxpMDQsf4OiyS2dL0Lw5-k4], 01, , } [PHONE0]
09-29 16:20:23.418955  1669  1669 D NRM-I-0 : Trying to bind com.android.phone for transport WLAN
09-29 16:20:23.422488  1669  1669 D MTKSST  : [GsmSST0] handle EVENT_RADIO_STATE_CHANGED
09-29 16:20:23.423220  1669  1669 D RatConfig: getActiveRatConfig: Lf/Lt/W/G
09-29 16:20:23.426423  1669  1669 D MtkTelephonyManagerEx: simSwitchMode result = 3
09-29 16:20:23.427120  1669  1669 D MTKSST  : [GsmSST0] setRadioPowerForReason power:true, mDesiredPowerState:true, forEmergencyCall:false, isSelectedPhoneForEmergencyCall:false, forceApply:false, radioState:0, reason:0
09-29 16:20:23.427932  1669  1669 D MTKSST  : [GsmSST0] setPowerStateToDesired: mDeviceShuttingDown=false, mDesiredPowerState=true, getRadioState=0, mRadioDisabledByCarrier=false, IMS reg state=false, pending radio off=false
09-29 16:20:23.428821  1669  1669 D ImsSwitchController: notifyRadioPowerChange, power:true phoneId:0
09-29 16:20:23.429049  1669  1669 D ImsSwitchController: [0] Modem auto registration so that we don't triggerImsService updateRadioState
09-29 16:20:23.431967  1669  1669 D RILJ    : [0037]> RADIO_POWER on = true forEmergencyCall= false preferredForEmergencyCall=false [PHONE0]
09-29 16:20:23.433196  1176  1180 I RfxMclMessenger: RFX_MSG_REQUEST_RADIO_POWER(56515) dispatchs to main protocol: 0
09-29 16:20:23.433477  1176  1206 I RmcRadioReq: [0] requestRadioPower, power = 1, mode = 1, forEcc 0, preEcc 0, caller: -1
09-29 16:20:23.437255  1669  1669 D MtkRILJ : [0038]> MTK: RIL_REQUEST_SET_VENDOR_SETTING [SUB0]
09-29 16:20:23.438563  1669  1669 D MTKSST  : [GsmSST0] pollState: modemTriggered=true, mPollingContext=0, RadioState=0, connected=false, support_ap_iwlan=1
09-29 16:20:23.438761  1669  1669 D NewNitzStateMachineImpl: handleNetworkUnavailable(): mLatestNitzSignal was already null. Nothing to do.
09-29 16:20:23.438808  1669  1669 D MTKSST  : [GsmSST0] Skip pollState due to disconnection of service
09-29 16:20:23.438872  1176  1206 I AT      : [0] AT> AT+EFUN=1 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:23.438980  1669  1669 D MTKSST  : [GsmSST0] handle EVENT_RADIO_STATE_CHANGED
09-29 16:20:23.439460  1669  1669 D RatConfig: getActiveRatConfig: Lf/Lt/W/G
09-29 16:20:23.441494  1669  1669 D MtkTelephonyManagerEx: simSwitchMode result = 3
09-29 16:20:23.441992  1669  1669 D MTKSST  : [GsmSST0] setRadioPowerForReason power:true, mDesiredPowerState:true, forEmergencyCall:false, isSelectedPhoneForEmergencyCall:false, forceApply:false, radioState:0, reason:0
09-29 16:20:23.442131  1669  1669 D MTKSST  : [GsmSST0] setPowerStateToDesired: mDeviceShuttingDown=false, mDesiredPowerState=true, getRadioState=0, mRadioDisabledByCarrier=false, IMS reg state=false, pending radio off=false
09-29 16:20:23.442308  1669  1811 D RILJ    : [0038]< MTK: RIL_REQUEST_SET_VENDOR_SETTING  [PHONE0]
09-29 16:20:23.442425  1669  1669 D ImsSwitchController: notifyRadioPowerChange, power:true phoneId:0
09-29 16:20:23.442545  1669  1669 D ImsSwitchController: [0] Modem auto registration so that we don't triggerImsService updateRadioState
09-29 16:20:23.443841  1669  1669 D RILJ    : [0039]> RADIO_POWER on = true forEmergencyCall= false preferredForEmergencyCall=false [PHONE0]
09-29 16:20:23.447115  1669  1669 D MtkRILJ : [0040]> MTK: RIL_REQUEST_SET_VENDOR_SETTING [SUB0]
09-29 16:20:23.448501  1669  1669 D MTKSST  : [GsmSST0] pollState: modemTriggered=true, mPollingContext=0, RadioState=0, connected=false, support_ap_iwlan=1
09-29 16:20:23.448671  1669  1669 D NewNitzStateMachineImpl: handleNetworkUnavailable(): mLatestNitzSignal was already null. Nothing to do.
09-29 16:20:23.448710  1669  1669 D MTKSST  : [GsmSST0] Skip pollState due to disconnection of service
09-29 16:20:23.451574  1669  1811 D RILJ    : [0040]< MTK: RIL_REQUEST_SET_VENDOR_SETTING  [PHONE0]
09-29 16:20:23.456254  1176  1184 I AT      : [0] AT< +CSCON: 0,,0 (RIL_URC_READER, tid:493447834880)
09-29 16:20:23.456795  1176  1185 E RmcNwHdlr: [0] There is something wrong with the handleConnectionStateReport URC
09-29 16:20:23.457311  1669  1669 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:23.463977  1669  1669 I CSST    : isNrSupported:  carrierConfigEnabled: true, AccessFamilySupported: false, isNrNetworkTypeAllowed: false
09-29 16:20:23.464193  1669  1669 I CSST    : PrefNetworkNotification: sendMessage() w/values: ,false,-1,false,false
09-29 16:20:23.465192  1669  1669 I CSST    : canceling notifications: 1000
09-29 16:20:23.465404  1669  1669 D CSST    : isPhoneRegisteredForWifiCalling: false
09-29 16:20:23.465522  1669  1669 I CSST    : EmergencyNetworkNotification: sendMessage() w/values: ,-1,false,false
09-29 16:20:23.466214  1669  1669 I CSST    : canceling notifications: 1001
09-29 16:20:23.468556  1669  1669 I CSST    : isNrSupported:  carrierConfigEnabled: true, AccessFamilySupported: false, isNrNetworkTypeAllowed: false
09-29 16:20:23.468896  1669  1669 I CSST    : PrefNetworkNotification: sendMessage() w/values: ,false,-1,false,false
09-29 16:20:23.469729  1669  1669 I CSST    : canceling notifications: 1000
09-29 16:20:23.469946  1669  1669 D CSST    : isPhoneRegisteredForWifiCalling: false
09-29 16:20:23.470056  1669  1669 I CSST    : EmergencyNetworkNotification: sendMessage() w/values: ,-1,false,false
09-29 16:20:23.470708  1669  1669 I CSST    : canceling notifications: 1001
09-29 16:20:23.472217  1669  1669 D NrMap-0 : loadCityFromXml.done: system_ext/etc/nr-city.xml
09-29 16:20:23.472519  1669  1669 D EmergencyNumberTracker: updateRadioEmergencyNumberListAndNotify(): receiving []
09-29 16:20:23.474550  1669  1669 D RILJ    : [0041]> SEND_DEVICE_STATE 1:true [PHONE0]
09-29 16:20:23.476341  1669  1669 D RILJ    : [0042]> SEND_DEVICE_STATE 2:true [PHONE0]
09-29 16:20:23.477037  1669  1811 D RILJ    : [0041]< SEND_DEVICE_STATE error 6 [PHONE0]
09-29 16:20:23.477190  1669  1811 D RilRequest: [0041]< SEND_DEVICE_STATE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result=null
09-29 16:20:23.478203  1669  1669 D RILJ    : [0043]> SEND_DEVICE_STATE 0:false [PHONE0]
09-29 16:20:23.478738  1176  1198 D RmcDcMiscHandler: [0][handleSendDeviceStateRequest]: state: 1
09-29 16:20:23.478840  1176  1198 I AT      : [0] AT> AT+EFD=1 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:23.479968  1669  1669 D RILJ    : [0044]> SET_UNSOLICITED_RESPONSE_FILTER -1 [PHONE0]
09-29 16:20:23.481367  1176  1192 I AT      : [0] AT> AT+ECSQ=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.481976  1669  1669 D RILJ    : [0045]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.483920  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:23.484104  1669  1669 D RILJ    : [0046]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.484390  1669  1811 D RILJ    : [0045]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error 1 [PHONE0]
09-29 16:20:23.484575  1669  1811 D RilRequest: [0045]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret= result=null
09-29 16:20:23.485732  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.485932  1669  1669 D RILJ    : [0047]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.487487  1176  1192 I AT      : [0] AT> AT+EREG=3 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.487848  1669  1669 D RILJ    : [0048]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.488060  1669  1811 D RILJ    : [0042]< SEND_DEVICE_STATE  [PHONE0]
09-29 16:20:23.489154  1669  1811 D RILJ    : [0043]< SEND_DEVICE_STATE error 6 [PHONE0]
09-29 16:20:23.489292  1669  1811 D RilRequest: [0043]< SEND_DEVICE_STATE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result=null
09-29 16:20:23.489393  1669  1669 D RILJ    : [0049]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.489580  1669  1811 D RILJ    : [0046]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error 1 [PHONE0]
09-29 16:20:23.489684  1669  1811 D RilRequest: [0046]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret= result=null
09-29 16:20:23.489964  1669  1811 D RILJ    : [0047]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error 1 [PHONE0]
09-29 16:20:23.490096  1669  1811 D RilRequest: [0047]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret= result=null
09-29 16:20:23.490935  1669  1669 D RILJ    : [0050]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.491985  1669  1811 D RILJ    : [0048]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error 1 [PHONE0]
09-29 16:20:23.492451  1669  1811 D RilRequest: [0048]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret= result=null
09-29 16:20:23.493245  1669  1669 D RILJ    : [0051]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.493624  1669  1811 D RILJ    : [0049]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error 1 [PHONE0]
09-29 16:20:23.493971  1669  1811 D RilRequest: [0049]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret= result=null
09-29 16:20:23.494958  1669  1669 D RILJ    : [0052]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.495214  1176  1184 I AT      : [0] AT< +EREG=*** (RIL_URC_READER, tid:493447834880)
09-29 16:20:23.495247  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.495387  1176  1192 I AT      : [0] AT> AT+EGREG=3 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.495987  1176  1185 D RmcNwHdlr: [0] [handleCsNetworkStateChanged] mMdEreg n=0, stat=0, lac=**FF, ci=***FFFF, eAct=0, nwk_existence=0, roam_indicator=0, cause_type=0, reject_cause=0 mMdEcell act=0, cid=*, mcc=0, mnc=0, lacTac=*, pscPci=*, sig1=0, sig2=0, rsrp=0, rsrq=0, timingAdvance=0, rssnr=0, cqi=0, bsic=0, arfcn=0
09-29 16:20:23.496750  1669  1669 D RILJ    : [0053]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.497908  1669  1811 D RILJ    : [0050]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error 1 [PHONE0]
09-29 16:20:23.498205  1669  1811 D RilRequest: [0050]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret= result=null
09-29 16:20:23.498240  1176  1184 I AT      : [0] AT< +EGREG=*** (RIL_URC_READER, tid:493447834880)
09-29 16:20:23.498372  1669  1669 D RILJ    : [0054]> SET_LINK_CAPACITY_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.498578  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.498711  1176  1192 I AT      : [0] AT> AT+PSBEARER=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.499938  1176  1198 I AT      : [0] AT> AT+EXLCE=2,3000,50,50,14,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,1000000,1500000,2000000,11,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,1 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:23.500304  1176  1185 D RmcNwHdlr: [0] [handlePsNetworkStateChanged] mMdEgreg n=0, stat=0, lac=**FF, ci=***FFFF, eAct=0, rac=255, nwk_existence=0, roam_indicator=0, cause_type=0, reject_cause=0, dcnr_restricted=0, endc_sib=0, endc_available=0.   mMdEcell act=0, cid=*, mcc=0, mnc=0, lacTac=*, pscPci=*, sig1=0, sig2=0, rsrp=0, rsrq=0, timingAdvance=0, rssnr=0, cqi=0, bsic=0, arfcn=0
09-29 16:20:23.500355  1176  1185 D RmcNwHdlr: [0] handleScgConnectionChange old=0, new=0
09-29 16:20:23.500471  1176  1200 I AT      : [0] AT> AT+EOPS? (RIL_ATCI_READER tid:493431254272)
09-29 16:20:23.502535  1669  1669 D RILJ    : [0055]> SET_LINK_CAPACITY_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.503199  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:23.504084  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_CS_NETWORK_STATE_CHANGED [PHONE0]
09-29 16:20:23.504877  1669  1669 D RILJ    : [0057]> SET_LINK_CAPACITY_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.505705  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:23.505966  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_NETWORK_STATE_CHANGED [PHONE0]
09-29 16:20:23.506297  1669  1833 D MTKSST  : [GsmSST0] MtkHandler: EVENT_NETWORK_STATE_CHANGED
09-29 16:20:23.506368  1669  1669 D RILJ    : [0059]> SET_LINK_CAPACITY_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.506424  1669  1811 D RILJ    : [0051]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error 1 [PHONE0]
09-29 16:20:23.506529  1669  1811 D RilRequest: [0051]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret= result=null
09-29 16:20:23.506841  1176  1184 I AT      : [0] AT< +ECEMODE: 1 (RIL_URC_READER, tid:493447834880)
09-29 16:20:23.507035  1176  1184 I AT      : [0] AT< +ECEVDP: 3 (RIL_URC_READER, tid:493447834880)
09-29 16:20:23.507124  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:23.507137  1176  1199 I AT      : [0] AT< +EOPS: 0,2,"000000",1 (RIL_ATCI_READER, tid:493432290560)
09-29 16:20:23.507159  1176  1184 I AT      : [0] AT< +EREG=*** (RIL_URC_READER, tid:493447834880)
09-29 16:20:23.507168  1176  1199 I AT      : [0] AT< OK (RIL_ATCI_READER, tid:493432290560)
09-29 16:20:23.507256  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:23.507342  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.507486  1176  1192 I AT      : [0] AT> AT+EREGINFO=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.507597  1176  1200 E RmcEmbmsReq: [0] Error due to cell_id = ***FFFF
09-29 16:20:23.507609  1176  1185 D RmcNwHdlr: [0] [handleCsNetworkStateChanged] mMdEreg n=0, stat=2, lac=**FF, ci=***FFFF, eAct=0, nwk_existence=0, roam_indicator=0, cause_type=0, reject_cause=0 mMdEcell act=0, cid=*, mcc=0, mnc=0, lacTac=*, pscPci=*, sig1=0, sig2=0, rsrp=0, rsrq=0, timingAdvance=0, rssnr=0, cqi=0, bsic=0, arfcn=0
09-29 16:20:23.507617  1176  1198 I AT      : [0] AT> AT+EXLCE=2,3000,50,50,14,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,1000000,1500000,2000000,11,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,2 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:23.507800  1669  1833 D RILJ    : [0060]> OPERATOR [PHONE0]
09-29 16:20:23.508354  1669  1811 D RILJ    : [0052]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error 1 [PHONE0]
09-29 16:20:23.508504  1669  1811 D RilRequest: [0052]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret= result=null
09-29 16:20:23.509011  1176  1182 I RtcRadioCont: [0] radio State: 0 -> 10, using google native API for urc
09-29 16:20:23.509510  1176  1182 I RIL-Fusion: getRadioState(): radioState=10
09-29 16:20:23.509669  1176  1182 E RILC    : radioStateChangedInd: radioService[4]->mRadioIndication == NULL
09-29 16:20:23.509722  1176  1182 E RILC    : radioStateChangedInd: radioService[8]->mRadioIndication == NULL
09-29 16:20:23.509762  1176  1182 E RILC    : radioStateChangedInd: radioService[12]->mRadioIndication == NULL
09-29 16:20:23.509837  1669  1833 D RILJ    : [0062]> DATA_REGISTRATION_STATE [PHONE0]
09-29 16:20:23.509856  1176  1182 I RtcImsConfigController: [0] onRadioStateChanged, state = 10
09-29 16:20:23.509931  1669  1833 D RILJ    : getDataRegistrationState: overrideHalVersion=null [PHONE0]
09-29 16:20:23.510697  1669  1669 D RILJ    : [0061]> SET_LINK_CAPACITY_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.511911  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:23.511912  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.512105  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:23.512197  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_RADIO_STATE_CHANGED radioStateChanged: 1 [PHONE0]
09-29 16:20:23.512281  1176  1198 I AT      : [0] AT> AT+EXLCE=2,3000,50,50,14,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,1000000,1500000,2000000,11,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,3 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:23.512734  1669  1833 D RILJ    : [0063]> VOICE_REGISTRATION_STATE [PHONE0]
09-29 16:20:23.512993  1669  1833 D RILJ    : getVoiceRegistrationState: overrideHalVersion=null [PHONE0]
09-29 16:20:23.513620  1669  1669 D RILJ    : [0065]> SEND_DEVICE_STATE 1:true [PHONE0]
09-29 16:20:23.513794  1176  1182 I RtcImsConfigController: [0] onRadioStateChanged, mECCAllowSendCmd = true
09-29 16:20:23.513848  1176  1182 D RTC_EMBMS_CON_PROXY: [0] radioState 10
09-29 16:20:23.514372  1176  1191 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.515934  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:23.516775  1176  1191 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.516960  1176  1192 W RmcNwReqHdlr: [0] There is something wrong with the exectution of AT+EDEFROAM=1
09-29 16:20:23.517293  1176  1180 I RfxMclMessenger: RFX_MSG_REQUEST_RADIO_POWER(56515) dispatchs to main protocol: 0
09-29 16:20:23.517462  1176  1192 I AT      : [0] AT> AT+CSCON=3 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.517736  1669  1833 D RILJ    : [0066]> SIGNAL_STRENGTH [PHONE0]
09-29 16:20:23.517890  1176  1206 I RmcRadioReq: [0] requestRadioPower, power = 1, mode = 1, forEcc 0, preEcc 0, caller: -1
09-29 16:20:23.518912  1176  1198 I AT      : [0] AT> AT+EXLCE=2,3000,50,50,14,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,1000000,1500000,2000000,11,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,4 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:23.519562  1669  1669 D RILJ    : [0067]> SEND_DEVICE_STATE 2:true [PHONE0]
09-29 16:20:23.521017  1176  1202 I AT      : [0] AT> AT+EOPS? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:23.521259  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.521911  1176  1192 I AT      : [0] AT> AT+CSCON? (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.522069  1176  1196 I AT      : [0] AT> AT+EIMSRCS=0,0 (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:23.522279  1669  1669 D RILJ    : [0068]> SEND_DEVICE_STATE 0:false [PHONE0]
09-29 16:20:23.522621  1176  1197 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:23.522973  1176  1198 I AT      : [0] AT> AT+EXLCE=2,3000,50,50,14,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,1000000,1500000,2000000,11,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,6 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:23.523580  1176  1201 I AT      : [0] AT< +EOPS: 0,2,"000000",1 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:23.523637  1176  1201 I AT      : [0] AT< OK (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:23.523736  1669  1669 D RILJ    : [0069]> SET_UNSOLICITED_RESPONSE_FILTER -1 [PHONE0]
09-29 16:20:23.524070  1176  1202 I AT      : [0] AT> AT+E5GOPT? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:23.524198  1176  1206 I AT      : [0] AT> AT+EFUN=1 (RIL_CMD_RADIO_9 tid:493335764224)
09-29 16:20:23.524696  1176  1191 I AT      : [0] AT< +CSCON: 3,0,,0 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.524743  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.524833  1176  1192 E RmcNwReqHdlr: [0] There is something wrong with the updateConnectionStateReport URC
09-29 16:20:23.524876  1176  1192 I AT      : [0] AT> AT+ECAMPUI=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.525045  1669  1811 D RILJ    : Broadcast for RadioStateChanged: state=1 [PHONE0]
09-29 16:20:23.525449  1669  1669 D RILJ    : [0070]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.525831  1669  1811 D RILJ    : [0053]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error 1 [PHONE0]
09-29 16:20:23.526781  1669  1811 D RilRequest: [0053]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret= result=null
09-29 16:20:23.527331  1669  1669 D RILJ    : [0071]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.527601  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:23.527959  1176  1196 I AT      : [0] AT> AT+EIMSCFG=1,0,0,0,1,1 (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:23.527987  1176  1197 I AT      : [0] AT< +CME ERROR: 3 (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:23.528451  1176  1198 D RmcDcMiscHandler: [0][handleSendDeviceStateRequest]: state: 1
09-29 16:20:23.528574  1176  1198 I AT      : [0] AT> AT+EFD=1 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:23.529780  1669  1669 D RILJ    : [0073]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.530228  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:23.530383  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_CS_NETWORK_STATE_CHANGED [PHONE0]
09-29 16:20:23.530545  1176  1201 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:23.530892  1669  1811 D RILJ    : [0037]< RADIO_POWER  [PHONE0]
09-29 16:20:23.531503  1669  1669 D RILJ    : [0074]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.532030  1669  1811 D RILJ    : [0054]< SET_LINK_CAPACITY_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:23.532505  1669  1811 D RILJ    : [0055]< SET_LINK_CAPACITY_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:23.532875  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.532957  1176  1205 I AT      : [0] AT< OK (RIL_CMD_RADIO_9, tid:493336800512)
09-29 16:20:23.533085  1176  1192 W RmcNwReqHdlr: [0] There is something wrong with the exectution of AT+ECAMPUI=1
09-29 16:20:23.533130  1176  1192 I AT      : [0] AT> AT+ECAPABILITY=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.533372  1176  1182 E RtcDC   : [0][onServiceStateChanged] old or new data reg state is not InService
09-29 16:20:23.533389  1669  1669 D RILJ    : [0075]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.533430  1176  1182 D RtcCC   : [0] updateImsCallRat dataRegState 0 dataRadioTech 0 wfcRegState 0
09-29 16:20:23.533849  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:23.534281  1176  1184 I AT      : [0] AT< +EIMS: 1 (RIL_URC_READER, tid:493447834880)
09-29 16:20:23.535312  1669  1669 D RILJ    : [0076]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.536853  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:23.537166  1669  1669 D RILJ    : [0077]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.537586  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.537761  1176  1192 W RmcNwReqHdlr: [0] There is something wrong with the exectution of AT+ECAPABILITY=1
09-29 16:20:23.537814  1176  1192 I AT      : [0] AT> AT+ECAPABILITY? (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.539129  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:23.540014  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.540208  1176  1192 E RmcNwReqHdlr: [0] There is something wrong with AT+ECAPABILITY
09-29 16:20:23.540305  1176  1192 I AT      : [0] AT> AT+EXLCE=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.540898  1669  1669 D RILJ    : [0079]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.541481  1669  1811 D RILJ    : [UNSL]< MTK: RIL_UNSOL_QUALIFIED_NETWORK_TYPES_CHANGED {1, 2178, 1} [PHONE0]
09-29 16:20:23.542034  1669  1811 D RILJ    : [0057]< SET_LINK_CAPACITY_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:23.542808  1669  1669 D RILJ    : [0080]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.543112  1669  1811 D RILJ    : [0059]< SET_LINK_CAPACITY_REPORTING_CRITERIA error 40 [PHONE0]
09-29 16:20:23.543343  1669  1811 D RilRequest: [0059]< SET_LINK_CAPACITY_REPORTING_CRITERIA error: com.android.internal.telephony.CommandException: MODEM_ERR ret= result=null
09-29 16:20:23.543368  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.543691  1176  1192 I AT      : [0] AT> AT+EBARRING=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.543994  1669  1811 D RILJ    : [0060]< OPERATOR {, , } [PHONE0]
09-29 16:20:23.544574  1669  1669 D RILJ    : [0081]> SET_LINK_CAPACITY_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.544953  1669  1811 D RILJ    : [0061]< SET_LINK_CAPACITY_REPORTING_CRITERIA error 40 [PHONE0]
09-29 16:20:23.545178  1669  1811 D RilRequest: [0061]< SET_LINK_CAPACITY_REPORTING_CRITERIA error: com.android.internal.telephony.CommandException: MODEM_ERR ret= result=null
09-29 16:20:23.546042  1176  1198 I AT      : [0] AT> AT+EXLCE=2,3000,50,50,14,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,1000000,1500000,2000000,11,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,1 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:23.546246  1669  1669 D RILJ    : [0082]> SET_LINK_CAPACITY_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.547356  1669  1811 D RILJ    : [0065]< SEND_DEVICE_STATE error 6 [PHONE0]
09-29 16:20:23.547541  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.547643  1669  1811 D RilRequest: [0065]< SEND_DEVICE_STATE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result=null
09-29 16:20:23.547918  1669  1669 D RILJ    : [0083]> SET_LINK_CAPACITY_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.547986  1176  1192 I AT      : [0] AT> AT+EOPS? (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.549019  1669  1811 D RILJ    : [0062]< DATA_REGISTRATION_STATE {.regState = NOT_REG_MT_NOT_SEARCHING_OP, .rat = UNKNOWN, .reasonForDenial = NONE, .cellIdentity = {.noinit = {}}, .registeredPlmn = , .accessTechnologySpecificInfo = {.noinit = {}}} [PHONE0]
09-29 16:20:23.549677  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:23.550112  1176  1198 I AT      : [0] AT> AT+EXLCE=2,3000,50,50,14,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,1000000,1500000,2000000,11,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,2 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:23.550530  1669  1669 D RILJ    : [0084]> SET_LINK_CAPACITY_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.550567  1176  1191 I AT      : [0] AT< +EOPS: 0,2,"000000",1 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.550633  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.550998  1176  1192 I AT      : [0] AT> AT+ECSQ (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.551855  1669  1811 D RILJ    : [0063]< VOICE_REGISTRATION_STATE {.regState = NOT_REG_MT_SEARCHING_OP, .rat = UNKNOWN, .reasonForDenial = NONE, .cellIdentity = {.noinit = {}}, .registeredPlmn = , .accessTechnologySpecificInfo = {.noinit = {}}} [PHONE0]
09-29 16:20:23.552292  1669  1669 D RILJ    : [0085]> SET_LINK_CAPACITY_REPORTING_CRITERIA [PHONE0]
09-29 16:20:23.553073  1669  1669 D NetworkTypeController: [0] DefaultState: process EVENT_INITIALIZE
09-29 16:20:23.553431  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:23.553600  1176  1191 I AT      : [0] AT< +ECSQ: 0,0,0,0,0,0,0,0,0,0 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.553646  1176  1191 I AT      : [0] AT< +ECSQ: 0,0,0,0,0,0,0,0,0,0 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.554717  1669  1811 D RILJ    : [0039]< RADIO_POWER  [PHONE0]
09-29 16:20:23.555312  1176  1198 I AT      : [0] AT> AT+EXLCE=2,3000,50,50,14,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,1000000,1500000,2000000,11,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,3 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:23.555574  1669  1669 D MtkNetworkTypeController: registerForAllEvents: register rat changed for TRANSPORT_TYPE_WLAN
09-29 16:20:23.556049  1176  1191 I AT      : [0] AT< +ECSQ: 0,0,0,0,0,0,0,0,0,0 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.556126  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.556242  1176  1192 D RmcNwReqHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0000]
09-29 16:20:23.556276  1176  1192 D RmcNwHdlr: [0] requestSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 99, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 255, wcdma_ecno: 255, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:20:23.556342  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:23.556498  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_PS_NETWORK_STATE_CHANGED [PHONE0]
09-29 16:20:23.556775  1176  1192 I AT      : [0] AT> AT+ECSQ=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.557050  1669  1811 D RILJ    : [0067]< SEND_DEVICE_STATE  [PHONE0]
09-29 16:20:23.557498  1669  1811 D RILJ    : [0068]< SEND_DEVICE_STATE error 6 [PHONE0]
09-29 16:20:23.557689  1669  1811 D RilRequest: [0068]< SEND_DEVICE_STATE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result=null
09-29 16:20:23.558178  1669  1811 D RILJ    : [0044]< SET_UNSOLICITED_RESPONSE_FILTER  [PHONE0]
09-29 16:20:23.558571  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:23.558596  1669  1811 D RILJ    : [0081]< SET_LINK_CAPACITY_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:23.558808  1669  1811 D RILJ    : [0082]< SET_LINK_CAPACITY_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:23.558817  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.558943  1176  1192 I AT      : [0] AT> AT+ECSQ (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.559002  1669  1669 D NetworkTypeController: [0] mOverrideTimerRules: {connected={mState=connected, mOverrideType=NR_NSA, mPrimaryTimers={}, mSecondaryTimers={}}, not_restricted_rrc_con={mState=not_restricted_rrc_con, mOverrideType=NR_NSA, mPrimaryTimers={}, mSecondaryTimers={}}, legacy={mState=legacy, mOverrideType=NONE, mPrimaryTimers={}, mSecondaryTimers={}}, not_restricted_rrc_idle={mState=not_restricted_rrc_idle, mOverrideType=NR_NSA, mPrimaryTimers={}, mSecondaryTimers={}}, restricted={mState=restricted, mOverrideType=NONE, mPrimaryTimers={}, mSecondaryTimers={}}, connected_mmwave={mState=connected_mmwave, mOverrideType=NR_NSA, mPrimaryTimers={}, mSecondaryTimers={}}}
09-29 16:20:23.559132  1176  1198 I AT      : [0] AT> AT+EXLCE=2,3000,50,50,14,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,1000000,1500000,2000000,11,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,4 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:23.559901  1669  1669 D NetworkTypeController: [0] DefaultState: process EVENT_UPDATE
09-29 16:20:23.560090  1669  1811 D RILJ    : [0066]< SIGNAL_STRENGTH SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=2147483647 ber=2147483647 rscp=2147483647 ecno=2147483647 level=0,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthLte} [PHONE0]
09-29 16:20:23.560158  1669  1669 D NetworkTypeController: [0] Remove all timers
09-29 16:20:23.560500  1669  1669 D NetworkTypeController: [0] Entering LegacyState
09-29 16:20:23.560628  1669  1811 D RILJ    : [0083]< SET_LINK_CAPACITY_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:23.560684  1669  1669 D NetworkTypeController: [0] Remove all timers
09-29 16:20:23.560736  1669  1833 D MTKSST  : [GsmSST0] notifyMtkSignalStrength level:0 raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=2147483647 ber=2147483647 rscp=2147483647 ecno=2147483647 level=0,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthLte}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null
09-29 16:20:23.560917  1669  1669 D MtkNetworkTypeController: [Override]getCurrentOverrideNetworkType: 0
09-29 16:20:23.561232  1669  1669 D MtkDisplayInfoController: TelephonyDisplayInfo[0] changed from null to TelephonyDisplayInfo {network=UNKNOWN, override=NONE}, turboSS alive:true
09-29 16:20:23.561423  1176  1191 I AT      : [0] AT< +ECSQ: 0,0,0,0,0,0,0,0,0,0 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.561980  1251  1557 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:23.562074  1251  1557 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:23.562182  1176  1191 I AT      : [0] AT< +ECSQ: 0,0,0,0,0,0,0,0,0,0 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.562234  1176  1191 I AT      : [0] AT< +ECSQ: 0,0,0,0,0,0,0,0,0,0 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.562255  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.562404  1176  1192 D RmcNwReqHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0000]
09-29 16:20:23.562486  1176  1192 D RmcNwHdlr: [0] requestSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 99, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 255, wcdma_ecno: 255, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:20:23.562511  1176  1192 E RmcNwReqHdlr: [0] requestSignalStrength must never return an error when radio is on
09-29 16:20:23.562575  1176  1192 I AT      : [0] AT> AT+EREG=3 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.563211  1176  1197 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:23.563609  1176  1198 I AT      : [0] AT> AT+EXLCE=2,3000,50,50,14,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,1000000,1500000,2000000,11,100,500,1000,5000,10000,20000,50000,75000,100000,200000,500000,6 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:23.564083  1669  1811 D RILJ    : [0084]< SET_LINK_CAPACITY_REPORTING_CRITERIA error 40 [PHONE0]
09-29 16:20:23.564232  1669  1811 D RilRequest: [0084]< SET_LINK_CAPACITY_REPORTING_CRITERIA error: com.android.internal.telephony.CommandException: MODEM_ERR ret= result=null
09-29 16:20:23.565412  1176  1184 I AT      : [0] AT< +EREG=*** (RIL_URC_READER, tid:493447834880)
09-29 16:20:23.565412  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.565590  1176  1192 I AT      : [0] AT> AT+EGREG=3 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.565933  1176  1185 D RmcNwHdlr: [0] [handleCsNetworkStateChanged] mMdEreg n=0, stat=2, lac=**FF, ci=***FFFF, eAct=0, nwk_existence=0, roam_indicator=0, cause_type=0, reject_cause=0 mMdEcell act=0, cid=*, mcc=0, mnc=0, lacTac=*, pscPci=*, sig1=0, sig2=0, rsrp=0, rsrq=0, timingAdvance=0, rssnr=0, cqi=0, bsic=0, arfcn=0
09-29 16:20:23.568442  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:23.568619  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_CS_NETWORK_STATE_CHANGED [PHONE0]
09-29 16:20:23.569909  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:23.569997  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_NETWORK_STATE_CHANGED [PHONE0]
09-29 16:20:23.570122  1669  1833 D MTKSST  : [GsmSST0] MtkHandler: EVENT_NETWORK_STATE_CHANGED
09-29 16:20:23.570354  1176  1197 I AT      : [0] AT< +CME ERROR: 3 (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:23.570468  1176  1184 I AT      : [0] AT< +EGREG=*** (RIL_URC_READER, tid:493447834880)
09-29 16:20:23.571089  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.571221  1669  1811 D RILJ    : [0085]< SET_LINK_CAPACITY_REPORTING_CRITERIA error 40 [PHONE0]
09-29 16:20:23.571328  1669  1833 D RILJ    : [0089]> OPERATOR [PHONE0]
09-29 16:20:23.571361  1669  1811 D RilRequest: [0085]< SET_LINK_CAPACITY_REPORTING_CRITERIA error: com.android.internal.telephony.CommandException: MODEM_ERR ret= result=null
09-29 16:20:23.571435  1176  1192 I AT      : [0] AT> AT+PSBEARER=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.571532  1176  1185 D RmcNwHdlr: [0] [handlePsNetworkStateChanged] mMdEgreg n=0, stat=0, lac=**FF, ci=***FFFF, eAct=0, rac=255, nwk_existence=0, roam_indicator=0, cause_type=0, reject_cause=0, dcnr_restricted=0, endc_sib=0, endc_available=0.   mMdEcell act=0, cid=*, mcc=0, mnc=0, lacTac=*, pscPci=*, sig1=0, sig2=0, rsrp=0, rsrq=0, timingAdvance=0, rssnr=0, cqi=0, bsic=0, arfcn=0
09-29 16:20:23.571569  1176  1185 D RmcNwHdlr: [0] handleScgConnectionChange old=0, new=0
09-29 16:20:23.572280  1176  1200 I AT      : [0] AT> AT+EOPS? (RIL_ATCI_READER tid:493431254272)
09-29 16:20:23.572853  1669  1833 D RILJ    : [0090]> DATA_REGISTRATION_STATE [PHONE0]
09-29 16:20:23.572855  1176  1202 I AT      : [0] AT> AT+EOPS? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:23.572989  1669  1833 D RILJ    : getDataRegistrationState: overrideHalVersion=null [PHONE0]
09-29 16:20:23.574133  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.574373  1669  1833 D RILJ    : [0091]> VOICE_REGISTRATION_STATE [PHONE0]
09-29 16:20:23.574395  1176  1192 I AT      : [0] AT> AT+EREGINFO=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.574553  1669  1833 D RILJ    : getVoiceRegistrationState: overrideHalVersion=null [PHONE0]
09-29 16:20:23.575940  1669  1833 D RILJ    : [0092]> SIGNAL_STRENGTH [PHONE0]
09-29 16:20:23.576035  1176  1199 I AT      : [0] AT< +EOPS: 0,2,"000000",1 (RIL_ATCI_READER, tid:493432290560)
09-29 16:20:23.576109  1176  1199 I AT      : [0] AT< OK (RIL_ATCI_READER, tid:493432290560)
09-29 16:20:23.576119  1176  1201 I AT      : [0] AT< +EOPS: 0,2,"000000",1 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:23.576168  1176  1201 I AT      : [0] AT< OK (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:23.576257  1176  1200 E RmcEmbmsReq: [0] Error due to cell_id = ***FFFF
09-29 16:20:23.576473  1176  1202 I AT      : [0] AT> AT+E5GOPT? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:23.577129  1669  1811 D RILJ    : [0089]< OPERATOR {, , } [PHONE0]
09-29 16:20:23.577703  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.579193  1176  1201 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:23.580057  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.580216  1176  1191 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.580479  1669  1811 D RILJ    : [0090]< DATA_REGISTRATION_STATE {.regState = NOT_REG_MT_NOT_SEARCHING_OP, .rat = UNKNOWN, .reasonForDenial = NONE, .cellIdentity = {.noinit = {}}, .registeredPlmn = , .accessTechnologySpecificInfo = {.noinit = {}}} [PHONE0]
09-29 16:20:23.581040  1669  1811 D RILJ    : [0091]< VOICE_REGISTRATION_STATE {.regState = NOT_REG_MT_SEARCHING_OP, .rat = UNKNOWN, .reasonForDenial = NONE, .cellIdentity = {.noinit = {}}, .registeredPlmn = , .accessTechnologySpecificInfo = {.noinit = {}}} [PHONE0]
09-29 16:20:23.582487  1176  1191 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.582681  1176  1192 W RmcNwReqHdlr: [0] There is something wrong with the exectution of AT+EDEFROAM=1
09-29 16:20:23.583010  1176  1192 I AT      : [0] AT> AT+CSCON=3 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.583284  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.585264  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.585459  1176  1192 I AT      : [0] AT> AT+CSCON? (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.586592  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.587917  1176  1191 I AT      : [0] AT< +CSCON: 3,0,,0 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.588041  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.588193  1176  1192 E RmcNwReqHdlr: [0] There is something wrong with the updateConnectionStateReport URC
09-29 16:20:23.588275  1176  1192 I AT      : [0] AT> AT+ECAMPUI=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.589764  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.590520  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.590707  1176  1192 W RmcNwReqHdlr: [0] There is something wrong with the exectution of AT+ECAMPUI=1
09-29 16:20:23.590786  1176  1192 I AT      : [0] AT> AT+ECAPABILITY=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.592672  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.592947  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.593105  1176  1192 W RmcNwReqHdlr: [0] There is something wrong with the exectution of AT+ECAPABILITY=1
09-29 16:20:23.593174  1176  1192 I AT      : [0] AT> AT+ECAPABILITY? (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.595319  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.595479  1176  1192 E RmcNwReqHdlr: [0] There is something wrong with AT+ECAPABILITY
09-29 16:20:23.595558  1176  1192 I AT      : [0] AT> AT+EXLCE=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.595593  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.597882  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.598084  1176  1192 I AT      : [0] AT> AT+EBARRING=1 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.598165  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.600437  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.600865  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 1, 1, 0, 3000, 2, 4, -109, -103, -97, -89 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.600980  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.601429  1669  1811 D RILJ    : [0069]< SET_UNSOLICITED_RESPONSE_FILTER  [PHONE0]
09-29 16:20:23.603535  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.603956  1176  1192 D RmcNwReqHdlr: [0] [currentPhysicalChannelConfigs] needNotifyEmpty and has notified empty list, return
09-29 16:20:23.604132  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 1, 2, 0, 3000, 2, 4, -114, -104, -94, -84 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.604855  1669  1811 D RILJ    : [0070]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:23.606050  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.607552  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.607955  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 1, 4, 0, 3000, 2, 4, -128, -118, -108, -98 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.608332  1669  1811 D RILJ    : [0071]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:23.608790  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.610356  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.610721  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 1, 16, 0, 3000, 2, 4, -105, -90, -75, -65 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.611111  1669  1811 D RILJ    : [0073]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:23.611402  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.613199  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.613556  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 0, 4, 1, 3000, 2, 4, 0, 0, 0, 0 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.614041  1669  1811 D RILJ    : [0074]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:23.614410  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.616145  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.616549  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 1, 4, 2, 3000, 2, 4, -3, 1, 5, 13 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.616947  1669  1811 D RILJ    : [0075]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:23.617416  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.619166  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.619615  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 1, 128, 0, 3000, 2, 4, -110, -90, -80, -65 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.620105  1669  1811 D RILJ    : [0076]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:23.620646  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.622219  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.622605  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 0, 128, 1, 3000, 2, 4, 0, 0, 0, 0 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.623017  1669  1811 D RILJ    : [0077]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:23.624476  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.624962  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.625327  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 0, 128, 2, 3000, 2, 4, 0, 0, 0, 0 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.625737  1669  1811 D RILJ    : [0079]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:23.627636  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.627833  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.628118  1176  1192 I AT      : [0] AT> AT+EOPS? (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.628529  1669  1811 D RILJ    : [0080]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:23.630400  1176  1191 I AT      : [0] AT< +EOPS: 0,2,"000000",1 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.630496  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.630817  1176  1192 I AT      : [0] AT> AT+ECSQ (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:23.632913  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:23.633017  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_PS_NETWORK_STATE_CHANGED [PHONE0]
09-29 16:20:23.633407  1176  1191 I AT      : [0] AT< +ECSQ: 0,0,0,0,0,0,0,0,0,0 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.633485  1176  1191 I AT      : [0] AT< +ECSQ: 0,0,0,0,0,0,0,0,0,0 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.633508  1176  1191 I AT      : [0] AT< +ECSQ: 0,0,0,0,0,0,0,0,0,0 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.633526  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:23.633666  1176  1192 D RmcNwReqHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0000]
09-29 16:20:23.633706  1176  1192 D RmcNwHdlr: [0] requestSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 99, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 255, wcdma_ecno: 255, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:20:23.634207  1176  1192 D RmcNwReqHdlr: [0] [currentPhysicalChannelConfigs] needNotifyEmpty and has notified empty list, return
09-29 16:20:23.634309  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.635097  1669  1811 D RILJ    : [0092]< SIGNAL_STRENGTH SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=2147483647 ber=2147483647 rscp=2147483647 ecno=2147483647 level=0,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthLte} [PHONE0]
09-29 16:20:23.637146  1669  1833 D MTKSST  : [GsmSST0] notifyMtkSignalStrength level:0 raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=2147483647 ber=2147483647 rscp=2147483647 ecno=2147483647 level=0,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthLte}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null
09-29 16:20:23.639105  1251  1557 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:23.639335  1251  1557 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:23.639756  1669  1669 D TDC     : getModemCount: 2
09-29 16:20:23.639915  1669  1669 D TDC     : getModem: 0
09-29 16:20:23.639969  1669  1669 D TDC     : getModemCount: 2
09-29 16:20:23.640012  1669  1669 D TDC     : getModem: 0
09-29 16:20:23.640199  1669  1669 D TDC     : getModemCount: 2
09-29 16:20:23.640253  1669  1669 D TDC     : getModem: 0
09-29 16:20:23.640318  1669  1669 D TDC     : getModemCount: 2
09-29 16:20:23.640418  1669  1669 D TDC     : getModem: 0
09-29 16:20:23.660764  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.663506  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.667977  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.671174  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.674459  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.677934  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.681928  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.684812  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.688653  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.692921  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.695758  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.699201  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.701734  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.706942  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.709740  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.712596  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.715332  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.718089  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.724401  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.729854  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.732691  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.735546  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.738051  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.740993  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.743420  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.746076  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.749267  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.752400  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.756316  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.758481  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.760802  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.763558  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.766546  1669  1669 D SubscriptionController: [getActiveSubscriptionInfo]- subId=-1 subList=[] subInfo=null
09-29 16:20:23.767792  1669  1669 D TDC     : getModemCount: 2
09-29 16:20:23.767870  1669  1669 D TDC     : getModem: 0
09-29 16:20:23.767890  1669  1669 D TDC     : getModemCount: 2
09-29 16:20:23.767900  1669  1669 D TDC     : getModem: 0
09-29 16:20:23.768024  1669  1669 D TDC     : getModemCount: 2
09-29 16:20:23.768050  1669  1669 D TDC     : getModem: 0
09-29 16:20:23.768062  1669  1669 D TDC     : getModemCount: 2
09-29 16:20:23.768071  1669  1669 D TDC     : getModem: 0
09-29 16:20:23.768335  1669  1669 D CarrierResolver: handleMessage: 2
09-29 16:20:23.769298  1669  1669 D MtkGsmCdmaPhone: correctPhoneTypeForCdma: change:false newVoiceRadioTech=1 mActivePhone=GSM
09-29 16:20:23.769588  1669  1669 D MtkSubscriptionInfoUpdater: handleMessage : <EVENT_RADIO_AVAILABLE> SIM1
09-29 16:20:23.769730  1669  1669 D MtkSubscriptionInfoUpdater: checkIsAvailable result = true
09-29 16:20:23.769806  1669  1669 D MtkSubscriptionInfoUpdater: checkAllIccIdReady +, retry_count = 0
09-29 16:20:23.770358  1669  1669 D MtkSubscriptionInfoUpdater: No SIM insert :0
09-29 16:20:23.770502  1669  1669 D MtkSubscriptionInfoUpdater: iccId[0] = N/A
09-29 16:20:23.770630  1669  1669 D MtkSubscriptionInfoUpdater: [updateSubscriptionInfoIfNeed] before update sIccId[0]: null
09-29 16:20:23.771171  1669  1669 D MtkSubscriptionInfoUpdater: [needUpdateSubscriptionInfo] sIccId[0]: N/A needUpdate: true  !TextUtils.isEmpty(sIccId[0]): true
09-29 16:20:23.771300  1669  1669 D MtkSubscriptionInfoUpdater: updateSubscriptionInfoByIccId:+ Start - phoneId: 0
09-29 16:20:23.771477  1669  1669 D SubscriptionController: [getSubInfoUsingSlotIndexPrivileged]+ slotIndex:0
09-29 16:20:23.777805  1669  1669 D SubscriptionController: [getSubInfoUsingSlotIndex]- null info return
09-29 16:20:23.777980  1669  1669 D MtkSubscriptionInfoUpdater: updateSubscriptionInfoByIccId: removing subscription info record: phoneId:0 oldIccId:N/A
09-29 16:20:23.783374  1669  1669 D SubscriptionController: activeSubscriptionInfoList is null.
09-29 16:20:23.789441  1669  1669 D SubscriptionController: [getSubInfoUsingSlotIndexPrivileged]+ slotIndex:0
09-29 16:20:23.793460  1669  1669 D SubscriptionController: [getSubInfoUsingSlotIndex]- null info return
09-29 16:20:23.794611  1669  1669 D MtkSubscriptionInfoUpdater: All IccIds query complete
09-29 16:20:23.795882  1669  1669 D MtkSubscriptionInfoUpdater: bypass reset default data sub if inactive
09-29 16:20:23.796061  1669  1669 D MtkSubscriptionInfoUpdater: SubInfo Initialized
09-29 16:20:23.798252  1669  1669 D MtkSubscriptionInfoUpdater: isNewSim newSim = false
09-29 16:20:23.799342  1669  1669 D MtkSubscriptionInfoUpdater: updateSubscriptionInfoByIccId: SubscriptionInfo update complete
09-29 16:20:23.799936  1251  1782 D TelephonyRegistry: notifySubscriptionInfoChanged: first invocation mRecords.size=35
09-29 16:20:23.805705  1669  1669 D MtkSubscriptionInfoUpdater: updateSubscriptionInfoByIccId: SubscriptionInfo update complete: phoneId0 detectedType = 4 subCount = 0
09-29 16:20:23.805937  1669  1669 D MtkSubscriptionInfoUpdater: All IccIds query complete
09-29 16:20:23.806075  1669  1669 D MtkSubscriptionInfoUpdater: Notify Subscription all Loaded.
09-29 16:20:23.806416  1669  1669 D MtkSuppServHelper: [0]handleMessage: EVENT_DATA_CONNECTION_DETACHED(3)
09-29 16:20:23.806479  1669  1669 D MtkSuppServHelper: [0]handleMessage: EVENT_ICC_CHANGED(13)
09-29 16:20:23.806499  1669  1669 D MtkSuppServHelper: [0]Bypass msg: 13
09-29 16:20:23.808341  1669  1669 D ImsPhoneCallTracker: [0] handleMessage what=23
09-29 16:20:23.808363  1669  1669 D ImsPhoneCallTracker: [0] handleMessage what=23
09-29 16:20:23.808379  1669  1669 D ImsPhoneCallTracker: [0] onDataEnabledChanged: enabled=true, reason=0
09-29 16:20:23.808394  1669  1669 D ImsPhoneCallTracker: [0] Ignore data enabled - carrier policy indicates that data is not metered for ViLTE calls.
09-29 16:20:23.809195  1669  1669 D MtkImsManager [0]: createMtkImsService binder is null
09-29 16:20:23.811732  1669  1669 D ImsPhoneCallTracker: [0] handleMessage what=102
09-29 16:20:23.811946  1669  1669 D ImsPhoneCallTracker: [0] onDataRoamingOff
09-29 16:20:23.812069  1669  1669 D ImsPhoneCallTracker: [0] onDataRoamingOff: device already not roaming. ignored the update.
09-29 16:20:23.812858  1669  1669 D MTKSST  : [GsmSST0] EVENT_IMS_SERVICE_STATE_CHANGED
09-29 16:20:23.813231  1669  1669 D PhoneCfgMgr: Received EVENT_RADIO_AVAILABLE/EVENT_RADIO_ON
09-29 16:20:23.816131  1669  1669 D RILJ    : [0094]> GET_MODEM_STATUS [PHONE0]
09-29 16:20:23.816548  1176  1176 I RIL-Fusion: getRadioState(): radioState=10
09-29 16:20:23.816758  1669  1669 D PhoneCfgMgr: getStaticPhoneCapability: sending the request for getting PhoneCapability
09-29 16:20:23.816964  1669  1669 D RadioConfig: [0095]> GET_PHONE_CAPABILITY
09-29 16:20:23.817416  1176  1176 D RadioConfig_service: radioConfig::getPhoneCapability serial=95
09-29 16:20:23.817441  1669  1811 D RILJ    : [0094]< GET_MODEM_STATUS true [PHONE0]
09-29 16:20:23.817574  1669  1669 D PhoneCfgMgr: getStaticPhoneCapability: mStaticCapability mMaxActiveVoiceSubscriptions=1 mMaxActiveDataSubscriptions=1 mNetworkValidationBeforeSwitchSupported=false mDeviceNrCapability []
09-29 16:20:23.817996  1669  1669 D ImsPhoneCallTracker: [0] handleMessage what=23
09-29 16:20:23.818031  1669  1669 D ImsPhoneCallTracker: [0] handleMessage what=23
09-29 16:20:23.818052  1669  1669 D ImsPhoneCallTracker: [0] onDataEnabledChanged: enabled=true, reason=0
09-29 16:20:23.818070  1669  1669 D ImsPhoneCallTracker: [0] Ignore data enabled - carrier policy indicates that data is not metered for ViLTE calls.
09-29 16:20:23.818469  1669  1669 D PhoneSwitcher: No active subscriptions: resetting preferred phone to 0 for emergency
09-29 16:20:23.818828  1669  1669 D PhoneSwitcher: evaluating due to EVENT_DATA_ENABLED_CHANGED phone[0] 0->-1
09-29 16:20:23.819138  1669  1669 D PhoneSwitcher: sendRilCommands: setPreferredDataModem - phoneId: 0
09-29 16:20:23.819404  1669  1669 D RadioConfig: [0096]> SET_PREFERRED_DATA_MODEM
09-29 16:20:23.819709  1669  1669 D PhoneSwitcher: logDataSwitchEvent subId -1 state 1 reason 2
09-29 16:20:23.819751  1176  1176 D RadioConfig_service: radioConfig::setPreferredDataModem serial=96
09-29 16:20:23.820366  1669  1811 D RadioConfigResponse: [0095]< GET_PHONE_CAPABILITY mMaxActiveVoiceSubscriptions=0 mMaxActiveDataSubscriptions=1 mNetworkValidationBeforeSwitchSupported=false mDeviceNrCapability []
09-29 16:20:23.825402  1176  1182 I RTC_DAC : [-1] getAllowDataSlot slot prop = 0
09-29 16:20:23.825708  1669  1811 D RadioConfigResponse: [0096]< SET_PREFERRED_DATA_MODEM
09-29 16:20:23.848291  1669  1669 D DebugService: DebugService DebugService:
09-29 16:20:23.852504  1669  1669 D UiccSlot: Creating
09-29 16:20:23.852777  1669  1669 D MtkUiccSlot: Creating
09-29 16:20:23.853011  1669  1669 D UiccSlot: cardStatus[0] update: IccCardState {CARDSTATE_ABSENT,PINSTATE_UNKNOWN,num_apps=0,gsm_id=-1,cdma_id=-1,ims_id=-1,physical_slot_id=0,atr=,iccid=,eid=}
09-29 16:20:23.853185  1669  1669 E AnswerToReset: Valid ATR string must at least contains TS and T0.
09-29 16:20:23.853506  1669  1669 D UiccSlot: update: radioState=1 mLastRadioState=2
09-29 16:20:23.855577  1669  1669 D SubscriptionInfoUpdater: updateInternalIccState to simStatus ABSENT reason null phoneId 0
09-29 16:20:23.856133  1669  1844 D SuppServConf: [0]handleMessage msg: EVENT_ICC_CHANGED
09-29 16:20:23.856725  1669  1669 D UiccSlot: cardStatus[0] update: IccCardState {CARDSTATE_ABSENT,PINSTATE_UNKNOWN,num_apps=0,gsm_id=-1,cdma_id=-1,ims_id=-1,physical_slot_id=0,atr=,iccid=,eid=}
09-29 16:20:23.856887  1669  1669 E AnswerToReset: Valid ATR string must at least contains TS and T0.
09-29 16:20:23.856975  1669  1669 D UiccSlot: update: radioState=1 mLastRadioState=1
09-29 16:20:23.857982  1669  1844 D SuppServConf: [0]handleMessage msg: EVENT_ICC_CHANGED
09-29 16:20:23.858243  1669  1669 D UiccSlot: cardStatus[0] update: IccCardState {CARDSTATE_ABSENT,PINSTATE_UNKNOWN,num_apps=0,gsm_id=-1,cdma_id=-1,ims_id=-1,physical_slot_id=0,atr=,iccid=,eid=}
09-29 16:20:23.858317  1669  1669 E AnswerToReset: Valid ATR string must at least contains TS and T0.
09-29 16:20:23.858381  1669  1669 D UiccSlot: update: radioState=1 mLastRadioState=1
09-29 16:20:23.858588  1669  1844 D SuppServConf: [0]handleMessage msg: EVENT_ICC_CHANGED
09-29 16:20:23.860552  1669  1669 D QualifiedNetworksService: Qualified networks service created
09-29 16:20:23.865149  1669  1669 D NetworkService: network service created
09-29 16:20:23.868867  1669  1669 D NetworkService: network service created
09-29 16:20:23.869587  1669  1669 D IWlanNetworkService: IWlanNetworkService init.
09-29 16:20:23.870530  1669  1874 D IWlanNetworkService: No MwiService exist
09-29 16:20:23.870652  1669  1874 D IWlanNetworkService: checkAndBindWifiOffloadService: sWifiOffloadService = null
09-29 16:20:23.870939  1669  1874 E IWlanNetworkService: can't get WifiOffloadService, retry after 1s.
09-29 16:20:23.884417  1669  1669 D MTKSST  : [GsmSST0] new:{level:0, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=2147483647 ber=2147483647 rscp=2147483647 ecno=2147483647 level=0,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthLte}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}, old:{level:0, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=2147483647 ber=2147483647 rscp=2147483647 ecno=2147483647 level=0,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthLte}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=false, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}
09-29 16:20:23.885543  1251  1782 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:23.885700  1251  1782 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:23.888068  1251  1782 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:23.888594  1251  1782 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:23.890265  1669  1669 D MTKSST  : [GsmSST0] onNetworkStateChangeResult state:0 Act:0 cause:0
09-29 16:20:23.891170  1669  1669 D MTKSST  : [GsmSST0] handle EVENT_RADIO_STATE_CHANGED
09-29 16:20:23.891842  1669  1669 D RatConfig: getActiveRatConfig: Lf/Lt/W/G
09-29 16:20:23.893472  1669  1669 D MtkTelephonyManagerEx: simSwitchMode result = 3
09-29 16:20:23.893969  1669  1669 D MTKSST  : [GsmSST0] setRadioPowerForReason power:true, mDesiredPowerState:true, forEmergencyCall:false, isSelectedPhoneForEmergencyCall:false, forceApply:false, radioState:1, reason:0
09-29 16:20:23.894219  1669  1669 D MTKSST  : [GsmSST0] setRadioPowerForReason mDesiredPowerState is already true Do nothing.
09-29 16:20:23.898808  1669  1669 D MtkRILJ : [0097]> MTK: RIL_REQUEST_SET_VENDOR_SETTING [SUB0]
09-29 16:20:23.900288  1669  1669 D MTKSST  : [GsmSST0] pollState: modemTriggered=true, mPollingContext=0, RadioState=1, connected=false, support_ap_iwlan=1
09-29 16:20:23.900602  1669  1669 D MTKSST  : [GsmSST0] Skip pollState due to disconnection of service
09-29 16:20:23.901035  1669  1669 V MtkSmsStorageMonitor: Sending pending memory status report : mStorageAvailable = true
09-29 16:20:23.902598  1669  1669 D RILJ    : [0098]> REPORT_SMS_MEMORY_STATUS available = true [PHONE0]
09-29 16:20:23.904379  1669  1669 D RILJ    : [0099]> GET_CURRENT_CALLS [PHONE0]
09-29 16:20:23.904852  1669  1811 D RILJ    : [0097]< MTK: RIL_REQUEST_SET_VENDOR_SETTING  [PHONE0]
09-29 16:20:23.904885  1176  1196 E RmcGsmSmsRequest: [0] SIM card was removed!
09-29 16:20:23.906410  1669  1669 D RILJ    : [0100]> IMS_REGISTRATION_STATE [PHONE0]
09-29 16:20:23.906746  1669  1811 D RILJ    : [0098]< REPORT_SMS_MEMORY_STATUS error 11 [PHONE0]
09-29 16:20:23.906800  1176  1194 D RmcCCReqHandler: [0] onHandleRequest: RFX_MSG_REQUEST_GET_CURRENT_CALLS
09-29 16:20:23.906847  1176  1194 D RmcCCBaseHandler: [0] isGsmRat, voiceRadioTech:0
09-29 16:20:23.906889  1176  1194 I AT      : [0] AT> AT+CLCC=*** (RIL_CMD_READER_2, tid:493437472000)
09-29 16:20:23.908220  1669  1669 D RILJ    : [0101]> VOICE_RADIO_TECH [PHONE0]
09-29 16:20:23.908443  1669  1811 D RilRequest: [0098]< REPORT_SMS_MEMORY_STATUS error: com.android.internal.telephony.CommandException: SIM_ABSENT ret= result={ when=-32s728ms what=2 target=com.mediatek.internal.telephony.MtkSmsStorageMonitor }
09-29 16:20:23.908825  1176  1196 I AT      : [0] AT> AT+CIREG? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:23.909617  1176  1193 I AT      : [0] AT< OK (RIL_CMD_READER_2, tid:493438508288)
09-29 16:20:23.909994  1669  1811 D RILJ    : [0101]< VOICE_RADIO_TECH {1} [PHONE0]
09-29 16:20:23.910869  1669  1811 D RILJ    : [0099]< GET_CURRENT_CALLS {} [PHONE0]
09-29 16:20:23.911503  1176  1195 I AT      : [0] AT< +CIREG: 2,0,0 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:23.911597  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:23.912363  1669  1669 D RILJ    : [0102]> CDMA_GET_SUBSCRIPTION_SOURCE [PHONE0]
09-29 16:20:23.912839  1669  1669 D PhoneSwitcher: updateHalCommandToUse, preferred mode already, no need update.
09-29 16:20:23.913628  1669  1669 D PhoneSwitcher: evaluating due to EVENT_RADIO_ON
09-29 16:20:23.913867  1669  1811 D RILJ    : [0100]< IMS_REGISTRATION_STATE {0, 2} [PHONE0]
09-29 16:20:23.913934  1669  1669 D PhoneSwitcher: sendRilCommands: setPreferredDataModem - phoneId: 0
09-29 16:20:23.914130  1669  1669 D RadioConfig: [0103]> SET_PREFERRED_DATA_MODEM
09-29 16:20:23.914692  1669  1669 D MTKSST  : [GsmSST0] onNetworkStateChangeResult state:2 Act:0 cause:0
09-29 16:20:23.914734  1176  1176 D RadioConfig_service: radioConfig::setPreferredDataModem serial=103
09-29 16:20:23.915152  1669  1669 D NetworkTypeController: [0] LegacyState: process EVENT_DATA_RAT_CHANGED
09-29 16:20:23.915507  1669  1669 D NetworkTypeController: [0] Remove all timers
09-29 16:20:23.915776  1669  1669 D NetworkTypeController: [0] Remove all timers
09-29 16:20:23.915994  1669  1669 D MtkNetworkTypeController: [Override]getCurrentOverrideNetworkType: 0
09-29 16:20:23.916712  1176  1196 E RmcGsmSimRequest: [0] Not support the request!
09-29 16:20:23.917101  1669  1669 D MTKSST  : [GsmSST0] onNetworkStateChangeResult state:2 Act:0 cause:0
09-29 16:20:23.918895  1669  1811 D RILJ    : [0102]< CDMA_GET_SUBSCRIPTION_SOURCE error 6 [PHONE0]
09-29 16:20:23.919048  1669  1811 D RilRequest: [0102]< CDMA_GET_SUBSCRIPTION_SOURCE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret={-1} result={ when=-32s739ms what=2 target=com.mediatek.internal.telephony.cdma.MtkCdmaSubscriptionSourceManager }
09-29 16:20:23.920317  1176  1182 I RTC_DAC : [-1] getAllowDataSlot slot prop = 0
09-29 16:20:23.922218  1669  1669 D DataService: Data service created
09-29 16:20:23.923964  1669  1811 D RadioConfigResponse: [0103]< SET_PREFERRED_DATA_MODEM
09-29 16:20:23.927182  1669  1669 D DataService: Data service created
09-29 16:20:23.929964  1669  1669 D MTKSST  : [GsmSST0] SubscriptionListener.onSubscriptionInfoChanged
09-29 16:20:23.930642  1669  1669 D ImsPhoneCallTracker: [0] SubscriptionListener.onSubscriptionInfoChanged, subId=-1
09-29 16:20:23.943543  1669  1669 E PhoneSubInfoController: getLine1Number phone is null for Subscription:-1
09-29 16:20:23.997781  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:1
09-29 16:20:23.998412  1669  1669 E MtkImsManagerIM [0]: isImsResourceSupport() failed!com.android.ims.ImsException: Service is unavailable(106)
09-29 16:20:23.998489  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(1) return true
09-29 16:20:23.998506  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:7
09-29 16:20:23.998667  1669  1669 E MtkImsManagerIM [0]: isImsResourceSupport() failed!com.android.ims.ImsException: Service is unavailable(106)
09-29 16:20:23.998700  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(7) return true
09-29 16:20:24.000348  1669  1669 D MtkImsManagerIM [0]: Vt, isVilteResourceSupport:true, isVinrResourceSupport:true, isCarrierConfigSupport:true, isGbaValidSupport:true, isFeatureEnableByPlatformExt:true
09-29 16:20:24.017630  1669  1669 D DSSExt  : handleSubinfoRecordUpdated: detectedType = 4
09-29 16:20:24.017841  1669  1669 D DSSExt  : getHighCapabilityPhoneIdBySimType : -1
09-29 16:20:24.018263  1669  1669 D DSSExt  : DataSubSelector for OM: no pin lock
09-29 16:20:24.019986  1669  1669 D DSSExt  : Default data phoneid = -1
09-29 16:20:24.038604  1669  1669 D SubscriptionController: [setDefaultVoiceSubId] default phone account not changed
09-29 16:20:24.050624  1669  1669 D PhoneSwitcher: onDdsSwitchResponse: DDS switch success on phoneId = 0
09-29 16:20:24.050892  1669  1669 D PhoneSwitcher: notifyPreferredDataSubIdChanged to -1
09-29 16:20:24.053146  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=7, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 1000 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:24.053938  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=31, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10099 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:24.054544  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=29, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10102 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:24.055141  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=27, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10104 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:24.055795  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=33, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 1000 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:24.056459  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=14, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10123 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:24.057075  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=18, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10119 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:24.057682  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=35, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 1073 RequestorUid: 1073 RequestorPkg: com.google.android.networkstack UnderlyingNetworks: Null] ]
09-29 16:20:24.058317  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=40, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10134 RequestorUid: 10134 RequestorPkg: com.android.systemui UnderlyingNetworks: Null] ]
09-29 16:20:24.058969  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN&NOT_VCN_MANAGED RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:24.059360  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=42, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10134 RequestorUid: 10134 RequestorPkg: com.android.systemui UnderlyingNetworks: Null] ]
09-29 16:20:24.059988  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=23, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10115 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:24.060554  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=25, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10111 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:24.061534  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=49, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 1001 RequestorUid: 1001 RequestorPkg: com.android.phone UnderlyingNetworks: Null] ]
09-29 16:20:24.063631  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=47, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 1001 RequestorUid: 1001 RequestorPkg: com.android.phone UnderlyingNetworks: Null] ]
09-29 16:20:24.064899  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=16, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10122 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:24.065657  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=20, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10116 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:24.066271  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ BACKGROUND_REQUEST id=2, [ Transports: CELLULAR Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN&NOT_VCN_MANAGED RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:24.068675  1669  1669 D MtkSubscriptionInfoUpdater: updateSubscriptionInfoByIccId:+ Start - phoneId: 0
09-29 16:20:24.069079  1669  1669 D SubscriptionController: [getSubInfoUsingSlotIndexPrivileged]+ slotIndex:0
09-29 16:20:24.072523  1669  1669 D SubscriptionController: [getSubInfoUsingSlotIndex]- null info return
09-29 16:20:24.072761  1669  1669 D MtkSubscriptionInfoUpdater: updateSubscriptionInfoByIccId: removing subscription info record: phoneId:0 oldIccId:N/A
09-29 16:20:24.077138  1669  1669 D SubscriptionController: activeSubscriptionInfoList is null.
09-29 16:20:24.082204  1669  1669 D SubscriptionController: [getSubInfoUsingSlotIndexPrivileged]+ slotIndex:0
09-29 16:20:24.085603  1669  1669 D SubscriptionController: [getSubInfoUsingSlotIndex]- null info return
09-29 16:20:24.087199  1669  1669 D MtkSubscriptionInfoUpdater: All IccIds query complete
09-29 16:20:24.087516  1669  1669 D MtkSubscriptionInfoUpdater: bypass reset default data sub if inactive
09-29 16:20:24.087577  1669  1669 D MtkSubscriptionInfoUpdater: isNewSim newSim = false
09-29 16:20:24.089802  1669  1669 D MtkSubscriptionInfoUpdater: updateSubscriptionInfoByIccId: SubscriptionInfo update complete
09-29 16:20:24.094880  1669  1669 D MtkSubscriptionInfoUpdater: updateSubscriptionInfoByIccId: SubscriptionInfo update complete: phoneId0 detectedType = 4 subCount = 0
09-29 16:20:24.094971  1669  1669 D MtkSubscriptionInfoUpdater: All IccIds query complete
09-29 16:20:24.094994  1669  1669 D MtkSubscriptionInfoUpdater: Notify Subscription all Loaded.
09-29 16:20:24.095256  1669  1669 D SubscriptionManager: putPhoneIdAndSubIdExtra: no valid subs
09-29 16:20:24.095371  1669  1669 D SubscriptionInfoUpdater: Broadcasting intent ACTION_SIM_STATE_CHANGED ABSENT reason null for phone: 0
09-29 16:20:24.097173  1669  1669 D SubscriptionManager: putPhoneIdAndSubIdExtra: no valid subs
09-29 16:20:24.097377  1669  1669 D SubscriptionInfoUpdater: Broadcasting intent ACTION_SIM_CARD_STATE_CHANGED ABSENT for phone: 0 slot: 0
09-29 16:20:24.099232  1669  1669 D CarrierResolver: [resolveSubscriptionCarrierId] simState: ABSENT
09-29 16:20:24.102174  1872  1872 I ImsApp  : ImsApp onCreate begin
09-29 16:20:24.103480  1872  1872 I IMS_RILA: Ims-RIL: init phone = 0
09-29 16:20:24.104576  1669  1669 D MtkGsmCdmaPhone: EVENT_ICC_CHANGED, phone id = 0, result = 0
09-29 16:20:24.105141  1669  1669 E GsmCdmaPhone: [0] reapplyUiccAppsEnablementIfNeeded(), CardState=CARDSTATE_ABSENT ,mUiccApplicationsEnabled = null
09-29 16:20:24.107054  1669  1669 D MtkGsmCdmaPhone: isPhoneTypeCdmaLte:false, phoneId: 0 isCdmaWithoutLteCard: false mNewVoiceTech: 1
09-29 16:20:24.107225  1669  1669 D MtkGsmSMSDispatcher: EVENT_ICC_CHANGED, PhoneId: 0 match exactly.
09-29 16:20:24.107345  1669  1669 D GsmSMSDispatcher: GsmSMSDispatcher: subId = -1 slotId = 0
09-29 16:20:24.107541  1669  1669 D MTKSST  : [GsmSST0] EVENT_ICC_CHANGED: SIM absent
09-29 16:20:24.107625  1669  1669 D MTKSST  : [GsmSST0] cancelAllNotifications: mPrevSubId=-1
09-29 16:20:24.110628  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: radio is on but out of service, set plmn='No service'
09-29 16:20:24.111552  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: rawSpn = 
09-29 16:20:24.112056  1669  1669 D CarrierResolver: handleMessage: 2
09-29 16:20:24.112235  1669  1669 D MtkSuppServHelper: [0]handleMessage: EVENT_ICC_CHANGED(13)
09-29 16:20:24.112302  1669  1669 D MtkSuppServHelper: [0]Bypass msg: 13
09-29 16:20:24.112378  1669  1669 D MtkGsmCdmaPhone: EVENT_ICC_CHANGED, phone id = 0, result = 0
09-29 16:20:24.112491  1669  1669 E GsmCdmaPhone: [0] reapplyUiccAppsEnablementIfNeeded(), CardState=CARDSTATE_ABSENT ,mUiccApplicationsEnabled = null
09-29 16:20:24.114187  1872  1872 E IMS_RILA: getRadioProxy: mRadioVersion 1.5 [SUB0]
09-29 16:20:24.114923  1872  1872 I IMS_RILA: getRadioProxy: android.hardware.radio@1.6::IRadio@Proxy [SUB0]
09-29 16:20:24.115589  1176  1176 I RILC    : setResponseFunctions, slotId = 4
09-29 16:20:24.119434  1176  1176 I RIL-Fusion: getRadioState(): radioState=10
09-29 16:20:24.119603  1176  1176 E RILC    : radioStateChangedInd: radioService[8]->mRadioIndication == NULL
09-29 16:20:24.119621  1176  1176 E RILC    : radioStateChangedInd: radioService[12]->mRadioIndication == NULL
09-29 16:20:24.119698  1176  1176 I RILC    : onNewCommandConnect, slot 0, client 2
09-29 16:20:24.119780  1176  1178 I RILC    : sendPendedUrcCallback 1 0 2
09-29 16:20:24.120212  1872  1872 I IMS_RILA: setResponseFunctionsIms [SUB0]
09-29 16:20:24.120386  1872  1872 I IMS_RILA: Ims-RIL: proxy = false [SUB0]
09-29 16:20:24.120809  1669  1669 D MtkGsmCdmaPhone: isPhoneTypeCdmaLte:false, phoneId: 0 isCdmaWithoutLteCard: false mNewVoiceTech: 1
09-29 16:20:24.121124  1669  1669 D MtkGsmSMSDispatcher: EVENT_ICC_CHANGED, PhoneId: 0 match exactly.
09-29 16:20:24.121337  1669  1669 D GsmSMSDispatcher: GsmSMSDispatcher: subId = -1 slotId = 0
09-29 16:20:24.121634  1669  1669 D MTKSST  : [GsmSST0] EVENT_ICC_CHANGED: SIM absent
09-29 16:20:24.121786  1669  1669 D MTKSST  : [GsmSST0] cancelAllNotifications: mPrevSubId=-1
09-29 16:20:24.121899  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:24.122012  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_RADIO_STATE_CHANGED radioStateChanged: 1 [PHONE0]
09-29 16:20:24.126345  1872  1872 I IMS_RILA: getMtkRadioProxy mMtkRadioVersion = 3.0 [SUB0]
09-29 16:20:24.126946  1176  1176 I RILC    : setResponseFunctionsIms, slotId = 4
09-29 16:20:24.127060  1176  1176 I RILC    : onNewCommandConnect, slot 0, client 3
09-29 16:20:24.127168  1176  1178 I RILC    : sendPendedUrcCallback 1 0 3
09-29 16:20:24.127188  1176  1178 I RILC    : sendPendedUrcs RIL_SOCKET_1, RIL_UNSOL_IMS_REGISTRATION_INFO, client 3
09-29 16:20:24.127780  1176  1178 I RILC    : sendPendedUrcs RIL_SOCKET_1, RIL_UNSOL_IMS_BEARER_INIT, client 3
09-29 16:20:24.127868  1176  1178 I RILC    : sendPendedUrcs RIL_SOCKET_1, RIL_UNSOL_IMS_ENABLE_START, client 3
09-29 16:20:24.127988  1872  1872 D OpImsRILUtil: OP packages classes are not found
09-29 16:20:24.128043  1872  1872 D OpImsRILUtil: Load default OP packages
09-29 16:20:24.128665  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: radio is on but out of service, set plmn='No service'
09-29 16:20:24.128892  1872  1872 D ImsDataTracker: mIsBearerNotify rule set to 1
09-29 16:20:24.130759  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: rawSpn = 
09-29 16:20:24.131827  1669  1669 D CarrierResolver: handleMessage: 2
09-29 16:20:24.133483  1669  1669 D MtkSuppServHelper: [0]handleMessage: EVENT_ICC_CHANGED(13)
09-29 16:20:24.133670  1669  1669 D MtkSuppServHelper: [0]Bypass msg: 13
09-29 16:20:24.133774  1669  1669 D MtkGsmCdmaPhone: EVENT_ICC_CHANGED, phone id = 0, result = 0
09-29 16:20:24.133931  1669  1669 E GsmCdmaPhone: [0] reapplyUiccAppsEnablementIfNeeded(), CardState=CARDSTATE_ABSENT ,mUiccApplicationsEnabled = null
09-29 16:20:24.134271  1872  1912 D DC-ims[0]: DefaultState: enter
09-29 16:20:24.134358  1872  1912 D DC-ims[0]: InactiveState: refreshNetworkLostListener
09-29 16:20:24.134496  1872  1872 D ImsDataTracker: setImsBearerNotification enable: 1
09-29 16:20:24.134547  1669  1669 D MtkGsmCdmaPhone: isPhoneTypeCdmaLte:false, phoneId: 0 isCdmaWithoutLteCard: false mNewVoiceTech: 1
09-29 16:20:24.134646  1669  1669 D MtkGsmSMSDispatcher: EVENT_ICC_CHANGED, PhoneId: 0 match exactly.
09-29 16:20:24.134690  1669  1669 D GsmSMSDispatcher: GsmSMSDispatcher: subId = -1 slotId = 0
09-29 16:20:24.134690  1872  1912 E DC-ims[0]: InactiveState: cb already has been released!!
09-29 16:20:24.134726  1872  1912 D DC-ims[0]: InactiveState: refreshNetworkLostListener, uid = 1001, package name: com.mediatek.ims
09-29 16:20:24.134783  1669  1669 D MTKSST  : [GsmSST0] EVENT_ICC_CHANGED: SIM absent
09-29 16:20:24.134800  1669  1669 D MTKSST  : [GsmSST0] cancelAllNotifications: mPrevSubId=-1
09-29 16:20:24.137709  1872  1872 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.mediatek.ims listener=com.mediatek.ims.internal.ImsDataTracker$2@79a6808
09-29 16:20:24.138634  1176  1208 D RmcDcImsDc2ReqHandler: [0][checkImsServiceRestartAfterSystemCrash] vendor.ril.zygote.state=
09-29 16:20:24.138699  1176  1208 D RmcDcImsDc2ReqHandler: [0][notifyUnsyncImsBearerRequest] ims State=0
09-29 16:20:24.138714  1176  1208 I RmcDcImsDc2ReqHandler: [0][notifyUnsyncImsBearerRequest] no ongoing ACTIVATED or DEACTIVATED event
09-29 16:20:24.138730  1176  1208 E RmcDcImsDc2ReqHandler: [0][handleImsBearerNotificationSet] isEnableBearerNotification: 1
09-29 16:20:24.145710  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: radio is on but out of service, set plmn='No service'
09-29 16:20:24.146409  1872  1912 D DC-ims[0]: InactiveState:  enter
09-29 16:20:24.146518  1872  1912 D DC-emergency[0]: DefaultState: enter
09-29 16:20:24.146536  1872  1912 D DC-emergency[0]: InactiveState: refreshNetworkLostListener
09-29 16:20:24.147264  1872  1912 E DC-emergency[0]: InactiveState: cb already has been released!!
09-29 16:20:24.147329  1872  1912 D DC-emergency[0]: InactiveState: refreshNetworkLostListener, uid = 1001, package name: com.mediatek.ims
09-29 16:20:24.150135  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: rawSpn = 
09-29 16:20:24.150599  1669  1669 D CarrierResolver: handleMessage: 2
09-29 16:20:24.150831  1669  1669 D MtkSuppServHelper: [0]handleMessage: EVENT_ICC_CHANGED(13)
09-29 16:20:24.150843  1872  1872 D ImsConfigEventReceiver[0]: init with phoneId:0, simState = 1, carrier config loaded: true
09-29 16:20:24.150949  1669  1669 D MtkSuppServHelper: [0]Bypass msg: 13
09-29 16:20:24.151109  1872  1912 D DC-emergency[0]: InactiveState:  enter
09-29 16:20:24.152661  1669  1669 D NRM-C-0 : service ComponentInfo{com.android.phone/com.android.internal.telephony.CellularNetworkService} for transport WWAN is now connected.
09-29 16:20:24.153116  1669  1870 D MtkQualifiedNetworksService: MtkQNS create MtkNetworkAvailabilityProvider for slot 0
09-29 16:20:24.153214  1669  1669 D NRM-I-0 : service ComponentInfo{com.android.phone/com.mediatek.internal.telephony.IWlanNetworkService} for transport WLAN is now connected.
09-29 16:20:24.153446  1669  1873 D IWlanNetworkService: IWlan network service created for slot 0
09-29 16:20:24.153547  1669  1669 V SmsStorageMonitor: Memory status report to modem pending : mStorageAvailable = true
09-29 16:20:24.153650  1669  1873 D IWlanNetworkService: IWlanNetworkServiceProvider construct.
09-29 16:20:24.153814  1669  1669 D MtkGsmCdmaPhone: correctPhoneTypeForCdma: change:false newVoiceRadioTech=1 mActivePhone=GSM
09-29 16:20:24.153966  1669  1669 D GsmCdmaCallTracker: Event EVENT_POLL_CALLS_RESULT Received
09-29 16:20:24.154021  1669  1669 D GsmCdmaCallTracker: [0] update phone state, old=IDLE new=IDLE
09-29 16:20:24.154266  1669  1669 D SmsDispatchersController: IMS registration state: false format: 3gpp2
09-29 16:20:24.154428  1669  1669 D CdmaSSM : CDMA_SUBSCRIPTION_SOURCE event = 2
09-29 16:20:24.154652  1669  1669 W CdmaSSM : Unable to get CDMA Subscription Source, Exception: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED, result: [I@4f90b1f
09-29 16:20:24.154837  1669  1669 D PhoneSwitcher: onDdsSwitchResponse: DDS switch success on phoneId = 0
09-29 16:20:24.155024  1669  1669 D PhoneSwitcher: notifyPreferredDataSubIdChanged to -1
09-29 16:20:24.159300  1669  1669 D DSM-C-0 : onServiceConnected
09-29 16:20:24.160792  1669  1870 D MtkQualifiedNetworksService: Register for qualified networks changed.
09-29 16:20:24.161094  1872  1872 D MtkImsManager [0]: createMtkImsService binder is null
09-29 16:20:24.161252  1669  1919 D MtkQualifiedNetworksService: UPDATE_QUALIFIED_NETWORKS mode=1 apnTypes=2178
09-29 16:20:24.161643  1669  1885 D CellularDataService: Cellular data service created for slot 0
09-29 16:20:24.161915  1669  1919 D MtkQualifiedNetworksService: availabilityUpdate[2]=3
09-29 16:20:24.163972  1669  1669 D DSM-I-0 : onServiceConnected
09-29 16:20:24.164170  1669  1870 D ANM-0   : onQualifiedNetworkTypesChanged. apnTypes = [mms,cbs,xcap], networks = [EUTRAN]
09-29 16:20:24.165041  1669  1889 D IwlanDataService: IWLAN data service created for slot 0
09-29 16:20:24.167043  1669  1669 E PhoneSubInfoController: getLine1Number phone is null for Subscription:-1
09-29 16:20:24.167232  1669  1889 D IwlanDataService: Register for data call list changed.
09-29 16:20:24.167419  1669  1889 D IwlanDataService: Register for apn unthrottled.
09-29 16:20:24.218000  1872  1872 D SuppServExt: [0]MtkSuppServExt init done.
09-29 16:20:24.218168  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:1
09-29 16:20:24.218280  1872  1872 D ImsEventPackageAdapter: ImsEventPackageAdapter()
09-29 16:20:24.218409  1669  1669 E MtkImsManagerIM [0]: isImsResourceSupport() failed!com.android.ims.ImsException: Service is unavailable(106)
09-29 16:20:24.218428  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(1) return true
09-29 16:20:24.218440  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:7
09-29 16:20:24.218519  1669  1669 E MtkImsManagerIM [0]: isImsResourceSupport() failed!com.android.ims.ImsException: Service is unavailable(106)
09-29 16:20:24.218517  1872  1872 D ImsEventPackageAdapter: Use AOSP default ImsExternalCallState.
09-29 16:20:24.218532  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(7) return true
09-29 16:20:24.218732  1872  1916 D SuppServExt: [0]handleMessage: EVENT_RADIO_ON(4)
09-29 16:20:24.219441  1872  1916 D SuppServExt: [0]startHandleXcapQueryProcess(), forceQuery: false, reason: Radio on, checkCriteria: false, criteriaFailReason: No need to support for this operator OR carrier config not ready, 
09-29 16:20:24.220666  1669  1669 D MtkImsManagerIM [0]: Vt, isVilteResourceSupport:true, isVinrResourceSupport:true, isCarrierConfigSupport:true, isGbaValidSupport:true, isFeatureEnableByPlatformExt:true
09-29 16:20:24.221815  1176  1196 I AT      : [0] AT> AT+CIREG=2 (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:24.224495  1176  1184 I AT      : [0] AT< +CIREGU: 0 (RIL_URC_READER, tid:493447834880)
09-29 16:20:24.224631  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:24.226911  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=7, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 1000 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.227462  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=31, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10099 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.228031  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=29, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10102 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.228507  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=27, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10104 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.228731  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:24.228860  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_IMS_NETWORK_STATE_CHANGED [PHONE0]
09-29 16:20:24.228975  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=33, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 1000 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.229228  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=14, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10123 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.229437  1872  1916 D SuppServExt: [0]handleMessage: EVENT_IMS_REGISTRATION_INFO(1)
09-29 16:20:24.229492  1872  1916 D SuppServExt: [0]EVENT_IMS_REGISTRATION_INFO: 0
09-29 16:20:24.229636  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=18, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10119 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.230048  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=35, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 1073 RequestorUid: 1073 RequestorPkg: com.google.android.networkstack UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.230442  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=40, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10134 RequestorUid: 10134 RequestorPkg: com.android.systemui UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.230875  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN&NOT_VCN_MANAGED RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.231285  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=42, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10134 RequestorUid: 10134 RequestorPkg: com.android.systemui UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.231762  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=23, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10115 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.232243  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=25, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10111 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.232720  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=49, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 1001 RequestorUid: 1001 RequestorPkg: com.android.phone UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.233257  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=47, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 1001 RequestorUid: 1001 RequestorPkg: com.android.phone UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.233677  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=16, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10122 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.234014  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=20, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10116 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.234443  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ BACKGROUND_REQUEST id=2, [ Transports: CELLULAR Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN&NOT_VCN_MANAGED RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.234931  1669  1669 D MTKSST  : [GsmSST0] SubscriptionListener.onSubscriptionInfoChanged
09-29 16:20:24.235133  1669  1669 D ImsPhoneCallTracker: [0] SubscriptionListener.onSubscriptionInfoChanged, subId=-1
09-29 16:20:24.243193  1669  1669 E PhoneSubInfoController: getLine1Number phone is null for Subscription:-1
09-29 16:20:24.273211  1872  1872 D ImsManagerOemPluginBase: default isWfcSupport
09-29 16:20:24.285917  1872  1872 D WfoService: WfoService new MWIService
09-29 16:20:24.287172  1872  1872 D MWIS    : [MwiService] Construct MwiService
09-29 16:20:24.287975  1872  1872 D MWIS    : [MwiService] mSimCount: 1
09-29 16:20:24.294539  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:1
09-29 16:20:24.294842  1669  1669 E MtkImsManagerIM [0]: isImsResourceSupport() failed!com.android.ims.ImsException: Service is unavailable(106)
09-29 16:20:24.294872  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(1) return true
09-29 16:20:24.294883  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:7
09-29 16:20:24.294999  1669  1669 E MtkImsManagerIM [0]: isImsResourceSupport() failed!com.android.ims.ImsException: Service is unavailable(106)
09-29 16:20:24.295020  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(7) return true
09-29 16:20:24.295582  1872  1872 E MwiRIL  : mRadioProxy getService() done [SUB0]
09-29 16:20:24.295872  1872  1872 E MwiRIL  : mRadioProxy getService() done 2 [SUB0]
09-29 16:20:24.296106  1872  1872 E MwiRIL  : mRadioProxy linkToDeath() done [SUB0]
09-29 16:20:24.296623  1176  1176 I RILC    : setResponseFunctionsMwi
09-29 16:20:24.296783  1176  1176 I RILC    : onNewCommandConnect, slot 0, client 4
09-29 16:20:24.296881  1176  1178 I RILC    : sendPendedUrcCallback 1 0 4
09-29 16:20:24.296902  1669  1669 D MtkImsManagerIM [0]: Vt, isVilteResourceSupport:true, isVinrResourceSupport:true, isCarrierConfigSupport:true, isGbaValidSupport:true, isFeatureEnableByPlatformExt:true
09-29 16:20:24.297261  1872  1872 E MwiRIL  : mRadioProxy setResponseFunctionsMwi() done [SUB0]
09-29 16:20:24.300070  1872  1923 D WifiPdnHandler: initWifiManager.
09-29 16:20:24.326896  1176  1182 D RtcMwi  : [0] onHandleRequest: request id 60525 is RFX_MSG_REQUEST_SET_WFC_CONFIG
09-29 16:20:24.328073  1176  1196 D RmcMwi  : [0] setWfcConfig: 1, locenable, 1
09-29 16:20:24.328132  1176  1196 D RmcMwi  : [0] setWfcConfig_LocationSetting: 1, locenable, 1
09-29 16:20:24.328203  1176  1196 I AT      : [0] AT> AT+ELOCAEN=1 (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:24.328646  1669  1896 D MtkIccSmsInterfaceManager: Cell broadcast ranges reset.
09-29 16:20:24.332696  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:24.333399  1669  1669 D SubscriptionController: [setDefaultVoiceSubId] default phone account not changed
09-29 16:20:24.333637  1176  1182 D RtcMwi  : [0] onHandleResponse, handle RFX_MSG_REQUEST_SET_WFC_CONFIG
09-29 16:20:24.345516  1176  1182 D RtcMwi  : [0] onHandleRequest: request id 60523 is RFX_MSG_REQUEST_SET_WIFI_ENABLED
09-29 16:20:24.346081  1176  1196 D RmcMwi  : [0] setWifiEnabled dataLen: 3
09-29 16:20:24.346180  1872  1872 I ImsApp  : ImsApp onCreate end
09-29 16:20:24.346234  1176  1196 I AT      : [0] AT> AT+EWIFIEN="wlan0",0,0 (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:24.348061  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:24.348493  1176  1182 D RtcMwi  : [0] onHandleResponse, handle RFX_MSG_REQUEST_SET_WIFI_ENABLED
09-29 16:20:24.348700  1176  1182 D RtcMwi  : [0] onHandleRequest: request id 60526 is RFX_MSG_REQUEST_GET_WFC_CONFIG
09-29 16:20:24.349968  1176  1196 D RmcMwi  : [0] getWfcConfig: 2
09-29 16:20:24.350276  1176  1182 D RtcMwi  : [0] onHandleResponse, handle RFX_MSG_REQUEST_GET_WFC_CONFIG
09-29 16:20:24.356400  1872  1930 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.mediatek.ims listener=com.mediatek.ims.internal.ImsVTProviderUtil$1@6a4b39b
09-29 16:20:24.361913  1669  1669 D DSSExt  : handleSubinfoRecordUpdated: detectedType = 4
09-29 16:20:24.362039  1669  1669 D DSSExt  : getHighCapabilityPhoneIdBySimType : -1
09-29 16:20:24.362217  1669  1669 D DSSExt  : DataSubSelector for OM: no pin lock
09-29 16:20:24.363585  1669  1669 D DSSExt  : Default data phoneid = -1
09-29 16:20:24.372950  1872  1872 D MWIS    : [MwiService] getWfcHandlerInterface
09-29 16:20:24.374512  1669  1669 D SAT     : [0]onSimAbsent, reset activation state to UNKNOWN
09-29 16:20:24.377757  1669  1669 D SAT     : [0]setVoiceActivationState=0
09-29 16:20:24.384363  1669  1669 D SAT     : [0]setDataActivationState=0
09-29 16:20:24.385112  1176  1213 D VT RIL THD: [VT RIL THD] msg_type = 103002, recv_length = 12
09-29 16:20:24.385173  1176  1213 I VT RIL PSR: [VT  PARSER] MSG_ID_WRAP_IMSVT_RILD_VTSERVICE_STATUS
09-29 16:20:24.385193  1176  1213 D VT RIL THD: [VT RIL THD] slot_id = 0, msg_data.size = 20, msg_data.data = 12970367423018448528
09-29 16:20:24.386280  1669  1846 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 1 configurations
09-29 16:20:24.388521  1176  1212 I VT RIL RMC: [Handle EVT] event = 59524
09-29 16:20:24.388578  1176  1212 D VT RIL RMC: [VTREQ SENT] pSendMsg->size = 20, pSendMsg->data = 12970367423018447520
09-29 16:20:24.388592  1176  1212 I VT RIL RMC: [VTREQ SENT] RILD_IMS_CLIENT_READY
09-29 16:20:24.389689  1872  1872 W OperatorUtils: getMccMnc, mccMnc value:
09-29 16:20:24.390892  1669  1669 D MTKSST  : [GsmSST0] SIM state change, slotId: 0 simState[1]
09-29 16:20:24.395885  1669  1846 D RILJ    : [0106]> GSM_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:24.396164  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4370] Code [0,255] ENABLED [PHONE0]
09-29 16:20:24.397605  1176  1182 D RtcGsmSmsCtrl: [0] SMS Md isn't ready yet. queue RFX_MSG_REQUEST_GSM_SET_BROADCAST_SMS_CONFIG
09-29 16:20:24.400009  1176  1211 I AT      : [0] fragData.getDataLength(): 12
09-29 16:20:24.400086  1176  1211 I AT      : [0] ViLTE read count: 12
09-29 16:20:24.400103  1176  1211 I AT      : [0] ViLTE read total count: 12
09-29 16:20:24.400118  1176  1211 I AT      : [0] handleUserDataEvent, len:12, client 1
09-29 16:20:24.401238  1176  1182 D RtcMwi  : [0] onHandleRequest: request id 60524 is RFX_MSG_REQUEST_SET_WIFI_ASSOCIATED
09-29 16:20:24.401867  1176  1196 I AT      : [0] AT> AT+EWIFIASC=*** (RIL_CMD_READER_3, tid:493435399424)
09-29 16:20:24.402580  1176  1212 I VT RIL RMC: [Handle EVT] event = 55526
09-29 16:20:24.402656  1176  1212 I VT RIL RMC: [VTREQ RECV] data length = 12, slot = 0
09-29 16:20:24.403036  1176  1214 D VT RIL THD: [RIL IMCB THD] id = 101505, size = 4
09-29 16:20:24.404593  1669  1669 D RILJ    : [0107]> IMS_REGISTRATION_STATE [PHONE0]
09-29 16:20:24.405730  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:24.406766  1176  1196 I AT      : [0] AT> AT+CIREG? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:24.406911  1176  1182 D RtcMwi  : [0] onHandleResponse, handle RFX_MSG_REQUEST_SET_WIFI_ASSOCIATED
09-29 16:20:24.408535  1669  1669 D RILJ    : [0108]> IMS_REGISTRATION_STATE [PHONE0]
09-29 16:20:24.408950  1176  1182 D RtcMwi  : [0] onHandleRequest: request id 60523 is RFX_MSG_REQUEST_SET_WIFI_ENABLED
09-29 16:20:24.412387  1669  1669 E PhoneSubInfoController: getLine1Number phone is null for Subscription:-1
09-29 16:20:24.415607  1176  1195 I AT      : [0] AT< +CIREG: 2,0,0 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:24.415789  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:24.416092  1176  1196 D RmcMwi  : [0] setWifiEnabled dataLen: 3
09-29 16:20:24.416248  1176  1196 I AT      : [0] AT> AT+EWIFIEN="wlan0",0,0 (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:24.418681  1669  1811 D RILJ    : [0107]< IMS_REGISTRATION_STATE {0, 2} [PHONE0]
09-29 16:20:24.418998  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:24.419956  1176  1196 I AT      : [0] AT> AT+CIREG? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:24.419976  1176  1182 D RtcMwi  : [0] onHandleResponse, handle RFX_MSG_REQUEST_SET_WIFI_ENABLED
09-29 16:20:24.424428  1176  1213 D VT RIL THD: [VT RIL THD] msg_type = 101506, recv_length = 60076
09-29 16:20:24.424589  1176  1213 I VT RIL PSR: [VT  PARSER] MSG_ID_WRAP_IMSVT_IMCB_GET_CAP_RSP
09-29 16:20:24.424622  1176  1213 D VT RIL THD: [VT RIL THD] slot_id = 0, msg_data.size = 60084, msg_data.data = 12970367431071485984
09-29 16:20:24.425272  1176  1195 I AT      : [0] AT< +CIREG: 2,0,0 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:24.425446  1176  1212 I VT RIL RMC: [Handle EVT] event = 59524
09-29 16:20:24.425478  1176  1212 D VT RIL RMC: [VTREQ SENT] pSendMsg->size = 60084, pSendMsg->data = 12970367431071420432
09-29 16:20:24.426185  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:24.427550  1669  1811 D RILJ    : [0108]< IMS_REGISTRATION_STATE {0, 2} [PHONE0]
09-29 16:20:24.441640  1872  1872 E ImsManagerIM [0]: updateImsServiceConfig: invalid sub id, skipping!
09-29 16:20:24.447471  1872  1872 W OperatorUtils: getMccMnc, mccMnc value:
09-29 16:20:24.452468  1872  1872 D ImsDataTracker: onSubscriptionsChanged
09-29 16:20:24.453941  1872  1872 I ImsConfigEventReceiver[0]: ACTION_SIM_STATE_CHANGED, state:ABSENT, phoneId:0
09-29 16:20:24.454067  1872  1872 D ImsConfigEventReceiver[0]: ICC_ABSENT[0], reset carrier config loaded flag.
09-29 16:20:24.456193  1872  1872 W OperatorUtils: getMccMnc, mccMnc value:
09-29 16:20:24.459937  1176  1176 I RILC    : [0]Fire Pending indication UNSOL_RESPONSE_RADIO_STATE_CHANGED(0)
09-29 16:20:24.460011  1176  1176 I RIL-Fusion: getRadioState(): radioState=10
09-29 16:20:24.461107  1669  1896 E PhoneSubInfoController: getIccSerialNumber phone is null for Subscription:-1
09-29 16:20:24.463505  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:1
09-29 16:20:24.463861  1669  1669 E MtkImsManagerIM [0]: isImsResourceSupport() failed!com.android.ims.ImsException: Service is unavailable(106)
09-29 16:20:24.463919  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(1) return true
09-29 16:20:24.463932  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:7
09-29 16:20:24.464084  1669  1669 E MtkImsManagerIM [0]: isImsResourceSupport() failed!com.android.ims.ImsException: Service is unavailable(106)
09-29 16:20:24.464114  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(7) return true
09-29 16:20:24.467084  1669  1669 D MtkImsManagerIM [0]: Vt, isVilteResourceSupport:true, isVinrResourceSupport:true, isCarrierConfigSupport:true, isGbaValidSupport:true, isFeatureEnableByPlatformExt:true
09-29 16:20:24.487397  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=53, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 1001 RequestorUid: 1001 RequestorPkg: com.mediatek.ims UnderlyingNetworks: Null] ]
09-29 16:20:24.488070  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=55, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 1001 RequestorUid: 1001 RequestorPkg: com.mediatek.ims UnderlyingNetworks: Null] ]
09-29 16:20:24.538724  1669  1669 D MtkImsManagerIM [0]: ImsConnectionStateListener removed: com.mediatek.internal.telephony.imsphone.MtkImsPhoneCallTracker$2@8d1c6e8, size: 0
09-29 16:20:24.538995  1669  1669 D MtkImsManagerIM [0]: ImsConnectionStateListener added: com.mediatek.internal.telephony.imsphone.MtkImsPhoneCallTracker$2@8d1c6e8
09-29 16:20:24.539017  1669  1669 D MtkImsManagerIM [0]: hookProprietaryImsListener get NULL mMtkImsService so create it
09-29 16:20:24.540689  1669  1669 D MtkImsManagerIM [0]: mMtkImsService = com.mediatek.ims.internal.IMtkImsService$Stub$Proxy@b5c9101
09-29 16:20:24.540756  1669  1669 D MtkImsManagerIM [0]: [0] hook proprietary IMS listener
09-29 16:20:24.546554  1669  1669 E ImsPhoneCallTracker: [0] ACTION_MTK_IMS_SERVICE_UP: register ims succeed, com.mediatek.internal.telephony.imsphone.MtkImsPhoneCallTracker$2@8d1c6e8
09-29 16:20:24.551912  1872  1893 D MtkMmTelFeature: [0] Set context to com.mediatek.ims.ImsApp@75e91b5
09-29 16:20:24.554113  1872  1872 D ImsConfigEventReceiver[0]: resetWfcModeFlag, reason: ACTION_MTK_MMTEL_READY
09-29 16:20:24.554368  1872  1918 D ImsConfigController[0]: resetWfcModeFlag()
09-29 16:20:24.554468  1872  1893 W OperatorUtils: getMccMnc, mccMnc value:
09-29 16:20:24.554625  1872  1893 D MtkMmTelFeature: [0] notifyCapabilitiesStatusChanged MmTel Capabilities - [Voice: false Video: false UT: false SMS: false CALL_COMPOSER: false]
09-29 16:20:24.554709  1872  1872 D ImsConfigEventReceiver[0]: ACTION_MTK_MMTEL_READY, update IMS config with phoneId:0, simState = 1, carrier config loaded: false, defaultSupportVolte: true
09-29 16:20:24.555030  1872  1893 D MtkMmTelFeature: [0] initialize mContext com.mediatek.ims.ImsApp@75e91b5 slotId 0
09-29 16:20:24.555229  1872  1893 D MtkMmTelFeature: [0] [0] MtkMmTelFeature created
09-29 16:20:24.565623  1872  1891 D MtkRcsFeature: [0] initialize mContext com.mediatek.ims.MtkDynamicImsService@87efce0 slotId 0
09-29 16:20:24.565791  1872  1891 D MtkRcsFeature: [0] notifyContextChanged to [com.mediatek.ims.ImsApp@75e91b5]
09-29 16:20:24.565977  1872  1891 D MtkRcsFeature: [0] notifyCapabilitiesStatusChanged to [Capabilities: 10]
09-29 16:20:24.566038  1872  1891 D MtkRcsFeature: [0] MtkRcsFeature created
09-29 16:20:24.566360  1872  1891 D MtkRcsFeature: [0] onFeatureReady called!
09-29 16:20:24.570623  1669  1669 E CarrierActionAgent: [0]Unsupported action: 7
09-29 16:20:24.570740  1669  1669 D CarrierActionAgent: [0]EVENT_SIM_STATE_CHANGED status: ABSENT
09-29 16:20:24.571509  1669  1669 D PinStorage: SIM card/application changed[0]: ABSENT
09-29 16:20:24.572211  1669  1669 D LocaleTracker-0: updateLocale: countryIso = , countryIsoDebugInfo = empty as default
09-29 16:20:24.572335  1669  1669 D LocaleTracker-0: updateLocale: Change the current country to "", countryIsoDebugInfo = empty as default, mCellInfoList = null
09-29 16:20:24.574189  1669  1669 D SubscriptionManager: putPhoneIdAndSubIdExtra: no valid subs
09-29 16:20:24.575440  1669  1669 D LocaleTracker-0: updateLocale: timeZoneCountryIso = , timeZoneCountryIsoDebugInfo = Defaulted: empty as default
09-29 16:20:24.575890  1669  1669 D NewNitzStateMachineImpl: handleCountryUnavailable: mLatestNitzSignal=null
09-29 16:20:24.576335  1669  1669 D NewNitzStateMachineImpl: doTimeZoneDetection: countryIsoCode=null, nitzSignal=null, suggestion=TelephonyTimeZoneSuggestion{mSlotIndex=0, mZoneId='null', mMatchType=0, mQuality=0, mDebugInfo=[getTimeZoneSuggestion: nitzSignal=null, countryIsoCode=null, Detection reason=handleCountryUnavailable()]}, reason=handleCountryUnavailable()
09-29 16:20:24.576423  1669  1685 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:24.576944  1669  1685 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:24.603819  1669  1669 D TransportManager-0: updateAvailableNetworks: [[QualifiedNetworks: apnType=mms, networks=EUTRAN], [QualifiedNetworks: apnType=cbs, networks=EUTRAN], [QualifiedNetworks: apnType=xcap, networks=EUTRAN]]
09-29 16:20:24.604326  1669  1669 D SmsDispatchersController: IMS registration state: false format: 3gpp2
09-29 16:20:24.605491  1872  1872 E ImsManagerIM [0]: updateImsServiceConfig: invalid sub id, skipping!
09-29 16:20:24.605975  1872  1872 W WfcLocationHandler: iso country code is null
09-29 16:20:24.607143  1669  1669 D MTKSST  : [GsmSST0] setImsRegistrationState: {registered=false mImsRegistrationOnOff=false}
09-29 16:20:24.608686  1669  1669 D MtkSubscriptionInfoUpdater: onReceive, Action: android.intent.action.CONFIGURATION_CHANGED
09-29 16:20:24.656509  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=53, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 1001 RequestorUid: 1001 RequestorPkg: com.mediatek.ims UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.657099  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=55, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 1001 RequestorUid: 1001 RequestorPkg: com.mediatek.ims UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:24.723048  1669  1669 D MTKCAT  : BootCompletedReceiver: [onReceive] action = android.intent.action.SIM_STATE_CHANGED
09-29 16:20:24.723449  1669  1669 D MTKCAT  : BootCompletedReceiver: ACTION_SIM_STATE_CHANGED, simStatus: ABSENT
09-29 16:20:24.723984  1669  1669 D FeatureConnector: [ImsSmsDispatcher, 0] imsFeatureCreated: FeatureContainer{imsFeature=android.os.BinderProxy@7803c3d, imsConfig=android.telephony.ims.aidl.IImsConfig$Stub$Proxy@8226c32, imsRegistration=android.telephony.ims.aidl.IImsRegistration$Stub$Proxy@44b7d83, sipTransport=null, state=READY, capabilities = capabilities={ EMERGENCY_OVER_MMTEL }}
09-29 16:20:24.724180  1669  1669 D FeatureConnector: [ImsSmsDispatcher, 0] imsStatusChanged: status=READY
09-29 16:20:24.724420  1669  1669 D FeatureConnector: [ImsPhoneCallTracker, 0] imsFeatureCreated: FeatureContainer{imsFeature=android.os.BinderProxy@7803c3d, imsConfig=android.telephony.ims.aidl.IImsConfig$Stub$Proxy@8226c32, imsRegistration=android.telephony.ims.aidl.IImsRegistration$Stub$Proxy@44b7d83, sipTransport=null, state=READY, capabilities = capabilities={ EMERGENCY_OVER_MMTEL }}
09-29 16:20:24.724536  1669  1669 D FeatureConnector: [ImsPhoneCallTracker, 0] imsStatusChanged: status=READY
09-29 16:20:24.724677  1669  1669 D FeatureConnector: [InstanceManager, 0] imsFeatureCreated: FeatureContainer{imsFeature=android.os.BinderProxy@7803c3d, imsConfig=android.telephony.ims.aidl.IImsConfig$Stub$Proxy@8226c32, imsRegistration=android.telephony.ims.aidl.IImsRegistration$Stub$Proxy@44b7d83, sipTransport=null, state=READY, capabilities = capabilities={ EMERGENCY_OVER_MMTEL }}
09-29 16:20:24.724750  1669  1669 D FeatureConnector: [InstanceManager, 0] imsStatusChanged: status=READY
09-29 16:20:24.725530  1669  1669 D FeatureConnector: [ImsSmsDispatcher, 0] imsStatusChanged: status=READY
09-29 16:20:24.725583  1872  1891 D FeatureConnector: [InstanceManager, 0] imsFeatureCreated: FeatureContainer{imsFeature=android.telephony.ims.feature.MmTelFeature$1@387070c, imsConfig=android.telephony.ims.stub.ImsConfigImplBase$ImsConfigStub@3ebd855, imsRegistration=android.telephony.ims.stub.ImsRegistrationImplBase$1@e13326a, sipTransport=null, state=READY, capabilities = capabilities={ EMERGENCY_OVER_MMTEL }}
09-29 16:20:24.725598  1669  1669 D FeatureConnector: [ImsSmsDispatcher, 0] imsStatusChanged: ready didn't change, ignore
09-29 16:20:24.725665  1669  1669 D FeatureConnector: [ImsPhoneCallTracker, 0] imsStatusChanged: status=READY
09-29 16:20:24.725681  1669  1669 D FeatureConnector: [ImsPhoneCallTracker, 0] imsStatusChanged: ready didn't change, ignore
09-29 16:20:24.725727  1669  1669 D FeatureConnector: [InstanceManager, 0] imsStatusChanged: status=READY
09-29 16:20:24.725732  1872  1891 D FeatureConnector: [InstanceManager, 0] imsStatusChanged: status=READY
09-29 16:20:24.725740  1669  1669 D FeatureConnector: [InstanceManager, 0] imsStatusChanged: ready didn't change, ignore
09-29 16:20:24.726413  1872  1891 D FeatureConnector: [InstanceManager, 0] imsStatusChanged: status=READY
09-29 16:20:24.726402  1669  1669 D EmergencyNumberTracker: ACTION_NETWORK_COUNTRY_CHANGED: PhoneId: 0 CountryIso: 
09-29 16:20:24.726487  1872  1891 D FeatureConnector: [InstanceManager, 0] imsStatusChanged: ready didn't change, ignore
09-29 16:20:24.731936  1669  1669 E PhoneSubInfoController: getLine1Number phone is null for Subscription:-1
09-29 16:20:24.732620  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:1
09-29 16:20:24.738287  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(1) return true
09-29 16:20:24.738364  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:7
09-29 16:20:24.742548  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(7) return false
09-29 16:20:24.745031  1669  1669 D MtkImsManagerIM [0]: Vt, isVilteResourceSupport:true, isVinrResourceSupport:false, isCarrierConfigSupport:true, isGbaValidSupport:true, isFeatureEnableByPlatformExt:true
09-29 16:20:24.757687  1669  1669 D ImsSmsDispatcher [0]: ImsManager: connection ready.
09-29 16:20:24.758585  1669  1669 D ImsManager [0]: Registration Callback registered.
09-29 16:20:24.761703  1669  1669 D MtkImsManager [0]: mMtkImsService = com.mediatek.ims.internal.IMtkImsService$Stub$Proxy@de12ede
09-29 16:20:24.762720  1669  1669 D ImsManager [0]: Capability Callback registered.
09-29 16:20:24.763728  1872  1893 D MtkImsSmsImpl: [0] configure phone 0
09-29 16:20:24.764667  1872  1893 D MtkImsSmsImpl: [0] onReady
09-29 16:20:24.764690  1669  1669 D ImsPhoneCallTracker: [0] startListeningForCalls
09-29 16:20:24.766225  1669  1669 D MtkImsManager [0]: mMtkImsService = com.mediatek.ims.internal.IMtkImsService$Stub$Proxy@80b52d5
09-29 16:20:24.767080  1872  1893 D MtkMmTelFeature: [0] onFeatureReady called!
09-29 16:20:24.767822  1872  1893 D MtkMmTelFeature: [0] getEcbmInterface
09-29 16:20:24.767997  1872  1893 D MtkMmTelFeature: [0] getEcbm
09-29 16:20:24.769888  1872  1893 D MtkMmTelFeature: [0] getMultiEndpointInterface
09-29 16:20:24.773810  1872  1893 D MtkMmTelFeature: [0] getMultiEndpoint
09-29 16:20:24.774483  1872  1893 D DialogEventPackageReceiver: DialogEventPackageReceiver
09-29 16:20:24.774822  1872  1893 D ImsMultiEndpointProxy: ImsMultiEndpointProxy
09-29 16:20:24.775445  1669  1669 D ImsMultiEndpoint: ImsMultiEndpoint created
09-29 16:20:24.775643  1669  1669 D ImsMultiEndpoint: setExternalCallStateListener
09-29 16:20:24.776821  1669  1669 D ImsManager [0]: Registration Callback registered.
09-29 16:20:24.777863  1669  1669 D ImsManager [0]: Capability Callback registered.
09-29 16:20:24.778222  1669  1669 D ImsConfig: addConfigCallback: android.telephony.ims.ProvisioningManager$Callback$CallbackBinder@9db2478
09-29 16:20:24.792237  1669  1669 D MtkImsManager [0]: iMtkUt.getUtInterface
09-29 16:20:24.794849  1669  1669 D MtkImsManager [0]: ImsConnectionStateListener added: com.mediatek.internal.telephony.imsphone.MtkImsPhoneCallTracker$2@8d1c6e8
09-29 16:20:24.794924  1669  1669 D MtkImsManager [0]: [0] hook proprietary IMS listener
09-29 16:20:24.796279  1669  1669 D ImsPhoneCallTracker: [0] startListeningForCalls() : register ims succeed, com.mediatek.internal.telephony.imsphone.MtkImsPhoneCallTracker$2@8d1c6e8
09-29 16:20:24.796499  1669  1669 D EmergencyNumberTracker: updateEmergencyNumberListDatabaseAndNotify(): receiving countryIso: 
09-29 16:20:24.797973  1669  1669 D EmergencyNumberTracker:  asset emergency database is loaded. Ver: 2 Phone Id: 0
09-29 16:20:24.798883  1669  1669 E EmergencyNumberTracker: Cache ota emergency database IOException: java.io.FileNotFoundException: /data/misc/emergencynumberdb/emergency_number_db: open failed: ENOENT (No such file or directory)
09-29 16:20:24.798953  1669  1669 D EmergencyNumberTracker: Using Asset Emergency database. Version: 2
09-29 16:20:24.799532  1669  1669 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:24.800606  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-112|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-112|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.800803  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-911|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-911|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.800880  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-000|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-000|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.800937  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-08|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-08|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.800994  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-110|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-110|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.801048  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-118|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-118|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.801103  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-119|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-119|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.801151  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-999|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-999|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.801411  1669  1669 E EmergencyNumberTracker: getEmergencyNumberListFromEccListDatabaseAndTest: radio indication is unavailable in 1.4 HAL.
09-29 16:20:24.803007  1669  1669 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:24.803332  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-112|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-112|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.803456  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-911|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-911|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.803530  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-000|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-000|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.803592  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-08|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-08|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.803715  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-110|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-110|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.803784  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-118|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-118|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.803830  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-119|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-119|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.803911  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-999|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-999|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.804065  1669  1669 E EmergencyNumberTracker: getEmergencyNumberListFromEccListDatabaseAndTest: radio indication is unavailable in 1.4 HAL.
09-29 16:20:24.804215  1669  1669 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:24.804405  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-112|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-112|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.804511  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-911|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-911|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.804593  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-000|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-000|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.804650  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-08|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-08|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.804706  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-110|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-110|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.804765  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-118|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-118|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.804822  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-119|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-119|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.804871  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-999|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-999|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:24.805024  1669  1669 E EmergencyNumberTracker: getEmergencyNumberListFromEccListDatabaseAndTest: radio indication is unavailable in 1.4 HAL.
09-29 16:20:24.806340  1669  1669 D EmergencyNumberTracker: notifyEmergencyNumberList(): notified
09-29 16:20:24.808080  1669  1669 E PhoneSubInfoController: getLine1Number phone is null for Subscription:-1
09-29 16:20:24.808712  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:1
09-29 16:20:24.809490  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(1) return true
09-29 16:20:24.809647  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:7
09-29 16:20:24.810355  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(7) return false
09-29 16:20:24.812450  1669  1669 D MtkImsManagerIM [0]: Vt, isVilteResourceSupport:true, isVinrResourceSupport:false, isCarrierConfigSupport:true, isGbaValidSupport:true, isFeatureEnableByPlatformExt:true
09-29 16:20:24.814106  1669  1669 D ImsSmsDispatcher [0]: onImsDisconnected imsReasonInfo=ImsReasonInfo :: {1000 : CODE_REGISTRATION_ERROR, 0, 0}
09-29 16:20:24.814684  1669  1669 D ImsPhoneCallTracker: [0] onCapabilitiesStatusChanged: MmTel Capabilities - [Voice: false Video: false UT: false SMS: false CALL_COMPOSER: false]
09-29 16:20:24.821876  1669  1669 D MTKSST  : [GsmSST0] setImsRegistrationState: {registered=false mImsRegistrationOnOff=false}
09-29 16:20:24.823935  1669  1669 D ImsSmsDispatcher [0]: onImsDisconnected imsReasonInfo=ImsReasonInfo :: {1000 : CODE_REGISTRATION_ERROR, 0, 0}
09-29 16:20:24.828772  1669  1669 D MTKSST  : [GsmSST0] setImsRegistrationState: {registered=false mImsRegistrationOnOff=false}
09-29 16:20:24.829940  1669  1669 D ImsPhoneCallTracker: [0] handleMessage what=26
09-29 16:20:24.829986  1669  1669 D ImsPhoneCallTracker: [0] handleMessage what=26
09-29 16:20:24.830018  1669  1669 D ImsPhoneCallTracker: [0] handleFeatureCapabilityChanged: MmTel Capabilities - [Voice: false Video: false UT: false SMS: false CALL_COMPOSER: false] isVideoEnabledStateChanged=false
09-29 16:20:24.830889  1669  1669 D ImsPhoneCallTracker: [0] handleFeatureCapabilityChanged: isVolteEnabled=false, isVideoCallEnabled=false, isVowifiEnabled=false, isUtEnabled=false
09-29 16:20:24.832799  1669  1669 D MTKSST  : [GsmSST0] EVENT_IMS_CAPABILITY_CHANGED
09-29 16:20:24.836539  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: radio is on but out of service, set plmn='No service'
09-29 16:20:24.837713  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: rawSpn = 
09-29 16:20:24.841786  1669  1669 D CSST    : isPhoneRegisteredForWifiCalling: false
09-29 16:20:24.842226  1669  1669 I CSST    : EmergencyNetworkNotification: sendMessage() w/values: ,-1,false,true
09-29 16:20:24.842770  1669  1669 I CSST    : canceling notifications: 1001
09-29 16:20:24.847115  1669  1669 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:24.848012  1872  1872 D SuppServExt: [0]ACTION_CARRIER_CONFIG_CHANGED: not loaded, subId: -1
09-29 16:20:24.862995  1872  1872 D MtkImsManager [-1]: mMtkImsService = com.mediatek.ims.MtkImsService@95480c5
09-29 16:20:24.869997  1669  1669 D SubscriptionController: [setDefaultVoiceSubId] default phone account not changed
09-29 16:20:24.880220  1669  1874 D IWlanNetworkService: linkToDeath
09-29 16:20:24.880961  1872  1933 D MWIS    : [MwiService] getWfcHandlerInterface
09-29 16:20:24.881704  1669  1874 D IWlanNetworkService: checkAndBindWifiOffloadService: sWifiOffloadService = com.mediatek.wfo.IWifiOffloadService$Stub$Proxy@76aedfd
09-29 16:20:24.881829  1669  1874 D IWlanNetworkService: create WifiOffloadListenerProxy
09-29 16:20:24.883608  1669  1669 D CarrierSignalAgent: [0]CarrierSignalAgent receiver action: android.telephony.action.CARRIER_CONFIG_CHANGED
09-29 16:20:24.891769  1669  1669 D CarrierSignalAgent: [0]Loading carrier config: carrier_app_wake_signal_config
09-29 16:20:24.892717  1669  1669 D CarrierSignalAgent: [0]Loading carrier config: carrier_app_no_wake_signal_config
09-29 16:20:24.902193  1669  1833 D MTKSST  : [GsmSST0] EVENT_RECHECK_NRM_STATUS connected=true
09-29 16:20:24.910425  1669  1669 D NRM-C-0 : Carrier config changed. Try to bind network service.
09-29 16:20:24.910673  1669  1669 D NRM-I-0 : Carrier config changed. Try to bind network service.
09-29 16:20:24.916436  1872  1872 D MtkImsManagerIM [-1]: isImsResourceSupport, feature:2
09-29 16:20:24.916684  1872  1872 E MtkImsManagerIM [-1]: Invalid main phone -1, return true as don't care
09-29 16:20:24.916908  1872  1872 D SubscriptionManager: [getSubId]- fail
09-29 16:20:24.917969  1669  1669 I CSST    : reading time to delay notification pref network: -1
09-29 16:20:24.919558  1872  1872 D SubscriptionManager: [getSubId]- fail
09-29 16:20:24.923621  1872  1872 D SubscriptionManager: [getSubId]- fail
09-29 16:20:24.927462  1872  1872 D MtkImsManagerIM [-1]: getAirplaneModeFromSettings: false
09-29 16:20:24.927905  1872  1872 D MtkImsManagerIM [-1]: Wfc, isResourceSupport:true, isCarrierConfigSupport:true, isGbaValidSupport:true, isFeatureEnableByPlatformExt:true, wfcSupportAirplaneMode:true, isAirplaneModeON:false
09-29 16:20:24.929704  1669  1669 I CSST    : reading time to delay notification emergency: -1
09-29 16:20:24.931215  1669  1669 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:24.932223  1669  1669 I CSST    : isNrSupported:  carrierConfigEnabled: true, AccessFamilySupported: false, isNrNetworkTypeAllowed: false
09-29 16:20:24.932412  1669  1669 I CSST    : PrefNetworkNotification: sendMessage() w/values: ,false,-1,false,true
09-29 16:20:24.933317  1669  1669 I CSST    : canceling notifications: 1000
09-29 16:20:24.934326  1669  1669 D CSST    : isPhoneRegisteredForWifiCalling: false
09-29 16:20:24.934751  1669  1669 I CSST    : EmergencyNetworkNotification: sendMessage() w/values: ,-1,false,true
09-29 16:20:24.935403  1669  1669 I CSST    : canceling notifications: 1001
09-29 16:20:24.937422  1669  1669 D DSM-C-0 : Carrier config changed. Try to bind data service.
09-29 16:20:24.940554  1669  1669 D RILJ    : [0109]> VOICE_RADIO_TECH [PHONE0]
09-29 16:20:24.942475  1669  1811 D RILJ    : [0109]< VOICE_RADIO_TECH {1} [PHONE0]
09-29 16:20:24.949243  1669  1669 D RILJ    : [0110]> GET_RADIO_CAPABILITY [PHONE0]
09-29 16:20:24.950336  1669  1669 D RetryManager: [ims] mBroadcastReceiver: action android.telephony.action.CARRIER_CONFIG_CHANGED, mSameApnRetryCount:0, networkSuggestedDelay:-1, mCurrentApnIndex:-1
09-29 16:20:24.950639  1669  1669 D RetryManager: [default] mBroadcastReceiver: action android.telephony.action.CARRIER_CONFIG_CHANGED, mSameApnRetryCount:0, networkSuggestedDelay:-1, mCurrentApnIndex:-1
09-29 16:20:24.950803  1669  1669 D DSM-I-0 : Carrier config changed. Try to bind data service.
09-29 16:20:24.951281  1669  1669 D RetryManager: [ims] mBroadcastReceiver: action android.telephony.action.CARRIER_CONFIG_CHANGED, mSameApnRetryCount:0, networkSuggestedDelay:-1, mCurrentApnIndex:-1
09-29 16:20:24.951545  1669  1669 D RetryManager: [default] mBroadcastReceiver: action android.telephony.action.CARRIER_CONFIG_CHANGED, mSameApnRetryCount:0, networkSuggestedDelay:-1, mCurrentApnIndex:-1
09-29 16:20:24.951856  1669  1669 D SuppServConf: [0]mBroadcastReceiver: action android.telephony.action.CARRIER_CONFIG_CHANGED
09-29 16:20:24.952358  1669  1669 I SuppServConf: [0]Receive ACTION_CARRIER_CONFIG_CHANGED: subId=-1, mPhone.getSubId()=-1
09-29 16:20:24.952575  1669  1669 I SuppServConf: [0]CarrierConfigLoader is loading complete!
09-29 16:20:24.952851  1669  1844 D SuppServConf: [0]handleMessage msg: EVENT_CARRIER_CONFIG_LOADED
09-29 16:20:24.952907  1669  1844 I SuppServConf: [0]resetConfig start.
09-29 16:20:24.952933  1669  1844 I SuppServConf: [0]resetConfig end.
09-29 16:20:24.953211  1669  1669 E ImsPhoneCallTracker: [0] cacheCarrierConfiguration: No carrier config service found or not active subId = -1
09-29 16:20:24.954080  1669  1844 I SuppServConf: [0]loadFromCarrierConfig start.
09-29 16:20:24.954669  1669  1844 I SuppServConf: [0]loadFromCarrierConfig end.
09-29 16:20:24.954745  1669  1844 I SuppServConf: [0]NEED_CHECK_DATA_ROAMING -> bValue: false, sValue: , iValue: -1
09-29 16:20:24.954767  1669  1844 I SuppServConf: [0]TBCLIR -> bValue: false, sValue: , iValue: -1
09-29 16:20:24.954806  1669  1844 I SuppServConf: [0]RE_REGISTER_FOR_CF -> bValue: false, sValue: , iValue: -1
09-29 16:20:24.954826  1669  1844 I SuppServConf: [0]SUPPORT_SAVE_CF_NUMBER -> bValue: false, sValue: , iValue: -1
09-29 16:20:24.954845  1669  1844 I SuppServConf: [0]TRANSFER_XCAP_404 -> bValue: false, sValue: , iValue: -1
09-29 16:20:24.954863  1669  1844 I SuppServConf: [0]NEED_CHECK_IMS_WHEN_ROAMING -> bValue: false, sValue: , iValue: -1
09-29 16:20:24.954881  1669  1844 I SuppServConf: [0]NOT_SUPPORT_XCAP -> bValue: false, sValue: , iValue: -1
09-29 16:20:24.954917  1669  1844 I SuppServConf: [0]NOT_SUPPORT_OCB -> bValue: false, sValue: , iValue: -1
09-29 16:20:24.954936  1669  1844 I SuppServConf: [0]GSM_UT_SUPPORT -> bValue: false, sValue: , iValue: -1
09-29 16:20:24.954954  1669  1844 I SuppServConf: [0]ENABLE_XCAP_HTTP_RESPONSE_409 -> bValue: false, sValue: , iValue: -1
09-29 16:20:24.954972  1669  1844 I SuppServConf: [0]QUERY_CFU_AGAIN_AFTER_SET -> bValue: false, sValue: , iValue: -1
09-29 16:20:24.954989  1669  1844 I SuppServConf: [0]NOT_SUPPORT_CALL_IDENTITY -> bValue: false, sValue: , iValue: -1
09-29 16:20:24.955046  1669  1844 I SuppServConf: [0]NEED_CHECK_DATA_ENABLE -> bValue: false, sValue: , iValue: -1
09-29 16:20:24.955073  1669  1844 I SuppServConf: [0]IMS_NW_CW -> bValue: false, sValue: , iValue: -1
09-29 16:20:24.955092  1669  1844 I SuppServConf: [0]NOT_SUPPORT_WFC_UT -> bValue: false, sValue: , iValue: -1
09-29 16:20:24.956074  1669  1669 D ImsPhoneCallTracker: [0] isTestSim: false
09-29 16:20:24.956394  1669  1669 D ImsPhoneCallTracker: [0] onReceive : Updating mAllowEmergencyVideoCalls = false
09-29 16:20:24.957947  1669  1811 D RILJ    : convertHalRadioCapability: session=-1, phase=3, rat=36869, logicModemUuid=modem_sys1_ps0, status=1, rcRil.raf=81930 [PHONE0]
09-29 16:20:24.958177  1669  1811 D RILJ    : [0110]< GET_RADIO_CAPABILITY {mPhoneId = 0 mVersion=1 mSession=-1 mPhase=3 mRadioAccessFamily=36869 mLogicModemId=modem_sys1_ps0 mStatus=1} [PHONE0]
09-29 16:20:24.981604  1669  1669 D MTKSST  : [GsmSST0] EVENT_RECHECK_NRM_STATUS trigger pollState
09-29 16:20:24.981653  1669  1669 D MTKSST  : [GsmSST0] pollState: modemTriggered=true, mPollingContext=0, RadioState=1, connected=true, support_ap_iwlan=1
09-29 16:20:24.982729  1669  1669 D RILJ    : [0111]> OPERATOR [PHONE0]
09-29 16:20:24.983297  1669  1873 D IWlanNetworkService: getNetworkRegistrationState for domain 2, slotid: 0
09-29 16:20:24.983638  1669  1920 D IWlanNetworkService: createRegistrationState.
09-29 16:20:24.983816  1669  1920 D IWlanNetworkService: getAvailableServices.
09-29 16:20:24.984117  1669  1669 D RILJ    : [0112]> QUERY_NETWORK_SELECTION_MODE [PHONE0]
09-29 16:20:24.984911  1669  1920 D IWlanNetworkService: Calling callback.onGetNetworkRegistrationStateComplete.resultCode = 0, netState = NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, slotid: 0
09-29 16:20:24.985199  1669  1920 D NRM-I-0 : onRequestNetworkRegistrationInfoComplete result: 0, info: NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}
09-29 16:20:24.986312  1669  1871 D RILJ    : [0113]> DATA_REGISTRATION_STATE [PHONE0]
09-29 16:20:24.986648  1669  1871 D RILJ    : getDataRegistrationState: overrideHalVersion=null [PHONE0]
09-29 16:20:24.987008  1176  1202 I AT      : [0] AT> AT+EOPS? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:24.989499  1669  1871 D RILJ    : [0114]> VOICE_REGISTRATION_STATE [PHONE0]
09-29 16:20:24.989614  1669  1871 D RILJ    : getVoiceRegistrationState: overrideHalVersion=null [PHONE0]
09-29 16:20:24.991597  1176  1201 I AT      : [0] AT< +EOPS: 0,2,"000000",1 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:24.991772  1176  1201 I AT      : [0] AT< OK (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:24.992193  1176  1202 D RmcNwRTReqHdlr: [0] requestQueryNetworkSelectionMode return 0
09-29 16:20:24.992355  1176  1202 I AT      : [0] AT> AT+E5GOPT? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:24.993464  1669  1811 D RILJ    : [0111]< OPERATOR {, , } [PHONE0]
09-29 16:20:24.994146  1669  1811 D RILJ    : [0112]< QUERY_NETWORK_SELECTION_MODE {0} [PHONE0]
09-29 16:20:24.995391  1176  1201 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:24.996411  1176  1192 D RmcNwReqHdlr: [0] [currentPhysicalChannelConfigs] needNotifyEmpty and has notified empty list, return
09-29 16:20:24.997217  1669  1811 D RILJ    : [0113]< DATA_REGISTRATION_STATE {.regState = NOT_REG_MT_NOT_SEARCHING_OP, .rat = UNKNOWN, .reasonForDenial = NONE, .cellIdentity = {.noinit = {}}, .registeredPlmn = , .accessTechnologySpecificInfo = {.noinit = {}}} [PHONE0]
09-29 16:20:24.997778  1669  1871 D CellularNetworkService: No access tech specific info passes for RegStateResult
09-29 16:20:24.997867  1669  1811 D RILJ    : [0114]< VOICE_REGISTRATION_STATE {.regState = NOT_REG_MT_SEARCHING_OP, .rat = UNKNOWN, .reasonForDenial = NONE, .cellIdentity = {.noinit = {}}, .registeredPlmn = , .accessTechnologySpecificInfo = {.noinit = {}}} [PHONE0]
09-29 16:20:24.998013  1669  1871 D NRM-C-0 : onRequestNetworkRegistrationInfoComplete result: 0, info: NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}
09-29 16:20:24.998144  1669  1871 D CellularNetworkService: No access tech specific info passes for RegStateResult
09-29 16:20:24.998304  1669  1871 D NRM-C-0 : onRequestNetworkRegistrationInfoComplete result: 0, info: NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}
09-29 16:20:24.998780  1669  1669 D NRM-C-0 : Service com.android.phone already bound or being bound.
09-29 16:20:24.999916  1669  1669 D NRM-I-0 : Service com.android.phone already bound or being bound.
09-29 16:20:25.003315  1669  1669 D MTKSST  : [GsmSST0] CarrierConfigChange PersistableBundle[{mtk_show_clir_setting_bool=true, mtk_default_enhanced_4g_mode_bool=true, carrier_volte_provisioned_bool=false, support_cdma_1x_voice_calls_bool=true, support_ss_over_cdma_bool=false, disable_charge_indication_bool=false, support_tdscdma_bool=false, httpSocketTimeout=60000, mtk_resume_hold_call_after_active_call_end_by_remote=false, allowed_initial_attach_apn_types_string_array=[ia, default, mms, dun], disable_supplementary_services_in_airplane_mode_bool=false, call_barring_default_service_class_int=1, call_redirection_service_component_name_string=null, carrier_wfc_supports_wifi_only_bool=false, carrier_default_actions_on_default_network_available_string_array=[false: 7, true: 8], mtk_ct_volte_status_bool=false, mtk_carrier_ss_need_check_data_roaming=false, operator_selection_expand_bool=true, disable_cdma_activation_code_bool=false, simplified_network_settings_bool=false, call_forwarding_when_unanswered_supported_bool=true, support_tdscdma_roaming_networks_string_array=null, gps.lpp_profile=2, call_barring_visibility_bool=true, gba_mode_int=1, gps.es_extension_sec=0, enable_apps_string_array=null, 5g_icon_display_secondary_grace_period_string=, carrier_default_wfc_ims_roaming_enabled_bool=false, mtk_show_call_barring_password_bool=false, cdma_nonroaming_networks_string_array=null, signal_strength_nr_nsa_use_lte_as_primary_bool=true, aliasMinChars=2, mtk_key_multiline_allow_cross_line_conference_bool=false, fdn_number_length_limit_int=20, support_ims_call_forwarding_while_roaming_bool=true, mtk_carrier_wfc_location_response_timeout=55000, wfc_data_spn_format_idx_int=0, hide_sim_lock_settings_bool=false, drop_video_call_when_answering_audio_call_bool=false, mtk_rtt_auto_accept_request_bool=false, mtk_show_open_mobile_data_dialog_bool=false, ci_action_on_sys_update_bool=false, carrier_certificate_string_array=[], convert_cdma_caller_id_mmi_codes_while_roaming_on_3gpp_bool=false, mtk_ignore_clir_when_ecc=true, support_enhanced_call_blocking_bool=true, iwlan.ike_rekey_hard_timer_in_sec=14400, vvm_port_number_int=0, carrier_default_wfc_ims_enabled_bool=false, iwlan.ike_session_encryption_aes_ctr_key_size_int_array=[128, 192, 256], dial_string_replace_string_array=null, opportunistic_network_entry_threshold_bandwidth_int=1024, opportunistic_network_data_switch_exit_hysteresis_time_long=3000, gsm_nonroaming_networks_string_array=null, imsserviceentitlement.ims_provisioning_bool=false, wifi.avoid_5ghz_softap_for_laa_bool=false, hide_ims_apn_bool=false, mtk_carrier_wfc_get_location_always=false, show_toast_when_conference_full=true, vvm_destination_number_string=, unmetered_nr_sa_mmwave_bool=false, dtmf_type_enabled_bool=false, allow_video_calling_fallback_bool=true, mtk_carrier_ims_ecbm_supported=false, mtk_domestic_roaming_enabled_only_by_mobile_data_setting=false, config_ims_package_override_string=null, only_auto_select_in_home_network=false, iwlan.supported_prf_algorithms_int_array=[2, 4, 5, 6, 7], mtk_support_enhanced_call_blocking_bool=false, show_data_connected_roaming_notification=false, support_auto_decline_upgrade_request_bool=true, gps.es_supl_data_plane_only_roaming_plmn_string_array=null, mtk_video_call_background_transmission=false, imsserviceentitlement.fcm_sender_id_string=, smsToMmsTextThreshold=-1, inflate_signal_strength_bool=false, force_home_network_bool=false, spdi_override_string_array=null, show_wfc_location_privacy_policy_bool=false, gps.supl_es=1, enableSMSDeliveryReports=true, iwlan.natt_keep_alive_timer_sec_int=20, missed_incoming_call_sms_originator_string_array=[], missed_incoming_call_sms_pattern_string_array=[], auto_retry_enabled_bool=false, ims.enable_presence_capability_exchange_bool=false, opportunistic_network_entry_threshold_rssnr_int=45, play_call_recording_tone_bool=false, unmetered_nr_nsa_sub6_bool=false, carrier_force_disable_etws_cmas_test_bool=false, call_waiting_service_class_int=1, allow_emergency_video_calls_bool=false, support_add_conference_participants_bool=false, csp_enabled_bool=false, mtk_dia
09-29 16:20:25.003588  1669  1669 D EriManager: loadEriFileFromXml: check for alternate file
09-29 16:20:25.004329  1669  1669 D EriManager: loadEriFileFromXml: no alternate file
09-29 16:20:25.005280  1669  1669 D EriManager: eriFile = eri.xml
09-29 16:20:25.009620  1669  1669 D EriManager: loadEriFileFromXml: eri parsing successful, file loaded. ver = 1357, # of entries = 176
09-29 16:20:25.011944  1669  1669 E MTKSST  : [GsmSST0] Invalid parameters for NR RSRP boost
09-29 16:20:25.013552  1669  1669 D RILJ    : [0115]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:25.015450  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 1, 4, 0, 3000, 2, 4, -128, -118, -108, -98 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:25.015361  1669  1669 D RILJ    : [0116]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:25.017014  1669  1669 D RILJ    : [0117]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:25.018136  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:25.018755  1669  1669 D RILJ    : [0118]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:25.018996  1669  1811 D RILJ    : [0115]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:25.020533  1669  1669 D RILJ    : [0119]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:25.020783  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 1, 2, 0, 3000, 2, 4, -115, -105, -95, -85 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:25.022863  1669  1669 D RILJ    : [0120]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:25.024034  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:25.024381  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 1, 1, 0, 3000, 2, 4, -107, -103, -97, -89 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:25.024434  1669  1669 D RILJ    : [0121]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:25.024848  1669  1811 D RILJ    : [0116]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:25.025972  1669  1669 D RILJ    : [0122]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:25.026704  1669  1669 D MtkGsmCdmaPhone: notifyCallForwardingIndicator: sim state = 1
09-29 16:20:25.026793  1669  1669 D MTKSST  : [GsmSST0] pollState: modemTriggered=false, mPollingContext=5, RadioState=1, connected=true, support_ap_iwlan=1
09-29 16:20:25.027407  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:25.027959  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 0, 4, 1, 3000, 2, 4, 0, 0, 0, 0 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:25.028442  1669  1811 D RILJ    : [0117]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:25.029342  1669  1669 D DSM-C-0 : Service com.android.phone already bound or being bound.
09-29 16:20:25.029768  1669  1669 D MtkGsmCdmaPhone: correctPhoneTypeForCdma: change:false newVoiceRadioTech=1 mActivePhone=GSM
09-29 16:20:25.031753  1669  1669 D DSM-I-0 : Service com.android.phone already bound or being bound.
09-29 16:20:25.032061  1669  1669 D MtkSuppServHelper: [0]handleMessage: EVENT_CARRIER_CONFIG_LOADED(15)
09-29 16:20:25.032231  1669  1669 I MtkSuppServHelper: [0]Set mCarrierConfigLoaded: true
09-29 16:20:25.032641  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:25.033089  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 0, 4, 2, 3000, 2, 4, 0, 0, 0, 0 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:25.034421  1669  1811 D RILJ    : [0118]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:25.035642  1669  1669 D NetworkTypeController: [0] LegacyState: process EVENT_CARRIER_CONFIG_CHANGED
09-29 16:20:25.036044  1669  1669 D NetworkTypeController: [0] Remove all timers
09-29 16:20:25.036172  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:25.036220  1669  1669 D NetworkTypeController: [0] DefaultState: process EVENT_CARRIER_CONFIG_CHANGED
09-29 16:20:25.036526  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 1, 128, 0, 3000, 2, 4, -110, -90, -80, -65 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:25.037894  1669  1669 D NetworkTypeController: [0] mOverrideTimerRules: {connected={mState=connected, mOverrideType=NR_NSA, mPrimaryTimers={}, mSecondaryTimers={}}, not_restricted_rrc_con={mState=not_restricted_rrc_con, mOverrideType=NR_NSA, mPrimaryTimers={}, mSecondaryTimers={}}, legacy={mState=legacy, mOverrideType=NONE, mPrimaryTimers={}, mSecondaryTimers={}}, not_restricted_rrc_idle={mState=not_restricted_rrc_idle, mOverrideType=NR_NSA, mPrimaryTimers={}, mSecondaryTimers={}}, restricted={mState=restricted, mOverrideType=NONE, mPrimaryTimers={}, mSecondaryTimers={}}, connected_mmwave={mState=connected_mmwave, mOverrideType=NR_NSA, mPrimaryTimers={}, mSecondaryTimers={}}}
09-29 16:20:25.038154  1669  1669 D NetworkTypeController: [0] Remove all timers
09-29 16:20:25.038374  1669  1669 D MtkNetworkTypeController: [Override]getCurrentOverrideNetworkType: 0
09-29 16:20:25.038832  1669  1811 D RILJ    : [0119]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:25.039294  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:25.039721  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 0, 128, 1, 3000, 2, 4, 0, 0, 0, 0 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:25.040445  1669  1811 D RILJ    : [0120]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:25.041455  1669  1669 D MTKSST  : [GsmSST0] handlePollStateResultMessage: PS IWLAN. NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}
09-29 16:20:25.042194  1669  1669 D MTKSST  : [GsmSST0] EVENT_POLL_STATE_NETWORK_SELECTION_MODE
09-29 16:20:25.043007  1669  1669 D MTKSST  : [GsmSST0] handlePollStateResultMessage: PS cellular. NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}
09-29 16:20:25.044092  1669  1669 E MTKSST  : [GsmSST0] Exception while polling service state. Probably malformed RIL response.java.lang.NullPointerException: Attempt to invoke virtual method 'int android.telephony.CellIdentity.getType()' on a null object reference
09-29 16:20:25.044644  1669  1669 D MTKSST  : [GsmSST0] Could not set ServiceState channel number. CellIdentity null
09-29 16:20:25.045453  1669  1669 D MTKSST  : [GsmSST0] combinePsRegistrationStates: {mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=, mOperatorAlphaShort=, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=false, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=, mOperatorAlphaShortRaw=, mIsIwlanPreferred=false, Ril Voice Regist state=2, Ril Data Regist state=0, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0}
09-29 16:20:25.047106  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:25.047291  1669  1669 D MtkRILJ : lookupOperatorNameNitz plmn name update to Nitz: 
09-29 16:20:25.047586  1669  1669 E MTKSST  : lookupOperatorName getPhone null subid=-1
09-29 16:20:25.047587  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 0, 128, 2, 3000, 2, 4, 0, 0, 0, 0 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:25.048104  1669  1811 D RILJ    : [0121]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:25.050501  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:25.053083  1669  1811 D RILJ    : [0122]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:25.081736  1669  1669 W MtkSpnOverride: test mccmncspn = 20408Hi, name = Hi
09-29 16:20:25.081877  1669  1669 W MtkSpnOverride: test mccmncspn = 20408Ortel NL, name = Ortel NL
09-29 16:20:25.081907  1669  1669 W MtkSpnOverride: test mccmncspn = 20408Rabo Mobiel, name = Rabo Mobiel
09-29 16:20:25.081930  1669  1669 W MtkSpnOverride: test mccmncspn = 20412Lebara, name = Lebara
09-29 16:20:25.081952  1669  1669 W MtkSpnOverride: test mccmncspn = 20610LYCAMOBILE, name = LYCAMOBILE
09-29 16:20:25.082082  1669  1669 W MtkSpnOverride: test mccmncspn = 20620Ortel BE, name = Ortel
09-29 16:20:25.082155  1669  1669 W MtkSpnOverride: test mccmncspn = 20801C le mobile, name = NRJ Mobile
09-29 16:20:25.082209  1669  1669 W MtkSpnOverride: test mccmncspn = 20801NRJ Mobile, name = NRJ Mobile
09-29 16:20:25.082261  1669  1669 W MtkSpnOverride: test mccmncspn = 20810A MOBILE, name = A MOBILE
09-29 16:20:25.082329  1669  1669 W MtkSpnOverride: test mccmncspn = 20810AfoneMobile, name = Afone
09-29 16:20:25.082384  1669  1669 W MtkSpnOverride: test mccmncspn = 20810C le mobile, name = NRJ
09-29 16:20:25.082440  1669  1669 W MtkSpnOverride: test mccmncspn = 20810La Poste Mobile, name = La Poste Mobile
09-29 16:20:25.082501  1669  1669 W MtkSpnOverride: test mccmncspn = 20810NRJ Mobile, name = NRJ
09-29 16:20:25.082555  1669  1669 W MtkSpnOverride: test mccmncspn = 20810Simplicime, name = Simplicime
09-29 16:20:25.082622  1669  1669 W MtkSpnOverride: test mccmncspn = 22201tiscalimobile, name = Tiscali Mobile
09-29 16:20:25.082674  1669  1669 W MtkSpnOverride: test mccmncspn = 22201COOP, name = Coop
09-29 16:20:25.082725  1669  1669 W MtkSpnOverride: test mccmncspn = 22201Noverca, name = Noverca
09-29 16:20:25.082775  1669  1669 W MtkSpnOverride: test mccmncspn = 22207Noverca, name = Noverca
09-29 16:20:25.082866  1669  1669 W MtkSpnOverride: test mccmncspn = 22210BT Italia, name = BT Italia Mobile
09-29 16:20:25.082918  1669  1669 W MtkSpnOverride: test mccmncspn = 22210ERG, name = ERG Mobile
09-29 16:20:25.082970  1669  1669 W MtkSpnOverride: test mccmncspn = 22210ERG mobile, name = ERG Mobile
09-29 16:20:25.083089  1669  1669 W MtkSpnOverride: test mccmncspn = 22210PosteMobile, name = Poste Mobile
09-29 16:20:25.083139  1669  1669 W MtkSpnOverride: test mccmncspn = 22299FASTWEB, name = Fastweb
09-29 16:20:25.083164  1669  1669 W MtkSpnOverride: test mccmncspn = 23401Vectone Mobile, name = Vectone
09-29 16:20:25.083186  1669  1669 W MtkSpnOverride: test mccmncspn = 23410TESCO, name = TESCO
09-29 16:20:25.083213  1669  1669 W MtkSpnOverride: test mccmncspn = 23415ASDA Mobile, name = ASDA Mobile
09-29 16:20:25.083286  1669  1669 W MtkSpnOverride: test mccmncspn = 23415BT, name = BT Mobile
09-29 16:20:25.083344  1669  1669 W MtkSpnOverride: test mccmncspn = 23415Lebara, name = Lebara
09-29 16:20:25.083398  1669  1669 W MtkSpnOverride: test mccmncspn = 23420Lebara, name = Lebara
09-29 16:20:25.083456  1669  1669 W MtkSpnOverride: test mccmncspn = 23426GT mobile, name = GT mobile
09-29 16:20:25.083529  1669  1669 W MtkSpnOverride: test mccmncspn = 23426Lycamobile, name = Lycamobile
09-29 16:20:25.083610  1669  1669 W MtkSpnOverride: test mccmncspn = 23430Virgin, name = Virgin
09-29 16:20:25.083720  1669  1669 W MtkSpnOverride: test mccmncspn = 23431Virgin, name = Virgin
09-29 16:20:25.083777  1669  1669 W MtkSpnOverride: test mccmncspn = 23432Virgin, name = Virgin
09-29 16:20:25.083831  1669  1669 W MtkSpnOverride: test mccmncspn = 23433Now mobile, name = Now mobile
09-29 16:20:25.083898  1669  1669 W MtkSpnOverride: test mccmncspn = 26201congstar, name = Telekom.de
09-29 16:20:25.083949  1669  1669 W MtkSpnOverride: test mccmncspn = 26203blau.de, name = blau.de
09-29 16:20:25.084001  1669  1669 W MtkSpnOverride: test mccmncspn = 26203AY YILDIZ, name = AY YILDIZ
09-29 16:20:25.084066  1669  1669 W MtkSpnOverride: test mccmncspn = 26203simVOICE, name = simVOICE
09-29 16:20:25.084120  1669  1669 W MtkSpnOverride: test mccmncspn = 26203ptt-mobile, name = ptt-mobile
09-29 16:20:25.084173  1669  1669 W MtkSpnOverride: test mccmncspn = 466017-Mobile, name = 7-Mobile
09-29 16:20:25.084229  1669  1669 W MtkSpnOverride: test mccmncspn = 46601統一超商, name = 統一超商
09-29 16:20:25.084281  1669  1669 W MtkSpnOverride: test mccmncspn = 46692家樂福電信, name = 家樂福
09-29 16:20:25.084333  1669  1669 W MtkSpnOverride: test mccmncspn = 20404中国电信, name = 中国电信
09-29 16:20:25.084386  1669  1669 W MtkSpnOverride: test mccmncspn = 45403中国电信, name = 中国电信
09-29 16:20:25.084451  1669  1669 W MtkSpnOverride: test mccmncspn = 46001京东通信, name = 京东通信
09-29 16:20:25.084505  1669  1669 W MtkSpnOverride: test mccmncspn = 46001阿里通信, name = 阿里通信
09-29 16:20:25.084559  1669  1669 W MtkSpnOverride: test mccmncspn = 204048.ta Δ, name = 8.ta
09-29 16:20:25.084612  1669  1669 W MtkSpnOverride: test mccmncspn = 46013中国广电, name = 中国广电
09-29 16:20:25.088120  1669  1669 W MtkSpnOverride: test imsipattern = 2080120801xxx67xxxxx, name = Virgin
09-29 16:20:25.108167  1669  1669 W MtkSpnOverride: test mccmncpnn = 26203Ortel D, name = Ortel D
09-29 16:20:25.108428  1669  1669 W MtkSpnOverride: test mccmncpnn = 23430EE, name = EE
09-29 16:20:25.247509  1176  1184 I AT      : [0] AT< +EBARRING: 2, 4, 0, 0, , , , 1, 0, , , , 2, 0, , , , 8, 0 (RIL_URC_READER, tid:493447834880)
09-29 16:20:25.272023  1176  1184 I AT      : [0] AT< +CSCON: 0,,2 (RIL_URC_READER, tid:493447834880)
09-29 16:20:25.272492  1176  1185 E RmcNwHdlr: [0] There is something wrong with the handleConnectionStateReport URC
09-29 16:20:25.272772  1176  1184 I AT      : [0] AT< +EREG=*** (RIL_URC_READER, tid:493447834880)
09-29 16:20:25.272894  1176  1184 I AT      : [0] AT< +EGREG=*** (RIL_URC_READER, tid:493447834880)
09-29 16:20:25.273185  1176  1185 D RmcNwHdlr: [0] [handleCsNetworkStateChanged] mMdEreg n=0, stat=0, lac=**91, ci=***8A80, eAct=4, nwk_existence=0, roam_indicator=0, cause_type=0, reject_cause=0 mMdEcell act=0, cid=*, mcc=0, mnc=0, lacTac=*, pscPci=*, sig1=0, sig2=0, rsrp=0, rsrq=0, timingAdvance=0, rssnr=0, cqi=0, bsic=0, arfcn=0
09-29 16:20:25.273576  1176  1185 D RmcNwHdlr: [0] [handlePsNetworkStateChanged] mMdEgreg n=0, stat=4, lac=**91, ci=***8A80, eAct=4, rac=145, nwk_existence=0, roam_indicator=0, cause_type=0, reject_cause=0, dcnr_restricted=0, endc_sib=0, endc_available=0.   mMdEcell act=0, cid=*, mcc=0, mnc=0, lacTac=*, pscPci=*, sig1=0, sig2=0, rsrp=0, rsrq=0, timingAdvance=0, rssnr=0, cqi=0, bsic=0, arfcn=0
09-29 16:20:25.273617  1176  1185 D RmcNwHdlr: [0] handleScgConnectionChange old=0, new=0
09-29 16:20:25.274435  1176  1192 I AT      : [0] AT> AT+EOPS? (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:25.274436  1176  1200 I AT      : [0] AT> AT+EOPS? (RIL_ATCI_READER tid:493431254272)
09-29 16:20:25.277371  1176  1199 I AT      : [0] AT< +EOPS: 0,2,"45005",1 (RIL_ATCI_READER, tid:493432290560)
09-29 16:20:25.277365  1176  1191 I AT      : [0] AT< +EOPS: 0,2,"45005",1 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:25.277444  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:25.278620  1176  1182 I RtcEccNumberController: [0] [updateEmergencyNumber] mIsFwkReady: 0, mIsPendingUpdate: 1, ecc list: 112,911,000,08,110,118,119,999
09-29 16:20:25.279189  1176  1199 I AT      : [0] AT< OK (RIL_ATCI_READER, tid:493432290560)
09-29 16:20:25.279910  1176  1182 D RtcEccNumberController: [0] [onPlmnChanged] valid:-1, network Plmn:, reg Plmn:45005
09-29 16:20:25.279984  1176  1182 D EccNumberSource: [XML][0][update] START for plmn: 45005, isSimInsert: 0
09-29 16:20:25.282160  1176  1182 D EccNumberPreference: [0][update] for PLMN: 45005 GSM only: , GSM prefer: , CDMA prefer: 
09-29 16:20:25.282305  1176  1182 I RtcEccNumberController: [0] [updateEmergencyNumber] mIsFwkReady: 0, mIsPendingUpdate: 1, ecc list: 112,911,000,08,110,118,119,999,111,113,117,125,122
09-29 16:20:25.283638  1176  1182 I RtcEmbmsAt: [0] Handle URC RFX_MSG_URC_EMBMS_CELL_INFO_NOTIFICATION Slot 0 (DefaultDataSlot:-1)
09-29 16:20:25.283723  1176  1182 W RtcEmbmsAt: [0] ignore URC due to not on DefaultDataSlot:-1
09-29 16:20:25.364261  1669  1669 W MtkSpnOverride: test mccmncgid1 = 2343040, name = Virgin
09-29 16:20:25.364704  1669  1669 D MtkRILJ : lookupOperatorNameMVNO plmn name update to TS.25/MVNO: 
09-29 16:20:25.364864  1669  1669 D MtkRILJ : lookupOperatorNameNitz plmn name update to Nitz: 
09-29 16:20:25.364913  1669  1669 E MTKSST  : lookupOperatorName getPhone null subid=-1
09-29 16:20:25.365013  1669  1669 D MtkRILJ : lookupOperatorNameMVNO plmn name update to TS.25/MVNO: 
09-29 16:20:25.365212  1669  1669 D MTKSST  : [GsmSST0] refreshSpn: null, null, fromPollState=true, mForceBroadcastServiceState=true
09-29 16:20:25.427990  1176  1184 I AT      : [0] AT< +ECSQ: 67,43,1,-214,-11,1,1,4,32767,1 (RIL_URC_READER, tid:493447834880)
09-29 16:20:25.428548  1176  1185 D RmcNwHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0X04]
09-29 16:20:25.428604  1176  1185 D RmcNwHdlr: [0] handleSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 29, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 67, wcdma_ecno: 43, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:20:25.476279  1669  1669 D MTKSST  : [GsmSST0] Could not set ServiceState channel number. CellIdentity null
09-29 16:20:25.476584  1669  1669 D MTKSST  : [GsmSST0] Poll ServiceState done: oldSS=[{mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=null, mOperatorAlphaShort=null, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=false, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=null, mOperatorAlphaShortRaw=null, mIsIwlanPreferred=false, Ril Voice Regist state=0, Ril Data Regist state=0, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0}]
09-29 16:20:25.476911  1669  1669 D MTKSST  : [GsmSST0] Poll ServiceState done: newSS=[{mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=null, mOperatorAlphaShort=null, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=false, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=, mOperatorAlphaShortRaw=, mIsIwlanPreferred=false, Ril Voice Regist state=2, Ril Data Regist state=0, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0}] oldMaxDataCalls=1 mNewMaxDataCalls=16 oldReasonDataDenied=-1 mNewReasonDataDenied=0 isImsEccOnly= false
09-29 16:20:25.477369  1669  1669 D MTKSST  : [GsmSST0] pollStateDone: hasRegistered = false hasDeregistered = false hasDataAttached = {1=false, 2=false} hasDataDetached = {1=false, 2=false} hasDataRegStateChanged = {1=true, 2=true} hasRilVoiceRadioTechnologyChanged = false hasRilDataRadioTechnologyChanged = {1=true, 2=true} hasDataTransportPreferenceChanged = false hasChanged = true hasVoiceRoamingOn = false hasVoiceRoamingOff = false hasDataRoamingOn =false hasDataRoamingOff = false hasLocationChanged = false has4gHandoff = false hasMultiApnSupport = false hasLostMultiApnSupport = false hasCssIndicatorChanged = false hasNrFrequencyRangeChanged = false hasNrStateChanged = false hasVoiceRoamingTypeChange = false hasDataRoamingTypeChange = false hasAirplaneModeOnlChanged = false hasPlmnChange = true
09-29 16:20:25.480698  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:25.480863  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_CS_NETWORK_STATE_CHANGED [PHONE0]
09-29 16:20:25.482358  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:25.482481  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_NETWORK_STATE_CHANGED [PHONE0]
09-29 16:20:25.482669  1669  1833 D MTKSST  : [GsmSST0] MtkHandler: stop MTK turbo
09-29 16:20:25.483033  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: radio is on but out of service, set plmn='No service'
09-29 16:20:25.483109  1669  1871 D NRM-C-0 : onNetworkStateChanged
09-29 16:20:25.484289  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:25.484358  1669  1811 D RILJ    : [UNSL]< UNSOL_RESPONSE_PS_NETWORK_STATE_CHANGED [PHONE0]
09-29 16:20:25.485207  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: rawSpn = 
09-29 16:20:25.487840  1669  1669 D MTKSST  : [GsmSST0] localeOperator  is invalid
09-29 16:20:25.489732  1669  1669 D MTKSST  : [GsmSST0] Broadcasting ServiceState : {mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=null, mOperatorAlphaShort=null, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=false, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=, mOperatorAlphaShortRaw=, mIsIwlanPreferred=false, Ril Voice Regist state=2, Ril Data Regist state=0, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0}
09-29 16:20:25.490425  1669  1834 D NrMap-0 : EVENT_SERVICE_STATE_CHANGE camp_SA=false listening=false
09-29 16:20:25.490987  1669  1669 D DefaultPhoneNotifier: notifyServiceStateForSubId: mRegistryMgr=android.telephony.TelephonyRegistryManager@a3d5fbd ss={mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=null, mOperatorAlphaShort=null, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=false, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=, mOperatorAlphaShortRaw=, mIsIwlanPreferred=false, Ril Voice Regist state=2, Ril Data Regist state=0, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0} sender=Handler (com.mediatek.internal.telephony.MtkGsmCdmaPhone) {f245017} phondId=0 subId=-1
09-29 16:20:25.492971  1251  1985 D TelephonyRegistry: notifyServiceStateForSubscriber: INVALID phoneId=0 or subId=-1
09-29 16:20:25.493983  1251  1985 E PHONE   : ServiceState.getRadioTechnology() DEPRECATED will be removed *******
09-29 16:20:25.493733  1669  1897 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:25.501873  1251  1985 E PHONE   : ServiceState.getRadioTechnology() DEPRECATED will be removed *******
09-29 16:20:25.509135  1251  1667 E PHONE   : ServiceState.getRadioTechnology() DEPRECATED will be removed *******
09-29 16:20:25.514264  1251  1667 E PHONE   : ServiceState.getRadioTechnology() DEPRECATED will be removed *******
09-29 16:20:25.526446  1669  1669 D MtkRILJ : [0126]> MTK: RIL_REQUEST_SET_SERVICE_STATE voiceRegState: 1 dataRegState: 1 voiceRoamingType: 0 dataRoamingType: 0 rilVoiceRegState: 2 rilDataRegState:0 [SUB0]
09-29 16:20:25.530058  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:25.534111  1669  1811 D RILJ    : [0126]< MTK: RIL_REQUEST_SET_SERVICE_STATE  [PHONE0]
09-29 16:20:25.538366  1669  1669 D MTKSST  : [GsmSST0] onNetworkStateChangeResult state:0 Act:3 cause:0
09-29 16:20:25.538552  1669  1669 D MTKSST  : [GsmSST0] pollState: modemTriggered=true, mPollingContext=0, RadioState=1, connected=true, support_ap_iwlan=1
09-29 16:20:25.539928  1669  1669 D RILJ    : [0127]> OPERATOR [PHONE0]
09-29 16:20:25.540422  1669  1873 D IWlanNetworkService: getNetworkRegistrationState for domain 2, slotid: 0
09-29 16:20:25.540640  1669  1920 D IWlanNetworkService: createRegistrationState.
09-29 16:20:25.540676  1669  1920 D IWlanNetworkService: getAvailableServices.
09-29 16:20:25.540873  1669  1920 D IWlanNetworkService: Calling callback.onGetNetworkRegistrationStateComplete.resultCode = 0, netState = NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, slotid: 0
09-29 16:20:25.540960  1669  1920 D NRM-I-0 : onRequestNetworkRegistrationInfoComplete result: 0, info: NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}
09-29 16:20:25.541628  1669  1669 D RILJ    : [0128]> QUERY_NETWORK_SELECTION_MODE [PHONE0]
09-29 16:20:25.541759  1176  1202 I AT      : [0] AT> AT+EOPS? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:25.542701  1669  2023 D MTKSST  : [GsmSST0] updateLocatedPlmn(),previous plmn= null ,update to: 45005
09-29 16:20:25.542816  1669  1871 D RILJ    : [0129]> DATA_REGISTRATION_STATE [PHONE0]
09-29 16:20:25.542897  1669  1871 D RILJ    : getDataRegistrationState: overrideHalVersion=null [PHONE0]
09-29 16:20:25.543101  1669  2023 D SubscriptionManager: putPhoneIdAndSubIdExtra: no valid subs
09-29 16:20:25.544333  1669  1871 D RILJ    : [0130]> VOICE_REGISTRATION_STATE [PHONE0]
09-29 16:20:25.544405  1669  1871 D RILJ    : getVoiceRegistrationState: overrideHalVersion=null [PHONE0]
09-29 16:20:25.545189  1176  1201 I AT      : [0] AT< +EOPS: 0,2,"45005",1 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:25.545251  1176  1201 I AT      : [0] AT< OK (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:25.545653  1176  1202 D RmcNwRTReqHdlr: [0] requestQueryNetworkSelectionMode return 0
09-29 16:20:25.545821  1176  1202 I AT      : [0] AT> AT+E5GOPT? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:25.546672  1669  1669 D MTKSST  : [GsmSST0] new:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-55 ber=99 rscp=-53 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}, old:{level:0, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=2147483647 ber=2147483647 rscp=2147483647 ecno=2147483647 level=0,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthLte}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}
09-29 16:20:25.546766  1669  1811 D RILJ    : [0127]< OPERATOR {, , } [PHONE0]
09-29 16:20:25.547245  1669  1811 D RILJ    : [0128]< QUERY_NETWORK_SELECTION_MODE {0} [PHONE0]
09-29 16:20:25.547495  1251  1985 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:25.547610  1251  1985 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:25.548179  1176  1201 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:25.548869  1176  1192 D RmcNwReqHdlr: [0] [currentPhysicalChannelConfigs] needNotifyEmpty and has notified empty list, return
09-29 16:20:25.549542  1251  1667 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:25.549658  1251  1667 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:25.550005  1669  1871 D CellularNetworkService: No access tech specific info passes for RegStateResult
09-29 16:20:25.550077  1669  1811 D RILJ    : [0129]< DATA_REGISTRATION_STATE {.regState = UNKNOWN, .rat = UNKNOWN, .reasonForDenial = NONE, .cellIdentity = {.noinit = {}}, .registeredPlmn = , .accessTechnologySpecificInfo = {.noinit = {}}} [PHONE0]
09-29 16:20:25.550208  1669  1871 D NRM-C-0 : onRequestNetworkRegistrationInfoComplete result: 0, info: NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}
09-29 16:20:25.550643  1669  1871 D CellularNetworkService: No access tech specific info passes for RegStateResult
09-29 16:20:25.550674  1176  1182 E RtcDC   : [0][onServiceStateChanged] old or new data reg state is not InService
09-29 16:20:25.550729  1669  1811 D RILJ    : [0130]< VOICE_REGISTRATION_STATE {.regState = NOT_REG_MT_NOT_SEARCHING_OP_EM, .rat = UNKNOWN, .reasonForDenial = NONE, .cellIdentity = {.noinit = {}}, .registeredPlmn = , .accessTechnologySpecificInfo = {.noinit = {}}} [PHONE0]
09-29 16:20:25.550749  1176  1182 D RtcCC   : [0] updateImsCallRat dataRegState 4 dataRadioTech 0 wfcRegState 0
09-29 16:20:25.550749  1669  1669 D LocaleTracker-0: updateLocale: countryIso = , countryIsoDebugInfo = empty as default
09-29 16:20:25.550777  1669  1669 D LocaleTracker-0: updateLocale: timeZoneCountryIso = , timeZoneCountryIsoDebugInfo = Defaulted: empty as default
09-29 16:20:25.550808  1669  1669 D NewNitzStateMachineImpl: handleCountryUnavailable: mLatestNitzSignal=null
09-29 16:20:25.550852  1669  1871 D NRM-C-0 : onRequestNetworkRegistrationInfoComplete result: 0, info: NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=true availableServices=[EMERGENCY] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}
09-29 16:20:25.550925  1669  1669 D NewNitzStateMachineImpl: doTimeZoneDetection: countryIsoCode=null, nitzSignal=null, suggestion=TelephonyTimeZoneSuggestion{mSlotIndex=0, mZoneId='null', mMatchType=0, mQuality=0, mDebugInfo=[getTimeZoneSuggestion: nitzSignal=null, countryIsoCode=null, Detection reason=handleCountryUnavailable()]}, reason=handleCountryUnavailable()
09-29 16:20:25.550976  1176  1182 E RtcDC   : [0][onServiceStateChanged] old or new data reg state is not InService
09-29 16:20:25.551040  1176  1182 D RtcCC   : [0] updateImsCallRat dataRegState 4 dataRadioTech 0 wfcRegState 0
09-29 16:20:25.551139  1669  1669 D LocaleTracker-0: Starting LocaleTracker
09-29 16:20:25.552335  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:25.554323  1669  1811 D RILJ    : [UNSL]< MTK: RIL_UNSOL_QUALIFIED_NETWORK_TYPES_CHANGED {1, 2178, 1} [PHONE0]
09-29 16:20:25.554679  1669  1919 D MtkQualifiedNetworksService: UPDATE_QUALIFIED_NETWORKS mode=1 apnTypes=2178
09-29 16:20:25.554780  1669  1919 D MtkQualifiedNetworksService: availabilityUpdate[2]=3
09-29 16:20:25.555054  1669  1870 D ANM-0   : onQualifiedNetworkTypesChanged. apnTypes = [mms,cbs,xcap], networks = [EUTRAN]
09-29 16:20:25.555260  1669  1870 D ANM-0   : Available networks for mms not changed.
09-29 16:20:25.555319  1669  1870 D ANM-0   : Available networks for cbs not changed.
09-29 16:20:25.555342  1669  1870 D ANM-0   : Available networks for xcap not changed.
09-29 16:20:25.555823  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:25.557407  1669  1811 D RILJ    : [UNSL]< MTK: RIL_UNSOL_QUALIFIED_NETWORK_TYPES_CHANGED {1, 2178, 1} [PHONE0]
09-29 16:20:25.557672  1669  1919 D MtkQualifiedNetworksService: UPDATE_QUALIFIED_NETWORKS mode=1 apnTypes=2178
09-29 16:20:25.557763  1669  1919 D MtkQualifiedNetworksService: availabilityUpdate[2]=3
09-29 16:20:25.557980  1669  1870 D ANM-0   : onQualifiedNetworkTypesChanged. apnTypes = [mms,cbs,xcap], networks = [EUTRAN]
09-29 16:20:25.558055  1669  1870 D ANM-0   : Available networks for mms not changed.
09-29 16:20:25.558073  1669  1870 D ANM-0   : Available networks for cbs not changed.
09-29 16:20:25.558090  1669  1870 D ANM-0   : Available networks for xcap not changed.
09-29 16:20:25.559091  1669  1669 D NetworkTypeController: [0] LegacyState: process EVENT_DATA_RAT_CHANGED
09-29 16:20:25.559409  1669  1669 D NetworkTypeController: [0] Remove all timers
09-29 16:20:25.559517  1669  1669 D NetworkTypeController: [0] Remove all timers
09-29 16:20:25.559616  1669  1669 D MtkNetworkTypeController: [Override]getCurrentOverrideNetworkType: 0
09-29 16:20:25.560727  1669  1669 D NetworkTypeController: [0] LegacyState: process EVENT_DATA_RAT_CHANGED
09-29 16:20:25.560955  1669  1669 D NetworkTypeController: [0] Remove all timers
09-29 16:20:25.561044  1669  1669 D NetworkTypeController: [0] Remove all timers
09-29 16:20:25.561171  1669  1669 D MtkNetworkTypeController: [Override]getCurrentOverrideNetworkType: 0
09-29 16:20:25.561424  1669  1669 D MtkNetworkTypeController: handleMessage: msg = 101
09-29 16:20:25.561648  1669  1669 D MTKSST  : [GsmSST0] pollState: modemTriggered=false, mPollingContext=5, RadioState=1, connected=true, support_ap_iwlan=1
09-29 16:20:25.561937  1669  1669 D MTKSST  : [GsmSST0] handlePollStateResultMessage: PS IWLAN. NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}
09-29 16:20:25.562356  1669  1669 D MTKSST  : [GsmSST0] EVENT_POLL_STATE_NETWORK_SELECTION_MODE
09-29 16:20:25.562643  1669  1669 D MTKSST  : [GsmSST0] handlePollStateResultMessage: PS cellular. NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}
09-29 16:20:25.563184  1669  1669 E MTKSST  : [GsmSST0] Exception while polling service state. Probably malformed RIL response.java.lang.NullPointerException: Attempt to invoke virtual method 'int android.telephony.CellIdentity.getType()' on a null object reference
09-29 16:20:25.563455  1669  1669 D MTKSST  : [GsmSST0] Could not set ServiceState channel number. CellIdentity null
09-29 16:20:25.563988  1669  1669 D MTKSST  : [GsmSST0] combinePsRegistrationStates: {mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=, mOperatorAlphaShort=, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=false, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=true availableServices=[EMERGENCY] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=, mOperatorAlphaShortRaw=, mIsIwlanPreferred=false, Ril Voice Regist state=0, Ril Data Regist state=4, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0}
09-29 16:20:25.564443  1669  1669 D MtkRILJ : lookupOperatorNameNitz plmn name update to Nitz: 
09-29 16:20:25.564573  1669  1669 E MTKSST  : lookupOperatorName getPhone null subid=-1
09-29 16:20:25.564834  1669  1669 D MtkRILJ : lookupOperatorNameMVNO plmn name update to TS.25/MVNO: 
09-29 16:20:25.565004  1669  1669 D MtkRILJ : lookupOperatorNameNitz plmn name update to Nitz: 
09-29 16:20:25.565080  1669  1669 E MTKSST  : lookupOperatorName getPhone null subid=-1
09-29 16:20:25.565194  1669  1669 D MtkRILJ : lookupOperatorNameMVNO plmn name update to TS.25/MVNO: 
09-29 16:20:25.565345  1669  1669 D MTKSST  : [GsmSST0] refreshSpn: null, null, fromPollState=true, mForceBroadcastServiceState=true
09-29 16:20:25.566934  1669  1669 D MTKSST  : [GsmSST0] Could not set ServiceState channel number. CellIdentity null
09-29 16:20:25.567588  1669  1669 D MTKSST  : [GsmSST0] Poll ServiceState done: oldSS=[{mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=null, mOperatorAlphaShort=null, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=false, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=, mOperatorAlphaShortRaw=, mIsIwlanPreferred=false, Ril Voice Regist state=2, Ril Data Regist state=0, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0}]
09-29 16:20:25.568661  1669  1669 D MTKSST  : [GsmSST0] Poll ServiceState done: newSS=[{mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=null, mOperatorAlphaShort=null, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=true, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=true availableServices=[EMERGENCY] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=, mOperatorAlphaShortRaw=, mIsIwlanPreferred=false, Ril Voice Regist state=0, Ril Data Regist state=4, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0}] oldMaxDataCalls=16 mNewMaxDataCalls=16 oldReasonDataDenied=0 mNewReasonDataDenied=0 isImsEccOnly= false
09-29 16:20:25.569144  1669  1669 D MTKSST  : [GsmSST0] pollStateDone: hasRegistered = false hasDeregistered = false hasDataAttached = {1=false, 2=false} hasDataDetached = {1=false, 2=false} hasDataRegStateChanged = {1=true, 2=false} hasRilVoiceRadioTechnologyChanged = false hasRilDataRadioTechnologyChanged = {1=false, 2=false} hasDataTransportPreferenceChanged = false hasChanged = true hasVoiceRoamingOn = false hasVoiceRoamingOff = false hasDataRoamingOn =false hasDataRoamingOff = false hasLocationChanged = false has4gHandoff = false hasMultiApnSupport = false hasLostMultiApnSupport = false hasCssIndicatorChanged = false hasNrFrequencyRangeChanged = false hasNrStateChanged = false hasVoiceRoamingTypeChange = false hasDataRoamingTypeChange = false hasAirplaneModeOnlChanged = false hasPlmnChange = false
09-29 16:20:25.572751  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: radio is on but out of service, set plmn='Emergency calls only'
09-29 16:20:25.574335  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: rawSpn = 
09-29 16:20:25.583496  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: updateSpnDisplay: changed sending intent, rule=2, showPlmn='true', plmn='Emergency calls only', showSpn='false', spn='null', dataSpn='', subId='-1'
09-29 16:20:25.583761  1669  1669 D SubscriptionManager: putPhoneIdAndSubIdExtra: no valid subs
09-29 16:20:25.585216  1669  1833 D MTKSST  : [GsmSST0] MtkHandler: EVENT_UPDATE_PLMN MtkPlmn showPlmn=true plmn=Emergency calls only showSpn=false spn=null
09-29 16:20:25.586171  1669  1833 D SubscriptionController: [setPlmnSpn] No valid subscription to store info
09-29 16:20:25.589585  1669  1669 D MTKSST  : [GsmSST0] localeOperator  is invalid
09-29 16:20:25.590192  1669  1833 D SubscriptionManager: [getSubId]- fail
09-29 16:20:25.591374  1872  1872 D ImsDataTracker: onSubscriptionsChanged
09-29 16:20:25.593062  1669  1669 D MTKSST  : [GsmSST0] Broadcasting ServiceState : {mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=null, mOperatorAlphaShort=null, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=true, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=true availableServices=[EMERGENCY] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=, mOperatorAlphaShortRaw=, mIsIwlanPreferred=false, Ril Voice Regist state=0, Ril Data Regist state=4, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0}
09-29 16:20:25.593300  1176  1184 I AT      : [0] AT< +EBARRING: 2, 4, 0, 0, , , , 1, 0, , , , 2, 0, , , , 8, 0 (RIL_URC_READER, tid:493447834880)
09-29 16:20:25.593461  1669  1834 D NrMap-0 : EVENT_SERVICE_STATE_CHANGE camp_SA=false listening=false
09-29 16:20:25.593944  1669  1669 D DefaultPhoneNotifier: notifyServiceStateForSubId: mRegistryMgr=android.telephony.TelephonyRegistryManager@a3d5fbd ss={mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=null, mOperatorAlphaShort=null, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=true, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=true availableServices=[EMERGENCY] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=, mOperatorAlphaShortRaw=, mIsIwlanPreferred=false, Ril Voice Regist state=0, Ril Data Regist state=4, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0} sender=Handler (com.mediatek.internal.telephony.MtkGsmCdmaPhone) {f245017} phondId=0 subId=-1
09-29 16:20:25.594215  1669  2002 E PhoneSubInfoController: getIccSerialNumber phone is null for Subscription:-1
09-29 16:20:25.594848  1251  1667 D TelephonyRegistry: notifyServiceStateForSubscriber: INVALID phoneId=0 or subId=-1
09-29 16:20:25.595213  1251  1667 E PHONE   : ServiceState.getRadioTechnology() DEPRECATED will be removed *******
09-29 16:20:25.599643  1251  1667 E PHONE   : ServiceState.getRadioTechnology() DEPRECATED will be removed *******
09-29 16:20:25.606939  1251  1985 E PHONE   : ServiceState.getRadioTechnology() DEPRECATED will be removed *******
09-29 16:20:25.612151  1251  1985 E PHONE   : ServiceState.getRadioTechnology() DEPRECATED will be removed *******
09-29 16:20:25.620679  1669  1669 D MtkRILJ : [0133]> MTK: RIL_REQUEST_SET_SERVICE_STATE voiceRegState: 1 dataRegState: 1 voiceRoamingType: 0 dataRoamingType: 0 rilVoiceRegState: 0 rilDataRegState:4 [SUB0]
09-29 16:20:25.625511  1669  1669 D RILJ    : [0134]> GET_CELL_INFO_LIST [PHONE0]
09-29 16:20:25.626124  1669  1669 D ImsPhoneCallTracker: [0] SubscriptionListener.onSubscriptionInfoChanged, subId=-1
09-29 16:20:25.628997  1669  1669 E PhoneSubInfoController: getLine1Number phone is null for Subscription:-1
09-29 16:20:25.629072  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:25.629499  1176  1192 I AT      : [0] AT> AT+ECELL (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:25.629613  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:1
09-29 16:20:25.630792  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(1) return true
09-29 16:20:25.630868  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:7
09-29 16:20:25.631432  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(7) return false
09-29 16:20:25.631944  1669  1811 D RILJ    : [0133]< MTK: RIL_REQUEST_SET_SERVICE_STATE  [PHONE0]
09-29 16:20:25.632962  1669  1669 D MtkImsManagerIM [0]: Vt, isVilteResourceSupport:true, isVinrResourceSupport:false, isCarrierConfigSupport:true, isGbaValidSupport:true, isFeatureEnableByPlatformExt:true
09-29 16:20:25.637572  1176  1191 I AT      : [0] AT< +ECELL=*** (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:25.637696  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:25.637822  1176  1192 D RmcNwReqHdlr: [0] No cell info listed, num=0
09-29 16:20:25.640391  1669  1811 D RILJ    : [0134]< GET_CELL_INFO_LIST [CellInfoGsm:{mRegistered=NO mTimeStamp=34459531770ns mCellConnectionStatus=0 CellIdentityGsm:{ mLac=0 mCid=0 mArfcn=0 mBsic=0x0 mMcc=450 mMnc=05 mAlphaLong= mAlphaShort= mAdditionalPlmns={}} CellSignalStrengthGsm: rssi=-113 ber=0 mTa=0 mLevel=0}] [PHONE0]
09-29 16:20:25.645697  1669  1669 D MTKSST  : [GsmSST0] SubscriptionListener.onSubscriptionInfoChanged
09-29 16:20:25.660193  1669  1669 D SubscriptionController: [setDefaultVoiceSubId] default phone account not changed
09-29 16:20:25.668514  1669  1669 D DSSExt  : handleSubinfoRecordUpdated: detectedType = 4
09-29 16:20:25.668995  1669  1669 D DSSExt  : getHighCapabilityPhoneIdBySimType : -1
09-29 16:20:25.669244  1669  1669 D DSSExt  : DataSubSelector for OM: no pin lock
09-29 16:20:25.670464  1669  1669 D DSSExt  : Default data phoneid = -1
09-29 16:20:25.672592  1669  1669 D LocaleTracker-0: updateLocale: countryIso = , countryIsoDebugInfo = empty as default
09-29 16:20:25.672719  1669  1669 D LocaleTracker-0: updateLocale: timeZoneCountryIso = , timeZoneCountryIsoDebugInfo = Defaulted: empty as default
09-29 16:20:25.672796  1669  1669 D NewNitzStateMachineImpl: handleCountryUnavailable: mLatestNitzSignal=null
09-29 16:20:25.674038  1669  1669 D NewNitzStateMachineImpl: doTimeZoneDetection: countryIsoCode=null, nitzSignal=null, suggestion=TelephonyTimeZoneSuggestion{mSlotIndex=0, mZoneId='null', mMatchType=0, mQuality=0, mDebugInfo=[getTimeZoneSuggestion: nitzSignal=null, countryIsoCode=null, Detection reason=handleCountryUnavailable()]}, reason=handleCountryUnavailable()
09-29 16:20:25.685558  1669  1669 D NetworkTypeController: [0] LegacyState: process EVENT_DATA_RAT_CHANGED
09-29 16:20:25.685897  1669  1669 D NetworkTypeController: [0] Remove all timers
09-29 16:20:25.686066  1669  1669 D NetworkTypeController: [0] Remove all timers
09-29 16:20:25.686217  1669  1669 D MtkNetworkTypeController: [Override]getCurrentOverrideNetworkType: 0
09-29 16:20:25.686526  1669  1669 D MTKSST  : [GsmSST0] pollState: modemTriggered=false, mPollingContext=0, RadioState=1, connected=true, support_ap_iwlan=1
09-29 16:20:25.687932  1669  1669 D RILJ    : [0135]> OPERATOR [PHONE0]
09-29 16:20:25.688559  1669  1873 D IWlanNetworkService: getNetworkRegistrationState for domain 2, slotid: 0
09-29 16:20:25.688713  1669  1920 D IWlanNetworkService: createRegistrationState.
09-29 16:20:25.688743  1669  1920 D IWlanNetworkService: getAvailableServices.
09-29 16:20:25.688951  1669  1920 D IWlanNetworkService: Calling callback.onGetNetworkRegistrationStateComplete.resultCode = 0, netState = NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, slotid: 0
09-29 16:20:25.689061  1669  1920 D NRM-I-0 : onRequestNetworkRegistrationInfoComplete result: 0, info: NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}
09-29 16:20:25.689496  1176  1202 I AT      : [0] AT> AT+EOPS? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:25.689581  1669  1669 D RILJ    : [0136]> QUERY_NETWORK_SELECTION_MODE [PHONE0]
09-29 16:20:25.690441  1669  1871 D RILJ    : [0137]> DATA_REGISTRATION_STATE [PHONE0]
09-29 16:20:25.690579  1669  1871 D RILJ    : getDataRegistrationState: overrideHalVersion=null [PHONE0]
09-29 16:20:25.691767  1669  1871 D RILJ    : [0138]> VOICE_REGISTRATION_STATE [PHONE0]
09-29 16:20:25.691828  1669  1871 D RILJ    : getVoiceRegistrationState: overrideHalVersion=null [PHONE0]
09-29 16:20:25.692566  1669  1669 E PhoneSubInfoController: getLine1Number phone is null for Subscription:-1
09-29 16:20:25.693493  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:1
09-29 16:20:25.694569  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(1) return true
09-29 16:20:25.694712  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:7
09-29 16:20:25.695526  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(7) return false
09-29 16:20:25.697072  1176  1201 I AT      : [0] AT< +EOPS: 0,2,"45005",1 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:25.697213  1176  1201 I AT      : [0] AT< OK (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:25.697489  1669  1669 D MtkImsManagerIM [0]: Vt, isVilteResourceSupport:true, isVinrResourceSupport:false, isCarrierConfigSupport:true, isGbaValidSupport:true, isFeatureEnableByPlatformExt:true
09-29 16:20:25.697565  1176  1202 D RmcNwRTReqHdlr: [0] requestQueryNetworkSelectionMode return 0
09-29 16:20:25.697727  1176  1202 I AT      : [0] AT> AT+E5GOPT? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:25.698125  1669  1811 D RILJ    : [0135]< OPERATOR {, , } [PHONE0]
09-29 16:20:25.698593  1669  1811 D RILJ    : [0136]< QUERY_NETWORK_SELECTION_MODE {0} [PHONE0]
09-29 16:20:25.705393  1176  1201 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:25.706075  1176  1192 D RmcNwReqHdlr: [0] [currentPhysicalChannelConfigs] needNotifyEmpty and has notified empty list, return
09-29 16:20:25.706948  1669  1871 D CellularNetworkService: No access tech specific info passes for RegStateResult
09-29 16:20:25.707022  1669  1811 D RILJ    : [0137]< DATA_REGISTRATION_STATE {.regState = UNKNOWN, .rat = UNKNOWN, .reasonForDenial = NONE, .cellIdentity = {.noinit = {}}, .registeredPlmn = , .accessTechnologySpecificInfo = {.noinit = {}}} [PHONE0]
09-29 16:20:25.707152  1669  1871 D NRM-C-0 : onRequestNetworkRegistrationInfoComplete result: 0, info: NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}
09-29 16:20:25.707569  1669  1871 D CellularNetworkService: No access tech specific info passes for RegStateResult
09-29 16:20:25.707718  1669  1811 D RILJ    : [0138]< VOICE_REGISTRATION_STATE {.regState = NOT_REG_MT_NOT_SEARCHING_OP_EM, .rat = UNKNOWN, .reasonForDenial = NONE, .cellIdentity = {.noinit = {}}, .registeredPlmn = , .accessTechnologySpecificInfo = {.noinit = {}}} [PHONE0]
09-29 16:20:25.707853  1669  1871 D NRM-C-0 : onRequestNetworkRegistrationInfoComplete result: 0, info: NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=true availableServices=[EMERGENCY] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}
09-29 16:20:25.741860  1669  1669 D MTKSST  : [GsmSST0] handlePollStateResultMessage: PS IWLAN. NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}
09-29 16:20:25.742262  1669  1669 D LocaleTracker-0: processCellInfo: cell info=[CellInfoGsm:{mRegistered=NO mTimeStamp=34459531770ns mCellConnectionStatus=0 CellIdentityGsm:{ mLac=0 mCid=0 mArfcn=0 mBsic=0x0 mMcc=450 mMnc=05 mAlphaLong= mAlphaShort= mAdditionalPlmns={}} CellSignalStrengthGsm: rssi=-113 ber=0 mTa=0 mLevel=0}]
09-29 16:20:25.766194  1669  1669 D LocaleTracker-0: updateLocale: countryIso = kr, countryIsoDebugInfo = CellInfo: MccTable.countryCodeForMcc("450")
09-29 16:20:25.766491  1669  1669 D LocaleTracker-0: updateLocale: Change the current country to "kr", countryIsoDebugInfo = CellInfo: MccTable.countryCodeForMcc("450"), mCellInfoList = [CellInfoGsm:{mRegistered=NO mTimeStamp=34459531770ns mCellConnectionStatus=0 CellIdentityGsm:{ mLac=0 mCid=0 mArfcn=0 mBsic=0x0 mMcc=450 mMnc=05 mAlphaLong= mAlphaShort= mAdditionalPlmns={}} CellSignalStrengthGsm: rssi=-113 ber=0 mTa=0 mLevel=0}]
09-29 16:20:25.766957  1669  1669 D LocaleTracker-0: update country iso in sharedPrefs kr
09-29 16:20:25.768318  1669  1669 D SubscriptionManager: putPhoneIdAndSubIdExtra: no valid subs
09-29 16:20:25.769436  1669  1669 D LocaleTracker-0: updateLocale: timeZoneCountryIso = kr, timeZoneCountryIsoDebugInfo = CellInfo: MccTable.geoCountryCodeForMccMnc(MccMnc{mcc='450', mnc='05'})
09-29 16:20:25.769606  1669  1669 D NewNitzStateMachineImpl: handleCountryDetected: countryIsoCode=kr, mLatestNitzSignal=null
09-29 16:20:25.770841  1872  1872 I WfcLocationHandler: ACTION_LOCATED_PLMN_CHANGED, iso: KR
09-29 16:20:25.772257  1872  1872 I WfcLocationHandler: isCtaNotAllow: false
09-29 16:20:25.773655  1872  1923 I WfcLocationHandler: setLocationInfo info=[LocationInfo objId: 37684093, phoneId: 0, transationId: 0, accuracy: 0.0, confidence: 0, vericalAxisAccuracy: 0.0, broadcastFlag: 1, method: , city: , state: ***nown, zip: , countryCode: *R, time: 0, mPlmnCountryCode:KR
09-29 16:20:25.777684  1176  1182 D RtcMwi  : [0] onHandleRequest: request id 60528 is RFX_MSG_REQUEST_SET_GEO_LOCATION
09-29 16:20:25.778057  1176  1196 D RmcMwi  : [0] setGeoLocation, original dataLen: 16
09-29 16:20:25.778145  1176  1196 I AT      : [0] AT> AT+EIMSGEO=*** (RIL_CMD_READER_3, tid:493435399424)
09-29 16:20:25.785253  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:25.785679  1176  1182 D RtcMwi  : [0] onHandleResponse, handle RFX_MSG_REQUEST_SET_GEO_LOCATION
09-29 16:20:25.791483  1669  1669 D NewNitzStateMachineImpl: doTimeZoneDetection: countryIsoCode=kr, nitzSignal=null, suggestion=TelephonyTimeZoneSuggestion{mSlotIndex=0, mZoneId='Asia/Seoul', mMatchType=2, mQuality=1, mDebugInfo=[findTimeZoneFromNetworkCountryCode: whenMillis=1664436025769, countryIsoCode=kr, findTimeZoneFromNetworkCountryCode: lookupResult=CountryResult{zoneId='Asia/Seoul', quality=1, mDebugInfo=One effective time zone found at whenMillis=1664436025769}, Detection reason=handleCountryDetected("kr")]}, reason=handleCountryDetected("kr")
09-29 16:20:25.792864  1669  1669 D MTKSST  : [GsmSST0] EVENT_POLL_STATE_NETWORK_SELECTION_MODE
09-29 16:20:25.793374  1669  1669 D MTKSST  : [GsmSST0] handlePollStateResultMessage: PS cellular. NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}
09-29 16:20:25.793813  1669  1669 E MTKSST  : [GsmSST0] Exception while polling service state. Probably malformed RIL response.java.lang.NullPointerException: Attempt to invoke virtual method 'int android.telephony.CellIdentity.getType()' on a null object reference
09-29 16:20:25.794042  1669  1669 D MTKSST  : [GsmSST0] Could not set ServiceState channel number. CellIdentity null
09-29 16:20:25.794604  1669  1669 D MTKSST  : [GsmSST0] combinePsRegistrationStates: {mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=, mOperatorAlphaShort=, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=false, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=true availableServices=[EMERGENCY] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=, mOperatorAlphaShortRaw=, mIsIwlanPreferred=false, Ril Voice Regist state=0, Ril Data Regist state=4, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0}
09-29 16:20:25.794987  1669  1669 D MtkRILJ : lookupOperatorNameNitz plmn name update to Nitz: 
09-29 16:20:25.795089  1669  1669 E MTKSST  : lookupOperatorName getPhone null subid=-1
09-29 16:20:25.795284  1669  1669 D MtkRILJ : lookupOperatorNameMVNO plmn name update to TS.25/MVNO: 
09-29 16:20:25.795416  1669  1669 D MtkRILJ : lookupOperatorNameNitz plmn name update to Nitz: 
09-29 16:20:25.795460  1669  1669 E MTKSST  : lookupOperatorName getPhone null subid=-1
09-29 16:20:25.795532  1669  1669 D MtkRILJ : lookupOperatorNameMVNO plmn name update to TS.25/MVNO: 
09-29 16:20:25.795725  1669  1669 D MTKSST  : [GsmSST0] refreshSpn: null, null, fromPollState=true, mForceBroadcastServiceState=true
09-29 16:20:25.796867  1669  1669 D MTKSST  : [GsmSST0] Could not set ServiceState channel number. CellIdentity null
09-29 16:20:25.797385  1669  1669 D MTKSST  : [GsmSST0] Poll ServiceState done: oldSS=[{mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=null, mOperatorAlphaShort=null, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=true, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=true availableServices=[EMERGENCY] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=, mOperatorAlphaShortRaw=, mIsIwlanPreferred=false, Ril Voice Regist state=0, Ril Data Regist state=4, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0}]
09-29 16:20:25.797846  1669  1669 D MTKSST  : [GsmSST0] Poll ServiceState done: newSS=[{mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=null, mOperatorAlphaShort=null, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=true, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=true availableServices=[EMERGENCY] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=, mOperatorAlphaShortRaw=, mIsIwlanPreferred=false, Ril Voice Regist state=0, Ril Data Regist state=4, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0}] oldMaxDataCalls=16 mNewMaxDataCalls=16 oldReasonDataDenied=0 mNewReasonDataDenied=0 isImsEccOnly= false
09-29 16:20:25.798426  1669  1669 D MTKSST  : [GsmSST0] pollStateDone: hasRegistered = false hasDeregistered = false hasDataAttached = {1=false, 2=false} hasDataDetached = {1=false, 2=false} hasDataRegStateChanged = {1=false, 2=false} hasRilVoiceRadioTechnologyChanged = false hasRilDataRadioTechnologyChanged = {1=false, 2=false} hasDataTransportPreferenceChanged = false hasChanged = true hasVoiceRoamingOn = false hasVoiceRoamingOff = false hasDataRoamingOn =false hasDataRoamingOff = false hasLocationChanged = false has4gHandoff = false hasMultiApnSupport = false hasLostMultiApnSupport = false hasCssIndicatorChanged = false hasNrFrequencyRangeChanged = false hasNrStateChanged = false hasVoiceRoamingTypeChange = false hasDataRoamingTypeChange = false hasAirplaneModeOnlChanged = false hasPlmnChange = false
09-29 16:20:25.802298  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: radio is on but out of service, set plmn='Emergency calls only'
09-29 16:20:25.803301  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: rawSpn = 
09-29 16:20:25.805532  1669  1669 D MTKSST  : [GsmSST0] localeOperator  is invalid
09-29 16:20:25.806951  1669  1669 D MTKSST  : [GsmSST0] Broadcasting ServiceState : {mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=null, mOperatorAlphaShort=null, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=true, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=true availableServices=[EMERGENCY] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=, mOperatorAlphaShortRaw=, mIsIwlanPreferred=false, Ril Voice Regist state=0, Ril Data Regist state=4, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0}
09-29 16:20:25.810510  1669  1669 D MtkRILJ : [0139]> MTK: RIL_REQUEST_SET_SERVICE_STATE voiceRegState: 1 dataRegState: 1 voiceRoamingType: 0 dataRoamingType: 0 rilVoiceRegState: 0 rilDataRegState:4 [SUB0]
09-29 16:20:25.815092  1669  1669 D EmergencyNumberTracker: ACTION_NETWORK_COUNTRY_CHANGED: PhoneId: 0 CountryIso: kr
09-29 16:20:25.818921  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:25.819825  1669  1669 E PhoneSubInfoController: getLine1Number phone is null for Subscription:-1
09-29 16:20:25.821107  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:1
09-29 16:20:25.821702  1669  1811 D RILJ    : [0139]< MTK: RIL_REQUEST_SET_SERVICE_STATE  [PHONE0]
09-29 16:20:25.822010  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(1) return true
09-29 16:20:25.822129  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:7
09-29 16:20:25.822735  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(7) return false
09-29 16:20:25.824238  1669  1669 D MtkImsManagerIM [0]: Vt, isVilteResourceSupport:true, isVinrResourceSupport:false, isCarrierConfigSupport:true, isGbaValidSupport:true, isFeatureEnableByPlatformExt:true
09-29 16:20:25.833572  1669  1669 D EmergencyNumberTracker: updateEmergencyNumberListDatabaseAndNotify(): receiving countryIso: kr
09-29 16:20:25.834949  1669  1669 D EmergencyNumberTracker: kr asset emergency database is loaded. Ver: 2 Phone Id: 0
09-29 16:20:25.836014  1669  1669 E EmergencyNumberTracker: Cache ota emergency database IOException: java.io.FileNotFoundException: /data/misc/emergencynumberdb/emergency_number_db: open failed: ENOENT (No such file or directory)
09-29 16:20:25.836081  1669  1669 D EmergencyNumberTracker: Using Asset Emergency database. Version: 2
09-29 16:20:25.836772  1669  1669 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:25.837250  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-112|CountryIso-kr|Mnc-|ServiceCategories-1|Urns-[]|Sources-10000|Routing-0 vs EmergencyNumber:Number-112|CountryIso-kr|Mnc-|ServiceCategories-1|Urns-[]|Sources-10000|Routing-0
09-29 16:20:25.837396  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-911|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-911|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.837469  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-000|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-000|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.837524  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-08|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-08|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.837574  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-110|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-110|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.837634  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-118|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-118|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.837700  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-119|CountryIso-kr|Mnc-|ServiceCategories-110|Urns-[]|Sources-10000|Routing-0 vs EmergencyNumber:Number-119|CountryIso-kr|Mnc-|ServiceCategories-110|Urns-[]|Sources-10000|Routing-0
09-29 16:20:25.837761  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-999|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-999|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.838006  1669  1669 E EmergencyNumberTracker: getEmergencyNumberListFromEccListDatabaseAndTest: radio indication is unavailable in 1.4 HAL.
09-29 16:20:25.838173  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-112|CountryIso-kr|Mnc-|ServiceCategories-1|Urns-[]|Sources-10000|Routing-0 vs EmergencyNumber:Number-112|CountryIso-kr|Mnc-|ServiceCategories-1|Urns-[]|Sources-10000|Routing-0
09-29 16:20:25.838278  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-119|CountryIso-kr|Mnc-|ServiceCategories-110|Urns-[]|Sources-10000|Routing-0 vs EmergencyNumber:Number-119|CountryIso-kr|Mnc-|ServiceCategories-110|Urns-[]|Sources-10000|Routing-0
09-29 16:20:25.839284  1669  1669 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:25.839599  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-112|CountryIso-kr|Mnc-|ServiceCategories-1|Urns-[]|Sources-10000|Routing-0 vs EmergencyNumber:Number-112|CountryIso-kr|Mnc-|ServiceCategories-1|Urns-[]|Sources-10000|Routing-0
09-29 16:20:25.839801  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-911|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-911|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.839916  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-000|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-000|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.839999  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-08|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-08|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.840064  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-110|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-110|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.840122  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-118|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-118|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.840194  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-119|CountryIso-kr|Mnc-|ServiceCategories-110|Urns-[]|Sources-10000|Routing-0 vs EmergencyNumber:Number-119|CountryIso-kr|Mnc-|ServiceCategories-110|Urns-[]|Sources-10000|Routing-0
09-29 16:20:25.840264  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-999|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-999|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.840463  1669  1669 E EmergencyNumberTracker: getEmergencyNumberListFromEccListDatabaseAndTest: radio indication is unavailable in 1.4 HAL.
09-29 16:20:25.840646  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-112|CountryIso-kr|Mnc-|ServiceCategories-1|Urns-[]|Sources-10000|Routing-0 vs EmergencyNumber:Number-112|CountryIso-kr|Mnc-|ServiceCategories-1|Urns-[]|Sources-10000|Routing-0
09-29 16:20:25.840752  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-119|CountryIso-kr|Mnc-|ServiceCategories-110|Urns-[]|Sources-10000|Routing-0 vs EmergencyNumber:Number-119|CountryIso-kr|Mnc-|ServiceCategories-110|Urns-[]|Sources-10000|Routing-0
09-29 16:20:25.841021  1669  1669 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:25.841517  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-112|CountryIso-kr|Mnc-|ServiceCategories-1|Urns-[]|Sources-10000|Routing-0 vs EmergencyNumber:Number-112|CountryIso-kr|Mnc-|ServiceCategories-1|Urns-[]|Sources-10000|Routing-0
09-29 16:20:25.841705  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-911|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-911|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.841803  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-000|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-000|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.841881  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-08|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-08|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.841955  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-110|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-110|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.842012  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-118|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-118|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.842076  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-119|CountryIso-kr|Mnc-|ServiceCategories-110|Urns-[]|Sources-10000|Routing-0 vs EmergencyNumber:Number-119|CountryIso-kr|Mnc-|ServiceCategories-110|Urns-[]|Sources-10000|Routing-0
09-29 16:20:25.842188  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-999|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0 vs EmergencyNumber:Number-999|CountryIso-|Mnc-|ServiceCategories-0|Urns-[]|Sources-0|Routing-0
09-29 16:20:25.842384  1669  1669 E EmergencyNumberTracker: getEmergencyNumberListFromEccListDatabaseAndTest: radio indication is unavailable in 1.4 HAL.
09-29 16:20:25.842571  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-112|CountryIso-kr|Mnc-|ServiceCategories-1|Urns-[]|Sources-10000|Routing-0 vs EmergencyNumber:Number-112|CountryIso-kr|Mnc-|ServiceCategories-1|Urns-[]|Sources-10000|Routing-0
09-29 16:20:25.842690  1669  1669 E EmergencyNumber: Found unexpected duplicate numbers: EmergencyNumber:Number-119|CountryIso-kr|Mnc-|ServiceCategories-110|Urns-[]|Sources-10000|Routing-0 vs EmergencyNumber:Number-119|CountryIso-kr|Mnc-|ServiceCategories-110|Urns-[]|Sources-10000|Routing-0
09-29 16:20:25.843714  1669  1669 D EmergencyNumberTracker: notifyEmergencyNumberList(): notified
09-29 16:20:25.845198  1669  1669 E PhoneSubInfoController: getLine1Number phone is null for Subscription:-1
09-29 16:20:25.846196  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:1
09-29 16:20:25.846940  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(1) return true
09-29 16:20:25.847061  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport, feature:7
09-29 16:20:25.847781  1669  1669 D MtkImsManagerIM [0]: isImsResourceSupport(7) return false
09-29 16:20:25.849440  1669  1669 D MtkImsManagerIM [0]: Vt, isVilteResourceSupport:true, isVinrResourceSupport:false, isCarrierConfigSupport:true, isGbaValidSupport:true, isFeatureEnableByPlatformExt:true
09-29 16:20:26.830141  1669  1669 D MtkTelephonyAssist: MtkPhoneAssistBroadcastReceiver: MtkPhoneAssistBroadcastReceiver action = android.telephony.action.SIM_CARD_STATE_CHANGED isSystemUser = true
09-29 16:20:26.841356  1669  1669 D MtkTelephonyAssist: MtkTelephonyAssistService: MtkTelephonyService created
09-29 16:20:26.850080  1669  1669 D MtkTelephonyAssist: MtkTelephonyAssistService: phoneCreated = false mPhoneCreated = true phone count = 1
09-29 16:20:26.856239  1176  1176 I RILC    : [16] setResponseFunctionsAssist
09-29 16:20:26.856795  1669  1669 D MtkTelephonyAssist: DataStateController: initialize
09-29 16:20:26.862917  1669  1669 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.mediatek.telephony listener=com.mediatek.telephony.DataStateController$1@bdce72b
09-29 16:20:26.865892  1669  1669 D MtkTelephonyAssist: DataStateController: phoneId = 0 old state = false new state = true
09-29 16:20:26.866828  1669  1669 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:26.866913  1176  1198 I AT      : [0] AT> AT+EFD=3,1 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:26.867828  1669  1669 D ImsPhoneCallTracker: [0] handleMessage what=23
09-29 16:20:26.867987  1669  1669 D ImsPhoneCallTracker: [0] handleMessage what=23
09-29 16:20:26.868049  1669  1669 D ImsPhoneCallTracker: [0] onDataEnabledChanged: enabled=true, reason=0
09-29 16:20:26.868100  1669  1669 D ImsPhoneCallTracker: [0] Ignore data enabled - carrier policy indicates that data is not metered for ViLTE calls.
09-29 16:20:26.868782  1669  1669 D MtkTelephonyAssist: DataStateController: handleMessage phoneId = 0 evendId = 10
09-29 16:20:26.869253  1669  1669 D ImsPhoneCallTracker: [0] handleMessage what=23
09-29 16:20:26.869422  1669  1669 D ImsPhoneCallTracker: [0] handleMessage what=23
09-29 16:20:26.869487  1669  1669 D ImsPhoneCallTracker: [0] onDataEnabledChanged: enabled=true, reason=0
09-29 16:20:26.869536  1669  1669 D ImsPhoneCallTracker: [0] Ignore data enabled - carrier policy indicates that data is not metered for ViLTE calls.
09-29 16:20:26.869918  1669  1669 D MtkTelephonyAssist: DataStateController: handleMessage phoneId = 0 evendId = 10
09-29 16:20:26.870359  1669  1669 D ImsPhoneCallTracker: [0] handleMessage what=23
09-29 16:20:26.870524  1669  1669 D ImsPhoneCallTracker: [0] handleMessage what=23
09-29 16:20:26.870628  1669  1669 D ImsPhoneCallTracker: [0] onDataEnabledChanged: enabled=true, reason=0
09-29 16:20:26.870695  1669  1669 D ImsPhoneCallTracker: [0] Ignore data enabled - carrier policy indicates that data is not metered for ViLTE calls.
09-29 16:20:26.871079  1669  1669 D MtkTelephonyAssist: DataStateController: handleMessage phoneId = 0 evendId = 10
09-29 16:20:26.871981  1669  1669 D MtkTelephonyAssist: DataStateController: onReceive action = android.intent.action.ACTION_DEFAULT_DATA_SUBSCRIPTION_CHANGED
09-29 16:20:26.872274  1669  1669 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:26.874255  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:26.874726  1176  1198 I AT      : [0] AT> AT+EDALLOW=2,0 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:26.881805  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:26.882163  1176  1198 I AT      : [0] AT> AT+EDALLOW=2,0 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:26.890043  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:27.481507  1176  1182 D RtcEccNumberController: [0] [delaySetFwkReady] mIsFwkReady: 0, mIsPendingUpdate: 1
09-29 16:20:27.481799  1176  1182 I RtcEccNumberController: [0] [updateEmergencyNumber] mIsFwkReady: 1, mIsPendingUpdate: 1, ecc list: 112,911,000,08,110,118,119,999,111,113,117,125,122
09-29 16:20:27.486082  1669  1811 D RILJ    : [UNSL]< UNSOL_EMERGENCY_NUMBER_LIST [EmergencyNumber:Number-112|CountryIso-kr|Mnc-05|ServiceCategories-1|Urns-[]|Sources-1100|Routing-0, EmergencyNumber:Number-911|CountryIso-kr|Mnc-05|ServiceCategories-100|Urns-[]|Sources-1100|Routing-0, EmergencyNumber:Number-000|CountryIso-kr|Mnc-05|ServiceCategories-0|Urns-[]|Sources-1000|Routing-0, EmergencyNumber:Number-08|CountryIso-kr|Mnc-05|ServiceCategories-0|Urns-[]|Sources-1000|Routing-0, EmergencyNumber:Number-110|CountryIso-kr|Mnc-05|ServiceCategories-0|Urns-[]|Sources-1000|Routing-0, EmergencyNumber:Number-118|CountryIso-kr|Mnc-05|ServiceCategories-10011|Urns-[]|Sources-1100|Routing-0, EmergencyNumber:Number-119|CountryIso-kr|Mnc-05|ServiceCategories-100|Urns-[]|Sources-1100|Routing-0, EmergencyNumber:Number-999|CountryIso-kr|Mnc-05|ServiceCategories-0|Urns-[]|Sources-1000|Routing-0, EmergencyNumber:Number-111|CountryIso-kr|Mnc-05|ServiceCategories-110|Urns-[]|Sources-100|Routing-0, EmergencyNumber:Number-113|CountryIso-kr|Mnc-05|ServiceCategories-11|Urns-[]|Sources-100|Routing-0, EmergencyNumber:Number-117|CountryIso-kr|Mnc-05|ServiceCategories-10010|Urns-[]|Sources-100|Routing-0, EmergencyNumber:Number-125|CountryIso-kr|Mnc-05|ServiceCategories-1001|Urns-[]|Sources-100|Routing-0, EmergencyNumber:Number-122|CountryIso-kr|Mnc-05|ServiceCategories-1000|Urns-[]|Sources-100|Routing-0] [PHONE0]
09-29 16:20:27.487231  1669  1669 D EmergencyNumberTracker: updateRadioEmergencyNumberListAndNotify(): receiving [EmergencyNumber:Number-112|CountryIso-kr|Mnc-05|ServiceCategories-1|Urns-[]|Sources-1100|Routing-0, EmergencyNumber:Number-118|CountryIso-kr|Mnc-05|ServiceCategories-10011|Urns-[]|Sources-1100|Routing-0, EmergencyNumber:Number-119|CountryIso-kr|Mnc-05|ServiceCategories-100|Urns-[]|Sources-1100|Routing-0, EmergencyNumber:Number-911|CountryIso-kr|Mnc-05|ServiceCategories-100|Urns-[]|Sources-1100|Routing-0, EmergencyNumber:Number-000|CountryIso-kr|Mnc-05|ServiceCategories-0|Urns-[]|Sources-1000|Routing-0, EmergencyNumber:Number-08|CountryIso-kr|Mnc-05|ServiceCategories-0|Urns-[]|Sources-1000|Routing-0, EmergencyNumber:Number-110|CountryIso-kr|Mnc-05|ServiceCategories-0|Urns-[]|Sources-1000|Routing-0, EmergencyNumber:Number-999|CountryIso-kr|Mnc-05|ServiceCategories-0|Urns-[]|Sources-1000|Routing-0, EmergencyNumber:Number-111|CountryIso-kr|Mnc-05|ServiceCategories-110|Urns-[]|Sources-100|Routing-0, EmergencyNumber:Number-113|CountryIso-kr|Mnc-05|ServiceCategories-11|Urns-[]|Sources-100|Routing-0, EmergencyNumber:Number-117|CountryIso-kr|Mnc-05|ServiceCategories-10010|Urns-[]|Sources-100|Routing-0, EmergencyNumber:Number-122|CountryIso-kr|Mnc-05|ServiceCategories-1000|Urns-[]|Sources-100|Routing-0, EmergencyNumber:Number-125|CountryIso-kr|Mnc-05|ServiceCategories-1001|Urns-[]|Sources-100|Routing-0]
09-29 16:20:27.491478  1669  1669 D EmergencyNumberTracker: notifyEmergencyNumberList(): notified
09-29 16:20:27.600980  1669  1669 D ONSNetworkScanCtlr: init called
09-29 16:20:27.607423  1251  1781 D TelephonyRegistry: listen ooscl: hasNotifyOpptSubInfoChangedOccurred==false no callback
09-29 16:20:27.607985  1669  1669 D ONSProfileSelector: ONSProfileSelector init complete
09-29 16:20:27.613589  1669  1669 D ONS     : service is enable state true
09-29 16:20:27.616677  1669  1669 D ONS     : SIM state changed
09-29 16:20:27.786865  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=59, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 1000 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:27.787499  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=59, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 1000 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:27.864894  1669  1669 D SmsBroadcastUndelivered: Received broadcast android.intent.action.USER_UNLOCKED
09-29 16:20:27.866099  1669  1669 D SmsDispatchersController: Received broadcast android.intent.action.USER_UNLOCKED
09-29 16:20:27.888334  1669  1669 D MtkTelephonyAssist: MtkPhoneAssistBroadcastReceiver: MtkPhoneAssistBroadcastReceiver action = android.intent.action.LOCKED_BOOT_COMPLETED isSystemUser = true
09-29 16:20:27.890784  1872  1872 I ImsConfigEventReceiver[0]: ACTION_SIM_STATE_CHANGED, state:ABSENT, phoneId:0
09-29 16:20:27.890840  1872  1872 D ImsConfigEventReceiver[0]: ICC_ABSENT[0], reset carrier config loaded flag.
09-29 16:20:27.896027  1669  2219 D MtkSmsBroadcastUndelivered: scanning raw table for undelivered messages
09-29 16:20:27.897206  1669  1868 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:27.899046  1669  1868 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:27.954550  1669  2219 D MtkSmsBroadcastUndelivered: finished scanning raw table in 57 ms
09-29 16:20:27.954698  1669  2219 D MtkSmsBroadcastUndelivered: scanning raw table for undelivered messages
09-29 16:20:27.961854  1669  2219 D MtkSmsBroadcastUndelivered: finished scanning raw table in 7 ms
09-29 16:20:27.996299  1669  1669 D SAT     : [0]onSimAbsent, reset activation state to UNKNOWN
09-29 16:20:27.996436  1669  1669 D SAT     : [0]setVoiceActivationState=0
09-29 16:20:27.997126  1669  1669 D SAT     : [0]setDataActivationState=0
09-29 16:20:27.999046  1669  1669 D ONS     : SIM state changed
09-29 16:20:28.039042  1669  1669 D FeatureConnector: [MtkSuppServHelper, 0] imsFeatureCreated: FeatureContainer{imsFeature=android.os.BinderProxy@7803c3d, imsConfig=android.telephony.ims.aidl.IImsConfig$Stub$Proxy@8226c32, imsRegistration=android.telephony.ims.aidl.IImsRegistration$Stub$Proxy@44b7d83, sipTransport=null, state=READY, capabilities = capabilities={ EMERGENCY_OVER_MMTEL }}
09-29 16:20:28.039206  1669  1669 D FeatureConnector: [MtkSuppServHelper, 0] imsStatusChanged: status=READY
09-29 16:20:28.040703  1669  1844 D ImsManager [0]: Registration Callback registered.
09-29 16:20:28.040744  1669  1844 D MtkSuppServHelper: [0]ImsManager addRegistrationCallback
09-29 16:20:28.202469  1669  1686 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:28.204461  1669  1686 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:28.414426  1669  1669 D MTKCAT  : BootCompletedReceiver: [onReceive] action = android.intent.action.SIM_STATE_CHANGED
09-29 16:20:28.414517  1669  1669 D MTKCAT  : BootCompletedReceiver: ACTION_SIM_STATE_CHANGED, simStatus: ABSENT
09-29 16:20:28.829004  1669  1669 D TelephonyNetworkFactory[0]: onReleaseNetworkFor NetworkRequest [ REQUEST id=49, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 1001 RequestorUid: 1001 RequestorPkg: com.android.phone UnderlyingNetworks: Null] ] applied false
09-29 16:20:28.983098  1669  1686 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:29.028832  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=61, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10099 RequestorUid: 10099 RequestorPkg: com.android.vending UnderlyingNetworks: Null] ]
09-29 16:20:29.029427  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=61, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10099 RequestorUid: 10099 RequestorPkg: com.android.vending UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:29.181500  1669  1686 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:29.193884  2376  2376 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.android.vending listener=gzv@70cb0d
09-29 16:20:29.486690  1176  1182 D RtcGsmSmsCtrl: [0] delaySetSmsFwkReady(to true)(slot0)
09-29 16:20:29.486966  1176  1182 D RtcGsmSmsCtrl: [0] SMS framework is ready. Let's resume RFX_MSG_URC_SMS_READY_NOTIFICATION!
09-29 16:20:29.489084  1176  1182 D RtcGsmSmsCtrl: [0] Stop sms md ready timer
09-29 16:20:29.490766  1176  1182 D RtcGsmSmsCtrl: [0] SMS Md is ready. Let's resume RFX_MSG_REQUEST_GSM_SET_BROADCAST_SMS_CONFIG
09-29 16:20:29.491926  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 1
09-29 16:20:29.492000  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370
09-29 16:20:29.492062  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:29.495049  1669  1811 D RILJ    : Unsol response received; Sending ack to ril.cpp [PHONE0]
09-29 16:20:29.495521  1669  1669 D MtkSmsDispatchersController: SMS is ready, Phone: 0
09-29 16:20:29.495849  1669  1669 D SubscriptionManager: putPhoneIdAndSubIdExtra: no valid subs
09-29 16:20:29.580765  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:29.583808  1669  1811 D RILJ    : [0106]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:29.584428  1669  1846 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4370 to 4370
09-29 16:20:29.584759  1669  1846 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:29.584872  1669  1846 D MtkIccSmsInterfaceManager: Calling setCellBroadcastActivation(true)
09-29 16:20:29.595603  1669  1846 D RILJ    : [0141]> GSM_BROADCAST_ACTIVATION activate = true [PHONE0]
09-29 16:20:29.599014  1176  1196 D RmcGsmSmsRequest: [0] Turn GSM CB on
09-29 16:20:29.599166  1176  1196 I AT      : [0] AT> AT+ECSCBSW=1 (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:29.646503  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:29.650869  1176  1196 I AT      : [0] AT> AT+ETWS=5 (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:29.700970  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:29.702106  1669  1811 D RILJ    : [0141]< GSM_BROADCAST_ACTIVATION  [PHONE0]
09-29 16:20:29.703557  1669  1846 D MtkIccSmsInterfaceManager: mCurrentCellBroadcastActivation change to 1
09-29 16:20:29.704296  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:29.712206  1669  1846 D MtkIccSmsInterfaceManager: Calling setCdmaBroadcastConfig with 1 configurations
09-29 16:20:29.727287  1669  1846 D RILJ    : [0142]> CDMA_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:29.728192  1669  1846 D RILJ    : {.serviceCategory = 4096, .language = 1, .selected = true} [PHONE0]
09-29 16:20:29.731547  1176  1196 I AT      : [0] AT> AT+ECSCBCHA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:29.749013  1176  1195 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:29.750105  1669  1811 D RILJ    : [0142]< CDMA_SET_BROADCAST_CONFIG error 6 [PHONE0]
09-29 16:20:29.750471  1669  1811 D RilRequest: [0142]< CDMA_SET_BROADCAST_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result={ when=-38s570ms what=4 obj=com.android.internal.telephony.IccSmsInterfaceManager$Request@f99833d target=com.android.internal.telephony.IccSmsInterfaceManager$1 }
09-29 16:20:29.751091  1669  1846 D MtkIccSmsInterfaceManager: Failed to add cdma broadcast channels range 4096 to 4096
09-29 16:20:29.751903  1894  1927 D SmsManager: enableCellBroadcastRange: failed at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:29.760890  1669  1846 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 2 configurations
09-29 16:20:29.765232  1669  1846 D RILJ    : [0143]> GSM_SET_BROADCAST_CONFIG with 2 configs :  [PHONE0]
09-29 16:20:29.765379  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4370] Code [0,255] ENABLED [PHONE0]
09-29 16:20:29.765408  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4383] Code [0,255] ENABLED [PHONE0]
09-29 16:20:29.770457  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 2
09-29 16:20:29.770528  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370,4383
09-29 16:20:29.770584  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370,4383","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:29.822190  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:29.824055  1669  1811 D RILJ    : [0143]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:29.825050  1669  1846 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4383 to 4383
09-29 16:20:29.825532  1669  1846 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:29.825895  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:29.837754  1669  1846 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:29.840538  1669  1846 D RILJ    : [0144]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:29.840781  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4370] Code [0,255] ENABLED [PHONE0]
09-29 16:20:29.840862  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4383] Code [0,255] ENABLED [PHONE0]
09-29 16:20:29.840922  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4371,4372] Code [0,255] ENABLED [PHONE0]
09-29 16:20:29.844142  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:29.844225  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370,4383,4371-4372
09-29 16:20:29.844287  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370,4383,4371-4372","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:29.887543  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:29.891620  1669  1811 D RILJ    : [0144]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:29.892378  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=64, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10104 RequestorUid: 10104 RequestorPkg: com.google.android.googlequicksearchbox UnderlyingNetworks: Null] ]
09-29 16:20:29.893214  1669  1846 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4371 to 4372
09-29 16:20:29.893436  1669  1846 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:29.893903  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:29.894409  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=64, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10104 RequestorUid: 10104 RequestorPkg: com.google.android.googlequicksearchbox UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:29.895878  1669  1686 D MtkIccSmsInterfaceManager: Calling setCdmaBroadcastConfig with 1 configurations
09-29 16:20:29.899363  1669  1686 D RILJ    : [0145]> CDMA_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:29.899542  1669  1686 D RILJ    : {.serviceCategory = 4097, .language = 1, .selected = true} [PHONE0]
09-29 16:20:29.902762  1176  1196 I AT      : [0] AT> AT+ECSCBCHA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:29.910325  1176  1195 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:29.911785  1669  1811 D RILJ    : [0145]< CDMA_SET_BROADCAST_CONFIG error 6 [PHONE0]
09-29 16:20:29.912079  1669  1811 D RilRequest: [0145]< CDMA_SET_BROADCAST_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result={ when=-38s732ms what=4 obj=com.android.internal.telephony.IccSmsInterfaceManager$Request@95f9c83 target=com.android.internal.telephony.IccSmsInterfaceManager$1 }
09-29 16:20:29.915868  1669  1686 D MtkIccSmsInterfaceManager: Failed to add cdma broadcast channels range 4097 to 4097
09-29 16:20:29.916257  1894  1927 D SmsManager: enableCellBroadcastRange: failed at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:29.920170  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:29.929617  1669  1686 D RILJ    : [0146]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:29.929689  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4372] Code [0,255] ENABLED [PHONE0]
09-29 16:20:29.929726  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4383] Code [0,255] ENABLED [PHONE0]
09-29 16:20:29.929746  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4384,4385] Code [0,255] ENABLED [PHONE0]
09-29 16:20:29.931081  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:29.931133  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4372,4383,4384-4385
09-29 16:20:29.931217  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4372,4383,4384-4385","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:29.984310  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:29.986749  1669  1811 D RILJ    : [0146]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:29.987462  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4384 to 4385
09-29 16:20:29.987785  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:29.989303  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:29.999224  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:30.017970  1669  1686 D RILJ    : [0147]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:30.018291  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4372] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.018342  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4385] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.018360  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4373,4378] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.021434  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:30.021527  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4372,4383-4385,4373-4378
09-29 16:20:30.021588  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4372,4383-4385,4373-4378","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:30.040375  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=66, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10099 RequestorUid: 10099 RequestorPkg: com.android.vending UnderlyingNetworks: Null] ]
09-29 16:20:30.040851  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=66, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10099 RequestorUid: 10099 RequestorPkg: com.android.vending UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:30.077293  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:30.078434  1669  1811 D RILJ    : [0147]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:30.079157  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4373 to 4378
09-29 16:20:30.079413  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:30.079828  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.096586  1669  1686 D MtkIccSmsInterfaceManager: Calling setCdmaBroadcastConfig with 1 configurations
09-29 16:20:30.113476  1669  1686 D RILJ    : [0148]> CDMA_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:30.113540  1669  1686 D RILJ    : {.serviceCategory = 4098, .language = 1, .selected = true} [PHONE0]
09-29 16:20:30.119216  1176  1196 I AT      : [0] AT> AT+ECSCBCHA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:30.130310  1176  1195 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:30.132819  1669  1811 D RILJ    : [0148]< CDMA_SET_BROADCAST_CONFIG error 6 [PHONE0]
09-29 16:20:30.132969  1669  1811 D RilRequest: [0148]< CDMA_SET_BROADCAST_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result={ when=-38s953ms what=4 obj=com.android.internal.telephony.IccSmsInterfaceManager$Request@a85047e target=com.android.internal.telephony.IccSmsInterfaceManager$1 }
09-29 16:20:30.133475  1669  1686 D MtkIccSmsInterfaceManager: Failed to add cdma broadcast channels range 4098 to 4098
09-29 16:20:30.134799  1894  1927 D SmsManager: enableCellBroadcastRange: failed at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.136147  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:30.138916  1669  1686 D RILJ    : [0149]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:30.139010  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4378] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.139032  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4385] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.139050  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4386,4391] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.141424  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:30.141503  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4378,4383-4385,4386-4391
09-29 16:20:30.141565  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4378,4383-4385,4386-4391","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:30.212283  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:30.219161  1669  1811 D RILJ    : [0149]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:30.220005  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4386 to 4391
09-29 16:20:30.220264  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:30.220634  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.226076  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:30.258976  1669  1686 D RILJ    : [0150]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:30.259069  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4378] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.259091  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4391] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.259106  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4379,4379] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.264225  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:30.264299  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4378,4383-4391,4379
09-29 16:20:30.264359  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4378,4383-4391,4379","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:30.348007  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:30.349251  1669  1811 D RILJ    : [0150]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:30.350266  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4379 to 4379
09-29 16:20:30.350476  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:30.351161  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.353278  1669  1686 D MtkIccSmsInterfaceManager: Calling setCdmaBroadcastConfig with 1 configurations
09-29 16:20:30.363013  1669  1686 D RILJ    : [0151]> CDMA_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:30.363170  1669  1686 D RILJ    : {.serviceCategory = 4099, .language = 1, .selected = true} [PHONE0]
09-29 16:20:30.365874  1176  1196 I AT      : [0] AT> AT+ECSCBCHA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:30.373903  1176  1195 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:30.375157  1669  1811 D RILJ    : [0151]< CDMA_SET_BROADCAST_CONFIG error 6 [PHONE0]
09-29 16:20:30.375362  1669  1811 D RilRequest: [0151]< CDMA_SET_BROADCAST_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result={ when=-39s195ms what=4 obj=com.android.internal.telephony.IccSmsInterfaceManager$Request@9757ddf target=com.android.internal.telephony.IccSmsInterfaceManager$1 }
09-29 16:20:30.375983  1669  1686 D MtkIccSmsInterfaceManager: Failed to add cdma broadcast channels range 4099 to 4099
09-29 16:20:30.376488  1894  1927 D SmsManager: enableCellBroadcastRange: failed at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.381129  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:30.400997  1669  1686 D RILJ    : [0152]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:30.401082  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4379] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.401102  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4391] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.401118  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4392,4392] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.403024  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:30.403093  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4379,4383-4391,4392
09-29 16:20:30.403155  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4379,4383-4391,4392","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:30.458206  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:30.462167  1669  1811 D RILJ    : [0152]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:30.463320  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4392 to 4392
09-29 16:20:30.464392  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:30.464805  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.469350  1669  1686 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4380 to 4380
09-29 16:20:30.469924  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.472740  1669  1686 D MtkIccSmsInterfaceManager: Failed to remove cdma broadcast channels range 4100 to 4100
09-29 16:20:30.473232  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.476566  1669  1846 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4393 to 4393
09-29 16:20:30.481469  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.484726  1669  1846 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4381 to 4381
09-29 16:20:30.486713  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.504763  1669  1686 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4394 to 4394
09-29 16:20:30.514052  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.515931  1669  1846 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4382 to 4382
09-29 16:20:30.517088  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.522321  1176  1182 D RtcMwi  : [0] onHandleRequest: request id 60533 is RFX_MSG_REQUEST_NOTIFY_EPDG_SCREEN_STATE
09-29 16:20:30.522571  1669  1846 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4395 to 4395
09-29 16:20:30.522800  1176  1196 D RmcMwi  : [0] notifyEPDGScreenState: state:0
09-29 16:20:30.522898  1176  1196 I AT      : [0] AT> AT+ESCREENSTATE = 0 (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:30.523121  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.525053  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:30.527623  1669  1686 D RILJ    : [0153]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:30.527958  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4379] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.533410  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4392] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.533647  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4352,4354] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.539276  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:30.539736  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:30.539793  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4379,4383-4392,4352-4354
09-29 16:20:30.539856  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4379,4383-4392,4352-4354","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:30.539888  1176  1182 D RtcMwi  : [0] onHandleResponse, handle RFX_MSG_REQUEST_NOTIFY_EPDG_SCREEN_STATE
09-29 16:20:30.579647  1176  1184 I AT      : [0] AT< +ECSQ: 63,42,1,-229,-14,1,1,4,32767,1 (RIL_URC_READER, tid:493447834880)
09-29 16:20:30.580436  1176  1185 D RmcNwHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0X04]
09-29 16:20:30.580499  1176  1185 D RmcNwHdlr: [0] handleSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 27, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 63, wcdma_ecno: 42, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:20:30.603093  1669  1669 D MTKSST  : [GsmSST0] new:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-59 ber=99 rscp=-57 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}, old:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-55 ber=99 rscp=-53 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}
09-29 16:20:30.603940  1251  1667 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:30.604042  1251  1667 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:30.608863  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:30.610052  1669  1811 D RILJ    : [0153]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:30.615351  1251  1269 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:30.615450  1251  1269 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:30.617113  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4352 to 4354
09-29 16:20:30.617302  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:30.617673  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.619488  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 4 configurations
09-29 16:20:30.624394  1669  1686 D RILJ    : [0154]> GSM_SET_BROADCAST_CONFIG with 4 configs :  [PHONE0]
09-29 16:20:30.624477  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4352,4354] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.624521  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4379] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.624542  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4392] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.624562  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4356,4356] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.626269  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 4
09-29 16:20:30.626323  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4352-4354,4370-4379,4383-4392,4356
09-29 16:20:30.626385  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4352-4354,4370-4379,4383-4392,4356","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:30.688377  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:30.689734  1669  1811 D RILJ    : [0154]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:30.690399  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4356 to 4356
09-29 16:20:30.690679  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:30.692923  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.707040  1669  1686 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4355 to 4355
09-29 16:20:30.708163  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.758299  1669  1686 D MtkIccSmsInterfaceManager: Cell broadcast ranges reset.
09-29 16:20:30.763180  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 1 configurations
09-29 16:20:30.764895  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=68, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10103 RequestorUid: 10103 RequestorPkg: com.google.android.gms UnderlyingNetworks: Null] ]
09-29 16:20:30.765405  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=68, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10103 RequestorUid: 10103 RequestorPkg: com.google.android.gms UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:30.768279  1669  1686 D RILJ    : [0155]> GSM_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:30.768365  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4370] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.770416  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 1
09-29 16:20:30.770489  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370
09-29 16:20:30.770546  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:30.811387  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=70, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10113 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:30.812187  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=70, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10113 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:30.829096  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:30.830261  1669  1811 D RILJ    : [0155]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:30.830375  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4370 to 4370
09-29 16:20:30.830685  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:30.832255  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.834906  1669  1686 D MtkIccSmsInterfaceManager: Calling setCdmaBroadcastConfig with 1 configurations
09-29 16:20:30.845425  1669  1686 D RILJ    : [0156]> CDMA_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:30.845672  1669  1686 D RILJ    : {.serviceCategory = 4096, .language = 1, .selected = true} [PHONE0]
09-29 16:20:30.847433  1176  1196 I AT      : [0] AT> AT+ECSCBCHA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:30.855332  1176  1195 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:30.858153  1669  1811 D RILJ    : [0156]< CDMA_SET_BROADCAST_CONFIG error 6 [PHONE0]
09-29 16:20:30.858355  1669  1811 D RilRequest: [0156]< CDMA_SET_BROADCAST_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result={ when=-39s678ms what=4 obj=com.android.internal.telephony.IccSmsInterfaceManager$Request@568ea8a target=com.android.internal.telephony.IccSmsInterfaceManager$1 }
09-29 16:20:30.865059  1669  1686 D MtkIccSmsInterfaceManager: Failed to add cdma broadcast channels range 4096 to 4096
09-29 16:20:30.865526  1894  1927 D SmsManager: enableCellBroadcastRange: failed at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.875551  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 2 configurations
09-29 16:20:30.881272  1669  1686 D RILJ    : [0157]> GSM_SET_BROADCAST_CONFIG with 2 configs :  [PHONE0]
09-29 16:20:30.881510  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4370] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.881638  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4383] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.884892  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 2
09-29 16:20:30.884960  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370,4383
09-29 16:20:30.885017  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370,4383","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:30.927969  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:30.930079  1669  1811 D RILJ    : [0157]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:30.930400  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4383 to 4383
09-29 16:20:30.930618  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:30.930949  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.934564  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:30.937680  1669  1686 D RILJ    : [0158]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:30.937920  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4370] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.938055  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4383] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.938179  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4371,4372] Code [0,255] ENABLED [PHONE0]
09-29 16:20:30.940937  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:30.941022  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370,4383,4371-4372
09-29 16:20:30.941083  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370,4383,4371-4372","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:30.986290  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:30.987362  1669  1811 D RILJ    : [0158]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:30.987756  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4371 to 4372
09-29 16:20:30.987979  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:30.988355  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:30.992079  1669  1686 D MtkIccSmsInterfaceManager: Calling setCdmaBroadcastConfig with 1 configurations
09-29 16:20:30.995990  1669  1686 D RILJ    : [0159]> CDMA_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:30.996230  1669  1686 D RILJ    : {.serviceCategory = 4097, .language = 1, .selected = true} [PHONE0]
09-29 16:20:30.997772  1176  1196 I AT      : [0] AT> AT+ECSCBCHA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:31.005313  1176  1195 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:31.006551  1669  1811 D RILJ    : [0159]< CDMA_SET_BROADCAST_CONFIG error 6 [PHONE0]
09-29 16:20:31.006855  1669  1811 D RilRequest: [0159]< CDMA_SET_BROADCAST_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result={ when=-39s827ms what=4 obj=com.android.internal.telephony.IccSmsInterfaceManager$Request@5de18fb target=com.android.internal.telephony.IccSmsInterfaceManager$1 }
09-29 16:20:31.007218  1669  1686 D MtkIccSmsInterfaceManager: Failed to add cdma broadcast channels range 4097 to 4097
09-29 16:20:31.007704  1894  1927 D SmsManager: enableCellBroadcastRange: failed at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.009336  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:31.038146  1669  1686 D RILJ    : [0160]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:31.038281  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4372] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.038313  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4383] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.038349  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4384,4385] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.044919  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:31.044988  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4372,4383,4384-4385
09-29 16:20:31.045045  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4372,4383,4384-4385","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:31.127232  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:31.128380  1669  1811 D RILJ    : [0160]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:31.129001  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4384 to 4385
09-29 16:20:31.129222  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:31.129567  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.131139  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:31.144540  1669  1686 D RILJ    : [0161]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:31.144673  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4372] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.144723  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4385] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.144745  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4373,4378] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.149139  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:31.149217  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4372,4383-4385,4373-4378
09-29 16:20:31.149280  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4372,4383-4385,4373-4378","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:31.213507  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:31.214626  1669  1811 D RILJ    : [0161]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:31.216406  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4373 to 4378
09-29 16:20:31.216675  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:31.216977  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.223525  1669  1686 D MtkIccSmsInterfaceManager: Calling setCdmaBroadcastConfig with 1 configurations
09-29 16:20:31.226294  1669  1846 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:31.228007  1669  1686 D RILJ    : [0162]> CDMA_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:31.228265  1669  1686 D RILJ    : {.serviceCategory = 4098, .language = 1, .selected = true} [PHONE0]
09-29 16:20:31.230117  1176  1196 I AT      : [0] AT> AT+ECSCBCHA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:31.237758  1176  1195 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:31.238844  1669  1811 D RILJ    : [0162]< CDMA_SET_BROADCAST_CONFIG error 6 [PHONE0]
09-29 16:20:31.239117  1669  1811 D RilRequest: [0162]< CDMA_SET_BROADCAST_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result={ when=-40s59ms what=4 obj=com.android.internal.telephony.IccSmsInterfaceManager$Request@84f4d18 target=com.android.internal.telephony.IccSmsInterfaceManager$1 }
09-29 16:20:31.239803  1669  1686 D MtkIccSmsInterfaceManager: Failed to add cdma broadcast channels range 4098 to 4098
09-29 16:20:31.240266  1894  1927 D SmsManager: enableCellBroadcastRange: failed at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.242029  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:31.247084  1669  1686 D RILJ    : [0163]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:31.247189  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4378] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.247214  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4385] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.247254  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4386,4391] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.248764  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:31.248855  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4378,4383-4385,4386-4391
09-29 16:20:31.248918  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4378,4383-4385,4386-4391","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:31.293984  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:31.295130  1669  1811 D RILJ    : [0163]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:31.295797  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4386 to 4391
09-29 16:20:31.296056  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:31.296557  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.298409  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:31.303601  1669  1686 D RILJ    : [0164]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:31.303865  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4378] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.303919  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4391] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.303940  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4379,4379] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.306080  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:31.306166  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4378,4383-4391,4379
09-29 16:20:31.306228  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4378,4383-4391,4379","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:31.349573  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:31.350631  1669  1811 D RILJ    : [0164]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:31.351483  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4379 to 4379
09-29 16:20:31.351867  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:31.352256  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.353501  1669  1686 D MtkIccSmsInterfaceManager: Calling setCdmaBroadcastConfig with 1 configurations
09-29 16:20:31.356153  1669  1686 D RILJ    : [0165]> CDMA_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:31.356300  1669  1686 D RILJ    : {.serviceCategory = 4099, .language = 1, .selected = true} [PHONE0]
09-29 16:20:31.357868  1176  1196 I AT      : [0] AT> AT+ECSCBCHA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:31.367082  1176  1195 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:31.368281  1669  1811 D RILJ    : [0165]< CDMA_SET_BROADCAST_CONFIG error 6 [PHONE0]
09-29 16:20:31.368738  1669  1811 D RilRequest: [0165]< CDMA_SET_BROADCAST_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result={ when=-40s188ms what=4 obj=com.android.internal.telephony.IccSmsInterfaceManager$Request@bd15371 target=com.android.internal.telephony.IccSmsInterfaceManager$1 }
09-29 16:20:31.369682  1669  1686 D MtkIccSmsInterfaceManager: Failed to add cdma broadcast channels range 4099 to 4099
09-29 16:20:31.370152  1894  1927 D SmsManager: enableCellBroadcastRange: failed at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.372103  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:31.374739  1669  1686 D RILJ    : [0166]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:31.374976  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4379] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.375061  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4391] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.375129  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4392,4392] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.376980  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:31.377039  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4379,4383-4391,4392
09-29 16:20:31.377097  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4379,4383-4391,4392","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:31.428218  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:31.429437  1669  1811 D RILJ    : [0166]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:31.430301  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4392 to 4392
09-29 16:20:31.430578  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:31.430951  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.433351  1669  1686 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4380 to 4380
09-29 16:20:31.433885  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.437035  1669  1846 D MtkIccSmsInterfaceManager: Failed to remove cdma broadcast channels range 4100 to 4100
09-29 16:20:31.437534  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.439308  1669  1846 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4393 to 4393
09-29 16:20:31.439806  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.441496  1669  1846 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4381 to 4381
09-29 16:20:31.442108  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.465707  1669  1846 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4394 to 4394
09-29 16:20:31.466351  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.469697  1669  1686 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4382 to 4382
09-29 16:20:31.470228  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.471531  1669  1686 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4395 to 4395
09-29 16:20:31.472169  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.473888  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:31.476970  1669  1686 D RILJ    : [0167]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:31.477977  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4379] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.478142  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4392] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.478209  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4352,4354] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.481232  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:31.481327  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4379,4383-4392,4352-4354
09-29 16:20:31.481392  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4379,4383-4392,4352-4354","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:31.550002  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:31.551884  1669  1811 D RILJ    : [0167]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:31.552744  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4352 to 4354
09-29 16:20:31.552995  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:31.553350  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.555011  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 4 configurations
09-29 16:20:31.563416  1669  1686 D RILJ    : [0168]> GSM_SET_BROADCAST_CONFIG with 4 configs :  [PHONE0]
09-29 16:20:31.563497  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4352,4354] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.563518  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4379] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.563533  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4392] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.563567  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4356,4356] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.565155  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 4
09-29 16:20:31.565229  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4352-4354,4370-4379,4383-4392,4356
09-29 16:20:31.565291  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4352-4354,4370-4379,4383-4392,4356","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:31.622510  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:31.623596  1669  1811 D RILJ    : [0168]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:31.623936  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4356 to 4356
09-29 16:20:31.624150  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:31.624513  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.644163  1669  1686 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4355 to 4355
09-29 16:20:31.644846  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.705864  1669  1686 D MtkIccSmsInterfaceManager: Cell broadcast ranges reset.
09-29 16:20:31.709952  1669  1846 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 1 configurations
09-29 16:20:31.712549  1669  1846 D RILJ    : [0169]> GSM_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:31.712631  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4370] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.716332  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 1
09-29 16:20:31.716396  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370
09-29 16:20:31.716486  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:31.801747  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:31.803008  1669  1811 D RILJ    : [0169]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:31.826833  1669  1846 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4370 to 4370
09-29 16:20:31.827049  1669  1846 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:31.827766  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.829644  1669  1846 D MtkIccSmsInterfaceManager: Calling setCdmaBroadcastConfig with 1 configurations
09-29 16:20:31.832992  1669  1846 D RILJ    : [0170]> CDMA_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:31.833102  1669  1846 D RILJ    : {.serviceCategory = 4096, .language = 1, .selected = true} [PHONE0]
09-29 16:20:31.835844  1176  1196 I AT      : [0] AT> AT+ECSCBCHA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:31.846295  1176  1195 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:31.848897  1669  1811 D RILJ    : [0170]< CDMA_SET_BROADCAST_CONFIG error 6 [PHONE0]
09-29 16:20:31.849142  1669  1811 D RilRequest: [0170]< CDMA_SET_BROADCAST_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result={ when=-40s669ms what=4 obj=com.android.internal.telephony.IccSmsInterfaceManager$Request@9f32556 target=com.android.internal.telephony.IccSmsInterfaceManager$1 }
09-29 16:20:31.850062  1669  1846 D MtkIccSmsInterfaceManager: Failed to add cdma broadcast channels range 4096 to 4096
09-29 16:20:31.850519  1894  1927 D SmsManager: enableCellBroadcastRange: failed at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.851939  1669  1846 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 2 configurations
09-29 16:20:31.854844  1669  1846 D RILJ    : [0171]> GSM_SET_BROADCAST_CONFIG with 2 configs :  [PHONE0]
09-29 16:20:31.855113  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4370] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.855246  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4383] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.858009  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 2
09-29 16:20:31.858097  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370,4383
09-29 16:20:31.858164  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370,4383","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:31.914103  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:31.915771  1669  1811 D RILJ    : [0171]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:31.916887  1669  1846 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4383 to 4383
09-29 16:20:31.917154  1669  1846 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:31.917474  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.925666  1669  1846 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:31.928552  1669  1846 D RILJ    : [0172]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:31.932660  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4370] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.932845  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4383] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.932934  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4371,4372] Code [0,255] ENABLED [PHONE0]
09-29 16:20:31.934715  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:31.934786  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370,4383,4371-4372
09-29 16:20:31.934850  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370,4383,4371-4372","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:31.985288  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:31.988690  1669  1811 D RILJ    : [0172]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:31.990255  1669  1846 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4371 to 4372
09-29 16:20:31.990534  1669  1846 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:31.990938  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:31.998359  1669  1846 D MtkIccSmsInterfaceManager: Calling setCdmaBroadcastConfig with 1 configurations
09-29 16:20:32.001955  1669  1846 D RILJ    : [0173]> CDMA_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:32.002222  1669  1846 D RILJ    : {.serviceCategory = 4097, .language = 1, .selected = true} [PHONE0]
09-29 16:20:32.004308  1176  1196 I AT      : [0] AT> AT+ECSCBCHA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:32.015314  1176  1195 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:32.018820  1669  1811 D RILJ    : [0173]< CDMA_SET_BROADCAST_CONFIG error 6 [PHONE0]
09-29 16:20:32.019100  1669  1811 D RilRequest: [0173]< CDMA_SET_BROADCAST_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result={ when=-40s839ms what=4 obj=com.android.internal.telephony.IccSmsInterfaceManager$Request@86b49d7 target=com.android.internal.telephony.IccSmsInterfaceManager$1 }
09-29 16:20:32.020423  1669  1846 D MtkIccSmsInterfaceManager: Failed to add cdma broadcast channels range 4097 to 4097
09-29 16:20:32.020980  1894  1927 D SmsManager: enableCellBroadcastRange: failed at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.024923  1669  1846 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:32.030960  1669  1846 D RILJ    : [0174]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:32.031252  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4372] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.031392  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4383] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.031473  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4384,4385] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.033044  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:32.033110  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4372,4383,4384-4385
09-29 16:20:32.033169  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4372,4383,4384-4385","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:32.210252  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:32.211359  1669  1811 D RILJ    : [0174]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:32.211969  1669  1846 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4384 to 4385
09-29 16:20:32.212187  1669  1846 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:32.217423  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.219094  1669  1846 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:32.222087  1669  1846 D RILJ    : [0175]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:32.222309  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4372] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.222390  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4385] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.222441  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4373,4378] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.228346  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:32.228402  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4372,4383-4385,4373-4378
09-29 16:20:32.228461  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4372,4383-4385,4373-4378","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:32.259628  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=72, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10104 RequestorUid: 10104 RequestorPkg: com.google.android.googlequicksearchbox UnderlyingNetworks: Null] ]
09-29 16:20:32.260208  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=72, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10104 RequestorUid: 10104 RequestorPkg: com.google.android.googlequicksearchbox UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:32.281803  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:32.282964  1669  1811 D RILJ    : [0175]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:32.286769  1669  1846 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4373 to 4378
09-29 16:20:32.286989  1669  1846 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:32.288014  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.294315  1669  1846 D MtkIccSmsInterfaceManager: Calling setCdmaBroadcastConfig with 1 configurations
09-29 16:20:32.301455  1669  1846 D RILJ    : [0176]> CDMA_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:32.301653  1669  1846 D RILJ    : {.serviceCategory = 4098, .language = 1, .selected = true} [PHONE0]
09-29 16:20:32.304920  1176  1196 I AT      : [0] AT> AT+ECSCBCHA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:32.313970  1176  1195 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:32.315346  1669  1811 D RILJ    : [0176]< CDMA_SET_BROADCAST_CONFIG error 6 [PHONE0]
09-29 16:20:32.315596  1669  1811 D RilRequest: [0176]< CDMA_SET_BROADCAST_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result={ when=-41s135ms what=4 obj=com.android.internal.telephony.IccSmsInterfaceManager$Request@a56b5ad target=com.android.internal.telephony.IccSmsInterfaceManager$1 }
09-29 16:20:32.316093  1669  1846 D MtkIccSmsInterfaceManager: Failed to add cdma broadcast channels range 4098 to 4098
09-29 16:20:32.316602  1894  1927 D SmsManager: enableCellBroadcastRange: failed at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.318245  1669  1846 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:32.320986  1669  1846 D RILJ    : [0177]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:32.321282  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4378] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.321497  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4385] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.321615  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4386,4391] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.323739  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:32.323822  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4378,4383-4385,4386-4391
09-29 16:20:32.323882  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4378,4383-4385,4386-4391","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:32.386391  1669  1686 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:32.416089  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:32.427259  1669  1811 D RILJ    : [0177]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:32.427490  1669  1846 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4386 to 4391
09-29 16:20:32.427767  1669  1846 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:32.428184  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.429772  1669  1846 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:32.433334  1669  1846 D RILJ    : [0178]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:32.433404  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4378] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.433443  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4391] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.433463  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4379,4379] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.434868  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:32.434930  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4378,4383-4391,4379
09-29 16:20:32.434985  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4378,4383-4391,4379","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:32.496428  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:32.497679  1669  1811 D RILJ    : [0178]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:32.499103  1669  1846 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4379 to 4379
09-29 16:20:32.499480  1669  1846 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:32.499850  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.501252  1669  1846 D MtkIccSmsInterfaceManager: Calling setCdmaBroadcastConfig with 1 configurations
09-29 16:20:32.505742  1669  1846 D RILJ    : [0179]> CDMA_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:32.505872  1669  1846 D RILJ    : {.serviceCategory = 4099, .language = 1, .selected = true} [PHONE0]
09-29 16:20:32.507264  1176  1196 I AT      : [0] AT> AT+ECSCBCHA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:32.515930  1176  1195 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:32.517148  1669  1811 D RILJ    : [0179]< CDMA_SET_BROADCAST_CONFIG error 6 [PHONE0]
09-29 16:20:32.517363  1669  1811 D RilRequest: [0179]< CDMA_SET_BROADCAST_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result={ when=-41s337ms what=4 obj=com.android.internal.telephony.IccSmsInterfaceManager$Request@31440e2 target=com.android.internal.telephony.IccSmsInterfaceManager$1 }
09-29 16:20:32.517779  1669  1846 D MtkIccSmsInterfaceManager: Failed to add cdma broadcast channels range 4099 to 4099
09-29 16:20:32.518250  1894  1927 D SmsManager: enableCellBroadcastRange: failed at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.520736  1669  1846 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:32.523257  1669  1846 D RILJ    : [0180]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:32.523795  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4379] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.523992  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4391] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.524096  1669  1846 D RILJ    : SmsBroadcastConfigInfo: Id [4392,4392] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.525988  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:32.526040  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4379,4383-4391,4392
09-29 16:20:32.526093  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4379,4383-4391,4392","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:32.528615  1669  1686 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:32.534277  1669  1686 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:32.541265  1669  1686 E PhoneSubInfoController: getGroupIdLevel1 phone is null for Subscription:-1
09-29 16:20:32.546249  1669  1686 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:32.570889  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:32.576137  1669  1811 D RILJ    : [0180]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:32.576729  1669  1846 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4392 to 4392
09-29 16:20:32.577048  1669  1846 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:32.577425  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.579036  1669  1846 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4380 to 4380
09-29 16:20:32.579585  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.583045  1669  1846 D MtkIccSmsInterfaceManager: Failed to remove cdma broadcast channels range 4100 to 4100
09-29 16:20:32.584004  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.586448  1669  1686 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4393 to 4393
09-29 16:20:32.586863  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.588385  1669  1846 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4381 to 4381
09-29 16:20:32.588790  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.589992  1669  1868 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4394 to 4394
09-29 16:20:32.590596  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.592095  1669  1868 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4382 to 4382
09-29 16:20:32.592659  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.594049  1669  1868 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4395 to 4395
09-29 16:20:32.594652  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.596118  1669  1868 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:32.598718  1669  1868 D RILJ    : [0181]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:32.598972  1669  1868 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4379] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.599065  1669  1868 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4392] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.599140  1669  1868 D RILJ    : SmsBroadcastConfigInfo: Id [4352,4354] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.602101  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:32.602158  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4379,4383-4392,4352-4354
09-29 16:20:32.602213  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4379,4383-4392,4352-4354","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:32.657859  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:32.659065  1669  1811 D RILJ    : [0181]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:32.660296  1669  1868 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4352 to 4354
09-29 16:20:32.660541  1669  1868 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:32.663620  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.666753  1669  1868 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 4 configurations
09-29 16:20:32.673095  1669  1868 D RILJ    : [0182]> GSM_SET_BROADCAST_CONFIG with 4 configs :  [PHONE0]
09-29 16:20:32.673342  1669  1868 D RILJ    : SmsBroadcastConfigInfo: Id [4352,4354] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.673463  1669  1868 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4379] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.673525  1669  1868 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4392] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.673577  1669  1868 D RILJ    : SmsBroadcastConfigInfo: Id [4356,4356] Code [0,255] ENABLED [PHONE0]
09-29 16:20:32.675260  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 4
09-29 16:20:32.675349  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4352-4354,4370-4379,4383-4392,4356
09-29 16:20:32.675407  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4352-4354,4370-4379,4383-4392,4356","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:32.765842  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:32.768742  1669  1811 D RILJ    : [0182]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:32.769730  1669  1868 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4356 to 4356
09-29 16:20:32.769980  1669  1868 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:32.770282  1894  1927 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.783276  1669  1868 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4355 to 4355
09-29 16:20:32.783970  1894  1927 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:32.811332  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=77, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10117 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:32.811929  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=77, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10117 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:33.004800  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=79, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10102 RequestorUid: 10102 RequestorPkg: com.google.android.dialer UnderlyingNetworks: Null] ]
09-29 16:20:33.005195  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=79, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10102 RequestorUid: 10102 RequestorPkg: com.google.android.dialer UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:33.637820  1669  1846 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:33.828993  1669  1686 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:34.163363  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=81, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10101 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:34.163817  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=81, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10101 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:34.270527  1669  1686 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:34.329818  1251  1251 D MtkImsManager [0]: mMtkImsService = com.mediatek.ims.internal.IMtkImsService$Stub$Proxy@edbf8e3
09-29 16:20:34.333184  1251  1270 D FeatureConnector: [LPPeService, 0] imsFeatureCreated: FeatureContainer{imsFeature=android.os.BinderProxy@2cb403f, imsConfig=android.telephony.ims.aidl.IImsConfig$Stub$Proxy@dd7bd0c, imsRegistration=android.telephony.ims.aidl.IImsRegistration$Stub$Proxy@3bd5655, sipTransport=null, state=READY, capabilities = capabilities={ EMERGENCY_OVER_MMTEL }}
09-29 16:20:34.333516  1251  1270 D FeatureConnector: [LPPeService, 0] imsStatusChanged: status=READY
09-29 16:20:34.407842  1251  1251 D ImsManager [0]: Registration Callback registered.
09-29 16:20:34.546478  1669  1686 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:34.721150  1669  1669 D SubscriptionInfoUpdater: No subscription is active for phone being updated
09-29 16:20:34.726020  1669  1669 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:34.726452  1669  1669 D CarrierSignalAgent: [0]CarrierSignalAgent receiver action: android.telephony.action.CARRIER_CONFIG_CHANGED
09-29 16:20:34.748655  1669  1669 D CarrierSignalAgent: [0]Loading carrier config: carrier_app_wake_signal_config
09-29 16:20:34.749583  1669  1669 D CarrierSignalAgent: [0]Loading carrier config: carrier_app_no_wake_signal_config
09-29 16:20:34.752924  1872  1872 D SuppServExt: [0]ACTION_CARRIER_CONFIG_CHANGED: not loaded, subId: -1
09-29 16:20:34.753683  1669  1669 D NRM-C-0 : Carrier config changed. Try to bind network service.
09-29 16:20:34.753836  1669  1669 D NRM-I-0 : Carrier config changed. Try to bind network service.
09-29 16:20:34.756502  1669  1669 I CSST    : reading time to delay notification pref network: -1
09-29 16:20:34.756592  1669  1669 I CSST    : reading time to delay notification emergency: -1
09-29 16:20:34.758537  1669  1669 I CSST    : isNrSupported:  carrierConfigEnabled: true, AccessFamilySupported: false, isNrNetworkTypeAllowed: false
09-29 16:20:34.758775  1669  1669 I CSST    : PrefNetworkNotification: sendMessage() w/values: ,false,-1,false,true
09-29 16:20:34.759441  1669  1669 I CSST    : canceling notifications: 1000
09-29 16:20:34.760480  1669  1669 D CSST    : isPhoneRegisteredForWifiCalling: false
09-29 16:20:34.760985  1669  1669 I CSST    : EmergencyNetworkNotification: sendMessage() w/values: ,-1,false,true
09-29 16:20:34.762286  1669  1669 I CSST    : canceling notifications: 1001
09-29 16:20:34.765003  1669  1669 D DSM-C-0 : Carrier config changed. Try to bind data service.
09-29 16:20:34.797843  1669  1669 D SubscriptionController: [setDefaultVoiceSubId] default phone account not changed
09-29 16:20:34.814826  1872  1872 D MtkImsManagerIM [-1]: isImsResourceSupport, feature:2
09-29 16:20:34.815060  1872  1872 E MtkImsManagerIM [-1]: Invalid main phone -1, return true as don't care
09-29 16:20:34.815133  1872  1872 D SubscriptionManager: [getSubId]- fail
09-29 16:20:34.828617  1872  1872 D SubscriptionManager: [getSubId]- fail
09-29 16:20:34.833616  1872  1872 D SubscriptionManager: [getSubId]- fail
09-29 16:20:34.838444  1872  1872 D MtkImsManagerIM [-1]: getAirplaneModeFromSettings: false
09-29 16:20:34.839503  1872  1872 D MtkImsManagerIM [-1]: Wfc, isResourceSupport:true, isCarrierConfigSupport:true, isGbaValidSupport:true, isFeatureEnableByPlatformExt:true, wfcSupportAirplaneMode:true, isAirplaneModeON:false
09-29 16:20:34.840830  1669  1669 D RetryManager: [ims] mBroadcastReceiver: action android.telephony.action.CARRIER_CONFIG_CHANGED, mSameApnRetryCount:0, networkSuggestedDelay:-1, mCurrentApnIndex:-1
09-29 16:20:34.841874  1669  1669 D RetryManager: [default] mBroadcastReceiver: action android.telephony.action.CARRIER_CONFIG_CHANGED, mSameApnRetryCount:0, networkSuggestedDelay:-1, mCurrentApnIndex:-1
09-29 16:20:34.842267  1669  1669 D DSM-I-0 : Carrier config changed. Try to bind data service.
09-29 16:20:34.846236  1669  1669 D RILJ    : [0183]> VOICE_RADIO_TECH [PHONE0]
09-29 16:20:34.850855  1669  1811 D RILJ    : [0183]< VOICE_RADIO_TECH {1} [PHONE0]
09-29 16:20:34.859042  1669  1669 D RILJ    : [0184]> GET_RADIO_CAPABILITY [PHONE0]
09-29 16:20:34.860125  1669  1669 D RetryManager: [ims] mBroadcastReceiver: action android.telephony.action.CARRIER_CONFIG_CHANGED, mSameApnRetryCount:0, networkSuggestedDelay:-1, mCurrentApnIndex:-1
09-29 16:20:34.860353  1669  1669 D RetryManager: [default] mBroadcastReceiver: action android.telephony.action.CARRIER_CONFIG_CHANGED, mSameApnRetryCount:0, networkSuggestedDelay:-1, mCurrentApnIndex:-1
09-29 16:20:34.860488  1669  1669 D SuppServConf: [0]mBroadcastReceiver: action android.telephony.action.CARRIER_CONFIG_CHANGED
09-29 16:20:34.860716  1669  1669 I SuppServConf: [0]Receive ACTION_CARRIER_CONFIG_CHANGED: subId=-1, mPhone.getSubId()=-1
09-29 16:20:34.860980  1669  1669 I SuppServConf: [0]CarrierConfigLoader is loading complete!
09-29 16:20:34.861523  1669  1844 D SuppServConf: [0]handleMessage msg: EVENT_CARRIER_CONFIG_LOADED
09-29 16:20:34.861616  1669  1844 I SuppServConf: [0]resetConfig start.
09-29 16:20:34.861647  1669  1844 I SuppServConf: [0]resetConfig end.
09-29 16:20:34.861840  1669  1669 E ImsPhoneCallTracker: [0] cacheCarrierConfiguration: No carrier config service found or not active subId = -1
09-29 16:20:34.863596  1669  1669 D ImsPhoneCallTracker: [0] isTestSim: false
09-29 16:20:34.863880  1669  1669 D ImsPhoneCallTracker: [0] onReceive : Updating mAllowEmergencyVideoCalls = false
09-29 16:20:34.863963  1669  1811 D RILJ    : convertHalRadioCapability: session=-1, phase=3, rat=36869, logicModemUuid=modem_sys1_ps0, status=1, rcRil.raf=81930 [PHONE0]
09-29 16:20:34.866467  1669  1844 I SuppServConf: [0]loadFromCarrierConfig start.
09-29 16:20:34.866748  1669  1844 I SuppServConf: [0]loadFromCarrierConfig end.
09-29 16:20:34.866812  1669  1844 I SuppServConf: [0]NEED_CHECK_DATA_ROAMING -> bValue: false, sValue: , iValue: -1
09-29 16:20:34.866832  1669  1844 I SuppServConf: [0]TBCLIR -> bValue: false, sValue: , iValue: -1
09-29 16:20:34.866850  1669  1844 I SuppServConf: [0]RE_REGISTER_FOR_CF -> bValue: false, sValue: , iValue: -1
09-29 16:20:34.866868  1669  1844 I SuppServConf: [0]SUPPORT_SAVE_CF_NUMBER -> bValue: false, sValue: , iValue: -1
09-29 16:20:34.866911  1669  1844 I SuppServConf: [0]TRANSFER_XCAP_404 -> bValue: false, sValue: , iValue: -1
09-29 16:20:34.866930  1669  1844 I SuppServConf: [0]NEED_CHECK_IMS_WHEN_ROAMING -> bValue: false, sValue: , iValue: -1
09-29 16:20:34.866949  1669  1844 I SuppServConf: [0]NOT_SUPPORT_XCAP -> bValue: false, sValue: , iValue: -1
09-29 16:20:34.866966  1669  1844 I SuppServConf: [0]NOT_SUPPORT_OCB -> bValue: false, sValue: , iValue: -1
09-29 16:20:34.866983  1669  1844 I SuppServConf: [0]GSM_UT_SUPPORT -> bValue: false, sValue: , iValue: -1
09-29 16:20:34.867000  1669  1844 I SuppServConf: [0]ENABLE_XCAP_HTTP_RESPONSE_409 -> bValue: false, sValue: , iValue: -1
09-29 16:20:34.867032  1669  1844 I SuppServConf: [0]QUERY_CFU_AGAIN_AFTER_SET -> bValue: false, sValue: , iValue: -1
09-29 16:20:34.867050  1669  1844 I SuppServConf: [0]NOT_SUPPORT_CALL_IDENTITY -> bValue: false, sValue: , iValue: -1
09-29 16:20:34.867067  1669  1844 I SuppServConf: [0]NEED_CHECK_DATA_ENABLE -> bValue: false, sValue: , iValue: -1
09-29 16:20:34.867084  1669  1844 I SuppServConf: [0]IMS_NW_CW -> bValue: false, sValue: , iValue: -1
09-29 16:20:34.867100  1669  1844 I SuppServConf: [0]NOT_SUPPORT_WFC_UT -> bValue: false, sValue: , iValue: -1
09-29 16:20:34.868123  1669  1811 D RILJ    : [0184]< GET_RADIO_CAPABILITY {mPhoneId = 0 mVersion=1 mSession=-1 mPhase=3 mRadioAccessFamily=36869 mLogicModemId=modem_sys1_ps0 mStatus=1} [PHONE0]
09-29 16:20:34.884294  1669  1669 D NRM-C-0 : Service com.android.phone already bound or being bound.
09-29 16:20:34.895901  1669  1669 D NRM-I-0 : Service com.android.phone already bound or being bound.
09-29 16:20:34.900667  1669  1669 D MTKSST  : [GsmSST0] CarrierConfigChange PersistableBundle[{mtk_show_clir_setting_bool=true, mtk_default_enhanced_4g_mode_bool=true, carrier_volte_provisioned_bool=false, support_cdma_1x_voice_calls_bool=true, support_ss_over_cdma_bool=false, disable_charge_indication_bool=false, support_tdscdma_bool=false, httpSocketTimeout=60000, mtk_resume_hold_call_after_active_call_end_by_remote=false, allowed_initial_attach_apn_types_string_array=[ia, default, mms, dun], disable_supplementary_services_in_airplane_mode_bool=false, call_barring_default_service_class_int=1, call_redirection_service_component_name_string=null, carrier_wfc_supports_wifi_only_bool=false, carrier_default_actions_on_default_network_available_string_array=[false: 7, true: 8], mtk_ct_volte_status_bool=false, mtk_carrier_ss_need_check_data_roaming=false, operator_selection_expand_bool=true, disable_cdma_activation_code_bool=false, simplified_network_settings_bool=false, call_forwarding_when_unanswered_supported_bool=true, support_tdscdma_roaming_networks_string_array=null, gps.lpp_profile=2, call_barring_visibility_bool=true, gba_mode_int=1, gps.es_extension_sec=0, enable_apps_string_array=null, 5g_icon_display_secondary_grace_period_string=, carrier_default_wfc_ims_roaming_enabled_bool=false, mtk_show_call_barring_password_bool=false, cdma_nonroaming_networks_string_array=null, signal_strength_nr_nsa_use_lte_as_primary_bool=true, aliasMinChars=2, mtk_key_multiline_allow_cross_line_conference_bool=false, fdn_number_length_limit_int=20, support_ims_call_forwarding_while_roaming_bool=true, mtk_carrier_wfc_location_response_timeout=55000, wfc_data_spn_format_idx_int=0, hide_sim_lock_settings_bool=false, drop_video_call_when_answering_audio_call_bool=false, mtk_rtt_auto_accept_request_bool=false, mtk_show_open_mobile_data_dialog_bool=false, ci_action_on_sys_update_bool=false, carrier_certificate_string_array=[], convert_cdma_caller_id_mmi_codes_while_roaming_on_3gpp_bool=false, mtk_ignore_clir_when_ecc=true, support_enhanced_call_blocking_bool=true, iwlan.ike_rekey_hard_timer_in_sec=14400, vvm_port_number_int=0, carrier_default_wfc_ims_enabled_bool=false, iwlan.ike_session_encryption_aes_ctr_key_size_int_array=[128, 192, 256], dial_string_replace_string_array=null, opportunistic_network_entry_threshold_bandwidth_int=1024, opportunistic_network_data_switch_exit_hysteresis_time_long=3000, gsm_nonroaming_networks_string_array=null, imsserviceentitlement.ims_provisioning_bool=false, wifi.avoid_5ghz_softap_for_laa_bool=false, hide_ims_apn_bool=false, mtk_carrier_wfc_get_location_always=false, show_toast_when_conference_full=true, vvm_destination_number_string=, unmetered_nr_sa_mmwave_bool=false, dtmf_type_enabled_bool=false, allow_video_calling_fallback_bool=true, mtk_carrier_ims_ecbm_supported=false, mtk_domestic_roaming_enabled_only_by_mobile_data_setting=false, config_ims_package_override_string=null, only_auto_select_in_home_network=false, iwlan.supported_prf_algorithms_int_array=[2, 4, 5, 6, 7], mtk_support_enhanced_call_blocking_bool=false, show_data_connected_roaming_notification=false, support_auto_decline_upgrade_request_bool=true, gps.es_supl_data_plane_only_roaming_plmn_string_array=null, mtk_video_call_background_transmission=false, imsserviceentitlement.fcm_sender_id_string=, smsToMmsTextThreshold=-1, inflate_signal_strength_bool=false, force_home_network_bool=false, spdi_override_string_array=null, show_wfc_location_privacy_policy_bool=false, gps.supl_es=1, enableSMSDeliveryReports=true, iwlan.natt_keep_alive_timer_sec_int=20, missed_incoming_call_sms_originator_string_array=[], missed_incoming_call_sms_pattern_string_array=[], auto_retry_enabled_bool=false, ims.enable_presence_capability_exchange_bool=false, opportunistic_network_entry_threshold_rssnr_int=45, play_call_recording_tone_bool=false, unmetered_nr_nsa_sub6_bool=false, carrier_force_disable_etws_cmas_test_bool=false, call_waiting_service_class_int=1, allow_emergency_video_calls_bool=false, support_add_conference_participants_bool=false, csp_enabled_bool=false, mtk_dia
09-29 16:20:34.900887  1669  1669 D EriManager: loadEriFileFromXml: check for alternate file
09-29 16:20:34.901456  1669  1669 D EriManager: loadEriFileFromXml: no alternate file
09-29 16:20:34.902362  1669  1669 D EriManager: eriFile = eri.xml
09-29 16:20:34.911123  1669  1669 D EriManager: loadEriFileFromXml: eri parsing successful, file loaded. ver = 1357, # of entries = 176
09-29 16:20:34.913223  1669  1669 E MTKSST  : [GsmSST0] Invalid parameters for NR RSRP boost
09-29 16:20:34.916914  1669  1669 D RILJ    : [0185]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:34.919032  1669  1669 D RILJ    : [0186]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:34.921292  1669  1669 D RILJ    : [0187]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:34.921596  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 1, 4, 0, 3000, 2, 4, -128, -118, -108, -98 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:34.923460  1669  1669 D RILJ    : [0188]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:34.925271  1669  1669 D RILJ    : [0189]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:34.927215  1669  1669 D RILJ    : [0190]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:34.929338  1669  1669 D RILJ    : [0191]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:34.931616  1669  1669 D RILJ    : [0192]> SET_SIGNAL_STRENGTH_REPORTING_CRITERIA [PHONE0]
09-29 16:20:34.932289  1669  1669 D MtkGsmCdmaPhone: notifyCallForwardingIndicator: sim state = 1
09-29 16:20:34.932409  1669  1669 D MTKSST  : [GsmSST0] pollState: modemTriggered=false, mPollingContext=0, RadioState=1, connected=true, support_ap_iwlan=1
09-29 16:20:34.932952  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:34.933352  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 1, 2, 0, 3000, 2, 4, -115, -105, -95, -85 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:34.933683  1669  1669 D RILJ    : [0193]> OPERATOR [PHONE0]
09-29 16:20:34.934372  1669  1811 D RILJ    : [0185]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:34.934658  1669  1873 D IWlanNetworkService: getNetworkRegistrationState for domain 2, slotid: 0
09-29 16:20:34.935364  1669  1669 D RILJ    : [0194]> QUERY_NETWORK_SELECTION_MODE [PHONE0]
09-29 16:20:34.935523  1176  1202 I AT      : [0] AT> AT+EOPS? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:34.935871  1669  1920 D IWlanNetworkService: createRegistrationState.
09-29 16:20:34.935947  1669  1920 D IWlanNetworkService: getAvailableServices.
09-29 16:20:34.936158  1669  1920 D IWlanNetworkService: Calling callback.onGetNetworkRegistrationStateComplete.resultCode = 0, netState = NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, slotid: 0
09-29 16:20:34.936265  1669  1920 D NRM-I-0 : onRequestNetworkRegistrationInfoComplete result: 0, info: NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}
09-29 16:20:34.936411  1669  1871 D RILJ    : [0195]> DATA_REGISTRATION_STATE [PHONE0]
09-29 16:20:34.936725  1669  1871 D RILJ    : getDataRegistrationState: overrideHalVersion=null [PHONE0]
09-29 16:20:34.937113  1669  1669 D DSM-C-0 : Service com.android.phone already bound or being bound.
09-29 16:20:34.937958  1669  1871 D RILJ    : [0196]> VOICE_REGISTRATION_STATE [PHONE0]
09-29 16:20:34.938058  1669  1871 D RILJ    : getVoiceRegistrationState: overrideHalVersion=null [PHONE0]
09-29 16:20:34.941319  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:34.941799  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 1, 1, 0, 3000, 2, 4, -107, -103, -97, -89 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:34.942013  1176  1201 I AT      : [0] AT< +EOPS: 0,2,"45005",1 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:34.942087  1176  1201 I AT      : [0] AT< OK (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:34.942284  1669  1811 D RILJ    : [0186]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:34.942432  1176  1202 D RmcNwRTReqHdlr: [0] requestQueryNetworkSelectionMode return 0
09-29 16:20:34.942609  1176  1202 I AT      : [0] AT> AT+E5GOPT? (RIL_CMD_RT_7 tid:493339909376)
09-29 16:20:34.942946  1669  1811 D RILJ    : [0193]< OPERATOR {, , } [PHONE0]
09-29 16:20:34.943377  1669  1811 D RILJ    : [0194]< QUERY_NETWORK_SELECTION_MODE {0} [PHONE0]
09-29 16:20:34.945173  1669  1669 D MtkTelephonyAssist: DataStateController: onReceive action = android.intent.action.ACTION_DEFAULT_DATA_SUBSCRIPTION_CHANGED
09-29 16:20:34.945440  1669  1669 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:34.947483  1176  1198 I AT      : [0] AT> AT+EDALLOW=2,0 (RIL_CMD_READER_4 tid:493433326848)
09-29 16:20:34.947532  1669  1669 D DSM-I-0 : Service com.android.phone already bound or being bound.
09-29 16:20:34.948493  1669  1669 D MtkGsmCdmaPhone: correctPhoneTypeForCdma: change:false newVoiceRadioTech=1 mActivePhone=GSM
09-29 16:20:34.949032  1669  1669 D MtkSuppServHelper: [0]handleMessage: EVENT_CARRIER_CONFIG_LOADED(15)
09-29 16:20:34.949580  1669  1669 I MtkSuppServHelper: [0]Set mCarrierConfigLoaded: true
09-29 16:20:34.950832  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:34.951392  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 0, 4, 1, 3000, 2, 4, 0, 0, 0, 0 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:34.952758  1176  1201 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_RT_7, tid:493391277312)
09-29 16:20:34.953512  1669  1669 D MTKSST  : [GsmSST0] handlePollStateResultMessage: PS IWLAN. NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}
09-29 16:20:34.954484  1669  1669 D MTKSST  : [GsmSST0] EVENT_POLL_STATE_NETWORK_SELECTION_MODE
09-29 16:20:34.955372  1176  1197 I AT      : [0] AT< OK (RIL_CMD_READER_4, tid:493434363136)
09-29 16:20:34.957189  1669  1811 D RILJ    : [0187]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:34.959803  1669  1871 D CellularNetworkService: No access tech specific info passes for RegStateResult
09-29 16:20:34.959867  1669  1811 D RILJ    : [0195]< DATA_REGISTRATION_STATE {.regState = UNKNOWN, .rat = UNKNOWN, .reasonForDenial = NONE, .cellIdentity = {.noinit = {}}, .registeredPlmn = , .accessTechnologySpecificInfo = {.noinit = {}}} [PHONE0]
09-29 16:20:34.960044  1669  1871 D NRM-C-0 : onRequestNetworkRegistrationInfoComplete result: 0, info: NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}
09-29 16:20:34.960641  1669  1669 D MTKSST  : [GsmSST0] handlePollStateResultMessage: PS cellular. NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}
09-29 16:20:34.960857  1669  1871 D CellularNetworkService: No access tech specific info passes for RegStateResult
09-29 16:20:34.961009  1669  1811 D RILJ    : [0196]< VOICE_REGISTRATION_STATE {.regState = NOT_REG_MT_NOT_SEARCHING_OP_EM, .rat = UNKNOWN, .reasonForDenial = NONE, .cellIdentity = {.noinit = {}}, .registeredPlmn = , .accessTechnologySpecificInfo = {.noinit = {}}} [PHONE0]
09-29 16:20:34.961160  1669  1871 D NRM-C-0 : onRequestNetworkRegistrationInfoComplete result: 0, info: NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=true availableServices=[EMERGENCY] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}
09-29 16:20:34.961305  1669  1669 E MTKSST  : [GsmSST0] Exception while polling service state. Probably malformed RIL response.java.lang.NullPointerException: Attempt to invoke virtual method 'int android.telephony.CellIdentity.getType()' on a null object reference
09-29 16:20:34.961600  1669  1669 D MTKSST  : [GsmSST0] Could not set ServiceState channel number. CellIdentity null
09-29 16:20:34.962212  1669  1669 D MTKSST  : [GsmSST0] combinePsRegistrationStates: {mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=, mOperatorAlphaShort=, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=false, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=true availableServices=[EMERGENCY] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=, mOperatorAlphaShortRaw=, mIsIwlanPreferred=false, Ril Voice Regist state=0, Ril Data Regist state=4, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0}
09-29 16:20:34.962905  1669  1669 D MtkRILJ : lookupOperatorNameNitz plmn name update to Nitz: 
09-29 16:20:34.963167  1669  1669 E MTKSST  : lookupOperatorName getPhone null subid=-1
09-29 16:20:34.963411  1669  1669 D MtkRILJ : lookupOperatorNameMVNO plmn name update to TS.25/MVNO: 
09-29 16:20:34.963548  1669  1669 D MtkRILJ : lookupOperatorNameNitz plmn name update to Nitz: 
09-29 16:20:34.963713  1669  1669 E MTKSST  : lookupOperatorName getPhone null subid=-1
09-29 16:20:34.963881  1669  1669 D MtkRILJ : lookupOperatorNameMVNO plmn name update to TS.25/MVNO: 
09-29 16:20:34.964272  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:34.964688  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 0, 4, 2, 3000, 2, 4, 0, 0, 0, 0 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:34.965184  1669  1669 D MTKSST  : [GsmSST0] refreshSpn: null, null, fromPollState=true, mForceBroadcastServiceState=true
09-29 16:20:34.967053  1669  1669 D MTKSST  : [GsmSST0] Could not set ServiceState channel number. CellIdentity null
09-29 16:20:34.967624  1669  1669 D MTKSST  : [GsmSST0] Poll ServiceState done: oldSS=[{mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=null, mOperatorAlphaShort=null, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=true, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=true availableServices=[EMERGENCY] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=, mOperatorAlphaShortRaw=, mIsIwlanPreferred=false, Ril Voice Regist state=0, Ril Data Regist state=4, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0}]
09-29 16:20:34.968317  1669  1669 D MTKSST  : [GsmSST0] Poll ServiceState done: newSS=[{mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=null, mOperatorAlphaShort=null, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=true, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=true availableServices=[EMERGENCY] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=, mOperatorAlphaShortRaw=, mIsIwlanPreferred=false, Ril Voice Regist state=0, Ril Data Regist state=4, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0}] oldMaxDataCalls=16 mNewMaxDataCalls=16 oldReasonDataDenied=0 mNewReasonDataDenied=0 isImsEccOnly= false
09-29 16:20:34.968993  1669  1669 D MTKSST  : [GsmSST0] pollStateDone: hasRegistered = false hasDeregistered = false hasDataAttached = {1=false, 2=false} hasDataDetached = {1=false, 2=false} hasDataRegStateChanged = {1=false, 2=false} hasRilVoiceRadioTechnologyChanged = false hasRilDataRadioTechnologyChanged = {1=false, 2=false} hasDataTransportPreferenceChanged = false hasChanged = true hasVoiceRoamingOn = false hasVoiceRoamingOff = false hasDataRoamingOn =false hasDataRoamingOff = false hasLocationChanged = false has4gHandoff = false hasMultiApnSupport = false hasLostMultiApnSupport = false hasCssIndicatorChanged = false hasNrFrequencyRangeChanged = false hasNrStateChanged = false hasVoiceRoamingTypeChange = false hasDataRoamingTypeChange = false hasAirplaneModeOnlChanged = false hasPlmnChange = false
09-29 16:20:34.969220  1669  1811 D RILJ    : [0188]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:34.972841  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:34.973341  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 1, 128, 0, 3000, 2, 4, -110, -90, -80, -65 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:34.973782  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: radio is on but out of service, set plmn='Emergency calls only'
09-29 16:20:34.974008  1669  1811 D RILJ    : [0189]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:34.974939  1669  1669 D MTKSST  : [GsmSST0] updateSpnDisplay: rawSpn = 
09-29 16:20:34.978138  1669  1669 D MTKSST  : [GsmSST0] localeOperator  is invalid
09-29 16:20:34.980085  1669  1669 D MTKSST  : [GsmSST0] Broadcasting ServiceState : {mVoiceRegState=1(OUT_OF_SERVICE), mDataRegState=1(OUT_OF_SERVICE), mChannelNumber=-1, duplexMode()=0, mCellBandwidths=[], mOperatorAlphaLong=null, mOperatorAlphaShort=null, isManualNetworkSelection=false(automatic), getRilVoiceRadioTechnology=0(Unknown), getRilDataRadioTechnology=0(Unknown), mCssIndicator=unsupported, mNetworkId=-1, mSystemId=-1, mCdmaRoamingIndicator=-1, mCdmaDefaultRoamingIndicator=-1, mIsEmergencyOnly=true, isUsingCarrierAggregation=false, mNetworkRegistrationInfos=[NetworkRegistrationInfo{ domain=PS transportType=WLAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 0 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false LteVopsSupportInfo :  mVopsSupport = 1 mEmcBearerSupport = 1 } nrState=NONE rRplmn=null isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=CS transportType=WWAN registrationState=NOT_REG_OR_SEARCHING roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=true availableServices=[EMERGENCY] cellIdentity=null voiceSpecificInfo=VoiceSpecificRegistrationInfo { mCssSupported=false mRoamingIndicator=0 mSystemIsInPrl=0 mDefaultRoamingIndicator=0} dataSpecificInfo=null nrState=NONE rRplmn= isUsingCarrierAggregation=false}, NetworkRegistrationInfo{ domain=PS transportType=WWAN registrationState=UNKNOWN roamingType=NOT_ROAMING accessNetworkTechnology=UNKNOWN rejectCause=0 emergencyEnabled=false availableServices=[] cellIdentity=null voiceSpecificInfo=null dataSpecificInfo=android.telephony.DataSpecificRegistrationInfo :{ maxDataCalls = 16 isDcNrRestricted = false isNrAvailable = false isEnDcAvailable = false null } nrState=NONE rRplmn= isUsingCarrierAggregation=false}], mNrFrequencyRange=0, mOperatorAlphaLongRaw=, mOperatorAlphaShortRaw=, mIsIwlanPreferred=false, Ril Voice Regist state=0, Ril Data Regist state=4, VoiceRejectCause=-1, DataRejectCause=-1, IwlanRegState=1, CellularVoiceRegState=1, CellularDataRegState=1, RilCellularDataRegState=0, CellularDataRoamingType=0, CellularDataNetworkType=0}
09-29 16:20:34.982556  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:34.982945  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 0, 128, 1, 3000, 2, 4, 0, 0, 0, 0 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:34.983823  1669  1811 D RILJ    : [0190]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:34.985542  1669  1669 D MtkRILJ : [0197]> MTK: RIL_REQUEST_SET_SERVICE_STATE voiceRegState: 1 dataRegState: 1 voiceRoamingType: 0 dataRoamingType: 0 rilVoiceRegState: 0 rilDataRegState:4 [SUB0]
09-29 16:20:34.991533  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:34.992053  1176  1192 I AT      : [0] AT> AT+ECSQ=4, 0, 128, 2, 3000, 2, 4, 0, 0, 0, 0 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:20:34.992921  1669  1811 D RILJ    : [0191]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:35.000992  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:35.001327  1176  1192 D RmcNwReqHdlr: [0] [currentPhysicalChannelConfigs] needNotifyEmpty and has notified empty list, return
09-29 16:20:35.001824  1669  1811 D RILJ    : [0192]< SET_SIGNAL_STRENGTH_REPORTING_CRITERIA  [PHONE0]
09-29 16:20:35.009153  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:20:35.019309  1669  1811 D RILJ    : [0197]< MTK: RIL_REQUEST_SET_SERVICE_STATE  [PHONE0]
09-29 16:20:35.692499  1176  1184 I AT      : [0] AT< +ECSQ: 63,44,1,-231,-9,1,1,4,32767,1 (RIL_URC_READER, tid:493447834880)
09-29 16:20:35.693459  1176  1185 D RmcNwHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0X04]
09-29 16:20:35.693511  1176  1185 D RmcNwHdlr: [0] handleSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 27, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 63, wcdma_ecno: 44, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:20:35.697972  1669  1669 D MTKSST  : [GsmSST0] new:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-59 ber=99 rscp=-57 ecno=-2 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}, old:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-59 ber=99 rscp=-57 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}
09-29 16:20:35.699358  1251  2906 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:35.699878  1251  2906 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:35.702423  1251  2906 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:35.702694  1251  2906 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:36.016809  1669  2002 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:36.017930  1669  2002 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:36.196815  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=83, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10095 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:36.197200  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=83, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10095 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:36.869905  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=85, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10089 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:36.870700  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=85, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10089 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:37.081699  1669  1669 D MTKCAT  : BootCompletedReceiver: [onReceive] action = android.intent.action.BOOT_COMPLETED
09-29 16:20:37.086363  1669  1669 D MTKCAT  : BootCompletedReceiver: [ACTION_BOOT_COMPLETED]
09-29 16:20:37.087914  1669  1669 D MTKCAT  : StkAppService: onCreate()+
09-29 16:20:37.088271  1669  1669 D MTKCAT  : StkAppService: simCount: 1, maxSimCount: 1
09-29 16:20:37.088628  1669  1669 D MTKCAT  : StkAppService: slotId: 0
09-29 16:20:37.088690  1669  1669 D MTKCAT  : CatService: call getInstance 3
09-29 16:20:37.095108  1669  1669 D MtkTelephonyManagerEx: isSimOnOffEnabled result = false
09-29 16:20:37.095350  1669  1669 D MTKCAT  : StkAppService: Register for phone state change
09-29 16:20:37.096788  1669  1669 D MTKCAT  : StkAppService: onStart sim id: 0, op: 5, *****
09-29 16:20:37.096936  1669  1669 D MTKCAT  : CatService: call getInstance 3
09-29 16:20:37.097012  1669  1669 D MTKCAT  : StkAppService: mStkService is: -1
09-29 16:20:37.099547  1669  1669 D MTKCAT  : StkAppInstaller: install, make sure stkMain be intalled
09-29 16:20:37.099809  1669  1669 D MTKCAT  : StkAppInstaller: installOrUpdate : 255, class: com.android.stk.StkMain
09-29 16:20:37.100059  1669  1669 D MTKCAT  : StkAppInstaller: label is null and set label to SIM Toolkit
09-29 16:20:37.100916  1669  1669 D MTKCAT  : StkAppInstaller: Set the label to SIM Toolkit
09-29 16:20:37.101901  1669  1669 D MTKCAT  : StkAppService: onDestroy()
09-29 16:20:37.106809  1669  1669 D MTKCAT  : StkAppService: unregister for phone state change
09-29 16:20:37.570577  3494  3541 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.google.android.ims listener=dkv@fbfa0dd
09-29 16:20:37.578725  1669  1866 D SubscriptionController: [getActiveSubscriptionInfoForSimSlotIndex]+ slotIndex=0 subId=null
09-29 16:20:37.722641  1669  1866 D SubscriptionController: [getActiveSubscriptionInfoForSimSlotIndex]+ slotIndex=0 subId=null
09-29 16:20:37.850460  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=87, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10091 RequestorUid: 10091 RequestorPkg: com.google.android.ims UnderlyingNetworks: Null] ]
09-29 16:20:37.851172  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=87, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10091 RequestorUid: 10091 RequestorPkg: com.google.android.ims UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:37.890169  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=89, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10091 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:37.890975  3494  3541 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.google.android.ims listener=dkv@45a179c
09-29 16:20:37.893070  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=89, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10091 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:37.899376  1669  1866 D SubscriptionController: [getActiveSubscriptionInfoForSimSlotIndex]+ slotIndex=0 subId=null
09-29 16:20:37.983201  1669  3209 D SubscriptionController: [getActiveSubscriptionInfoForSimSlotIndex]+ slotIndex=0 subId=null
09-29 16:20:38.408102  1669  1866 D SubscriptionController: [getActiveSubscriptionInfoForSimSlotIndex]+ slotIndex=0 subId=null
09-29 16:20:39.621690  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=91, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10116 RequestorUid: 10116 RequestorPkg: com.google.android.apps.maps UnderlyingNetworks: Null] ]
09-29 16:20:39.622325  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=91, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10116 RequestorUid: 10116 RequestorPkg: com.google.android.apps.maps UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:39.687844  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=93, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10116 RequestorUid: 10116 RequestorPkg: com.google.android.apps.maps UnderlyingNetworks: Null] ]
09-29 16:20:39.688399  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=93, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10116 RequestorUid: 10116 RequestorPkg: com.google.android.apps.maps UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:40.307961  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=96, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10100 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:40.308599  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=96, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10100 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:40.811852  1176  1184 I AT      : [0] AT< +ECSQ: 63,43,1,-230,-11,1,1,4,32767,1 (RIL_URC_READER, tid:493447834880)
09-29 16:20:40.812703  1176  1185 D RmcNwHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0X04]
09-29 16:20:40.812796  1176  1185 D RmcNwHdlr: [0] handleSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 27, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 63, wcdma_ecno: 43, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:20:40.818821  1669  1669 D MTKSST  : [GsmSST0] new:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-59 ber=99 rscp=-57 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}, old:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-59 ber=99 rscp=-57 ecno=-2 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}
09-29 16:20:40.820138  1251  1270 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:40.820357  1251  1270 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:40.823313  1251  1517 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:40.823473  1251  1517 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:41.763123  1669  3209 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:41.765049  1669  3209 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:42.358612  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=98, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10123 RequestorUid: 10123 RequestorPkg: com.google.android.apps.photos UnderlyingNetworks: Null] ]
09-29 16:20:42.359320  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=98, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10123 RequestorUid: 10123 RequestorPkg: com.google.android.apps.photos UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:42.531722  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=100, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10123 RequestorUid: 10123 RequestorPkg: com.google.android.apps.photos UnderlyingNetworks: Null] ]
09-29 16:20:42.532277  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=100, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10123 RequestorUid: 10123 RequestorPkg: com.google.android.apps.photos UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:45.934171  1176  1184 I AT      : [0] AT< +ECSQ: 64,42,1,-225,-14,1,1,4,32767,1 (RIL_URC_READER, tid:493447834880)
09-29 16:20:45.935204  1176  1185 D RmcNwHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0X04]
09-29 16:20:45.935296  1176  1185 D RmcNwHdlr: [0] handleSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 28, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 64, wcdma_ecno: 42, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:20:45.940678  1669  1669 D MTKSST  : [GsmSST0] new:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-57 ber=99 rscp=-56 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}, old:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-59 ber=99 rscp=-57 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}
09-29 16:20:45.942138  1251  1667 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:45.942285  1251  1667 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:45.944640  1251  1667 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:45.944787  1251  1667 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:46.992137  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=102, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10121 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:46.992705  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=102, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10121 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:49.823629  4244  4244 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.google.android.setupwizard listener=bic@3523e80
09-29 16:20:49.965740  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=106, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10132 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:49.966493  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=106, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10132 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:50.592987  3246  4122 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.google.android.apps.messaging listener=abjl@c01ff8f
09-29 16:20:50.604786  3246  4347 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.google.android.apps.messaging listener=ayso@e66bcdd
09-29 16:20:50.609706  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=108, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10118 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:50.610278  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=108, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10118 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:50.613562  1669  1846 D SubscriptionController: [getActiveSubscriptionInfoForSimSlotIndex]+ slotIndex=0 subId=null
09-29 16:20:50.624184  1669  1686 D SubscriptionController: [getActiveSubscriptionInfoForSimSlotIndex]+ slotIndex=0 subId=null
09-29 16:20:50.861784  1669  1686 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:51.054470  1176  1184 I AT      : [0] AT< +ECSQ: 65,43,1,-222,-11,1,1,4,32767,1 (RIL_URC_READER, tid:493447834880)
09-29 16:20:51.055131  1176  1185 D RmcNwHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0X04]
09-29 16:20:51.055200  1176  1185 D RmcNwHdlr: [0] handleSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 28, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 65, wcdma_ecno: 43, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:20:51.058340  1669  1669 D MTKSST  : [GsmSST0] new:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-57 ber=99 rscp=-55 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}, old:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-57 ber=99 rscp=-56 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}
09-29 16:20:51.059485  1251  1667 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:51.059769  1251  1667 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:51.059856  1251  1667 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:51.061522  1251  1667 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:51.061746  1251  1667 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:51.061839  1251  1667 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:20:51.274098  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=110, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10111 RequestorUid: 10111 RequestorPkg: com.google.android.videos UnderlyingNetworks: Null] ]
09-29 16:20:51.274440  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=110, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10111 RequestorUid: 10111 RequestorPkg: com.google.android.videos UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:51.406965  1669  1686 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:51.644590  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=113, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10100 RequestorUid: 10100 RequestorPkg: com.google.android.apps.messaging UnderlyingNetworks: Null] ]
09-29 16:20:51.645129  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=113, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10100 RequestorUid: 10100 RequestorPkg: com.google.android.apps.messaging UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:51.840487  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=116, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10112 RequestorUid: 10112 RequestorPkg: com.google.android.youtube UnderlyingNetworks: Null] ]
09-29 16:20:51.840991  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=116, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10112 RequestorUid: 10112 RequestorPkg: com.google.android.youtube UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:51.876289  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=118, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10112 RequestorUid: 10112 RequestorPkg: com.google.android.youtube UnderlyingNetworks: Null] ]
09-29 16:20:51.876639  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=118, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10112 RequestorUid: 10112 RequestorPkg: com.google.android.youtube UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:51.889575  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=121, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10112 RequestorUid: 10112 RequestorPkg: com.google.android.youtube UnderlyingNetworks: Null] ]
09-29 16:20:51.889967  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=121, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10112 RequestorUid: 10112 RequestorPkg: com.google.android.youtube UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:51.900896  1669  1686 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:51.903323  1669  1686 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:51.903532  1669  1896 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:20:51.975524  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=123, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10112 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:51.976005  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=123, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10112 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:52.020074  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=125, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10112 RequestorUid: 10112 RequestorPkg: com.google.android.youtube UnderlyingNetworks: Null] ]
09-29 16:20:52.020518  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=125, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10112 RequestorUid: 10112 RequestorPkg: com.google.android.youtube UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:52.398704  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=127, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10112 RequestorUid: 10112 RequestorPkg: com.google.android.youtube UnderlyingNetworks: Null] ]
09-29 16:20:52.399324  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=127, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10112 RequestorUid: 10112 RequestorPkg: com.google.android.youtube UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:52.743235  1669  1669 D MtkCapCtrlReceiver: onReceive action = android.intent.action.BOOT_COMPLETED
09-29 16:20:52.754708  1669  1669 D MtkCapService: created
09-29 16:20:52.755277  1669  1669 D MtkCapService: onStartCommand
09-29 16:20:52.755949  1669  1669 D MtkCapService: initCapRIL, sim count 1
09-29 16:20:52.772300  1176  1176 I RILC    : [24] setResponseFunctionsCap
09-29 16:20:52.773974  1669  1669 D MtkCapCtrlIntfMgrEx: publish: com.mediatek.capctrl.service.MtkCapCtrlInterfaceManager@ed220b0
09-29 16:20:53.211972  1669  1669 D MtkTelephonyAssist: MtkPhoneAssistBroadcastReceiver: MtkPhoneAssistBroadcastReceiver action = android.intent.action.BOOT_COMPLETED isSystemUser = true
09-29 16:20:55.048853  1669  1686 D MtkIccSmsInterfaceManager: Cell broadcast ranges reset.
09-29 16:20:55.055251  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 1 configurations
09-29 16:20:55.063283  1669  1686 D RILJ    : [0198]> GSM_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:55.063617  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4370] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.066465  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 1
09-29 16:20:55.066548  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370
09-29 16:20:55.066634  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:55.115555  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:55.117192  1669  1811 D RILJ    : [0198]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:55.117520  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4370 to 4370
09-29 16:20:55.117826  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:55.118665  1894  4708 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.121186  1669  1896 D MtkIccSmsInterfaceManager: Calling setCdmaBroadcastConfig with 1 configurations
09-29 16:20:55.124402  1669  1896 D RILJ    : [0199]> CDMA_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:55.124723  1669  1896 D RILJ    : {.serviceCategory = 4096, .language = 1, .selected = true} [PHONE0]
09-29 16:20:55.126581  1176  1196 I AT      : [0] AT> AT+ECSCBCHA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:55.137119  1176  1195 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:55.138218  1669  1811 D RILJ    : [0199]< CDMA_SET_BROADCAST_CONFIG error 6 [PHONE0]
09-29 16:20:55.138787  1669  1811 D RilRequest: [0199]< CDMA_SET_BROADCAST_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result={ when=-1m3s959ms what=4 obj=com.android.internal.telephony.IccSmsInterfaceManager$Request@d8dbb29 target=com.android.internal.telephony.IccSmsInterfaceManager$1 }
09-29 16:20:55.140105  1669  1896 D MtkIccSmsInterfaceManager: Failed to add cdma broadcast channels range 4096 to 4096
09-29 16:20:55.140733  1894  4708 D SmsManager: enableCellBroadcastRange: failed at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.143086  1669  1896 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 2 configurations
09-29 16:20:55.148267  1669  1896 D RILJ    : [0200]> GSM_SET_BROADCAST_CONFIG with 2 configs :  [PHONE0]
09-29 16:20:55.148465  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4370] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.148547  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4383] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.150707  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 2
09-29 16:20:55.150796  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370,4383
09-29 16:20:55.150865  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370,4383","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:55.192166  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:55.193248  1669  1811 D RILJ    : [0200]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:55.193429  1669  1896 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4383 to 4383
09-29 16:20:55.193756  1669  1896 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:55.194101  1894  4708 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.196640  1669  1896 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:55.200425  1669  1896 D RILJ    : [0201]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:55.200521  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4370] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.200553  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4383] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.200580  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4371,4372] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.202277  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:55.202359  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370,4383,4371-4372
09-29 16:20:55.202445  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370,4383,4371-4372","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:55.245010  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:55.246122  1669  1811 D RILJ    : [0201]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:55.246344  1669  1896 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4371 to 4372
09-29 16:20:55.246527  1669  1896 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:55.246865  1894  4708 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.248653  1669  1896 D MtkIccSmsInterfaceManager: Calling setCdmaBroadcastConfig with 1 configurations
09-29 16:20:55.251081  1669  1896 D RILJ    : [0202]> CDMA_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:55.251307  1669  1896 D RILJ    : {.serviceCategory = 4097, .language = 1, .selected = true} [PHONE0]
09-29 16:20:55.253162  1176  1196 I AT      : [0] AT> AT+ECSCBCHA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:55.262335  1176  1195 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:55.263740  1669  1811 D RILJ    : [0202]< CDMA_SET_BROADCAST_CONFIG error 6 [PHONE0]
09-29 16:20:55.264006  1669  1811 D RilRequest: [0202]< CDMA_SET_BROADCAST_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result={ when=-1m4s84ms what=4 obj=com.android.internal.telephony.IccSmsInterfaceManager$Request@f155eae target=com.android.internal.telephony.IccSmsInterfaceManager$1 }
09-29 16:20:55.265578  1669  1896 D MtkIccSmsInterfaceManager: Failed to add cdma broadcast channels range 4097 to 4097
09-29 16:20:55.266222  1894  4708 D SmsManager: enableCellBroadcastRange: failed at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.269317  1669  1896 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:55.272046  1669  1896 D RILJ    : [0203]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:55.272259  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4372] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.272341  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4383] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.272419  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4384,4385] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.274014  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:55.274094  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4372,4383,4384-4385
09-29 16:20:55.274174  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4372,4383,4384-4385","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:55.315532  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:55.317229  1669  1811 D RILJ    : [0203]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:55.317454  1669  1896 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4384 to 4385
09-29 16:20:55.317730  1669  1896 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:55.318753  1894  4708 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.320658  1669  1896 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:55.323442  1669  1896 D RILJ    : [0204]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:55.323792  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4372] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.323912  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4385] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.323993  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4373,4378] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.325810  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:55.325951  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4372,4383-4385,4373-4378
09-29 16:20:55.326033  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4372,4383-4385,4373-4378","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:55.374408  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:55.375768  1669  1811 D RILJ    : [0204]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:55.376083  1669  1896 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4373 to 4378
09-29 16:20:55.376280  1669  1896 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:55.376673  1894  4708 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.380641  1669  1896 D MtkIccSmsInterfaceManager: Calling setCdmaBroadcastConfig with 1 configurations
09-29 16:20:55.383145  1669  1896 D RILJ    : [0205]> CDMA_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:55.383352  1669  1896 D RILJ    : {.serviceCategory = 4098, .language = 1, .selected = true} [PHONE0]
09-29 16:20:55.384968  1176  1196 I AT      : [0] AT> AT+ECSCBCHA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:55.393332  1176  1195 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:55.394777  1669  1811 D RILJ    : [0205]< CDMA_SET_BROADCAST_CONFIG error 6 [PHONE0]
09-29 16:20:55.395054  1669  1811 D RilRequest: [0205]< CDMA_SET_BROADCAST_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result={ when=-1m4s215ms what=4 obj=com.android.internal.telephony.IccSmsInterfaceManager$Request@786844f target=com.android.internal.telephony.IccSmsInterfaceManager$1 }
09-29 16:20:55.395457  1669  1896 D MtkIccSmsInterfaceManager: Failed to add cdma broadcast channels range 4098 to 4098
09-29 16:20:55.397508  1894  4708 D SmsManager: enableCellBroadcastRange: failed at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.399550  1669  1896 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:55.402837  1669  1896 D RILJ    : [0206]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:55.403049  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4378] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.403150  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4385] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.403225  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4386,4391] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.404961  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:55.405047  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4378,4383-4385,4386-4391
09-29 16:20:55.405122  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4378,4383-4385,4386-4391","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:55.443050  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:55.444266  1669  1811 D RILJ    : [0206]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:55.444927  1669  1896 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4386 to 4391
09-29 16:20:55.445232  1669  1896 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:55.445675  1894  4708 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.447296  1669  1896 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:55.450727  1669  1896 D RILJ    : [0207]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:55.451036  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4378] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.451163  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4391] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.451279  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4379,4379] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.452971  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:55.453072  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4378,4383-4391,4379
09-29 16:20:55.453162  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4378,4383-4391,4379","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:55.497762  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:55.499210  1669  1811 D RILJ    : [0207]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:55.499644  1669  1896 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4379 to 4379
09-29 16:20:55.499933  1669  1896 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:55.500360  1894  4708 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.504068  1669  1896 D MtkIccSmsInterfaceManager: Calling setCdmaBroadcastConfig with 1 configurations
09-29 16:20:55.507900  1669  1896 D RILJ    : [0208]> CDMA_SET_BROADCAST_CONFIG with 1 configs :  [PHONE0]
09-29 16:20:55.508031  1669  1896 D RILJ    : {.serviceCategory = 4099, .language = 1, .selected = true} [PHONE0]
09-29 16:20:55.511135  1176  1196 I AT      : [0] AT> AT+ECSCBCHA? (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:55.519123  1176  1195 I AT      : [0] AT< +CME ERROR: 65535 (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:55.520491  1669  1811 D RILJ    : [0208]< CDMA_SET_BROADCAST_CONFIG error 6 [PHONE0]
09-29 16:20:55.520773  1669  1811 D RilRequest: [0208]< CDMA_SET_BROADCAST_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret= result={ when=-1m4s341ms what=4 obj=com.android.internal.telephony.IccSmsInterfaceManager$Request@4b097dc target=com.android.internal.telephony.IccSmsInterfaceManager$1 }
09-29 16:20:55.522109  1669  1896 D MtkIccSmsInterfaceManager: Failed to add cdma broadcast channels range 4099 to 4099
09-29 16:20:55.522696  1894  4708 D SmsManager: enableCellBroadcastRange: failed at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.525348  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:55.528230  1669  1686 D RILJ    : [0209]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:55.528334  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4379] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.528365  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4391] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.528420  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4392,4392] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.530981  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:55.531085  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4379,4383-4391,4392
09-29 16:20:55.531165  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4379,4383-4391,4392","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:55.573286  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:55.574979  1669  1811 D RILJ    : [0209]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:55.575634  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4392 to 4392
09-29 16:20:55.575948  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:55.576490  1894  4708 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.578321  1669  1686 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4380 to 4380
09-29 16:20:55.578991  1894  4708 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.580390  1669  1896 D MtkIccSmsInterfaceManager: Failed to remove cdma broadcast channels range 4100 to 4100
09-29 16:20:55.580969  1894  4708 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.582147  1669  1896 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4393 to 4393
09-29 16:20:55.582630  1894  4708 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.583915  1669  1896 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4381 to 4381
09-29 16:20:55.584401  1894  4708 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.585314  1669  1896 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4394 to 4394
09-29 16:20:55.585810  1894  4708 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.586760  1669  1896 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4382 to 4382
09-29 16:20:55.587178  1894  4708 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.588263  1669  1896 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4395 to 4395
09-29 16:20:55.588694  1894  4708 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.589773  1669  1686 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 3 configurations
09-29 16:20:55.592073  1669  1686 D RILJ    : [0210]> GSM_SET_BROADCAST_CONFIG with 3 configs :  [PHONE0]
09-29 16:20:55.592281  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4379] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.592366  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4392] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.592460  1669  1686 D RILJ    : SmsBroadcastConfigInfo: Id [4352,4354] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.595003  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 3
09-29 16:20:55.595154  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4370-4379,4383-4392,4352-4354
09-29 16:20:55.595303  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4370-4379,4383-4392,4352-4354","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:55.641036  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:55.643065  1669  1811 D RILJ    : [0210]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:55.643586  1669  1686 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4352 to 4354
09-29 16:20:55.644157  1669  1686 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:55.644744  1894  4708 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.647203  1669  1896 D MtkIccSmsInterfaceManager: Calling setGsmBroadcastConfig with 4 configurations
09-29 16:20:55.650926  1669  1896 D RILJ    : [0211]> GSM_SET_BROADCAST_CONFIG with 4 configs :  [PHONE0]
09-29 16:20:55.651242  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4352,4354] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.653020  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4370,4379] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.653097  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4383,4392] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.653152  1669  1896 D RILJ    : SmsBroadcastConfigInfo: Id [4356,4356] Code [0,255] ENABLED [PHONE0]
09-29 16:20:55.655981  1176  1196 D RmcGsmSmsRequest: [0] Set CB channel array num 4
09-29 16:20:55.656168  1176  1196 D RmcGsmSmsRequest: [0] Set CB channels 4352-4354,4370-4379,4383-4392,4356
09-29 16:20:55.656297  1176  1196 I AT      : [0] AT> AT+ECSCBCFG="4352-4354,4370-4379,4383-4392,4356","--" (RIL_CMD_READER_3 tid:493435399424)
09-29 16:20:55.700685  1176  1195 I AT      : [0] AT< OK (RIL_CMD_READER_3, tid:493436435712)
09-29 16:20:55.702301  1669  1811 D RILJ    : [0211]< GSM_SET_BROADCAST_CONFIG  [PHONE0]
09-29 16:20:55.702765  1669  1896 D MtkIccSmsInterfaceManager: Added GSM cell broadcast channels range 4356 to 4356
09-29 16:20:55.703340  1669  1896 D MtkIccSmsInterfaceManager: Calling proprietary setCellBroadcastActivation(true)
09-29 16:20:55.704123  1894  4708 D SmsManager: enableCellBroadcastRange: succeeded at calling enableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:55.706565  1669  1896 D MtkIccSmsInterfaceManager: Failed to remove GSM cell broadcast channels range 4355 to 4355
09-29 16:20:55.707315  1894  4708 D SmsManager: disableCellBroadcastRange: failed at calling disableCellBroadcastRangeForSubscriber. subId = -1
09-29 16:20:58.912112  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=129, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10103 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ]
09-29 16:20:58.912807  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=129, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10103 RequestorUid: 1000 RequestorPkg: android UnderlyingNetworks: Null] ] shouldApply false
09-29 16:20:59.069043  1669  1846 E PhoneSubInfoController: getIccSerialNumber phone is null for Subscription:-1
09-29 16:21:00.981674  1669  1846 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:21:01.297746  1176  1184 I AT      : [0] AT< +ECSQ: 62,43,1,-235,-12,1,1,4,32767,1 (RIL_URC_READER, tid:493447834880)
09-29 16:21:01.298891  1176  1185 D RmcNwHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0X04]
09-29 16:21:01.298974  1176  1185 D RmcNwHdlr: [0] handleSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 27, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 62, wcdma_ecno: 43, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:21:01.302972  1669  1669 D MTKSST  : [GsmSST0] new:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-59 ber=99 rscp=-58 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}, old:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-57 ber=99 rscp=-55 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}
09-29 16:21:01.303926  1251  2254 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:01.304180  1251  2254 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:01.304319  1251  2254 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:01.306472  1251  2254 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:01.306690  1251  2254 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:01.306784  1251  2254 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:04.834846  1669  1686 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:21:05.107303  1669  1669 D TelephonyNetworkFactory[0]: onReleaseNetworkFor NetworkRequest [ REQUEST id=68, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10103 RequestorUid: 10103 RequestorPkg: com.google.android.gms UnderlyingNetworks: Null] ] applied false
09-29 16:21:06.072630  1669  1669 D TelephonyNetworkFactory[0]: got request NetworkRequest [ REQUEST id=131, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10103 RequestorUid: 10103 RequestorPkg: com.google.android.gms UnderlyingNetworks: Null] ]
09-29 16:21:06.073435  1669  1669 D TelephonyNetworkFactory[0]: onNeedNetworkFor NetworkRequest [ REQUEST id=131, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VCN_MANAGED Uid: 10103 RequestorUid: 10103 RequestorPkg: com.google.android.gms UnderlyingNetworks: Null] ] shouldApply false
09-29 16:21:06.418384  1176  1184 I AT      : [0] AT< +ECSQ: 60,43,1,-241,-11,1,1,4,32767,1 (RIL_URC_READER, tid:493447834880)
09-29 16:21:06.419119  1176  1185 D RmcNwHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0X04]
09-29 16:21:06.419215  1176  1185 D RmcNwHdlr: [0] handleSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 26, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 60, wcdma_ecno: 43, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:21:06.422904  1669  1669 D MTKSST  : [GsmSST0] new:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-61 ber=99 rscp=-60 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}, old:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-59 ber=99 rscp=-58 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}
09-29 16:21:06.424044  1251  1547 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:06.424160  1251  1547 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:06.424206  1251  1547 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:06.426268  1251  1547 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:06.426519  1251  1547 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:06.426677  1251  1547 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:06.866175  1176  1223 I RilClient: initialize: commandFd is 44
09-29 16:21:06.866816  1176  1223 I RilClient: start listen on fd: 30, socket name: rild-oem
09-29 16:21:06.867537  1176  1192 I RmcOemHandler: requestQueryThermal Enter: 0,0,0
09-29 16:21:06.867645  1176  1192 I AT      : [0] AT> AT+ETHERMAL=0,0,0 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:21:06.875268  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:21:06.875498  1176  1192 I RmcOemHandler: requestQueryThermal error
09-29 16:21:06.875874  1176  1182 D RtcRilClientController: client 1001 handle requestComplete
09-29 16:21:06.876316  1176  1223 I RilClient: initialize: commandFd is 67
09-29 16:21:06.876705  1176  1223 I RilClient: start listen on fd: 30, socket name: rild-oem
09-29 16:21:06.877314  1176  1192 I RmcOemHandler: requestQueryThermal Enter: 0,1,0
09-29 16:21:06.877389  1176  1192 I AT      : [0] AT> AT+ETHERMAL=0,1,0 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:21:06.885246  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:21:06.885427  1176  1192 I RmcOemHandler: requestQueryThermal error
09-29 16:21:06.885718  1176  1182 D RtcRilClientController: client 1001 handle requestComplete
09-29 16:21:06.886137  1176  1223 I RilClient: initialize: commandFd is 44
09-29 16:21:06.886595  1176  1223 I RilClient: start listen on fd: 30, socket name: rild-oem
09-29 16:21:06.887103  1176  1192 I RmcOemHandler: requestQueryThermal Enter: 0,2,0
09-29 16:21:06.887227  1176  1192 I AT      : [0] AT> AT+ETHERMAL=0,2,0 (RIL_CMD_READER_1 tid:493439544576)
09-29 16:21:06.894652  1176  1191 I AT      : [0] AT< +CME ERROR: 100 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:21:06.894873  1176  1192 I RmcOemHandler: requestQueryThermal error
09-29 16:21:06.895161  1176  1182 D RtcRilClientController: client 1001 handle requestComplete
09-29 16:21:06.895532  1176  1223 I RilClient: initialize: commandFd is 67
09-29 16:21:06.895965  1176  1223 I RilClient: start listen on fd: 30, socket name: rild-oem
09-29 16:21:06.896448  1176  1192 I RmcOemHandler: requestQueryThermal Enter: -1
09-29 16:21:06.896581  1176  1192 I AT      : [0] AT> AT+ETHERMAL (RIL_CMD_READER_1 tid:493439544576)
09-29 16:21:06.904654  1176  1191 I AT      : [0] AT< +ETHERMAL: 2, 32767, -127, 111, 32767, 4046 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:21:06.904727  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:21:06.904849  1176  1192 I RmcOemHandler: requestQueryThermal success
09-29 16:21:06.905159  1176  1182 D RtcRilClientController: client 1001 handle requestComplete
09-29 16:21:11.539453  1176  1184 I AT      : [0] AT< +ECSQ: 60,41,1,-241,-15,1,1,4,32767,1 (RIL_URC_READER, tid:493447834880)
09-29 16:21:11.540110  1176  1185 D RmcNwHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0X04]
09-29 16:21:11.540171  1176  1185 D RmcNwHdlr: [0] handleSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 26, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 60, wcdma_ecno: 41, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:21:11.543815  1669  1669 D MTKSST  : [GsmSST0] new:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-61 ber=99 rscp=-60 ecno=-4 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}, old:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-61 ber=99 rscp=-60 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}
09-29 16:21:11.544755  1251  1557 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:11.544861  1251  1557 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:11.544893  1251  1557 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:11.546719  1251  1557 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:11.546922  1251  1557 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:11.546992  1251  1557 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:16.652344  1176  1184 I AT      : [0] AT< +ECSQ: 60,41,1,-243,-15,1,1,4,32767,1 (RIL_URC_READER, tid:493447834880)
09-29 16:21:16.908646  1176  1223 I RilClient: initialize: commandFd is 44
09-29 16:21:16.909562  1176  1223 I RilClient: start listen on fd: 30, socket name: rild-oem
09-29 16:21:16.910180  1176  1192 I RmcOemHandler: requestQueryThermal Enter: -1
09-29 16:21:16.910295  1176  1192 I AT      : [0] AT> AT+ETHERMAL (RIL_CMD_READER_1 tid:493439544576)
09-29 16:21:16.919237  1176  1191 I AT      : [0] AT< +ETHERMAL: 2, 32767, -127, 111, 32767, 4046 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:21:16.919328  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:21:16.919549  1176  1192 I RmcOemHandler: requestQueryThermal success
09-29 16:21:16.920318  1176  1182 D RtcRilClientController: client 1001 handle requestComplete
09-29 16:21:21.773903  1176  1184 I AT      : [0] AT< +ECSQ: 59,42,1,-247,-14,1,1,4,32767,1 (RIL_URC_READER, tid:493447834880)
09-29 16:21:21.775600  1176  1185 D RmcNwHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0X04]
09-29 16:21:21.775854  1176  1185 D RmcNwHdlr: [0] handleSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 25, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 59, wcdma_ecno: 42, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:21:21.782553  1669  1669 D MTKSST  : [GsmSST0] new:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-63 ber=99 rscp=-61 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}, old:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-61 ber=99 rscp=-60 ecno=-4 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}
09-29 16:21:21.783796  1251  2734 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:21.783965  1251  2734 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:21.784016  1251  2734 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:21.786304  1251  2734 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:21.786539  1251  2734 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:21.786644  1251  2734 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:25.380951  5201  5201 D SubscriptionManager: register OnSubscriptionsChangedListener pkgName=com.android.bluetooth listener=com.android.bluetooth.hfp.HeadsetPhoneState$HeadsetPhoneStateOnSubscriptionChangedListener@1b6f457
09-29 16:21:25.398041  1669  1686 D SubscriptionController: [getSlotIndex]- subId invalid
09-29 16:21:25.751351  1669  1686 E PhoneSubInfoController: getLine1Number phone is null for Subscription:-1
09-29 16:21:26.545421  1680  5305 D RatConfig: getMaxRat: initial Lf/Lt/W/G 29
09-29 16:21:26.895708  1176  1184 I AT      : [0] AT< +ECSQ: 57,43,1,-255,-12,1,1,4,32767,1 (RIL_URC_READER, tid:493447834880)
09-29 16:21:26.896961  1176  1185 D RmcNwHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0X04]
09-29 16:21:26.897045  1176  1185 D RmcNwHdlr: [0] handleSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 24, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 57, wcdma_ecno: 43, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:21:26.902613  1669  1669 D MTKSST  : [GsmSST0] new:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-65 ber=99 rscp=-63 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}, old:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-63 ber=99 rscp=-61 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}
09-29 16:21:26.903636  1251  4917 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:26.904332  1251  4917 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:26.904529  1251  4917 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:26.934903  1251  4917 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:26.934940  1251  4917 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:26.937017  1176  1192 I RmcOemHandler: requestQueryThermal Enter: -1
09-29 16:21:26.937133  1176  1192 I AT      : [0] AT> AT+ETHERMAL (RIL_CMD_READER_1 tid:493439544576)
09-29 16:21:26.950935  1176  1191 I AT      : [0] AT< +ETHERMAL: 2, 32767, -127, 196, 32767, 0 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:21:26.951043  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:21:26.954233  1176  1192 I RmcOemHandler: requestQueryThermal success
09-29 16:21:26.954655  1176  1182 D RtcRilClientController: client 1001 handle requestComplete
09-29 16:21:32.014806  1176  1184 I AT      : [0] AT< +ECSQ: 59,43,1,-245,-12,1,1,4,32767,1 (RIL_URC_READER, tid:493447834880)
09-29 16:21:32.015360  1176  1185 D RmcNwHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0X04]
09-29 16:21:32.015410  1176  1185 D RmcNwHdlr: [0] handleSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 25, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 59, wcdma_ecno: 43, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:21:32.019247  1669  1669 D MTKSST  : [GsmSST0] new:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-63 ber=99 rscp=-61 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}, old:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-65 ber=99 rscp=-63 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}
09-29 16:21:32.020321  1251  4918 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:32.020519  1251  4918 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:32.020608  1251  4918 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:32.022415  1251  4911 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:32.022519  1251  4911 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:32.022552  1251  4911 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:36.960582  1176  1223 I RilClient: initialize: commandFd is 44
09-29 16:21:36.961350  1176  1223 I RilClient: start listen on fd: 30, socket name: rild-oem
09-29 16:21:36.961889  1176  1192 I RmcOemHandler: requestQueryThermal Enter: -1
09-29 16:21:36.961982  1176  1192 I AT      : [0] AT> AT+ETHERMAL (RIL_CMD_READER_1 tid:493439544576)
09-29 16:21:36.971137  1176  1191 I AT      : [0] AT< +ETHERMAL: 2, 32767, -127, 196, 32767, 0 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:21:36.971459  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:21:36.971607  1176  1192 I RmcOemHandler: requestQueryThermal success
09-29 16:21:36.972092  1176  1182 D RtcRilClientController: client 1001 handle requestComplete
09-29 16:21:37.137209  1176  1184 I AT      : [0] AT< +ECSQ: 62,42,1,-234,-13,1,1,4,32767,1 (RIL_URC_READER, tid:493447834880)
09-29 16:21:37.137915  1176  1185 D RmcNwHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0X04]
09-29 16:21:37.137962  1176  1185 D RmcNwHdlr: [0] handleSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 27, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 62, wcdma_ecno: 42, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:21:37.141700  1669  1669 D MTKSST  : [GsmSST0] new:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-59 ber=99 rscp=-58 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}, old:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-63 ber=99 rscp=-61 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}
09-29 16:21:37.142417  1251  2246 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:37.142491  1251  2246 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:37.142521  1251  2246 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:37.144643  1251  2246 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:37.144747  1251  2246 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:37.144781  1251  2246 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:42.257949  1176  1184 I AT      : [0] AT< +ECSQ: 65,41,1,-224,-15,1,1,4,32767,1 (RIL_URC_READER, tid:493447834880)
09-29 16:21:42.258688  1176  1185 D RmcNwHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0X04]
09-29 16:21:42.258734  1176  1185 D RmcNwHdlr: [0] handleSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 28, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 65, wcdma_ecno: 41, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:21:42.261834  1669  1669 D MTKSST  : [GsmSST0] new:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-57 ber=99 rscp=-55 ecno=-4 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}, old:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-59 ber=99 rscp=-58 ecno=-3 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}
09-29 16:21:42.262642  1251  1269 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:42.262808  1251  1269 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:42.262901  1251  1269 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:42.264778  1251  1547 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:42.265007  1251  1547 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:42.265102  1251  1547 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:46.979380  1176  1223 I RilClient: initialize: commandFd is 67
09-29 16:21:46.980512  1176  1223 I RilClient: start listen on fd: 30, socket name: rild-oem
09-29 16:21:46.982599  1176  1192 I RmcOemHandler: requestQueryThermal Enter: -1
09-29 16:21:46.982781  1176  1192 I AT      : [0] AT> AT+ETHERMAL (RIL_CMD_READER_1 tid:493439544576)
09-29 16:21:46.993751  1176  1191 I AT      : [0] AT< +ETHERMAL: 2, 32767, -127, 196, 32767, 0 (RIL_CMD_READER_1, tid:493440580864)
09-29 16:21:46.993982  1176  1191 I AT      : [0] AT< OK (RIL_CMD_READER_1, tid:493440580864)
09-29 16:21:46.994385  1176  1192 I RmcOemHandler: requestQueryThermal success
09-29 16:21:46.995283  1176  1182 D RtcRilClientController: client 1001 handle requestComplete
09-29 16:21:47.380513  1176  1184 I AT      : [0] AT< +ECSQ: 66,41,1,-218,-16,1,1,4,32767,1 (RIL_URC_READER, tid:493447834880)
09-29 16:21:47.381747  1176  1185 D RmcNwHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0X04]
09-29 16:21:47.381836  1176  1185 D RmcNwHdlr: [0] handleSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 29, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 66, wcdma_ecno: 41, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:21:47.387074  1669  1669 D MTKSST  : [GsmSST0] new:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-55 ber=99 rscp=-54 ecno=-4 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}, old:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-57 ber=99 rscp=-55 ecno=-4 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}
09-29 16:21:47.388835  1251  1547 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:47.389139  1251  1547 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:47.389247  1251  1547 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:47.391499  1251  4911 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:47.391635  1251  4911 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:47.391785  1251  4911 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:52.499584  1176  1184 I AT      : [0] AT< +ECSQ: 68,41,1,-212,-15,1,1,4,32767,1 (RIL_URC_READER, tid:493447834880)
09-29 16:21:52.500308  1176  1185 D RmcNwHdlr: [0] requestSignalStrength:sigRegisted[0000], sigUpdated[0X04]
09-29 16:21:52.500383  1176  1185 D RmcNwHdlr: [0] handleSignalStrength, gsm_signal_strength: 99, gsm_bit_error_rate: 99, gsm_timing_advance: 2147483647, cdma_dbm: 2147483647, cdma_ecio: 2147483647, evdo_dbm: 2147483647, evdo_ecio: 2147483647, evdo_snr: 2147483647, lte_signal_strength: 99, lte_rsrp: 2147483647, lte_rsrq: 2147483647, lte_rssnr: 2147483647, lte_cqi: 2147483647, lte_timing_advance: 2147483647, tdscdma_signal_strength: 99, tdscdma_bit_error_rate: 99, tdscdma_rscp: 255, wcdma_signal_strength: 30, wcdma_bit_error_rate: 99, wcdma_scdma_rscp: 68, wcdma_ecno: 41, ssRsrp: 2147483647, ssRsrq: 2147483647, ssSinr: 2147483647, csiRsrp: 2147483647, csiRsrq: 2147483647, csiSinr: 2147483647
09-29 16:21:52.503600  1669  1669 D MTKSST  : [GsmSST0] new:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-53 ber=99 rscp=-52 ecno=-4 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}, old:{level:4, raw:SignalStrength:{mCdma=CellSignalStrengthCdma: cdmaDbm=2147483647 cdmaEcio=2147483647 evdoDbm=2147483647 evdoEcio=2147483647 evdoSnr=2147483647 level=0,mGsm=CellSignalStrengthGsm: rssi=2147483647 ber=2147483647 mTa=2147483647 mLevel=0,mWcdma=CellSignalStrengthWcdma: ss=-55 ber=99 rscp=-54 ecno=-4 level=4,mTdscdma=CellSignalStrengthTdscdma: rssi=2147483647 ber=2147483647 rscp=2147483647 level=0,mLte=CellSignalStrengthLte: rssi=2147483647 rsrp=2147483647 rsrq=2147483647 rssnr=2147483647 cqiTableIndex=2147483647 cqi=2147483647 ta=2147483647 level=0 parametersUseForLevel=1,mNr=CellSignalStrengthNr:{ csiRsrp = 2147483647 csiRsrq = 2147483647 csiCqiTableIndex = 2147483647 csiCqiReport = [] ssRsrp = 2147483647 ssRsrq = 2147483647 ssSinr = 2147483647 level = 0 parametersUseForLevel = 1 },primary=CellSignalStrengthWcdma}, phoneId=0, mMtkLevel=0, mMtkRsrpOnly=true, mMtkLteRsrpThreshold=null, mMtkLteRssnrThreshold=null}
09-29 16:21:52.504845  1251  2734 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:52.505049  1251  2734 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:52.505129  1251  2734 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=-1, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:52.507012  1251  4918 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:52.507108  1251  4918 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
09-29 16:21:52.507166  1251  4918 D MtkTelephonyRegistryEx: idMatchEx: rSubId=2147483647, subId=2147483646, dSubId=-1, rPhoneId=-1, phoneId=0
