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BT Qualification and Listing Requirements Form
V1.3.3
	A. Applicant information

	Company Name:
	     

	Company Address:
	     

	Contact Person:
	     

	TEL:
	     

	Email Address:
	     

	Website:
	     

	Bluetooth.org(SIG log in)
	Member ID:                    Member P/W:             



	B. Manufacture information

	Same as Applicant
	|X|

	Company Name:
	     

	Company Address:
	     

	Contact Person:
	     

	TEL:
	     

	Email Address:
	     

	Website:
	     



	[bookmark: OLE_LINK15][bookmark: OLE_LINK16]C. Product Information

	[bookmark: OLE_LINK29][bookmark: OLE_LINK30]The Bluetooth design/product will be a/an:
	|X| End Product  
[bookmark: OLE_LINK10][bookmark: OLE_LINK11][bookmark: OLE_LINK12]|X| Subsystem (Please Select)
|X| Component

	Brand Name:
	     

	Product Name:
	FC3

	Product Model:
	SL1

	Series Model:
	     

	HW version:
	V61

	SW version:
	fw-ble-v1.0

	Product Description:
	The FC3 is a connected wearable IoT device.

	Core Specification
	4.2
	Product Category
	Unique Products


Note: \ / * = $ ( ) @ # : , ; “ ‘ < > are not allowed to use in Product Name and Product Model.




	D. Listing/Publish Date

	Listing Date
	Please Select a date


	Publish Date
	Please Select a date




	E. List of Bluetooth Core Protocols Supported

	BR/EDR Core Controller:
	|X| RF    |X| BB     |X| LMP   

	LE Controller:
	|X| RF-PHY    |X| LL    |X| IAL

	Host Controller Interface:
	|X| HCI   |X| 4.0 HCI

	Host Protocol
	|X| L2CAP |X| SDP  |X| GAP |X| ATT |X| GATT |X| SM



	F. List of Bluetooth Protocols And Profiles Supported

	◆RFCOMM：Version
	|X|RFCOMM

	◆A2DP：Version
	|X| Source (SRC)	|X| Sink (SNK)
Note: Both AVDTP and GAVDP shall be supported

	◆AVCTP：Version
	|X| Controller (CT)	|X| Target (TG)

	◆AVDTP：Version
	|X| Source	|X| Sink	  |X| Initiator	   |X| Acceptor 

	◆GAVDP：Version
	|X| Initiator	|X| Acceptor

	◆AVRCP：Version
	|X| Controller  |X| Target    Note: AVCTP shall be supported

	◆DUN：Version
	|X| Gateway (GW)	|X| Data Terminal (DT)

	◆DID：Version
	|X| DID

	◆FTP：Version
	|X| File Transfer Server  |X| File Transfer Client

	◆MCAP
	|X| Supports Source Role      |X| Supports Sink Role 
|X| Supports Sync-Slave Role  |X| Supports Sync-Master Role

	◆HDP：Version
	|X| Source    |X| Sink    Note: MCAP shall be supported

	◆HFP：Version
	|X| Audio Gateway (AG)   |X| Heads-Free (HF)
Note: SPP shall be supported

	◆HID：Version
	|X| Host, Report protocol  |X| HID Role  |X| Host, Boot protocol

	◆HID1.1：Version
	|X| General HID Host, Report protocol  
|X| Limited HID Host, Report protocol  
|X| Limited HID Host, Boot protocol
|X| HID Device Role

	◆HSP：Version
	|X| Audio Gateway (AG)  |X| Headset (HS)
Note: SPP shall be supported

	◆IOP
	|X| IOP

	◆MAP：Version
	|X| Messaging Server Equipment (MSE) 
|X| Messaging Client Equipment (MCE)

	◆OPP：Version
	|X| Object Push Client	|X| Object Push Server

	◆BNEP :
	|X| BNEP

	◆PAN：Version
	|X| Network Access Point (NAP) |_|	Group Ad-hoc Network (GN)
|X| PAN User (PANU)    Note: BNEP shall be supported

	◆PBAP：Version
	|X| Phone Book Server Equipment (PSE)
|X| Phone Book Client Equipment (PCE)

	◆SAP：Version
	|X| SIM Access Server (Server) |X| SIM Access Client (Client)

	◆SPP：Version
	|X| Device A (DevA) 	|X| Device B (DevB)
Note: RFCOMM shall be supported

	[bookmark: Check60][bookmark: OLE_LINK1][bookmark: OLE_LINK2]◆Others : 
	[bookmark: OLE_LINK3][bookmark: OLE_LINK4][bookmark: OLE_LINK5]|X|               



	G. List of Bluetooth GATT-Based service And Profiles Supported

	◆ANP    
	|X| Alert Notification Server  |X|Alert Notification Client

	◆ANS    
	|X| ANS

	◆BAS
	|X| BAS

	◆BLP
	|X| Blood Pressure Sensor (Server)  |X| Blood Pressure Collector (Client)

	◆BLS
	|X| BLS

	◆CPP   
	|X| CP Sensor |X| Collector |X| CP Observer |X| CP Broadcaster 

	◆CPS   
	|X| CPS

	◆CSCP
	|X| CSC Sensor (Server)  |X| CSC Sensor (Client) 

	◆CSCS
	|X| CSCS

	◆CTS
	|X| CTS

	◆DIS
	|X| DIS

	◆FMP
	|X| Find Me Target (Server)  |X| Find Me Locator (Client)

	◆GLS
	|X| GLS

	◆GLP
	|X| Glucose Sensor (Server)  |X| Glucose Collector (Client)

	◆HTP
	|X| Thermometer (Server)  |X| Collector (Client)

	◆HTS
	|X| HTS

	◆HRP
	|X| Heart Rate Sensor (Server)  |X| Heart Rate Collector (Client)

	◆HRS
	|X| HRS

	◆HOGP  
	|X| HID Device (Server)  |X| Report Host (Client) |X| Boot Host (Client)

	◆HIDS
	|X| HIDS

	◆IAS
	|X| IAS

	◆LNP
	|X| LN Sensor  |X| Collector

	◆LNS
	|X| LNS

	◆LLS
	|X| LLS

	◆NDCS
	|X| NDCS

	◆PASP
	|X| Phone Alert Status Server  |X| Phone Alert Status Client

	◆PASS
	|X| PASS

	◆PXP
	|X| Proximity Reporter (Server) |X|  Proximity Monitor (Client)

	◆RSCP
	|X| RSC Sensor (Server)  |X| Collector (Client)

	◆RSCS
	|X| RSCS

	◆ScPP
	|X| Scan Server  |X| Scan Client

	◆ScPS
	|X| Scan Service

	◆Others 
	|X|               



	H. List of applicable Qualified Pre-tested Components

	QDID No.
	Model
	Manufacturer

	   187856  
	      nRF52840         
	        Nordic Semiconductor       

	   188441  
	[bookmark: _GoBack]      nRF52840       
	             Nordic Semiconductor  

	     
	               
	               

	     
	               
	               



Bureau Veritas Shenzhen Co., Ltd., Dongguan Branch 
No. 96, Guantai Road (Houjie Section), Houjie Town, Dongguan City, Guangdong,China
Tel.: + 86-769 89982098

image1.jpeg




