ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x16ed
  Start of program headers:          52 (bytes into file)
  Start of section headers:          1127836 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         4
  Size of section headers:           40 (bytes)
  Number of section headers:         28
  Section header string table index: 27

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        00000000 0000c0 000100 00 WAX  0   0  4
  [ 2] text              PROGBITS        00000100 0001c0 007308 00  AX  0   0  4
  [ 3] .ARM.exidx        ARM_EXIDX       00007408 0074c8 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        00007410 0074d0 000068 00   A  0   0  4
  [ 5] devices           PROGBITS        00007478 007538 0000d8 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        00007550 007610 000180 00  WA  0   0  4
  [ 7] zephyr_dbg_info   PROGBITS        000076d0 007790 00003c 00  WA  0   0  4
  [ 8] device_handles    PROGBITS        0000770c 0077cc 000042 00   A  0   0  2
  [ 9] rodata            PROGBITS        00007750 007810 00026c 00   A  0   0 16
  [10] .ramfunc          PROGBITS        20000000 007c40 000000 00   W  0   0  1
  [11] datas             PROGBITS        20000000 007a7c 0001a0 00  WA  0   0  4
  [12] device_states     PROGBITS        200001a0 007c1c 000024 00  WA  0   0  4
  [13] bss               NOBITS          200001c8 007c48 00091b 00  WA  0   0  8
  [14] noinit            NOBITS          20000b00 007c48 0011c0 00  WA  0   0 32
  [15] .comment          PROGBITS        00000000 007c40 000079 01  MS  0   0  1
  [16] .debug_aranges    PROGBITS        00000000 007cc0 001920 00      0   0  8
  [17] .debug_info       PROGBITS        00000000 0095e0 087e79 00      0   0  1
  [18] .debug_abbrev     PROGBITS        00000000 091459 00d6c7 00      0   0  1
  [19] .debug_line       PROGBITS        00000000 09eb20 02a74a 00      0   0  1
  [20] .debug_frame      PROGBITS        00000000 0c926c 003d5c 00      0   0  4
  [21] .debug_str        PROGBITS        00000000 0ccfc8 00cca1 01  MS  0   0  1
  [22] .debug_loc        PROGBITS        00000000 0d9c69 0284c3 00      0   0  1
  [23] .debug_ranges     PROGBITS        00000000 102130 005158 00      0   0  8
  [24] .ARM.attributes   ARM_ATTRIBUTES  00000000 107288 000033 00      0   0  1
  [25] .symtab           SYMTAB          00000000 1072bc 006e00 10     26 1033  4
  [26] .strtab           STRTAB          00000000 10e0bc 0053be 00      0   0  1
  [27] .shstrtab         STRTAB          00000000 11347a 000121 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x0074c8 0x00007408 0x00007408 0x00008 0x00008 R   0x4
  LOAD           0x0000c0 0x00000000 0x00000000 0x079bc 0x079bc RWE 0x10
  LOAD           0x007a7c 0x20000000 0x000079bc 0x001c4 0x001c4 RW  0x4
  LOAD           0x007c48 0x200001c8 0x200001c8 0x00000 0x01af8 RW  0x20

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel devices sw_isr_table zephyr_dbg_info device_handles rodata 
   02     datas device_states 
   03     bss noinit 
