Component: ARM Compiler 5.06 update 6 (build 750) Tool: armlink [4d35ed]

==============================================================================

Section Cross References

    main.o(i.assert_nrf_callback) refers to app_error_handler_keil.o(.emb_text) for app_error_handler
    main.o(i.ble_evt_handler) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_0) for nrf_log_frontend_std_0
    main.o(i.ble_evt_handler) refers to bsp.o(i.bsp_indication_set) for bsp_indication_set
    main.o(i.ble_evt_handler) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.ble_evt_handler) refers to nrf_ble_qwr.o(i.nrf_ble_qwr_conn_handle_assign) for nrf_ble_qwr_conn_handle_assign
    main.o(i.ble_evt_handler) refers to main.o(.data) for .data
    main.o(i.ble_evt_handler) refers to nrf_log_frontend.o(log_const_data) for m_nrf_log_app_logs_data_const
    main.o(i.ble_evt_handler) refers to main.o(.bss) for .bss
    main.o(i.bsp_event_handler) refers to bsp.o(i.bsp_indication_set) for bsp_indication_set
    main.o(i.bsp_event_handler) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.bsp_event_handler) refers to bsp_btn_ble.o(i.bsp_btn_ble_sleep_mode_prepare) for bsp_btn_ble_sleep_mode_prepare
    main.o(i.bsp_event_handler) refers to ble_advertising.o(i.ble_advertising_restart_without_whitelist) for ble_advertising_restart_without_whitelist
    main.o(i.bsp_event_handler) refers to main.o(.data) for .data
    main.o(i.bsp_event_handler) refers to main.o(.bss) for .bss
    main.o(i.conn_params_error_handler) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.gatt_evt_handler) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_2) for nrf_log_frontend_std_2
    main.o(i.gatt_evt_handler) refers to main.o(.data) for .data
    main.o(i.gatt_evt_handler) refers to nrf_log_frontend.o(log_const_data) for m_nrf_log_app_logs_data_const
    main.o(i.gatt_init) refers to nrf_ble_gatt.o(i.nrf_ble_gatt_init) for nrf_ble_gatt_init
    main.o(i.gatt_init) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.gatt_init) refers to nrf_ble_gatt.o(i.nrf_ble_gatt_att_mtu_periph_set) for nrf_ble_gatt_att_mtu_periph_set
    main.o(i.gatt_init) refers to main.o(i.gatt_evt_handler) for gatt_evt_handler
    main.o(i.gatt_init) refers to main.o(.bss) for .bss
    main.o(i.main) refers to memcpya.o(.text) for __aeabi_memcpy4
    main.o(i.main) refers to app_uart_fifo.o(i.app_uart_init) for app_uart_init
    main.o(i.main) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.main) refers to nrf_log_frontend.o(i.nrf_log_init) for nrf_log_init
    main.o(i.main) refers to nrf_log_default_backends.o(i.nrf_log_default_backends_init) for nrf_log_default_backends_init
    main.o(i.main) refers to app_timer.o(i.app_timer_init) for app_timer_init
    main.o(i.main) refers to bsp.o(i.bsp_init) for bsp_init
    main.o(i.main) refers to bsp_btn_ble.o(i.bsp_btn_ble_init) for bsp_btn_ble_init
    main.o(i.main) refers to nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_init) for nrf_pwr_mgmt_init
    main.o(i.main) refers to nrf_sdh.o(i.nrf_sdh_enable_request) for nrf_sdh_enable_request
    main.o(i.main) refers to nrf_sdh_ble.o(i.nrf_sdh_ble_default_cfg_set) for nrf_sdh_ble_default_cfg_set
    main.o(i.main) refers to nrf_sdh_ble.o(i.nrf_sdh_ble_enable) for nrf_sdh_ble_enable
    main.o(i.main) refers to main.o(i.gatt_init) for gatt_init
    main.o(i.main) refers to nrf_ble_qwr.o(i.nrf_ble_qwr_init) for nrf_ble_qwr_init
    main.o(i.main) refers to ble_nus.o(i.ble_nus_init) for ble_nus_init
    main.o(i.main) refers to memseta.o(.text) for __aeabi_memclr4
    main.o(i.main) refers to ble_advertising.o(i.ble_advertising_init) for ble_advertising_init
    main.o(i.main) refers to ble_advertising.o(i.ble_advertising_conn_cfg_tag_set) for ble_advertising_conn_cfg_tag_set
    main.o(i.main) refers to ble_conn_params.o(i.ble_conn_params_init) for ble_conn_params_init
    main.o(i.main) refers to main.o(i.saadc_init) for saadc_init
    main.o(i.main) refers to main.o(i.saadc_sampling_event_init) for saadc_sampling_event_init
    main.o(i.main) refers to main.o(i.saadc_sampling_event_enable) for saadc_sampling_event_enable
    main.o(i.main) refers to printfa.o(i.__0printf) for __2printf
    main.o(i.main) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_0) for nrf_log_frontend_std_0
    main.o(i.main) refers to ble_advertising.o(i.ble_advertising_start) for ble_advertising_start
    main.o(i.main) refers to nrf_log_frontend.o(i.nrf_log_frontend_dequeue) for nrf_log_frontend_dequeue
    main.o(i.main) refers to nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_run) for nrf_pwr_mgmt_run
    main.o(i.main) refers to main.o(.constdata) for .constdata
    main.o(i.main) refers to main.o(.bss) for .bss
    main.o(i.main) refers to main.o(i.uart_event_handle) for uart_event_handle
    main.o(i.main) refers to main.o(i.bsp_event_handler) for bsp_event_handler
    main.o(i.main) refers to main.o(i.nrf_qwr_error_handler) for nrf_qwr_error_handler
    main.o(i.main) refers to main.o(i.nus_data_handler) for nus_data_handler
    main.o(i.main) refers to main.o(.data) for .data
    main.o(i.main) refers to main.o(i.on_adv_evt) for on_adv_evt
    main.o(i.main) refers to main.o(i.on_conn_params_evt) for on_conn_params_evt
    main.o(i.main) refers to main.o(i.conn_params_error_handler) for conn_params_error_handler
    main.o(i.main) refers to nrf_log_frontend.o(log_const_data) for m_nrf_log_app_logs_data_const
    main.o(i.nrf_qwr_error_handler) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.nus_data_handler) refers to app_uart_fifo.o(i.app_uart_put) for app_uart_put
    main.o(i.nus_data_handler) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_1) for nrf_log_frontend_std_1
    main.o(i.nus_data_handler) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.nus_data_handler) refers to main.o(.data) for .data
    main.o(i.nus_data_handler) refers to nrf_log_frontend.o(log_const_data) for m_nrf_log_app_logs_data_const
    main.o(i.on_adv_evt) refers to bsp.o(i.bsp_indication_set) for bsp_indication_set
    main.o(i.on_adv_evt) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.on_adv_evt) refers to printfa.o(i.__0printf) for __2printf
    main.o(i.on_conn_params_evt) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.on_conn_params_evt) refers to main.o(.data) for .data
    main.o(i.saadc_callback) refers to printfa.o(i.__0printf) for __2printf
    main.o(i.saadc_callback) refers to memseta.o(.text) for __aeabi_memclr4
    main.o(i.saadc_callback) refers to nrfx_saadc.o(i.nrfx_saadc_buffer_convert) for nrfx_saadc_buffer_convert
    main.o(i.saadc_callback) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.saadc_callback) refers to f2d.o(.text) for __aeabi_f2d
    main.o(i.saadc_callback) refers to printfa.o(i.__0sprintf) for __2sprintf
    main.o(i.saadc_callback) refers to strcat.o(.text) for strcat
    main.o(i.saadc_callback) refers to strcpy.o(.text) for strcpy
    main.o(i.saadc_callback) refers to ble_nus.o(i.ble_nus_data_send) for ble_nus_data_send
    main.o(i.saadc_callback) refers to main.o(.data) for .data
    main.o(i.saadc_callback) refers to main.o(.bss) for .bss
    main.o(i.saadc_init) refers to nrfx_saadc.o(i.nrfx_saadc_init) for nrfx_saadc_init
    main.o(i.saadc_init) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.saadc_init) refers to nrfx_saadc.o(i.nrfx_saadc_channel_init) for nrfx_saadc_channel_init
    main.o(i.saadc_init) refers to nrfx_saadc.o(i.nrfx_saadc_buffer_convert) for nrfx_saadc_buffer_convert
    main.o(i.saadc_init) refers to main.o(.constdata) for .constdata
    main.o(i.saadc_init) refers to main.o(i.saadc_callback) for saadc_callback
    main.o(i.saadc_init) refers to main.o(.data) for .data
    main.o(i.saadc_sampling_event_enable) refers to nrfx_ppi.o(i.nrfx_ppi_channel_enable) for nrfx_ppi_channel_enable
    main.o(i.saadc_sampling_event_enable) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.saadc_sampling_event_enable) refers to main.o(.data) for .data
    main.o(i.saadc_sampling_event_init) refers to nrf_drv_ppi.o(i.nrf_drv_ppi_init) for nrf_drv_ppi_init
    main.o(i.saadc_sampling_event_init) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.saadc_sampling_event_init) refers to nrfx_timer.o(i.nrfx_timer_init) for nrfx_timer_init
    main.o(i.saadc_sampling_event_init) refers to llushr.o(.text) for __aeabi_llsr
    main.o(i.saadc_sampling_event_init) refers to nrfx_timer.o(i.nrfx_timer_extended_compare) for nrfx_timer_extended_compare
    main.o(i.saadc_sampling_event_init) refers to nrfx_timer.o(i.nrfx_timer_enable) for nrfx_timer_enable
    main.o(i.saadc_sampling_event_init) refers to nrfx_saadc.o(i.nrfx_saadc_sample_task_get) for nrfx_saadc_sample_task_get
    main.o(i.saadc_sampling_event_init) refers to nrfx_ppi.o(i.nrfx_ppi_channel_alloc) for nrfx_ppi_channel_alloc
    main.o(i.saadc_sampling_event_init) refers to nrfx_ppi.o(i.nrfx_ppi_channel_assign) for nrfx_ppi_channel_assign
    main.o(i.saadc_sampling_event_init) refers to main.o(.constdata) for .constdata
    main.o(i.saadc_sampling_event_init) refers to main.o(i.timer_handler) for timer_handler
    main.o(i.saadc_sampling_event_init) refers to main.o(.data) for .data
    main.o(i.uart_event_handle) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.uart_event_handle) refers to app_uart_fifo.o(i.app_uart_get) for app_uart_get
    main.o(i.uart_event_handle) refers to ble_nus.o(i.ble_nus_data_send) for ble_nus_data_send
    main.o(i.uart_event_handle) refers to main.o(.bss) for .bss
    main.o(i.uart_event_handle) refers to main.o(.data) for .data
    main.o(.data) refers to main.o(.data) for m_nus_link_ctx_storage
    main.o(.data) refers to main.o(.data) for m_nus_link_ctx_storage_ctx_data_pool
    main.o(sdh_ble_observers1) refers to nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) for nrf_ble_gatt_on_ble_evt
    main.o(sdh_ble_observers1) refers to main.o(.bss) for m_gatt
    main.o(sdh_ble_observers1) refers to ble_advertising.o(i.ble_advertising_on_ble_evt) for ble_advertising_on_ble_evt
    main.o(sdh_ble_observers2) refers to ble_nus.o(i.ble_nus_on_ble_evt) for ble_nus_on_ble_evt
    main.o(sdh_ble_observers2) refers to main.o(.data) for m_nus
    main.o(sdh_ble_observers2) refers to nrf_ble_qwr.o(i.nrf_ble_qwr_on_ble_evt) for nrf_ble_qwr_on_ble_evt
    main.o(sdh_ble_observers2) refers to main.o(.bss) for m_qwr
    main.o(sdh_ble_observers3) refers to main.o(i.ble_evt_handler) for ble_evt_handler
    main.o(sdh_soc_observers1) refers to ble_advertising.o(i.ble_advertising_on_sys_evt) for ble_advertising_on_sys_evt
    main.o(sdh_soc_observers1) refers to main.o(.bss) for m_advertising
    boards.o(i.bsp_board_button_idx_to_pin) refers to boards.o(.constdata) for .constdata
    boards.o(i.bsp_board_button_state_get) refers to boards.o(.constdata) for .constdata
    boards.o(i.bsp_board_init) refers to boards.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    boards.o(i.bsp_board_init) refers to boards.o(i.bsp_board_leds_off) for bsp_board_leds_off
    boards.o(i.bsp_board_init) refers to boards.o(.constdata) for .constdata
    boards.o(i.bsp_board_led_idx_to_pin) refers to boards.o(.constdata) for .constdata
    boards.o(i.bsp_board_led_invert) refers to boards.o(.constdata) for .constdata
    boards.o(i.bsp_board_led_off) refers to boards.o(i.nrf_gpio_pin_write) for nrf_gpio_pin_write
    boards.o(i.bsp_board_led_off) refers to boards.o(.constdata) for .constdata
    boards.o(i.bsp_board_led_on) refers to boards.o(i.nrf_gpio_pin_write) for nrf_gpio_pin_write
    boards.o(i.bsp_board_led_on) refers to boards.o(.constdata) for .constdata
    boards.o(i.bsp_board_led_state_get) refers to boards.o(.constdata) for .constdata
    boards.o(i.bsp_board_leds_off) refers to boards.o(i.bsp_board_led_off) for bsp_board_led_off
    boards.o(i.bsp_board_leds_on) refers to boards.o(i.bsp_board_led_on) for bsp_board_led_on
    boards.o(i.bsp_board_pin_to_button_idx) refers to boards.o(.constdata) for .constdata
    boards.o(i.bsp_board_pin_to_led_idx) refers to boards.o(.constdata) for .constdata
    bsp.o(i.alert_timer_handler) refers to boards.o(i.bsp_board_led_invert) for bsp_board_led_invert
    bsp.o(i.bsp_button_event_handler) refers to boards.o(i.bsp_board_pin_to_button_idx) for bsp_board_pin_to_button_idx
    bsp.o(i.bsp_button_event_handler) refers to app_timer.o(i.app_timer_start) for app_timer_start
    bsp.o(i.bsp_button_event_handler) refers to app_timer.o(i.app_timer_stop) for app_timer_stop
    bsp.o(i.bsp_button_event_handler) refers to bsp.o(.constdata) for .constdata
    bsp.o(i.bsp_button_event_handler) refers to bsp.o(.data) for .data
    bsp.o(i.bsp_button_event_handler) refers to bsp.o(.bss) for .bss
    bsp.o(i.bsp_button_is_pressed) refers to boards.o(i.bsp_board_button_state_get) for bsp_board_button_state_get
    bsp.o(i.bsp_buttons_disable) refers to app_button.o(i.app_button_disable) for app_button_disable
    bsp.o(i.bsp_buttons_enable) refers to app_button.o(i.app_button_enable) for app_button_enable
    bsp.o(i.bsp_event_to_button_action_assign) refers to bsp.o(.bss) for .bss
    bsp.o(i.bsp_indication_set) refers to bsp.o(i.bsp_led_indication) for bsp_led_indication
    bsp.o(i.bsp_indication_set) refers to bsp.o(.data) for .data
    bsp.o(i.bsp_init) refers to bsp.o(i.bsp_event_to_button_action_assign) for bsp_event_to_button_action_assign
    bsp.o(i.bsp_init) refers to app_button.o(i.app_button_init) for app_button_init
    bsp.o(i.bsp_init) refers to app_button.o(i.app_button_enable) for app_button_enable
    bsp.o(i.bsp_init) refers to app_timer.o(i.app_timer_create) for app_timer_create
    bsp.o(i.bsp_init) refers to boards.o(i.bsp_board_init) for bsp_board_init
    bsp.o(i.bsp_init) refers to bsp.o(.data) for .data
    bsp.o(i.bsp_init) refers to bsp.o(.constdata) for .constdata
    bsp.o(i.bsp_init) refers to bsp.o(i.button_timer_handler) for button_timer_handler
    bsp.o(i.bsp_init) refers to bsp.o(i.leds_timer_handler) for leds_timer_handler
    bsp.o(i.bsp_init) refers to bsp.o(i.alert_timer_handler) for alert_timer_handler
    bsp.o(i.bsp_led_indication) refers to bsp.o(i.leds_off) for leds_off
    bsp.o(i.bsp_led_indication) refers to app_timer.o(i.app_timer_stop) for app_timer_stop
    bsp.o(i.bsp_led_indication) refers to boards.o(i.bsp_board_led_state_get) for bsp_board_led_state_get
    bsp.o(i.bsp_led_indication) refers to boards.o(i.bsp_board_led_off) for bsp_board_led_off
    bsp.o(i.bsp_led_indication) refers to boards.o(i.bsp_board_led_on) for bsp_board_led_on
    bsp.o(i.bsp_led_indication) refers to uldiv.o(.text) for __aeabi_uldivmod
    bsp.o(i.bsp_led_indication) refers to app_timer.o(i.app_timer_start) for app_timer_start
    bsp.o(i.bsp_led_indication) refers to boards.o(i.bsp_board_led_invert) for bsp_board_led_invert
    bsp.o(i.bsp_led_indication) refers to boards.o(i.bsp_board_leds_on) for bsp_board_leds_on
    bsp.o(i.bsp_led_indication) refers to bsp.o(.data) for .data
    bsp.o(i.bsp_led_indication) refers to bsp.o(.constdata) for .constdata
    bsp.o(i.bsp_wakeup_button_disable) refers to bsp.o(i.wakeup_button_cfg) for wakeup_button_cfg
    bsp.o(i.bsp_wakeup_button_enable) refers to bsp.o(i.wakeup_button_cfg) for wakeup_button_cfg
    bsp.o(i.button_timer_handler) refers to bsp.o(i.bsp_button_event_handler) for bsp_button_event_handler
    bsp.o(i.leds_off) refers to boards.o(i.bsp_board_led_off) for bsp_board_led_off
    bsp.o(i.leds_off) refers to boards.o(i.bsp_board_leds_off) for bsp_board_leds_off
    bsp.o(i.leds_off) refers to bsp.o(.data) for .data
    bsp.o(i.leds_timer_handler) refers to bsp.o(i.bsp_led_indication) for bsp_led_indication
    bsp.o(i.leds_timer_handler) refers to bsp.o(.data) for .data
    bsp.o(i.wakeup_button_cfg) refers to boards.o(i.bsp_board_button_idx_to_pin) for bsp_board_button_idx_to_pin
    bsp.o(.constdata) refers to bsp.o(.bss) for m_bsp_leds_tmr_data
    bsp.o(.constdata) refers to bsp.o(.bss) for m_bsp_alert_tmr_data
    bsp.o(.constdata) refers to bsp.o(.bss) for m_bsp_button_tmr_data
    bsp.o(.constdata) refers to bsp.o(i.bsp_button_event_handler) for bsp_button_event_handler
    bsp_btn_ble.o(i.advertising_buttons_configure) refers to bsp.o(i.bsp_event_to_button_action_assign) for bsp_event_to_button_action_assign
    bsp_btn_ble.o(i.ble_evt_handler) refers to bsp_btn_ble.o(i.advertising_buttons_configure) for advertising_buttons_configure
    bsp_btn_ble.o(i.ble_evt_handler) refers to bsp.o(i.bsp_event_to_button_action_assign) for bsp_event_to_button_action_assign
    bsp_btn_ble.o(i.ble_evt_handler) refers to bsp_btn_ble.o(.data) for .data
    bsp_btn_ble.o(i.bsp_btn_ble_init) refers to bsp.o(i.bsp_button_is_pressed) for bsp_button_is_pressed
    bsp_btn_ble.o(i.bsp_btn_ble_init) refers to bsp_btn_ble.o(i.advertising_buttons_configure) for advertising_buttons_configure
    bsp_btn_ble.o(i.bsp_btn_ble_init) refers to bsp_btn_ble.o(.data) for .data
    bsp_btn_ble.o(i.bsp_btn_ble_sleep_mode_prepare) refers to bsp.o(i.bsp_wakeup_button_enable) for bsp_wakeup_button_enable
    bsp_btn_ble.o(sdh_ble_observers1) refers to bsp_btn_ble.o(i.ble_evt_handler) for ble_evt_handler
    utf.o(i.utf16RuneCount) refers to utf.o(i.utf16DecodeRune) for utf16DecodeRune
    utf.o(i.utf16UTF8Count) refers to utf.o(i.utf16DecodeRune) for utf16DecodeRune
    utf.o(i.utf16UTF8Count) refers to utf.o(i.utf8EncodeRune) for utf8EncodeRune
    utf.o(i.utf8RuneCount) refers to utf.o(i.utf8DecodeRune) for utf8DecodeRune
    utf.o(i.utf8UTF16Count) refers to utf.o(i.utf8DecodeRune) for utf8DecodeRune
    utf.o(i.utf8UTF16Count) refers to utf.o(i.utf16EncodeRune) for utf16EncodeRune
    ble_advdata.o(i.ble_advdata_appearance_find) refers to ble_advdata.o(i.ble_advdata_search) for ble_advdata_search
    ble_advdata.o(i.ble_advdata_encode) refers to ble_advdata.o(i.ble_device_addr_encode) for ble_device_addr_encode
    ble_advdata.o(i.ble_advdata_encode) refers to ble_advdata.o(i.uint16_encode) for uint16_encode
    ble_advdata.o(i.ble_advdata_encode) refers to ble_advdata.o(i.uuid_list_encode) for uuid_list_encode
    ble_advdata.o(i.ble_advdata_encode) refers to ble_advdata.o(i.conn_int_encode) for conn_int_encode
    ble_advdata.o(i.ble_advdata_encode) refers to ble_advdata.o(i.manuf_specific_data_encode) for manuf_specific_data_encode
    ble_advdata.o(i.ble_advdata_encode) refers to ble_advdata.o(i.service_data_encode) for service_data_encode
    ble_advdata.o(i.ble_advdata_encode) refers to ble_advdata.o(i.name_encode) for name_encode
    ble_advdata.o(i.ble_advdata_name_find) refers to ble_advdata.o(i.ble_advdata_search) for ble_advdata_search
    ble_advdata.o(i.ble_advdata_name_find) refers to strlen.o(.text) for strlen
    ble_advdata.o(i.ble_advdata_name_find) refers to memcmp.o(.text) for memcmp
    ble_advdata.o(i.ble_advdata_parse) refers to ble_advdata.o(i.ble_advdata_search) for ble_advdata_search
    ble_advdata.o(i.ble_advdata_short_name_find) refers to ble_advdata.o(i.ble_advdata_search) for ble_advdata_search
    ble_advdata.o(i.ble_advdata_short_name_find) refers to strlen.o(.text) for strlen
    ble_advdata.o(i.ble_advdata_short_name_find) refers to memcmp.o(.text) for memcmp
    ble_advdata.o(i.ble_advdata_uuid_find) refers to ble_advdata.o(i.ble_advdata_search) for ble_advdata_search
    ble_advdata.o(i.ble_advdata_uuid_find) refers to memcmp.o(.text) for memcmp
    ble_advdata.o(i.conn_int_encode) refers to ble_advdata.o(i.uint16_encode) for uint16_encode
    ble_advdata.o(i.manuf_specific_data_encode) refers to ble_advdata.o(i.uint16_encode) for uint16_encode
    ble_advdata.o(i.manuf_specific_data_encode) refers to memcpya.o(.text) for __aeabi_memcpy
    ble_advdata.o(i.service_data_encode) refers to ble_advdata.o(i.uint16_encode) for uint16_encode
    ble_advdata.o(i.service_data_encode) refers to memcpya.o(.text) for __aeabi_memcpy
    ble_advdata.o(i.uuid_list_encode) refers to ble_advdata.o(i.uuid_list_sized_encode) for uuid_list_sized_encode
    ble_advertising.o(i.ble_advertising_init) refers to memcpya.o(.text) for __aeabi_memcpy4
    ble_advertising.o(i.ble_advertising_init) refers to ble_advdata.o(i.ble_advdata_encode) for ble_advdata_encode
    ble_advertising.o(i.ble_advertising_modes_config_set) refers to memcpya.o(.text) for __aeabi_memcpy4
    ble_advertising.o(i.ble_advertising_on_ble_evt) refers to ble_advertising.o(i.ble_advertising_start) for ble_advertising_start
    ble_advertising.o(i.ble_advertising_restart_without_whitelist) refers to ble_advertising.o(i.flags_set) for flags_set
    ble_advertising.o(i.ble_advertising_restart_without_whitelist) refers to ble_advertising.o(i.ble_advertising_start) for ble_advertising_start
    ble_advertising.o(i.ble_advertising_start) refers to memseta.o(.text) for __aeabi_memclr4
    ble_advertising.o(i.ble_advertising_start) refers to ble_advertising.o(i.phy_is_valid) for phy_is_valid
    ble_advertising.o(i.ble_advertising_start) refers to ble_advertising.o(i.use_whitelist) for use_whitelist
    ble_advertising.o(i.ble_advertising_start) refers to ble_advertising.o(i.flags_set) for flags_set
    ble_advertising.o(i.flags_set) refers to ble_advdata.o(i.ble_advdata_parse) for ble_advdata_parse
    ble_conn_params.o(i.ble_conn_params_change_conn_params) refers to ble_conn_params.o(i.instance_get) for instance_get
    ble_conn_params.o(i.ble_conn_params_change_conn_params) refers to ble_conn_params.o(.data) for .data
    ble_conn_params.o(i.ble_conn_params_init) refers to memcpya.o(.text) for __aeabi_memcpy4
    ble_conn_params.o(i.ble_conn_params_init) refers to app_timer.o(i.app_timer_create) for app_timer_create
    ble_conn_params.o(i.ble_conn_params_init) refers to ble_conn_params.o(.bss) for .bss
    ble_conn_params.o(i.ble_conn_params_init) refers to ble_conn_params.o(.data) for .data
    ble_conn_params.o(i.ble_conn_params_init) refers to ble_conn_params.o(i.update_timeout_handler) for update_timeout_handler
    ble_conn_params.o(i.ble_conn_params_stop) refers to app_timer.o(i.app_timer_stop) for app_timer_stop
    ble_conn_params.o(i.ble_conn_params_stop) refers to ble_conn_params.o(.bss) for .bss
    ble_conn_params.o(i.ble_evt_handler) refers to ble_conn_params.o(i.instance_get) for instance_get
    ble_conn_params.o(i.ble_evt_handler) refers to ble_srv_common.o(i.ble_srv_is_notification_enabled) for ble_srv_is_notification_enabled
    ble_conn_params.o(i.ble_evt_handler) refers to ble_conn_params.o(i.is_conn_params_ok) for is_conn_params_ok
    ble_conn_params.o(i.ble_evt_handler) refers to app_timer.o(i.app_timer_stop) for app_timer_stop
    ble_conn_params.o(i.ble_evt_handler) refers to ble_conn_params.o(i.send_error_evt) for send_error_evt
    ble_conn_params.o(i.ble_evt_handler) refers to ble_conn_params.o(i.conn_params_negotiation) for conn_params_negotiation
    ble_conn_params.o(i.ble_evt_handler) refers to ble_conn_params.o(.bss) for .bss
    ble_conn_params.o(i.ble_evt_handler) refers to ble_conn_params.o(.data) for .data
    ble_conn_params.o(i.conn_params_negotiation) refers to app_timer.o(i.app_timer_start) for app_timer_start
    ble_conn_params.o(i.conn_params_negotiation) refers to ble_conn_params.o(i.send_error_evt) for send_error_evt
    ble_conn_params.o(i.conn_params_negotiation) refers to ble_conn_params.o(.bss) for .bss
    ble_conn_params.o(i.instance_get) refers to ble_conn_params.o(.bss) for .bss
    ble_conn_params.o(i.send_error_evt) refers to ble_conn_params.o(.bss) for .bss
    ble_conn_params.o(i.update_timeout_handler) refers to ble_conn_params.o(i.instance_get) for instance_get
    ble_conn_params.o(i.update_timeout_handler) refers to ble_conn_params.o(i.send_error_evt) for send_error_evt
    ble_conn_params.o(i.update_timeout_handler) refers to ble_conn_params.o(.bss) for .bss
    ble_conn_params.o(sdh_ble_observers1) refers to ble_conn_params.o(i.ble_evt_handler) for ble_evt_handler
    ble_conn_state.o(i.active_flag_count) refers to nrf_atflags.o(i.nrf_atflags_get) for nrf_atflags_get
    ble_conn_state.o(i.bcs_internal_state_reset) refers to memseta.o(.text) for __aeabi_memclr4
    ble_conn_state.o(i.bcs_internal_state_reset) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(i.ble_conn_state_central_conn_count) refers to nrf_atomic.o(i.nrf_atomic_u32_and) for nrf_atomic_u32_and
    ble_conn_state.o(i.ble_conn_state_central_conn_count) refers to ble_conn_state.o(i.active_flag_count) for active_flag_count
    ble_conn_state.o(i.ble_conn_state_central_conn_count) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(i.ble_conn_state_central_handles) refers to nrf_atomic.o(i.nrf_atomic_u32_and) for nrf_atomic_u32_and
    ble_conn_state.o(i.ble_conn_state_central_handles) refers to ble_conn_state.o(i.conn_handle_list_get) for conn_handle_list_get
    ble_conn_state.o(i.ble_conn_state_central_handles) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(i.ble_conn_state_conn_count) refers to ble_conn_state.o(i.active_flag_count) for active_flag_count
    ble_conn_state.o(i.ble_conn_state_conn_count) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(i.ble_conn_state_conn_handles) refers to ble_conn_state.o(i.conn_handle_list_get) for conn_handle_list_get
    ble_conn_state.o(i.ble_conn_state_conn_handles) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(i.ble_conn_state_conn_idx) refers to ble_conn_state.o(i.ble_conn_state_valid) for ble_conn_state_valid
    ble_conn_state.o(i.ble_conn_state_encrypted) refers to ble_conn_state.o(i.ble_conn_state_valid) for ble_conn_state_valid
    ble_conn_state.o(i.ble_conn_state_encrypted) refers to nrf_atflags.o(i.nrf_atflags_get) for nrf_atflags_get
    ble_conn_state.o(i.ble_conn_state_encrypted) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(i.ble_conn_state_for_each_connected) refers to ble_conn_state.o(i.for_each_set_flag) for for_each_set_flag
    ble_conn_state.o(i.ble_conn_state_for_each_connected) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(i.ble_conn_state_for_each_set_user_flag) refers to ble_conn_state.o(i.user_flag_is_acquired) for user_flag_is_acquired
    ble_conn_state.o(i.ble_conn_state_for_each_set_user_flag) refers to ble_conn_state.o(i.for_each_set_flag) for for_each_set_flag
    ble_conn_state.o(i.ble_conn_state_for_each_set_user_flag) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(i.ble_conn_state_init) refers to ble_conn_state.o(i.bcs_internal_state_reset) for bcs_internal_state_reset
    ble_conn_state.o(i.ble_conn_state_mitm_protected) refers to ble_conn_state.o(i.ble_conn_state_valid) for ble_conn_state_valid
    ble_conn_state.o(i.ble_conn_state_mitm_protected) refers to nrf_atflags.o(i.nrf_atflags_get) for nrf_atflags_get
    ble_conn_state.o(i.ble_conn_state_mitm_protected) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(i.ble_conn_state_periph_handles) refers to nrf_atomic.o(i.nrf_atomic_u32_and) for nrf_atomic_u32_and
    ble_conn_state.o(i.ble_conn_state_periph_handles) refers to ble_conn_state.o(i.conn_handle_list_get) for conn_handle_list_get
    ble_conn_state.o(i.ble_conn_state_periph_handles) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(i.ble_conn_state_peripheral_conn_count) refers to nrf_atomic.o(i.nrf_atomic_u32_and) for nrf_atomic_u32_and
    ble_conn_state.o(i.ble_conn_state_peripheral_conn_count) refers to ble_conn_state.o(i.active_flag_count) for active_flag_count
    ble_conn_state.o(i.ble_conn_state_peripheral_conn_count) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(i.ble_conn_state_role) refers to ble_conn_state.o(i.ble_conn_state_valid) for ble_conn_state_valid
    ble_conn_state.o(i.ble_conn_state_status) refers to ble_conn_state.o(i.ble_conn_state_valid) for ble_conn_state_valid
    ble_conn_state.o(i.ble_conn_state_status) refers to nrf_atflags.o(i.nrf_atflags_get) for nrf_atflags_get
    ble_conn_state.o(i.ble_conn_state_status) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(i.ble_conn_state_user_flag_acquire) refers to nrf_atflags.o(i.nrf_atflags_find_and_set_flag) for nrf_atflags_find_and_set_flag
    ble_conn_state.o(i.ble_conn_state_user_flag_acquire) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(i.ble_conn_state_user_flag_get) refers to ble_conn_state.o(i.user_flag_is_acquired) for user_flag_is_acquired
    ble_conn_state.o(i.ble_conn_state_user_flag_get) refers to ble_conn_state.o(i.ble_conn_state_valid) for ble_conn_state_valid
    ble_conn_state.o(i.ble_conn_state_user_flag_get) refers to nrf_atflags.o(i.nrf_atflags_get) for nrf_atflags_get
    ble_conn_state.o(i.ble_conn_state_user_flag_get) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(i.ble_conn_state_user_flag_set) refers to ble_conn_state.o(i.user_flag_is_acquired) for user_flag_is_acquired
    ble_conn_state.o(i.ble_conn_state_user_flag_set) refers to ble_conn_state.o(i.ble_conn_state_valid) for ble_conn_state_valid
    ble_conn_state.o(i.ble_conn_state_user_flag_set) refers to nrf_atflags.o(i.nrf_atflags_set) for nrf_atflags_set
    ble_conn_state.o(i.ble_conn_state_user_flag_set) refers to nrf_atflags.o(i.nrf_atflags_clear) for nrf_atflags_clear
    ble_conn_state.o(i.ble_conn_state_user_flag_set) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(i.ble_conn_state_valid) refers to nrf_atflags.o(i.nrf_atflags_get) for nrf_atflags_get
    ble_conn_state.o(i.ble_conn_state_valid) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(i.ble_evt_handler) refers to nrf_atomic.o(i.nrf_atomic_u32_and) for nrf_atomic_u32_and
    ble_conn_state.o(i.ble_evt_handler) refers to ble_conn_state.o(i.conn_handle_list_get) for conn_handle_list_get
    ble_conn_state.o(i.ble_evt_handler) refers to memcpya.o(.text) for __aeabi_memcpy4
    ble_conn_state.o(i.ble_evt_handler) refers to nrf_atflags.o(i.nrf_atflags_clear) for nrf_atflags_clear
    ble_conn_state.o(i.ble_evt_handler) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    ble_conn_state.o(i.ble_evt_handler) refers to nrf_atflags.o(i.nrf_atflags_set) for nrf_atflags_set
    ble_conn_state.o(i.ble_evt_handler) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(i.conn_handle_list_get) refers to nrf_atflags.o(i.nrf_atflags_get) for nrf_atflags_get
    ble_conn_state.o(i.conn_handle_list_get) refers to memcpya.o(.text) for __aeabi_memcpy4
    ble_conn_state.o(i.for_each_set_flag) refers to nrf_atflags.o(i.nrf_atflags_get) for nrf_atflags_get
    ble_conn_state.o(i.user_flag_is_acquired) refers to nrf_atflags.o(i.nrf_atflags_get) for nrf_atflags_get
    ble_conn_state.o(i.user_flag_is_acquired) refers to ble_conn_state.o(.bss) for .bss
    ble_conn_state.o(sdh_ble_observers0) refers to ble_conn_state.o(i.ble_evt_handler) for ble_evt_handler
    ble_link_ctx_manager.o(i.blcm_link_ctx_get) refers to ble_conn_state.o(i.ble_conn_state_conn_idx) for ble_conn_state_conn_idx
    ble_srv_common.o(i.ble_srv_ascii_to_utf8) refers to strlen.o(.text) for strlen
    ble_srv_common.o(i.characteristic_add) refers to ble_srv_common.o(i.set_security_req) for set_security_req
    ble_srv_common.o(i.characteristic_add) refers to memseta.o(.text) for __aeabi_memclr4
    ble_srv_common.o(i.descriptor_add) refers to memseta.o(.text) for __aeabi_memclr4
    ble_srv_common.o(i.descriptor_add) refers to ble_srv_common.o(i.set_security_req) for set_security_req
    nrf_ble_gatt.o(i.nrf_ble_gatt_init) refers to nrf_ble_gatt.o(i.link_init) for link_init
    nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) refers to nrf_ble_gatt.o(i.on_connected_evt) for on_connected_evt
    nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) refers to nrf_ble_gatt.o(i.link_init) for link_init
    nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) refers to nrf_ble_gatt.o(i.on_exchange_mtu_request_evt) for on_exchange_mtu_request_evt
    nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) refers to nrf_strerror.o(i.nrf_strerror_get) for nrf_strerror_get
    nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_1) for nrf_log_frontend_std_1
    nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) refers to nrf_ble_gatt.o(.constdata) for .constdata
    nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) refers to nrf_ble_gatt.o(log_const_data) for log_const_data
    nrf_ble_gatt.o(i.on_connected_evt) refers to nrf_strerror.o(i.nrf_strerror_get) for nrf_strerror_get
    nrf_ble_gatt.o(i.on_connected_evt) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_1) for nrf_log_frontend_std_1
    nrf_ble_gatt.o(i.on_connected_evt) refers to nrf_ble_gatt.o(log_const_data) for log_const_data
    nrf_ble_gatt.o(i.on_exchange_mtu_request_evt) refers to nrf_strerror.o(i.nrf_strerror_get) for nrf_strerror_get
    nrf_ble_gatt.o(i.on_exchange_mtu_request_evt) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_1) for nrf_log_frontend_std_1
    nrf_ble_gatt.o(i.on_exchange_mtu_request_evt) refers to nrf_ble_gatt.o(log_const_data) for log_const_data
    nrf_ble_gatt.o(i.on_exchange_mtu_request_evt) refers to nrf_ble_gatt.o(.constdata) for .constdata
    nrf_ble_gatt.o(log_const_data) refers to nrf_ble_gatt.o(.conststrlit) for .conststrlit
    nrf_ble_qwr.o(i.nrf_ble_qwr_on_ble_evt) refers to nrf_ble_qwr.o(i.user_mem_reply) for user_mem_reply
    ble_nus.o(i.ble_nus_data_send) refers to ble_link_ctx_manager.o(i.blcm_link_ctx_get) for blcm_link_ctx_get
    ble_nus.o(i.ble_nus_init) refers to memseta.o(.text) for __aeabi_memclr4
    ble_nus.o(i.ble_nus_init) refers to ble_srv_common.o(i.characteristic_add) for characteristic_add
    ble_nus.o(i.ble_nus_init) refers to ble_nus.o(.constdata) for .constdata
    ble_nus.o(i.ble_nus_on_ble_evt) refers to ble_link_ctx_manager.o(i.blcm_link_ctx_get) for blcm_link_ctx_get
    ble_nus.o(i.ble_nus_on_ble_evt) refers to memseta.o(.text) for __aeabi_memclr4
    ble_nus.o(i.ble_nus_on_ble_evt) refers to ble_nus.o(i.on_connect) for on_connect
    ble_nus.o(i.ble_nus_on_ble_evt) refers to ble_nus.o(i.on_write) for on_write
    ble_nus.o(i.on_connect) refers to ble_link_ctx_manager.o(i.blcm_link_ctx_get) for blcm_link_ctx_get
    ble_nus.o(i.on_connect) refers to ble_srv_common.o(i.ble_srv_is_notification_enabled) for ble_srv_is_notification_enabled
    ble_nus.o(i.on_connect) refers to memseta.o(.text) for __aeabi_memclr4
    ble_nus.o(i.on_write) refers to ble_link_ctx_manager.o(i.blcm_link_ctx_get) for blcm_link_ctx_get
    ble_nus.o(i.on_write) refers to memseta.o(.text) for __aeabi_memclr4
    ble_nus.o(i.on_write) refers to ble_srv_common.o(i.ble_srv_is_notification_enabled) for ble_srv_is_notification_enabled
    ble_nus.o(log_const_data) refers to ble_nus.o(.conststrlit) for .conststrlit
    nrf_drv_clock.o(i.clock_clk_started_notify) refers to nrf_drv_clock.o(.bss) for .bss
    nrf_drv_clock.o(i.clock_irq_handler) refers to nrf_drv_clock.o(i.clock_clk_started_notify) for clock_clk_started_notify
    nrf_drv_clock.o(i.clock_irq_handler) refers to nrf_drv_clock.o(.bss) for .bss
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_is_running) refers to nrf_sdh.o(i.nrf_sdh_is_enabled) for nrf_sdh_is_enabled
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_release) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_release) refers to nrf_sdh.o(i.nrf_sdh_is_enabled) for nrf_sdh_is_enabled
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_release) refers to nrfx_clock.o(i.nrfx_clock_hfclk_stop) for nrfx_clock_hfclk_stop
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_release) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_release) refers to nrf_drv_clock.o(.bss) for .bss
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_request) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_request) refers to nrf_drv_clock.o(i.item_enqueue) for item_enqueue
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_request) refers to nrf_sdh.o(i.nrf_sdh_is_enabled) for nrf_sdh_is_enabled
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_request) refers to nrfx_clock.o(i.nrfx_clock_hfclk_start) for nrfx_clock_hfclk_start
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_request) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_request) refers to nrf_drv_clock.o(.bss) for .bss
    nrf_drv_clock.o(i.nrf_drv_clock_init) refers to nrfx_clock.o(i.nrfx_clock_init) for nrfx_clock_init
    nrf_drv_clock.o(i.nrf_drv_clock_init) refers to nrf_sdh.o(i.nrf_sdh_is_enabled) for nrf_sdh_is_enabled
    nrf_drv_clock.o(i.nrf_drv_clock_init) refers to nrfx_clock.o(i.nrfx_clock_enable) for nrfx_clock_enable
    nrf_drv_clock.o(i.nrf_drv_clock_init) refers to nrf_drv_clock.o(.bss) for .bss
    nrf_drv_clock.o(i.nrf_drv_clock_init) refers to nrf_drv_clock.o(i.clock_irq_handler) for clock_irq_handler
    nrf_drv_clock.o(i.nrf_drv_clock_init_check) refers to nrf_drv_clock.o(.bss) for .bss
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_is_running) refers to nrf_sdh.o(i.nrf_sdh_is_enabled) for nrf_sdh_is_enabled
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_release) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_release) refers to nrfx_clock.o(i.nrfx_clock_lfclk_stop) for nrfx_clock_lfclk_stop
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_release) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_release) refers to nrf_drv_clock.o(.bss) for .bss
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_request) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_request) refers to nrf_drv_clock.o(i.item_enqueue) for item_enqueue
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_request) refers to nrfx_clock.o(i.nrfx_clock_lfclk_start) for nrfx_clock_lfclk_start
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_request) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_request) refers to nrf_drv_clock.o(.bss) for .bss
    nrf_drv_clock.o(i.nrf_drv_clock_uninit) refers to nrfx_clock.o(i.nrfx_clock_disable) for nrfx_clock_disable
    nrf_drv_clock.o(i.nrf_drv_clock_uninit) refers to nrfx_clock.o(i.nrfx_clock_uninit) for nrfx_clock_uninit
    nrf_drv_clock.o(i.nrf_drv_clock_uninit) refers to nrf_drv_clock.o(.bss) for .bss
    nrf_drv_clock.o(i.sd_state_evt_handler) refers to nrfx_clock.o(i.nrfx_clock_enable) for nrfx_clock_enable
    nrf_drv_clock.o(i.sd_state_evt_handler) refers to nrf_drv_clock.o(i.nrf_drv_clock_lfclk_release) for nrf_drv_clock_lfclk_release
    nrf_drv_clock.o(i.sd_state_evt_handler) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_drv_clock.o(i.sd_state_evt_handler) refers to nrf_drv_clock.o(i.nrf_drv_clock_init) for nrf_drv_clock_init
    nrf_drv_clock.o(i.sd_state_evt_handler) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_drv_clock.o(i.sd_state_evt_handler) refers to nrf_drv_clock.o(.bss) for .bss
    nrf_drv_clock.o(i.soc_evt_handler) refers to nrf_drv_clock.o(i.clock_clk_started_notify) for clock_clk_started_notify
    nrf_drv_clock.o(i.soc_evt_handler) refers to nrf_drv_clock.o(.bss) for .bss
    nrf_drv_clock.o(log_const_data) refers to nrf_drv_clock.o(.conststrlit) for .conststrlit
    nrf_drv_clock.o(sdh_soc_observers0) refers to nrf_drv_clock.o(i.soc_evt_handler) for soc_evt_handler
    nrf_drv_clock.o(sdh_state_observers0) refers to nrf_drv_clock.o(i.sd_state_evt_handler) for sd_state_evt_handler
    nrf_drv_uart.o(i.nrf_drv_uart_init) refers to memcpya.o(.text) for __aeabi_memcpy4
    nrf_drv_uart.o(i.nrf_drv_uart_init) refers to nrfx_uarte.o(i.nrfx_uarte_init) for nrfx_uarte_init
    nrf_drv_uart.o(i.nrf_drv_uart_init) refers to nrfx_uart.o(i.nrfx_uart_init) for nrfx_uart_init
    nrf_drv_uart.o(i.nrf_drv_uart_init) refers to nrf_drv_uart.o(.data) for .data
    nrf_drv_uart.o(i.nrf_drv_uart_init) refers to nrf_drv_uart.o(i.uarte_evt_handler) for uarte_evt_handler
    nrf_drv_uart.o(i.nrf_drv_uart_init) refers to nrf_drv_uart.o(i.uart_evt_handler) for uart_evt_handler
    nrf_drv_uart.o(i.uart_evt_handler) refers to nrf_drv_uart.o(.data) for .data
    nrf_drv_uart.o(i.uarte_evt_handler) refers to nrf_drv_uart.o(.data) for .data
    nrfx_atomic.o(i.nrfx_atomic_flag_clear) refers to nrfx_atomic.o(i.nrfx_atomic_u32_and) for nrfx_atomic_u32_and
    nrfx_atomic.o(i.nrfx_atomic_flag_clear_fetch) refers to nrfx_atomic.o(i.nrfx_atomic_u32_fetch_and) for nrfx_atomic_u32_fetch_and
    nrfx_atomic.o(i.nrfx_atomic_flag_set) refers to nrfx_atomic.o(i.nrfx_atomic_u32_or) for nrfx_atomic_u32_or
    nrfx_atomic.o(i.nrfx_atomic_flag_set_fetch) refers to nrfx_atomic.o(i.nrfx_atomic_u32_fetch_or) for nrfx_atomic_u32_fetch_or
    nrfx_atomic.o(i.nrfx_atomic_u32_add) refers to nrfx_atomic.o(.emb_text) for __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_add
    nrfx_atomic.o(i.nrfx_atomic_u32_and) refers to nrfx_atomic.o(.emb_text) for __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_and
    nrfx_atomic.o(i.nrfx_atomic_u32_cmp_exch) refers to nrfx_atomic.o(.emb_text) for __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_cmp_exch
    nrfx_atomic.o(i.nrfx_atomic_u32_fetch_add) refers to nrfx_atomic.o(.emb_text) for __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_add
    nrfx_atomic.o(i.nrfx_atomic_u32_fetch_and) refers to nrfx_atomic.o(.emb_text) for __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_and
    nrfx_atomic.o(i.nrfx_atomic_u32_fetch_or) refers to nrfx_atomic.o(.emb_text) for __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_orr
    nrfx_atomic.o(i.nrfx_atomic_u32_fetch_store) refers to nrfx_atomic.o(.emb_text) for __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_mov
    nrfx_atomic.o(i.nrfx_atomic_u32_fetch_sub) refers to nrfx_atomic.o(.emb_text) for __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_sub
    nrfx_atomic.o(i.nrfx_atomic_u32_fetch_sub_hs) refers to nrfx_atomic.o(.emb_text) for __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_sub_hs
    nrfx_atomic.o(i.nrfx_atomic_u32_fetch_xor) refers to nrfx_atomic.o(.emb_text) for __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_eor
    nrfx_atomic.o(i.nrfx_atomic_u32_or) refers to nrfx_atomic.o(.emb_text) for __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_orr
    nrfx_atomic.o(i.nrfx_atomic_u32_store) refers to nrfx_atomic.o(.emb_text) for __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_mov
    nrfx_atomic.o(i.nrfx_atomic_u32_sub) refers to nrfx_atomic.o(.emb_text) for __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_sub
    nrfx_atomic.o(i.nrfx_atomic_u32_sub_hs) refers to nrfx_atomic.o(.emb_text) for __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_sub_hs
    nrfx_atomic.o(i.nrfx_atomic_u32_xor) refers to nrfx_atomic.o(.emb_text) for __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_eor
    nrfx_clock.o(i.POWER_CLOCK_IRQHandler) refers to nrfx_clock.o(i.nrf_clock_event_check) for nrf_clock_event_check
    nrfx_clock.o(i.POWER_CLOCK_IRQHandler) refers to nrfx_clock.o(i.nrf_clock_event_clear) for nrf_clock_event_clear
    nrfx_clock.o(i.POWER_CLOCK_IRQHandler) refers to nrfx_clock.o(.data) for .data
    nrfx_clock.o(i.nrfx_clock_hfclk_start) refers to nrfx_clock.o(i.nrf_clock_event_clear) for nrf_clock_event_clear
    nrfx_clock.o(i.nrfx_clock_hfclk_stop) refers to nrfx_clock.o(.data) for .data
    nrfx_clock.o(i.nrfx_clock_init) refers to nrfx_clock.o(.data) for .data
    nrfx_clock.o(i.nrfx_clock_lfclk_start) refers to nrfx_clock.o(i.nrf_clock_event_clear) for nrf_clock_event_clear
    nrfx_clock.o(i.nrfx_clock_uninit) refers to nrfx_clock.o(i.nrfx_clock_lfclk_stop) for nrfx_clock_lfclk_stop
    nrfx_clock.o(i.nrfx_clock_uninit) refers to nrfx_clock.o(i.nrfx_clock_hfclk_stop) for nrfx_clock_hfclk_stop
    nrfx_clock.o(i.nrfx_clock_uninit) refers to nrfx_clock.o(.data) for .data
    nrfx_clock.o(log_const_data) refers to nrfx_clock.o(.conststrlit) for .conststrlit
    nrfx_gpiote.o(i.GPIOTE_IRQHandler) refers to nrfx_gpiote.o(i.nrf_gpiote_event_is_set) for nrf_gpiote_event_is_set
    nrfx_gpiote.o(i.GPIOTE_IRQHandler) refers to nrfx_gpiote.o(i.nrf_gpiote_event_clear) for nrf_gpiote_event_clear
    nrfx_gpiote.o(i.GPIOTE_IRQHandler) refers to nrfx_gpiote.o(i.nrf_gpio_ports_read) for nrf_gpio_ports_read
    nrfx_gpiote.o(i.GPIOTE_IRQHandler) refers to nrfx_gpiote.o(i.nrf_bitmask_bit_is_set) for nrf_bitmask_bit_is_set
    nrfx_gpiote.o(i.GPIOTE_IRQHandler) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.GPIOTE_IRQHandler) refers to nrfx_gpiote.o(i.nrf_bitmask_bit_set) for nrf_bitmask_bit_set
    nrfx_gpiote.o(i.GPIOTE_IRQHandler) refers to nrfx_gpiote.o(i.nrf_gpio_cfg_sense_set) for nrf_gpio_cfg_sense_set
    nrfx_gpiote.o(i.GPIOTE_IRQHandler) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.channel_free) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.channel_port_alloc) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.channel_port_get) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.nrf_gpio_cfg_default) refers to nrfx_gpiote.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_gpiote.o(i.nrf_gpio_ports_read) refers to nrfx_gpiote.o(.constdata) for .constdata
    nrfx_gpiote.o(i.nrfx_gpiote_clr_task_addr_get) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_clr_task_trigger) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_addr_get) refers to nrfx_gpiote.o(i.pin_in_use_by_te) for pin_in_use_by_te
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_addr_get) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_disable) refers to nrfx_gpiote.o(i.pin_in_use_by_port) for pin_in_use_by_port
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_disable) refers to nrfx_gpiote.o(i.nrf_gpio_cfg_sense_set) for nrf_gpio_cfg_sense_set
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_disable) refers to nrfx_gpiote.o(i.pin_in_use_by_te) for pin_in_use_by_te
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_disable) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable) refers to nrfx_gpiote.o(i.pin_in_use_by_port) for pin_in_use_by_port
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable) refers to nrfx_gpiote.o(i.nrf_gpio_cfg_sense_set) for nrf_gpio_cfg_sense_set
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable) refers to nrfx_gpiote.o(i.pin_in_use_by_te) for pin_in_use_by_te
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable) refers to nrfx_gpiote.o(i.nrf_gpiote_event_clear) for nrf_gpiote_event_clear
    nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.nrfx_gpiote_in_init) refers to nrfx_gpiote.o(i.channel_port_alloc) for channel_port_alloc
    nrfx_gpiote.o(i.nrfx_gpiote_in_init) refers to nrfx_gpiote.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_gpiote.o(i.nrfx_gpiote_in_init) refers to nrfx_gpiote.o(i.nrf_bitmask_bit_set) for nrf_bitmask_bit_set
    nrfx_gpiote.o(i.nrfx_gpiote_in_init) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) refers to nrfx_gpiote.o(i.nrfx_gpiote_in_event_disable) for nrfx_gpiote_in_event_disable
    nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) refers to nrfx_gpiote.o(i.pin_in_use_by_te) for pin_in_use_by_te
    nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) refers to nrfx_gpiote.o(i.pin_configured_check) for pin_configured_check
    nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) refers to nrfx_gpiote.o(i.nrf_gpio_cfg_default) for nrf_gpio_cfg_default
    nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) refers to nrfx_gpiote.o(i.pin_configured_clear) for pin_configured_clear
    nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) refers to nrfx_gpiote.o(i.channel_free) for channel_free
    nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.nrfx_gpiote_init) refers to nrfx_gpiote.o(i.channel_free) for channel_free
    nrfx_gpiote.o(i.nrfx_gpiote_init) refers to nrfx_gpiote.o(i.nrf_gpiote_event_clear) for nrf_gpiote_event_clear
    nrfx_gpiote.o(i.nrfx_gpiote_init) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.nrfx_gpiote_is_init) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.nrfx_gpiote_out_init) refers to nrfx_gpiote.o(i.channel_port_alloc) for channel_port_alloc
    nrfx_gpiote.o(i.nrfx_gpiote_out_init) refers to nrfx_gpiote.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_gpiote.o(i.nrfx_gpiote_out_init) refers to nrfx_gpiote.o(i.nrf_bitmask_bit_set) for nrf_bitmask_bit_set
    nrfx_gpiote.o(i.nrfx_gpiote_out_init) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.nrfx_gpiote_out_task_addr_get) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_out_task_disable) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.nrfx_gpiote_out_task_enable) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.nrfx_gpiote_out_task_force) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.nrfx_gpiote_out_task_trigger) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_out_uninit) refers to nrfx_gpiote.o(i.pin_in_use_by_te) for pin_in_use_by_te
    nrfx_gpiote.o(i.nrfx_gpiote_out_uninit) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_out_uninit) refers to nrfx_gpiote.o(i.channel_free) for channel_free
    nrfx_gpiote.o(i.nrfx_gpiote_out_uninit) refers to nrfx_gpiote.o(i.pin_configured_check) for pin_configured_check
    nrfx_gpiote.o(i.nrfx_gpiote_out_uninit) refers to nrfx_gpiote.o(i.nrf_gpio_cfg_default) for nrf_gpio_cfg_default
    nrfx_gpiote.o(i.nrfx_gpiote_out_uninit) refers to nrfx_gpiote.o(i.pin_configured_clear) for pin_configured_clear
    nrfx_gpiote.o(i.nrfx_gpiote_out_uninit) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.nrfx_gpiote_set_task_addr_get) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_set_task_trigger) refers to nrfx_gpiote.o(i.channel_port_get) for channel_port_get
    nrfx_gpiote.o(i.nrfx_gpiote_uninit) refers to nrfx_gpiote.o(i.nrfx_gpiote_in_uninit) for nrfx_gpiote_in_uninit
    nrfx_gpiote.o(i.nrfx_gpiote_uninit) refers to nrfx_gpiote.o(i.nrfx_gpiote_out_uninit) for nrfx_gpiote_out_uninit
    nrfx_gpiote.o(i.nrfx_gpiote_uninit) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.pin_configured_check) refers to nrfx_gpiote.o(i.nrf_bitmask_bit_is_set) for nrf_bitmask_bit_is_set
    nrfx_gpiote.o(i.pin_configured_check) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.pin_configured_clear) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.pin_in_use_by_port) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(i.pin_in_use_by_te) refers to nrfx_gpiote.o(.bss) for .bss
    nrfx_gpiote.o(log_const_data) refers to nrfx_gpiote.o(.conststrlit) for .conststrlit
    nrfx_prs.o(i.UARTE0_UART0_IRQHandler) refers to nrfx_prs.o(.data) for .data
    nrfx_prs.o(i.nrfx_prs_acquire) refers to nrfx_prs.o(i.prs_box_get) for prs_box_get
    nrfx_prs.o(i.nrfx_prs_acquire) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrfx_prs.o(i.nrfx_prs_acquire) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrfx_prs.o(i.nrfx_prs_release) refers to nrfx_prs.o(i.prs_box_get) for prs_box_get
    nrfx_prs.o(i.prs_box_get) refers to nrfx_prs.o(.data) for .data
    nrfx_prs.o(log_const_data) refers to nrfx_prs.o(.conststrlit) for .conststrlit
    nrfx_uart.o(i.apply_config) refers to nrfx_uart.o(i.nrf_gpio_cfg_output) for nrf_gpio_cfg_output
    nrfx_uart.o(i.apply_config) refers to nrfx_uart.o(i.nrf_gpio_cfg_input) for nrf_gpio_cfg_input
    nrfx_uart.o(i.nrf_gpio_cfg_default) refers to nrfx_uart.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_uart.o(i.nrf_gpio_cfg_input) refers to nrfx_uart.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_uart.o(i.nrf_gpio_cfg_output) refers to nrfx_uart.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_uart.o(i.nrfx_uart_0_irq_handler) refers to nrfx_uart.o(i.uart_irq_handler) for uart_irq_handler
    nrfx_uart.o(i.nrfx_uart_0_irq_handler) refers to nrfx_uart.o(.bss) for .bss
    nrfx_uart.o(i.nrfx_uart_errorsrc_get) refers to nrfx_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrfx_uart.o(i.nrfx_uart_init) refers to nrfx_prs.o(i.nrfx_prs_acquire) for nrfx_prs_acquire
    nrfx_uart.o(i.nrfx_uart_init) refers to nrfx_uart.o(i.apply_config) for apply_config
    nrfx_uart.o(i.nrfx_uart_init) refers to nrfx_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrfx_uart.o(i.nrfx_uart_init) refers to nrfx_uart.o(.bss) for .bss
    nrfx_uart.o(i.nrfx_uart_init) refers to nrfx_uart.o(.constdata) for .constdata
    nrfx_uart.o(i.nrfx_uart_rx) refers to nrfx_uart.o(i.rx_enable) for rx_enable
    nrfx_uart.o(i.nrfx_uart_rx) refers to nrfx_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrfx_uart.o(i.nrfx_uart_rx) refers to nrfx_uart.o(i.nrf_uart_event_check) for nrf_uart_event_check
    nrfx_uart.o(i.nrfx_uart_rx) refers to nrfx_uart.o(i.rx_byte) for rx_byte
    nrfx_uart.o(i.nrfx_uart_rx) refers to nrfx_uart.o(.bss) for .bss
    nrfx_uart.o(i.nrfx_uart_rx_disable) refers to nrfx_uart.o(.bss) for .bss
    nrfx_uart.o(i.nrfx_uart_rx_enable) refers to nrfx_uart.o(i.rx_enable) for rx_enable
    nrfx_uart.o(i.nrfx_uart_rx_enable) refers to nrfx_uart.o(.bss) for .bss
    nrfx_uart.o(i.nrfx_uart_tx) refers to nrfx_uart.o(i.nrfx_uart_tx_in_progress) for nrfx_uart_tx_in_progress
    nrfx_uart.o(i.nrfx_uart_tx) refers to nrfx_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrfx_uart.o(i.nrfx_uart_tx) refers to nrfx_uart.o(i.tx_byte) for tx_byte
    nrfx_uart.o(i.nrfx_uart_tx) refers to nrfx_uart.o(i.nrf_uart_event_check) for nrf_uart_event_check
    nrfx_uart.o(i.nrfx_uart_tx) refers to nrfx_uart.o(.bss) for .bss
    nrfx_uart.o(i.nrfx_uart_tx_abort) refers to nrfx_uart.o(i.tx_done_event) for tx_done_event
    nrfx_uart.o(i.nrfx_uart_tx_abort) refers to nrfx_uart.o(.bss) for .bss
    nrfx_uart.o(i.nrfx_uart_tx_in_progress) refers to nrfx_uart.o(.bss) for .bss
    nrfx_uart.o(i.nrfx_uart_uninit) refers to nrfx_uart.o(i.nrf_gpio_cfg_default) for nrf_gpio_cfg_default
    nrfx_uart.o(i.nrfx_uart_uninit) refers to nrfx_prs.o(i.nrfx_prs_release) for nrfx_prs_release
    nrfx_uart.o(i.nrfx_uart_uninit) refers to nrfx_uart.o(.bss) for .bss
    nrfx_uart.o(i.rx_byte) refers to nrfx_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrfx_uart.o(i.rx_enable) refers to nrfx_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrfx_uart.o(i.tx_byte) refers to nrfx_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrfx_uart.o(i.uart_irq_handler) refers to nrfx_uart.o(i.nrf_uart_int_enable_check) for nrf_uart_int_enable_check
    nrfx_uart.o(i.uart_irq_handler) refers to nrfx_uart.o(i.nrf_uart_event_check) for nrf_uart_event_check
    nrfx_uart.o(i.uart_irq_handler) refers to nrfx_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrfx_uart.o(i.uart_irq_handler) refers to nrfx_uart.o(i.rx_byte) for rx_byte
    nrfx_uart.o(i.uart_irq_handler) refers to nrfx_uart.o(i.rx_done_event) for rx_done_event
    nrfx_uart.o(i.uart_irq_handler) refers to nrfx_uart.o(i.tx_done_event) for tx_done_event
    nrfx_uart.o(i.uart_irq_handler) refers to nrfx_uart.o(i.tx_byte) for tx_byte
    nrfx_uart.o(.constdata) refers to nrfx_uart.o(i.nrfx_uart_0_irq_handler) for nrfx_uart_0_irq_handler
    nrfx_uart.o(log_const_data) refers to nrfx_uart.o(.conststrlit) for .conststrlit
    nrfx_uarte.o(i.apply_config) refers to nrfx_uarte.o(i.nrf_gpio_cfg_output) for nrf_gpio_cfg_output
    nrfx_uarte.o(i.apply_config) refers to nrfx_uarte.o(i.nrf_gpio_cfg_input) for nrf_gpio_cfg_input
    nrfx_uarte.o(i.interrupts_enable) refers to nrfx_uarte.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrfx_uarte.o(i.nrf_gpio_cfg_default) refers to nrfx_uarte.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_uarte.o(i.nrf_gpio_cfg_input) refers to nrfx_uarte.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_uarte.o(i.nrf_gpio_cfg_output) refers to nrfx_uarte.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_uarte.o(i.nrfx_uarte_0_irq_handler) refers to nrfx_uarte.o(i.uarte_irq_handler) for uarte_irq_handler
    nrfx_uarte.o(i.nrfx_uarte_0_irq_handler) refers to nrfx_uarte.o(.bss) for .bss
    nrfx_uarte.o(i.nrfx_uarte_errorsrc_get) refers to nrfx_uarte.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrfx_uarte.o(i.nrfx_uarte_init) refers to nrfx_prs.o(i.nrfx_prs_acquire) for nrfx_prs_acquire
    nrfx_uarte.o(i.nrfx_uarte_init) refers to nrfx_uarte.o(i.apply_config) for apply_config
    nrfx_uarte.o(i.nrfx_uarte_init) refers to nrfx_uarte.o(i.interrupts_enable) for interrupts_enable
    nrfx_uarte.o(i.nrfx_uarte_init) refers to nrfx_uarte.o(.bss) for .bss
    nrfx_uarte.o(i.nrfx_uarte_init) refers to nrfx_uarte.o(.constdata) for .constdata
    nrfx_uarte.o(i.nrfx_uarte_rx) refers to nrfx_uarte.o(i.nrfx_is_in_ram) for nrfx_is_in_ram
    nrfx_uarte.o(i.nrfx_uarte_rx) refers to nrfx_uarte.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrfx_uarte.o(i.nrfx_uarte_rx) refers to nrfx_uarte.o(i.nrf_uarte_event_check) for nrf_uarte_event_check
    nrfx_uarte.o(i.nrfx_uarte_rx) refers to nrfx_uarte.o(.bss) for .bss
    nrfx_uarte.o(i.nrfx_uarte_rx_abort) refers to nrfx_uarte.o(.bss) for .bss
    nrfx_uarte.o(i.nrfx_uarte_tx) refers to nrfx_uarte.o(i.nrfx_is_in_ram) for nrfx_is_in_ram
    nrfx_uarte.o(i.nrfx_uarte_tx) refers to nrfx_uarte.o(i.nrfx_uarte_tx_in_progress) for nrfx_uarte_tx_in_progress
    nrfx_uarte.o(i.nrfx_uarte_tx) refers to nrfx_uarte.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrfx_uarte.o(i.nrfx_uarte_tx) refers to nrfx_uarte.o(i.nrf_uarte_event_check) for nrf_uarte_event_check
    nrfx_uarte.o(i.nrfx_uarte_tx) refers to nrfx_uarte.o(.bss) for .bss
    nrfx_uarte.o(i.nrfx_uarte_tx_abort) refers to nrfx_uarte.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrfx_uarte.o(i.nrfx_uarte_tx_abort) refers to nrfx_uarte.o(i.nrf_uarte_event_check) for nrf_uarte_event_check
    nrfx_uarte.o(i.nrfx_uarte_tx_abort) refers to nrfx_uarte.o(.bss) for .bss
    nrfx_uarte.o(i.nrfx_uarte_tx_in_progress) refers to nrfx_uarte.o(.bss) for .bss
    nrfx_uarte.o(i.nrfx_uarte_uninit) refers to nrfx_uarte.o(i.nrf_gpio_cfg_default) for nrf_gpio_cfg_default
    nrfx_uarte.o(i.nrfx_uarte_uninit) refers to nrfx_prs.o(i.nrfx_prs_release) for nrfx_prs_release
    nrfx_uarte.o(i.nrfx_uarte_uninit) refers to nrfx_uarte.o(.bss) for .bss
    nrfx_uarte.o(i.uarte_irq_handler) refers to nrfx_uarte.o(i.nrf_uarte_event_check) for nrf_uarte_event_check
    nrfx_uarte.o(i.uarte_irq_handler) refers to nrfx_uarte.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrfx_uarte.o(i.uarte_irq_handler) refers to nrfx_uarte.o(i.rx_done_event) for rx_done_event
    nrfx_uarte.o(.constdata) refers to nrfx_uarte.o(i.nrfx_uarte_0_irq_handler) for nrfx_uarte_0_irq_handler
    nrfx_uarte.o(log_const_data) refers to nrfx_uarte.o(.conststrlit) for .conststrlit
    nrf_drv_ppi.o(i.nrf_drv_ppi_init) refers to nrf_drv_ppi.o(.data) for .data
    nrf_drv_ppi.o(i.nrf_drv_ppi_uninit) refers to nrfx_ppi.o(i.nrfx_ppi_free_all) for nrfx_ppi_free_all
    nrf_drv_ppi.o(i.nrf_drv_ppi_uninit) refers to nrf_drv_ppi.o(.data) for .data
    nrfx_ppi.o(i.is_allocated_channel) refers to nrfx_ppi.o(.data) for .data
    nrfx_ppi.o(i.is_allocated_group) refers to nrfx_ppi.o(.data) for .data
    nrfx_ppi.o(i.is_app_channel) refers to nrfx_ppi.o(i.are_app_channels) for are_app_channels
    nrfx_ppi.o(i.nrfx_ppi_channel_alloc) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrfx_ppi.o(i.nrfx_ppi_channel_alloc) refers to nrfx_ppi.o(i.is_allocated_channel) for is_allocated_channel
    nrfx_ppi.o(i.nrfx_ppi_channel_alloc) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrfx_ppi.o(i.nrfx_ppi_channel_alloc) refers to nrfx_ppi.o(.data) for .data
    nrfx_ppi.o(i.nrfx_ppi_channel_assign) refers to nrfx_ppi.o(i.is_programmable_app_channel) for is_programmable_app_channel
    nrfx_ppi.o(i.nrfx_ppi_channel_assign) refers to nrfx_ppi.o(i.is_allocated_channel) for is_allocated_channel
    nrfx_ppi.o(i.nrfx_ppi_channel_disable) refers to nrfx_ppi.o(i.is_app_channel) for is_app_channel
    nrfx_ppi.o(i.nrfx_ppi_channel_disable) refers to nrfx_ppi.o(i.is_programmable_app_channel) for is_programmable_app_channel
    nrfx_ppi.o(i.nrfx_ppi_channel_disable) refers to nrfx_ppi.o(i.is_allocated_channel) for is_allocated_channel
    nrfx_ppi.o(i.nrfx_ppi_channel_enable) refers to nrfx_ppi.o(i.is_app_channel) for is_app_channel
    nrfx_ppi.o(i.nrfx_ppi_channel_enable) refers to nrfx_ppi.o(i.is_programmable_app_channel) for is_programmable_app_channel
    nrfx_ppi.o(i.nrfx_ppi_channel_enable) refers to nrfx_ppi.o(i.is_allocated_channel) for is_allocated_channel
    nrfx_ppi.o(i.nrfx_ppi_channel_fork_assign) refers to nrfx_ppi.o(i.is_allocated_channel) for is_allocated_channel
    nrfx_ppi.o(i.nrfx_ppi_channel_free) refers to nrfx_ppi.o(i.is_programmable_app_channel) for is_programmable_app_channel
    nrfx_ppi.o(i.nrfx_ppi_channel_free) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrfx_ppi.o(i.nrfx_ppi_channel_free) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrfx_ppi.o(i.nrfx_ppi_channel_free) refers to nrfx_ppi.o(.data) for .data
    nrfx_ppi.o(i.nrfx_ppi_channels_include_in_group) refers to nrfx_ppi.o(i.is_app_group) for is_app_group
    nrfx_ppi.o(i.nrfx_ppi_channels_include_in_group) refers to nrfx_ppi.o(i.is_allocated_group) for is_allocated_group
    nrfx_ppi.o(i.nrfx_ppi_channels_include_in_group) refers to nrfx_ppi.o(i.are_app_channels) for are_app_channels
    nrfx_ppi.o(i.nrfx_ppi_channels_include_in_group) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrfx_ppi.o(i.nrfx_ppi_channels_include_in_group) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrfx_ppi.o(i.nrfx_ppi_channels_remove_from_group) refers to nrfx_ppi.o(i.is_app_group) for is_app_group
    nrfx_ppi.o(i.nrfx_ppi_channels_remove_from_group) refers to nrfx_ppi.o(i.is_allocated_group) for is_allocated_group
    nrfx_ppi.o(i.nrfx_ppi_channels_remove_from_group) refers to nrfx_ppi.o(i.are_app_channels) for are_app_channels
    nrfx_ppi.o(i.nrfx_ppi_channels_remove_from_group) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrfx_ppi.o(i.nrfx_ppi_channels_remove_from_group) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrfx_ppi.o(i.nrfx_ppi_free_all) refers to nrfx_ppi.o(.data) for .data
    nrfx_ppi.o(i.nrfx_ppi_group_alloc) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrfx_ppi.o(i.nrfx_ppi_group_alloc) refers to nrfx_ppi.o(i.is_allocated_group) for is_allocated_group
    nrfx_ppi.o(i.nrfx_ppi_group_alloc) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrfx_ppi.o(i.nrfx_ppi_group_alloc) refers to nrfx_ppi.o(.data) for .data
    nrfx_ppi.o(i.nrfx_ppi_group_disable) refers to nrfx_ppi.o(i.is_app_group) for is_app_group
    nrfx_ppi.o(i.nrfx_ppi_group_enable) refers to nrfx_ppi.o(i.is_app_group) for is_app_group
    nrfx_ppi.o(i.nrfx_ppi_group_enable) refers to nrfx_ppi.o(i.is_allocated_group) for is_allocated_group
    nrfx_ppi.o(i.nrfx_ppi_group_free) refers to nrfx_ppi.o(i.is_app_group) for is_app_group
    nrfx_ppi.o(i.nrfx_ppi_group_free) refers to nrfx_ppi.o(i.is_allocated_group) for is_allocated_group
    nrfx_ppi.o(i.nrfx_ppi_group_free) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrfx_ppi.o(i.nrfx_ppi_group_free) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrfx_ppi.o(i.nrfx_ppi_group_free) refers to nrfx_ppi.o(.data) for .data
    nrfx_ppi.o(log_const_data) refers to nrfx_ppi.o(.conststrlit) for .conststrlit
    nrfx_saadc.o(i.SAADC_IRQHandler) refers to nrfx_saadc.o(i.nrf_saadc_event_check) for nrf_saadc_event_check
    nrfx_saadc.o(i.SAADC_IRQHandler) refers to nrfx_saadc.o(i.nrf_saadc_event_clear) for nrf_saadc_event_clear
    nrfx_saadc.o(i.SAADC_IRQHandler) refers to nrfx_saadc.o(i.nrf_saadc_buffer_init) for nrf_saadc_buffer_init
    nrfx_saadc.o(i.SAADC_IRQHandler) refers to nrfx_saadc.o(.bss) for .bss
    nrfx_saadc.o(i.nrfx_coredep_delay_us) refers to nrfx_saadc.o(.constdata) for .constdata
    nrfx_saadc.o(i.nrfx_saadc_abort) refers to nrfx_saadc.o(i.nrfx_saadc_is_busy) for nrfx_saadc_is_busy
    nrfx_saadc.o(i.nrfx_saadc_abort) refers to nrfx_saadc.o(i.nrf_saadc_event_clear) for nrf_saadc_event_clear
    nrfx_saadc.o(i.nrfx_saadc_abort) refers to nrfx_saadc.o(i.nrfx_coredep_delay_us) for nrfx_coredep_delay_us
    nrfx_saadc.o(i.nrfx_saadc_abort) refers to nrfx_saadc.o(.bss) for .bss
    nrfx_saadc.o(i.nrfx_saadc_buffer_convert) refers to nrfx_saadc.o(i.nrf_saadc_buffer_init) for nrf_saadc_buffer_init
    nrfx_saadc.o(i.nrfx_saadc_buffer_convert) refers to nrfx_saadc.o(i.nrf_saadc_event_check) for nrf_saadc_event_check
    nrfx_saadc.o(i.nrfx_saadc_buffer_convert) refers to nrfx_saadc.o(i.nrf_saadc_event_clear) for nrf_saadc_event_clear
    nrfx_saadc.o(i.nrfx_saadc_buffer_convert) refers to nrfx_saadc.o(.bss) for .bss
    nrfx_saadc.o(i.nrfx_saadc_calibrate_offset) refers to nrfx_saadc.o(i.nrf_saadc_event_clear) for nrf_saadc_event_clear
    nrfx_saadc.o(i.nrfx_saadc_calibrate_offset) refers to nrfx_saadc.o(.bss) for .bss
    nrfx_saadc.o(i.nrfx_saadc_channel_init) refers to nrfx_saadc.o(i.nrf_saadc_channel_input_set) for nrf_saadc_channel_input_set
    nrfx_saadc.o(i.nrfx_saadc_channel_init) refers to nrfx_saadc.o(.bss) for .bss
    nrfx_saadc.o(i.nrfx_saadc_channel_uninit) refers to nrfx_saadc.o(i.nrf_saadc_channel_input_set) for nrf_saadc_channel_input_set
    nrfx_saadc.o(i.nrfx_saadc_channel_uninit) refers to nrfx_saadc.o(i.nrfx_saadc_limits_set) for nrfx_saadc_limits_set
    nrfx_saadc.o(i.nrfx_saadc_channel_uninit) refers to nrfx_saadc.o(.bss) for .bss
    nrfx_saadc.o(i.nrfx_saadc_init) refers to nrfx_saadc.o(i.nrf_saadc_event_clear) for nrf_saadc_event_clear
    nrfx_saadc.o(i.nrfx_saadc_init) refers to nrfx_saadc.o(.bss) for .bss
    nrfx_saadc.o(i.nrfx_saadc_is_busy) refers to nrfx_saadc.o(.bss) for .bss
    nrfx_saadc.o(i.nrfx_saadc_limits_set) refers to nrfx_saadc.o(i.nrf_saadc_limit_int_get) for nrf_saadc_limit_int_get
    nrfx_saadc.o(i.nrfx_saadc_limits_set) refers to nrfx_saadc.o(.bss) for .bss
    nrfx_saadc.o(i.nrfx_saadc_sample) refers to nrfx_saadc.o(.bss) for .bss
    nrfx_saadc.o(i.nrfx_saadc_sample_convert) refers to nrfx_saadc.o(i.nrf_saadc_buffer_init) for nrf_saadc_buffer_init
    nrfx_saadc.o(i.nrfx_saadc_sample_convert) refers to nrfx_saadc.o(i.nrf_saadc_channel_input_set) for nrf_saadc_channel_input_set
    nrfx_saadc.o(i.nrfx_saadc_sample_convert) refers to nrfx_saadc.o(i.nrf_saadc_event_check) for nrf_saadc_event_check
    nrfx_saadc.o(i.nrfx_saadc_sample_convert) refers to nrfx_saadc.o(i.nrfx_coredep_delay_us) for nrfx_coredep_delay_us
    nrfx_saadc.o(i.nrfx_saadc_sample_convert) refers to nrfx_saadc.o(i.nrf_saadc_event_clear) for nrf_saadc_event_clear
    nrfx_saadc.o(i.nrfx_saadc_sample_convert) refers to nrfx_saadc.o(.bss) for .bss
    nrfx_saadc.o(i.nrfx_saadc_sample_task_get) refers to nrfx_saadc.o(.bss) for .bss
    nrfx_saadc.o(i.nrfx_saadc_uninit) refers to nrfx_saadc.o(i.nrf_saadc_event_check) for nrf_saadc_event_check
    nrfx_saadc.o(i.nrfx_saadc_uninit) refers to nrfx_saadc.o(i.nrfx_coredep_delay_us) for nrfx_coredep_delay_us
    nrfx_saadc.o(i.nrfx_saadc_uninit) refers to nrfx_saadc.o(i.nrfx_saadc_channel_uninit) for nrfx_saadc_channel_uninit
    nrfx_saadc.o(i.nrfx_saadc_uninit) refers to nrfx_saadc.o(.bss) for .bss
    nrfx_saadc.o(log_const_data) refers to nrfx_saadc.o(.conststrlit) for .conststrlit
    nrfx_timer.o(i.TIMER0_IRQHandler) refers to nrfx_timer.o(i.nrf_timer_event_clear) for nrf_timer_event_clear
    nrfx_timer.o(i.TIMER0_IRQHandler) refers to nrfx_timer.o(.bss) for .bss
    nrfx_timer.o(i.nrfx_timer_compare) refers to nrfx_timer.o(i.nrf_timer_event_clear) for nrf_timer_event_clear
    nrfx_timer.o(i.nrfx_timer_compare_int_enable) refers to nrfx_timer.o(i.nrf_timer_event_clear) for nrf_timer_event_clear
    nrfx_timer.o(i.nrfx_timer_disable) refers to nrfx_timer.o(.bss) for .bss
    nrfx_timer.o(i.nrfx_timer_enable) refers to nrfx_timer.o(.bss) for .bss
    nrfx_timer.o(i.nrfx_timer_extended_compare) refers to nrfx_timer.o(i.nrfx_timer_compare) for nrfx_timer_compare
    nrfx_timer.o(i.nrfx_timer_init) refers to nrfx_timer.o(i.nrf_timer_event_clear) for nrf_timer_event_clear
    nrfx_timer.o(i.nrfx_timer_init) refers to nrfx_timer.o(.bss) for .bss
    nrfx_timer.o(i.nrfx_timer_is_enabled) refers to nrfx_timer.o(.bss) for .bss
    nrfx_timer.o(i.nrfx_timer_uninit) refers to nrfx_timer.o(i.nrfx_timer_disable) for nrfx_timer_disable
    nrfx_timer.o(i.nrfx_timer_uninit) refers to nrfx_timer.o(.bss) for .bss
    nrfx_timer.o(log_const_data) refers to nrfx_timer.o(.conststrlit) for .conststrlit
    nrf_drv_twi.o(i.nrf_drv_twi_init) refers to nrf_drv_twi.o(i.twi_clear_bus) for twi_clear_bus
    nrf_drv_twi.o(i.nrf_drv_twi_init) refers to nrfx_twim.o(i.nrfx_twim_init) for nrfx_twim_init
    nrf_drv_twi.o(i.nrf_drv_twi_init) refers to nrf_drv_twi.o(.data) for .data
    nrf_drv_twi.o(i.nrf_drv_twi_init) refers to nrf_drv_twi.o(i.twim_evt_handler) for twim_evt_handler
    nrf_drv_twi.o(i.nrfx_coredep_delay_us) refers to nrf_drv_twi.o(.constdata) for .constdata
    nrf_drv_twi.o(i.twi_clear_bus) refers to nrf_drv_twi.o(i.nrf_gpio_pin_set) for nrf_gpio_pin_set
    nrf_drv_twi.o(i.twi_clear_bus) refers to nrf_drv_twi.o(i.nrfx_coredep_delay_us) for nrfx_coredep_delay_us
    nrf_drv_twi.o(i.twim_evt_handler) refers to nrf_drv_twi.o(.data) for .data
    nrfx_twim.o(i.SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler) refers to nrfx_twim.o(i.twim_irq_handler) for twim_irq_handler
    nrfx_twim.o(i.SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler) refers to nrfx_twim.o(.bss) for .bss
    nrfx_twim.o(i.nrf_gpio_cfg_default) refers to nrfx_twim.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_twim.o(i.nrfx_twim_disable) refers to nrfx_twim.o(.bss) for .bss
    nrfx_twim.o(i.nrfx_twim_enable) refers to nrfx_twim.o(.bss) for .bss
    nrfx_twim.o(i.nrfx_twim_init) refers to nrfx_prs.o(i.nrfx_prs_acquire) for nrfx_prs_acquire
    nrfx_twim.o(i.nrfx_twim_init) refers to nrfx_twim.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrfx_twim.o(i.nrfx_twim_init) refers to nrfx_twim.o(.bss) for .bss
    nrfx_twim.o(i.nrfx_twim_init) refers to nrfx_twim.o(.constdata) for .constdata
    nrfx_twim.o(i.nrfx_twim_is_busy) refers to nrfx_twim.o(.bss) for .bss
    nrfx_twim.o(i.nrfx_twim_rx) refers to memcpya.o(.text) for __aeabi_memcpy4
    nrfx_twim.o(i.nrfx_twim_rx) refers to nrfx_twim.o(i.nrfx_twim_xfer) for nrfx_twim_xfer
    nrfx_twim.o(i.nrfx_twim_rx) refers to nrfx_twim.o(.constdata) for .constdata
    nrfx_twim.o(i.nrfx_twim_tx) refers to memseta.o(.text) for __aeabi_memclr4
    nrfx_twim.o(i.nrfx_twim_tx) refers to nrfx_twim.o(i.nrfx_twim_xfer) for nrfx_twim_xfer
    nrfx_twim.o(i.nrfx_twim_uninit) refers to nrfx_twim.o(i.nrfx_twim_disable) for nrfx_twim_disable
    nrfx_twim.o(i.nrfx_twim_uninit) refers to nrfx_prs.o(i.nrfx_prs_release) for nrfx_prs_release
    nrfx_twim.o(i.nrfx_twim_uninit) refers to nrfx_twim.o(i.nrf_gpio_cfg_default) for nrf_gpio_cfg_default
    nrfx_twim.o(i.nrfx_twim_uninit) refers to nrfx_twim.o(.bss) for .bss
    nrfx_twim.o(i.nrfx_twim_xfer) refers to nrfx_twim.o(i.twim_xfer) for twim_xfer
    nrfx_twim.o(i.nrfx_twim_xfer) refers to nrfx_twim.o(.bss) for .bss
    nrfx_twim.o(i.twim_irq_handler) refers to nrfx_twim.o(i.nrf_twim_event_check) for nrf_twim_event_check
    nrfx_twim.o(i.twim_irq_handler) refers to nrfx_twim.o(i.nrf_twim_event_clear) for nrf_twim_event_clear
    nrfx_twim.o(i.twim_irq_handler) refers to memcpya.o(.text) for __aeabi_memcpy4
    nrfx_twim.o(i.twim_xfer) refers to nrfx_twim.o(i.nrfx_is_in_ram) for nrfx_is_in_ram
    nrfx_twim.o(i.twim_xfer) refers to memcpya.o(.text) for __aeabi_memcpy4
    nrfx_twim.o(i.twim_xfer) refers to nrfx_twim.o(i.nrf_twim_event_clear) for nrf_twim_event_clear
    nrfx_twim.o(i.twim_xfer) refers to nrfx_twim.o(i.nrf_twim_event_check) for nrf_twim_event_check
    nrfx_twim.o(.constdata) refers to nrfx_twim.o(i.SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler) for SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler
    nrfx_twim.o(log_const_data) refers to nrfx_twim.o(.conststrlit) for .conststrlit
    app_button.o(i.app_button_disable) refers to nrfx_gpiote.o(i.nrfx_gpiote_in_event_disable) for nrfx_gpiote_in_event_disable
    app_button.o(i.app_button_disable) refers to app_timer.o(i.app_timer_stop) for app_timer_stop
    app_button.o(i.app_button_disable) refers to app_button.o(.data) for .data
    app_button.o(i.app_button_disable) refers to app_button.o(.constdata) for .constdata
    app_button.o(i.app_button_enable) refers to nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable) for nrfx_gpiote_in_event_enable
    app_button.o(i.app_button_enable) refers to app_button.o(.data) for .data
    app_button.o(i.app_button_init) refers to nrfx_gpiote.o(i.nrfx_gpiote_is_init) for nrfx_gpiote_is_init
    app_button.o(i.app_button_init) refers to nrfx_gpiote.o(i.nrfx_gpiote_init) for nrfx_gpiote_init
    app_button.o(i.app_button_init) refers to nrfx_gpiote.o(i.nrfx_gpiote_in_init) for nrfx_gpiote_in_init
    app_button.o(i.app_button_init) refers to app_timer.o(i.app_timer_create) for app_timer_create
    app_button.o(i.app_button_init) refers to app_button.o(.data) for .data
    app_button.o(i.app_button_init) refers to app_button.o(.constdata) for .constdata
    app_button.o(i.app_button_init) refers to app_button.o(i.gpiote_event_handler) for gpiote_event_handler
    app_button.o(i.app_button_init) refers to app_button.o(i.detection_delay_timeout_handler) for detection_delay_timeout_handler
    app_button.o(i.app_button_is_pushed) refers to nrfx_gpiote.o(i.nrfx_gpiote_in_is_set) for nrfx_gpiote_in_is_set
    app_button.o(i.app_button_is_pushed) refers to app_button.o(.data) for .data
    app_button.o(i.detection_delay_timeout_handler) refers to llshl.o(.text) for __aeabi_llsl
    app_button.o(i.detection_delay_timeout_handler) refers to nrfx_gpiote.o(i.nrfx_gpiote_in_is_set) for nrfx_gpiote_in_is_set
    app_button.o(i.detection_delay_timeout_handler) refers to app_button.o(.data) for .data
    app_button.o(i.gpiote_event_handler) refers to llshl.o(.text) for __aeabi_llsl
    app_button.o(i.gpiote_event_handler) refers to app_timer.o(i.app_timer_stop) for app_timer_stop
    app_button.o(i.gpiote_event_handler) refers to nrfx_gpiote.o(i.nrfx_gpiote_in_is_set) for nrfx_gpiote_in_is_set
    app_button.o(i.gpiote_event_handler) refers to app_timer.o(i.app_timer_start) for app_timer_start
    app_button.o(i.gpiote_event_handler) refers to app_button.o(.constdata) for .constdata
    app_button.o(i.gpiote_event_handler) refers to app_button.o(.data) for .data
    app_button.o(.constdata) refers to app_button.o(.bss) for m_detection_delay_timer_id_data
    app_error.o(i.app_error_handler_bare) refers to app_error_weak.o(i.app_error_fault_handler) for app_error_fault_handler
    app_error.o(i.app_error_save_and_stop) refers to app_error.o(.bss) for .bss
    app_error_handler_keil.o(.emb_text) refers to app_error_weak.o(i.app_error_fault_handler) for app_error_fault_handler
    app_error_weak.o(i.app_error_fault_handler) refers to nrf_log_frontend.o(i.nrf_log_panic) for nrf_log_panic
    app_error_weak.o(i.app_error_fault_handler) refers to nrf_log_frontend.o(i.nrf_log_frontend_dequeue) for nrf_log_frontend_dequeue
    app_error_weak.o(i.app_error_fault_handler) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_0) for nrf_log_frontend_std_0
    app_error_weak.o(i.app_error_fault_handler) refers to nrf_log_frontend.o(log_const_data) for m_nrf_log_app_logs_data_const
    app_fifo.o(i.app_fifo_get) refers to app_fifo.o(i.fifo_get) for fifo_get
    app_fifo.o(i.app_fifo_put) refers to app_fifo.o(i.fifo_put) for fifo_put
    app_fifo.o(i.app_fifo_read) refers to app_fifo.o(i.fifo_get) for fifo_get
    app_fifo.o(i.app_fifo_write) refers to app_fifo.o(i.fifo_put) for fifo_put
    app_scheduler.o(i.app_sched_event_put) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    app_scheduler.o(i.app_sched_event_put) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    app_scheduler.o(i.app_sched_event_put) refers to memcpya.o(.text) for __aeabi_memcpy
    app_scheduler.o(i.app_sched_event_put) refers to app_scheduler.o(.data) for .data
    app_scheduler.o(i.app_sched_execute) refers to app_scheduler.o(.data) for .data
    app_scheduler.o(i.app_sched_init) refers to app_scheduler.o(.data) for .data
    app_scheduler.o(i.app_sched_queue_space_get) refers to app_scheduler.o(.data) for .data
    app_timer.o(i.RTC1_IRQHandler) refers to app_timer.o(i.timer_timeouts_check) for timer_timeouts_check
    app_timer.o(i.SWI0_EGU0_IRQHandler) refers to app_timer.o(i.timer_list_handler) for timer_list_handler
    app_timer.o(i.app_timer_create) refers to app_timer.o(.bss) for .bss
    app_timer.o(i.app_timer_init) refers to app_timer.o(i.rtc1_stop) for rtc1_stop
    app_timer.o(i.app_timer_init) refers to app_timer.o(i.NVIC_ClearPendingIRQ) for NVIC_ClearPendingIRQ
    app_timer.o(i.app_timer_init) refers to app_timer.o(i.NVIC_SetPriority) for NVIC_SetPriority
    app_timer.o(i.app_timer_init) refers to app_timer.o(i.NVIC_EnableIRQ) for NVIC_EnableIRQ
    app_timer.o(i.app_timer_init) refers to app_timer.o(.bss) for .bss
    app_timer.o(i.app_timer_init) refers to app_timer.o(.data) for .data
    app_timer.o(i.app_timer_start) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    app_timer.o(i.app_timer_start) refers to app_timer.o(i.user_op_alloc) for user_op_alloc
    app_timer.o(i.app_timer_start) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    app_timer.o(i.app_timer_start) refers to app_timer.o(i.NVIC_SetPendingIRQ) for NVIC_SetPendingIRQ
    app_timer.o(i.app_timer_start) refers to app_timer.o(.bss) for .bss
    app_timer.o(i.app_timer_stop) refers to app_timer.o(i.timer_stop_op_schedule) for timer_stop_op_schedule
    app_timer.o(i.app_timer_stop) refers to app_timer.o(.bss) for .bss
    app_timer.o(i.app_timer_stop_all) refers to app_timer.o(i.timer_stop_op_schedule) for timer_stop_op_schedule
    app_timer.o(i.app_timer_stop_all) refers to app_timer.o(.bss) for .bss
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.NVIC_ClearPendingIRQ) for NVIC_ClearPendingIRQ
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.NVIC_EnableIRQ) for NVIC_EnableIRQ
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.nrfx_coredep_delay_us) for nrfx_coredep_delay_us
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.NVIC_SetPendingIRQ) for NVIC_SetPendingIRQ
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.rtc1_stop) for rtc1_stop
    app_timer.o(i.compare_reg_update) refers to app_timer.o(.data) for .data
    app_timer.o(i.elapsed_ticks_acquire) refers to app_timer.o(.data) for .data
    app_timer.o(i.list_insertions_handler) refers to app_timer.o(i.timer_list_remove) for timer_list_remove
    app_timer.o(i.list_insertions_handler) refers to app_timer.o(i.timer_list_insert) for timer_list_insert
    app_timer.o(i.list_insertions_handler) refers to app_timer.o(.data) for .data
    app_timer.o(i.list_insertions_handler) refers to app_timer.o(.bss) for .bss
    app_timer.o(i.nrfx_coredep_delay_us) refers to app_timer.o(.constdata) for .constdata
    app_timer.o(i.rtc1_stop) refers to app_timer.o(i.nrfx_coredep_delay_us) for nrfx_coredep_delay_us
    app_timer.o(i.rtc1_stop) refers to app_timer.o(.data) for .data
    app_timer.o(i.timer_list_handler) refers to app_timer.o(i.elapsed_ticks_acquire) for elapsed_ticks_acquire
    app_timer.o(i.timer_list_handler) refers to app_timer.o(i.list_insertions_handler) for list_insertions_handler
    app_timer.o(i.timer_list_handler) refers to app_timer.o(i.compare_reg_update) for compare_reg_update
    app_timer.o(i.timer_list_handler) refers to app_timer.o(.data) for .data
    app_timer.o(i.timer_list_insert) refers to app_timer.o(.data) for .data
    app_timer.o(i.timer_list_remove) refers to app_timer.o(i.nrfx_coredep_delay_us) for nrfx_coredep_delay_us
    app_timer.o(i.timer_list_remove) refers to app_timer.o(.data) for .data
    app_timer.o(i.timer_stop_op_schedule) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    app_timer.o(i.timer_stop_op_schedule) refers to app_timer.o(i.user_op_alloc) for user_op_alloc
    app_timer.o(i.timer_stop_op_schedule) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    app_timer.o(i.timer_stop_op_schedule) refers to app_timer.o(i.NVIC_SetPendingIRQ) for NVIC_SetPendingIRQ
    app_timer.o(i.timer_stop_op_schedule) refers to app_timer.o(.bss) for .bss
    app_timer.o(i.timer_timeouts_check) refers to app_timer.o(i.NVIC_SetPendingIRQ) for NVIC_SetPendingIRQ
    app_timer.o(i.timer_timeouts_check) refers to app_timer.o(.data) for .data
    app_timer.o(i.user_op_alloc) refers to app_timer.o(.bss) for .bss
    app_uart_fifo.o(i.app_uart_close) refers to nrfx_uarte.o(i.nrfx_uarte_uninit) for nrfx_uarte_uninit
    app_uart_fifo.o(i.app_uart_close) refers to nrfx_uart.o(i.nrfx_uart_uninit) for nrfx_uart_uninit
    app_uart_fifo.o(i.app_uart_close) refers to app_uart_fifo.o(.data) for .data
    app_uart_fifo.o(i.app_uart_close) refers to nrf_drv_uart.o(.data) for nrf_drv_uart_use_easy_dma
    app_uart_fifo.o(i.app_uart_flush) refers to app_fifo.o(i.app_fifo_flush) for app_fifo_flush
    app_uart_fifo.o(i.app_uart_flush) refers to app_uart_fifo.o(.bss) for .bss
    app_uart_fifo.o(i.app_uart_get) refers to app_fifo.o(i.app_fifo_get) for app_fifo_get
    app_uart_fifo.o(i.app_uart_get) refers to app_uart_fifo.o(i.nrf_drv_uart_rx) for nrf_drv_uart_rx
    app_uart_fifo.o(i.app_uart_get) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    app_uart_fifo.o(i.app_uart_get) refers to app_uart_fifo.o(.data) for .data
    app_uart_fifo.o(i.app_uart_get) refers to app_uart_fifo.o(.bss) for .bss
    app_uart_fifo.o(i.app_uart_init) refers to app_fifo.o(i.app_fifo_init) for app_fifo_init
    app_uart_fifo.o(i.app_uart_init) refers to memcpya.o(.text) for __aeabi_memcpy4
    app_uart_fifo.o(i.app_uart_init) refers to nrf_drv_uart.o(i.nrf_drv_uart_init) for nrf_drv_uart_init
    app_uart_fifo.o(i.app_uart_init) refers to app_uart_fifo.o(i.nrf_drv_uart_rx) for nrf_drv_uart_rx
    app_uart_fifo.o(i.app_uart_init) refers to app_uart_fifo.o(.data) for .data
    app_uart_fifo.o(i.app_uart_init) refers to app_uart_fifo.o(.bss) for .bss
    app_uart_fifo.o(i.app_uart_init) refers to app_uart_fifo.o(.constdata) for .constdata
    app_uart_fifo.o(i.app_uart_init) refers to app_uart_fifo.o(i.uart_event_handler) for uart_event_handler
    app_uart_fifo.o(i.app_uart_put) refers to app_fifo.o(i.app_fifo_put) for app_fifo_put
    app_uart_fifo.o(i.app_uart_put) refers to nrfx_uarte.o(i.nrfx_uarte_tx_in_progress) for nrfx_uarte_tx_in_progress
    app_uart_fifo.o(i.app_uart_put) refers to nrfx_uart.o(i.nrfx_uart_tx_in_progress) for nrfx_uart_tx_in_progress
    app_uart_fifo.o(i.app_uart_put) refers to app_fifo.o(i.app_fifo_get) for app_fifo_get
    app_uart_fifo.o(i.app_uart_put) refers to app_uart_fifo.o(i.nrf_drv_uart_tx) for nrf_drv_uart_tx
    app_uart_fifo.o(i.app_uart_put) refers to app_uart_fifo.o(.bss) for .bss
    app_uart_fifo.o(i.app_uart_put) refers to app_uart_fifo.o(.data) for .data
    app_uart_fifo.o(i.app_uart_put) refers to nrf_drv_uart.o(.data) for nrf_drv_uart_use_easy_dma
    app_uart_fifo.o(i.nrf_drv_uart_rx) refers to nrfx_uarte.o(i.nrfx_uarte_rx) for nrfx_uarte_rx
    app_uart_fifo.o(i.nrf_drv_uart_rx) refers to nrfx_uart.o(i.nrfx_uart_rx) for nrfx_uart_rx
    app_uart_fifo.o(i.nrf_drv_uart_rx) refers to nrf_drv_uart.o(.data) for nrf_drv_uart_use_easy_dma
    app_uart_fifo.o(i.nrf_drv_uart_tx) refers to nrfx_uarte.o(i.nrfx_uarte_tx) for nrfx_uarte_tx
    app_uart_fifo.o(i.nrf_drv_uart_tx) refers to nrfx_uart.o(i.nrfx_uart_tx) for nrfx_uart_tx
    app_uart_fifo.o(i.nrf_drv_uart_tx) refers to nrf_drv_uart.o(.data) for nrf_drv_uart_use_easy_dma
    app_uart_fifo.o(i.uart_event_handler) refers to app_uart_fifo.o(i.nrf_drv_uart_rx) for nrf_drv_uart_rx
    app_uart_fifo.o(i.uart_event_handler) refers to app_fifo.o(i.app_fifo_put) for app_fifo_put
    app_uart_fifo.o(i.uart_event_handler) refers to app_fifo.o(i.app_fifo_get) for app_fifo_get
    app_uart_fifo.o(i.uart_event_handler) refers to app_uart_fifo.o(i.nrf_drv_uart_tx) for nrf_drv_uart_tx
    app_uart_fifo.o(i.uart_event_handler) refers to app_uart_fifo.o(.data) for .data
    app_uart_fifo.o(i.uart_event_handler) refers to app_uart_fifo.o(.bss) for .bss
    app_util_platform.o(i.app_util_critical_region_enter) refers to app_util_platform.o(.bss) for .bss
    app_util_platform.o(i.app_util_critical_region_exit) refers to app_util_platform.o(.bss) for .bss
    app_util_platform.o(i.app_util_disable_irq) refers to app_util_platform.o(.data) for .data
    app_util_platform.o(i.app_util_enable_irq) refers to app_util_platform.o(.data) for .data
    nrf_assert.o(i.assert_nrf_callback) refers to app_error_weak.o(i.app_error_fault_handler) for app_error_fault_handler
    nrf_atfifo.o(i.nrf_atfifo_alloc_put) refers to nrf_atfifo.o(i.nrf_atfifo_item_alloc) for nrf_atfifo_item_alloc
    nrf_atfifo.o(i.nrf_atfifo_alloc_put) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_atfifo.o(i.nrf_atfifo_alloc_put) refers to nrf_atfifo.o(i.nrf_atfifo_item_put) for nrf_atfifo_item_put
    nrf_atfifo.o(i.nrf_atfifo_clear) refers to nrf_atfifo.o(.emb_text) for __asm___12_nrf_atfifo_c_51f461e1__nrf_atfifo_space_clear
    nrf_atfifo.o(i.nrf_atfifo_get_free) refers to nrf_atfifo.o(i.nrf_atfifo_item_get) for nrf_atfifo_item_get
    nrf_atfifo.o(i.nrf_atfifo_get_free) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_atfifo.o(i.nrf_atfifo_get_free) refers to nrf_atfifo.o(i.nrf_atfifo_item_free) for nrf_atfifo_item_free
    nrf_atfifo.o(i.nrf_atfifo_item_alloc) refers to nrf_atfifo.o(.emb_text) for __asm___12_nrf_atfifo_c_51f461e1__nrf_atfifo_wspace_req
    nrf_atfifo.o(i.nrf_atfifo_item_free) refers to nrf_atfifo.o(.emb_text) for __asm___12_nrf_atfifo_c_51f461e1__nrf_atfifo_rspace_close
    nrf_atfifo.o(i.nrf_atfifo_item_get) refers to nrf_atfifo.o(.emb_text) for __asm___12_nrf_atfifo_c_51f461e1__nrf_atfifo_rspace_req
    nrf_atfifo.o(i.nrf_atfifo_item_put) refers to nrf_atfifo.o(.emb_text) for __asm___12_nrf_atfifo_c_51f461e1__nrf_atfifo_wspace_close
    nrf_atflags.o(i.nrf_atflags_clear) refers to nrf_atomic.o(i.nrf_atomic_u32_and) for nrf_atomic_u32_and
    nrf_atflags.o(i.nrf_atflags_fetch_clear) refers to nrf_atomic.o(i.nrf_atomic_u32_fetch_and) for nrf_atomic_u32_fetch_and
    nrf_atflags.o(i.nrf_atflags_fetch_set) refers to nrf_atomic.o(i.nrf_atomic_u32_fetch_or) for nrf_atomic_u32_fetch_or
    nrf_atflags.o(i.nrf_atflags_find_and_clear_flag) refers to nrf_atflags.o(i.nrf_atflags_fetch_clear) for nrf_atflags_fetch_clear
    nrf_atflags.o(i.nrf_atflags_find_and_set_flag) refers to nrf_atflags.o(i.nrf_atflags_fetch_set) for nrf_atflags_fetch_set
    nrf_atflags.o(i.nrf_atflags_set) refers to nrf_atomic.o(i.nrf_atomic_u32_or) for nrf_atomic_u32_or
    nrf_atomic.o(i.nrf_atomic_flag_clear) refers to nrf_atomic.o(i.nrf_atomic_u32_and) for nrf_atomic_u32_and
    nrf_atomic.o(i.nrf_atomic_flag_clear_fetch) refers to nrf_atomic.o(i.nrf_atomic_u32_fetch_and) for nrf_atomic_u32_fetch_and
    nrf_atomic.o(i.nrf_atomic_flag_set) refers to nrf_atomic.o(i.nrf_atomic_u32_or) for nrf_atomic_u32_or
    nrf_atomic.o(i.nrf_atomic_flag_set_fetch) refers to nrf_atomic.o(i.nrf_atomic_u32_fetch_or) for nrf_atomic_u32_fetch_or
    nrf_atomic.o(i.nrf_atomic_u32_add) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_add
    nrf_atomic.o(i.nrf_atomic_u32_and) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_and
    nrf_atomic.o(i.nrf_atomic_u32_cmp_exch) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_cmp_exch
    nrf_atomic.o(i.nrf_atomic_u32_fetch_add) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_add
    nrf_atomic.o(i.nrf_atomic_u32_fetch_and) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_and
    nrf_atomic.o(i.nrf_atomic_u32_fetch_or) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_orr
    nrf_atomic.o(i.nrf_atomic_u32_fetch_store) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_mov
    nrf_atomic.o(i.nrf_atomic_u32_fetch_sub) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_sub
    nrf_atomic.o(i.nrf_atomic_u32_fetch_sub_hs) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_sub_hs
    nrf_atomic.o(i.nrf_atomic_u32_fetch_xor) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_eor
    nrf_atomic.o(i.nrf_atomic_u32_or) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_orr
    nrf_atomic.o(i.nrf_atomic_u32_store) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_mov
    nrf_atomic.o(i.nrf_atomic_u32_sub) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_sub
    nrf_atomic.o(i.nrf_atomic_u32_sub_hs) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_sub_hs
    nrf_atomic.o(i.nrf_atomic_u32_xor) refers to nrf_atomic.o(.emb_text) for __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_eor
    nrf_balloc.o(i.nrf_balloc_alloc) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_balloc.o(i.nrf_balloc_alloc) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_balloc.o(i.nrf_balloc_free) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_balloc.o(i.nrf_balloc_free) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_fprintf.o(i.nrf_fprintf) refers to nrf_fprintf_format.o(i.nrf_fprintf_fmt) for nrf_fprintf_fmt
    nrf_fprintf_format.o(i.buffer_add) refers to nrf_fprintf.o(i.nrf_fprintf_buffer_flush) for nrf_fprintf_buffer_flush
    nrf_fprintf_format.o(i.int_print) refers to nrf_fprintf_format.o(i.buffer_add) for buffer_add
    nrf_fprintf_format.o(i.int_print) refers to nrf_fprintf_format.o(i.unsigned_print) for unsigned_print
    nrf_fprintf_format.o(i.nrf_fprintf_fmt) refers to nrf_fprintf_format.o(i.buffer_add) for buffer_add
    nrf_fprintf_format.o(i.nrf_fprintf_fmt) refers to nrf_fprintf.o(i.nrf_fprintf_buffer_flush) for nrf_fprintf_buffer_flush
    nrf_fprintf_format.o(i.nrf_fprintf_fmt) refers to nrf_fprintf_format.o(i.int_print) for int_print
    nrf_fprintf_format.o(i.nrf_fprintf_fmt) refers to nrf_fprintf_format.o(i.unsigned_print) for unsigned_print
    nrf_fprintf_format.o(i.nrf_fprintf_fmt) refers to strlen.o(.text) for strlen
    nrf_fprintf_format.o(i.unsigned_print) refers to nrf_fprintf_format.o(i.buffer_add) for buffer_add
    nrf_fprintf_format.o(i.unsigned_print) refers to nrf_fprintf_format.o(.constdata) for .constdata
    nrf_memobj.o(i.memobj_op) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_memobj.o(i.nrf_memobj_alloc) refers to nrf_balloc.o(i.nrf_balloc_alloc) for nrf_balloc_alloc
    nrf_memobj.o(i.nrf_memobj_alloc) refers to nrf_memobj.o(i.nrf_memobj_free) for nrf_memobj_free
    nrf_memobj.o(i.nrf_memobj_free) refers to nrf_balloc.o(i.nrf_balloc_free) for nrf_balloc_free
    nrf_memobj.o(i.nrf_memobj_get) refers to nrf_atomic.o(i.nrf_atomic_u32_add) for nrf_atomic_u32_add
    nrf_memobj.o(i.nrf_memobj_pool_init) refers to nrf_balloc.o(i.nrf_balloc_init) for nrf_balloc_init
    nrf_memobj.o(i.nrf_memobj_put) refers to nrf_atomic.o(i.nrf_atomic_u32_sub) for nrf_atomic_u32_sub
    nrf_memobj.o(i.nrf_memobj_put) refers to nrf_memobj.o(i.nrf_memobj_free) for nrf_memobj_free
    nrf_memobj.o(i.nrf_memobj_read) refers to nrf_memobj.o(i.memobj_op) for memobj_op
    nrf_memobj.o(i.nrf_memobj_write) refers to nrf_memobj.o(i.memobj_op) for memobj_op
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_init) refers to nrf_section_iter.o(i.nrf_section_iter_init) for nrf_section_iter_init
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_init) refers to nrf_pwr_mgmt.o(.data) for .data
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_init) refers to nrf_pwr_mgmt.o(.constdata) for .constdata
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_init) refers to nrf_pwr_mgmt.o(.bss) for .bss
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_run) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_run) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_run) refers to nrf_sdh.o(i.nrf_sdh_is_enabled) for nrf_sdh_is_enabled
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_shutdown) refers to nrf_atomic.o(i.nrf_atomic_u32_fetch_store) for nrf_atomic_u32_fetch_store
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_shutdown) refers to nrf_pwr_mgmt.o(i.shutdown_process) for shutdown_process
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_shutdown) refers to nrf_pwr_mgmt.o(.data) for .data
    nrf_pwr_mgmt.o(i.shutdown_process) refers to nrf_section_iter.o(i.nrf_section_iter_next) for nrf_section_iter_next
    nrf_pwr_mgmt.o(i.shutdown_process) refers to nrf_log_frontend.o(i.nrf_log_panic) for nrf_log_panic
    nrf_pwr_mgmt.o(i.shutdown_process) refers to nrf_log_frontend.o(i.nrf_log_frontend_dequeue) for nrf_log_frontend_dequeue
    nrf_pwr_mgmt.o(i.shutdown_process) refers to nrf_sdh.o(i.nrf_sdh_is_enabled) for nrf_sdh_is_enabled
    nrf_pwr_mgmt.o(i.shutdown_process) refers to nrf_pwr_mgmt.o(.bss) for .bss
    nrf_pwr_mgmt.o(i.shutdown_process) refers to nrf_pwr_mgmt.o(.data) for .data
    nrf_pwr_mgmt.o(.constdata) refers to nrf_pwr_mgmt.o(.constdata) for pwr_mgmt_data_array
    nrf_pwr_mgmt.o(log_const_data) refers to nrf_pwr_mgmt.o(.conststrlit) for .conststrlit
    nrf_ringbuf.o(i.nrf_ringbuf_alloc) refers to nrf_atomic.o(i.nrf_atomic_flag_set_fetch) for nrf_atomic_flag_set_fetch
    nrf_ringbuf.o(i.nrf_ringbuf_alloc) refers to nrf_atomic.o(i.nrf_atomic_flag_clear) for nrf_atomic_flag_clear
    nrf_ringbuf.o(i.nrf_ringbuf_cpy_get) refers to nrf_atomic.o(i.nrf_atomic_flag_set_fetch) for nrf_atomic_flag_set_fetch
    nrf_ringbuf.o(i.nrf_ringbuf_cpy_get) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_ringbuf.o(i.nrf_ringbuf_cpy_get) refers to nrf_atomic.o(i.nrf_atomic_flag_clear) for nrf_atomic_flag_clear
    nrf_ringbuf.o(i.nrf_ringbuf_cpy_put) refers to nrf_atomic.o(i.nrf_atomic_flag_set_fetch) for nrf_atomic_flag_set_fetch
    nrf_ringbuf.o(i.nrf_ringbuf_cpy_put) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_ringbuf.o(i.nrf_ringbuf_cpy_put) refers to nrf_atomic.o(i.nrf_atomic_flag_clear) for nrf_atomic_flag_clear
    nrf_ringbuf.o(i.nrf_ringbuf_free) refers to nrf_atomic.o(i.nrf_atomic_flag_clear) for nrf_atomic_flag_clear
    nrf_ringbuf.o(i.nrf_ringbuf_get) refers to nrf_atomic.o(i.nrf_atomic_flag_set_fetch) for nrf_atomic_flag_set_fetch
    nrf_ringbuf.o(i.nrf_ringbuf_get) refers to nrf_atomic.o(i.nrf_atomic_flag_clear) for nrf_atomic_flag_clear
    nrf_ringbuf.o(i.nrf_ringbuf_put) refers to nrf_atomic.o(i.nrf_atomic_flag_clear_fetch) for nrf_atomic_flag_clear_fetch
    nrf_section_iter.o(i.nrf_section_iter_init) refers to nrf_section_iter.o(i.nrf_section_iter_item_set) for nrf_section_iter_item_set
    nrf_section_iter.o(i.nrf_section_iter_next) refers to nrf_section_iter.o(i.nrf_section_iter_item_set) for nrf_section_iter_item_set
    nrf_strerror.o(i.nrf_strerror_find) refers to nrf_strerror.o(.constdata) for .constdata
    nrf_strerror.o(i.nrf_strerror_get) refers to nrf_strerror.o(i.nrf_strerror_find) for nrf_strerror_find
    nrf_strerror.o(i.nrf_strerror_get) refers to nrf_strerror.o(.constdata) for .constdata
    nrf_strerror.o(.constdata) refers to nrf_strerror.o(.conststring) for .conststring
    retarget.o(i.fgetc) refers to app_uart_fifo.o(i.app_uart_get) for app_uart_get
    retarget.o(i.fputc) refers to app_uart_fifo.o(i.app_uart_put) for app_uart_put
    nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_init) refers to segger_rtt.o(i.SEGGER_RTT_Init) for SEGGER_RTT_Init
    nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_put) refers to nrf_log_backend_serial.o(i.nrf_log_backend_serial_put) for nrf_log_backend_serial_put
    nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_put) refers to nrf_log_backend_rtt.o(i.serial_tx) for serial_tx
    nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_put) refers to nrf_log_backend_rtt.o(.bss) for .bss
    nrf_log_backend_rtt.o(i.serial_tx) refers to segger_rtt.o(i.SEGGER_RTT_WriteNoLock) for SEGGER_RTT_WriteNoLock
    nrf_log_backend_rtt.o(i.serial_tx) refers to nrf_log_backend_rtt.o(.data) for .data
    nrf_log_backend_rtt.o(i.serial_tx) refers to nrf_log_backend_rtt.o(.constdata) for .constdata
    nrf_log_backend_rtt.o(.constdata) refers to nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_put) for nrf_log_backend_rtt_put
    nrf_log_backend_rtt.o(.constdata) refers to nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_panic_set) for nrf_log_backend_rtt_panic_set
    nrf_log_backend_rtt.o(.constdata) refers to nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_flush) for nrf_log_backend_rtt_flush
    nrf_log_backend_serial.o(i.nrf_log_backend_serial_put) refers to nrf_memobj.o(i.nrf_memobj_get) for nrf_memobj_get
    nrf_log_backend_serial.o(i.nrf_log_backend_serial_put) refers to memseta.o(.text) for __aeabi_memclr4
    nrf_log_backend_serial.o(i.nrf_log_backend_serial_put) refers to nrf_memobj.o(i.nrf_memobj_read) for nrf_memobj_read
    nrf_log_backend_serial.o(i.nrf_log_backend_serial_put) refers to nrf_log_str_formatter.o(i.nrf_log_std_entry_process) for nrf_log_std_entry_process
    nrf_log_backend_serial.o(i.nrf_log_backend_serial_put) refers to nrf_log_str_formatter.o(i.nrf_log_hexdump_entry_process) for nrf_log_hexdump_entry_process
    nrf_log_backend_serial.o(i.nrf_log_backend_serial_put) refers to nrf_memobj.o(i.nrf_memobj_put) for nrf_memobj_put
    nrf_log_default_backends.o(i.nrf_log_default_backends_init) refers to nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_init) for nrf_log_backend_rtt_init
    nrf_log_default_backends.o(i.nrf_log_default_backends_init) refers to nrf_log_frontend.o(i.nrf_log_backend_add) for nrf_log_backend_add
    nrf_log_default_backends.o(i.nrf_log_default_backends_init) refers to nrf_log_default_backends.o(log_backends) for log_backends
    nrf_log_default_backends.o(log_backends) refers to nrf_log_backend_rtt.o(.constdata) for nrf_log_backend_rtt_api
    nrf_log_default_backends.o(log_backends) refers to nrf_log_default_backends.o(.conststrlit) for .conststrlit
    nrf_log_default_backends.o(log_backends) refers to nrf_log_default_backends.o(.data) for log_backend_cb_rtt_log_backend
    nrf_log_frontend.o(i.buf_prealloc) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_log_frontend.o(i.buf_prealloc) refers to nrf_atomic.o(i.nrf_atomic_u32_add) for nrf_atomic_u32_add
    nrf_log_frontend.o(i.buf_prealloc) refers to nrf_log_frontend.o(i.log_skip) for log_skip
    nrf_log_frontend.o(i.buf_prealloc) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_log_frontend.o(i.buf_prealloc) refers to nrf_log_frontend.o(.bss) for .bss
    nrf_log_frontend.o(i.buffer_is_empty) refers to nrf_log_frontend.o(.bss) for .bss
    nrf_log_frontend.o(i.dropped_sat16_get) refers to nrf_atomic.o(i.nrf_atomic_u32_fetch_store) for nrf_atomic_u32_fetch_store
    nrf_log_frontend.o(i.dropped_sat16_get) refers to nrf_log_frontend.o(.bss) for .bss
    nrf_log_frontend.o(i.log_skip) refers to nrf_atomic.o(i.nrf_atomic_flag_set) for nrf_atomic_flag_set
    nrf_log_frontend.o(i.log_skip) refers to nrf_log_frontend.o(i.invalid_packets_omit) for invalid_packets_omit
    nrf_log_frontend.o(i.log_skip) refers to nrf_atomic.o(i.nrf_atomic_flag_clear_fetch) for nrf_atomic_flag_clear_fetch
    nrf_log_frontend.o(i.log_skip) refers to nrf_log_frontend.o(.bss) for .bss
    nrf_log_frontend.o(i.module_idx_get) refers to nrf_log_frontend.o(i.nrf_log_module_cnt_get) for nrf_log_module_cnt_get
    nrf_log_frontend.o(i.nrf_log_backend_add) refers to nrf_log_frontend.o(.bss) for .bss
    nrf_log_frontend.o(i.nrf_log_backend_remove) refers to nrf_log_frontend.o(.bss) for .bss
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to nrf_log_frontend.o(i.buffer_is_empty) for buffer_is_empty
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to nrf_log_frontend.o(i.invalid_packets_omit) for invalid_packets_omit
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to nrf_memobj.o(i.nrf_memobj_alloc) for nrf_memobj_alloc
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to nrf_memobj.o(i.nrf_memobj_get) for nrf_memobj_get
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to nrf_memobj.o(i.nrf_memobj_write) for nrf_memobj_write
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to nrf_memobj.o(i.nrf_memobj_put) for nrf_memobj_put
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_0) for nrf_log_frontend_std_0
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to nrf_log_frontend.o(.bss) for .bss
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to nrf_log_frontend.o(nrf_balloc) for nrf_balloc
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to nrf_log_frontend.o(log_const_data) for log_const_data
    nrf_log_frontend.o(i.nrf_log_frontend_hexdump) refers to nrf_log_frontend.o(i.buf_prealloc) for buf_prealloc
    nrf_log_frontend.o(i.nrf_log_frontend_hexdump) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_log_frontend.o(i.nrf_log_frontend_hexdump) refers to nrf_log_frontend.o(i.dropped_sat16_get) for dropped_sat16_get
    nrf_log_frontend.o(i.nrf_log_frontend_hexdump) refers to nrf_log_frontend.o(i.nrf_log_frontend_dequeue) for nrf_log_frontend_dequeue
    nrf_log_frontend.o(i.nrf_log_frontend_hexdump) refers to nrf_log_frontend.o(.bss) for .bss
    nrf_log_frontend.o(i.nrf_log_frontend_std_0) refers to nrf_log_frontend.o(i.std_n) for std_n
    nrf_log_frontend.o(i.nrf_log_frontend_std_1) refers to nrf_log_frontend.o(i.std_n) for std_n
    nrf_log_frontend.o(i.nrf_log_frontend_std_2) refers to nrf_log_frontend.o(i.std_n) for std_n
    nrf_log_frontend.o(i.nrf_log_frontend_std_3) refers to nrf_log_frontend.o(i.std_n) for std_n
    nrf_log_frontend.o(i.nrf_log_frontend_std_4) refers to nrf_log_frontend.o(i.std_n) for std_n
    nrf_log_frontend.o(i.nrf_log_frontend_std_5) refers to nrf_log_frontend.o(i.std_n) for std_n
    nrf_log_frontend.o(i.nrf_log_frontend_std_6) refers to nrf_log_frontend.o(i.std_n) for std_n
    nrf_log_frontend.o(i.nrf_log_init) refers to nrf_memobj.o(i.nrf_memobj_pool_init) for nrf_memobj_pool_init
    nrf_log_frontend.o(i.nrf_log_init) refers to nrf_ringbuf.o(i.nrf_ringbuf_init) for nrf_ringbuf_init
    nrf_log_frontend.o(i.nrf_log_init) refers to nrf_log_frontend.o(.bss) for .bss
    nrf_log_frontend.o(i.nrf_log_init) refers to nrf_log_frontend.o(nrf_balloc) for nrf_balloc
    nrf_log_frontend.o(i.nrf_log_init) refers to nrf_log_frontend.o(.constdata) for .constdata
    nrf_log_frontend.o(i.nrf_log_module_filter_get) refers to nrf_log_frontend.o(i.module_idx_get) for module_idx_get
    nrf_log_frontend.o(i.nrf_log_module_name_get) refers to nrf_log_frontend.o(i.module_idx_get) for module_idx_get
    nrf_log_frontend.o(i.nrf_log_panic) refers to nrf_log_frontend.o(.bss) for .bss
    nrf_log_frontend.o(i.nrf_log_push) refers to strlen.o(.text) for strlen
    nrf_log_frontend.o(i.nrf_log_push) refers to nrf_ringbuf.o(i.nrf_ringbuf_alloc) for nrf_ringbuf_alloc
    nrf_log_frontend.o(i.nrf_log_push) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_log_frontend.o(i.nrf_log_push) refers to nrf_ringbuf.o(i.nrf_ringbuf_put) for nrf_ringbuf_put
    nrf_log_frontend.o(i.nrf_log_push) refers to nrf_ringbuf.o(i.nrf_ringbuf_free) for nrf_ringbuf_free
    nrf_log_frontend.o(i.nrf_log_push) refers to nrf_log_frontend.o(.bss) for .bss
    nrf_log_frontend.o(i.nrf_log_push) refers to nrf_log_frontend.o(.constdata) for .constdata
    nrf_log_frontend.o(i.std_n) refers to nrf_log_frontend.o(i.buf_prealloc) for buf_prealloc
    nrf_log_frontend.o(i.std_n) refers to nrf_log_frontend.o(i.dropped_sat16_get) for dropped_sat16_get
    nrf_log_frontend.o(i.std_n) refers to nrf_log_frontend.o(i.nrf_log_frontend_dequeue) for nrf_log_frontend_dequeue
    nrf_log_frontend.o(i.std_n) refers to nrf_log_frontend.o(.bss) for .bss
    nrf_log_frontend.o(.constdata) refers to nrf_log_frontend.o(.bss) for m_log_push_ringbuf_buf
    nrf_log_frontend.o(.constdata) refers to nrf_log_frontend.o(.bss) for m_log_push_ringbuf_cb
    nrf_log_frontend.o(log_const_data) refers to nrf_log_frontend.o(.conststrlit) for .conststrlit
    nrf_log_frontend.o(nrf_balloc) refers to nrf_log_frontend.o(.data) for log_mempool_nrf_balloc_cb
    nrf_log_frontend.o(nrf_balloc) refers to nrf_log_frontend.o(.data) for log_mempool_nrf_balloc_pool_stack
    nrf_log_frontend.o(nrf_balloc) refers to nrf_log_frontend.o(.bss) for log_mempool_nrf_balloc_pool_mem
    nrf_log_str_formatter.o(i.nrf_log_hexdump_entry_process) refers to nrf_log_str_formatter.o(i.prefix_process) for prefix_process
    nrf_log_str_formatter.o(i.nrf_log_hexdump_entry_process) refers to nrf_fprintf.o(i.nrf_fprintf) for nrf_fprintf
    nrf_log_str_formatter.o(i.nrf_log_hexdump_entry_process) refers to ctype_o.o(.text) for __rt_ctype_table
    nrf_log_str_formatter.o(i.nrf_log_hexdump_entry_process) refers to nrf_log_str_formatter.o(i.postfix_process) for postfix_process
    nrf_log_str_formatter.o(i.nrf_log_std_entry_process) refers to nrf_log_str_formatter.o(i.prefix_process) for prefix_process
    nrf_log_str_formatter.o(i.nrf_log_std_entry_process) refers to nrf_fprintf.o(i.nrf_fprintf) for nrf_fprintf
    nrf_log_str_formatter.o(i.nrf_log_std_entry_process) refers to nrf_log_str_formatter.o(i.postfix_process) for postfix_process
    nrf_log_str_formatter.o(i.nrf_log_str_formatter_timestamp_freq_set) refers to nrf_log_str_formatter.o(.data) for .data
    nrf_log_str_formatter.o(i.postfix_process) refers to nrf_fprintf.o(i.nrf_fprintf) for nrf_fprintf
    nrf_log_str_formatter.o(i.postfix_process) refers to nrf_fprintf.o(i.nrf_fprintf_buffer_flush) for nrf_fprintf_buffer_flush
    nrf_log_str_formatter.o(i.postfix_process) refers to nrf_log_str_formatter.o(.data) for .data
    nrf_log_str_formatter.o(i.prefix_process) refers to nrf_fprintf.o(i.nrf_fprintf) for nrf_fprintf
    nrf_log_str_formatter.o(i.prefix_process) refers to nrf_log_frontend.o(i.nrf_log_color_id_get) for nrf_log_color_id_get
    nrf_log_str_formatter.o(i.prefix_process) refers to nrf_log_frontend.o(i.nrf_log_module_name_get) for nrf_log_module_name_get
    nrf_log_str_formatter.o(i.prefix_process) refers to nrf_log_str_formatter.o(.data) for .data
    nrf_log_str_formatter.o(.data) refers to nrf_log_str_formatter.o(.conststring) for .conststring
    segger_rtt.o(i.SEGGER_RTT_AllocDownBuffer) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_AllocDownBuffer) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_AllocDownBuffer) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_AllocDownBuffer) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_AllocUpBuffer) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_AllocUpBuffer) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_AllocUpBuffer) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_AllocUpBuffer) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_ConfigDownBuffer) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_ConfigDownBuffer) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_ConfigDownBuffer) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_ConfigDownBuffer) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_ConfigUpBuffer) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_ConfigUpBuffer) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_ConfigUpBuffer) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_ConfigUpBuffer) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_GetKey) refers to segger_rtt.o(i.SEGGER_RTT_Read) for SEGGER_RTT_Read
    segger_rtt.o(i.SEGGER_RTT_HasData) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_HasKey) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_HasKey) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_Init) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_PutChar) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_PutChar) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_PutChar) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_PutChar) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_PutCharSkip) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_PutCharSkip) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_PutCharSkip) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_PutCharSkip) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_PutCharSkipNoLock) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_Read) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_Read) refers to segger_rtt.o(i.SEGGER_RTT_ReadNoLock) for SEGGER_RTT_ReadNoLock
    segger_rtt.o(i.SEGGER_RTT_Read) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_ReadNoLock) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_ReadNoLock) refers to memcpya.o(.text) for __aeabi_memcpy
    segger_rtt.o(i.SEGGER_RTT_ReadNoLock) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_SetFlagsDownBuffer) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_SetFlagsDownBuffer) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_SetFlagsDownBuffer) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_SetFlagsDownBuffer) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_SetFlagsUpBuffer) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_SetFlagsUpBuffer) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_SetFlagsUpBuffer) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_SetFlagsUpBuffer) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_SetNameDownBuffer) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_SetNameDownBuffer) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_SetNameDownBuffer) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_SetNameDownBuffer) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_SetNameUpBuffer) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_SetNameUpBuffer) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_SetNameUpBuffer) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_SetNameUpBuffer) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_SetTerminal) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_SetTerminal) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_SetTerminal) refers to segger_rtt.o(i._GetAvailWriteSpace) for _GetAvailWriteSpace
    segger_rtt.o(i.SEGGER_RTT_SetTerminal) refers to segger_rtt.o(i._WriteNoCheck) for _WriteNoCheck
    segger_rtt.o(i.SEGGER_RTT_SetTerminal) refers to segger_rtt.o(i._WriteBlocking) for _WriteBlocking
    segger_rtt.o(i.SEGGER_RTT_SetTerminal) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_SetTerminal) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_SetTerminal) refers to segger_rtt.o(.data) for .data
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to strlen.o(.text) for strlen
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to segger_rtt.o(i._GetAvailWriteSpace) for _GetAvailWriteSpace
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to segger_rtt.o(i._PostTerminalSwitch) for _PostTerminalSwitch
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to segger_rtt.o(i._WriteBlocking) for _WriteBlocking
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to segger_rtt.o(.data) for .data
    segger_rtt.o(i.SEGGER_RTT_WaitKey) refers to segger_rtt.o(i.SEGGER_RTT_GetKey) for SEGGER_RTT_GetKey
    segger_rtt.o(i.SEGGER_RTT_Write) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_Write) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_Write) refers to segger_rtt.o(i.SEGGER_RTT_WriteNoLock) for SEGGER_RTT_WriteNoLock
    segger_rtt.o(i.SEGGER_RTT_Write) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_Write) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_WriteNoLock) refers to segger_rtt.o(i._GetAvailWriteSpace) for _GetAvailWriteSpace
    segger_rtt.o(i.SEGGER_RTT_WriteNoLock) refers to segger_rtt.o(i._WriteNoCheck) for _WriteNoCheck
    segger_rtt.o(i.SEGGER_RTT_WriteNoLock) refers to segger_rtt.o(i._WriteBlocking) for _WriteBlocking
    segger_rtt.o(i.SEGGER_RTT_WriteNoLock) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_WriteSkipNoLock) refers to memcpya.o(.text) for __aeabi_memcpy
    segger_rtt.o(i.SEGGER_RTT_WriteSkipNoLock) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i.SEGGER_RTT_WriteString) refers to strlen.o(.text) for strlen
    segger_rtt.o(i.SEGGER_RTT_WriteString) refers to segger_rtt.o(i.SEGGER_RTT_Write) for SEGGER_RTT_Write
    segger_rtt.o(i.SEGGER_RTT_WriteWithOverwriteNoLock) refers to memcpya.o(.text) for __aeabi_memcpy
    segger_rtt.o(i.SEGGER_RTT_WriteWithOverwriteNoLock) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i._DoInit) refers to strcpy.o(.text) for strcpy
    segger_rtt.o(i._DoInit) refers to segger_rtt.o(.bss) for .bss
    segger_rtt.o(i._PostTerminalSwitch) refers to segger_rtt.o(i._WriteBlocking) for _WriteBlocking
    segger_rtt.o(i._PostTerminalSwitch) refers to segger_rtt.o(.data) for .data
    segger_rtt.o(i._WriteBlocking) refers to memcpya.o(.text) for __aeabi_memcpy
    segger_rtt.o(i._WriteNoCheck) refers to memcpya.o(.text) for __aeabi_memcpy
    segger_rtt_printf.o(i.SEGGER_RTT_printf) refers to segger_rtt_printf.o(i.SEGGER_RTT_vprintf) for SEGGER_RTT_vprintf
    segger_rtt_printf.o(i.SEGGER_RTT_vprintf) refers to segger_rtt_printf.o(i._StoreChar) for _StoreChar
    segger_rtt_printf.o(i.SEGGER_RTT_vprintf) refers to segger_rtt_printf.o(i._PrintInt) for _PrintInt
    segger_rtt_printf.o(i.SEGGER_RTT_vprintf) refers to segger_rtt_printf.o(i._PrintUnsigned) for _PrintUnsigned
    segger_rtt_printf.o(i.SEGGER_RTT_vprintf) refers to segger_rtt.o(i.SEGGER_RTT_Write) for SEGGER_RTT_Write
    segger_rtt_printf.o(i._PrintInt) refers to segger_rtt_printf.o(i._StoreChar) for _StoreChar
    segger_rtt_printf.o(i._PrintInt) refers to segger_rtt_printf.o(i._PrintUnsigned) for _PrintUnsigned
    segger_rtt_printf.o(i._PrintUnsigned) refers to segger_rtt_printf.o(i._StoreChar) for _StoreChar
    segger_rtt_printf.o(i._PrintUnsigned) refers to segger_rtt_printf.o(.constdata) for .constdata
    segger_rtt_printf.o(i._StoreChar) refers to segger_rtt.o(i.SEGGER_RTT_Write) for SEGGER_RTT_Write
    nrf_sdh.o(i.SWI2_EGU2_IRQHandler) refers to nrf_sdh.o(i.nrf_sdh_evts_poll) for nrf_sdh_evts_poll
    nrf_sdh.o(i.nrf_sdh_disable_request) refers to nrf_sdh.o(i.sdh_request_observer_notify) for sdh_request_observer_notify
    nrf_sdh.o(i.nrf_sdh_disable_request) refers to nrf_sdh.o(i.sdh_state_observer_notify) for sdh_state_observer_notify
    nrf_sdh.o(i.nrf_sdh_disable_request) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_sdh.o(i.nrf_sdh_disable_request) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_sdh.o(i.nrf_sdh_disable_request) refers to nrf_sdh.o(i.softdevice_evt_irq_disable) for softdevice_evt_irq_disable
    nrf_sdh.o(i.nrf_sdh_disable_request) refers to nrf_sdh.o(.data) for .data
    nrf_sdh.o(i.nrf_sdh_enable_request) refers to nrf_sdh.o(i.sdh_request_observer_notify) for sdh_request_observer_notify
    nrf_sdh.o(i.nrf_sdh_enable_request) refers to nrf_sdh.o(i.sdh_state_observer_notify) for sdh_state_observer_notify
    nrf_sdh.o(i.nrf_sdh_enable_request) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_sdh.o(i.nrf_sdh_enable_request) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_sdh.o(i.nrf_sdh_enable_request) refers to nrf_sdh.o(i.softdevices_evt_irq_enable) for softdevices_evt_irq_enable
    nrf_sdh.o(i.nrf_sdh_enable_request) refers to nrf_sdh.o(.data) for .data
    nrf_sdh.o(i.nrf_sdh_enable_request) refers to nrf_sdh.o(.constdata) for .constdata
    nrf_sdh.o(i.nrf_sdh_enable_request) refers to app_error_weak.o(i.app_error_fault_handler) for app_error_fault_handler
    nrf_sdh.o(i.nrf_sdh_evts_poll) refers to nrf_section_iter.o(i.nrf_section_iter_init) for nrf_section_iter_init
    nrf_sdh.o(i.nrf_sdh_evts_poll) refers to nrf_section_iter.o(i.nrf_section_iter_next) for nrf_section_iter_next
    nrf_sdh.o(i.nrf_sdh_evts_poll) refers to nrf_sdh.o(.constdata) for .constdata
    nrf_sdh.o(i.nrf_sdh_is_enabled) refers to nrf_sdh.o(.data) for .data
    nrf_sdh.o(i.nrf_sdh_is_suspended) refers to nrf_sdh.o(.data) for .data
    nrf_sdh.o(i.nrf_sdh_request_continue) refers to nrf_sdh.o(i.nrf_sdh_disable_request) for nrf_sdh_disable_request
    nrf_sdh.o(i.nrf_sdh_request_continue) refers to nrf_sdh.o(i.nrf_sdh_enable_request) for nrf_sdh_enable_request
    nrf_sdh.o(i.nrf_sdh_request_continue) refers to nrf_sdh.o(.data) for .data
    nrf_sdh.o(i.nrf_sdh_resume) refers to nrf_sdh.o(i.__sd_nvic_app_accessible_irq) for __sd_nvic_app_accessible_irq
    nrf_sdh.o(i.nrf_sdh_resume) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    nrf_sdh.o(i.nrf_sdh_resume) refers to nrf_sdh.o(i.softdevices_evt_irq_enable) for softdevices_evt_irq_enable
    nrf_sdh.o(i.nrf_sdh_resume) refers to nrf_sdh.o(.data) for .data
    nrf_sdh.o(i.nrf_sdh_suspend) refers to nrf_sdh.o(i.softdevice_evt_irq_disable) for softdevice_evt_irq_disable
    nrf_sdh.o(i.nrf_sdh_suspend) refers to nrf_sdh.o(.data) for .data
    nrf_sdh.o(i.sdh_request_observer_notify) refers to nrf_section_iter.o(i.nrf_section_iter_init) for nrf_section_iter_init
    nrf_sdh.o(i.sdh_request_observer_notify) refers to nrf_section_iter.o(i.nrf_section_iter_next) for nrf_section_iter_next
    nrf_sdh.o(i.sdh_request_observer_notify) refers to nrf_sdh.o(.constdata) for .constdata
    nrf_sdh.o(i.sdh_state_observer_notify) refers to nrf_section_iter.o(i.nrf_section_iter_init) for nrf_section_iter_init
    nrf_sdh.o(i.sdh_state_observer_notify) refers to nrf_section_iter.o(i.nrf_section_iter_next) for nrf_section_iter_next
    nrf_sdh.o(i.sdh_state_observer_notify) refers to nrf_sdh.o(.constdata) for .constdata
    nrf_sdh.o(i.softdevice_evt_irq_disable) refers to nrf_sdh.o(i.__sd_nvic_app_accessible_irq) for __sd_nvic_app_accessible_irq
    nrf_sdh.o(i.softdevice_evt_irq_disable) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    nrf_sdh.o(i.softdevice_evt_irq_disable) refers to app_util_platform.o(.bss) for nrf_nvic_state
    nrf_sdh.o(i.softdevices_evt_irq_enable) refers to nrf_sdh.o(i.__sd_nvic_app_accessible_irq) for __sd_nvic_app_accessible_irq
    nrf_sdh.o(i.softdevices_evt_irq_enable) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    nrf_sdh.o(i.softdevices_evt_irq_enable) refers to app_util_platform.o(.bss) for nrf_nvic_state
    nrf_sdh.o(.constdata) refers to nrf_sdh.o(.constdata) for sdh_req_observers_array
    nrf_sdh.o(.constdata) refers to nrf_sdh.o(.constdata) for sdh_state_observers_array
    nrf_sdh.o(.constdata) refers to nrf_sdh.o(.constdata) for sdh_stack_observers_array
    nrf_sdh.o(log_const_data) refers to nrf_sdh.o(.conststrlit) for .conststrlit
    nrf_sdh_ble.o(i.nrf_sdh_ble_app_ram_start_get) refers to nrf_sdh_ble.o(.constdata) for .constdata
    nrf_sdh_ble.o(i.nrf_sdh_ble_default_cfg_set) refers to nrf_sdh_ble.o(i.nrf_sdh_ble_app_ram_start_get) for nrf_sdh_ble_app_ram_start_get
    nrf_sdh_ble.o(i.nrf_sdh_ble_default_cfg_set) refers to nrf_strerror.o(i.nrf_strerror_get) for nrf_strerror_get
    nrf_sdh_ble.o(i.nrf_sdh_ble_default_cfg_set) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_1) for nrf_log_frontend_std_1
    nrf_sdh_ble.o(i.nrf_sdh_ble_default_cfg_set) refers to nrf_sdh_ble.o(log_const_data) for log_const_data
    nrf_sdh_ble.o(i.nrf_sdh_ble_default_cfg_set) refers to nrf_sdh_ble.o(.conststring) for .conststring
    nrf_sdh_ble.o(i.nrf_sdh_ble_enable) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_0) for nrf_log_frontend_std_0
    nrf_sdh_ble.o(i.nrf_sdh_ble_enable) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_2) for nrf_log_frontend_std_2
    nrf_sdh_ble.o(i.nrf_sdh_ble_enable) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_1) for nrf_log_frontend_std_1
    nrf_sdh_ble.o(i.nrf_sdh_ble_enable) refers to nrf_strerror.o(i.nrf_strerror_get) for nrf_strerror_get
    nrf_sdh_ble.o(i.nrf_sdh_ble_enable) refers to nrf_sdh_ble.o(log_const_data) for log_const_data
    nrf_sdh_ble.o(i.nrf_sdh_ble_enable) refers to nrf_sdh_ble.o(.data) for .data
    nrf_sdh_ble.o(i.nrf_sdh_ble_evts_poll) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    nrf_sdh_ble.o(i.nrf_sdh_ble_evts_poll) refers to nrf_section_iter.o(i.nrf_section_iter_init) for nrf_section_iter_init
    nrf_sdh_ble.o(i.nrf_sdh_ble_evts_poll) refers to nrf_section_iter.o(i.nrf_section_iter_next) for nrf_section_iter_next
    nrf_sdh_ble.o(i.nrf_sdh_ble_evts_poll) refers to nrf_sdh_ble.o(.data) for .data
    nrf_sdh_ble.o(i.nrf_sdh_ble_evts_poll) refers to nrf_sdh_ble.o(.constdata) for .constdata
    nrf_sdh_ble.o(.constdata) refers to nrf_sdh_ble.o(.constdata) for sdh_ble_observers_array
    nrf_sdh_ble.o(log_const_data) refers to nrf_sdh_ble.o(.conststrlit) for .conststrlit
    nrf_sdh_ble.o(sdh_stack_observers0) refers to nrf_sdh_ble.o(i.nrf_sdh_ble_evts_poll) for nrf_sdh_ble_evts_poll
    nrf_sdh_soc.o(i.nrf_sdh_soc_evts_poll) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    nrf_sdh_soc.o(i.nrf_sdh_soc_evts_poll) refers to nrf_section_iter.o(i.nrf_section_iter_init) for nrf_section_iter_init
    nrf_sdh_soc.o(i.nrf_sdh_soc_evts_poll) refers to nrf_section_iter.o(i.nrf_section_iter_next) for nrf_section_iter_next
    nrf_sdh_soc.o(i.nrf_sdh_soc_evts_poll) refers to nrf_sdh_soc.o(.constdata) for .constdata
    nrf_sdh_soc.o(.constdata) refers to nrf_sdh_soc.o(.constdata) for sdh_soc_observers_array
    nrf_sdh_soc.o(log_const_data) refers to nrf_sdh_soc.o(.conststrlit) for .conststrlit
    nrf_sdh_soc.o(sdh_stack_observers0) refers to nrf_sdh_soc.o(i.nrf_sdh_soc_evts_poll) for nrf_sdh_soc_evts_poll
    arm_startup_nrf52.o(RESET) refers to arm_startup_nrf52.o(STACK) for __initial_sp
    arm_startup_nrf52.o(RESET) refers to arm_startup_nrf52.o(.text) for Reset_Handler
    arm_startup_nrf52.o(RESET) refers to nrfx_clock.o(i.POWER_CLOCK_IRQHandler) for POWER_CLOCK_IRQHandler
    arm_startup_nrf52.o(RESET) refers to nrfx_prs.o(i.UARTE0_UART0_IRQHandler) for UARTE0_UART0_IRQHandler
    arm_startup_nrf52.o(RESET) refers to nrfx_twim.o(i.SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler) for SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler
    arm_startup_nrf52.o(RESET) refers to nrfx_gpiote.o(i.GPIOTE_IRQHandler) for GPIOTE_IRQHandler
    arm_startup_nrf52.o(RESET) refers to nrfx_saadc.o(i.SAADC_IRQHandler) for SAADC_IRQHandler
    arm_startup_nrf52.o(RESET) refers to nrfx_timer.o(i.TIMER0_IRQHandler) for TIMER0_IRQHandler
    arm_startup_nrf52.o(RESET) refers to app_timer.o(i.RTC1_IRQHandler) for RTC1_IRQHandler
    arm_startup_nrf52.o(RESET) refers to app_timer.o(i.SWI0_EGU0_IRQHandler) for SWI0_EGU0_IRQHandler
    arm_startup_nrf52.o(RESET) refers to nrf_sdh.o(i.SWI2_EGU2_IRQHandler) for SWI2_EGU2_IRQHandler
    arm_startup_nrf52.o(.text) refers to system_nrf52.o(i.SystemInit) for SystemInit
    arm_startup_nrf52.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    system_nrf52.o(i.SystemCoreClockUpdate) refers to system_nrf52.o(.data) for .data
    system_nrf52.o(i.SystemInit) refers to system_nrf52.o(.data) for .data
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    ctype_o.o(.text) refers to ctype_o.o(.constdata) for .constdata
    ctype_o.o(.constdata) refers to ctype_o.o(.constdata) for __ctype_table
    isalnum_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    isalpha_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    isblank_o.o(.text) refers to ctype_o.o(.constdata) for __ctype_table
    iscntrl_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    isdigit_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    isgraph_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    islower_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    isprint_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    ispunct_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    isspace_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    isupper_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    isxdigit_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to retarget.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to retarget.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to retarget.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to retarget.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to retarget.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to retarget.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to retarget.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to retarget.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to retarget.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to retarget.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to retarget.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to retarget.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to retarget.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to retarget.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to retarget.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to retarget.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to retarget.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to retarget.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to retarget.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to retarget.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to retarget.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to retarget.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to retarget.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to retarget.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to retarget.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to retarget.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to retarget.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to retarget.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to retarget.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to retarget.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to retarget.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to retarget.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to retarget.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to retarget.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to retarget.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to retarget.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to retarget.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to retarget.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to retarget.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to retarget.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to retarget.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to retarget.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to retarget.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to retarget.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to retarget.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to retarget.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to retarget.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to retarget.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to retarget.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to retarget.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to retarget.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to retarget.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to retarget.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to retarget.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to retarget.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to retarget.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to retarget.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to retarget.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to retarget.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to retarget.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to retarget.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to retarget.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to retarget.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to retarget.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to retarget.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to retarget.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    f2d.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to arm_startup_nrf52.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to arm_startup_nrf52.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr


==============================================================================

Removing Unused input sections from the image.

    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing main.o(.rrx_text), (6 bytes).
    Removing main.o(i.assert_nrf_callback), (16 bytes).
    Removing main.o(.data), (1 bytes).
    Removing boards.o(.rev16_text), (4 bytes).
    Removing boards.o(.revsh_text), (4 bytes).
    Removing boards.o(.rrx_text), (6 bytes).
    Removing boards.o(i.bsp_board_led_idx_to_pin), (12 bytes).
    Removing boards.o(i.bsp_board_pin_to_led_idx), (36 bytes).
    Removing bsp.o(.rev16_text), (4 bytes).
    Removing bsp.o(.revsh_text), (4 bytes).
    Removing bsp.o(.rrx_text), (6 bytes).
    Removing bsp.o(i.bsp_buttons_disable), (4 bytes).
    Removing bsp.o(i.bsp_buttons_enable), (4 bytes).
    Removing bsp.o(i.bsp_wakeup_button_disable), (6 bytes).
    Removing bsp_btn_ble.o(.rev16_text), (4 bytes).
    Removing bsp_btn_ble.o(.revsh_text), (4 bytes).
    Removing bsp_btn_ble.o(.rrx_text), (6 bytes).
    Removing utf.o(i.utf16DecodeRune), (74 bytes).
    Removing utf.o(i.utf16EncodeRune), (64 bytes).
    Removing utf.o(i.utf16RuneCount), (60 bytes).
    Removing utf.o(i.utf16UTF8Count), (78 bytes).
    Removing utf.o(i.utf8DecodeRune), (174 bytes).
    Removing utf.o(i.utf8EncodeRune), (160 bytes).
    Removing utf.o(i.utf8RuneCount), (58 bytes).
    Removing utf.o(i.utf8UTF16Count), (76 bytes).
    Removing ble_advdata.o(.rev16_text), (4 bytes).
    Removing ble_advdata.o(.revsh_text), (4 bytes).
    Removing ble_advdata.o(.rrx_text), (6 bytes).
    Removing ble_advdata.o(i.ble_advdata_appearance_find), (52 bytes).
    Removing ble_advdata.o(i.ble_advdata_name_find), (68 bytes).
    Removing ble_advdata.o(i.ble_advdata_short_name_find), (74 bytes).
    Removing ble_advdata.o(i.ble_advdata_uuid_find), (182 bytes).
    Removing ble_advertising.o(.rev16_text), (4 bytes).
    Removing ble_advertising.o(.revsh_text), (4 bytes).
    Removing ble_advertising.o(.rrx_text), (6 bytes).
    Removing ble_advertising.o(i.ble_advertising_advdata_update), (32 bytes).
    Removing ble_advertising.o(i.ble_advertising_modes_config_set), (8 bytes).
    Removing ble_advertising.o(i.ble_advertising_peer_addr_reply), (34 bytes).
    Removing ble_advertising.o(i.ble_advertising_whitelist_reply), (36 bytes).
    Removing ble_conn_params.o(.rev16_text), (4 bytes).
    Removing ble_conn_params.o(.revsh_text), (4 bytes).
    Removing ble_conn_params.o(.rrx_text), (6 bytes).
    Removing ble_conn_params.o(i.ble_conn_params_change_conn_params), (64 bytes).
    Removing ble_conn_params.o(i.ble_conn_params_stop), (36 bytes).
    Removing ble_conn_state.o(.rev16_text), (4 bytes).
    Removing ble_conn_state.o(.revsh_text), (4 bytes).
    Removing ble_conn_state.o(.rrx_text), (6 bytes).
    Removing ble_conn_state.o(i.active_flag_count), (28 bytes).
    Removing ble_conn_state.o(i.bcs_internal_state_reset), (12 bytes).
    Removing ble_conn_state.o(i.ble_conn_state_central_conn_count), (28 bytes).
    Removing ble_conn_state.o(i.ble_conn_state_central_handles), (32 bytes).
    Removing ble_conn_state.o(i.ble_conn_state_conn_count), (12 bytes).
    Removing ble_conn_state.o(i.ble_conn_state_conn_handles), (12 bytes).
    Removing ble_conn_state.o(i.ble_conn_state_encrypted), (32 bytes).
    Removing ble_conn_state.o(i.ble_conn_state_for_each_connected), (20 bytes).
    Removing ble_conn_state.o(i.ble_conn_state_for_each_set_user_flag), (44 bytes).
    Removing ble_conn_state.o(i.ble_conn_state_init), (4 bytes).
    Removing ble_conn_state.o(i.ble_conn_state_mitm_protected), (32 bytes).
    Removing ble_conn_state.o(i.ble_conn_state_periph_handles), (36 bytes).
    Removing ble_conn_state.o(i.ble_conn_state_peripheral_conn_count), (32 bytes).
    Removing ble_conn_state.o(i.ble_conn_state_role), (16 bytes).
    Removing ble_conn_state.o(i.ble_conn_state_status), (36 bytes).
    Removing ble_conn_state.o(i.ble_conn_state_user_flag_acquire), (24 bytes).
    Removing ble_conn_state.o(i.ble_conn_state_user_flag_get), (48 bytes).
    Removing ble_conn_state.o(i.ble_conn_state_user_flag_set), (64 bytes).
    Removing ble_conn_state.o(i.for_each_set_flag), (48 bytes).
    Removing ble_conn_state.o(i.user_flag_is_acquired), (12 bytes).
    Removing ble_link_ctx_manager.o(.rev16_text), (4 bytes).
    Removing ble_link_ctx_manager.o(.revsh_text), (4 bytes).
    Removing ble_link_ctx_manager.o(.rrx_text), (6 bytes).
    Removing ble_srv_common.o(.rev16_text), (4 bytes).
    Removing ble_srv_common.o(.revsh_text), (4 bytes).
    Removing ble_srv_common.o(.rrx_text), (6 bytes).
    Removing ble_srv_common.o(i.ble_srv_ascii_to_utf8), (18 bytes).
    Removing ble_srv_common.o(i.ble_srv_is_indication_enabled), (8 bytes).
    Removing ble_srv_common.o(i.ble_srv_report_ref_encode), (12 bytes).
    Removing ble_srv_common.o(i.descriptor_add), (170 bytes).
    Removing nrf_ble_gatt.o(.rev16_text), (4 bytes).
    Removing nrf_ble_gatt.o(.revsh_text), (4 bytes).
    Removing nrf_ble_gatt.o(.rrx_text), (6 bytes).
    Removing nrf_ble_gatt.o(i.nrf_ble_gatt_att_mtu_central_set), (24 bytes).
    Removing nrf_ble_gatt.o(i.nrf_ble_gatt_eff_mtu_get), (12 bytes).
    Removing nrf_ble_qwr.o(.rev16_text), (4 bytes).
    Removing nrf_ble_qwr.o(.revsh_text), (4 bytes).
    Removing nrf_ble_qwr.o(.rrx_text), (6 bytes).
    Removing ble_nus.o(.rev16_text), (4 bytes).
    Removing ble_nus.o(.revsh_text), (4 bytes).
    Removing ble_nus.o(.rrx_text), (6 bytes).
    Removing nrf_drv_clock.o(.rev16_text), (4 bytes).
    Removing nrf_drv_clock.o(.revsh_text), (4 bytes).
    Removing nrf_drv_clock.o(.rrx_text), (6 bytes).
    Removing nrf_drv_clock.o(i.item_enqueue), (22 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_calibration_abort), (4 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_calibration_start), (4 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_hfclk_is_running), (44 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_hfclk_release), (56 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_hfclk_request), (92 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_init_check), (12 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_is_calibrating), (4 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_lfclk_is_running), (28 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_lfclk_request), (84 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_uninit), (24 bytes).
    Removing nrf_drv_clock.o(.constdata), (19 bytes).
    Removing nrf_drv_clock.o(.constdata), (32 bytes).
    Removing nrf_drv_clock.o(.constdata), (32 bytes).
    Removing nrf_drv_clock.o(.constdata), (29 bytes).
    Removing nrf_drv_uart.o(.rev16_text), (4 bytes).
    Removing nrf_drv_uart.o(.revsh_text), (4 bytes).
    Removing nrf_drv_uart.o(.rrx_text), (6 bytes).
    Removing nrfx_atomic.o(.rev16_text), (4 bytes).
    Removing nrfx_atomic.o(.revsh_text), (4 bytes).
    Removing nrfx_atomic.o(.rrx_text), (6 bytes).
    Removing nrfx_atomic.o(.emb_text), (226 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_flag_clear), (6 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_flag_clear_fetch), (6 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_flag_set), (6 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_flag_set_fetch), (6 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_u32_add), (12 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_u32_and), (12 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_u32_cmp_exch), (4 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_u32_fetch_add), (10 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_u32_fetch_and), (10 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_u32_fetch_or), (10 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_u32_fetch_store), (10 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_u32_fetch_sub), (10 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_u32_fetch_sub_hs), (10 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_u32_fetch_xor), (10 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_u32_or), (12 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_u32_store), (12 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_u32_sub), (12 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_u32_sub_hs), (12 bytes).
    Removing nrfx_atomic.o(i.nrfx_atomic_u32_xor), (12 bytes).
    Removing nrfx_clock.o(.rev16_text), (4 bytes).
    Removing nrfx_clock.o(.revsh_text), (4 bytes).
    Removing nrfx_clock.o(.rrx_text), (6 bytes).
    Removing nrfx_clock.o(i.nrfx_clock_calibration_start), (4 bytes).
    Removing nrfx_clock.o(i.nrfx_clock_calibration_timer_start), (2 bytes).
    Removing nrfx_clock.o(i.nrfx_clock_calibration_timer_stop), (2 bytes).
    Removing nrfx_clock.o(i.nrfx_clock_disable), (22 bytes).
    Removing nrfx_clock.o(i.nrfx_clock_hfclk_start), (22 bytes).
    Removing nrfx_clock.o(i.nrfx_clock_hfclk_stop), (44 bytes).
    Removing nrfx_clock.o(i.nrfx_clock_is_calibrating), (4 bytes).
    Removing nrfx_clock.o(i.nrfx_clock_lfclk_start), (76 bytes).
    Removing nrfx_clock.o(i.nrfx_clock_uninit), (24 bytes).
    Removing nrfx_clock.o(.constdata), (16 bytes).
    Removing nrfx_clock.o(.constdata), (29 bytes).
    Removing nrfx_gpiote.o(.rev16_text), (4 bytes).
    Removing nrfx_gpiote.o(.revsh_text), (4 bytes).
    Removing nrfx_gpiote.o(.rrx_text), (6 bytes).
    Removing nrfx_gpiote.o(i.nrf_gpio_cfg_default), (18 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_clr_task_addr_get), (24 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_clr_task_trigger), (28 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_in_event_addr_get), (40 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_in_event_disable), (72 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_in_uninit), (88 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_clear), (14 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_init), (192 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_set), (14 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_task_addr_get), (20 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_task_disable), (36 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_task_enable), (36 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_task_force), (40 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_task_trigger), (24 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_toggle), (28 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_out_uninit), (88 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_set_task_addr_get), (24 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_set_task_trigger), (28 bytes).
    Removing nrfx_gpiote.o(i.nrfx_gpiote_uninit), (56 bytes).
    Removing nrfx_gpiote.o(i.pin_configured_check), (20 bytes).
    Removing nrfx_gpiote.o(i.pin_configured_clear), (28 bytes).
    Removing nrfx_gpiote.o(.constdata), (17 bytes).
    Removing nrfx_gpiote.o(.constdata), (21 bytes).
    Removing nrfx_gpiote.o(.constdata), (20 bytes).
    Removing nrfx_prs.o(.rev16_text), (4 bytes).
    Removing nrfx_prs.o(.revsh_text), (4 bytes).
    Removing nrfx_prs.o(.rrx_text), (6 bytes).
    Removing nrfx_prs.o(i.nrfx_prs_release), (18 bytes).
    Removing nrfx_prs.o(.constdata), (17 bytes).
    Removing nrfx_uart.o(.rev16_text), (4 bytes).
    Removing nrfx_uart.o(.revsh_text), (4 bytes).
    Removing nrfx_uart.o(.rrx_text), (6 bytes).
    Removing nrfx_uart.o(i.nrf_gpio_cfg_default), (18 bytes).
    Removing nrfx_uart.o(i.nrfx_uart_errorsrc_get), (26 bytes).
    Removing nrfx_uart.o(i.nrfx_uart_rx_abort), (18 bytes).
    Removing nrfx_uart.o(i.nrfx_uart_rx_disable), (36 bytes).
    Removing nrfx_uart.o(i.nrfx_uart_rx_enable), (60 bytes).
    Removing nrfx_uart.o(i.nrfx_uart_rx_ready), (14 bytes).
    Removing nrfx_uart.o(i.nrfx_uart_tx_abort), (48 bytes).
    Removing nrfx_uart.o(i.nrfx_uart_uninit), (180 bytes).
    Removing nrfx_uart.o(.constdata), (15 bytes).
    Removing nrfx_uart.o(.constdata), (13 bytes).
    Removing nrfx_uart.o(.constdata), (13 bytes).
    Removing nrfx_uarte.o(.rev16_text), (4 bytes).
    Removing nrfx_uarte.o(.revsh_text), (4 bytes).
    Removing nrfx_uarte.o(.rrx_text), (6 bytes).
    Removing nrfx_uarte.o(i.nrf_gpio_cfg_default), (18 bytes).
    Removing nrfx_uarte.o(i.nrfx_uarte_errorsrc_get), (26 bytes).
    Removing nrfx_uarte.o(i.nrfx_uarte_rx_abort), (44 bytes).
    Removing nrfx_uarte.o(i.nrfx_uarte_rx_ready), (14 bytes).
    Removing nrfx_uarte.o(i.nrfx_uarte_tx_abort), (56 bytes).
    Removing nrfx_uarte.o(i.nrfx_uarte_uninit), (176 bytes).
    Removing nrfx_uarte.o(.constdata), (16 bytes).
    Removing nrfx_uarte.o(.constdata), (14 bytes).
    Removing nrfx_uarte.o(.constdata), (14 bytes).
    Removing nrf_drv_ppi.o(.rev16_text), (4 bytes).
    Removing nrf_drv_ppi.o(.revsh_text), (4 bytes).
    Removing nrf_drv_ppi.o(.rrx_text), (6 bytes).
    Removing nrf_drv_ppi.o(i.nrf_drv_ppi_uninit), (28 bytes).
    Removing nrfx_ppi.o(.rev16_text), (4 bytes).
    Removing nrfx_ppi.o(.revsh_text), (4 bytes).
    Removing nrfx_ppi.o(.rrx_text), (6 bytes).
    Removing nrfx_ppi.o(i.is_allocated_group), (24 bytes).
    Removing nrfx_ppi.o(i.is_app_group), (14 bytes).
    Removing nrfx_ppi.o(i.nrfx_ppi_channel_disable), (52 bytes).
    Removing nrfx_ppi.o(i.nrfx_ppi_channel_fork_assign), (36 bytes).
    Removing nrfx_ppi.o(i.nrfx_ppi_channel_free), (64 bytes).
    Removing nrfx_ppi.o(i.nrfx_ppi_channels_include_in_group), (84 bytes).
    Removing nrfx_ppi.o(i.nrfx_ppi_channels_remove_from_group), (84 bytes).
    Removing nrfx_ppi.o(i.nrfx_ppi_free_all), (84 bytes).
    Removing nrfx_ppi.o(i.nrfx_ppi_group_alloc), (104 bytes).
    Removing nrfx_ppi.o(i.nrfx_ppi_group_disable), (36 bytes).
    Removing nrfx_ppi.o(i.nrfx_ppi_group_enable), (44 bytes).
    Removing nrfx_ppi.o(i.nrfx_ppi_group_free), (80 bytes).
    Removing nrfx_ppi.o(.constdata), (23 bytes).
    Removing nrfx_ppi.o(.constdata), (22 bytes).
    Removing nrfx_ppi.o(.constdata), (24 bytes).
    Removing nrfx_ppi.o(.constdata), (29 bytes).
    Removing nrfx_ppi.o(.constdata), (24 bytes).
    Removing nrfx_ppi.o(.constdata), (25 bytes).
    Removing nrfx_ppi.o(.constdata), (21 bytes).
    Removing nrfx_ppi.o(.constdata), (20 bytes).
    Removing nrfx_ppi.o(.constdata), (22 bytes).
    Removing nrfx_ppi.o(.constdata), (23 bytes).
    Removing nrfx_ppi.o(.constdata), (36 bytes).
    Removing nrfx_ppi.o(.constdata), (35 bytes).
    Removing nrfx_saadc.o(.rev16_text), (4 bytes).
    Removing nrfx_saadc.o(.revsh_text), (4 bytes).
    Removing nrfx_saadc.o(.rrx_text), (6 bytes).
    Removing nrfx_saadc.o(i.nrf_saadc_limit_int_get), (16 bytes).
    Removing nrfx_saadc.o(i.nrfx_coredep_delay_us), (16 bytes).
    Removing nrfx_saadc.o(i.nrfx_saadc_abort), (92 bytes).
    Removing nrfx_saadc.o(i.nrfx_saadc_calibrate_offset), (52 bytes).
    Removing nrfx_saadc.o(i.nrfx_saadc_channel_uninit), (68 bytes).
    Removing nrfx_saadc.o(i.nrfx_saadc_is_busy), (16 bytes).
    Removing nrfx_saadc.o(i.nrfx_saadc_limits_set), (128 bytes).
    Removing nrfx_saadc.o(i.nrfx_saadc_sample), (44 bytes).
    Removing nrfx_saadc.o(i.nrfx_saadc_sample_convert), (192 bytes).
    Removing nrfx_saadc.o(i.nrfx_saadc_uninit), (108 bytes).
    Removing nrfx_saadc.o(.constdata), (6 bytes).
    Removing nrfx_saadc.o(.constdata), (16 bytes).
    Removing nrfx_saadc.o(.constdata), (24 bytes).
    Removing nrfx_saadc.o(.constdata), (26 bytes).
    Removing nrfx_saadc.o(.constdata), (26 bytes).
    Removing nrfx_saadc.o(.constdata), (26 bytes).
    Removing nrfx_saadc.o(.constdata), (18 bytes).
    Removing nrfx_saadc.o(.constdata), (28 bytes).
    Removing nrfx_timer.o(.rev16_text), (4 bytes).
    Removing nrfx_timer.o(.revsh_text), (4 bytes).
    Removing nrfx_timer.o(.rrx_text), (6 bytes).
    Removing nrfx_timer.o(i.nrfx_timer_capture), (30 bytes).
    Removing nrfx_timer.o(i.nrfx_timer_clear), (8 bytes).
    Removing nrfx_timer.o(i.nrfx_timer_compare_int_disable), (14 bytes).
    Removing nrfx_timer.o(i.nrfx_timer_compare_int_enable), (36 bytes).
    Removing nrfx_timer.o(i.nrfx_timer_disable), (28 bytes).
    Removing nrfx_timer.o(i.nrfx_timer_increment), (8 bytes).
    Removing nrfx_timer.o(i.nrfx_timer_is_enabled), (32 bytes).
    Removing nrfx_timer.o(i.nrfx_timer_pause), (8 bytes).
    Removing nrfx_timer.o(i.nrfx_timer_resume), (8 bytes).
    Removing nrfx_timer.o(i.nrfx_timer_uninit), (80 bytes).
    Removing nrfx_timer.o(.constdata), (16 bytes).
    Removing nrf_drv_twi.o(.rev16_text), (4 bytes).
    Removing nrf_drv_twi.o(.revsh_text), (4 bytes).
    Removing nrf_drv_twi.o(.rrx_text), (6 bytes).
    Removing nrf_drv_twi.o(i.nrf_drv_twi_init), (64 bytes).
    Removing nrf_drv_twi.o(i.nrf_gpio_pin_set), (14 bytes).
    Removing nrf_drv_twi.o(i.nrfx_coredep_delay_us), (16 bytes).
    Removing nrf_drv_twi.o(i.twi_clear_bus), (170 bytes).
    Removing nrf_drv_twi.o(i.twim_evt_handler), (64 bytes).
    Removing nrf_drv_twi.o(.constdata), (6 bytes).
    Removing nrf_drv_twi.o(.data), (16 bytes).
    Removing nrfx_twi.o(.rev16_text), (4 bytes).
    Removing nrfx_twi.o(.revsh_text), (4 bytes).
    Removing nrfx_twi.o(.rrx_text), (6 bytes).
    Removing nrfx_twim.o(.rev16_text), (4 bytes).
    Removing nrfx_twim.o(.revsh_text), (4 bytes).
    Removing nrfx_twim.o(.rrx_text), (6 bytes).
    Removing nrfx_twim.o(i.nrf_gpio_cfg), (36 bytes).
    Removing nrfx_twim.o(i.nrf_gpio_cfg_default), (18 bytes).
    Removing nrfx_twim.o(i.nrfx_is_in_ram), (16 bytes).
    Removing nrfx_twim.o(i.nrfx_twim_disable), (60 bytes).
    Removing nrfx_twim.o(i.nrfx_twim_enable), (36 bytes).
    Removing nrfx_twim.o(i.nrfx_twim_init), (224 bytes).
    Removing nrfx_twim.o(i.nrfx_twim_is_busy), (28 bytes).
    Removing nrfx_twim.o(i.nrfx_twim_rx), (48 bytes).
    Removing nrfx_twim.o(i.nrfx_twim_start_task_get), (16 bytes).
    Removing nrfx_twim.o(i.nrfx_twim_stopped_event_get), (8 bytes).
    Removing nrfx_twim.o(i.nrfx_twim_tx), (54 bytes).
    Removing nrfx_twim.o(i.nrfx_twim_uninit), (100 bytes).
    Removing nrfx_twim.o(i.nrfx_twim_xfer), (40 bytes).
    Removing nrfx_twim.o(i.twim_xfer), (560 bytes).
    Removing nrfx_twim.o(.constdata), (15 bytes).
    Removing nrfx_twim.o(.constdata), (24 bytes).
    Removing nrfx_twim.o(.constdata), (10 bytes).
    Removing nrfx_twim.o(.constdata), (15 bytes).
    Removing app_button.o(.rev16_text), (4 bytes).
    Removing app_button.o(.revsh_text), (4 bytes).
    Removing app_button.o(.rrx_text), (6 bytes).
    Removing app_button.o(i.app_button_disable), (48 bytes).
    Removing app_button.o(i.app_button_is_pushed), (36 bytes).
    Removing app_error.o(.rev16_text), (4 bytes).
    Removing app_error.o(.revsh_text), (4 bytes).
    Removing app_error.o(.rrx_text), (6 bytes).
    Removing app_error.o(i.app_error_save_and_stop), (100 bytes).
    Removing app_error.o(.bss), (32 bytes).
    Removing app_error_handler_keil.o(.rev16_text), (4 bytes).
    Removing app_error_handler_keil.o(.revsh_text), (4 bytes).
    Removing app_error_handler_keil.o(.rrx_text), (6 bytes).
    Removing app_error_handler_keil.o(.emb_text), (26 bytes).
    Removing app_error_weak.o(.rev16_text), (4 bytes).
    Removing app_error_weak.o(.revsh_text), (4 bytes).
    Removing app_error_weak.o(.rrx_text), (6 bytes).
    Removing app_fifo.o(.rev16_text), (4 bytes).
    Removing app_fifo.o(.revsh_text), (4 bytes).
    Removing app_fifo.o(.rrx_text), (6 bytes).
    Removing app_fifo.o(i.app_fifo_flush), (8 bytes).
    Removing app_fifo.o(i.app_fifo_peek), (34 bytes).
    Removing app_fifo.o(i.app_fifo_read), (74 bytes).
    Removing app_fifo.o(i.app_fifo_write), (82 bytes).
    Removing app_scheduler.o(.rev16_text), (4 bytes).
    Removing app_scheduler.o(.revsh_text), (4 bytes).
    Removing app_scheduler.o(.rrx_text), (6 bytes).
    Removing app_scheduler.o(i.app_sched_event_put), (160 bytes).
    Removing app_scheduler.o(i.app_sched_execute), (64 bytes).
    Removing app_scheduler.o(i.app_sched_init), (44 bytes).
    Removing app_scheduler.o(i.app_sched_queue_space_get), (36 bytes).
    Removing app_scheduler.o(.data), (16 bytes).
    Removing app_timer.o(.rev16_text), (4 bytes).
    Removing app_timer.o(.revsh_text), (4 bytes).
    Removing app_timer.o(.rrx_text), (6 bytes).
    Removing app_timer.o(i.app_timer_cnt_diff_compute), (8 bytes).
    Removing app_timer.o(i.app_timer_cnt_get), (12 bytes).
    Removing app_timer.o(i.app_timer_pause), (12 bytes).
    Removing app_timer.o(i.app_timer_resume), (12 bytes).
    Removing app_timer.o(i.app_timer_stop_all), (24 bytes).
    Removing app_uart_fifo.o(.rev16_text), (4 bytes).
    Removing app_uart_fifo.o(.revsh_text), (4 bytes).
    Removing app_uart_fifo.o(.rrx_text), (6 bytes).
    Removing app_uart_fifo.o(i.app_uart_close), (40 bytes).
    Removing app_uart_fifo.o(i.app_uart_flush), (32 bytes).
    Removing app_util_platform.o(.rev16_text), (4 bytes).
    Removing app_util_platform.o(.revsh_text), (4 bytes).
    Removing app_util_platform.o(.rrx_text), (6 bytes).
    Removing app_util_platform.o(i.app_util_disable_irq), (16 bytes).
    Removing app_util_platform.o(i.app_util_enable_irq), (20 bytes).
    Removing app_util_platform.o(i.current_int_priority_get), (48 bytes).
    Removing app_util_platform.o(i.privilege_level_get), (26 bytes).
    Removing app_util_platform.o(.data), (4 bytes).
    Removing hardfault_implementation.o(.rev16_text), (4 bytes).
    Removing hardfault_implementation.o(.revsh_text), (4 bytes).
    Removing hardfault_implementation.o(.rrx_text), (6 bytes).
    Removing nrf_assert.o(.rev16_text), (4 bytes).
    Removing nrf_assert.o(.revsh_text), (4 bytes).
    Removing nrf_assert.o(.rrx_text), (6 bytes).
    Removing nrf_assert.o(i.assert_nrf_callback), (22 bytes).
    Removing nrf_atfifo.o(.rev16_text), (4 bytes).
    Removing nrf_atfifo.o(.revsh_text), (4 bytes).
    Removing nrf_atfifo.o(.rrx_text), (6 bytes).
    Removing nrf_atfifo.o(.emb_text), (200 bytes).
    Removing nrf_atfifo.o(i.nrf_atfifo_alloc_put), (46 bytes).
    Removing nrf_atfifo.o(i.nrf_atfifo_clear), (16 bytes).
    Removing nrf_atfifo.o(i.nrf_atfifo_get_free), (48 bytes).
    Removing nrf_atfifo.o(i.nrf_atfifo_init), (38 bytes).
    Removing nrf_atfifo.o(i.nrf_atfifo_item_alloc), (22 bytes).
    Removing nrf_atfifo.o(i.nrf_atfifo_item_free), (22 bytes).
    Removing nrf_atfifo.o(i.nrf_atfifo_item_get), (22 bytes).
    Removing nrf_atfifo.o(i.nrf_atfifo_item_put), (22 bytes).
    Removing nrf_atflags.o(.rev16_text), (4 bytes).
    Removing nrf_atflags.o(.revsh_text), (4 bytes).
    Removing nrf_atflags.o(.rrx_text), (6 bytes).
    Removing nrf_atflags.o(i.nrf_atflags_fetch_clear), (32 bytes).
    Removing nrf_atflags.o(i.nrf_atflags_fetch_set), (32 bytes).
    Removing nrf_atflags.o(i.nrf_atflags_find_and_clear_flag), (72 bytes).
    Removing nrf_atflags.o(i.nrf_atflags_find_and_set_flag), (74 bytes).
    Removing nrf_atflags.o(i.nrf_atflags_init), (36 bytes).
    Removing nrf_atomic.o(.rev16_text), (4 bytes).
    Removing nrf_atomic.o(.revsh_text), (4 bytes).
    Removing nrf_atomic.o(.rrx_text), (6 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_flag_clear), (6 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_flag_set_fetch), (6 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_cmp_exch), (4 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_fetch_add), (10 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_fetch_or), (10 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_fetch_sub), (10 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_fetch_sub_hs), (10 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_fetch_xor), (10 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_store), (12 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_sub_hs), (12 bytes).
    Removing nrf_atomic.o(i.nrf_atomic_u32_xor), (12 bytes).
    Removing nrf_balloc.o(.rev16_text), (4 bytes).
    Removing nrf_balloc.o(.revsh_text), (4 bytes).
    Removing nrf_balloc.o(.rrx_text), (6 bytes).
    Removing nrf_fprintf.o(.rev16_text), (4 bytes).
    Removing nrf_fprintf.o(.revsh_text), (4 bytes).
    Removing nrf_fprintf.o(.rrx_text), (6 bytes).
    Removing nrf_fprintf_format.o(.rev16_text), (4 bytes).
    Removing nrf_fprintf_format.o(.revsh_text), (4 bytes).
    Removing nrf_fprintf_format.o(.rrx_text), (6 bytes).
    Removing nrf_memobj.o(.rev16_text), (4 bytes).
    Removing nrf_memobj.o(.revsh_text), (4 bytes).
    Removing nrf_memobj.o(.rrx_text), (6 bytes).
    Removing nrf_pwr_mgmt.o(.rev16_text), (4 bytes).
    Removing nrf_pwr_mgmt.o(.revsh_text), (4 bytes).
    Removing nrf_pwr_mgmt.o(.rrx_text), (6 bytes).
    Removing nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_feed), (2 bytes).
    Removing nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_shutdown), (60 bytes).
    Removing nrf_pwr_mgmt.o(i.shutdown_process), (124 bytes).
    Removing nrf_ringbuf.o(.rev16_text), (4 bytes).
    Removing nrf_ringbuf.o(.revsh_text), (4 bytes).
    Removing nrf_ringbuf.o(.rrx_text), (6 bytes).
    Removing nrf_ringbuf.o(i.nrf_ringbuf_alloc), (112 bytes).
    Removing nrf_ringbuf.o(i.nrf_ringbuf_cpy_get), (124 bytes).
    Removing nrf_ringbuf.o(i.nrf_ringbuf_cpy_put), (114 bytes).
    Removing nrf_ringbuf.o(i.nrf_ringbuf_free), (38 bytes).
    Removing nrf_ringbuf.o(i.nrf_ringbuf_get), (112 bytes).
    Removing nrf_ringbuf.o(i.nrf_ringbuf_put), (48 bytes).
    Removing nrf_section_iter.o(.rev16_text), (4 bytes).
    Removing nrf_section_iter.o(.revsh_text), (4 bytes).
    Removing nrf_section_iter.o(.rrx_text), (6 bytes).
    Removing nrf_strerror.o(.rev16_text), (4 bytes).
    Removing nrf_strerror.o(.revsh_text), (4 bytes).
    Removing nrf_strerror.o(.rrx_text), (6 bytes).
    Removing retarget.o(.rev16_text), (4 bytes).
    Removing retarget.o(.revsh_text), (4 bytes).
    Removing retarget.o(.rrx_text), (6 bytes).
    Removing retarget.o(i.fgetc), (18 bytes).
    Removing retarget.o(.data), (4 bytes).
    Removing nrf_log_backend_rtt.o(.rev16_text), (4 bytes).
    Removing nrf_log_backend_rtt.o(.revsh_text), (4 bytes).
    Removing nrf_log_backend_rtt.o(.rrx_text), (6 bytes).
    Removing nrf_log_backend_serial.o(.rev16_text), (4 bytes).
    Removing nrf_log_backend_serial.o(.revsh_text), (4 bytes).
    Removing nrf_log_backend_serial.o(.rrx_text), (6 bytes).
    Removing nrf_log_default_backends.o(.rev16_text), (4 bytes).
    Removing nrf_log_default_backends.o(.revsh_text), (4 bytes).
    Removing nrf_log_default_backends.o(.rrx_text), (6 bytes).
    Removing nrf_log_frontend.o(.rev16_text), (4 bytes).
    Removing nrf_log_frontend.o(.revsh_text), (4 bytes).
    Removing nrf_log_frontend.o(.rrx_text), (6 bytes).
    Removing nrf_log_frontend.o(i.nrf_log_backend_remove), (52 bytes).
    Removing nrf_log_frontend.o(i.nrf_log_frontend_hexdump), (168 bytes).
    Removing nrf_log_frontend.o(i.nrf_log_frontend_std_3), (18 bytes).
    Removing nrf_log_frontend.o(i.nrf_log_frontend_std_4), (20 bytes).
    Removing nrf_log_frontend.o(i.nrf_log_frontend_std_5), (28 bytes).
    Removing nrf_log_frontend.o(i.nrf_log_frontend_std_6), (28 bytes).
    Removing nrf_log_frontend.o(i.nrf_log_module_filter_get), (36 bytes).
    Removing nrf_log_frontend.o(i.nrf_log_module_filter_set), (2 bytes).
    Removing nrf_log_frontend.o(i.nrf_log_push), (96 bytes).
    Removing nrf_log_str_formatter.o(.rev16_text), (4 bytes).
    Removing nrf_log_str_formatter.o(.revsh_text), (4 bytes).
    Removing nrf_log_str_formatter.o(.rrx_text), (6 bytes).
    Removing nrf_log_str_formatter.o(i.nrf_log_str_formatter_timestamp_freq_set), (32 bytes).
    Removing segger_rtt.o(.rev16_text), (4 bytes).
    Removing segger_rtt.o(.revsh_text), (4 bytes).
    Removing segger_rtt.o(.rrx_text), (6 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_AllocDownBuffer), (112 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_AllocUpBuffer), (112 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_ConfigDownBuffer), (96 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_ConfigUpBuffer), (96 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_GetKey), (28 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_HasData), (24 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_HasKey), (32 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_PutChar), (96 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_PutCharSkip), (84 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_PutCharSkipNoLock), (52 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_Read), (44 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_ReadNoLock), (120 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_SetFlagsDownBuffer), (68 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_SetFlagsUpBuffer), (68 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_SetNameDownBuffer), (68 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_SetNameUpBuffer), (68 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_SetTerminal), (136 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_TerminalOut), (176 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_WaitKey), (14 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_Write), (60 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_WriteSkipNoLock), (116 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_WriteString), (26 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_WriteWithOverwriteNoLock), (148 bytes).
    Removing segger_rtt.o(i._PostTerminalSwitch), (32 bytes).
    Removing segger_rtt.o(.data), (17 bytes).
    Removing segger_rtt_printf.o(.rev16_text), (4 bytes).
    Removing segger_rtt_printf.o(.revsh_text), (4 bytes).
    Removing segger_rtt_printf.o(.rrx_text), (6 bytes).
    Removing segger_rtt_printf.o(i.SEGGER_RTT_printf), (22 bytes).
    Removing segger_rtt_printf.o(i.SEGGER_RTT_vprintf), (406 bytes).
    Removing segger_rtt_printf.o(i._PrintInt), (198 bytes).
    Removing segger_rtt_printf.o(i._PrintUnsigned), (212 bytes).
    Removing segger_rtt_printf.o(i._StoreChar), (62 bytes).
    Removing segger_rtt_printf.o(.constdata), (16 bytes).
    Removing nrf_sdh.o(.rev16_text), (4 bytes).
    Removing nrf_sdh.o(.revsh_text), (4 bytes).
    Removing nrf_sdh.o(.rrx_text), (6 bytes).
    Removing nrf_sdh.o(i.nrf_sdh_disable_request), (84 bytes).
    Removing nrf_sdh.o(i.nrf_sdh_is_suspended), (20 bytes).
    Removing nrf_sdh.o(i.nrf_sdh_request_continue), (28 bytes).
    Removing nrf_sdh.o(i.nrf_sdh_resume), (56 bytes).
    Removing nrf_sdh.o(i.nrf_sdh_suspend), (24 bytes).
    Removing nrf_sdh.o(i.softdevice_evt_irq_disable), (56 bytes).
    Removing nrf_sdh_ble.o(.rev16_text), (4 bytes).
    Removing nrf_sdh_ble.o(.revsh_text), (4 bytes).
    Removing nrf_sdh_ble.o(.rrx_text), (6 bytes).
    Removing nrf_sdh_soc.o(.rev16_text), (4 bytes).
    Removing nrf_sdh_soc.o(.revsh_text), (4 bytes).
    Removing nrf_sdh_soc.o(.rrx_text), (6 bytes).
    Removing arm_startup_nrf52.o(HEAP), (2048 bytes).
    Removing system_nrf52.o(.rev16_text), (4 bytes).
    Removing system_nrf52.o(.revsh_text), (4 bytes).
    Removing system_nrf52.o(.rrx_text), (6 bytes).
    Removing system_nrf52.o(i.SystemCoreClockUpdate), (16 bytes).

520 unused section(s) (total 18125 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isupper_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isspace_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isxdigit_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  ispunct_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isprint_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  islower_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isgraph_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isdigit_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  iscntrl_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isblank_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isalpha_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isalnum_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  ctype_o.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/string/memcmp.c         0x00000000   Number         0  memcmp.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/string/strcat.c         0x00000000   Number         0  strcat.o ABSOLUTE
    ../clib/microlib/string/strcpy.c         0x00000000   Number         0  strcpy.o ABSOLUTE
    ../clib/microlib/string/strlen.c         0x00000000   Number         0  strlen.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/f2d.c                  0x00000000   Number         0  f2d.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ..\..\..\..\..\..\components\ble\ble_advertising\ble_advertising.c 0x00000000   Number         0  ble_advertising.o ABSOLUTE
    ..\..\..\..\..\..\components\ble\ble_link_ctx_manager\ble_link_ctx_manager.c 0x00000000   Number         0  ble_link_ctx_manager.o ABSOLUTE
    ..\..\..\..\..\..\components\ble\ble_services\ble_nus\ble_nus.c 0x00000000   Number         0  ble_nus.o ABSOLUTE
    ..\..\..\..\..\..\components\ble\common\ble_advdata.c 0x00000000   Number         0  ble_advdata.o ABSOLUTE
    ..\..\..\..\..\..\components\ble\common\ble_conn_params.c 0x00000000   Number         0  ble_conn_params.o ABSOLUTE
    ..\..\..\..\..\..\components\ble\common\ble_conn_state.c 0x00000000   Number         0  ble_conn_state.o ABSOLUTE
    ..\..\..\..\..\..\components\ble\common\ble_srv_common.c 0x00000000   Number         0  ble_srv_common.o ABSOLUTE
    ..\..\..\..\..\..\components\ble\nrf_ble_gatt\nrf_ble_gatt.c 0x00000000   Number         0  nrf_ble_gatt.o ABSOLUTE
    ..\..\..\..\..\..\components\ble\nrf_ble_qwr\nrf_ble_qwr.c 0x00000000   Number         0  nrf_ble_qwr.o ABSOLUTE
    ..\..\..\..\..\..\components\boards\boards.c 0x00000000   Number         0  boards.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\atomic\nrf_atomic.c 0x00000000   Number         0  nrf_atomic.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\atomic_fifo\nrf_atfifo.c 0x00000000   Number         0  nrf_atfifo.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\atomic_flags\nrf_atflags.c 0x00000000   Number         0  nrf_atflags.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\balloc\nrf_balloc.c 0x00000000   Number         0  nrf_balloc.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\bsp\bsp.c 0x00000000   Number         0  bsp.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\bsp\bsp_btn_ble.c 0x00000000   Number         0  bsp_btn_ble.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\button\app_button.c 0x00000000   Number         0  app_button.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section_iter.c 0x00000000   Number         0  nrf_section_iter.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\fifo\app_fifo.c 0x00000000   Number         0  app_fifo.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\hardfault\hardfault_implementation.c 0x00000000   Number         0  hardfault_implementation.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\log\src\nrf_log_backend_rtt.c 0x00000000   Number         0  nrf_log_backend_rtt.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\log\src\nrf_log_backend_serial.c 0x00000000   Number         0  nrf_log_backend_serial.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\log\src\nrf_log_default_backends.c 0x00000000   Number         0  nrf_log_default_backends.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\log\src\nrf_log_frontend.c 0x00000000   Number         0  nrf_log_frontend.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\log\src\nrf_log_str_formatter.c 0x00000000   Number         0  nrf_log_str_formatter.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\memobj\nrf_memobj.c 0x00000000   Number         0  nrf_memobj.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\pwr_mgmt\nrf_pwr_mgmt.c 0x00000000   Number         0  nrf_pwr_mgmt.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\ringbuf\nrf_ringbuf.c 0x00000000   Number         0  nrf_ringbuf.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\scheduler\app_scheduler.c 0x00000000   Number         0  app_scheduler.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\strerror\nrf_strerror.c 0x00000000   Number         0  nrf_strerror.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\timer\app_timer.c 0x00000000   Number         0  app_timer.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\uart\app_uart_fifo.c 0x00000000   Number         0  app_uart_fifo.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\uart\retarget.c 0x00000000   Number         0  retarget.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\util\app_error.c 0x00000000   Number         0  app_error.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\util\app_error_handler_keil.c 0x00000000   Number         0  app_error_handler_keil.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\util\app_error_weak.c 0x00000000   Number         0  app_error_weak.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\util\app_util_platform.c 0x00000000   Number         0  app_util_platform.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\util\nrf_assert.c 0x00000000   Number         0  nrf_assert.o ABSOLUTE
    ..\..\..\..\..\..\components\softdevice\common\nrf_sdh.c 0x00000000   Number         0  nrf_sdh.o ABSOLUTE
    ..\..\..\..\..\..\components\softdevice\common\nrf_sdh_ble.c 0x00000000   Number         0  nrf_sdh_ble.o ABSOLUTE
    ..\..\..\..\..\..\components\softdevice\common\nrf_sdh_soc.c 0x00000000   Number         0  nrf_sdh_soc.o ABSOLUTE
    ..\..\..\..\..\..\external\fprintf\nrf_fprintf.c 0x00000000   Number         0  nrf_fprintf.o ABSOLUTE
    ..\..\..\..\..\..\external\fprintf\nrf_fprintf_format.c 0x00000000   Number         0  nrf_fprintf_format.o ABSOLUTE
    ..\..\..\..\..\..\external\segger_rtt\SEGGER_RTT.c 0x00000000   Number         0  segger_rtt.o ABSOLUTE
    ..\..\..\..\..\..\external\segger_rtt\SEGGER_RTT_Syscalls_KEIL.c 0x00000000   Number         0  segger_rtt_syscalls_keil.o ABSOLUTE
    ..\..\..\..\..\..\external\segger_rtt\SEGGER_RTT_printf.c 0x00000000   Number         0  segger_rtt_printf.o ABSOLUTE
    ..\..\..\..\..\..\external\utf_converter\utf.c 0x00000000   Number         0  utf.o ABSOLUTE
    ..\..\..\..\..\..\integration\nrfx\legacy\nrf_drv_clock.c 0x00000000   Number         0  nrf_drv_clock.o ABSOLUTE
    ..\..\..\..\..\..\integration\nrfx\legacy\nrf_drv_ppi.c 0x00000000   Number         0  nrf_drv_ppi.o ABSOLUTE
    ..\..\..\..\..\..\integration\nrfx\legacy\nrf_drv_twi.c 0x00000000   Number         0  nrf_drv_twi.o ABSOLUTE
    ..\..\..\..\..\..\integration\nrfx\legacy\nrf_drv_uart.c 0x00000000   Number         0  nrf_drv_uart.o ABSOLUTE
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_clock.c 0x00000000   Number         0  nrfx_clock.o ABSOLUTE
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_gpiote.c 0x00000000   Number         0  nrfx_gpiote.o ABSOLUTE
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_ppi.c 0x00000000   Number         0  nrfx_ppi.o ABSOLUTE
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_saadc.c 0x00000000   Number         0  nrfx_saadc.o ABSOLUTE
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_timer.c 0x00000000   Number         0  nrfx_timer.o ABSOLUTE
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_twi.c 0x00000000   Number         0  nrfx_twi.o ABSOLUTE
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_twim.c 0x00000000   Number         0  nrfx_twim.o ABSOLUTE
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_uart.c 0x00000000   Number         0  nrfx_uart.o ABSOLUTE
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_uarte.c 0x00000000   Number         0  nrfx_uarte.o ABSOLUTE
    ..\..\..\..\..\..\modules\nrfx\drivers\src\prs\nrfx_prs.c 0x00000000   Number         0  nrfx_prs.o ABSOLUTE
    ..\..\..\..\..\..\modules\nrfx\soc\nrfx_atomic.c 0x00000000   Number         0  nrfx_atomic.o ABSOLUTE
    ..\..\..\main.c                          0x00000000   Number         0  main.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\ble\\ble_advertising\\ble_advertising.c 0x00000000   Number         0  ble_advertising.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\ble\\ble_link_ctx_manager\\ble_link_ctx_manager.c 0x00000000   Number         0  ble_link_ctx_manager.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\ble\\ble_services\\ble_nus\\ble_nus.c 0x00000000   Number         0  ble_nus.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\ble\\common\\ble_advdata.c 0x00000000   Number         0  ble_advdata.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\ble\\common\\ble_conn_params.c 0x00000000   Number         0  ble_conn_params.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\ble\\common\\ble_conn_state.c 0x00000000   Number         0  ble_conn_state.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\ble\\common\\ble_srv_common.c 0x00000000   Number         0  ble_srv_common.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\ble\\nrf_ble_gatt\\nrf_ble_gatt.c 0x00000000   Number         0  nrf_ble_gatt.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\ble\\nrf_ble_qwr\\nrf_ble_qwr.c 0x00000000   Number         0  nrf_ble_qwr.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\boards\\boards.c 0x00000000   Number         0  boards.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\atomic\\nrf_atomic.c 0x00000000   Number         0  nrf_atomic.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\atomic_fifo\\nrf_atfifo.c 0x00000000   Number         0  nrf_atfifo.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\atomic_flags\\nrf_atflags.c 0x00000000   Number         0  nrf_atflags.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\balloc\\nrf_balloc.c 0x00000000   Number         0  nrf_balloc.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\bsp\\bsp.c 0x00000000   Number         0  bsp.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\bsp\\bsp_btn_ble.c 0x00000000   Number         0  bsp_btn_ble.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\button\\app_button.c 0x00000000   Number         0  app_button.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\experimental_section_vars\\nrf_section_iter.c 0x00000000   Number         0  nrf_section_iter.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\fifo\\app_fifo.c 0x00000000   Number         0  app_fifo.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\hardfault\\hardfault_implementation.c 0x00000000   Number         0  hardfault_implementation.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\log\\src\\nrf_log_backend_rtt.c 0x00000000   Number         0  nrf_log_backend_rtt.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\log\\src\\nrf_log_backend_serial.c 0x00000000   Number         0  nrf_log_backend_serial.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\log\\src\\nrf_log_default_backends.c 0x00000000   Number         0  nrf_log_default_backends.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\log\\src\\nrf_log_frontend.c 0x00000000   Number         0  nrf_log_frontend.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\log\\src\\nrf_log_str_formatter.c 0x00000000   Number         0  nrf_log_str_formatter.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\memobj\\nrf_memobj.c 0x00000000   Number         0  nrf_memobj.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\pwr_mgmt\\nrf_pwr_mgmt.c 0x00000000   Number         0  nrf_pwr_mgmt.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\ringbuf\\nrf_ringbuf.c 0x00000000   Number         0  nrf_ringbuf.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\scheduler\\app_scheduler.c 0x00000000   Number         0  app_scheduler.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\strerror\\nrf_strerror.c 0x00000000   Number         0  nrf_strerror.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\timer\\app_timer.c 0x00000000   Number         0  app_timer.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\uart\\app_uart_fifo.c 0x00000000   Number         0  app_uart_fifo.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\uart\\retarget.c 0x00000000   Number         0  retarget.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\util\\app_error.c 0x00000000   Number         0  app_error.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\util\\app_error_handler_keil.c 0x00000000   Number         0  app_error_handler_keil.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\util\\app_error_weak.c 0x00000000   Number         0  app_error_weak.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\util\\app_util_platform.c 0x00000000   Number         0  app_util_platform.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\util\\nrf_assert.c 0x00000000   Number         0  nrf_assert.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\softdevice\\common\\nrf_sdh.c 0x00000000   Number         0  nrf_sdh.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\softdevice\\common\\nrf_sdh_ble.c 0x00000000   Number         0  nrf_sdh_ble.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\softdevice\\common\\nrf_sdh_soc.c 0x00000000   Number         0  nrf_sdh_soc.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\external\\fprintf\\nrf_fprintf.c 0x00000000   Number         0  nrf_fprintf.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\external\\fprintf\\nrf_fprintf_format.c 0x00000000   Number         0  nrf_fprintf_format.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\external\\segger_rtt\\SEGGER_RTT.c 0x00000000   Number         0  segger_rtt.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\external\\segger_rtt\\SEGGER_RTT_printf.c 0x00000000   Number         0  segger_rtt_printf.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\integration\\nrfx\\legacy\\nrf_drv_clock.c 0x00000000   Number         0  nrf_drv_clock.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\integration\\nrfx\\legacy\\nrf_drv_ppi.c 0x00000000   Number         0  nrf_drv_ppi.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\integration\\nrfx\\legacy\\nrf_drv_twi.c 0x00000000   Number         0  nrf_drv_twi.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\integration\\nrfx\\legacy\\nrf_drv_uart.c 0x00000000   Number         0  nrf_drv_uart.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\modules\\nrfx\\drivers\\src\\nrfx_clock.c 0x00000000   Number         0  nrfx_clock.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\modules\\nrfx\\drivers\\src\\nrfx_gpiote.c 0x00000000   Number         0  nrfx_gpiote.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\modules\\nrfx\\drivers\\src\\nrfx_ppi.c 0x00000000   Number         0  nrfx_ppi.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\modules\\nrfx\\drivers\\src\\nrfx_saadc.c 0x00000000   Number         0  nrfx_saadc.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\modules\\nrfx\\drivers\\src\\nrfx_timer.c 0x00000000   Number         0  nrfx_timer.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\modules\\nrfx\\drivers\\src\\nrfx_twi.c 0x00000000   Number         0  nrfx_twi.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\modules\\nrfx\\drivers\\src\\nrfx_twim.c 0x00000000   Number         0  nrfx_twim.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\modules\\nrfx\\drivers\\src\\nrfx_uart.c 0x00000000   Number         0  nrfx_uart.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\modules\\nrfx\\drivers\\src\\nrfx_uarte.c 0x00000000   Number         0  nrfx_uarte.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\modules\\nrfx\\drivers\\src\\prs\\nrfx_prs.c 0x00000000   Number         0  nrfx_prs.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\modules\\nrfx\\soc\\nrfx_atomic.c 0x00000000   Number         0  nrfx_atomic.o ABSOLUTE
    ..\\..\\..\\main.c                       0x00000000   Number         0  main.o ABSOLUTE
    RTE\Device\nRF52832_xxAA\arm_startup_nrf52.s 0x00000000   Number         0  arm_startup_nrf52.o ABSOLUTE
    RTE\Device\nRF52832_xxAA\system_nrf52.c  0x00000000   Number         0  system_nrf52.o ABSOLUTE
    RTE\\Device\\nRF52832_xxAA\\system_nrf52.c 0x00000000   Number         0  system_nrf52.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    RESET                                    0x00019000   Section      512  arm_startup_nrf52.o(RESET)
    .ARM.Collect$$$$00000000                 0x00019200   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x00019200   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x00019204   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x00019208   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x00019208   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x00019208   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x00019210   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x00019210   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x00019210   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x00019210   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .emb_text                                0x00019214   Section      226  nrf_atomic.o(.emb_text)
    $v0                                      0x00019214   Number         0  nrf_atomic.o(.emb_text)
    .text                                    0x000192f8   Section       36  arm_startup_nrf52.o(.text)
    $v0                                      0x000192f8   Number         0  arm_startup_nrf52.o(.text)
    .text                                    0x0001931c   Section        0  uldiv.o(.text)
    .text                                    0x0001937e   Section        0  llshl.o(.text)
    .text                                    0x0001939c   Section        0  llushr.o(.text)
    .text                                    0x000193bc   Section        0  ctype_o.o(.text)
    .text                                    0x000193c4   Section        0  memcpya.o(.text)
    .text                                    0x000193e8   Section        0  memseta.o(.text)
    .text                                    0x0001940c   Section        0  strcat.o(.text)
    .text                                    0x00019424   Section        0  strlen.o(.text)
    .text                                    0x00019432   Section        0  strcpy.o(.text)
    .text                                    0x00019444   Section        0  f2d.o(.text)
    .text                                    0x0001946a   Section        0  uidiv.o(.text)
    .text                                    0x00019496   Section        0  iusefp.o(.text)
    .text                                    0x00019496   Section        0  dadd.o(.text)
    .text                                    0x000195e4   Section        0  dmul.o(.text)
    .text                                    0x000196c8   Section        0  ddiv.o(.text)
    .text                                    0x000197a6   Section        0  dfixul.o(.text)
    .text                                    0x000197d8   Section       48  cdrcmple.o(.text)
    .text                                    0x00019808   Section       36  init.o(.text)
    .text                                    0x0001982c   Section        0  llsshr.o(.text)
    .text                                    0x00019850   Section        0  depilogue.o(.text)
    .text                                    0x0001990a   Section        0  __dczerorl2.o(.text)
    i.GPIOTE_IRQHandler                      0x00019960   Section        0  nrfx_gpiote.o(i.GPIOTE_IRQHandler)
    i.NVIC_ClearPendingIRQ                   0x00019ac4   Section        0  app_timer.o(i.NVIC_ClearPendingIRQ)
    NVIC_ClearPendingIRQ                     0x00019ac5   Thumb Code    22  app_timer.o(i.NVIC_ClearPendingIRQ)
    i.NVIC_EnableIRQ                         0x00019ada   Section        0  app_timer.o(i.NVIC_EnableIRQ)
    NVIC_EnableIRQ                           0x00019adb   Thumb Code    22  app_timer.o(i.NVIC_EnableIRQ)
    i.NVIC_SetPendingIRQ                     0x00019af0   Section        0  app_timer.o(i.NVIC_SetPendingIRQ)
    NVIC_SetPendingIRQ                       0x00019af1   Thumb Code    22  app_timer.o(i.NVIC_SetPendingIRQ)
    i.NVIC_SetPriority                       0x00019b06   Section        0  app_timer.o(i.NVIC_SetPriority)
    NVIC_SetPriority                         0x00019b07   Thumb Code    32  app_timer.o(i.NVIC_SetPriority)
    i.POWER_CLOCK_IRQHandler                 0x00019b28   Section        0  nrfx_clock.o(i.POWER_CLOCK_IRQHandler)
    i.RTC1_IRQHandler                        0x00019b80   Section        0  app_timer.o(i.RTC1_IRQHandler)
    i.SAADC_IRQHandler                       0x00019ba4   Section        0  nrfx_saadc.o(i.SAADC_IRQHandler)
    i.SEGGER_RTT_Init                        0x00019cec   Section        0  segger_rtt.o(i.SEGGER_RTT_Init)
    i.SEGGER_RTT_WriteNoLock                 0x00019cf0   Section        0  segger_rtt.o(i.SEGGER_RTT_WriteNoLock)
    i.SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler 0x00019d4c   Section        0  nrfx_twim.o(i.SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler)
    i.SWI0_EGU0_IRQHandler                   0x00019d5c   Section        0  app_timer.o(i.SWI0_EGU0_IRQHandler)
    i.SWI2_EGU2_IRQHandler                   0x00019d60   Section        0  nrf_sdh.o(i.SWI2_EGU2_IRQHandler)
    i.SystemInit                             0x00019d64   Section        0  system_nrf52.o(i.SystemInit)
    i.TIMER0_IRQHandler                      0x0001a080   Section        0  nrfx_timer.o(i.TIMER0_IRQHandler)
    i.UARTE0_UART0_IRQHandler                0x0001a0d0   Section        0  nrfx_prs.o(i.UARTE0_UART0_IRQHandler)
    i._DoInit                                0x0001a0dc   Section        0  segger_rtt.o(i._DoInit)
    _DoInit                                  0x0001a0dd   Thumb Code    76  segger_rtt.o(i._DoInit)
    i._GetAvailWriteSpace                    0x0001a144   Section        0  segger_rtt.o(i._GetAvailWriteSpace)
    _GetAvailWriteSpace                      0x0001a145   Thumb Code    22  segger_rtt.o(i._GetAvailWriteSpace)
    i._WriteBlocking                         0x0001a15a   Section        0  segger_rtt.o(i._WriteBlocking)
    _WriteBlocking                           0x0001a15b   Thumb Code    90  segger_rtt.o(i._WriteBlocking)
    i._WriteNoCheck                          0x0001a1b4   Section        0  segger_rtt.o(i._WriteNoCheck)
    _WriteNoCheck                            0x0001a1b5   Thumb Code    66  segger_rtt.o(i._WriteNoCheck)
    i.__0printf                              0x0001a1f8   Section        0  printfa.o(i.__0printf)
    i.__0sprintf                             0x0001a218   Section        0  printfa.o(i.__0sprintf)
    i.__scatterload_copy                     0x0001a240   Section       14  handlers.o(i.__scatterload_copy)
    i.__scatterload_null                     0x0001a24e   Section        2  handlers.o(i.__scatterload_null)
    i.__scatterload_zeroinit                 0x0001a250   Section       14  handlers.o(i.__scatterload_zeroinit)
    i.__sd_nvic_app_accessible_irq           0x0001a260   Section        0  nrf_sdh.o(i.__sd_nvic_app_accessible_irq)
    __sd_nvic_app_accessible_irq             0x0001a261   Thumb Code    32  nrf_sdh.o(i.__sd_nvic_app_accessible_irq)
    i._fp_digits                             0x0001a284   Section        0  printfa.o(i._fp_digits)
    _fp_digits                               0x0001a285   Thumb Code   366  printfa.o(i._fp_digits)
    i._printf_core                           0x0001a408   Section        0  printfa.o(i._printf_core)
    _printf_core                             0x0001a409   Thumb Code  1744  printfa.o(i._printf_core)
    i._printf_post_padding                   0x0001aae4   Section        0  printfa.o(i._printf_post_padding)
    _printf_post_padding                     0x0001aae5   Thumb Code    36  printfa.o(i._printf_post_padding)
    i._printf_pre_padding                    0x0001ab08   Section        0  printfa.o(i._printf_pre_padding)
    _printf_pre_padding                      0x0001ab09   Thumb Code    46  printfa.o(i._printf_pre_padding)
    i._sputc                                 0x0001ab36   Section        0  printfa.o(i._sputc)
    _sputc                                   0x0001ab37   Thumb Code    10  printfa.o(i._sputc)
    i.advertising_buttons_configure          0x0001ab40   Section        0  bsp_btn_ble.o(i.advertising_buttons_configure)
    advertising_buttons_configure            0x0001ab41   Thumb Code    54  bsp_btn_ble.o(i.advertising_buttons_configure)
    i.alert_timer_handler                    0x0001ab76   Section        0  bsp.o(i.alert_timer_handler)
    alert_timer_handler                      0x0001ab77   Thumb Code     6  bsp.o(i.alert_timer_handler)
    i.app_button_enable                      0x0001ab7c   Section        0  app_button.o(i.app_button_enable)
    i.app_button_init                        0x0001aba0   Section        0  app_button.o(i.app_button_init)
    i.app_error_fault_handler                0x0001ac18   Section        0  app_error_weak.o(i.app_error_fault_handler)
    i.app_error_handler_bare                 0x0001ac9c   Section        0  app_error.o(i.app_error_handler_bare)
    i.app_fifo_get                           0x0001acb2   Section        0  app_fifo.o(i.app_fifo_get)
    i.app_fifo_init                          0x0001acc8   Section        0  app_fifo.o(i.app_fifo_init)
    i.app_fifo_put                           0x0001ace8   Section        0  app_fifo.o(i.app_fifo_put)
    i.app_timer_create                       0x0001ad04   Section        0  app_timer.o(i.app_timer_create)
    i.app_timer_init                         0x0001ad2c   Section        0  app_timer.o(i.app_timer_init)
    i.app_timer_start                        0x0001ad80   Section        0  app_timer.o(i.app_timer_start)
    i.app_timer_stop                         0x0001ae08   Section        0  app_timer.o(i.app_timer_stop)
    i.app_uart_get                           0x0001ae28   Section        0  app_uart_fifo.o(i.app_uart_get)
    i.app_uart_init                          0x0001ae5c   Section        0  app_uart_fifo.o(i.app_uart_init)
    i.app_uart_put                           0x0001af00   Section        0  app_uart_fifo.o(i.app_uart_put)
    i.app_util_critical_region_enter         0x0001af54   Section        0  app_util_platform.o(i.app_util_critical_region_enter)
    i.app_util_critical_region_exit          0x0001af9c   Section        0  app_util_platform.o(i.app_util_critical_region_exit)
    i.apply_config                           0x0001afd0   Section        0  nrfx_uart.o(i.apply_config)
    apply_config                             0x0001afd1   Thumb Code   136  nrfx_uart.o(i.apply_config)
    i.apply_config                           0x0001b058   Section        0  nrfx_uarte.o(i.apply_config)
    apply_config                             0x0001b059   Thumb Code   136  nrfx_uarte.o(i.apply_config)
    i.are_app_channels                       0x0001b0e0   Section        0  nrfx_ppi.o(i.are_app_channels)
    are_app_channels                         0x0001b0e1   Thumb Code    12  nrfx_ppi.o(i.are_app_channels)
    i.blcm_link_ctx_get                      0x0001b0ec   Section        0  ble_link_ctx_manager.o(i.blcm_link_ctx_get)
    i.ble_advdata_encode                     0x0001b134   Section        0  ble_advdata.o(i.ble_advdata_encode)
    i.ble_advdata_parse                      0x0001b2b6   Section        0  ble_advdata.o(i.ble_advdata_parse)
    i.ble_advdata_search                     0x0001b2d6   Section        0  ble_advdata.o(i.ble_advdata_search)
    i.ble_advertising_conn_cfg_tag_set       0x0001b30e   Section        0  ble_advertising.o(i.ble_advertising_conn_cfg_tag_set)
    i.ble_advertising_init                   0x0001b314   Section        0  ble_advertising.o(i.ble_advertising_init)
    i.ble_advertising_on_ble_evt             0x0001b3fe   Section        0  ble_advertising.o(i.ble_advertising_on_ble_evt)
    i.ble_advertising_on_sys_evt             0x0001b468   Section        0  ble_advertising.o(i.ble_advertising_on_sys_evt)
    i.ble_advertising_restart_without_whitelist 0x0001b46a   Section        0  ble_advertising.o(i.ble_advertising_restart_without_whitelist)
    i.ble_advertising_start                  0x0001b4a4   Section        0  ble_advertising.o(i.ble_advertising_start)
    i.ble_conn_params_init                   0x0001b6a8   Section        0  ble_conn_params.o(i.ble_conn_params_init)
    i.ble_conn_state_conn_idx                0x0001b710   Section        0  ble_conn_state.o(i.ble_conn_state_conn_idx)
    i.ble_conn_state_valid                   0x0001b724   Section        0  ble_conn_state.o(i.ble_conn_state_valid)
    i.ble_device_addr_encode                 0x0001b738   Section        0  ble_advdata.o(i.ble_device_addr_encode)
    ble_device_addr_encode                   0x0001b739   Thumb Code    96  ble_advdata.o(i.ble_device_addr_encode)
    i.ble_evt_handler                        0x0001b798   Section        0  main.o(i.ble_evt_handler)
    ble_evt_handler                          0x0001b799   Thumb Code   172  main.o(i.ble_evt_handler)
    i.ble_evt_handler                        0x0001b870   Section        0  bsp_btn_ble.o(i.ble_evt_handler)
    ble_evt_handler                          0x0001b871   Thumb Code   106  bsp_btn_ble.o(i.ble_evt_handler)
    i.ble_evt_handler                        0x0001b8e0   Section        0  ble_conn_params.o(i.ble_evt_handler)
    ble_evt_handler                          0x0001b8e1   Thumb Code   242  ble_conn_params.o(i.ble_evt_handler)
    i.ble_evt_handler                        0x0001b9dc   Section        0  ble_conn_state.o(i.ble_evt_handler)
    ble_evt_handler                          0x0001b9dd   Thumb Code   254  ble_conn_state.o(i.ble_evt_handler)
    i.ble_nus_data_send                      0x0001bae0   Section        0  ble_nus.o(i.ble_nus_data_send)
    i.ble_nus_init                           0x0001bb48   Section        0  ble_nus.o(i.ble_nus_init)
    i.ble_nus_on_ble_evt                     0x0001bc1c   Section        0  ble_nus.o(i.ble_nus_on_ble_evt)
    i.ble_srv_is_notification_enabled        0x0001bc8c   Section        0  ble_srv_common.o(i.ble_srv_is_notification_enabled)
    i.bsp_board_button_idx_to_pin            0x0001bc94   Section        0  boards.o(i.bsp_board_button_idx_to_pin)
    i.bsp_board_button_state_get             0x0001bca0   Section        0  boards.o(i.bsp_board_button_state_get)
    i.bsp_board_init                         0x0001bcc0   Section        0  boards.o(i.bsp_board_init)
    i.bsp_board_led_invert                   0x0001bd14   Section        0  boards.o(i.bsp_board_led_invert)
    i.bsp_board_led_off                      0x0001bd38   Section        0  boards.o(i.bsp_board_led_off)
    i.bsp_board_led_on                       0x0001bd48   Section        0  boards.o(i.bsp_board_led_on)
    i.bsp_board_led_state_get                0x0001bd58   Section        0  boards.o(i.bsp_board_led_state_get)
    i.bsp_board_leds_off                     0x0001bd78   Section        0  boards.o(i.bsp_board_leds_off)
    i.bsp_board_leds_on                      0x0001bd8a   Section        0  boards.o(i.bsp_board_leds_on)
    i.bsp_board_pin_to_button_idx            0x0001bd9c   Section        0  boards.o(i.bsp_board_pin_to_button_idx)
    i.bsp_btn_ble_init                       0x0001bdc0   Section        0  bsp_btn_ble.o(i.bsp_btn_ble_init)
    i.bsp_btn_ble_sleep_mode_prepare         0x0001bdf8   Section        0  bsp_btn_ble.o(i.bsp_btn_ble_sleep_mode_prepare)
    i.bsp_button_event_handler               0x0001be18   Section        0  bsp.o(i.bsp_button_event_handler)
    bsp_button_event_handler                 0x0001be19   Thumb Code   132  bsp.o(i.bsp_button_event_handler)
    i.bsp_button_is_pressed                  0x0001bea8   Section        0  bsp.o(i.bsp_button_is_pressed)
    i.bsp_event_handler                      0x0001beb4   Section        0  main.o(i.bsp_event_handler)
    i.bsp_event_to_button_action_assign      0x0001bf10   Section        0  bsp.o(i.bsp_event_to_button_action_assign)
    i.bsp_indication_set                     0x0001bf54   Section        0  bsp.o(i.bsp_indication_set)
    i.bsp_init                               0x0001bf6c   Section        0  bsp.o(i.bsp_init)
    i.bsp_led_indication                     0x0001c000   Section        0  bsp.o(i.bsp_led_indication)
    bsp_led_indication                       0x0001c001   Thumb Code   446  bsp.o(i.bsp_led_indication)
    i.bsp_wakeup_button_enable               0x0001c1c8   Section        0  bsp.o(i.bsp_wakeup_button_enable)
    i.buf_prealloc                           0x0001c1d0   Section        0  nrf_log_frontend.o(i.buf_prealloc)
    buf_prealloc                             0x0001c1d1   Thumb Code   138  nrf_log_frontend.o(i.buf_prealloc)
    i.buffer_add                             0x0001c260   Section        0  nrf_fprintf_format.o(i.buffer_add)
    buffer_add                               0x0001c261   Thumb Code    46  nrf_fprintf_format.o(i.buffer_add)
    i.buffer_is_empty                        0x0001c290   Section        0  nrf_log_frontend.o(i.buffer_is_empty)
    i.button_timer_handler                   0x0001c2a4   Section        0  bsp.o(i.button_timer_handler)
    button_timer_handler                     0x0001c2a5   Thumb Code     8  bsp.o(i.button_timer_handler)
    i.channel_free                           0x0001c2ac   Section        0  nrfx_gpiote.o(i.channel_free)
    channel_free                             0x0001c2ad   Thumb Code    22  nrfx_gpiote.o(i.channel_free)
    i.channel_port_alloc                     0x0001c2c8   Section        0  nrfx_gpiote.o(i.channel_port_alloc)
    channel_port_alloc                       0x0001c2c9   Thumb Code    66  nrfx_gpiote.o(i.channel_port_alloc)
    i.channel_port_get                       0x0001c310   Section        0  nrfx_gpiote.o(i.channel_port_get)
    channel_port_get                         0x0001c311   Thumb Code    10  nrfx_gpiote.o(i.channel_port_get)
    i.characteristic_add                     0x0001c320   Section        0  ble_srv_common.o(i.characteristic_add)
    i.clock_clk_started_notify               0x0001c4b0   Section        0  nrf_drv_clock.o(i.clock_clk_started_notify)
    clock_clk_started_notify                 0x0001c4b1   Thumb Code    34  nrf_drv_clock.o(i.clock_clk_started_notify)
    i.clock_irq_handler                      0x0001c4d8   Section        0  nrf_drv_clock.o(i.clock_irq_handler)
    clock_irq_handler                        0x0001c4d9   Thumb Code    24  nrf_drv_clock.o(i.clock_irq_handler)
    i.compare_reg_update                     0x0001c4f4   Section        0  app_timer.o(i.compare_reg_update)
    compare_reg_update                       0x0001c4f5   Thumb Code   160  app_timer.o(i.compare_reg_update)
    i.conn_handle_list_get                   0x0001c5a0   Section        0  ble_conn_state.o(i.conn_handle_list_get)
    i.conn_int_encode                        0x0001c5de   Section        0  ble_advdata.o(i.conn_int_encode)
    conn_int_encode                          0x0001c5df   Thumb Code   136  ble_advdata.o(i.conn_int_encode)
    i.conn_params_error_handler              0x0001c666   Section        0  main.o(i.conn_params_error_handler)
    conn_params_error_handler                0x0001c667   Thumb Code     4  main.o(i.conn_params_error_handler)
    i.conn_params_negotiation                0x0001c66c   Section        0  ble_conn_params.o(i.conn_params_negotiation)
    conn_params_negotiation                  0x0001c66d   Thumb Code    68  ble_conn_params.o(i.conn_params_negotiation)
    i.detection_delay_timeout_handler        0x0001c6b4   Section        0  app_button.o(i.detection_delay_timeout_handler)
    detection_delay_timeout_handler          0x0001c6b5   Thumb Code   150  app_button.o(i.detection_delay_timeout_handler)
    i.dropped_sat16_get                      0x0001c750   Section        0  nrf_log_frontend.o(i.dropped_sat16_get)
    dropped_sat16_get                        0x0001c751   Thumb Code    16  nrf_log_frontend.o(i.dropped_sat16_get)
    i.elapsed_ticks_acquire                  0x0001c764   Section        0  app_timer.o(i.elapsed_ticks_acquire)
    elapsed_ticks_acquire                    0x0001c765   Thumb Code    58  app_timer.o(i.elapsed_ticks_acquire)
    i.fifo_get                               0x0001c7a4   Section        0  app_fifo.o(i.fifo_get)
    fifo_get                                 0x0001c7a5   Thumb Code    20  app_fifo.o(i.fifo_get)
    i.fifo_put                               0x0001c7b8   Section        0  app_fifo.o(i.fifo_put)
    fifo_put                                 0x0001c7b9   Thumb Code    18  app_fifo.o(i.fifo_put)
    i.flags_set                              0x0001c7ca   Section        0  ble_advertising.o(i.flags_set)
    flags_set                                0x0001c7cb   Thumb Code    40  ble_advertising.o(i.flags_set)
    i.fputc                                  0x0001c7f2   Section        0  retarget.o(i.fputc)
    i.gatt_evt_handler                       0x0001c800   Section        0  main.o(i.gatt_evt_handler)
    i.gatt_init                              0x0001c85c   Section        0  main.o(i.gatt_init)
    i.gpiote_event_handler                   0x0001c88c   Section        0  app_button.o(i.gpiote_event_handler)
    gpiote_event_handler                     0x0001c88d   Thumb Code   122  app_button.o(i.gpiote_event_handler)
    i.instance_get                           0x0001c910   Section        0  ble_conn_params.o(i.instance_get)
    instance_get                             0x0001c911   Thumb Code    14  ble_conn_params.o(i.instance_get)
    i.int_print                              0x0001c924   Section        0  nrf_fprintf_format.o(i.int_print)
    int_print                                0x0001c925   Thumb Code   166  nrf_fprintf_format.o(i.int_print)
    i.interrupts_enable                      0x0001c9cc   Section        0  nrfx_uarte.o(i.interrupts_enable)
    interrupts_enable                        0x0001c9cd   Thumb Code   118  nrfx_uarte.o(i.interrupts_enable)
    i.invalid_packets_omit                   0x0001ca48   Section        0  nrf_log_frontend.o(i.invalid_packets_omit)
    invalid_packets_omit                     0x0001ca49   Thumb Code    52  nrf_log_frontend.o(i.invalid_packets_omit)
    i.is_allocated_channel                   0x0001ca7c   Section        0  nrfx_ppi.o(i.is_allocated_channel)
    is_allocated_channel                     0x0001ca7d   Thumb Code    20  nrfx_ppi.o(i.is_allocated_channel)
    i.is_app_channel                         0x0001ca94   Section        0  nrfx_ppi.o(i.is_app_channel)
    is_app_channel                           0x0001ca95   Thumb Code    10  nrfx_ppi.o(i.is_app_channel)
    i.is_conn_params_ok                      0x0001ca9e   Section        0  ble_conn_params.o(i.is_conn_params_ok)
    is_conn_params_ok                        0x0001ca9f   Thumb Code    68  ble_conn_params.o(i.is_conn_params_ok)
    i.is_programmable_app_channel            0x0001cae2   Section        0  nrfx_ppi.o(i.is_programmable_app_channel)
    is_programmable_app_channel              0x0001cae3   Thumb Code    12  nrfx_ppi.o(i.is_programmable_app_channel)
    i.leds_off                               0x0001caf0   Section        0  bsp.o(i.leds_off)
    leds_off                                 0x0001caf1   Thumb Code    38  bsp.o(i.leds_off)
    i.leds_timer_handler                     0x0001cb1c   Section        0  bsp.o(i.leds_timer_handler)
    leds_timer_handler                       0x0001cb1d   Thumb Code    16  bsp.o(i.leds_timer_handler)
    i.link_init                              0x0001cb30   Section        0  nrf_ble_gatt.o(i.link_init)
    link_init                                0x0001cb31   Thumb Code    16  nrf_ble_gatt.o(i.link_init)
    i.list_insertions_handler                0x0001cb40   Section        0  app_timer.o(i.list_insertions_handler)
    list_insertions_handler                  0x0001cb41   Thumb Code   234  app_timer.o(i.list_insertions_handler)
    i.log_skip                               0x0001cc38   Section        0  nrf_log_frontend.o(i.log_skip)
    log_skip                                 0x0001cc39   Thumb Code   148  nrf_log_frontend.o(i.log_skip)
    i.main                                   0x0001ccd4   Section        0  main.o(i.main)
    i.manuf_specific_data_encode             0x0001cf74   Section        0  ble_advdata.o(i.manuf_specific_data_encode)
    manuf_specific_data_encode               0x0001cf75   Thumb Code   100  ble_advdata.o(i.manuf_specific_data_encode)
    i.memobj_op                              0x0001cfd8   Section        0  nrf_memobj.o(i.memobj_op)
    memobj_op                                0x0001cfd9   Thumb Code   126  nrf_memobj.o(i.memobj_op)
    i.module_idx_get                         0x0001d058   Section        0  nrf_log_frontend.o(i.module_idx_get)
    module_idx_get                           0x0001d059   Thumb Code    42  nrf_log_frontend.o(i.module_idx_get)
    i.name_encode                            0x0001d088   Section        0  ble_advdata.o(i.name_encode)
    name_encode                              0x0001d089   Thumb Code   166  ble_advdata.o(i.name_encode)
    i.nrf_atflags_clear                      0x0001d12e   Section        0  nrf_atflags.o(i.nrf_atflags_clear)
    i.nrf_atflags_get                        0x0001d144   Section        0  nrf_atflags.o(i.nrf_atflags_get)
    i.nrf_atflags_set                        0x0001d15a   Section        0  nrf_atflags.o(i.nrf_atflags_set)
    i.nrf_atomic_flag_clear_fetch            0x0001d16e   Section        0  nrf_atomic.o(i.nrf_atomic_flag_clear_fetch)
    i.nrf_atomic_flag_set                    0x0001d174   Section        0  nrf_atomic.o(i.nrf_atomic_flag_set)
    i.nrf_atomic_u32_add                     0x0001d17a   Section        0  nrf_atomic.o(i.nrf_atomic_u32_add)
    i.nrf_atomic_u32_and                     0x0001d186   Section        0  nrf_atomic.o(i.nrf_atomic_u32_and)
    i.nrf_atomic_u32_fetch_and               0x0001d192   Section        0  nrf_atomic.o(i.nrf_atomic_u32_fetch_and)
    i.nrf_atomic_u32_fetch_store             0x0001d19c   Section        0  nrf_atomic.o(i.nrf_atomic_u32_fetch_store)
    i.nrf_atomic_u32_or                      0x0001d1a6   Section        0  nrf_atomic.o(i.nrf_atomic_u32_or)
    i.nrf_atomic_u32_sub                     0x0001d1b2   Section        0  nrf_atomic.o(i.nrf_atomic_u32_sub)
    i.nrf_balloc_alloc                       0x0001d1be   Section        0  nrf_balloc.o(i.nrf_balloc_alloc)
    i.nrf_balloc_free                        0x0001d202   Section        0  nrf_balloc.o(i.nrf_balloc_free)
    i.nrf_balloc_init                        0x0001d232   Section        0  nrf_balloc.o(i.nrf_balloc_init)
    i.nrf_bitmask_bit_is_set                 0x0001d262   Section        0  nrfx_gpiote.o(i.nrf_bitmask_bit_is_set)
    nrf_bitmask_bit_is_set                   0x0001d263   Thumb Code    16  nrfx_gpiote.o(i.nrf_bitmask_bit_is_set)
    i.nrf_bitmask_bit_set                    0x0001d272   Section        0  nrfx_gpiote.o(i.nrf_bitmask_bit_set)
    nrf_bitmask_bit_set                      0x0001d273   Thumb Code    20  nrfx_gpiote.o(i.nrf_bitmask_bit_set)
    i.nrf_ble_gatt_att_mtu_periph_set        0x0001d286   Section        0  nrf_ble_gatt.o(i.nrf_ble_gatt_att_mtu_periph_set)
    i.nrf_ble_gatt_init                      0x0001d29e   Section        0  nrf_ble_gatt.o(i.nrf_ble_gatt_init)
    i.nrf_ble_gatt_on_ble_evt                0x0001d2c0   Section        0  nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt)
    i.nrf_ble_qwr_conn_handle_assign         0x0001d3b4   Section        0  nrf_ble_qwr.o(i.nrf_ble_qwr_conn_handle_assign)
    i.nrf_ble_qwr_init                       0x0001d3ca   Section        0  nrf_ble_qwr.o(i.nrf_ble_qwr_init)
    i.nrf_ble_qwr_on_ble_evt                 0x0001d3ee   Section        0  nrf_ble_qwr.o(i.nrf_ble_qwr_on_ble_evt)
    i.nrf_clock_event_check                  0x0001d4a4   Section        0  nrfx_clock.o(i.nrf_clock_event_check)
    nrf_clock_event_check                    0x0001d4a5   Thumb Code    14  nrfx_clock.o(i.nrf_clock_event_check)
    i.nrf_clock_event_clear                  0x0001d4b2   Section        0  nrfx_clock.o(i.nrf_clock_event_clear)
    nrf_clock_event_clear                    0x0001d4b3   Thumb Code    16  nrfx_clock.o(i.nrf_clock_event_clear)
    i.nrf_drv_clock_init                     0x0001d4c4   Section        0  nrf_drv_clock.o(i.nrf_drv_clock_init)
    i.nrf_drv_clock_lfclk_release            0x0001d4fc   Section        0  nrf_drv_clock.o(i.nrf_drv_clock_lfclk_release)
    i.nrf_drv_ppi_init                       0x0001d52c   Section        0  nrf_drv_ppi.o(i.nrf_drv_ppi_init)
    i.nrf_drv_uart_init                      0x0001d544   Section        0  nrf_drv_uart.o(i.nrf_drv_uart_init)
    i.nrf_drv_uart_rx                        0x0001d5ac   Section        0  app_uart_fifo.o(i.nrf_drv_uart_rx)
    nrf_drv_uart_rx                          0x0001d5ad   Thumb Code    26  app_uart_fifo.o(i.nrf_drv_uart_rx)
    i.nrf_drv_uart_tx                        0x0001d5cc   Section        0  app_uart_fifo.o(i.nrf_drv_uart_tx)
    nrf_drv_uart_tx                          0x0001d5cd   Thumb Code    26  app_uart_fifo.o(i.nrf_drv_uart_tx)
    i.nrf_fprintf                            0x0001d5ec   Section        0  nrf_fprintf.o(i.nrf_fprintf)
    i.nrf_fprintf_buffer_flush               0x0001d606   Section        0  nrf_fprintf.o(i.nrf_fprintf_buffer_flush)
    i.nrf_fprintf_fmt                        0x0001d61e   Section        0  nrf_fprintf_format.o(i.nrf_fprintf_fmt)
    i.nrf_gpio_cfg                           0x0001d7f8   Section        0  boards.o(i.nrf_gpio_cfg)
    nrf_gpio_cfg                             0x0001d7f9   Thumb Code    36  boards.o(i.nrf_gpio_cfg)
    i.nrf_gpio_cfg                           0x0001d81c   Section        0  nrfx_gpiote.o(i.nrf_gpio_cfg)
    nrf_gpio_cfg                             0x0001d81d   Thumb Code    36  nrfx_gpiote.o(i.nrf_gpio_cfg)
    i.nrf_gpio_cfg                           0x0001d840   Section        0  nrfx_uart.o(i.nrf_gpio_cfg)
    nrf_gpio_cfg                             0x0001d841   Thumb Code    36  nrfx_uart.o(i.nrf_gpio_cfg)
    i.nrf_gpio_cfg                           0x0001d864   Section        0  nrfx_uarte.o(i.nrf_gpio_cfg)
    nrf_gpio_cfg                             0x0001d865   Thumb Code    36  nrfx_uarte.o(i.nrf_gpio_cfg)
    i.nrf_gpio_cfg_input                     0x0001d888   Section        0  nrfx_uart.o(i.nrf_gpio_cfg_input)
    nrf_gpio_cfg_input                       0x0001d889   Thumb Code    18  nrfx_uart.o(i.nrf_gpio_cfg_input)
    i.nrf_gpio_cfg_input                     0x0001d89a   Section        0  nrfx_uarte.o(i.nrf_gpio_cfg_input)
    nrf_gpio_cfg_input                       0x0001d89b   Thumb Code    18  nrfx_uarte.o(i.nrf_gpio_cfg_input)
    i.nrf_gpio_cfg_output                    0x0001d8ac   Section        0  nrfx_uart.o(i.nrf_gpio_cfg_output)
    nrf_gpio_cfg_output                      0x0001d8ad   Thumb Code    20  nrfx_uart.o(i.nrf_gpio_cfg_output)
    i.nrf_gpio_cfg_output                    0x0001d8c0   Section        0  nrfx_uarte.o(i.nrf_gpio_cfg_output)
    nrf_gpio_cfg_output                      0x0001d8c1   Thumb Code    20  nrfx_uarte.o(i.nrf_gpio_cfg_output)
    i.nrf_gpio_cfg_sense_set                 0x0001d8d4   Section        0  nrfx_gpiote.o(i.nrf_gpio_cfg_sense_set)
    nrf_gpio_cfg_sense_set                   0x0001d8d5   Thumb Code    34  nrfx_gpiote.o(i.nrf_gpio_cfg_sense_set)
    i.nrf_gpio_pin_write                     0x0001d8f6   Section        0  boards.o(i.nrf_gpio_pin_write)
    nrf_gpio_pin_write                       0x0001d8f7   Thumb Code    22  boards.o(i.nrf_gpio_pin_write)
    i.nrf_gpio_ports_read                    0x0001d90c   Section        0  nrfx_gpiote.o(i.nrf_gpio_ports_read)
    nrf_gpio_ports_read                      0x0001d90d   Thumb Code    34  nrfx_gpiote.o(i.nrf_gpio_ports_read)
    i.nrf_gpiote_event_clear                 0x0001d934   Section        0  nrfx_gpiote.o(i.nrf_gpiote_event_clear)
    nrf_gpiote_event_clear                   0x0001d935   Thumb Code    16  nrfx_gpiote.o(i.nrf_gpiote_event_clear)
    i.nrf_gpiote_event_is_set                0x0001d948   Section        0  nrfx_gpiote.o(i.nrf_gpiote_event_is_set)
    nrf_gpiote_event_is_set                  0x0001d949   Thumb Code    12  nrfx_gpiote.o(i.nrf_gpiote_event_is_set)
    i.nrf_log_backend_add                    0x0001d958   Section        0  nrf_log_frontend.o(i.nrf_log_backend_add)
    i.nrf_log_backend_rtt_flush              0x0001d9b4   Section        0  nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_flush)
    nrf_log_backend_rtt_flush                0x0001d9b5   Thumb Code     2  nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_flush)
    i.nrf_log_backend_rtt_init               0x0001d9b6   Section        0  nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_init)
    i.nrf_log_backend_rtt_panic_set          0x0001d9ba   Section        0  nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_panic_set)
    nrf_log_backend_rtt_panic_set            0x0001d9bb   Thumb Code     2  nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_panic_set)
    i.nrf_log_backend_rtt_put                0x0001d9bc   Section        0  nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_put)
    nrf_log_backend_rtt_put                  0x0001d9bd   Thumb Code    16  nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_put)
    i.nrf_log_backend_serial_put             0x0001d9d4   Section        0  nrf_log_backend_serial.o(i.nrf_log_backend_serial_put)
    i.nrf_log_color_id_get                   0x0001da9c   Section        0  nrf_log_frontend.o(i.nrf_log_color_id_get)
    i.nrf_log_default_backends_init          0x0001dacc   Section        0  nrf_log_default_backends.o(i.nrf_log_default_backends_init)
    i.nrf_log_frontend_dequeue               0x0001dae8   Section        0  nrf_log_frontend.o(i.nrf_log_frontend_dequeue)
    i.nrf_log_frontend_std_0                 0x0001dd1c   Section        0  nrf_log_frontend.o(i.nrf_log_frontend_std_0)
    i.nrf_log_frontend_std_1                 0x0001dd24   Section        0  nrf_log_frontend.o(i.nrf_log_frontend_std_1)
    i.nrf_log_frontend_std_2                 0x0001dd32   Section        0  nrf_log_frontend.o(i.nrf_log_frontend_std_2)
    i.nrf_log_hexdump_entry_process          0x0001dd44   Section        0  nrf_log_str_formatter.o(i.nrf_log_hexdump_entry_process)
    i.nrf_log_init                           0x0001ddf4   Section        0  nrf_log_frontend.o(i.nrf_log_init)
    i.nrf_log_module_cnt_get                 0x0001de30   Section        0  nrf_log_frontend.o(i.nrf_log_module_cnt_get)
    i.nrf_log_module_name_get                0x0001de44   Section        0  nrf_log_frontend.o(i.nrf_log_module_name_get)
    i.nrf_log_panic                          0x0001de60   Section        0  nrf_log_frontend.o(i.nrf_log_panic)
    i.nrf_log_std_entry_process              0x0001de8c   Section        0  nrf_log_str_formatter.o(i.nrf_log_std_entry_process)
    i.nrf_memobj_alloc                       0x0001df42   Section        0  nrf_memobj.o(i.nrf_memobj_alloc)
    i.nrf_memobj_free                        0x0001dfa2   Section        0  nrf_memobj.o(i.nrf_memobj_free)
    i.nrf_memobj_get                         0x0001dfd4   Section        0  nrf_memobj.o(i.nrf_memobj_get)
    i.nrf_memobj_pool_init                   0x0001dfdc   Section        0  nrf_memobj.o(i.nrf_memobj_pool_init)
    i.nrf_memobj_put                         0x0001dfe0   Section        0  nrf_memobj.o(i.nrf_memobj_put)
    i.nrf_memobj_read                        0x0001dffe   Section        0  nrf_memobj.o(i.nrf_memobj_read)
    i.nrf_memobj_write                       0x0001e00e   Section        0  nrf_memobj.o(i.nrf_memobj_write)
    i.nrf_pwr_mgmt_init                      0x0001e020   Section        0  nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_init)
    i.nrf_pwr_mgmt_run                       0x0001e048   Section        0  nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_run)
    i.nrf_qwr_error_handler                  0x0001e08c   Section        0  main.o(i.nrf_qwr_error_handler)
    nrf_qwr_error_handler                    0x0001e08d   Thumb Code     4  main.o(i.nrf_qwr_error_handler)
    i.nrf_ringbuf_init                       0x0001e090   Section        0  nrf_ringbuf.o(i.nrf_ringbuf_init)
    i.nrf_saadc_buffer_init                  0x0001e0ac   Section        0  nrfx_saadc.o(i.nrf_saadc_buffer_init)
    nrf_saadc_buffer_init                    0x0001e0ad   Thumb Code    10  nrfx_saadc.o(i.nrf_saadc_buffer_init)
    i.nrf_saadc_channel_input_set            0x0001e0bc   Section        0  nrfx_saadc.o(i.nrf_saadc_channel_input_set)
    nrf_saadc_channel_input_set              0x0001e0bd   Thumb Code    16  nrfx_saadc.o(i.nrf_saadc_channel_input_set)
    i.nrf_saadc_event_check                  0x0001e0d0   Section        0  nrfx_saadc.o(i.nrf_saadc_event_check)
    nrf_saadc_event_check                    0x0001e0d1   Thumb Code    12  nrfx_saadc.o(i.nrf_saadc_event_check)
    i.nrf_saadc_event_clear                  0x0001e0e0   Section        0  nrfx_saadc.o(i.nrf_saadc_event_clear)
    nrf_saadc_event_clear                    0x0001e0e1   Thumb Code    16  nrfx_saadc.o(i.nrf_saadc_event_clear)
    i.nrf_sdh_ble_app_ram_start_get          0x0001e0f4   Section        0  nrf_sdh_ble.o(i.nrf_sdh_ble_app_ram_start_get)
    i.nrf_sdh_ble_default_cfg_set            0x0001e108   Section        0  nrf_sdh_ble.o(i.nrf_sdh_ble_default_cfg_set)
    i.nrf_sdh_ble_enable                     0x0001e230   Section        0  nrf_sdh_ble.o(i.nrf_sdh_ble_enable)
    i.nrf_sdh_ble_evts_poll                  0x0001e360   Section        0  nrf_sdh_ble.o(i.nrf_sdh_ble_evts_poll)
    nrf_sdh_ble_evts_poll                    0x0001e361   Thumb Code    88  nrf_sdh_ble.o(i.nrf_sdh_ble_evts_poll)
    i.nrf_sdh_enable_request                 0x0001e3c0   Section        0  nrf_sdh.o(i.nrf_sdh_enable_request)
    i.nrf_sdh_evts_poll                      0x0001e434   Section        0  nrf_sdh.o(i.nrf_sdh_evts_poll)
    i.nrf_sdh_is_enabled                     0x0001e458   Section        0  nrf_sdh.o(i.nrf_sdh_is_enabled)
    i.nrf_sdh_soc_evts_poll                  0x0001e464   Section        0  nrf_sdh_soc.o(i.nrf_sdh_soc_evts_poll)
    nrf_sdh_soc_evts_poll                    0x0001e465   Thumb Code    56  nrf_sdh_soc.o(i.nrf_sdh_soc_evts_poll)
    i.nrf_section_iter_init                  0x0001e4a0   Section        0  nrf_section_iter.o(i.nrf_section_iter_init)
    i.nrf_section_iter_item_set              0x0001e4aa   Section        0  nrf_section_iter.o(i.nrf_section_iter_item_set)
    nrf_section_iter_item_set                0x0001e4ab   Thumb Code    36  nrf_section_iter.o(i.nrf_section_iter_item_set)
    i.nrf_section_iter_next                  0x0001e4ce   Section        0  nrf_section_iter.o(i.nrf_section_iter_next)
    i.nrf_strerror_find                      0x0001e4f0   Section        0  nrf_strerror.o(i.nrf_strerror_find)
    i.nrf_strerror_get                       0x0001e528   Section        0  nrf_strerror.o(i.nrf_strerror_get)
    i.nrf_timer_event_clear                  0x0001e53c   Section        0  nrfx_timer.o(i.nrf_timer_event_clear)
    nrf_timer_event_clear                    0x0001e53d   Thumb Code    12  nrfx_timer.o(i.nrf_timer_event_clear)
    i.nrf_twim_event_check                   0x0001e548   Section        0  nrfx_twim.o(i.nrf_twim_event_check)
    nrf_twim_event_check                     0x0001e549   Thumb Code    10  nrfx_twim.o(i.nrf_twim_event_check)
    i.nrf_twim_event_clear                   0x0001e552   Section        0  nrfx_twim.o(i.nrf_twim_event_clear)
    nrf_twim_event_clear                     0x0001e553   Thumb Code    12  nrfx_twim.o(i.nrf_twim_event_clear)
    i.nrf_uart_event_check                   0x0001e55e   Section        0  nrfx_uart.o(i.nrf_uart_event_check)
    nrf_uart_event_check                     0x0001e55f   Thumb Code    10  nrfx_uart.o(i.nrf_uart_event_check)
    i.nrf_uart_event_clear                   0x0001e568   Section        0  nrfx_uart.o(i.nrf_uart_event_clear)
    nrf_uart_event_clear                     0x0001e569   Thumb Code    12  nrfx_uart.o(i.nrf_uart_event_clear)
    i.nrf_uart_int_enable_check              0x0001e574   Section        0  nrfx_uart.o(i.nrf_uart_int_enable_check)
    nrf_uart_int_enable_check                0x0001e575   Thumb Code    12  nrfx_uart.o(i.nrf_uart_int_enable_check)
    i.nrf_uarte_event_check                  0x0001e580   Section        0  nrfx_uarte.o(i.nrf_uarte_event_check)
    nrf_uarte_event_check                    0x0001e581   Thumb Code    10  nrfx_uarte.o(i.nrf_uarte_event_check)
    i.nrf_uarte_event_clear                  0x0001e58a   Section        0  nrfx_uarte.o(i.nrf_uarte_event_clear)
    nrf_uarte_event_clear                    0x0001e58b   Thumb Code    12  nrfx_uarte.o(i.nrf_uarte_event_clear)
    i.nrfx_clock_enable                      0x0001e598   Section        0  nrfx_clock.o(i.nrfx_clock_enable)
    i.nrfx_clock_init                        0x0001e5c4   Section        0  nrfx_clock.o(i.nrfx_clock_init)
    i.nrfx_clock_lfclk_stop                  0x0001e5e4   Section        0  nrfx_clock.o(i.nrfx_clock_lfclk_stop)
    i.nrfx_coredep_delay_us                  0x0001e600   Section        0  app_timer.o(i.nrfx_coredep_delay_us)
    nrfx_coredep_delay_us                    0x0001e601   Thumb Code    12  app_timer.o(i.nrfx_coredep_delay_us)
    i.nrfx_gpiote_in_event_enable            0x0001e610   Section        0  nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable)
    i.nrfx_gpiote_in_init                    0x0001e6b4   Section        0  nrfx_gpiote.o(i.nrfx_gpiote_in_init)
    i.nrfx_gpiote_in_is_set                  0x0001e784   Section        0  nrfx_gpiote.o(i.nrfx_gpiote_in_is_set)
    i.nrfx_gpiote_init                       0x0001e798   Section        0  nrfx_gpiote.o(i.nrfx_gpiote_init)
    i.nrfx_gpiote_is_init                    0x0001e804   Section        0  nrfx_gpiote.o(i.nrfx_gpiote_is_init)
    i.nrfx_is_in_ram                         0x0001e818   Section        0  nrfx_uarte.o(i.nrfx_is_in_ram)
    nrfx_is_in_ram                           0x0001e819   Thumb Code    16  nrfx_uarte.o(i.nrfx_is_in_ram)
    i.nrfx_ppi_channel_alloc                 0x0001e828   Section        0  nrfx_ppi.o(i.nrfx_ppi_channel_alloc)
    i.nrfx_ppi_channel_assign                0x0001e894   Section        0  nrfx_ppi.o(i.nrfx_ppi_channel_assign)
    i.nrfx_ppi_channel_enable                0x0001e8d8   Section        0  nrfx_ppi.o(i.nrfx_ppi_channel_enable)
    i.nrfx_prs_acquire                       0x0001e90c   Section        0  nrfx_prs.o(i.nrfx_prs_acquire)
    i.nrfx_saadc_buffer_convert              0x0001e948   Section        0  nrfx_saadc.o(i.nrfx_saadc_buffer_convert)
    i.nrfx_saadc_channel_init                0x0001e9ec   Section        0  nrfx_saadc.o(i.nrfx_saadc_channel_init)
    i.nrfx_saadc_init                        0x0001ea98   Section        0  nrfx_saadc.o(i.nrfx_saadc_init)
    i.nrfx_saadc_sample_task_get             0x0001eb2c   Section        0  nrfx_saadc.o(i.nrfx_saadc_sample_task_get)
    i.nrfx_timer_compare                     0x0001eb48   Section        0  nrfx_timer.o(i.nrfx_timer_compare)
    i.nrfx_timer_enable                      0x0001eb84   Section        0  nrfx_timer.o(i.nrfx_timer_enable)
    i.nrfx_timer_extended_compare            0x0001eba0   Section        0  nrfx_timer.o(i.nrfx_timer_extended_compare)
    i.nrfx_timer_init                        0x0001ebcc   Section        0  nrfx_timer.o(i.nrfx_timer_init)
    i.nrfx_uart_0_irq_handler                0x0001ec88   Section        0  nrfx_uart.o(i.nrfx_uart_0_irq_handler)
    i.nrfx_uart_init                         0x0001ec98   Section        0  nrfx_uart.o(i.nrfx_uart_init)
    i.nrfx_uart_rx                           0x0001ed68   Section        0  nrfx_uart.o(i.nrfx_uart_rx)
    i.nrfx_uart_tx                           0x0001ee54   Section        0  nrfx_uart.o(i.nrfx_uart_tx)
    i.nrfx_uart_tx_in_progress               0x0001eef8   Section        0  nrfx_uart.o(i.nrfx_uart_tx_in_progress)
    i.nrfx_uarte_0_irq_handler               0x0001ef18   Section        0  nrfx_uarte.o(i.nrfx_uarte_0_irq_handler)
    i.nrfx_uarte_init                        0x0001ef28   Section        0  nrfx_uarte.o(i.nrfx_uarte_init)
    i.nrfx_uarte_rx                          0x0001ef94   Section        0  nrfx_uarte.o(i.nrfx_uarte_rx)
    i.nrfx_uarte_tx                          0x0001f098   Section        0  nrfx_uarte.o(i.nrfx_uarte_tx)
    i.nrfx_uarte_tx_in_progress              0x0001f128   Section        0  nrfx_uarte.o(i.nrfx_uarte_tx_in_progress)
    i.nus_data_handler                       0x0001f144   Section        0  main.o(i.nus_data_handler)
    nus_data_handler                         0x0001f145   Thumb Code   198  main.o(i.nus_data_handler)
    i.on_adv_evt                             0x0001f244   Section        0  main.o(i.on_adv_evt)
    on_adv_evt                               0x0001f245   Thumb Code    38  main.o(i.on_adv_evt)
    i.on_conn_params_evt                     0x0001f274   Section        0  main.o(i.on_conn_params_evt)
    on_conn_params_evt                       0x0001f275   Thumb Code    24  main.o(i.on_conn_params_evt)
    i.on_connect                             0x0001f290   Section        0  ble_nus.o(i.on_connect)
    on_connect                               0x0001f291   Thumb Code   106  ble_nus.o(i.on_connect)
    i.on_connected_evt                       0x0001f2fc   Section        0  nrf_ble_gatt.o(i.on_connected_evt)
    on_connected_evt                         0x0001f2fd   Thumb Code    80  nrf_ble_gatt.o(i.on_connected_evt)
    i.on_exchange_mtu_request_evt            0x0001f388   Section        0  nrf_ble_gatt.o(i.on_exchange_mtu_request_evt)
    on_exchange_mtu_request_evt              0x0001f389   Thumb Code   114  nrf_ble_gatt.o(i.on_exchange_mtu_request_evt)
    i.on_write                               0x0001f438   Section        0  ble_nus.o(i.on_write)
    on_write                                 0x0001f439   Thumb Code   132  ble_nus.o(i.on_write)
    i.phy_is_valid                           0x0001f4bc   Section        0  ble_advertising.o(i.phy_is_valid)
    phy_is_valid                             0x0001f4bd   Thumb Code    18  ble_advertising.o(i.phy_is_valid)
    i.pin_in_use_by_port                     0x0001f4d0   Section        0  nrfx_gpiote.o(i.pin_in_use_by_port)
    pin_in_use_by_port                       0x0001f4d1   Thumb Code    20  nrfx_gpiote.o(i.pin_in_use_by_port)
    i.pin_in_use_by_te                       0x0001f4e8   Section        0  nrfx_gpiote.o(i.pin_in_use_by_te)
    pin_in_use_by_te                         0x0001f4e9   Thumb Code    20  nrfx_gpiote.o(i.pin_in_use_by_te)
    i.postfix_process                        0x0001f500   Section        0  nrf_log_str_formatter.o(i.postfix_process)
    postfix_process                          0x0001f501   Thumb Code    48  nrf_log_str_formatter.o(i.postfix_process)
    i.prefix_process                         0x0001f53c   Section        0  nrf_log_str_formatter.o(i.prefix_process)
    prefix_process                           0x0001f53d   Thumb Code    90  nrf_log_str_formatter.o(i.prefix_process)
    i.prs_box_get                            0x0001f5d4   Section        0  nrfx_prs.o(i.prs_box_get)
    prs_box_get                              0x0001f5d5   Thumb Code    14  nrfx_prs.o(i.prs_box_get)
    i.rtc1_stop                              0x0001f5ec   Section        0  app_timer.o(i.rtc1_stop)
    rtc1_stop                                0x0001f5ed   Thumb Code    52  app_timer.o(i.rtc1_stop)
    i.rx_byte                                0x0001f628   Section        0  nrfx_uart.o(i.rx_byte)
    rx_byte                                  0x0001f629   Thumb Code    50  nrfx_uart.o(i.rx_byte)
    i.rx_done_event                          0x0001f65a   Section        0  nrfx_uart.o(i.rx_done_event)
    rx_done_event                            0x0001f65b   Thumb Code    22  nrfx_uart.o(i.rx_done_event)
    i.rx_done_event                          0x0001f670   Section        0  nrfx_uarte.o(i.rx_done_event)
    rx_done_event                            0x0001f671   Thumb Code    22  nrfx_uarte.o(i.rx_done_event)
    i.rx_enable                              0x0001f686   Section        0  nrfx_uart.o(i.rx_enable)
    rx_enable                                0x0001f687   Thumb Code    32  nrfx_uart.o(i.rx_enable)
    i.saadc_callback                         0x0001f6a8   Section        0  main.o(i.saadc_callback)
    i.saadc_init                             0x0001f7c0   Section        0  main.o(i.saadc_init)
    i.saadc_sampling_event_enable            0x0001f82c   Section        0  main.o(i.saadc_sampling_event_enable)
    i.saadc_sampling_event_init              0x0001f848   Section        0  main.o(i.saadc_sampling_event_init)
    i.sd_state_evt_handler                   0x0001f8e0   Section        0  nrf_drv_clock.o(i.sd_state_evt_handler)
    sd_state_evt_handler                     0x0001f8e1   Thumb Code    76  nrf_drv_clock.o(i.sd_state_evt_handler)
    i.sdh_request_observer_notify            0x0001f930   Section        0  nrf_sdh.o(i.sdh_request_observer_notify)
    sdh_request_observer_notify              0x0001f931   Thumb Code    44  nrf_sdh.o(i.sdh_request_observer_notify)
    i.sdh_state_observer_notify              0x0001f960   Section        0  nrf_sdh.o(i.sdh_state_observer_notify)
    sdh_state_observer_notify                0x0001f961   Thumb Code    38  nrf_sdh.o(i.sdh_state_observer_notify)
    i.send_error_evt                         0x0001f98c   Section        0  ble_conn_params.o(i.send_error_evt)
    send_error_evt                           0x0001f98d   Thumb Code    12  ble_conn_params.o(i.send_error_evt)
    i.serial_tx                              0x0001f99c   Section        0  nrf_log_backend_rtt.o(i.serial_tx)
    serial_tx                                0x0001f99d   Thumb Code    70  nrf_log_backend_rtt.o(i.serial_tx)
    i.service_data_encode                    0x0001f9ec   Section        0  ble_advdata.o(i.service_data_encode)
    service_data_encode                      0x0001f9ed   Thumb Code   136  ble_advdata.o(i.service_data_encode)
    i.set_security_req                       0x0001fa74   Section        0  ble_srv_common.o(i.set_security_req)
    set_security_req                         0x0001fa75   Thumb Code    48  ble_srv_common.o(i.set_security_req)
    i.soc_evt_handler                        0x0001faa4   Section        0  nrf_drv_clock.o(i.soc_evt_handler)
    soc_evt_handler                          0x0001faa5   Thumb Code    18  nrf_drv_clock.o(i.soc_evt_handler)
    i.softdevices_evt_irq_enable             0x0001fabc   Section        0  nrf_sdh.o(i.softdevices_evt_irq_enable)
    softdevices_evt_irq_enable               0x0001fabd   Thumb Code    80  nrf_sdh.o(i.softdevices_evt_irq_enable)
    i.std_n                                  0x0001fb14   Section        0  nrf_log_frontend.o(i.std_n)
    std_n                                    0x0001fb15   Thumb Code   136  nrf_log_frontend.o(i.std_n)
    i.timer_handler                          0x0001fba0   Section        0  main.o(i.timer_handler)
    i.timer_list_handler                     0x0001fba4   Section        0  app_timer.o(i.timer_list_handler)
    timer_list_handler                       0x0001fba5   Thumb Code   122  app_timer.o(i.timer_list_handler)
    i.timer_list_insert                      0x0001fc24   Section        0  app_timer.o(i.timer_list_insert)
    timer_list_insert                        0x0001fc25   Thumb Code    56  app_timer.o(i.timer_list_insert)
    i.timer_list_remove                      0x0001fc60   Section        0  app_timer.o(i.timer_list_remove)
    timer_list_remove                        0x0001fc61   Thumb Code    88  app_timer.o(i.timer_list_remove)
    i.timer_stop_op_schedule                 0x0001fcc0   Section        0  app_timer.o(i.timer_stop_op_schedule)
    timer_stop_op_schedule                   0x0001fcc1   Thumb Code    68  app_timer.o(i.timer_stop_op_schedule)
    i.timer_timeouts_check                   0x0001fd08   Section        0  app_timer.o(i.timer_timeouts_check)
    timer_timeouts_check                     0x0001fd09   Thumb Code   106  app_timer.o(i.timer_timeouts_check)
    i.twim_irq_handler                       0x0001fd7c   Section        0  nrfx_twim.o(i.twim_irq_handler)
    twim_irq_handler                         0x0001fd7d   Thumb Code   328  nrfx_twim.o(i.twim_irq_handler)
    i.tx_byte                                0x0001fec8   Section        0  nrfx_uart.o(i.tx_byte)
    tx_byte                                  0x0001fec9   Thumb Code    32  nrfx_uart.o(i.tx_byte)
    i.tx_done_event                          0x0001fee8   Section        0  nrfx_uart.o(i.tx_done_event)
    tx_done_event                            0x0001fee9   Thumb Code    26  nrfx_uart.o(i.tx_done_event)
    i.uart_event_handle                      0x0001ff04   Section        0  main.o(i.uart_event_handle)
    i.uart_event_handler                     0x0001ff7c   Section        0  app_uart_fifo.o(i.uart_event_handler)
    uart_event_handler                       0x0001ff7d   Thumb Code   152  app_uart_fifo.o(i.uart_event_handler)
    i.uart_evt_handler                       0x0002001c   Section        0  nrf_drv_uart.o(i.uart_evt_handler)
    uart_evt_handler                         0x0002001d   Thumb Code    42  nrf_drv_uart.o(i.uart_evt_handler)
    i.uart_irq_handler                       0x0002004c   Section        0  nrfx_uart.o(i.uart_irq_handler)
    uart_irq_handler                         0x0002004d   Thumb Code   296  nrfx_uart.o(i.uart_irq_handler)
    i.uarte_evt_handler                      0x00020174   Section        0  nrf_drv_uart.o(i.uarte_evt_handler)
    uarte_evt_handler                        0x00020175   Thumb Code    42  nrf_drv_uart.o(i.uarte_evt_handler)
    i.uarte_irq_handler                      0x000201a4   Section        0  nrfx_uarte.o(i.uarte_irq_handler)
    uarte_irq_handler                        0x000201a5   Thumb Code   242  nrfx_uarte.o(i.uarte_irq_handler)
    i.uint16_encode                          0x00020296   Section        0  ble_advdata.o(i.uint16_encode)
    uint16_encode                            0x00020297   Thumb Code    10  ble_advdata.o(i.uint16_encode)
    i.unsigned_print                         0x000202a0   Section        0  nrf_fprintf_format.o(i.unsigned_print)
    unsigned_print                           0x000202a1   Thumb Code   176  nrf_fprintf_format.o(i.unsigned_print)
    i.update_timeout_handler                 0x00020354   Section        0  ble_conn_params.o(i.update_timeout_handler)
    update_timeout_handler                   0x00020355   Thumb Code    98  ble_conn_params.o(i.update_timeout_handler)
    i.use_whitelist                          0x000203bc   Section        0  ble_advertising.o(i.use_whitelist)
    use_whitelist                            0x000203bd   Thumb Code    24  ble_advertising.o(i.use_whitelist)
    i.user_mem_reply                         0x000203d4   Section        0  nrf_ble_qwr.o(i.user_mem_reply)
    user_mem_reply                           0x000203d5   Thumb Code    36  nrf_ble_qwr.o(i.user_mem_reply)
    i.user_op_alloc                          0x000203f8   Section        0  app_timer.o(i.user_op_alloc)
    user_op_alloc                            0x000203f9   Thumb Code    42  app_timer.o(i.user_op_alloc)
    i.uuid_list_encode                       0x00020428   Section        0  ble_advdata.o(i.uuid_list_encode)
    uuid_list_encode                         0x00020429   Thumb Code    48  ble_advdata.o(i.uuid_list_encode)
    i.uuid_list_sized_encode                 0x00020458   Section        0  ble_advdata.o(i.uuid_list_sized_encode)
    uuid_list_sized_encode                   0x00020459   Thumb Code   158  ble_advdata.o(i.uuid_list_sized_encode)
    i.wakeup_button_cfg                      0x000204f6   Section        0  bsp.o(i.wakeup_button_cfg)
    wakeup_button_cfg                        0x000204f7   Thumb Code    58  bsp.o(i.wakeup_button_cfg)
    .constdata                               0x00020530   Section       73  main.o(.constdata)
    default_config                           0x00020530   Data           4  main.o(.constdata)
    delay_machine_code                       0x00020540   Data           6  main.o(.constdata)
    m_timer                                  0x00020548   Data           8  main.o(.constdata)
    .constdata                               0x00020579   Section        8  boards.o(.constdata)
    m_board_led_list                         0x00020579   Data           4  boards.o(.constdata)
    m_board_btn_list                         0x0002057d   Data           4  boards.o(.constdata)
    .constdata                               0x00020584   Section       44  bsp.o(.constdata)
    m_bsp_leds_tmr                           0x00020584   Data           4  bsp.o(.constdata)
    m_bsp_alert_tmr                          0x00020588   Data           4  bsp.o(.constdata)
    m_bsp_button_tmr                         0x0002058c   Data           4  bsp.o(.constdata)
    app_buttons                              0x00020590   Data          32  bsp.o(.constdata)
    .constdata                               0x000205b0   Section       14  nrf_ble_gatt.o(.constdata)
    .constdata                               0x000205c0   Section       16  ble_nus.o(.constdata)
    .constdata                               0x000205d0   Section        4  nrfx_gpiote.o(.constdata)
    .constdata                               0x000205d4   Section        4  nrfx_uart.o(.constdata)
    irq_handlers                             0x000205d4   Data           4  nrfx_uart.o(.constdata)
    .constdata                               0x000205d8   Section        4  nrfx_uarte.o(.constdata)
    irq_handlers                             0x000205d8   Data           4  nrfx_uarte.o(.constdata)
    .constdata                               0x000205dc   Section        8  app_button.o(.constdata)
    m_detection_delay_timer_id               0x000205e0   Data           4  app_button.o(.constdata)
    .constdata                               0x000205f0   Section        6  app_timer.o(.constdata)
    delay_machine_code                       0x000205f0   Data           6  app_timer.o(.constdata)
    .constdata                               0x000205f8   Section       32  app_uart_fifo.o(.constdata)
    .constdata                               0x00020618   Section       16  nrf_fprintf_format.o(.constdata)
    _aV2C                                    0x00020618   Data          16  nrf_fprintf_format.o(.constdata)
    .constdata                               0x00020628   Section       24  nrf_pwr_mgmt.o(.constdata)
    pwr_mgmt_data_array                      0x00020628   Data          24  nrf_pwr_mgmt.o(.constdata)
    .constdata                               0x00020640   Section       12  nrf_pwr_mgmt.o(.constdata)
    pwr_mgmt_data                            0x00020640   Data          12  nrf_pwr_mgmt.o(.constdata)
    .constdata                               0x0002064c   Section      316  nrf_strerror.o(.constdata)
    m_unknown_str                            0x0002064c   Data          19  nrf_strerror.o(.constdata)
    nrf_strerror_array                       0x00020660   Data         296  nrf_strerror.o(.constdata)
    .constdata                               0x00020788   Section       12  nrf_log_backend_rtt.o(.constdata)
    .constdata                               0x000207a0   Section        6  nrf_log_backend_rtt.o(.constdata)
    delay_machine_code                       0x000207a0   Data           6  nrf_log_backend_rtt.o(.constdata)
    .constdata                               0x000207a8   Section       12  nrf_log_frontend.o(.constdata)
    m_log_push_ringbuf                       0x000207a8   Data          12  nrf_log_frontend.o(.constdata)
    .constdata                               0x000207b4   Section       16  nrf_sdh.o(.constdata)
    sdh_req_observers_array                  0x000207b4   Data          16  nrf_sdh.o(.constdata)
    .constdata                               0x000207c4   Section       40  nrf_sdh.o(.constdata)
    sdh_req_observers                        0x000207c8   Data          12  nrf_sdh.o(.constdata)
    sdh_state_observers                      0x000207d4   Data          12  nrf_sdh.o(.constdata)
    sdh_stack_observers                      0x000207e0   Data          12  nrf_sdh.o(.constdata)
    .constdata                               0x000207ec   Section       16  nrf_sdh.o(.constdata)
    sdh_state_observers_array                0x000207ec   Data          16  nrf_sdh.o(.constdata)
    .constdata                               0x000207fc   Section       16  nrf_sdh.o(.constdata)
    sdh_stack_observers_array                0x000207fc   Data          16  nrf_sdh.o(.constdata)
    .constdata                               0x0002080c   Section       32  nrf_sdh_ble.o(.constdata)
    sdh_ble_observers_array                  0x0002080c   Data          32  nrf_sdh_ble.o(.constdata)
    .constdata                               0x0002082c   Section       16  nrf_sdh_ble.o(.constdata)
    sdh_ble_observers                        0x00020830   Data          12  nrf_sdh_ble.o(.constdata)
    .constdata                               0x0002083c   Section       16  nrf_sdh_soc.o(.constdata)
    sdh_soc_observers_array                  0x0002083c   Data          16  nrf_sdh_soc.o(.constdata)
    .constdata                               0x0002084c   Section       12  nrf_sdh_soc.o(.constdata)
    sdh_soc_observers                        0x0002084c   Data          12  nrf_sdh_soc.o(.constdata)
    .constdata                               0x00020858   Section      129  ctype_o.o(.constdata)
    .constdata                               0x000208dc   Section        4  ctype_o.o(.constdata)
    table                                    0x000208dc   Data           4  ctype_o.o(.constdata)
    .conststring                             0x000208e0   Section     1003  nrf_strerror.o(.conststring)
    .conststring                             0x00020ccc   Section      102  nrf_log_str_formatter.o(.conststring)
    .conststring                             0x00020d34   Section      463  nrf_sdh_ble.o(.conststring)
    .conststrlit                             0x00020f04   Section       13  nrf_ble_gatt.o(.conststrlit)
    .conststrlit                             0x00020f14   Section        8  ble_nus.o(.conststrlit)
    .conststrlit                             0x00020f1c   Section        6  nrf_drv_clock.o(.conststrlit)
    .conststrlit                             0x00020f24   Section        6  nrfx_clock.o(.conststrlit)
    .conststrlit                             0x00020f2c   Section        7  nrfx_gpiote.o(.conststrlit)
    .conststrlit                             0x00020f34   Section        4  nrfx_prs.o(.conststrlit)
    .conststrlit                             0x00020f38   Section        5  nrfx_uart.o(.conststrlit)
    .conststrlit                             0x00020f40   Section        6  nrfx_uarte.o(.conststrlit)
    .conststrlit                             0x00020f48   Section        4  nrfx_ppi.o(.conststrlit)
    .conststrlit                             0x00020f4c   Section        6  nrfx_saadc.o(.conststrlit)
    .conststrlit                             0x00020f54   Section        6  nrfx_timer.o(.conststrlit)
    .conststrlit                             0x00020f5c   Section        5  nrfx_twim.o(.conststrlit)
    .conststrlit                             0x00020f64   Section        9  nrf_pwr_mgmt.o(.conststrlit)
    .conststrlit                             0x00020f70   Section       16  nrf_log_default_backends.o(.conststrlit)
    .conststrlit                             0x00020f80   Section        4  nrf_log_frontend.o(.conststrlit)
    .conststrlit                             0x00020f84   Section        8  nrf_sdh.o(.conststrlit)
    .conststrlit                             0x00020f8c   Section       12  nrf_sdh_ble.o(.conststrlit)
    .conststrlit                             0x00020f98   Section       12  nrf_sdh_soc.o(.conststrlit)
    log_backends                             0x00020fc4   Section       16  nrf_log_default_backends.o(log_backends)
    __tagsym$$used                           0x00020fc4   Number         0  nrf_log_default_backends.o(log_backends)
    rtt_log_backend                          0x00020fc4   Data          16  nrf_log_default_backends.o(log_backends)
    log_const_data                           0x00020fd4   Section        8  nrf_ble_gatt.o(log_const_data)
    __tagsym$$used                           0x00020fd4   Number         0  nrf_ble_gatt.o(log_const_data)
    log_const_data                           0x00020fdc   Section        8  ble_nus.o(log_const_data)
    __tagsym$$used                           0x00020fdc   Number         0  ble_nus.o(log_const_data)
    log_const_data                           0x00020fe4   Section        8  nrf_drv_clock.o(log_const_data)
    __tagsym$$used                           0x00020fe4   Number         0  nrf_drv_clock.o(log_const_data)
    log_const_data                           0x00020fec   Section        8  nrfx_clock.o(log_const_data)
    __tagsym$$used                           0x00020fec   Number         0  nrfx_clock.o(log_const_data)
    log_const_data                           0x00020ff4   Section        8  nrfx_gpiote.o(log_const_data)
    __tagsym$$used                           0x00020ff4   Number         0  nrfx_gpiote.o(log_const_data)
    log_const_data                           0x00020ffc   Section        8  nrfx_prs.o(log_const_data)
    __tagsym$$used                           0x00020ffc   Number         0  nrfx_prs.o(log_const_data)
    log_const_data                           0x00021004   Section        8  nrfx_uart.o(log_const_data)
    __tagsym$$used                           0x00021004   Number         0  nrfx_uart.o(log_const_data)
    log_const_data                           0x0002100c   Section        8  nrfx_uarte.o(log_const_data)
    __tagsym$$used                           0x0002100c   Number         0  nrfx_uarte.o(log_const_data)
    log_const_data                           0x00021014   Section        8  nrfx_ppi.o(log_const_data)
    __tagsym$$used                           0x00021014   Number         0  nrfx_ppi.o(log_const_data)
    log_const_data                           0x0002101c   Section        8  nrfx_saadc.o(log_const_data)
    __tagsym$$used                           0x0002101c   Number         0  nrfx_saadc.o(log_const_data)
    log_const_data                           0x00021024   Section        8  nrfx_timer.o(log_const_data)
    __tagsym$$used                           0x00021024   Number         0  nrfx_timer.o(log_const_data)
    log_const_data                           0x0002102c   Section        8  nrfx_twim.o(log_const_data)
    __tagsym$$used                           0x0002102c   Number         0  nrfx_twim.o(log_const_data)
    log_const_data                           0x00021034   Section        8  nrf_pwr_mgmt.o(log_const_data)
    __tagsym$$used                           0x00021034   Number         0  nrf_pwr_mgmt.o(log_const_data)
    log_const_data                           0x0002103c   Section        8  nrf_log_frontend.o(log_const_data)
    __tagsym$$used                           0x0002103c   Number         0  nrf_log_frontend.o(log_const_data)
    log_const_data                           0x00021044   Section        8  nrf_sdh.o(log_const_data)
    __tagsym$$used                           0x00021044   Number         0  nrf_sdh.o(log_const_data)
    log_const_data                           0x0002104c   Section        8  nrf_sdh_ble.o(log_const_data)
    __tagsym$$used                           0x0002104c   Number         0  nrf_sdh_ble.o(log_const_data)
    log_const_data                           0x00021054   Section        8  nrf_sdh_soc.o(log_const_data)
    __tagsym$$used                           0x00021054   Number         0  nrf_sdh_soc.o(log_const_data)
    nrf_balloc                               0x0002105c   Section       20  nrf_log_frontend.o(nrf_balloc)
    __tagsym$$used                           0x0002105c   Number         0  nrf_log_frontend.o(nrf_balloc)
    sdh_ble_observers0                       0x00021070   Section        8  ble_conn_state.o(sdh_ble_observers0)
    __tagsym$$used                           0x00021070   Number         0  ble_conn_state.o(sdh_ble_observers0)
    m_ble_evt_observer                       0x00021070   Data           8  ble_conn_state.o(sdh_ble_observers0)
    sdh_ble_observers1                       0x00021078   Section       16  main.o(sdh_ble_observers1)
    __tagsym$$used                           0x00021078   Number         0  main.o(sdh_ble_observers1)
    m_gatt_obs                               0x00021078   Data           8  main.o(sdh_ble_observers1)
    __tagsym$$used                           0x00021080   Number         0  main.o(sdh_ble_observers1)
    m_advertising_ble_obs                    0x00021080   Data           8  main.o(sdh_ble_observers1)
    sdh_ble_observers1                       0x00021088   Section        8  bsp_btn_ble.o(sdh_ble_observers1)
    __tagsym$$used                           0x00021088   Number         0  bsp_btn_ble.o(sdh_ble_observers1)
    m_ble_observer                           0x00021088   Data           8  bsp_btn_ble.o(sdh_ble_observers1)
    sdh_ble_observers1                       0x00021090   Section        8  ble_conn_params.o(sdh_ble_observers1)
    __tagsym$$used                           0x00021090   Number         0  ble_conn_params.o(sdh_ble_observers1)
    m_ble_observer                           0x00021090   Data           8  ble_conn_params.o(sdh_ble_observers1)
    sdh_ble_observers2                       0x00021098   Section       16  main.o(sdh_ble_observers2)
    __tagsym$$used                           0x00021098   Number         0  main.o(sdh_ble_observers2)
    m_nus_obs                                0x00021098   Data           8  main.o(sdh_ble_observers2)
    __tagsym$$used                           0x000210a0   Number         0  main.o(sdh_ble_observers2)
    m_qwr_obs                                0x000210a0   Data           8  main.o(sdh_ble_observers2)
    sdh_ble_observers3                       0x000210a8   Section        8  main.o(sdh_ble_observers3)
    __tagsym$$used                           0x000210a8   Number         0  main.o(sdh_ble_observers3)
    m_ble_observer                           0x000210a8   Data           8  main.o(sdh_ble_observers3)
    sdh_soc_observers0                       0x000210b0   Section        8  nrf_drv_clock.o(sdh_soc_observers0)
    __tagsym$$used                           0x000210b0   Number         0  nrf_drv_clock.o(sdh_soc_observers0)
    m_soc_evt_observer                       0x000210b0   Data           8  nrf_drv_clock.o(sdh_soc_observers0)
    sdh_soc_observers1                       0x000210b8   Section        8  main.o(sdh_soc_observers1)
    __tagsym$$used                           0x000210b8   Number         0  main.o(sdh_soc_observers1)
    m_advertising_soc_obs                    0x000210b8   Data           8  main.o(sdh_soc_observers1)
    sdh_stack_observers0                     0x000210c0   Section        8  nrf_sdh_ble.o(sdh_stack_observers0)
    __tagsym$$used                           0x000210c0   Number         0  nrf_sdh_ble.o(sdh_stack_observers0)
    m_nrf_sdh_ble_evts_poll                  0x000210c0   Data           8  nrf_sdh_ble.o(sdh_stack_observers0)
    sdh_stack_observers0                     0x000210c8   Section        8  nrf_sdh_soc.o(sdh_stack_observers0)
    __tagsym$$used                           0x000210c8   Number         0  nrf_sdh_soc.o(sdh_stack_observers0)
    m_nrf_sdh_soc_evts_poll                  0x000210c8   Data           8  nrf_sdh_soc.o(sdh_stack_observers0)
    sdh_state_observers0                     0x000210d0   Section        8  nrf_drv_clock.o(sdh_state_observers0)
    __tagsym$$used                           0x000210d0   Number         0  nrf_drv_clock.o(sdh_state_observers0)
    m_sd_state_observer                      0x000210d0   Data           8  nrf_drv_clock.o(sdh_state_observers0)
    .data                                    0x20002500   Section       52  main.o(.data)
    pressure_counter                         0x20002501   Data           1  main.o(.data)
    index                                    0x20002502   Data           1  main.o(.data)
    m_ppi_channel                            0x20002503   Data           1  main.o(.data)
    m_conn_handle                            0x20002504   Data           2  main.o(.data)
    m_ble_nus_max_data_len                   0x20002506   Data           2  main.o(.data)
    m_adv_uuids                              0x20002508   Data           4  main.o(.data)
    max_pressure_value                       0x2000250c   Data           4  main.o(.data)
    m_buffer_pool                            0x20002510   Data           4  main.o(.data)
    m_adc_evt_counter                        0x20002514   Data           4  main.o(.data)
    m_nus                                    0x20002518   Data          28  main.o(.data)
    .data                                    0x20002534   Section        8  main.o(.data)
    m_nus_link_ctx_storage                   0x20002534   Data           8  main.o(.data)
    .data                                    0x2000253c   Section        4  main.o(.data)
    m_nus_link_ctx_storage_ctx_data_pool     0x2000253c   Data           4  main.o(.data)
    .data                                    0x20002540   Section       16  bsp.o(.data)
    m_stable_state                           0x20002540   Data           1  bsp.o(.data)
    m_leds_clear                             0x20002541   Data           1  bsp.o(.data)
    m_alert_on                               0x20002542   Data           1  bsp.o(.data)
    current_long_push_pin_no                 0x20002543   Data           1  bsp.o(.data)
    m_indication_type                        0x20002544   Data           4  bsp.o(.data)
    m_registered_callback                    0x20002548   Data           4  bsp.o(.data)
    release_event_at_push                    0x2000254c   Data           4  bsp.o(.data)
    .data                                    0x20002550   Section        8  bsp_btn_ble.o(.data)
    m_error_handler                          0x20002550   Data           4  bsp_btn_ble.o(.data)
    m_num_connections                        0x20002554   Data           4  bsp_btn_ble.o(.data)
    .data                                    0x20002558   Section        8  ble_conn_params.o(.data)
    m_preferred_conn_params                  0x20002558   Data           8  ble_conn_params.o(.data)
    .data                                    0x20002560   Section       12  nrf_drv_uart.o(.data)
    m_handlers                               0x20002564   Data           4  nrf_drv_uart.o(.data)
    m_contexts                               0x20002568   Data           4  nrf_drv_uart.o(.data)
    .data                                    0x2000256c   Section        8  nrfx_clock.o(.data)
    m_clock_cb                               0x2000256c   Data           8  nrfx_clock.o(.data)
    .data                                    0x20002574   Section        8  nrfx_prs.o(.data)
    m_prs_box_4                              0x20002574   Data           8  nrfx_prs.o(.data)
    .data                                    0x2000257c   Section        1  nrf_drv_ppi.o(.data)
    m_drv_state                              0x2000257c   Data           1  nrf_drv_ppi.o(.data)
    .data                                    0x20002580   Section        8  nrfx_ppi.o(.data)
    m_groups_allocated                       0x20002580   Data           1  nrfx_ppi.o(.data)
    m_channels_allocated                     0x20002584   Data           4  nrfx_ppi.o(.data)
    .data                                    0x20002588   Section       32  app_button.o(.data)
    m_button_count                           0x20002588   Data           1  app_button.o(.data)
    mp_buttons                               0x2000258c   Data           4  app_button.o(.data)
    m_detection_delay                        0x20002590   Data           4  app_button.o(.data)
    m_pin_state                              0x20002598   Data           8  app_button.o(.data)
    m_pin_transition                         0x200025a0   Data           8  app_button.o(.data)
    .data                                    0x200025a8   Section       20  app_timer.o(.data)
    m_ticks_elapsed_q_read_ind               0x200025a8   Data           1  app_timer.o(.data)
    m_ticks_elapsed_q_write_ind              0x200025a9   Data           1  app_timer.o(.data)
    m_rtc1_running                           0x200025aa   Data           1  app_timer.o(.data)
    m_rtc1_reset                             0x200025ab   Data           1  app_timer.o(.data)
    mp_timer_id_head                         0x200025ac   Data           4  app_timer.o(.data)
    m_ticks_latest                           0x200025b0   Data           4  app_timer.o(.data)
    m_ticks_elapsed                          0x200025b4   Data           8  app_timer.o(.data)
    .data                                    0x200025bc   Section       28  app_uart_fifo.o(.data)
    tx_buffer                                0x200025bc   Data           1  app_uart_fifo.o(.data)
    rx_buffer                                0x200025bd   Data           1  app_uart_fifo.o(.data)
    m_rx_ovf                                 0x200025be   Data           1  app_uart_fifo.o(.data)
    m_event_handler                          0x200025c0   Data           4  app_uart_fifo.o(.data)
    app_uart_inst                            0x200025c4   Data          20  app_uart_fifo.o(.data)
    .data                                    0x200025d8   Section        8  nrf_pwr_mgmt.o(.data)
    m_pwr_mgmt_evt                           0x200025d8   Data           1  nrf_pwr_mgmt.o(.data)
    m_shutdown_started                       0x200025d9   Data           1  nrf_pwr_mgmt.o(.data)
    m_sysoff_mtx                             0x200025dc   Data           4  nrf_pwr_mgmt.o(.data)
    .data                                    0x200025e0   Section        4  retarget.o(.data)
    .data                                    0x200025e4   Section        1  nrf_log_backend_rtt.o(.data)
    m_host_present                           0x200025e4   Data           1  nrf_log_backend_rtt.o(.data)
    .data                                    0x200025e8   Section        8  nrf_log_default_backends.o(.data)
    log_backend_cb_rtt_log_backend           0x200025e8   Data           8  nrf_log_default_backends.o(.data)
    .data                                    0x200025f0   Section        8  nrf_log_frontend.o(.data)
    log_mempool_nrf_balloc_pool_stack        0x200025f0   Data           8  nrf_log_frontend.o(.data)
    .data                                    0x200025f8   Section        8  nrf_log_frontend.o(.data)
    log_mempool_nrf_balloc_cb                0x200025f8   Data           8  nrf_log_frontend.o(.data)
    .data                                    0x20002600   Section       64  nrf_log_str_formatter.o(.data)
    m_freq                                   0x20002600   Data           4  nrf_log_str_formatter.o(.data)
    m_timestamp_div                          0x20002604   Data           4  nrf_log_str_formatter.o(.data)
    severity_names                           0x20002608   Data          20  nrf_log_str_formatter.o(.data)
    m_colors                                 0x2000261c   Data          36  nrf_log_str_formatter.o(.data)
    .data                                    0x20002640   Section        3  nrf_sdh.o(.data)
    m_nrf_sdh_enabled                        0x20002640   Data           1  nrf_sdh.o(.data)
    m_nrf_sdh_suspended                      0x20002641   Data           1  nrf_sdh.o(.data)
    m_nrf_sdh_continue                       0x20002642   Data           1  nrf_sdh.o(.data)
    .data                                    0x20002643   Section        1  nrf_sdh_ble.o(.data)
    m_stack_is_enabled                       0x20002643   Data           1  nrf_sdh_ble.o(.data)
    .data                                    0x20002644   Section        4  system_nrf52.o(.data)
    __tagsym$$used                           0x20002644   Number         0  system_nrf52.o(.data)
    .bss                                     0x20002648   Section      989  main.o(.bss)
    data_array                               0x20002648   Data         244  main.o(.bss)
    rx_buf                                   0x2000273c   Data         256  main.o(.bss)
    tx_buf                                   0x2000283c   Data         256  main.o(.bss)
    m_gatt                                   0x2000293c   Data          16  main.o(.bss)
    m_qwr                                    0x2000294c   Data          12  main.o(.bss)
    m_advertising                            0x20002958   Data         184  main.o(.bss)
    .bss                                     0x20002a28   Section       32  bsp.o(.bss)
    m_bsp_leds_tmr_data                      0x20002a28   Data          32  bsp.o(.bss)
    .bss                                     0x20002a48   Section       32  bsp.o(.bss)
    m_bsp_alert_tmr_data                     0x20002a48   Data          32  bsp.o(.bss)
    .bss                                     0x20002a68   Section       12  bsp.o(.bss)
    m_events_list                            0x20002a68   Data          12  bsp.o(.bss)
    .bss                                     0x20002a74   Section       32  bsp.o(.bss)
    m_bsp_button_tmr_data                    0x20002a74   Data          32  bsp.o(.bss)
    .bss                                     0x20002a94   Section       80  ble_conn_params.o(.bss)
    m_timer_data                             0x20002a94   Data          32  ble_conn_params.o(.bss)
    m_conn_params_instances                  0x20002ab4   Data          20  ble_conn_params.o(.bss)
    m_conn_params_config                     0x20002ac8   Data          28  ble_conn_params.o(.bss)
    .bss                                     0x20002ae4   Section      120  ble_conn_state.o(.bss)
    m_bcs                                    0x20002ae4   Data         120  ble_conn_state.o(.bss)
    .bss                                     0x20002b5c   Section       20  nrf_drv_clock.o(.bss)
    m_clock_cb                               0x20002b5c   Data          20  nrf_drv_clock.o(.bss)
    .bss                                     0x20002b70   Section       92  nrfx_gpiote.o(.bss)
    m_cb                                     0x20002b70   Data          92  nrfx_gpiote.o(.bss)
    .bss                                     0x20002bcc   Section       44  nrfx_uart.o(.bss)
    m_cb                                     0x20002bcc   Data          44  nrfx_uart.o(.bss)
    .bss                                     0x20002bf8   Section       36  nrfx_uarte.o(.bss)
    m_cb                                     0x20002bf8   Data          36  nrfx_uarte.o(.bss)
    .bss                                     0x20002c1c   Section       48  nrfx_saadc.o(.bss)
    m_cb                                     0x20002c1c   Data          48  nrfx_saadc.o(.bss)
    .bss                                     0x20002c4c   Section       12  nrfx_timer.o(.bss)
    m_cb                                     0x20002c4c   Data          12  nrfx_timer.o(.bss)
    .bss                                     0x20002c58   Section       52  nrfx_twim.o(.bss)
    m_cb                                     0x20002c58   Data          52  nrfx_twim.o(.bss)
    .bss                                     0x20002c8c   Section       32  app_button.o(.bss)
    m_detection_delay_timer_id_data          0x20002c8c   Data          32  app_button.o(.bss)
    .bss                                     0x20002cac   Section      268  app_timer.o(.bss)
    m_op_queue                               0x20002cac   Data         268  app_timer.o(.bss)
    .bss                                     0x20002db8   Section       32  app_uart_fifo.o(.bss)
    m_rx_fifo                                0x20002db8   Data          16  app_uart_fifo.o(.bss)
    m_tx_fifo                                0x20002dc8   Data          16  app_uart_fifo.o(.bss)
    .bss                                     0x20002dd8   Section       12  app_util_platform.o(.bss)
    .bss                                     0x20002de4   Section       12  nrf_pwr_mgmt.o(.bss)
    m_handlers_iter                          0x20002de4   Data          12  nrf_pwr_mgmt.o(.bss)
    .bss                                     0x20002df0   Section       64  nrf_log_backend_rtt.o(.bss)
    m_string_buff                            0x20002df0   Data          64  nrf_log_backend_rtt.o(.bss)
    .bss                                     0x20002e30   Section      192  nrf_log_frontend.o(.bss)
    log_mempool_nrf_balloc_pool_mem          0x20002e30   Data         192  nrf_log_frontend.o(.bss)
    .bss                                     0x20002ef0   Section      128  nrf_log_frontend.o(.bss)
    m_log_push_ringbuf_buf                   0x20002ef0   Data         128  nrf_log_frontend.o(.bss)
    .bss                                     0x20002f70   Section       24  nrf_log_frontend.o(.bss)
    m_log_push_ringbuf_cb                    0x20002f70   Data          24  nrf_log_frontend.o(.bss)
    .bss                                     0x20002f88   Section     1060  nrf_log_frontend.o(.bss)
    m_log_data                               0x20002f88   Data        1060  nrf_log_frontend.o(.bss)
    .bss                                     0x200033ac   Section      648  segger_rtt.o(.bss)
    _acUpBuffer                              0x20003424   Data         512  segger_rtt.o(.bss)
    _acDownBuffer                            0x20003624   Data          16  segger_rtt.o(.bss)
    STACK                                    0x20003638   Section     2048  arm_startup_nrf52.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv4$E$P$D$K$B$S$7EM$VFPi3$EXTD16$VFPS$VFMA$PE$A:L22UL41UL21$X:L11$S22US41US21$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OSPACE$ROPI$EBA8$MICROLIB$REQ8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    log_dynamic_data$$Base                    - Undefined Reference
    pwr_mgmt_data0$$Base                      - Undefined Reference
    pwr_mgmt_data0$$Limit                     - Undefined Reference
    pwr_mgmt_data1$$Base                      - Undefined Reference
    pwr_mgmt_data1$$Limit                     - Undefined Reference
    pwr_mgmt_data2$$Base                      - Undefined Reference
    pwr_mgmt_data2$$Limit                     - Undefined Reference
    sdh_req_observers0$$Base                  - Undefined Reference
    sdh_req_observers0$$Limit                 - Undefined Reference
    sdh_req_observers1$$Base                  - Undefined Reference
    sdh_req_observers1$$Limit                 - Undefined Reference
    sdh_stack_observers1$$Base                - Undefined Reference
    sdh_stack_observers1$$Limit               - Undefined Reference
    sdh_state_observers1$$Base                - Undefined Reference
    sdh_state_observers1$$Limit               - Undefined Reference
    __Vectors_Size                           0x00000200   Number         0  arm_startup_nrf52.o ABSOLUTE
    __Vectors                                0x00019000   Data           4  arm_startup_nrf52.o(RESET)
    __Vectors_End                            0x00019200   Data           0  arm_startup_nrf52.o(RESET)
    __main                                   0x00019201   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x00019201   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x00019205   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x00019209   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x00019209   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x00019209   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x00019209   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x00019211   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x00019211   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_mov 0x00019215   Thumb Code    24  nrf_atomic.o(.emb_text)
    __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_orr 0x0001922d   Thumb Code    26  nrf_atomic.o(.emb_text)
    __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_and 0x00019247   Thumb Code    26  nrf_atomic.o(.emb_text)
    __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_eor 0x00019261   Thumb Code    26  nrf_atomic.o(.emb_text)
    __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_add 0x0001927b   Thumb Code    26  nrf_atomic.o(.emb_text)
    __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_sub 0x00019295   Thumb Code    26  nrf_atomic.o(.emb_text)
    __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_cmp_exch 0x000192af   Thumb Code    42  nrf_atomic.o(.emb_text)
    __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_sub_hs 0x000192d9   Thumb Code    30  nrf_atomic.o(.emb_text)
    Reset_Handler                            0x000192f9   Thumb Code     8  arm_startup_nrf52.o(.text)
    NMI_Handler                              0x00019301   Thumb Code     2  arm_startup_nrf52.o(.text)
    HardFault_Handler                        0x00019303   Thumb Code     2  arm_startup_nrf52.o(.text)
    MemoryManagement_Handler                 0x00019305   Thumb Code     2  arm_startup_nrf52.o(.text)
    BusFault_Handler                         0x00019307   Thumb Code     2  arm_startup_nrf52.o(.text)
    UsageFault_Handler                       0x00019309   Thumb Code     2  arm_startup_nrf52.o(.text)
    SVC_Handler                              0x0001930b   Thumb Code     2  arm_startup_nrf52.o(.text)
    DebugMon_Handler                         0x0001930d   Thumb Code     2  arm_startup_nrf52.o(.text)
    PendSV_Handler                           0x0001930f   Thumb Code     2  arm_startup_nrf52.o(.text)
    SysTick_Handler                          0x00019311   Thumb Code     2  arm_startup_nrf52.o(.text)
    CCM_AAR_IRQHandler                       0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    COMP_LPCOMP_IRQHandler                   0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    ECB_IRQHandler                           0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    FPU_IRQHandler                           0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    I2S_IRQHandler                           0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    MWU_IRQHandler                           0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    NFCT_IRQHandler                          0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    PDM_IRQHandler                           0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    PWM0_IRQHandler                          0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    PWM1_IRQHandler                          0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    PWM2_IRQHandler                          0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    QDEC_IRQHandler                          0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    RADIO_IRQHandler                         0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    RNG_IRQHandler                           0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    RTC0_IRQHandler                          0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    RTC2_IRQHandler                          0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    SPIM1_SPIS1_TWIM1_TWIS1_SPI1_TWI1_IRQHandler 0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    SPIM2_SPIS2_SPI2_IRQHandler              0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    SWI1_EGU1_IRQHandler                     0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    SWI3_EGU3_IRQHandler                     0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    SWI4_EGU4_IRQHandler                     0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    SWI5_EGU5_IRQHandler                     0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    TEMP_IRQHandler                          0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    TIMER1_IRQHandler                        0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    TIMER2_IRQHandler                        0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    TIMER3_IRQHandler                        0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    TIMER4_IRQHandler                        0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    WDT_IRQHandler                           0x00019313   Thumb Code     0  arm_startup_nrf52.o(.text)
    __aeabi_uldivmod                         0x0001931d   Thumb Code    98  uldiv.o(.text)
    __aeabi_llsl                             0x0001937f   Thumb Code    30  llshl.o(.text)
    _ll_shift_l                              0x0001937f   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x0001939d   Thumb Code    32  llushr.o(.text)
    _ll_ushift_r                             0x0001939d   Thumb Code     0  llushr.o(.text)
    __rt_ctype_table                         0x000193bd   Thumb Code     4  ctype_o.o(.text)
    __aeabi_memcpy                           0x000193c5   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x000193c5   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x000193c5   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x000193e9   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x000193e9   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x000193e9   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x000193f7   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x000193f7   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x000193f7   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x000193fb   Thumb Code    18  memseta.o(.text)
    strcat                                   0x0001940d   Thumb Code    24  strcat.o(.text)
    strlen                                   0x00019425   Thumb Code    14  strlen.o(.text)
    strcpy                                   0x00019433   Thumb Code    18  strcpy.o(.text)
    __aeabi_f2d                              0x00019445   Thumb Code    38  f2d.o(.text)
    __aeabi_uidiv                            0x0001946b   Thumb Code     0  uidiv.o(.text)
    __aeabi_uidivmod                         0x0001946b   Thumb Code    44  uidiv.o(.text)
    __I$use$fp                               0x00019497   Thumb Code     0  iusefp.o(.text)
    __aeabi_dadd                             0x00019497   Thumb Code   322  dadd.o(.text)
    __aeabi_dsub                             0x000195d9   Thumb Code     6  dadd.o(.text)
    __aeabi_drsub                            0x000195df   Thumb Code     6  dadd.o(.text)
    __aeabi_dmul                             0x000195e5   Thumb Code   228  dmul.o(.text)
    __aeabi_ddiv                             0x000196c9   Thumb Code   222  ddiv.o(.text)
    __aeabi_d2ulz                            0x000197a7   Thumb Code    48  dfixul.o(.text)
    __aeabi_cdrcmple                         0x000197d9   Thumb Code    48  cdrcmple.o(.text)
    __scatterload                            0x00019809   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x00019809   Thumb Code     0  init.o(.text)
    __aeabi_lasr                             0x0001982d   Thumb Code    36  llsshr.o(.text)
    _ll_sshift_r                             0x0001982d   Thumb Code     0  llsshr.o(.text)
    _double_round                            0x00019851   Thumb Code    30  depilogue.o(.text)
    _double_epilogue                         0x0001986f   Thumb Code   156  depilogue.o(.text)
    __decompress                             0x0001990b   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x0001990b   Thumb Code    86  __dczerorl2.o(.text)
    GPIOTE_IRQHandler                        0x00019961   Thumb Code   346  nrfx_gpiote.o(i.GPIOTE_IRQHandler)
    POWER_CLOCK_IRQHandler                   0x00019b29   Thumb Code    82  nrfx_clock.o(i.POWER_CLOCK_IRQHandler)
    RTC1_IRQHandler                          0x00019b81   Thumb Code    32  app_timer.o(i.RTC1_IRQHandler)
    SAADC_IRQHandler                         0x00019ba5   Thumb Code   320  nrfx_saadc.o(i.SAADC_IRQHandler)
    SEGGER_RTT_Init                          0x00019ced   Thumb Code     4  segger_rtt.o(i.SEGGER_RTT_Init)
    SEGGER_RTT_WriteNoLock                   0x00019cf1   Thumb Code    86  segger_rtt.o(i.SEGGER_RTT_WriteNoLock)
    SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler 0x00019d4d   Thumb Code     8  nrfx_twim.o(i.SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler)
    SWI0_EGU0_IRQHandler                     0x00019d5d   Thumb Code     4  app_timer.o(i.SWI0_EGU0_IRQHandler)
    SWI2_EGU2_IRQHandler                     0x00019d61   Thumb Code     4  nrf_sdh.o(i.SWI2_EGU2_IRQHandler)
    SystemInit                               0x00019d65   Thumb Code   726  system_nrf52.o(i.SystemInit)
    TIMER0_IRQHandler                        0x0001a081   Thumb Code    70  nrfx_timer.o(i.TIMER0_IRQHandler)
    UARTE0_UART0_IRQHandler                  0x0001a0d1   Thumb Code     6  nrfx_prs.o(i.UARTE0_UART0_IRQHandler)
    __0printf                                0x0001a1f9   Thumb Code    22  printfa.o(i.__0printf)
    __1printf                                0x0001a1f9   Thumb Code     0  printfa.o(i.__0printf)
    __2printf                                0x0001a1f9   Thumb Code     0  printfa.o(i.__0printf)
    __c89printf                              0x0001a1f9   Thumb Code     0  printfa.o(i.__0printf)
    printf                                   0x0001a1f9   Thumb Code     0  printfa.o(i.__0printf)
    __0sprintf                               0x0001a219   Thumb Code    34  printfa.o(i.__0sprintf)
    __1sprintf                               0x0001a219   Thumb Code     0  printfa.o(i.__0sprintf)
    __2sprintf                               0x0001a219   Thumb Code     0  printfa.o(i.__0sprintf)
    __c89sprintf                             0x0001a219   Thumb Code     0  printfa.o(i.__0sprintf)
    sprintf                                  0x0001a219   Thumb Code     0  printfa.o(i.__0sprintf)
    __scatterload_copy                       0x0001a241   Thumb Code    14  handlers.o(i.__scatterload_copy)
    __scatterload_null                       0x0001a24f   Thumb Code     2  handlers.o(i.__scatterload_null)
    __scatterload_zeroinit                   0x0001a251   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    app_button_enable                        0x0001ab7d   Thumb Code    32  app_button.o(i.app_button_enable)
    app_button_init                          0x0001aba1   Thumb Code   102  app_button.o(i.app_button_init)
    app_error_fault_handler                  0x0001ac19   Thumb Code    86  app_error_weak.o(i.app_error_fault_handler)
    app_error_handler_bare                   0x0001ac9d   Thumb Code    22  app_error.o(i.app_error_handler_bare)
    app_fifo_get                             0x0001acb3   Thumb Code    22  app_fifo.o(i.app_fifo_get)
    app_fifo_init                            0x0001acc9   Thumb Code    32  app_fifo.o(i.app_fifo_init)
    app_fifo_put                             0x0001ace9   Thumb Code    26  app_fifo.o(i.app_fifo_put)
    app_timer_create                         0x0001ad05   Thumb Code    36  app_timer.o(i.app_timer_create)
    app_timer_init                           0x0001ad2d   Thumb Code    70  app_timer.o(i.app_timer_init)
    app_timer_start                          0x0001ad81   Thumb Code   128  app_timer.o(i.app_timer_start)
    app_timer_stop                           0x0001ae09   Thumb Code    26  app_timer.o(i.app_timer_stop)
    app_uart_get                             0x0001ae29   Thumb Code    42  app_uart_fifo.o(i.app_uart_get)
    app_uart_init                            0x0001ae5d   Thumb Code   148  app_uart_fifo.o(i.app_uart_init)
    app_uart_put                             0x0001af01   Thumb Code    70  app_uart_fifo.o(i.app_uart_put)
    app_util_critical_region_enter           0x0001af55   Thumb Code    64  app_util_platform.o(i.app_util_critical_region_enter)
    app_util_critical_region_exit            0x0001af9d   Thumb Code    46  app_util_platform.o(i.app_util_critical_region_exit)
    blcm_link_ctx_get                        0x0001b0ed   Thumb Code    72  ble_link_ctx_manager.o(i.blcm_link_ctx_get)
    ble_advdata_encode                       0x0001b135   Thumb Code   386  ble_advdata.o(i.ble_advdata_encode)
    ble_advdata_parse                        0x0001b2b7   Thumb Code    32  ble_advdata.o(i.ble_advdata_parse)
    ble_advdata_search                       0x0001b2d7   Thumb Code    56  ble_advdata.o(i.ble_advdata_search)
    ble_advertising_conn_cfg_tag_set         0x0001b30f   Thumb Code     6  ble_advertising.o(i.ble_advertising_conn_cfg_tag_set)
    ble_advertising_init                     0x0001b315   Thumb Code   234  ble_advertising.o(i.ble_advertising_init)
    ble_advertising_on_ble_evt               0x0001b3ff   Thumb Code   106  ble_advertising.o(i.ble_advertising_on_ble_evt)
    ble_advertising_on_sys_evt               0x0001b469   Thumb Code     2  ble_advertising.o(i.ble_advertising_on_sys_evt)
    ble_advertising_restart_without_whitelist 0x0001b46b   Thumb Code    58  ble_advertising.o(i.ble_advertising_restart_without_whitelist)
    ble_advertising_start                    0x0001b4a5   Thumb Code   514  ble_advertising.o(i.ble_advertising_start)
    ble_conn_params_init                     0x0001b6a9   Thumb Code    90  ble_conn_params.o(i.ble_conn_params_init)
    ble_conn_state_conn_idx                  0x0001b711   Thumb Code    18  ble_conn_state.o(i.ble_conn_state_conn_idx)
    ble_conn_state_valid                     0x0001b725   Thumb Code    16  ble_conn_state.o(i.ble_conn_state_valid)
    ble_nus_data_send                        0x0001bae1   Thumb Code   102  ble_nus.o(i.ble_nus_data_send)
    ble_nus_init                             0x0001bb49   Thumb Code   206  ble_nus.o(i.ble_nus_init)
    ble_nus_on_ble_evt                       0x0001bc1d   Thumb Code   112  ble_nus.o(i.ble_nus_on_ble_evt)
    ble_srv_is_notification_enabled          0x0001bc8d   Thumb Code     8  ble_srv_common.o(i.ble_srv_is_notification_enabled)
    bsp_board_button_idx_to_pin              0x0001bc95   Thumb Code     6  boards.o(i.bsp_board_button_idx_to_pin)
    bsp_board_button_state_get               0x0001bca1   Thumb Code    28  boards.o(i.bsp_board_button_state_get)
    bsp_board_init                           0x0001bcc1   Thumb Code    80  boards.o(i.bsp_board_init)
    bsp_board_led_invert                     0x0001bd15   Thumb Code    32  boards.o(i.bsp_board_led_invert)
    bsp_board_led_off                        0x0001bd39   Thumb Code    10  boards.o(i.bsp_board_led_off)
    bsp_board_led_on                         0x0001bd49   Thumb Code    10  boards.o(i.bsp_board_led_on)
    bsp_board_led_state_get                  0x0001bd59   Thumb Code    28  boards.o(i.bsp_board_led_state_get)
    bsp_board_leds_off                       0x0001bd79   Thumb Code    18  boards.o(i.bsp_board_leds_off)
    bsp_board_leds_on                        0x0001bd8b   Thumb Code    18  boards.o(i.bsp_board_leds_on)
    bsp_board_pin_to_button_idx              0x0001bd9d   Thumb Code    30  boards.o(i.bsp_board_pin_to_button_idx)
    bsp_btn_ble_init                         0x0001bdc1   Thumb Code    52  bsp_btn_ble.o(i.bsp_btn_ble_init)
    bsp_btn_ble_sleep_mode_prepare           0x0001bdf9   Thumb Code    30  bsp_btn_ble.o(i.bsp_btn_ble_sleep_mode_prepare)
    bsp_button_is_pressed                    0x0001bea9   Thumb Code    12  bsp.o(i.bsp_button_is_pressed)
    bsp_event_handler                        0x0001beb5   Thumb Code    84  main.o(i.bsp_event_handler)
    bsp_event_to_button_action_assign        0x0001bf11   Thumb Code    64  bsp.o(i.bsp_event_to_button_action_assign)
    bsp_indication_set                       0x0001bf55   Thumb Code    20  bsp.o(i.bsp_indication_set)
    bsp_init                                 0x0001bf6d   Thumb Code   128  bsp.o(i.bsp_init)
    bsp_wakeup_button_enable                 0x0001c1c9   Thumb Code     6  bsp.o(i.bsp_wakeup_button_enable)
    buffer_is_empty                          0x0001c291   Thumb Code    16  nrf_log_frontend.o(i.buffer_is_empty)
    characteristic_add                       0x0001c321   Thumb Code   400  ble_srv_common.o(i.characteristic_add)
    conn_handle_list_get                     0x0001c5a1   Thumb Code    62  ble_conn_state.o(i.conn_handle_list_get)
    fputc                                    0x0001c7f3   Thumb Code    14  retarget.o(i.fputc)
    gatt_evt_handler                         0x0001c801   Thumb Code    52  main.o(i.gatt_evt_handler)
    gatt_init                                0x0001c85d   Thumb Code    38  main.o(i.gatt_init)
    main                                     0x0001ccd5   Thumb Code   502  main.o(i.main)
    nrf_atflags_clear                        0x0001d12f   Thumb Code    22  nrf_atflags.o(i.nrf_atflags_clear)
    nrf_atflags_get                          0x0001d145   Thumb Code    22  nrf_atflags.o(i.nrf_atflags_get)
    nrf_atflags_set                          0x0001d15b   Thumb Code    20  nrf_atflags.o(i.nrf_atflags_set)
    nrf_atomic_flag_clear_fetch              0x0001d16f   Thumb Code     6  nrf_atomic.o(i.nrf_atomic_flag_clear_fetch)
    nrf_atomic_flag_set                      0x0001d175   Thumb Code     6  nrf_atomic.o(i.nrf_atomic_flag_set)
    nrf_atomic_u32_add                       0x0001d17b   Thumb Code    12  nrf_atomic.o(i.nrf_atomic_u32_add)
    nrf_atomic_u32_and                       0x0001d187   Thumb Code    12  nrf_atomic.o(i.nrf_atomic_u32_and)
    nrf_atomic_u32_fetch_and                 0x0001d193   Thumb Code    10  nrf_atomic.o(i.nrf_atomic_u32_fetch_and)
    nrf_atomic_u32_fetch_store               0x0001d19d   Thumb Code    10  nrf_atomic.o(i.nrf_atomic_u32_fetch_store)
    nrf_atomic_u32_or                        0x0001d1a7   Thumb Code    12  nrf_atomic.o(i.nrf_atomic_u32_or)
    nrf_atomic_u32_sub                       0x0001d1b3   Thumb Code    12  nrf_atomic.o(i.nrf_atomic_u32_sub)
    nrf_balloc_alloc                         0x0001d1bf   Thumb Code    68  nrf_balloc.o(i.nrf_balloc_alloc)
    nrf_balloc_free                          0x0001d203   Thumb Code    48  nrf_balloc.o(i.nrf_balloc_free)
    nrf_balloc_init                          0x0001d233   Thumb Code    48  nrf_balloc.o(i.nrf_balloc_init)
    nrf_ble_gatt_att_mtu_periph_set          0x0001d287   Thumb Code    24  nrf_ble_gatt.o(i.nrf_ble_gatt_att_mtu_periph_set)
    nrf_ble_gatt_init                        0x0001d29f   Thumb Code    34  nrf_ble_gatt.o(i.nrf_ble_gatt_init)
    nrf_ble_gatt_on_ble_evt                  0x0001d2c1   Thumb Code   180  nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt)
    nrf_ble_qwr_conn_handle_assign           0x0001d3b5   Thumb Code    22  nrf_ble_qwr.o(i.nrf_ble_qwr_conn_handle_assign)
    nrf_ble_qwr_init                         0x0001d3cb   Thumb Code    36  nrf_ble_qwr.o(i.nrf_ble_qwr_init)
    nrf_ble_qwr_on_ble_evt                   0x0001d3ef   Thumb Code   182  nrf_ble_qwr.o(i.nrf_ble_qwr_on_ble_evt)
    nrf_drv_clock_init                       0x0001d4c5   Thumb Code    48  nrf_drv_clock.o(i.nrf_drv_clock_init)
    nrf_drv_clock_lfclk_release              0x0001d4fd   Thumb Code    42  nrf_drv_clock.o(i.nrf_drv_clock_lfclk_release)
    nrf_drv_ppi_init                         0x0001d52d   Thumb Code    18  nrf_drv_ppi.o(i.nrf_drv_ppi_init)
    nrf_drv_uart_init                        0x0001d545   Thumb Code    90  nrf_drv_uart.o(i.nrf_drv_uart_init)
    nrf_fprintf                              0x0001d5ed   Thumb Code    26  nrf_fprintf.o(i.nrf_fprintf)
    nrf_fprintf_buffer_flush                 0x0001d607   Thumb Code    24  nrf_fprintf.o(i.nrf_fprintf_buffer_flush)
    nrf_fprintf_fmt                          0x0001d61f   Thumb Code   474  nrf_fprintf_format.o(i.nrf_fprintf_fmt)
    nrf_log_backend_add                      0x0001d959   Thumb Code    86  nrf_log_frontend.o(i.nrf_log_backend_add)
    nrf_log_backend_rtt_init                 0x0001d9b7   Thumb Code     4  nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_init)
    nrf_log_backend_serial_put               0x0001d9d5   Thumb Code   200  nrf_log_backend_serial.o(i.nrf_log_backend_serial_put)
    nrf_log_color_id_get                     0x0001da9d   Thumb Code    42  nrf_log_frontend.o(i.nrf_log_color_id_get)
    nrf_log_default_backends_init            0x0001dacd   Thumb Code    24  nrf_log_default_backends.o(i.nrf_log_default_backends_init)
    nrf_log_frontend_dequeue                 0x0001dae9   Thumb Code   528  nrf_log_frontend.o(i.nrf_log_frontend_dequeue)
    nrf_log_frontend_std_0                   0x0001dd1d   Thumb Code     8  nrf_log_frontend.o(i.nrf_log_frontend_std_0)
    nrf_log_frontend_std_1                   0x0001dd25   Thumb Code    14  nrf_log_frontend.o(i.nrf_log_frontend_std_1)
    nrf_log_frontend_std_2                   0x0001dd33   Thumb Code    16  nrf_log_frontend.o(i.nrf_log_frontend_std_2)
    nrf_log_hexdump_entry_process            0x0001dd45   Thumb Code   150  nrf_log_str_formatter.o(i.nrf_log_hexdump_entry_process)
    nrf_log_init                             0x0001ddf5   Thumb Code    46  nrf_log_frontend.o(i.nrf_log_init)
    nrf_log_module_cnt_get                   0x0001de31   Thumb Code    10  nrf_log_frontend.o(i.nrf_log_module_cnt_get)
    nrf_log_module_name_get                  0x0001de45   Thumb Code    24  nrf_log_frontend.o(i.nrf_log_module_name_get)
    nrf_log_panic                            0x0001de61   Thumb Code    38  nrf_log_frontend.o(i.nrf_log_panic)
    nrf_log_std_entry_process                0x0001de8d   Thumb Code   182  nrf_log_str_formatter.o(i.nrf_log_std_entry_process)
    nrf_memobj_alloc                         0x0001df43   Thumb Code    96  nrf_memobj.o(i.nrf_memobj_alloc)
    nrf_memobj_free                          0x0001dfa3   Thumb Code    50  nrf_memobj.o(i.nrf_memobj_free)
    nrf_memobj_get                           0x0001dfd5   Thumb Code     8  nrf_memobj.o(i.nrf_memobj_get)
    nrf_memobj_pool_init                     0x0001dfdd   Thumb Code     4  nrf_memobj.o(i.nrf_memobj_pool_init)
    nrf_memobj_put                           0x0001dfe1   Thumb Code    30  nrf_memobj.o(i.nrf_memobj_put)
    nrf_memobj_read                          0x0001dfff   Thumb Code    16  nrf_memobj.o(i.nrf_memobj_read)
    nrf_memobj_write                         0x0001e00f   Thumb Code    16  nrf_memobj.o(i.nrf_memobj_write)
    nrf_pwr_mgmt_init                        0x0001e021   Thumb Code    28  nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_init)
    nrf_pwr_mgmt_run                         0x0001e049   Thumb Code    64  nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_run)
    nrf_ringbuf_init                         0x0001e091   Thumb Code    28  nrf_ringbuf.o(i.nrf_ringbuf_init)
    nrf_sdh_ble_app_ram_start_get            0x0001e0f5   Thumb Code    16  nrf_sdh_ble.o(i.nrf_sdh_ble_app_ram_start_get)
    nrf_sdh_ble_default_cfg_set              0x0001e109   Thumb Code   264  nrf_sdh_ble.o(i.nrf_sdh_ble_default_cfg_set)
    nrf_sdh_ble_enable                       0x0001e231   Thumb Code   116  nrf_sdh_ble.o(i.nrf_sdh_ble_enable)
    nrf_sdh_enable_request                   0x0001e3c1   Thumb Code   102  nrf_sdh.o(i.nrf_sdh_enable_request)
    nrf_sdh_evts_poll                        0x0001e435   Thumb Code    32  nrf_sdh.o(i.nrf_sdh_evts_poll)
    nrf_sdh_is_enabled                       0x0001e459   Thumb Code     6  nrf_sdh.o(i.nrf_sdh_is_enabled)
    nrf_section_iter_init                    0x0001e4a1   Thumb Code    10  nrf_section_iter.o(i.nrf_section_iter_init)
    nrf_section_iter_next                    0x0001e4cf   Thumb Code    32  nrf_section_iter.o(i.nrf_section_iter_next)
    nrf_strerror_find                        0x0001e4f1   Thumb Code    52  nrf_strerror.o(i.nrf_strerror_find)
    nrf_strerror_get                         0x0001e529   Thumb Code    14  nrf_strerror.o(i.nrf_strerror_get)
    nrfx_clock_enable                        0x0001e599   Thumb Code    34  nrfx_clock.o(i.nrfx_clock_enable)
    nrfx_clock_init                          0x0001e5c5   Thumb Code    26  nrfx_clock.o(i.nrfx_clock_init)
    nrfx_clock_lfclk_stop                    0x0001e5e5   Thumb Code    20  nrfx_clock.o(i.nrfx_clock_lfclk_stop)
    nrfx_gpiote_in_event_enable              0x0001e611   Thumb Code   156  nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable)
    nrfx_gpiote_in_init                      0x0001e6b5   Thumb Code   194  nrfx_gpiote.o(i.nrfx_gpiote_in_init)
    nrfx_gpiote_in_is_set                    0x0001e785   Thumb Code    20  nrfx_gpiote.o(i.nrfx_gpiote_in_is_set)
    nrfx_gpiote_init                         0x0001e799   Thumb Code    94  nrfx_gpiote.o(i.nrfx_gpiote_init)
    nrfx_gpiote_is_init                      0x0001e805   Thumb Code    14  nrfx_gpiote.o(i.nrfx_gpiote_is_init)
    nrfx_ppi_channel_alloc                   0x0001e829   Thumb Code   100  nrfx_ppi.o(i.nrfx_ppi_channel_alloc)
    nrfx_ppi_channel_assign                  0x0001e895   Thumb Code    62  nrfx_ppi.o(i.nrfx_ppi_channel_assign)
    nrfx_ppi_channel_enable                  0x0001e8d9   Thumb Code    48  nrfx_ppi.o(i.nrfx_ppi_channel_enable)
    nrfx_prs_acquire                         0x0001e90d   Thumb Code    58  nrfx_prs.o(i.nrfx_prs_acquire)
    nrfx_saadc_buffer_convert                0x0001e949   Thumb Code   154  nrfx_saadc.o(i.nrfx_saadc_buffer_convert)
    nrfx_saadc_channel_init                  0x0001e9ed   Thumb Code   160  nrfx_saadc.o(i.nrfx_saadc_channel_init)
    nrfx_saadc_init                          0x0001ea99   Thumb Code   130  nrfx_saadc.o(i.nrfx_saadc_init)
    nrfx_saadc_sample_task_get               0x0001eb2d   Thumb Code    20  nrfx_saadc.o(i.nrfx_saadc_sample_task_get)
    nrfx_timer_compare                       0x0001eb49   Thumb Code    58  nrfx_timer.o(i.nrfx_timer_compare)
    nrfx_timer_enable                        0x0001eb85   Thumb Code    24  nrfx_timer.o(i.nrfx_timer_enable)
    nrfx_timer_extended_compare              0x0001eba1   Thumb Code    42  nrfx_timer.o(i.nrfx_timer_extended_compare)
    nrfx_timer_init                          0x0001ebcd   Thumb Code   184  nrfx_timer.o(i.nrfx_timer_init)
    nrfx_uart_0_irq_handler                  0x0001ec89   Thumb Code     8  nrfx_uart.o(i.nrfx_uart_0_irq_handler)
    nrfx_uart_init                           0x0001ec99   Thumb Code   196  nrfx_uart.o(i.nrfx_uart_init)
    nrfx_uart_rx                             0x0001ed69   Thumb Code   230  nrfx_uart.o(i.nrfx_uart_rx)
    nrfx_uart_tx                             0x0001ee55   Thumb Code   160  nrfx_uart.o(i.nrfx_uart_tx)
    nrfx_uart_tx_in_progress                 0x0001eef9   Thumb Code    26  nrfx_uart.o(i.nrfx_uart_tx_in_progress)
    nrfx_uarte_0_irq_handler                 0x0001ef19   Thumb Code     8  nrfx_uarte.o(i.nrfx_uarte_0_irq_handler)
    nrfx_uarte_init                          0x0001ef29   Thumb Code   100  nrfx_uarte.o(i.nrfx_uarte_init)
    nrfx_uarte_rx                            0x0001ef95   Thumb Code   256  nrfx_uarte.o(i.nrfx_uarte_rx)
    nrfx_uarte_tx                            0x0001f099   Thumb Code   138  nrfx_uarte.o(i.nrfx_uarte_tx)
    nrfx_uarte_tx_in_progress                0x0001f129   Thumb Code    22  nrfx_uarte.o(i.nrfx_uarte_tx_in_progress)
    saadc_callback                           0x0001f6a9   Thumb Code   230  main.o(i.saadc_callback)
    saadc_init                               0x0001f7c1   Thumb Code    94  main.o(i.saadc_init)
    saadc_sampling_event_enable              0x0001f82d   Thumb Code    24  main.o(i.saadc_sampling_event_enable)
    saadc_sampling_event_init                0x0001f849   Thumb Code   136  main.o(i.saadc_sampling_event_init)
    timer_handler                            0x0001fba1   Thumb Code     2  main.o(i.timer_handler)
    uart_event_handle                        0x0001ff05   Thumb Code   112  main.o(i.uart_event_handle)
    nrf_log_backend_rtt_api                  0x00020788   Data          12  nrf_log_backend_rtt.o(.constdata)
    m_ram_start                              0x0002082c   Data           4  nrf_sdh_ble.o(.constdata)
    __ctype_table                            0x00020858   Data         129  ctype_o.o(.constdata)
    Region$$Table$$Base                      0x00020fa4   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x00020fc4   Number         0  anon$$obj.o(Region$$Table)
    log_const_data$$Base                     0x00020fd4   Number         0  nrf_ble_gatt.o(log_const_data)
    m_nrf_log_nrf_ble_gatt_logs_data_const   0x00020fd4   Data           8  nrf_ble_gatt.o(log_const_data)
    m_nrf_log_ble_nus_logs_data_const        0x00020fdc   Data           8  ble_nus.o(log_const_data)
    m_nrf_log_clock_logs_data_const          0x00020fe4   Data           8  nrf_drv_clock.o(log_const_data)
    m_nrf_log_CLOCK_logs_data_const          0x00020fec   Data           8  nrfx_clock.o(log_const_data)
    m_nrf_log_GPIOTE_logs_data_const         0x00020ff4   Data           8  nrfx_gpiote.o(log_const_data)
    m_nrf_log_PRS_logs_data_const            0x00020ffc   Data           8  nrfx_prs.o(log_const_data)
    m_nrf_log_UART_logs_data_const           0x00021004   Data           8  nrfx_uart.o(log_const_data)
    m_nrf_log_UARTE_logs_data_const          0x0002100c   Data           8  nrfx_uarte.o(log_const_data)
    m_nrf_log_PPI_logs_data_const            0x00021014   Data           8  nrfx_ppi.o(log_const_data)
    m_nrf_log_SAADC_logs_data_const          0x0002101c   Data           8  nrfx_saadc.o(log_const_data)
    m_nrf_log_TIMER_logs_data_const          0x00021024   Data           8  nrfx_timer.o(log_const_data)
    m_nrf_log_TWIM_logs_data_const           0x0002102c   Data           8  nrfx_twim.o(log_const_data)
    m_nrf_log_pwr_mgmt_logs_data_const       0x00021034   Data           8  nrf_pwr_mgmt.o(log_const_data)
    m_nrf_log_app_logs_data_const            0x0002103c   Data           8  nrf_log_frontend.o(log_const_data)
    m_nrf_log_nrf_sdh_logs_data_const        0x00021044   Data           8  nrf_sdh.o(log_const_data)
    m_nrf_log_nrf_sdh_ble_logs_data_const    0x0002104c   Data           8  nrf_sdh_ble.o(log_const_data)
    m_nrf_log_nrf_sdh_soc_logs_data_const    0x00021054   Data           8  nrf_sdh_soc.o(log_const_data)
    log_const_data$$Limit                    0x0002105c   Number         0  nrf_sdh_soc.o(log_const_data)
    log_mempool                              0x0002105c   Data          20  nrf_log_frontend.o(nrf_balloc)
    sdh_ble_observers0$$Base                 0x00021070   Number         0  ble_conn_state.o(sdh_ble_observers0)
    sdh_ble_observers0$$Limit                0x00021078   Number         0  ble_conn_state.o(sdh_ble_observers0)
    sdh_ble_observers1$$Base                 0x00021078   Number         0  main.o(sdh_ble_observers1)
    sdh_ble_observers1$$Limit                0x00021098   Number         0  ble_conn_params.o(sdh_ble_observers1)
    sdh_ble_observers2$$Base                 0x00021098   Number         0  main.o(sdh_ble_observers2)
    sdh_ble_observers2$$Limit                0x000210a8   Number         0  main.o(sdh_ble_observers2)
    sdh_ble_observers3$$Base                 0x000210a8   Number         0  main.o(sdh_ble_observers3)
    sdh_ble_observers3$$Limit                0x000210b0   Number         0  main.o(sdh_ble_observers3)
    sdh_soc_observers0$$Base                 0x000210b0   Number         0  nrf_drv_clock.o(sdh_soc_observers0)
    sdh_soc_observers0$$Limit                0x000210b8   Number         0  nrf_drv_clock.o(sdh_soc_observers0)
    sdh_soc_observers1$$Base                 0x000210b8   Number         0  main.o(sdh_soc_observers1)
    sdh_soc_observers1$$Limit                0x000210c0   Number         0  main.o(sdh_soc_observers1)
    sdh_stack_observers0$$Base               0x000210c0   Number         0  nrf_sdh_ble.o(sdh_stack_observers0)
    sdh_stack_observers0$$Limit              0x000210d0   Number         0  nrf_sdh_soc.o(sdh_stack_observers0)
    sdh_state_observers0$$Base               0x000210d0   Number         0  nrf_drv_clock.o(sdh_state_observers0)
    sdh_state_observers0$$Limit              0x000210d8   Number         0  nrf_drv_clock.o(sdh_state_observers0)
    Image$$RW_IRAM1$$Base                    0x20002500   Number         0  anon$$obj.o ABSOLUTE
    ReportDataTimeOut                        0x20002500   Data           1  main.o(.data)
    nrf_drv_uart_use_easy_dma                0x20002560   Data           1  nrf_drv_uart.o(.data)
    __stdout                                 0x200025e0   Data           4  retarget.o(.data)
    SystemCoreClock                          0x20002644   Data           4  system_nrf52.o(.data)
    CurrentPressure                          0x20002a10   Data          21  main.o(.bss)
    nrf_nvic_state                           0x20002dd8   Data          12  app_util_platform.o(.bss)
    _SEGGER_RTT                              0x200033ac   Data         120  segger_rtt.o(.bss)
    __initial_sp                             0x20003e38   Data           0  arm_startup_nrf52.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x00019201

  Load Region LR_IROM1 (Base: 0x00019000, Size: 0x00008220, Max: 0x00067000, ABSOLUTE, COMPRESSED[0x0000812c])

    Execution Region ER_IROM1 (Exec base: 0x00019000, Load base: 0x00019000, Size: 0x000080d8, Max: 0x00067000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00019000   0x00019000   0x00000200   Data   RO         5566    RESET               arm_startup_nrf52.o
    0x00019200   0x00019200   0x00000000   Code   RO         5607  * .ARM.Collect$$$$00000000  mc_w.l(entry.o)
    0x00019200   0x00019200   0x00000004   Code   RO         5921    .ARM.Collect$$$$00000001  mc_w.l(entry2.o)
    0x00019204   0x00019204   0x00000004   Code   RO         5924    .ARM.Collect$$$$00000004  mc_w.l(entry5.o)
    0x00019208   0x00019208   0x00000000   Code   RO         5926    .ARM.Collect$$$$00000008  mc_w.l(entry7b.o)
    0x00019208   0x00019208   0x00000000   Code   RO         5928    .ARM.Collect$$$$0000000A  mc_w.l(entry8b.o)
    0x00019208   0x00019208   0x00000008   Code   RO         5929    .ARM.Collect$$$$0000000B  mc_w.l(entry9a.o)
    0x00019210   0x00019210   0x00000000   Code   RO         5931    .ARM.Collect$$$$0000000D  mc_w.l(entry10a.o)
    0x00019210   0x00019210   0x00000000   Code   RO         5933    .ARM.Collect$$$$0000000F  mc_w.l(entry11a.o)
    0x00019210   0x00019210   0x00000004   Code   RO         5922    .ARM.Collect$$$$00002712  mc_w.l(entry2.o)
    0x00019214   0x00019214   0x000000e2   Code   RO         4153    .emb_text           nrf_atomic.o
    0x000192f6   0x000192f6   0x00000002   PAD
    0x000192f8   0x000192f8   0x00000024   Code   RO         5567    .text               arm_startup_nrf52.o
    0x0001931c   0x0001931c   0x00000062   Code   RO         5610    .text               mc_w.l(uldiv.o)
    0x0001937e   0x0001937e   0x0000001e   Code   RO         5612    .text               mc_w.l(llshl.o)
    0x0001939c   0x0001939c   0x00000020   Code   RO         5614    .text               mc_w.l(llushr.o)
    0x000193bc   0x000193bc   0x00000008   Code   RO         5616    .text               mc_w.l(ctype_o.o)
    0x000193c4   0x000193c4   0x00000024   Code   RO         5644    .text               mc_w.l(memcpya.o)
    0x000193e8   0x000193e8   0x00000024   Code   RO         5646    .text               mc_w.l(memseta.o)
    0x0001940c   0x0001940c   0x00000018   Code   RO         5648    .text               mc_w.l(strcat.o)
    0x00019424   0x00019424   0x0000000e   Code   RO         5650    .text               mc_w.l(strlen.o)
    0x00019432   0x00019432   0x00000012   Code   RO         5654    .text               mc_w.l(strcpy.o)
    0x00019444   0x00019444   0x00000026   Code   RO         5919    .text               mf_w.l(f2d.o)
    0x0001946a   0x0001946a   0x0000002c   Code   RO         5935    .text               mc_w.l(uidiv.o)
    0x00019496   0x00019496   0x00000000   Code   RO         5937    .text               mc_w.l(iusefp.o)
    0x00019496   0x00019496   0x0000014e   Code   RO         5938    .text               mf_w.l(dadd.o)
    0x000195e4   0x000195e4   0x000000e4   Code   RO         5940    .text               mf_w.l(dmul.o)
    0x000196c8   0x000196c8   0x000000de   Code   RO         5942    .text               mf_w.l(ddiv.o)
    0x000197a6   0x000197a6   0x00000030   Code   RO         5944    .text               mf_w.l(dfixul.o)
    0x000197d6   0x000197d6   0x00000002   PAD
    0x000197d8   0x000197d8   0x00000030   Code   RO         5946    .text               mf_w.l(cdrcmple.o)
    0x00019808   0x00019808   0x00000024   Code   RO         5948    .text               mc_w.l(init.o)
    0x0001982c   0x0001982c   0x00000024   Code   RO         5950    .text               mc_w.l(llsshr.o)
    0x00019850   0x00019850   0x000000ba   Code   RO         5952    .text               mf_w.l(depilogue.o)
    0x0001990a   0x0001990a   0x00000056   Code   RO         5962    .text               mc_w.l(__dczerorl2.o)
    0x00019960   0x00019960   0x00000164   Code   RO         2008    i.GPIOTE_IRQHandler  nrfx_gpiote.o
    0x00019ac4   0x00019ac4   0x00000016   Code   RO         3651    i.NVIC_ClearPendingIRQ  app_timer.o
    0x00019ada   0x00019ada   0x00000016   Code   RO         3652    i.NVIC_EnableIRQ    app_timer.o
    0x00019af0   0x00019af0   0x00000016   Code   RO         3653    i.NVIC_SetPendingIRQ  app_timer.o
    0x00019b06   0x00019b06   0x00000020   Code   RO         3654    i.NVIC_SetPriority  app_timer.o
    0x00019b26   0x00019b26   0x00000002   PAD
    0x00019b28   0x00019b28   0x00000058   Code   RO         1870    i.POWER_CLOCK_IRQHandler  nrfx_clock.o
    0x00019b80   0x00019b80   0x00000024   Code   RO         3655    i.RTC1_IRQHandler   app_timer.o
    0x00019ba4   0x00019ba4   0x00000148   Code   RO         2865    i.SAADC_IRQHandler  nrfx_saadc.o
    0x00019cec   0x00019cec   0x00000004   Code   RO         5106    i.SEGGER_RTT_Init   segger_rtt.o
    0x00019cf0   0x00019cf0   0x0000005c   Code   RO         5120    i.SEGGER_RTT_WriteNoLock  segger_rtt.o
    0x00019d4c   0x00019d4c   0x00000010   Code   RO         3232    i.SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler  nrfx_twim.o
    0x00019d5c   0x00019d5c   0x00000004   Code   RO         3656    i.SWI0_EGU0_IRQHandler  app_timer.o
    0x00019d60   0x00019d60   0x00000004   Code   RO         5357    i.SWI2_EGU2_IRQHandler  nrf_sdh.o
    0x00019d64   0x00019d64   0x0000031c   Code   RO         5575    i.SystemInit        system_nrf52.o
    0x0001a080   0x0001a080   0x00000050   Code   RO         3017    i.TIMER0_IRQHandler  nrfx_timer.o
    0x0001a0d0   0x0001a0d0   0x0000000c   Code   RO         2277    i.UARTE0_UART0_IRQHandler  nrfx_prs.o
    0x0001a0dc   0x0001a0dc   0x00000068   Code   RO         5124    i._DoInit           segger_rtt.o
    0x0001a144   0x0001a144   0x00000016   Code   RO         5125    i._GetAvailWriteSpace  segger_rtt.o
    0x0001a15a   0x0001a15a   0x0000005a   Code   RO         5127    i._WriteBlocking    segger_rtt.o
    0x0001a1b4   0x0001a1b4   0x00000042   Code   RO         5128    i._WriteNoCheck     segger_rtt.o
    0x0001a1f6   0x0001a1f6   0x00000002   PAD
    0x0001a1f8   0x0001a1f8   0x00000020   Code   RO         5891    i.__0printf         mc_w.l(printfa.o)
    0x0001a218   0x0001a218   0x00000028   Code   RO         5893    i.__0sprintf        mc_w.l(printfa.o)
    0x0001a240   0x0001a240   0x0000000e   Code   RO         5956    i.__scatterload_copy  mc_w.l(handlers.o)
    0x0001a24e   0x0001a24e   0x00000002   Code   RO         5957    i.__scatterload_null  mc_w.l(handlers.o)
    0x0001a250   0x0001a250   0x0000000e   Code   RO         5958    i.__scatterload_zeroinit  mc_w.l(handlers.o)
    0x0001a25e   0x0001a25e   0x00000002   PAD
    0x0001a260   0x0001a260   0x00000024   Code   RO         5358    i.__sd_nvic_app_accessible_irq  nrf_sdh.o
    0x0001a284   0x0001a284   0x00000184   Code   RO         5898    i._fp_digits        mc_w.l(printfa.o)
    0x0001a408   0x0001a408   0x000006dc   Code   RO         5899    i._printf_core      mc_w.l(printfa.o)
    0x0001aae4   0x0001aae4   0x00000024   Code   RO         5900    i._printf_post_padding  mc_w.l(printfa.o)
    0x0001ab08   0x0001ab08   0x0000002e   Code   RO         5901    i._printf_pre_padding  mc_w.l(printfa.o)
    0x0001ab36   0x0001ab36   0x0000000a   Code   RO         5903    i._sputc            mc_w.l(printfa.o)
    0x0001ab40   0x0001ab40   0x00000036   Code   RO          712    i.advertising_buttons_configure  bsp_btn_ble.o
    0x0001ab76   0x0001ab76   0x00000006   Code   RO          595    i.alert_timer_handler  bsp.o
    0x0001ab7c   0x0001ab7c   0x00000024   Code   RO         3373    i.app_button_enable  app_button.o
    0x0001aba0   0x0001aba0   0x00000078   Code   RO         3374    i.app_button_init   app_button.o
    0x0001ac18   0x0001ac18   0x00000084   Code   RO         3493    i.app_error_fault_handler  app_error_weak.o
    0x0001ac9c   0x0001ac9c   0x00000016   Code   RO         3437    i.app_error_handler_bare  app_error.o
    0x0001acb2   0x0001acb2   0x00000016   Code   RO         3528    i.app_fifo_get      app_fifo.o
    0x0001acc8   0x0001acc8   0x00000020   Code   RO         3529    i.app_fifo_init     app_fifo.o
    0x0001ace8   0x0001ace8   0x0000001a   Code   RO         3531    i.app_fifo_put      app_fifo.o
    0x0001ad02   0x0001ad02   0x00000002   PAD
    0x0001ad04   0x0001ad04   0x00000028   Code   RO         3659    i.app_timer_create  app_timer.o
    0x0001ad2c   0x0001ad2c   0x00000054   Code   RO         3660    i.app_timer_init    app_timer.o
    0x0001ad80   0x0001ad80   0x00000088   Code   RO         3663    i.app_timer_start   app_timer.o
    0x0001ae08   0x0001ae08   0x00000020   Code   RO         3664    i.app_timer_stop    app_timer.o
    0x0001ae28   0x0001ae28   0x00000034   Code   RO         3820    i.app_uart_get      app_uart_fifo.o
    0x0001ae5c   0x0001ae5c   0x000000a4   Code   RO         3821    i.app_uart_init     app_uart_fifo.o
    0x0001af00   0x0001af00   0x00000054   Code   RO         3822    i.app_uart_put      app_uart_fifo.o
    0x0001af54   0x0001af54   0x00000048   Code   RO         3901    i.app_util_critical_region_enter  app_util_platform.o
    0x0001af9c   0x0001af9c   0x00000034   Code   RO         3902    i.app_util_critical_region_exit  app_util_platform.o
    0x0001afd0   0x0001afd0   0x00000088   Code   RO         2331    i.apply_config      nrfx_uart.o
    0x0001b058   0x0001b058   0x00000088   Code   RO         2519    i.apply_config      nrfx_uarte.o
    0x0001b0e0   0x0001b0e0   0x0000000c   Code   RO         2712    i.are_app_channels  nrfx_ppi.o
    0x0001b0ec   0x0001b0ec   0x00000048   Code   RO         1273    i.blcm_link_ctx_get  ble_link_ctx_manager.o
    0x0001b134   0x0001b134   0x00000182   Code   RO          822    i.ble_advdata_encode  ble_advdata.o
    0x0001b2b6   0x0001b2b6   0x00000020   Code   RO          824    i.ble_advdata_parse  ble_advdata.o
    0x0001b2d6   0x0001b2d6   0x00000038   Code   RO          825    i.ble_advdata_search  ble_advdata.o
    0x0001b30e   0x0001b30e   0x00000006   Code   RO          935    i.ble_advertising_conn_cfg_tag_set  ble_advertising.o
    0x0001b314   0x0001b314   0x000000ea   Code   RO          936    i.ble_advertising_init  ble_advertising.o
    0x0001b3fe   0x0001b3fe   0x0000006a   Code   RO          938    i.ble_advertising_on_ble_evt  ble_advertising.o
    0x0001b468   0x0001b468   0x00000002   Code   RO          939    i.ble_advertising_on_sys_evt  ble_advertising.o
    0x0001b46a   0x0001b46a   0x0000003a   Code   RO          941    i.ble_advertising_restart_without_whitelist  ble_advertising.o
    0x0001b4a4   0x0001b4a4   0x00000202   Code   RO          942    i.ble_advertising_start  ble_advertising.o
    0x0001b6a6   0x0001b6a6   0x00000002   PAD
    0x0001b6a8   0x0001b6a8   0x00000068   Code   RO         1034    i.ble_conn_params_init  ble_conn_params.o
    0x0001b710   0x0001b710   0x00000012   Code   RO         1116    i.ble_conn_state_conn_idx  ble_conn_state.o
    0x0001b722   0x0001b722   0x00000002   PAD
    0x0001b724   0x0001b724   0x00000014   Code   RO         1129    i.ble_conn_state_valid  ble_conn_state.o
    0x0001b738   0x0001b738   0x00000060   Code   RO          828    i.ble_device_addr_encode  ble_advdata.o
    0x0001b798   0x0001b798   0x000000d8   Code   RO            5    i.ble_evt_handler   main.o
    0x0001b870   0x0001b870   0x00000070   Code   RO          713    i.ble_evt_handler   bsp_btn_ble.o
    0x0001b8e0   0x0001b8e0   0x000000fc   Code   RO         1036    i.ble_evt_handler   ble_conn_params.o
    0x0001b9dc   0x0001b9dc   0x00000104   Code   RO         1130    i.ble_evt_handler   ble_conn_state.o
    0x0001bae0   0x0001bae0   0x00000066   Code   RO         1475    i.ble_nus_data_send  ble_nus.o
    0x0001bb46   0x0001bb46   0x00000002   PAD
    0x0001bb48   0x0001bb48   0x000000d4   Code   RO         1476    i.ble_nus_init      ble_nus.o
    0x0001bc1c   0x0001bc1c   0x00000070   Code   RO         1477    i.ble_nus_on_ble_evt  ble_nus.o
    0x0001bc8c   0x0001bc8c   0x00000008   Code   RO         1299    i.ble_srv_is_notification_enabled  ble_srv_common.o
    0x0001bc94   0x0001bc94   0x0000000c   Code   RO          456    i.bsp_board_button_idx_to_pin  boards.o
    0x0001bca0   0x0001bca0   0x00000020   Code   RO          457    i.bsp_board_button_state_get  boards.o
    0x0001bcc0   0x0001bcc0   0x00000054   Code   RO          458    i.bsp_board_init    boards.o
    0x0001bd14   0x0001bd14   0x00000024   Code   RO          460    i.bsp_board_led_invert  boards.o
    0x0001bd38   0x0001bd38   0x00000010   Code   RO          461    i.bsp_board_led_off  boards.o
    0x0001bd48   0x0001bd48   0x00000010   Code   RO          462    i.bsp_board_led_on  boards.o
    0x0001bd58   0x0001bd58   0x00000020   Code   RO          463    i.bsp_board_led_state_get  boards.o
    0x0001bd78   0x0001bd78   0x00000012   Code   RO          464    i.bsp_board_leds_off  boards.o
    0x0001bd8a   0x0001bd8a   0x00000012   Code   RO          465    i.bsp_board_leds_on  boards.o
    0x0001bd9c   0x0001bd9c   0x00000024   Code   RO          466    i.bsp_board_pin_to_button_idx  boards.o
    0x0001bdc0   0x0001bdc0   0x00000038   Code   RO          714    i.bsp_btn_ble_init  bsp_btn_ble.o
    0x0001bdf8   0x0001bdf8   0x0000001e   Code   RO          715    i.bsp_btn_ble_sleep_mode_prepare  bsp_btn_ble.o
    0x0001be16   0x0001be16   0x00000002   PAD
    0x0001be18   0x0001be18   0x00000090   Code   RO          596    i.bsp_button_event_handler  bsp.o
    0x0001bea8   0x0001bea8   0x0000000c   Code   RO          597    i.bsp_button_is_pressed  bsp.o
    0x0001beb4   0x0001beb4   0x0000005c   Code   RO            6    i.bsp_event_handler  main.o
    0x0001bf10   0x0001bf10   0x00000044   Code   RO          600    i.bsp_event_to_button_action_assign  bsp.o
    0x0001bf54   0x0001bf54   0x00000018   Code   RO          601    i.bsp_indication_set  bsp.o
    0x0001bf6c   0x0001bf6c   0x00000094   Code   RO          602    i.bsp_init          bsp.o
    0x0001c000   0x0001c000   0x000001c8   Code   RO          603    i.bsp_led_indication  bsp.o
    0x0001c1c8   0x0001c1c8   0x00000006   Code   RO          605    i.bsp_wakeup_button_enable  bsp.o
    0x0001c1ce   0x0001c1ce   0x00000002   PAD
    0x0001c1d0   0x0001c1d0   0x00000090   Code   RO         4861    i.buf_prealloc      nrf_log_frontend.o
    0x0001c260   0x0001c260   0x0000002e   Code   RO         4365    i.buffer_add        nrf_fprintf_format.o
    0x0001c28e   0x0001c28e   0x00000002   PAD
    0x0001c290   0x0001c290   0x00000014   Code   RO         4862    i.buffer_is_empty   nrf_log_frontend.o
    0x0001c2a4   0x0001c2a4   0x00000008   Code   RO          606    i.button_timer_handler  bsp.o
    0x0001c2ac   0x0001c2ac   0x0000001c   Code   RO         2009    i.channel_free      nrfx_gpiote.o
    0x0001c2c8   0x0001c2c8   0x00000048   Code   RO         2010    i.channel_port_alloc  nrfx_gpiote.o
    0x0001c310   0x0001c310   0x00000010   Code   RO         2011    i.channel_port_get  nrfx_gpiote.o
    0x0001c320   0x0001c320   0x00000190   Code   RO         1301    i.characteristic_add  ble_srv_common.o
    0x0001c4b0   0x0001c4b0   0x00000028   Code   RO         1533    i.clock_clk_started_notify  nrf_drv_clock.o
    0x0001c4d8   0x0001c4d8   0x0000001c   Code   RO         1534    i.clock_irq_handler  nrf_drv_clock.o
    0x0001c4f4   0x0001c4f4   0x000000ac   Code   RO         3666    i.compare_reg_update  app_timer.o
    0x0001c5a0   0x0001c5a0   0x0000003e   Code   RO         1131    i.conn_handle_list_get  ble_conn_state.o
    0x0001c5de   0x0001c5de   0x00000088   Code   RO          829    i.conn_int_encode   ble_advdata.o
    0x0001c666   0x0001c666   0x00000004   Code   RO            7    i.conn_params_error_handler  main.o
    0x0001c66a   0x0001c66a   0x00000002   PAD
    0x0001c66c   0x0001c66c   0x00000048   Code   RO         1037    i.conn_params_negotiation  ble_conn_params.o
    0x0001c6b4   0x0001c6b4   0x0000009c   Code   RO         3376    i.detection_delay_timeout_handler  app_button.o
    0x0001c750   0x0001c750   0x00000014   Code   RO         4863    i.dropped_sat16_get  nrf_log_frontend.o
    0x0001c764   0x0001c764   0x00000040   Code   RO         3667    i.elapsed_ticks_acquire  app_timer.o
    0x0001c7a4   0x0001c7a4   0x00000014   Code   RO         3534    i.fifo_get          app_fifo.o
    0x0001c7b8   0x0001c7b8   0x00000012   Code   RO         3535    i.fifo_put          app_fifo.o
    0x0001c7ca   0x0001c7ca   0x00000028   Code   RO          944    i.flags_set         ble_advertising.o
    0x0001c7f2   0x0001c7f2   0x0000000e   Code   RO         4688    i.fputc             retarget.o
    0x0001c800   0x0001c800   0x0000005c   Code   RO            8    i.gatt_evt_handler  main.o
    0x0001c85c   0x0001c85c   0x00000030   Code   RO            9    i.gatt_init         main.o
    0x0001c88c   0x0001c88c   0x00000084   Code   RO         3377    i.gpiote_event_handler  app_button.o
    0x0001c910   0x0001c910   0x00000014   Code   RO         1038    i.instance_get      ble_conn_params.o
    0x0001c924   0x0001c924   0x000000a6   Code   RO         4366    i.int_print         nrf_fprintf_format.o
    0x0001c9ca   0x0001c9ca   0x00000002   PAD
    0x0001c9cc   0x0001c9cc   0x0000007c   Code   RO         2520    i.interrupts_enable  nrfx_uarte.o
    0x0001ca48   0x0001ca48   0x00000034   Code   RO         4864    i.invalid_packets_omit  nrf_log_frontend.o
    0x0001ca7c   0x0001ca7c   0x00000018   Code   RO         2713    i.is_allocated_channel  nrfx_ppi.o
    0x0001ca94   0x0001ca94   0x0000000a   Code   RO         2715    i.is_app_channel    nrfx_ppi.o
    0x0001ca9e   0x0001ca9e   0x00000044   Code   RO         1039    i.is_conn_params_ok  ble_conn_params.o
    0x0001cae2   0x0001cae2   0x0000000c   Code   RO         2717    i.is_programmable_app_channel  nrfx_ppi.o
    0x0001caee   0x0001caee   0x00000002   PAD
    0x0001caf0   0x0001caf0   0x0000002c   Code   RO          607    i.leds_off          bsp.o
    0x0001cb1c   0x0001cb1c   0x00000014   Code   RO          608    i.leds_timer_handler  bsp.o
    0x0001cb30   0x0001cb30   0x00000010   Code   RO         1359    i.link_init         nrf_ble_gatt.o
    0x0001cb40   0x0001cb40   0x000000f8   Code   RO         3668    i.list_insertions_handler  app_timer.o
    0x0001cc38   0x0001cc38   0x0000009c   Code   RO         4865    i.log_skip          nrf_log_frontend.o
    0x0001ccd4   0x0001ccd4   0x000002a0   Code   RO           10    i.main              main.o
    0x0001cf74   0x0001cf74   0x00000064   Code   RO          830    i.manuf_specific_data_encode  ble_advdata.o
    0x0001cfd8   0x0001cfd8   0x0000007e   Code   RO         4405    i.memobj_op         nrf_memobj.o
    0x0001d056   0x0001d056   0x00000002   PAD
    0x0001d058   0x0001d058   0x00000030   Code   RO         4866    i.module_idx_get    nrf_log_frontend.o
    0x0001d088   0x0001d088   0x000000a6   Code   RO          831    i.name_encode       ble_advdata.o
    0x0001d12e   0x0001d12e   0x00000016   Code   RO         4087    i.nrf_atflags_clear  nrf_atflags.o
    0x0001d144   0x0001d144   0x00000016   Code   RO         4092    i.nrf_atflags_get   nrf_atflags.o
    0x0001d15a   0x0001d15a   0x00000014   Code   RO         4094    i.nrf_atflags_set   nrf_atflags.o
    0x0001d16e   0x0001d16e   0x00000006   Code   RO         4155    i.nrf_atomic_flag_clear_fetch  nrf_atomic.o
    0x0001d174   0x0001d174   0x00000006   Code   RO         4156    i.nrf_atomic_flag_set  nrf_atomic.o
    0x0001d17a   0x0001d17a   0x0000000c   Code   RO         4158    i.nrf_atomic_u32_add  nrf_atomic.o
    0x0001d186   0x0001d186   0x0000000c   Code   RO         4159    i.nrf_atomic_u32_and  nrf_atomic.o
    0x0001d192   0x0001d192   0x0000000a   Code   RO         4162    i.nrf_atomic_u32_fetch_and  nrf_atomic.o
    0x0001d19c   0x0001d19c   0x0000000a   Code   RO         4164    i.nrf_atomic_u32_fetch_store  nrf_atomic.o
    0x0001d1a6   0x0001d1a6   0x0000000c   Code   RO         4168    i.nrf_atomic_u32_or  nrf_atomic.o
    0x0001d1b2   0x0001d1b2   0x0000000c   Code   RO         4170    i.nrf_atomic_u32_sub  nrf_atomic.o
    0x0001d1be   0x0001d1be   0x00000044   Code   RO         4289    i.nrf_balloc_alloc  nrf_balloc.o
    0x0001d202   0x0001d202   0x00000030   Code   RO         4290    i.nrf_balloc_free   nrf_balloc.o
    0x0001d232   0x0001d232   0x00000030   Code   RO         4291    i.nrf_balloc_init   nrf_balloc.o
    0x0001d262   0x0001d262   0x00000010   Code   RO         2012    i.nrf_bitmask_bit_is_set  nrfx_gpiote.o
    0x0001d272   0x0001d272   0x00000014   Code   RO         2013    i.nrf_bitmask_bit_set  nrfx_gpiote.o
    0x0001d286   0x0001d286   0x00000018   Code   RO         1361    i.nrf_ble_gatt_att_mtu_periph_set  nrf_ble_gatt.o
    0x0001d29e   0x0001d29e   0x00000022   Code   RO         1363    i.nrf_ble_gatt_init  nrf_ble_gatt.o
    0x0001d2c0   0x0001d2c0   0x000000f4   Code   RO         1364    i.nrf_ble_gatt_on_ble_evt  nrf_ble_gatt.o
    0x0001d3b4   0x0001d3b4   0x00000016   Code   RO         1434    i.nrf_ble_qwr_conn_handle_assign  nrf_ble_qwr.o
    0x0001d3ca   0x0001d3ca   0x00000024   Code   RO         1435    i.nrf_ble_qwr_init  nrf_ble_qwr.o
    0x0001d3ee   0x0001d3ee   0x000000b6   Code   RO         1436    i.nrf_ble_qwr_on_ble_evt  nrf_ble_qwr.o
    0x0001d4a4   0x0001d4a4   0x0000000e   Code   RO         1871    i.nrf_clock_event_check  nrfx_clock.o
    0x0001d4b2   0x0001d4b2   0x00000010   Code   RO         1872    i.nrf_clock_event_clear  nrfx_clock.o
    0x0001d4c2   0x0001d4c2   0x00000002   PAD
    0x0001d4c4   0x0001d4c4   0x00000038   Code   RO         1541    i.nrf_drv_clock_init  nrf_drv_clock.o
    0x0001d4fc   0x0001d4fc   0x00000030   Code   RO         1545    i.nrf_drv_clock_lfclk_release  nrf_drv_clock.o
    0x0001d52c   0x0001d52c   0x00000018   Code   RO         2674    i.nrf_drv_ppi_init  nrf_drv_ppi.o
    0x0001d544   0x0001d544   0x00000068   Code   RO         1679    i.nrf_drv_uart_init  nrf_drv_uart.o
    0x0001d5ac   0x0001d5ac   0x00000020   Code   RO         3823    i.nrf_drv_uart_rx   app_uart_fifo.o
    0x0001d5cc   0x0001d5cc   0x00000020   Code   RO         3824    i.nrf_drv_uart_tx   app_uart_fifo.o
    0x0001d5ec   0x0001d5ec   0x0000001a   Code   RO         4326    i.nrf_fprintf       nrf_fprintf.o
    0x0001d606   0x0001d606   0x00000018   Code   RO         4327    i.nrf_fprintf_buffer_flush  nrf_fprintf.o
    0x0001d61e   0x0001d61e   0x000001da   Code   RO         4367    i.nrf_fprintf_fmt   nrf_fprintf_format.o
    0x0001d7f8   0x0001d7f8   0x00000024   Code   RO          468    i.nrf_gpio_cfg      boards.o
    0x0001d81c   0x0001d81c   0x00000024   Code   RO         2014    i.nrf_gpio_cfg      nrfx_gpiote.o
    0x0001d840   0x0001d840   0x00000024   Code   RO         2332    i.nrf_gpio_cfg      nrfx_uart.o
    0x0001d864   0x0001d864   0x00000024   Code   RO         2521    i.nrf_gpio_cfg      nrfx_uarte.o
    0x0001d888   0x0001d888   0x00000012   Code   RO         2334    i.nrf_gpio_cfg_input  nrfx_uart.o
    0x0001d89a   0x0001d89a   0x00000012   Code   RO         2523    i.nrf_gpio_cfg_input  nrfx_uarte.o
    0x0001d8ac   0x0001d8ac   0x00000014   Code   RO         2335    i.nrf_gpio_cfg_output  nrfx_uart.o
    0x0001d8c0   0x0001d8c0   0x00000014   Code   RO         2524    i.nrf_gpio_cfg_output  nrfx_uarte.o
    0x0001d8d4   0x0001d8d4   0x00000022   Code   RO         2016    i.nrf_gpio_cfg_sense_set  nrfx_gpiote.o
    0x0001d8f6   0x0001d8f6   0x00000016   Code   RO          469    i.nrf_gpio_pin_write  boards.o
    0x0001d90c   0x0001d90c   0x00000028   Code   RO         2017    i.nrf_gpio_ports_read  nrfx_gpiote.o
    0x0001d934   0x0001d934   0x00000014   Code   RO         2018    i.nrf_gpiote_event_clear  nrfx_gpiote.o
    0x0001d948   0x0001d948   0x00000010   Code   RO         2019    i.nrf_gpiote_event_is_set  nrfx_gpiote.o
    0x0001d958   0x0001d958   0x0000005c   Code   RO         4867    i.nrf_log_backend_add  nrf_log_frontend.o
    0x0001d9b4   0x0001d9b4   0x00000002   Code   RO         4725    i.nrf_log_backend_rtt_flush  nrf_log_backend_rtt.o
    0x0001d9b6   0x0001d9b6   0x00000004   Code   RO         4726    i.nrf_log_backend_rtt_init  nrf_log_backend_rtt.o
    0x0001d9ba   0x0001d9ba   0x00000002   Code   RO         4727    i.nrf_log_backend_rtt_panic_set  nrf_log_backend_rtt.o
    0x0001d9bc   0x0001d9bc   0x00000018   Code   RO         4728    i.nrf_log_backend_rtt_put  nrf_log_backend_rtt.o
    0x0001d9d4   0x0001d9d4   0x000000c8   Code   RO         4791    i.nrf_log_backend_serial_put  nrf_log_backend_serial.o
    0x0001da9c   0x0001da9c   0x00000030   Code   RO         4869    i.nrf_log_color_id_get  nrf_log_frontend.o
    0x0001dacc   0x0001dacc   0x0000001c   Code   RO         4825    i.nrf_log_default_backends_init  nrf_log_default_backends.o
    0x0001dae8   0x0001dae8   0x00000234   Code   RO         4870    i.nrf_log_frontend_dequeue  nrf_log_frontend.o
    0x0001dd1c   0x0001dd1c   0x00000008   Code   RO         4872    i.nrf_log_frontend_std_0  nrf_log_frontend.o
    0x0001dd24   0x0001dd24   0x0000000e   Code   RO         4873    i.nrf_log_frontend_std_1  nrf_log_frontend.o
    0x0001dd32   0x0001dd32   0x00000010   Code   RO         4874    i.nrf_log_frontend_std_2  nrf_log_frontend.o
    0x0001dd42   0x0001dd42   0x00000002   PAD
    0x0001dd44   0x0001dd44   0x000000b0   Code   RO         5047    i.nrf_log_hexdump_entry_process  nrf_log_str_formatter.o
    0x0001ddf4   0x0001ddf4   0x0000003c   Code   RO         4879    i.nrf_log_init      nrf_log_frontend.o
    0x0001de30   0x0001de30   0x00000014   Code   RO         4880    i.nrf_log_module_cnt_get  nrf_log_frontend.o
    0x0001de44   0x0001de44   0x0000001c   Code   RO         4883    i.nrf_log_module_name_get  nrf_log_frontend.o
    0x0001de60   0x0001de60   0x0000002c   Code   RO         4884    i.nrf_log_panic     nrf_log_frontend.o
    0x0001de8c   0x0001de8c   0x000000b6   Code   RO         5048    i.nrf_log_std_entry_process  nrf_log_str_formatter.o
    0x0001df42   0x0001df42   0x00000060   Code   RO         4406    i.nrf_memobj_alloc  nrf_memobj.o
    0x0001dfa2   0x0001dfa2   0x00000032   Code   RO         4407    i.nrf_memobj_free   nrf_memobj.o
    0x0001dfd4   0x0001dfd4   0x00000008   Code   RO         4408    i.nrf_memobj_get    nrf_memobj.o
    0x0001dfdc   0x0001dfdc   0x00000004   Code   RO         4409    i.nrf_memobj_pool_init  nrf_memobj.o
    0x0001dfe0   0x0001dfe0   0x0000001e   Code   RO         4410    i.nrf_memobj_put    nrf_memobj.o
    0x0001dffe   0x0001dffe   0x00000010   Code   RO         4411    i.nrf_memobj_read   nrf_memobj.o
    0x0001e00e   0x0001e00e   0x00000010   Code   RO         4412    i.nrf_memobj_write  nrf_memobj.o
    0x0001e01e   0x0001e01e   0x00000002   PAD
    0x0001e020   0x0001e020   0x00000028   Code   RO         4484    i.nrf_pwr_mgmt_init  nrf_pwr_mgmt.o
    0x0001e048   0x0001e048   0x00000044   Code   RO         4485    i.nrf_pwr_mgmt_run  nrf_pwr_mgmt.o
    0x0001e08c   0x0001e08c   0x00000004   Code   RO           11    i.nrf_qwr_error_handler  main.o
    0x0001e090   0x0001e090   0x0000001c   Code   RO         4561    i.nrf_ringbuf_init  nrf_ringbuf.o
    0x0001e0ac   0x0001e0ac   0x00000010   Code   RO         2866    i.nrf_saadc_buffer_init  nrfx_saadc.o
    0x0001e0bc   0x0001e0bc   0x00000014   Code   RO         2867    i.nrf_saadc_channel_input_set  nrfx_saadc.o
    0x0001e0d0   0x0001e0d0   0x00000010   Code   RO         2868    i.nrf_saadc_event_check  nrfx_saadc.o
    0x0001e0e0   0x0001e0e0   0x00000014   Code   RO         2869    i.nrf_saadc_event_clear  nrfx_saadc.o
    0x0001e0f4   0x0001e0f4   0x00000014   Code   RO         5478    i.nrf_sdh_ble_app_ram_start_get  nrf_sdh_ble.o
    0x0001e108   0x0001e108   0x00000128   Code   RO         5479    i.nrf_sdh_ble_default_cfg_set  nrf_sdh_ble.o
    0x0001e230   0x0001e230   0x00000130   Code   RO         5480    i.nrf_sdh_ble_enable  nrf_sdh_ble.o
    0x0001e360   0x0001e360   0x00000060   Code   RO         5481    i.nrf_sdh_ble_evts_poll  nrf_sdh_ble.o
    0x0001e3c0   0x0001e3c0   0x00000074   Code   RO         5360    i.nrf_sdh_enable_request  nrf_sdh.o
    0x0001e434   0x0001e434   0x00000024   Code   RO         5361    i.nrf_sdh_evts_poll  nrf_sdh.o
    0x0001e458   0x0001e458   0x0000000c   Code   RO         5362    i.nrf_sdh_is_enabled  nrf_sdh.o
    0x0001e464   0x0001e464   0x0000003c   Code   RO         5532    i.nrf_sdh_soc_evts_poll  nrf_sdh_soc.o
    0x0001e4a0   0x0001e4a0   0x0000000a   Code   RO         4619    i.nrf_section_iter_init  nrf_section_iter.o
    0x0001e4aa   0x0001e4aa   0x00000024   Code   RO         4620    i.nrf_section_iter_item_set  nrf_section_iter.o
    0x0001e4ce   0x0001e4ce   0x00000020   Code   RO         4621    i.nrf_section_iter_next  nrf_section_iter.o
    0x0001e4ee   0x0001e4ee   0x00000002   PAD
    0x0001e4f0   0x0001e4f0   0x00000038   Code   RO         4654    i.nrf_strerror_find  nrf_strerror.o
    0x0001e528   0x0001e528   0x00000014   Code   RO         4655    i.nrf_strerror_get  nrf_strerror.o
    0x0001e53c   0x0001e53c   0x0000000c   Code   RO         3018    i.nrf_timer_event_clear  nrfx_timer.o
    0x0001e548   0x0001e548   0x0000000a   Code   RO         3235    i.nrf_twim_event_check  nrfx_twim.o
    0x0001e552   0x0001e552   0x0000000c   Code   RO         3236    i.nrf_twim_event_clear  nrfx_twim.o
    0x0001e55e   0x0001e55e   0x0000000a   Code   RO         2336    i.nrf_uart_event_check  nrfx_uart.o
    0x0001e568   0x0001e568   0x0000000c   Code   RO         2337    i.nrf_uart_event_clear  nrfx_uart.o
    0x0001e574   0x0001e574   0x0000000c   Code   RO         2338    i.nrf_uart_int_enable_check  nrfx_uart.o
    0x0001e580   0x0001e580   0x0000000a   Code   RO         2525    i.nrf_uarte_event_check  nrfx_uarte.o
    0x0001e58a   0x0001e58a   0x0000000c   Code   RO         2526    i.nrf_uarte_event_clear  nrfx_uarte.o
    0x0001e596   0x0001e596   0x00000002   PAD
    0x0001e598   0x0001e598   0x0000002c   Code   RO         1877    i.nrfx_clock_enable  nrfx_clock.o
    0x0001e5c4   0x0001e5c4   0x00000020   Code   RO         1880    i.nrfx_clock_init   nrfx_clock.o
    0x0001e5e4   0x0001e5e4   0x0000001c   Code   RO         1883    i.nrfx_clock_lfclk_stop  nrfx_clock.o
    0x0001e600   0x0001e600   0x00000010   Code   RO         3669    i.nrfx_coredep_delay_us  app_timer.o
    0x0001e610   0x0001e610   0x000000a4   Code   RO         2024    i.nrfx_gpiote_in_event_enable  nrfx_gpiote.o
    0x0001e6b4   0x0001e6b4   0x000000d0   Code   RO         2025    i.nrfx_gpiote_in_init  nrfx_gpiote.o
    0x0001e784   0x0001e784   0x00000014   Code   RO         2026    i.nrfx_gpiote_in_is_set  nrfx_gpiote.o
    0x0001e798   0x0001e798   0x0000006c   Code   RO         2028    i.nrfx_gpiote_init  nrfx_gpiote.o
    0x0001e804   0x0001e804   0x00000014   Code   RO         2029    i.nrfx_gpiote_is_init  nrfx_gpiote.o
    0x0001e818   0x0001e818   0x00000010   Code   RO         2527    i.nrfx_is_in_ram    nrfx_uarte.o
    0x0001e828   0x0001e828   0x0000006c   Code   RO         2718    i.nrfx_ppi_channel_alloc  nrfx_ppi.o
    0x0001e894   0x0001e894   0x00000044   Code   RO         2719    i.nrfx_ppi_channel_assign  nrfx_ppi.o
    0x0001e8d8   0x0001e8d8   0x00000034   Code   RO         2721    i.nrfx_ppi_channel_enable  nrfx_ppi.o
    0x0001e90c   0x0001e90c   0x0000003a   Code   RO         2278    i.nrfx_prs_acquire  nrfx_prs.o
    0x0001e946   0x0001e946   0x00000002   PAD
    0x0001e948   0x0001e948   0x000000a4   Code   RO         2873    i.nrfx_saadc_buffer_convert  nrfx_saadc.o
    0x0001e9ec   0x0001e9ec   0x000000ac   Code   RO         2875    i.nrfx_saadc_channel_init  nrfx_saadc.o
    0x0001ea98   0x0001ea98   0x00000094   Code   RO         2877    i.nrfx_saadc_init   nrfx_saadc.o
    0x0001eb2c   0x0001eb2c   0x0000001c   Code   RO         2882    i.nrfx_saadc_sample_task_get  nrfx_saadc.o
    0x0001eb48   0x0001eb48   0x0000003a   Code   RO         3021    i.nrfx_timer_compare  nrfx_timer.o
    0x0001eb82   0x0001eb82   0x00000002   PAD
    0x0001eb84   0x0001eb84   0x0000001c   Code   RO         3025    i.nrfx_timer_enable  nrfx_timer.o
    0x0001eba0   0x0001eba0   0x0000002a   Code   RO         3026    i.nrfx_timer_extended_compare  nrfx_timer.o
    0x0001ebca   0x0001ebca   0x00000002   PAD
    0x0001ebcc   0x0001ebcc   0x000000bc   Code   RO         3028    i.nrfx_timer_init   nrfx_timer.o
    0x0001ec88   0x0001ec88   0x00000010   Code   RO         2339    i.nrfx_uart_0_irq_handler  nrfx_uart.o
    0x0001ec98   0x0001ec98   0x000000d0   Code   RO         2341    i.nrfx_uart_init    nrfx_uart.o
    0x0001ed68   0x0001ed68   0x000000ec   Code   RO         2342    i.nrfx_uart_rx      nrfx_uart.o
    0x0001ee54   0x0001ee54   0x000000a4   Code   RO         2347    i.nrfx_uart_tx      nrfx_uart.o
    0x0001eef8   0x0001eef8   0x00000020   Code   RO         2349    i.nrfx_uart_tx_in_progress  nrfx_uart.o
    0x0001ef18   0x0001ef18   0x00000010   Code   RO         2528    i.nrfx_uarte_0_irq_handler  nrfx_uarte.o
    0x0001ef28   0x0001ef28   0x0000006c   Code   RO         2530    i.nrfx_uarte_init   nrfx_uarte.o
    0x0001ef94   0x0001ef94   0x00000104   Code   RO         2531    i.nrfx_uarte_rx     nrfx_uarte.o
    0x0001f098   0x0001f098   0x00000090   Code   RO         2534    i.nrfx_uarte_tx     nrfx_uarte.o
    0x0001f128   0x0001f128   0x0000001c   Code   RO         2536    i.nrfx_uarte_tx_in_progress  nrfx_uarte.o
    0x0001f144   0x0001f144   0x00000100   Code   RO           12    i.nus_data_handler  main.o
    0x0001f244   0x0001f244   0x00000030   Code   RO           13    i.on_adv_evt        main.o
    0x0001f274   0x0001f274   0x0000001c   Code   RO           14    i.on_conn_params_evt  main.o
    0x0001f290   0x0001f290   0x0000006a   Code   RO         1478    i.on_connect        ble_nus.o
    0x0001f2fa   0x0001f2fa   0x00000002   PAD
    0x0001f2fc   0x0001f2fc   0x0000008c   Code   RO         1365    i.on_connected_evt  nrf_ble_gatt.o
    0x0001f388   0x0001f388   0x000000b0   Code   RO         1366    i.on_exchange_mtu_request_evt  nrf_ble_gatt.o
    0x0001f438   0x0001f438   0x00000084   Code   RO         1479    i.on_write          ble_nus.o
    0x0001f4bc   0x0001f4bc   0x00000012   Code   RO          945    i.phy_is_valid      ble_advertising.o
    0x0001f4ce   0x0001f4ce   0x00000002   PAD
    0x0001f4d0   0x0001f4d0   0x00000018   Code   RO         2045    i.pin_in_use_by_port  nrfx_gpiote.o
    0x0001f4e8   0x0001f4e8   0x00000018   Code   RO         2046    i.pin_in_use_by_te  nrfx_gpiote.o
    0x0001f500   0x0001f500   0x0000003c   Code   RO         5050    i.postfix_process   nrf_log_str_formatter.o
    0x0001f53c   0x0001f53c   0x00000098   Code   RO         5051    i.prefix_process    nrf_log_str_formatter.o
    0x0001f5d4   0x0001f5d4   0x00000018   Code   RO         2280    i.prs_box_get       nrfx_prs.o
    0x0001f5ec   0x0001f5ec   0x0000003c   Code   RO         3670    i.rtc1_stop         app_timer.o
    0x0001f628   0x0001f628   0x00000032   Code   RO         2351    i.rx_byte           nrfx_uart.o
    0x0001f65a   0x0001f65a   0x00000016   Code   RO         2352    i.rx_done_event     nrfx_uart.o
    0x0001f670   0x0001f670   0x00000016   Code   RO         2538    i.rx_done_event     nrfx_uarte.o
    0x0001f686   0x0001f686   0x00000020   Code   RO         2353    i.rx_enable         nrfx_uart.o
    0x0001f6a6   0x0001f6a6   0x00000002   PAD
    0x0001f6a8   0x0001f6a8   0x00000118   Code   RO           15    i.saadc_callback    main.o
    0x0001f7c0   0x0001f7c0   0x0000006c   Code   RO           16    i.saadc_init        main.o
    0x0001f82c   0x0001f82c   0x0000001c   Code   RO           17    i.saadc_sampling_event_enable  main.o
    0x0001f848   0x0001f848   0x00000098   Code   RO           18    i.saadc_sampling_event_init  main.o
    0x0001f8e0   0x0001f8e0   0x00000050   Code   RO         1548    i.sd_state_evt_handler  nrf_drv_clock.o
    0x0001f930   0x0001f930   0x00000030   Code   RO         5367    i.sdh_request_observer_notify  nrf_sdh.o
    0x0001f960   0x0001f960   0x0000002c   Code   RO         5368    i.sdh_state_observer_notify  nrf_sdh.o
    0x0001f98c   0x0001f98c   0x00000010   Code   RO         1040    i.send_error_evt    ble_conn_params.o
    0x0001f99c   0x0001f99c   0x00000050   Code   RO         4729    i.serial_tx         nrf_log_backend_rtt.o
    0x0001f9ec   0x0001f9ec   0x00000088   Code   RO          832    i.service_data_encode  ble_advdata.o
    0x0001fa74   0x0001fa74   0x00000030   Code   RO         1303    i.set_security_req  ble_srv_common.o
    0x0001faa4   0x0001faa4   0x00000018   Code   RO         1549    i.soc_evt_handler   nrf_drv_clock.o
    0x0001fabc   0x0001fabc   0x00000058   Code   RO         5370    i.softdevices_evt_irq_enable  nrf_sdh.o
    0x0001fb14   0x0001fb14   0x0000008c   Code   RO         4886    i.std_n             nrf_log_frontend.o
    0x0001fba0   0x0001fba0   0x00000002   Code   RO           19    i.timer_handler     main.o
    0x0001fba2   0x0001fba2   0x00000002   PAD
    0x0001fba4   0x0001fba4   0x00000080   Code   RO         3671    i.timer_list_handler  app_timer.o
    0x0001fc24   0x0001fc24   0x0000003c   Code   RO         3672    i.timer_list_insert  app_timer.o
    0x0001fc60   0x0001fc60   0x00000060   Code   RO         3673    i.timer_list_remove  app_timer.o
    0x0001fcc0   0x0001fcc0   0x00000048   Code   RO         3674    i.timer_stop_op_schedule  app_timer.o
    0x0001fd08   0x0001fd08   0x00000074   Code   RO         3675    i.timer_timeouts_check  app_timer.o
    0x0001fd7c   0x0001fd7c   0x0000014c   Code   RO         3248    i.twim_irq_handler  nrfx_twim.o
    0x0001fec8   0x0001fec8   0x00000020   Code   RO         2354    i.tx_byte           nrfx_uart.o
    0x0001fee8   0x0001fee8   0x0000001a   Code   RO         2355    i.tx_done_event     nrfx_uart.o
    0x0001ff02   0x0001ff02   0x00000002   PAD
    0x0001ff04   0x0001ff04   0x00000078   Code   RO           20    i.uart_event_handle  main.o
    0x0001ff7c   0x0001ff7c   0x000000a0   Code   RO         3825    i.uart_event_handler  app_uart_fifo.o
    0x0002001c   0x0002001c   0x00000030   Code   RO         1680    i.uart_evt_handler  nrf_drv_uart.o
    0x0002004c   0x0002004c   0x00000128   Code   RO         2356    i.uart_irq_handler  nrfx_uart.o
    0x00020174   0x00020174   0x00000030   Code   RO         1681    i.uarte_evt_handler  nrf_drv_uart.o
    0x000201a4   0x000201a4   0x000000f2   Code   RO         2539    i.uarte_irq_handler  nrfx_uarte.o
    0x00020296   0x00020296   0x0000000a   Code   RO          833    i.uint16_encode     ble_advdata.o
    0x000202a0   0x000202a0   0x000000b4   Code   RO         4368    i.unsigned_print    nrf_fprintf_format.o
    0x00020354   0x00020354   0x00000068   Code   RO         1041    i.update_timeout_handler  ble_conn_params.o
    0x000203bc   0x000203bc   0x00000018   Code   RO          946    i.use_whitelist     ble_advertising.o
    0x000203d4   0x000203d4   0x00000024   Code   RO         1437    i.user_mem_reply    nrf_ble_qwr.o
    0x000203f8   0x000203f8   0x00000030   Code   RO         3676    i.user_op_alloc     app_timer.o
    0x00020428   0x00020428   0x00000030   Code   RO          834    i.uuid_list_encode  ble_advdata.o
    0x00020458   0x00020458   0x0000009e   Code   RO          835    i.uuid_list_sized_encode  ble_advdata.o
    0x000204f6   0x000204f6   0x0000003a   Code   RO          609    i.wakeup_button_cfg  bsp.o
    0x00020530   0x00020530   0x00000049   Data   RO           22    .constdata          main.o
    0x00020579   0x00020579   0x00000008   Data   RO          470    .constdata          boards.o
    0x00020581   0x00020581   0x00000003   PAD
    0x00020584   0x00020584   0x0000002c   Data   RO          614    .constdata          bsp.o
    0x000205b0   0x000205b0   0x0000000e   Data   RO         1367    .constdata          nrf_ble_gatt.o
    0x000205be   0x000205be   0x00000002   PAD
    0x000205c0   0x000205c0   0x00000010   Data   RO         1480    .constdata          ble_nus.o
    0x000205d0   0x000205d0   0x00000004   Data   RO         2048    .constdata          nrfx_gpiote.o
    0x000205d4   0x000205d4   0x00000004   Data   RO         2359    .constdata          nrfx_uart.o
    0x000205d8   0x000205d8   0x00000004   Data   RO         2542    .constdata          nrfx_uarte.o
    0x000205dc   0x000205dc   0x00000008   Data   RO         3379    .constdata          app_button.o
    0x000205e4   0x000205e4   0x0000000c   PAD
    0x000205f0   0x000205f0   0x00000006   Data   RO         3678    .constdata          app_timer.o
    0x000205f6   0x000205f6   0x00000002   PAD
    0x000205f8   0x000205f8   0x00000020   Data   RO         3827    .constdata          app_uart_fifo.o
    0x00020618   0x00020618   0x00000010   Data   RO         4369    .constdata          nrf_fprintf_format.o
    0x00020628   0x00020628   0x00000018   Data   RO         4489    .constdata          nrf_pwr_mgmt.o
    0x00020640   0x00020640   0x0000000c   Data   RO         4490    .constdata          nrf_pwr_mgmt.o
    0x0002064c   0x0002064c   0x0000013c   Data   RO         4656    .constdata          nrf_strerror.o
    0x00020788   0x00020788   0x0000000c   Data   RO         4731    .constdata          nrf_log_backend_rtt.o
    0x00020794   0x00020794   0x0000000c   PAD
    0x000207a0   0x000207a0   0x00000006   Data   RO         4732    .constdata          nrf_log_backend_rtt.o
    0x000207a6   0x000207a6   0x00000002   PAD
    0x000207a8   0x000207a8   0x0000000c   Data   RO         4891    .constdata          nrf_log_frontend.o
    0x000207b4   0x000207b4   0x00000010   Data   RO         5371    .constdata          nrf_sdh.o
    0x000207c4   0x000207c4   0x00000028   Data   RO         5372    .constdata          nrf_sdh.o
    0x000207ec   0x000207ec   0x00000010   Data   RO         5373    .constdata          nrf_sdh.o
    0x000207fc   0x000207fc   0x00000010   Data   RO         5374    .constdata          nrf_sdh.o
    0x0002080c   0x0002080c   0x00000020   Data   RO         5482    .constdata          nrf_sdh_ble.o
    0x0002082c   0x0002082c   0x00000010   Data   RO         5483    .constdata          nrf_sdh_ble.o
    0x0002083c   0x0002083c   0x00000010   Data   RO         5533    .constdata          nrf_sdh_soc.o
    0x0002084c   0x0002084c   0x0000000c   Data   RO         5534    .constdata          nrf_sdh_soc.o
    0x00020858   0x00020858   0x00000081   Data   RO         5617    .constdata          mc_w.l(ctype_o.o)
    0x000208d9   0x000208d9   0x00000003   PAD
    0x000208dc   0x000208dc   0x00000004   Data   RO         5618    .constdata          mc_w.l(ctype_o.o)
    0x000208e0   0x000208e0   0x000003eb   Data   RO         4657    .conststring        nrf_strerror.o
    0x00020ccb   0x00020ccb   0x00000001   PAD
    0x00020ccc   0x00020ccc   0x00000066   Data   RO         5052    .conststring        nrf_log_str_formatter.o
    0x00020d32   0x00020d32   0x00000002   PAD
    0x00020d34   0x00020d34   0x000001cf   Data   RO         5484    .conststring        nrf_sdh_ble.o
    0x00020f03   0x00020f03   0x00000001   PAD
    0x00020f04   0x00020f04   0x0000000d   Data   RO         1368    .conststrlit        nrf_ble_gatt.o
    0x00020f11   0x00020f11   0x00000003   PAD
    0x00020f14   0x00020f14   0x00000008   Data   RO         1481    .conststrlit        ble_nus.o
    0x00020f1c   0x00020f1c   0x00000006   Data   RO         1555    .conststrlit        nrf_drv_clock.o
    0x00020f22   0x00020f22   0x00000002   PAD
    0x00020f24   0x00020f24   0x00000006   Data   RO         1887    .conststrlit        nrfx_clock.o
    0x00020f2a   0x00020f2a   0x00000002   PAD
    0x00020f2c   0x00020f2c   0x00000007   Data   RO         2052    .conststrlit        nrfx_gpiote.o
    0x00020f33   0x00020f33   0x00000001   PAD
    0x00020f34   0x00020f34   0x00000004   Data   RO         2282    .conststrlit        nrfx_prs.o
    0x00020f38   0x00020f38   0x00000005   Data   RO         2362    .conststrlit        nrfx_uart.o
    0x00020f3d   0x00020f3d   0x00000003   PAD
    0x00020f40   0x00020f40   0x00000006   Data   RO         2545    .conststrlit        nrfx_uarte.o
    0x00020f46   0x00020f46   0x00000002   PAD
    0x00020f48   0x00020f48   0x00000004   Data   RO         2743    .conststrlit        nrfx_ppi.o
    0x00020f4c   0x00020f4c   0x00000006   Data   RO         2893    .conststrlit        nrfx_saadc.o
    0x00020f52   0x00020f52   0x00000002   PAD
    0x00020f54   0x00020f54   0x00000006   Data   RO         3035    .conststrlit        nrfx_timer.o
    0x00020f5a   0x00020f5a   0x00000002   PAD
    0x00020f5c   0x00020f5c   0x00000005   Data   RO         3255    .conststrlit        nrfx_twim.o
    0x00020f61   0x00020f61   0x00000003   PAD
    0x00020f64   0x00020f64   0x00000009   Data   RO         4491    .conststrlit        nrf_pwr_mgmt.o
    0x00020f6d   0x00020f6d   0x00000003   PAD
    0x00020f70   0x00020f70   0x00000010   Data   RO         4826    .conststrlit        nrf_log_default_backends.o
    0x00020f80   0x00020f80   0x00000004   Data   RO         4892    .conststrlit        nrf_log_frontend.o
    0x00020f84   0x00020f84   0x00000008   Data   RO         5375    .conststrlit        nrf_sdh.o
    0x00020f8c   0x00020f8c   0x0000000c   Data   RO         5485    .conststrlit        nrf_sdh_ble.o
    0x00020f98   0x00020f98   0x0000000c   Data   RO         5535    .conststrlit        nrf_sdh_soc.o
    0x00020fa4   0x00020fa4   0x00000020   Data   RO         5954    Region$$Table       anon$$obj.o
    0x00020fc4   0x00020fc4   0x00000010   Data   RO         4828    log_backends        nrf_log_default_backends.o
    0x00020fd4   0x00020fd4   0x00000008   Data   RO         1369    log_const_data      nrf_ble_gatt.o
    0x00020fdc   0x00020fdc   0x00000008   Data   RO         1482    log_const_data      ble_nus.o
    0x00020fe4   0x00020fe4   0x00000008   Data   RO         1556    log_const_data      nrf_drv_clock.o
    0x00020fec   0x00020fec   0x00000008   Data   RO         1889    log_const_data      nrfx_clock.o
    0x00020ff4   0x00020ff4   0x00000008   Data   RO         2053    log_const_data      nrfx_gpiote.o
    0x00020ffc   0x00020ffc   0x00000008   Data   RO         2284    log_const_data      nrfx_prs.o
    0x00021004   0x00021004   0x00000008   Data   RO         2363    log_const_data      nrfx_uart.o
    0x0002100c   0x0002100c   0x00000008   Data   RO         2546    log_const_data      nrfx_uarte.o
    0x00021014   0x00021014   0x00000008   Data   RO         2745    log_const_data      nrfx_ppi.o
    0x0002101c   0x0002101c   0x00000008   Data   RO         2894    log_const_data      nrfx_saadc.o
    0x00021024   0x00021024   0x00000008   Data   RO         3036    log_const_data      nrfx_timer.o
    0x0002102c   0x0002102c   0x00000008   Data   RO         3256    log_const_data      nrfx_twim.o
    0x00021034   0x00021034   0x00000008   Data   RO         4493    log_const_data      nrf_pwr_mgmt.o
    0x0002103c   0x0002103c   0x00000008   Data   RO         4895    log_const_data      nrf_log_frontend.o
    0x00021044   0x00021044   0x00000008   Data   RO         5377    log_const_data      nrf_sdh.o
    0x0002104c   0x0002104c   0x00000008   Data   RO         5487    log_const_data      nrf_sdh_ble.o
    0x00021054   0x00021054   0x00000008   Data   RO         5536    log_const_data      nrf_sdh_soc.o
    0x0002105c   0x0002105c   0x00000014   Data   RO         4896    nrf_balloc          nrf_log_frontend.o
    0x00021070   0x00021070   0x00000008   Data   RO         1135    sdh_ble_observers0  ble_conn_state.o
    0x00021078   0x00021078   0x00000010   Data   RO           27    sdh_ble_observers1  main.o
    0x00021088   0x00021088   0x00000008   Data   RO          717    sdh_ble_observers1  bsp_btn_ble.o
    0x00021090   0x00021090   0x00000008   Data   RO         1044    sdh_ble_observers1  ble_conn_params.o
    0x00021098   0x00021098   0x00000010   Data   RO           28    sdh_ble_observers2  main.o
    0x000210a8   0x000210a8   0x00000008   Data   RO           29    sdh_ble_observers3  main.o
    0x000210b0   0x000210b0   0x00000008   Data   RO         1557    sdh_soc_observers0  nrf_drv_clock.o
    0x000210b8   0x000210b8   0x00000008   Data   RO           30    sdh_soc_observers1  main.o
    0x000210c0   0x000210c0   0x00000008   Data   RO         5488    sdh_stack_observers0  nrf_sdh_ble.o
    0x000210c8   0x000210c8   0x00000008   Data   RO         5537    sdh_stack_observers0  nrf_sdh_soc.o
    0x000210d0   0x000210d0   0x00000008   Data   RO         1558    sdh_state_observers0  nrf_drv_clock.o


    Execution Region RW_IRAM1 (Exec base: 0x20002500, Load base: 0x000210d8, Size: 0x00001938, Max: 0x0000db00, ABSOLUTE, COMPRESSED[0x00000054])

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x20002500   COMPRESSED   0x00000034   Data   RW           23    .data               main.o
    0x20002534   COMPRESSED   0x00000008   Data   RW           24    .data               main.o
    0x2000253c   COMPRESSED   0x00000004   Data   RW           26    .data               main.o
    0x20002540   COMPRESSED   0x00000010   Data   RW          615    .data               bsp.o
    0x20002550   COMPRESSED   0x00000008   Data   RW          716    .data               bsp_btn_ble.o
    0x20002558   COMPRESSED   0x00000008   Data   RW         1043    .data               ble_conn_params.o
    0x20002560   COMPRESSED   0x0000000c   Data   RW         1682    .data               nrf_drv_uart.o
    0x2000256c   COMPRESSED   0x00000008   Data   RW         1888    .data               nrfx_clock.o
    0x20002574   COMPRESSED   0x00000008   Data   RW         2283    .data               nrfx_prs.o
    0x2000257c   COMPRESSED   0x00000001   Data   RW         2676    .data               nrf_drv_ppi.o
    0x2000257d   COMPRESSED   0x00000003   PAD
    0x20002580   COMPRESSED   0x00000008   Data   RW         2744    .data               nrfx_ppi.o
    0x20002588   COMPRESSED   0x00000020   Data   RW         3380    .data               app_button.o
    0x200025a8   COMPRESSED   0x00000014   Data   RW         3679    .data               app_timer.o
    0x200025bc   COMPRESSED   0x0000001c   Data   RW         3828    .data               app_uart_fifo.o
    0x200025d8   COMPRESSED   0x00000008   Data   RW         4492    .data               nrf_pwr_mgmt.o
    0x200025e0   COMPRESSED   0x00000004   Data   RW         4689    .data               retarget.o
    0x200025e4   COMPRESSED   0x00000001   Data   RW         4733    .data               nrf_log_backend_rtt.o
    0x200025e5   COMPRESSED   0x00000003   PAD
    0x200025e8   COMPRESSED   0x00000008   Data   RW         4827    .data               nrf_log_default_backends.o
    0x200025f0   COMPRESSED   0x00000008   Data   RW         4893    .data               nrf_log_frontend.o
    0x200025f8   COMPRESSED   0x00000008   Data   RW         4894    .data               nrf_log_frontend.o
    0x20002600   COMPRESSED   0x00000040   Data   RW         5053    .data               nrf_log_str_formatter.o
    0x20002640   COMPRESSED   0x00000003   Data   RW         5376    .data               nrf_sdh.o
    0x20002643   COMPRESSED   0x00000001   Data   RW         5486    .data               nrf_sdh_ble.o
    0x20002644   COMPRESSED   0x00000004   Data   RW         5576    .data               system_nrf52.o
    0x20002648        -       0x000003dd   Zero   RW           21    .bss                main.o
    0x20002a25   COMPRESSED   0x00000003   PAD
    0x20002a28        -       0x00000020   Zero   RW          610    .bss                bsp.o
    0x20002a48        -       0x00000020   Zero   RW          611    .bss                bsp.o
    0x20002a68        -       0x0000000c   Zero   RW          612    .bss                bsp.o
    0x20002a74        -       0x00000020   Zero   RW          613    .bss                bsp.o
    0x20002a94        -       0x00000050   Zero   RW         1042    .bss                ble_conn_params.o
    0x20002ae4        -       0x00000078   Zero   RW         1134    .bss                ble_conn_state.o
    0x20002b5c        -       0x00000014   Zero   RW         1550    .bss                nrf_drv_clock.o
    0x20002b70        -       0x0000005c   Zero   RW         2047    .bss                nrfx_gpiote.o
    0x20002bcc        -       0x0000002c   Zero   RW         2357    .bss                nrfx_uart.o
    0x20002bf8        -       0x00000024   Zero   RW         2540    .bss                nrfx_uarte.o
    0x20002c1c        -       0x00000030   Zero   RW         2884    .bss                nrfx_saadc.o
    0x20002c4c        -       0x0000000c   Zero   RW         3033    .bss                nrfx_timer.o
    0x20002c58        -       0x00000034   Zero   RW         3250    .bss                nrfx_twim.o
    0x20002c8c        -       0x00000020   Zero   RW         3378    .bss                app_button.o
    0x20002cac        -       0x0000010c   Zero   RW         3677    .bss                app_timer.o
    0x20002db8        -       0x00000020   Zero   RW         3826    .bss                app_uart_fifo.o
    0x20002dd8        -       0x0000000c   Zero   RW         3907    .bss                app_util_platform.o
    0x20002de4        -       0x0000000c   Zero   RW         4488    .bss                nrf_pwr_mgmt.o
    0x20002df0        -       0x00000040   Zero   RW         4730    .bss                nrf_log_backend_rtt.o
    0x20002e30        -       0x000000c0   Zero   RW         4887    .bss                nrf_log_frontend.o
    0x20002ef0        -       0x00000080   Zero   RW         4888    .bss                nrf_log_frontend.o
    0x20002f70        -       0x00000018   Zero   RW         4889    .bss                nrf_log_frontend.o
    0x20002f88        -       0x00000424   Zero   RW         4890    .bss                nrf_log_frontend.o
    0x200033ac        -       0x00000288   Zero   RW         5129    .bss                segger_rtt.o
    0x20003634   COMPRESSED   0x00000004   PAD
    0x20003638        -       0x00000800   Zero   RW         5564    STACK               arm_startup_nrf52.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

       444         38          8         32         32      13154   app_button.o
        22          0          0          0          0       2457   app_error.o
       132         46          0          0          0      30581   app_error_weak.o
       118          0          0          0          0       5026   app_fifo.o
      1510        118          6         20        268      47923   app_timer.o
       524         60         32         28         32      21266   app_uart_fifo.o
       124         14          0          0         12       9606   app_util_platform.o
        36          8        512          0       2048        928   arm_startup_nrf52.o
      1324          0          0          0          0      53684   ble_advdata.o
      1002          6          0          0          0      12556   ble_advertising.o
       636         44          8          8         80       9263   ble_conn_params.o
       360         10          8          0        120       6915   ble_conn_state.o
        72          0          0          0          0       1652   ble_link_ctx_manager.o
       664          6         32          0          0       6964   ble_nus.o
       456          6          0          0          0       3379   ble_srv_common.o
       358         40          8          0          0      48943   boards.o
       994         84         44         16        108      15635   bsp.o
       252         10          8          8          0       9260   bsp_btn_ble.o
      2150        442        121         64        989     197203   main.o
        64          0          0          0          0       2972   nrf_atflags.o
       306          0          0          0          0       8039   nrf_atomic.o
       164          0          0          0          0       3640   nrf_balloc.o
       634        186         35          0          0       8465   nrf_ble_gatt.o
       276          0          0          0          0       4713   nrf_ble_qwr.o
       276         34         30          0         20      37764   nrf_drv_clock.o
        24          6          0          1          0        967   nrf_drv_ppi.o
       200         26          0         12          0      17884   nrf_drv_uart.o
        50          0          0          0          0       3541   nrf_fprintf.o
       866          4         16          0          0       5518   nrf_fprintf_format.o
       112         18         18          1         64       5637   nrf_log_backend_rtt.o
       200          0          0          0          0      10869   nrf_log_backend_serial.o
        28          4         32          8          0       3349   nrf_log_default_backends.o
      1474        114         44         16       1404      29770   nrf_log_frontend.o
       570        108        102         64          0       5668   nrf_log_str_formatter.o
       346          0          0          0          0       9587   nrf_memobj.o
       108         16         53          8         12      36366   nrf_pwr_mgmt.o
        28          0          0          0          0       2375   nrf_ringbuf.o
       384         46        104          3          0      39255   nrf_sdh.o
       716        232        539          1          0       5929   nrf_sdh_ble.o
        60          4         56          0          0       2476   nrf_sdh_soc.o
        78          0          0          0          0       2788   nrf_section_iter.o
        76         10       1319          0          0       2751   nrf_strerror.o
       222         30         14          8          0      43654   nrfx_clock.o
      1222         92         19          0         92      59399   nrfx_gpiote.o
       286         22         12          8          0      11789   nrfx_ppi.o
        94         16         12          8          0       3777   nrfx_prs.o
       912         74         14          0         48      18799   nrfx_saadc.o
       408         18         14          0         12      14488   nrfx_timer.o
       370         12         13          0         52      12927   nrfx_twim.o
      1358         36         17          0         44      30221   nrfx_uart.o
      1192         38         18          0         36      24271   nrfx_uarte.o
        14          0          0          4          0       2878   retarget.o
       378         34          0          0        648       9017   segger_rtt.o
       796         70          0          4          0       2951   system_nrf52.o

    ----------------------------------------------------------------------
     25524       2182       3360        328       6128     980889   Object Totals
         0          0         32          0          0          0   (incl. Generated)
        54          0         60          6          7          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

        86          0          0          0          0          0   __dczerorl2.o
         8          4        133          0          0         68   ctype_o.o
         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        30          0          0          0          0          0   handlers.o
        36          8          0          0          0         68   init.o
         0          0          0          0          0          0   iusefp.o
        30          0          0          0          0         68   llshl.o
        36          0          0          0          0         68   llsshr.o
        32          0          0          0          0         68   llushr.o
        36          0          0          0          0         68   memcpya.o
        36          0          0          0          0        108   memseta.o
      2308         96          0          0          0        604   printfa.o
        24          0          0          0          0         68   strcat.o
        18          0          0          0          0         68   strcpy.o
        14          0          0          0          0         68   strlen.o
        44          0          0          0          0         80   uidiv.o
        98          0          0          0          0         92   uldiv.o
        48          0          0          0          0         68   cdrcmple.o
       334          0          0          0          0        148   dadd.o
       222          0          0          0          0        100   ddiv.o
       186          0          0          0          0        176   depilogue.o
        48          0          0          0          0         68   dfixul.o
       228          0          0          0          0         96   dmul.o
        38          0          0          0          0         68   f2d.o

    ----------------------------------------------------------------------
      3964        116        136          0          0       2220   Library Totals
         4          0          3          0          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

      2856        116        133          0          0       1496   mc_w.l
      1104          0          0          0          0        724   mf_w.l

    ----------------------------------------------------------------------
      3964        116        136          0          0       2220   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     29488       2298       3496        328       6128     951249   Grand Totals
     29488       2298       3496         84       6128     951249   ELF Image Totals (compressed)
     29488       2298       3496         84          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                32984 (  32.21kB)
    Total RW  Size (RW Data + ZI Data)              6456 (   6.30kB)
    Total ROM Size (Code + RO Data + RW Data)      33068 (  32.29kB)

==============================================================================

