# Static Call Graph for image .\_build\ble_app_proximity.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 76]: Last Updated: Sat Dec 07 00:36:33 2013

### Maximum Stack Usage = 392 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

ble_evt_dispatch ⇒ on_ble_evt ⇒ advertising_start ⇒ advertising_init ⇒ ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- SVC_Handler ⇒ SVC_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- CCM_AAR_IRQHandler ⇒ CCM_AAR_IRQHandler
- __asm___11_app_timer_c_cd27f9c3__nrf_delay_us ⇒ __asm___11_app_timer_c_cd27f9c3__nrf_delay_us

  ### Function Pointers

  - ADC_IRQHandler from main.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - CCM_AAR_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - ECB_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - GPIOTE_IRQHandler from app_gpiote.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - HardFault_Handler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - LPCOMP_COMP_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - NMI_Handler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - POWER_CLOCK_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - PendSV_Handler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - QDEC_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - RADIO_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - RNG_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - RTC0_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - RTC1_IRQHandler from app_timer.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - Reset_Handler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SPI0_TWI0_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SPI1_TWI1_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SVC_Handler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SWI0_IRQHandler from app_timer.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SWI1_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SWI2_IRQHandler from softdevice_handler.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SWI3_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SWI4_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SWI5_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SysTick_Handler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - SystemInit from system_nrf51.o(.text) referenced from arm_startup_nrf51.o(.text)
  - TEMP_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - TIMER0_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - TIMER1_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - TIMER2_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - UART0_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - WDT_IRQHandler from arm_startup_nrf51.o(.text) referenced from arm_startup_nrf51.o(RESET)
  - __main from __main.o(!!!main) referenced from arm_startup_nrf51.o(.text)
  - adv_led_blink_timeout_handler from main.o(.text) referenced from main.o(.text)
  - battery_level_meas_timeout_handler from main.o(.text) referenced from main.o(.text)
  - ble_evt_dispatch from main.o(.text) referenced from main.o(.text)
  - bm_pstorage_cb_handler from ble_bondmngr.o(.text) referenced from ble_bondmngr.o(.text)
  - bond_manager_error_handler from main.o(.text) referenced from main.o(.text)
  - button_event_handler from main.o(.text) referenced 2 times from main.o(.data)
  - conn_params_error_handler from main.o(.text) referenced from main.o(.text)
  - detection_delay_timeout_handler from app_button.o(.text) referenced from app_button.o(.text)
  - gpiote_event_handler from app_button.o(.text) referenced from app_button.o(.text)
  - mild_alert_timeout_handler from main.o(.text) referenced from main.o(.text)
  - on_bas_evt from main.o(.text) referenced from main.o(.text)
  - on_ias_c_evt from main.o(.text) referenced from main.o(.text)
  - on_ias_evt from main.o(.text) referenced from main.o(.text)
  - on_lls_evt from main.o(.text) referenced from main.o(.text)
  - service_error_handler from main.o(.text) referenced 2 times from main.o(.text)
  - softdevice_assertion_handler from softdevice_handler.o(.text) referenced from softdevice_handler.o(.text)
  - sys_evt_dispatch from main.o(.text) referenced from main.o(.text)
  - update_timeout_handler from ble_conn_params.o(.text) referenced from ble_conn_params.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 52 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000001))

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000031))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 368 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ advertising_start ⇒ advertising_init ⇒ ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  __asm___11_app_timer_c_cd27f9c3__nrf_delay_us (Thumb, 30 bytes, Stack size 0 bytes, app_timer.o(.emb_text))
  [Calls]

  - >> __asm___11_app_timer_c_cd27f9c3__nrf_delay_us
  [Called By]
  - >> __asm___11_app_timer_c_cd27f9c3__nrf_delay_us
  - >> rtc1_stop
  - >> rtc1_start

  __aeabi_memcpy4 (Thumb, 56 bytes, Stack size 0 bytes, rt_memcpy.o(.emb_text))
  [Called By]

  - >> ble_conn_params_init
  - >> __aeabi_memcpy
  - >> ble_bondmngr_bonded_central_delete
  - >> ble_bondmngr_sys_attr_store
  - >> auth_status_update
  - >> on_connect
  - >> load_all_from_flash
  - >> central_find_in_db
  - >> central_update
  - >> on_auth_status_from_new_central

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, rt_memcpy.o(.emb_text), UNUSED)

  Reset_Handler (Thumb, 18 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  CCM_AAR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Calls]

  - >> CCM_AAR_IRQHandler
  [Called By]
  - >> CCM_AAR_IRQHandler
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  ECB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  LPCOMP_COMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  POWER_CLOCK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  QDEC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  RADIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  RTC0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  SPI0_TWI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  SPI1_TWI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  SWI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  SWI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  SWI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  SWI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  TEMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  TIMER0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  TIMER1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  TIMER2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf51.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf51.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, arm_startup_nrf51.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  SystemCoreClockUpdate (Thumb, 8 bytes, Stack size 0 bytes, system_nrf51.o(.text), UNUSED)

  SystemInit (Thumb, 38 bytes, Stack size 8 bytes, system_nrf51.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SystemInit
  [Calls]
  - >> is_manual_peripheral_setup_needed
  - >> is_disabled_in_debug_needed
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(.text)

  app_error_handler (Thumb, 22 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> timeout_handler_exec
  - >> ble_srv_report_ref_encode
  - >> ADC_IRQHandler
  - >> assert_nrf_callback
  - >> power_manage
  - >> buttons_init
  - >> gpiote_init
  - >> button_event_handler
  - >> bond_manager_init
  - >> bond_manager_error_handler
  - >> ble_stack_init
  - >> on_ble_evt
  - >> conn_params_init
  - >> conn_params_error_handler
  - >> ias_client_init
  - >> on_ias_c_evt
  - >> bas_init
  - >> on_bas_evt
  - >> lls_init
  - >> ias_init
  - >> tps_init
  - >> gap_params_init
  - >> timers_init
  - >> adv_led_blink_timeout_handler
  - >> mild_alert_timeout_handler
  - >> advertising_start
  - >> advertising_init
  - >> alert_led_blink_stop
  - >> alert_led_blink_start
  - >> adv_led_blink_stop
  - >> adv_led_blink_start
  - >> adc_start
  - >> service_error_handler
  - >> button_handler_execute
  - >> SWI2_IRQHandler
  - >> intern_softdevice_events_execute

  assert_nrf_callback (Thumb, 14 bytes, Stack size 0 bytes, main.o(.text))
  [Calls]

  - >> app_error_handler
  [Called By]
  - >> softdevice_assertion_handler

  ADC_IRQHandler (Thumb, 106 bytes, Stack size 24 bytes, main.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = ADC_IRQHandler ⇒ ble_bas_battery_level_update
  [Calls]
  - >> ble_bas_battery_level_update
  - >> app_error_handler
  - >> battery_level_in_percent
  - >> __aeabi_idivmod
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  main (Thumb, 58 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 368
  - Call Chain = main ⇒ advertising_start ⇒ advertising_init ⇒ ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> power_manage
  - >> buttons_init
  - >> gpiote_init
  - >> bond_manager_init
  - >> ble_stack_init
  - >> conn_params_init
  - >> sec_params_init
  - >> services_init
  - >> gap_params_init
  - >> timers_init
  - >> leds_init
  - >> advertising_start
  - >> advertising_init
  [Called By]
  - >> __rt_entry_main

  ble_tps_init (Thumb, 48 bytes, Stack size 24 bytes, ble_tps.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = ble_tps_init ⇒ tx_power_level_char_add
  [Calls]
  - >> tx_power_level_char_add
  [Called By]
  - >> tps_init

  ble_tps_tx_power_level_set (Thumb, 24 bytes, Stack size 24 bytes, ble_tps.o(.text), UNUSED)

  ble_ias_on_ble_evt (Thumb, 28 bytes, Stack size 16 bytes, ble_ias.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = ble_ias_on_ble_evt ⇒ on_write
  [Calls]
  - >> on_write
  [Called By]
  - >> ble_evt_dispatch

  ble_ias_init (Thumb, 60 bytes, Stack size 24 bytes, ble_ias.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = ble_ias_init ⇒ alert_level_char_add
  [Calls]
  - >> alert_level_char_add
  [Called By]
  - >> ias_init

  ble_ias_alert_level_get (Thumb, 22 bytes, Stack size 16 bytes, ble_ias.o(.text), UNUSED)

  ble_lls_alert_level_get (Thumb, 22 bytes, Stack size 16 bytes, ble_lls.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = ble_lls_alert_level_get
  [Called By]
  - >> on_disconnect

  ble_lls_on_ble_evt (Thumb, 56 bytes, Stack size 16 bytes, ble_lls.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = ble_lls_on_ble_evt ⇒ on_disconnect ⇒ ble_lls_alert_level_get
  [Calls]
  - >> on_auth_status
  - >> on_disconnect
  - >> on_connect
  [Called By]
  - >> ble_evt_dispatch

  ble_lls_init (Thumb, 68 bytes, Stack size 24 bytes, ble_lls.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = ble_lls_init ⇒ alert_level_char_add
  [Calls]
  - >> alert_level_char_add
  [Called By]
  - >> lls_init

  ble_bas_on_ble_evt (Thumb, 58 bytes, Stack size 16 bytes, ble_bas.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = ble_bas_on_ble_evt ⇒ on_write
  [Calls]
  - >> on_write
  - >> on_disconnect
  - >> on_connect
  [Called By]
  - >> ble_evt_dispatch

  ble_bas_init (Thumb, 66 bytes, Stack size 24 bytes, ble_bas.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = ble_bas_init ⇒ battery_level_char_add ⇒ ble_srv_report_ref_encode
  [Calls]
  - >> battery_level_char_add
  [Called By]
  - >> bas_init

  ble_bas_battery_level_update (Thumb, 118 bytes, Stack size 40 bytes, ble_bas.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = ble_bas_battery_level_update
  [Called By]
  - >> ADC_IRQHandler

  ble_ias_c_init (Thumb, 48 bytes, Stack size 0 bytes, ble_ias_c.o(.text))
  [Called By]

  - >> ias_client_init

  ble_ias_c_on_ble_evt (Thumb, 94 bytes, Stack size 16 bytes, ble_ias_c.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = ble_ias_c_on_ble_evt ⇒ on_char_disc_resp
  [Calls]
  - >> on_disconnect
  - >> on_char_disc_resp
  - >> on_srv_disc_resp
  - >> on_connect
  [Called By]
  - >> ble_evt_dispatch

  ble_ias_c_send_alert_level (Thumb, 40 bytes, Stack size 16 bytes, ble_ias_c.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = ble_ias_c_send_alert_level ⇒ write_characteristic_value
  [Calls]
  - >> write_characteristic_value
  [Called By]
  - >> button_event_handler

  ble_advdata_set (Thumb, 122 bytes, Stack size 104 bytes, ble_advdata.o(.text))
  [Stack]

  - Max Depth = 232
  - Call Chain = ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> srdata_check
  - >> advdata_check
  - >> adv_data_encode
  [Called By]
  - >> advertising_init

  ble_srv_report_ref_encode (Thumb, 60 bytes, Stack size 24 bytes, ble_srv_common.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = ble_srv_report_ref_encode
  [Calls]
  - >> app_error_handler
  [Called By]
  - >> battery_level_char_add

  ble_srv_ascii_to_utf8 (Thumb, 18 bytes, Stack size 16 bytes, ble_srv_common.o(.text), UNUSED)
  [Calls]

  - >> strlen

  ble_conn_params_init (Thumb, 90 bytes, Stack size 16 bytes, ble_conn_params.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = ble_conn_params_init ⇒ __aeabi_memcpy
  [Calls]
  - >> app_timer_create
  - >> __aeabi_memcpy
  - >> __aeabi_memcpy4
  [Called By]
  - >> conn_params_init

  ble_conn_params_stop (Thumb, 12 bytes, Stack size 8 bytes, ble_conn_params.o(.text), UNUSED)
  [Calls]

  - >> app_timer_stop

  ble_conn_params_on_ble_evt (Thumb, 62 bytes, Stack size 8 bytes, ble_conn_params.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = ble_conn_params_on_ble_evt ⇒ on_write ⇒ conn_params_negotiation ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> on_conn_params_update
  - >> on_write
  - >> on_disconnect
  - >> on_connect
  [Called By]
  - >> ble_evt_dispatch

  ble_conn_params_change_conn_params (Thumb, 86 bytes, Stack size 16 bytes, ble_conn_params.o(.text), UNUSED)
  [Calls]

  - >> is_conn_params_ok
  - >> __aeabi_memcpy

  RTC1_IRQHandler (Thumb, 34 bytes, Stack size 8 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = RTC1_IRQHandler ⇒ timer_timeouts_check ⇒ timeout_handler_exec
  [Calls]
  - >> timer_timeouts_check
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  SWI0_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = SWI0_IRQHandler ⇒ timer_list_handler ⇒ list_insertions_handler ⇒ timer_list_insert
  [Calls]
  - >> timer_list_handler
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  app_timer_init (Thumb, 254 bytes, Stack size 40 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = app_timer_init ⇒ rtc1_init ⇒ NVIC_SetPriority
  [Calls]
  - >> rtc1_counter_get
  - >> NVIC_ClearPendingIRQ
  - >> NVIC_EnableIRQ
  - >> rtc1_stop
  - >> rtc1_init
  - >> NVIC_SetPriority
  [Called By]
  - >> timers_init

  app_timer_create (Thumb, 108 bytes, Stack size 16 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = app_timer_create
  [Called By]
  - >> ble_conn_params_init
  - >> app_button_init
  - >> timers_init

  app_timer_start (Thumb, 98 bytes, Stack size 32 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> user_id_get
  - >> timer_start_op_schedule
  [Called By]
  - >> conn_params_negotiation
  - >> on_bas_evt
  - >> adv_led_blink_timeout_handler
  - >> mild_alert_timeout_handler
  - >> alert_led_blink_start
  - >> adv_led_blink_start
  - >> gpiote_event_handler

  app_timer_stop (Thumb, 60 bytes, Stack size 16 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = app_timer_stop ⇒ timer_stop_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> user_id_get
  - >> timer_stop_op_schedule
  [Called By]
  - >> ble_conn_params_stop
  - >> on_write
  - >> on_disconnect
  - >> app_button_disable
  - >> on_bas_evt
  - >> alert_led_blink_stop
  - >> adv_led_blink_stop
  - >> gpiote_event_handler

  app_timer_stop_all (Thumb, 26 bytes, Stack size 8 bytes, app_timer.o(.text), UNUSED)
  [Calls]

  - >> user_id_get
  - >> timer_stop_all_op_schedule

  app_timer_cnt_get (Thumb, 14 bytes, Stack size 8 bytes, app_timer.o(.text), UNUSED)
  [Calls]

  - >> rtc1_counter_get

  app_timer_cnt_diff_compute (Thumb, 22 bytes, Stack size 16 bytes, app_timer.o(.text), UNUSED)
  [Calls]

  - >> ticks_diff_get

  softdevice_assertion_handler (Thumb, 18 bytes, Stack size 16 bytes, softdevice_handler.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = softdevice_assertion_handler
  [Calls]
  - >> assert_nrf_callback
  [Address Reference Count : 1]
  - softdevice_handler.o(.text)

  intern_softdevice_events_execute (Thumb, 168 bytes, Stack size 24 bytes, softdevice_handler.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = intern_softdevice_events_execute
  [Calls]
  - >> app_error_handler
  [Called By]
  - >> SWI2_IRQHandler

  softdevice_handler_init (Thumb, 82 bytes, Stack size 40 bytes, softdevice_handler.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = softdevice_handler_init
  [Called By]
  - >> ble_stack_init

  softdevice_handler_sd_disable (Thumb, 24 bytes, Stack size 8 bytes, softdevice_handler.o(.text), UNUSED)

  softdevice_ble_evt_handler_set (Thumb, 18 bytes, Stack size 0 bytes, softdevice_handler.o(.text))
  [Called By]

  - >> ble_stack_init

  softdevice_sys_evt_handler_set (Thumb, 18 bytes, Stack size 0 bytes, softdevice_handler.o(.text))
  [Called By]

  - >> ble_stack_init

  SWI2_IRQHandler (Thumb, 52 bytes, Stack size 16 bytes, softdevice_handler.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = SWI2_IRQHandler ⇒ intern_softdevice_events_execute
  [Calls]
  - >> app_error_handler
  - >> intern_softdevice_events_execute
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  ble_bondmngr_on_ble_evt (Thumb, 122 bytes, Stack size 8 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = ble_bondmngr_on_ble_evt ⇒ on_auth_status ⇒ auth_status_update ⇒ bond_info_store ⇒ pstorage_store ⇒ cmd_queue_enqueue ⇒ process_cmd
  [Calls]
  - >> on_sec_param_request
  - >> on_sec_update
  - >> on_sec_info_request
  - >> on_auth_status
  - >> on_sys_attr_missing
  - >> on_connect
  [Called By]
  - >> ble_evt_dispatch

  ble_bondmngr_bonded_centrals_store (Thumb, 258 bytes, Stack size 16 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = ble_bondmngr_bonded_centrals_store ⇒ sys_attr_store ⇒ pstorage_store ⇒ cmd_queue_enqueue ⇒ process_cmd
  [Calls]
  - >> pstorage_clear
  - >> central_update
  - >> sys_attr_changed
  - >> bond_info_changed
  - >> sys_attr_store
  - >> bond_info_store
  [Called By]
  - >> on_ble_evt

  ble_bondmngr_sys_attr_store (Thumb, 142 bytes, Stack size 16 bytes, ble_bondmngr.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memcpy4
  - >> sys_attr_store

  ble_bondmngr_bonded_centrals_delete (Thumb, 38 bytes, Stack size 8 bytes, ble_bondmngr.o(.text), UNUSED)
  [Calls]

  - >> flash_pages_erase

  ble_bondmngr_central_addr_get (Thumb, 66 bytes, Stack size 16 bytes, ble_bondmngr.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memcpy

  ble_bondmngr_whitelist_get (Thumb, 108 bytes, Stack size 8 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = ble_bondmngr_whitelist_get
  [Called By]
  - >> advertising_start

  ble_bondmngr_init (Thumb, 216 bytes, Stack size 24 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 200
  - Call Chain = ble_bondmngr_init ⇒ load_all_from_flash ⇒ sys_attr_load_from_flash ⇒ pstorage_load ⇒ __aeabi_memcpy
  [Calls]
  - >> __aeabi_memclr4
  - >> pstorage_register
  - >> load_all_from_flash
  - >> flash_pages_erase
  [Called By]
  - >> bond_manager_init

  ble_bondmngr_central_ids_get (Thumb, 88 bytes, Stack size 8 bytes, ble_bondmngr.o(.text), UNUSED)

  ble_bondmngr_bonded_central_delete (Thumb, 302 bytes, Stack size 24 bytes, ble_bondmngr.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memclr4
  - >> __aeabi_memcpy4
  - >> update_whitelist
  - >> flash_pages_erase
  - >> sys_attr_store
  - >> bond_info_store

  ble_bondmngr_is_link_encrypted (Thumb, 32 bytes, Stack size 0 bytes, ble_bondmngr.o(.text), UNUSED)

  pstorage_sys_event_handler (Thumb, 102 bytes, Stack size 16 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = pstorage_sys_event_handler ⇒ cmd_queue_dequeue ⇒ app_notify
  [Calls]
  - >> cmd_queue_dequeue
  - >> app_notify
  [Called By]
  - >> sys_evt_dispatch

  pstorage_init (Thumb, 106 bytes, Stack size 8 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = pstorage_init ⇒ cmd_queue_init
  [Calls]
  - >> __aeabi_uidivmod
  - >> cmd_queue_init
  [Called By]
  - >> bond_manager_init

  pstorage_register (Thumb, 334 bytes, Stack size 24 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = pstorage_register
  [Calls]
  - >> __aeabi_uidivmod
  [Called By]
  - >> ble_bondmngr_init

  pstorage_block_identifier_get (Thumb, 136 bytes, Stack size 20 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = pstorage_block_identifier_get
  [Called By]
  - >> sys_attr_load_from_flash
  - >> bonding_info_load_from_flash
  - >> sys_attr_store
  - >> bond_info_store

  pstorage_store (Thumb, 188 bytes, Stack size 24 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = pstorage_store ⇒ cmd_queue_enqueue ⇒ process_cmd
  [Calls]
  - >> is_word_aligned
  - >> cmd_queue_enqueue
  [Called By]
  - >> sys_attr_store
  - >> bond_info_store

  pstorage_load (Thumb, 188 bytes, Stack size 24 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = pstorage_load ⇒ __aeabi_memcpy
  [Calls]
  - >> __aeabi_memcpy
  - >> is_word_aligned
  [Called By]
  - >> sys_attr_load_from_flash
  - >> bonding_info_load_from_flash

  pstorage_clear (Thumb, 126 bytes, Stack size 24 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = pstorage_clear ⇒ cmd_queue_enqueue ⇒ process_cmd
  [Calls]
  - >> cmd_queue_enqueue
  [Called By]
  - >> ble_bondmngr_bonded_centrals_store
  - >> flash_pages_erase

  crc16_compute (Thumb, 62 bytes, Stack size 16 bytes, crc16.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = crc16_compute
  [Called By]
  - >> sys_attr_changed
  - >> bond_info_changed
  - >> sys_attr_load_from_flash
  - >> bonding_info_load_from_flash
  - >> sys_attr_store
  - >> bond_info_store

  app_button_init (Thumb, 188 bytes, Stack size 48 bytes, app_button.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = app_button_init ⇒ app_gpiote_user_register ⇒ pins_sense_disable
  [Calls]
  - >> app_timer_create
  - >> app_gpiote_user_register
  [Called By]
  - >> buttons_init

  app_button_enable (Thumb, 24 bytes, Stack size 8 bytes, app_button.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = app_button_enable ⇒ app_gpiote_user_enable
  [Calls]
  - >> app_gpiote_user_enable
  [Called By]
  - >> on_ble_evt

  app_button_disable (Thumb, 42 bytes, Stack size 8 bytes, app_button.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = app_button_disable ⇒ app_timer_stop ⇒ timer_stop_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> app_timer_stop
  - >> app_gpiote_user_disable
  [Called By]
  - >> on_ias_c_evt

  app_button_is_pushed (Thumb, 90 bytes, Stack size 24 bytes, app_button.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = app_button_is_pushed ⇒ app_gpiote_pins_state_get
  [Calls]
  - >> app_gpiote_pins_state_get
  [Called By]
  - >> bond_manager_init

  GPIOTE_IRQHandler (Thumb, 106 bytes, Stack size 32 bytes, app_gpiote.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = GPIOTE_IRQHandler ⇒ sense_level_toggle
  [Calls]
  - >> sense_level_toggle
  [Address Reference Count : 1]
  - arm_startup_nrf51.o(RESET)

  app_gpiote_init (Thumb, 114 bytes, Stack size 16 bytes, app_gpiote.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = app_gpiote_init ⇒ NVIC_SetPriority
  [Calls]
  - >> __aeabi_memclr4
  - >> NVIC_SetPriority
  [Called By]
  - >> gpiote_init

  app_gpiote_user_register (Thumb, 138 bytes, Stack size 24 bytes, app_gpiote.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = app_gpiote_user_register ⇒ pins_sense_disable
  [Calls]
  - >> pins_sense_disable
  [Called By]
  - >> app_button_init

  app_gpiote_user_enable (Thumb, 222 bytes, Stack size 20 bytes, app_gpiote.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = app_gpiote_user_enable
  [Called By]
  - >> app_button_enable

  app_gpiote_user_disable (Thumb, 66 bytes, Stack size 8 bytes, app_gpiote.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = app_gpiote_user_disable ⇒ pins_sense_disable
  [Calls]
  - >> pins_sense_disable
  [Called By]
  - >> app_button_disable

  app_gpiote_pins_state_get (Thumb, 52 bytes, Stack size 8 bytes, app_gpiote.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = app_gpiote_pins_state_get
  [Called By]
  - >> app_button_is_pushed
  - >> detection_delay_timeout_handler

  memcmp (Thumb, 90 bytes, Stack size 8 bytes, memcmp.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = memcmp
  [Called By]
  - >> on_connect

  strlen (Thumb, 62 bytes, Stack size 12 bytes, strlen.o(.text), UNUSED)
  [Called By]

  - >> ble_srv_ascii_to_utf8

  __aeabi_memcpy (Thumb, 130 bytes, Stack size 24 bytes, rt_memcpy.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = __aeabi_memcpy
  [Calls]
  - >> __aeabi_memcpy4
  [Called By]
  - >> ble_conn_params_change_conn_params
  - >> on_conn_params_update
  - >> on_connect
  - >> service_data_encode
  - >> manuf_specific_data_encode
  - >> uint8_array_encode
  - >> ble_conn_params_init
  - >> pstorage_load
  - >> ble_bondmngr_central_addr_get
  - >> on_sec_info_request
  - >> auth_status_update
  - >> on_connect
  - >> on_auth_status_from_new_central

  __rt_memcpy (Thumb, 0 bytes, Stack size 24 bytes, rt_memcpy.o(.text), UNUSED)

  _memset_w (Thumb, 26 bytes, Stack size 0 bytes, rt_memclr.o(.text), UNUSED)
  [Called By]

  - >> __rt_memclr_w
  - >> _memset

  _memset (Thumb, 30 bytes, Stack size 0 bytes, rt_memclr.o(.text), UNUSED)
  [Calls]

  - >> _memset_w
  [Called By]
  - >> __aeabi_memclr

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, rt_memclr.o(.text), UNUSED)
  [Calls]

  - >> _memset

  __rt_memclr (Thumb, 0 bytes, Stack size 0 bytes, rt_memclr.o(.text), UNUSED)

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, rt_memclr.o(.text))
  [Called By]

  - >> battery_level_char_add
  - >> alert_level_char_add
  - >> alert_level_char_add
  - >> tx_power_level_char_add
  - >> ble_bondmngr_init
  - >> app_gpiote_init
  - >> conn_params_init
  - >> bas_init
  - >> advertising_start
  - >> advertising_init
  - >> ble_bondmngr_bonded_central_delete
  - >> on_sec_param_request
  - >> auth_status_update

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, rt_memclr.o(.text), UNUSED)

  __rt_memclr_w (Thumb, 4 bytes, Stack size 0 bytes, rt_memclr.o(.text), UNUSED)
  [Calls]

  - >> _memset_w

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 0 bytes, aeabi_sdiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 20 bytes, Stack size 0 bytes, aeabi_sdiv.o(.text))
  [Called By]

  - >> pstorage_init
  - >> bond_manager_init
  - >> process_cmd
  - >> pstorage_register

  __aeabi_idiv (Thumb, 0 bytes, Stack size 8 bytes, aeabi_sdiv.o(.text), UNUSED)

  __aeabi_idivmod (Thumb, 326 bytes, Stack size 8 bytes, aeabi_sdiv.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_idivmod
  [Called By]
  - >> ADC_IRQHandler
  - >> battery_level_in_percent

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 62 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  - >> _call_atexit_fns (Weak Reference)
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size unknown bytes, indicate_semi.o(.text), UNUSED)

  ### Local Symbols

  is_disabled_in_debug_needed (Thumb, 48 bytes, Stack size 0 bytes, system_nrf51.o(.text))
  [Called By]

  - >> SystemInit

  is_manual_peripheral_setup_needed (Thumb, 94 bytes, Stack size 0 bytes, system_nrf51.o(.text))
  [Called By]

  - >> SystemInit

  nrf_gpio_cfg_sense_input (Thumb, 24 bytes, Stack size 12 bytes, main.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = nrf_gpio_cfg_sense_input
  [Called By]
  - >> on_ble_evt

  service_error_handler (Thumb, 14 bytes, Stack size 0 bytes, main.o(.text))
  [Calls]

  - >> app_error_handler
  [Address Reference Count : 1]
  - main.o(.text)

  adc_start (Thumb, 132 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = adc_start
  [Calls]
  - >> app_error_handler
  [Called By]
  - >> battery_level_meas_timeout_handler

  adv_led_blink_start (Thumb, 74 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = adv_led_blink_start ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> app_timer_start
  - >> app_error_handler
  - >> nrf_gpio_pin_set
  [Called By]
  - >> advertising_start

  adv_led_blink_stop (Thumb, 50 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = adv_led_blink_stop ⇒ app_timer_stop ⇒ timer_stop_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> app_timer_stop
  - >> app_error_handler
  - >> nrf_gpio_pin_clear
  [Called By]
  - >> on_ble_evt

  alert_led_blink_start (Thumb, 70 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = alert_led_blink_start ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> app_timer_start
  - >> app_error_handler
  - >> nrf_gpio_pin_set
  [Called By]
  - >> alert_signal

  alert_led_blink_stop (Thumb, 50 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = alert_led_blink_stop ⇒ app_timer_stop ⇒ timer_stop_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> app_timer_stop
  - >> app_error_handler
  - >> nrf_gpio_pin_clear
  [Called By]
  - >> button_event_handler
  - >> on_ble_evt
  - >> alert_signal

  advertising_init (Thumb, 98 bytes, Stack size 88 bytes, main.o(.text))
  [Stack]

  - Max Depth = 320
  - Call Chain = advertising_init ⇒ ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> ble_advdata_set
  - >> app_error_handler
  - >> __aeabi_memclr4
  [Called By]
  - >> main
  - >> advertising_start

  advertising_start (Thumb, 242 bytes, Stack size 48 bytes, main.o(.text))
  [Stack]

  - Max Depth = 368
  - Call Chain = advertising_start ⇒ advertising_init ⇒ ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> ble_bondmngr_whitelist_get
  - >> app_error_handler
  - >> advertising_init
  - >> adv_led_blink_start
  - >> __aeabi_memclr4
  [Called By]
  - >> main
  - >> on_ble_evt

  battery_level_meas_timeout_handler (Thumb, 10 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = battery_level_meas_timeout_handler ⇒ adc_start
  [Calls]
  - >> adc_start
  [Address Reference Count : 1]
  - main.o(.text)

  mild_alert_timeout_handler (Thumb, 218 bytes, Stack size 24 bytes, main.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = mild_alert_timeout_handler ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> app_timer_start
  - >> app_error_handler
  - >> nrf_gpio_pin_toggle
  [Address Reference Count : 1]
  - main.o(.text)

  adv_led_blink_timeout_handler (Thumb, 118 bytes, Stack size 24 bytes, main.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = adv_led_blink_timeout_handler ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> app_timer_start
  - >> app_error_handler
  - >> nrf_gpio_pin_toggle
  [Address Reference Count : 1]
  - main.o(.text)

  leds_init (Thumb, 16 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = leds_init
  [Calls]
  - >> nrf_gpio_cfg_output
  [Called By]
  - >> main

  timers_init (Thumb, 156 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = timers_init ⇒ app_timer_init ⇒ rtc1_init ⇒ NVIC_SetPriority
  [Calls]
  - >> app_timer_init
  - >> app_timer_create
  - >> app_error_handler
  [Called By]
  - >> main

  gap_params_init (Thumb, 188 bytes, Stack size 24 bytes, main.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = gap_params_init
  [Calls]
  - >> app_error_handler
  [Called By]
  - >> main

  tps_init (Thumb, 104 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = tps_init ⇒ ble_tps_init ⇒ tx_power_level_char_add
  [Calls]
  - >> ble_tps_init
  - >> app_error_handler
  [Called By]
  - >> services_init

  alert_signal (Thumb, 54 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = alert_signal ⇒ alert_led_blink_start ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> nrf_gpio_pin_set
  - >> alert_led_blink_stop
  - >> alert_led_blink_start
  [Called By]
  - >> on_lls_evt
  - >> on_ias_evt

  on_ias_evt (Thumb, 26 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = on_ias_evt ⇒ alert_signal ⇒ alert_led_blink_start ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> alert_signal
  [Address Reference Count : 1]
  - main.o(.text)

  ias_init (Thumb, 46 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = ias_init ⇒ ble_ias_init ⇒ alert_level_char_add
  [Calls]
  - >> ble_ias_init
  - >> app_error_handler
  [Called By]
  - >> services_init

  on_lls_evt (Thumb, 32 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = on_lls_evt ⇒ alert_signal ⇒ alert_led_blink_start ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> alert_signal
  [Address Reference Count : 1]
  - main.o(.text)

  lls_init (Thumb, 124 bytes, Stack size 24 bytes, main.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = lls_init ⇒ ble_lls_init ⇒ alert_level_char_add
  [Calls]
  - >> ble_lls_init
  - >> app_error_handler
  [Called By]
  - >> services_init

  on_bas_evt (Thumb, 100 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = on_bas_evt ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> app_timer_stop
  - >> app_timer_start
  - >> app_error_handler
  [Address Reference Count : 1]
  - main.o(.text)

  bas_init (Thumb, 282 bytes, Stack size 32 bytes, main.o(.text))
  [Stack]

  - Max Depth = 168
  - Call Chain = bas_init ⇒ ble_bas_init ⇒ battery_level_char_add ⇒ ble_srv_report_ref_encode
  [Calls]
  - >> ble_bas_init
  - >> app_error_handler
  - >> __aeabi_memclr4
  [Called By]
  - >> services_init

  on_ias_c_evt (Thumb, 64 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = on_ias_c_evt ⇒ app_button_disable ⇒ app_timer_stop ⇒ timer_stop_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> app_button_disable
  - >> app_error_handler
  [Address Reference Count : 1]
  - main.o(.text)

  ias_client_init (Thumb, 56 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = ias_client_init
  [Calls]
  - >> ble_ias_c_init
  - >> app_error_handler
  [Called By]
  - >> services_init

  services_init (Thumb, 24 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 176
  - Call Chain = services_init ⇒ bas_init ⇒ ble_bas_init ⇒ battery_level_char_add ⇒ ble_srv_report_ref_encode
  [Calls]
  - >> ias_client_init
  - >> bas_init
  - >> lls_init
  - >> ias_init
  - >> tps_init
  [Called By]
  - >> main

  sec_params_init (Thumb, 66 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> main

  conn_params_error_handler (Thumb, 16 bytes, Stack size 0 bytes, main.o(.text))
  [Calls]

  - >> app_error_handler
  [Address Reference Count : 1]
  - main.o(.text)

  conn_params_init (Thumb, 82 bytes, Stack size 40 bytes, main.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = conn_params_init ⇒ ble_conn_params_init ⇒ __aeabi_memcpy
  [Calls]
  - >> ble_conn_params_init
  - >> app_error_handler
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  on_ble_evt (Thumb, 318 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 384
  - Call Chain = on_ble_evt ⇒ advertising_start ⇒ advertising_init ⇒ ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> ble_bondmngr_bonded_centrals_store
  - >> app_button_enable
  - >> app_error_handler
  - >> advertising_start
  - >> alert_led_blink_stop
  - >> adv_led_blink_stop
  - >> nrf_gpio_cfg_sense_input
  [Called By]
  - >> ble_evt_dispatch

  ble_evt_dispatch (Thumb, 56 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 392
  - Call Chain = ble_evt_dispatch ⇒ on_ble_evt ⇒ advertising_start ⇒ advertising_init ⇒ ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> ble_lls_on_ble_evt
  - >> ble_ias_on_ble_evt
  - >> ble_ias_c_on_ble_evt
  - >> ble_conn_params_on_ble_evt
  - >> ble_bondmngr_on_ble_evt
  - >> ble_bas_on_ble_evt
  - >> on_ble_evt
  [Address Reference Count : 1]
  - main.o(.text)

  sys_evt_dispatch (Thumb, 12 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = sys_evt_dispatch ⇒ pstorage_sys_event_handler ⇒ cmd_queue_dequeue ⇒ app_notify
  [Calls]
  - >> pstorage_sys_event_handler
  [Address Reference Count : 1]
  - main.o(.text)

  ble_stack_init (Thumb, 110 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = ble_stack_init ⇒ softdevice_handler_init
  [Calls]
  - >> softdevice_sys_evt_handler_set
  - >> softdevice_handler_init
  - >> softdevice_ble_evt_handler_set
  - >> app_error_handler
  [Called By]
  - >> main

  bond_manager_error_handler (Thumb, 16 bytes, Stack size 0 bytes, main.o(.text))
  [Calls]

  - >> app_error_handler
  [Address Reference Count : 1]
  - main.o(.text)

  bond_manager_init (Thumb, 272 bytes, Stack size 24 bytes, main.o(.text))
  [Stack]

  - Max Depth = 224
  - Call Chain = bond_manager_init ⇒ ble_bondmngr_init ⇒ load_all_from_flash ⇒ sys_attr_load_from_flash ⇒ pstorage_load ⇒ __aeabi_memcpy
  [Calls]
  - >> pstorage_init
  - >> ble_bondmngr_init
  - >> app_button_is_pushed
  - >> app_error_handler
  - >> __aeabi_uidivmod
  [Called By]
  - >> main

  button_event_handler (Thumb, 118 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = button_event_handler ⇒ alert_led_blink_stop ⇒ app_timer_stop ⇒ timer_stop_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> ble_ias_c_send_alert_level
  - >> app_error_handler
  - >> alert_led_blink_stop
  [Address Reference Count : 1]
  - main.o(.data)

  gpiote_init (Thumb, 42 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = gpiote_init ⇒ app_gpiote_init ⇒ NVIC_SetPriority
  [Calls]
  - >> app_gpiote_init
  - >> app_error_handler
  [Called By]
  - >> main

  buttons_init (Thumb, 46 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = buttons_init ⇒ app_button_init ⇒ app_gpiote_user_register ⇒ pins_sense_disable
  [Calls]
  - >> app_button_init
  - >> app_error_handler
  [Called By]
  - >> main

  power_manage (Thumb, 32 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = power_manage
  [Calls]
  - >> app_error_handler
  [Called By]
  - >> main

  nrf_gpio_cfg_output (Thumb, 18 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> leds_init

  nrf_gpio_pin_set (Thumb, 10 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> alert_signal
  - >> alert_led_blink_start
  - >> adv_led_blink_start

  nrf_gpio_pin_clear (Thumb, 10 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> alert_led_blink_stop
  - >> adv_led_blink_stop

  nrf_gpio_pin_toggle (Thumb, 16 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> adv_led_blink_timeout_handler
  - >> mild_alert_timeout_handler

  battery_level_in_percent (Thumb, 148 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = battery_level_in_percent ⇒ __aeabi_idivmod
  [Calls]
  - >> __aeabi_idivmod
  [Called By]
  - >> ADC_IRQHandler

  tx_power_level_char_add (Thumb, 162 bytes, Stack size 72 bytes, ble_tps.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = tx_power_level_char_add
  [Calls]
  - >> __aeabi_memclr4
  [Called By]
  - >> ble_tps_init

  on_write (Thumb, 42 bytes, Stack size 24 bytes, ble_ias.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = on_write
  [Called By]
  - >> ble_ias_on_ble_evt

  alert_level_char_add (Thumb, 214 bytes, Stack size 72 bytes, ble_ias.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = alert_level_char_add
  [Calls]
  - >> __aeabi_memclr4
  [Called By]
  - >> ble_ias_init

  on_connect (Thumb, 20 bytes, Stack size 16 bytes, ble_lls.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = on_connect
  [Called By]
  - >> ble_lls_on_ble_evt

  on_disconnect (Thumb, 56 bytes, Stack size 32 bytes, ble_lls.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = on_disconnect ⇒ ble_lls_alert_level_get
  [Calls]
  - >> ble_lls_alert_level_get
  [Called By]
  - >> ble_lls_on_ble_evt

  on_auth_status (Thumb, 28 bytes, Stack size 24 bytes, ble_lls.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = on_auth_status
  [Called By]
  - >> ble_lls_on_ble_evt

  alert_level_char_add (Thumb, 180 bytes, Stack size 72 bytes, ble_lls.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = alert_level_char_add
  [Calls]
  - >> __aeabi_memclr4
  [Called By]
  - >> ble_lls_init

  on_connect (Thumb, 6 bytes, Stack size 0 bytes, ble_bas.o(.text))
  [Called By]

  - >> ble_bas_on_ble_evt

  on_disconnect (Thumb, 8 bytes, Stack size 0 bytes, ble_bas.o(.text))
  [Called By]

  - >> ble_bas_on_ble_evt

  on_write (Thumb, 80 bytes, Stack size 24 bytes, ble_bas.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = on_write
  [Called By]
  - >> ble_bas_on_ble_evt

  battery_level_char_add (Thumb, 448 bytes, Stack size 88 bytes, ble_bas.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = battery_level_char_add ⇒ ble_srv_report_ref_encode
  [Calls]
  - >> ble_srv_report_ref_encode
  - >> __aeabi_memclr4
  [Called By]
  - >> ble_bas_init

  on_connect (Thumb, 34 bytes, Stack size 16 bytes, ble_ias_c.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = on_connect
  [Called By]
  - >> ble_ias_c_on_ble_evt

  on_srv_disc_resp (Thumb, 52 bytes, Stack size 24 bytes, ble_ias_c.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = on_srv_disc_resp
  [Called By]
  - >> ble_ias_c_on_ble_evt

  on_char_disc_resp (Thumb, 122 bytes, Stack size 24 bytes, ble_ias_c.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = on_char_disc_resp
  [Called By]
  - >> ble_ias_c_on_ble_evt

  on_disconnect (Thumb, 38 bytes, Stack size 16 bytes, ble_ias_c.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = on_disconnect
  [Called By]
  - >> ble_ias_c_on_ble_evt

  write_characteristic_value (Thumb, 48 bytes, Stack size 40 bytes, ble_ias_c.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = write_characteristic_value
  [Called By]
  - >> ble_ias_c_send_alert_level

  name_encode (Thumb, 150 bytes, Stack size 48 bytes, ble_advdata.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = name_encode
  [Called By]
  - >> adv_data_encode

  appearance_encode (Thumb, 74 bytes, Stack size 24 bytes, ble_advdata.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = appearance_encode
  [Calls]
  - >> uint16_encode
  [Called By]
  - >> adv_data_encode

  uint8_array_encode (Thumb, 82 bytes, Stack size 24 bytes, ble_advdata.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = uint8_array_encode ⇒ __aeabi_memcpy
  [Calls]
  - >> __aeabi_memcpy
  [Called By]
  - >> adv_data_encode

  tx_power_level_encode (Thumb, 48 bytes, Stack size 12 bytes, ble_advdata.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = tx_power_level_encode
  [Called By]
  - >> adv_data_encode

  uuid_list_sized_encode (Thumb, 196 bytes, Stack size 64 bytes, ble_advdata.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = uuid_list_sized_encode
  [Called By]
  - >> uuid_list_encode

  uuid_list_encode (Thumb, 64 bytes, Stack size 40 bytes, ble_advdata.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> uuid_list_sized_encode
  [Called By]
  - >> adv_data_encode

  conn_int_check (Thumb, 88 bytes, Stack size 0 bytes, ble_advdata.o(.text))
  [Called By]

  - >> conn_int_encode

  conn_int_encode (Thumb, 92 bytes, Stack size 24 bytes, ble_advdata.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = conn_int_encode
  [Calls]
  - >> uint16_encode
  - >> conn_int_check
  [Called By]
  - >> adv_data_encode

  manuf_specific_data_encode (Thumb, 106 bytes, Stack size 24 bytes, ble_advdata.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = manuf_specific_data_encode ⇒ __aeabi_memcpy
  [Calls]
  - >> uint16_encode
  - >> __aeabi_memcpy
  [Called By]
  - >> adv_data_encode

  service_data_encode (Thumb, 140 bytes, Stack size 32 bytes, ble_advdata.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = service_data_encode ⇒ __aeabi_memcpy
  [Calls]
  - >> uint16_encode
  - >> __aeabi_memcpy
  [Called By]
  - >> adv_data_encode

  adv_data_encode (Thumb, 304 bytes, Stack size 24 bytes, ble_advdata.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> service_data_encode
  - >> manuf_specific_data_encode
  - >> conn_int_encode
  - >> uuid_list_encode
  - >> tx_power_level_encode
  - >> uint8_array_encode
  - >> appearance_encode
  - >> name_encode
  [Called By]
  - >> ble_advdata_set

  advdata_check (Thumb, 32 bytes, Stack size 0 bytes, ble_advdata.o(.text))
  [Called By]

  - >> ble_advdata_set

  srdata_check (Thumb, 16 bytes, Stack size 0 bytes, ble_advdata.o(.text))
  [Called By]

  - >> ble_advdata_set

  uint16_encode (Thumb, 18 bytes, Stack size 0 bytes, ble_advdata.o(.text))
  [Called By]

  - >> service_data_encode
  - >> manuf_specific_data_encode
  - >> conn_int_encode
  - >> appearance_encode

  is_conn_params_ok (Thumb, 30 bytes, Stack size 0 bytes, ble_conn_params.o(.text))
  [Called By]

  - >> ble_conn_params_change_conn_params
  - >> conn_params_negotiation

  update_timeout_handler (Thumb, 136 bytes, Stack size 16 bytes, ble_conn_params.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = update_timeout_handler
  [Address Reference Count : 1]
  - ble_conn_params.o(.text)

  conn_params_negotiation (Thumb, 126 bytes, Stack size 16 bytes, ble_conn_params.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = conn_params_negotiation ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> is_conn_params_ok
  - >> app_timer_start
  [Called By]
  - >> on_conn_params_update
  - >> on_write
  - >> on_connect

  on_connect (Thumb, 42 bytes, Stack size 8 bytes, ble_conn_params.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = on_connect ⇒ conn_params_negotiation ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> conn_params_negotiation
  - >> __aeabi_memcpy
  [Called By]
  - >> ble_conn_params_on_ble_evt

  on_disconnect (Thumb, 50 bytes, Stack size 16 bytes, ble_conn_params.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = on_disconnect ⇒ app_timer_stop ⇒ timer_stop_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> app_timer_stop
  [Called By]
  - >> ble_conn_params_on_ble_evt

  on_write (Thumb, 84 bytes, Stack size 16 bytes, ble_conn_params.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = on_write ⇒ conn_params_negotiation ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> conn_params_negotiation
  - >> app_timer_stop
  [Called By]
  - >> ble_conn_params_on_ble_evt

  on_conn_params_update (Thumb, 20 bytes, Stack size 8 bytes, ble_conn_params.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = on_conn_params_update ⇒ conn_params_negotiation ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> conn_params_negotiation
  - >> __aeabi_memcpy
  [Called By]
  - >> ble_conn_params_on_ble_evt

  NVIC_SetPriority (Thumb, 110 bytes, Stack size 8 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = NVIC_SetPriority
  [Called By]
  - >> rtc1_init
  - >> app_timer_init

  rtc1_init (Thumb, 18 bytes, Stack size 8 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = rtc1_init ⇒ NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> app_timer_init

  rtc1_start (Thumb, 42 bytes, Stack size 8 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = rtc1_start
  [Calls]
  - >> __asm___11_app_timer_c_cd27f9c3__nrf_delay_us
  - >> NVIC_ClearPendingIRQ
  - >> NVIC_EnableIRQ
  [Called By]
  - >> compare_reg_update

  rtc1_stop (Thumb, 44 bytes, Stack size 8 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = rtc1_stop
  [Calls]
  - >> __asm___11_app_timer_c_cd27f9c3__nrf_delay_us
  [Called By]
  - >> compare_reg_update
  - >> app_timer_init

  timer_list_insert (Thumb, 206 bytes, Stack size 20 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = timer_list_insert
  [Called By]
  - >> list_insertions_handler

  timer_list_remove (Thumb, 150 bytes, Stack size 16 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = timer_list_remove
  [Called By]
  - >> list_deletions_handler

  timer_timeouts_check_sched (Thumb, 10 bytes, Stack size 8 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = timer_timeouts_check_sched
  [Calls]
  - >> NVIC_SetPendingIRQ
  [Called By]
  - >> compare_reg_update

  timer_list_handler_sched (Thumb, 10 bytes, Stack size 8 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = timer_list_handler_sched
  [Calls]
  - >> NVIC_SetPendingIRQ
  [Called By]
  - >> timer_stop_all_op_schedule
  - >> timer_stop_op_schedule
  - >> timer_start_op_schedule
  - >> timer_timeouts_check

  timeout_handler_exec (Thumb, 60 bytes, Stack size 16 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = timeout_handler_exec
  [Calls]
  - >> app_error_handler
  [Called By]
  - >> timer_timeouts_check

  timer_timeouts_check (Thumb, 128 bytes, Stack size 24 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = timer_timeouts_check ⇒ timeout_handler_exec
  [Calls]
  - >> ticks_diff_get
  - >> rtc1_counter_get
  - >> timeout_handler_exec
  - >> timer_list_handler_sched
  [Called By]
  - >> RTC1_IRQHandler

  elapsed_ticks_acquire (Thumb, 82 bytes, Stack size 0 bytes, app_timer.o(.text))
  [Called By]

  - >> timer_list_handler

  list_deletions_handler (Thumb, 280 bytes, Stack size 32 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = list_deletions_handler ⇒ timer_list_remove
  [Calls]
  - >> timer_list_remove
  [Called By]
  - >> timer_list_handler

  expired_timers_handler (Thumb, 98 bytes, Stack size 20 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = expired_timers_handler
  [Called By]
  - >> timer_list_handler

  list_insertions_handler (Thumb, 260 bytes, Stack size 32 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = list_insertions_handler ⇒ timer_list_insert
  [Calls]
  - >> ticks_diff_get
  - >> timer_list_insert
  [Called By]
  - >> timer_list_handler

  compare_reg_update (Thumb, 124 bytes, Stack size 32 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = compare_reg_update ⇒ timer_timeouts_check_sched
  [Calls]
  - >> ticks_diff_get
  - >> rtc1_counter_get
  - >> timer_timeouts_check_sched
  - >> rtc1_stop
  - >> rtc1_start
  [Called By]
  - >> timer_list_handler

  timer_list_handler (Thumb, 70 bytes, Stack size 32 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 84
  - Call Chain = timer_list_handler ⇒ list_insertions_handler ⇒ timer_list_insert
  [Calls]
  - >> compare_reg_update
  - >> list_insertions_handler
  - >> expired_timers_handler
  - >> list_deletions_handler
  - >> elapsed_ticks_acquire
  [Called By]
  - >> SWI0_IRQHandler

  user_op_enque (Thumb, 4 bytes, Stack size 0 bytes, app_timer.o(.text))
  [Called By]

  - >> timer_stop_all_op_schedule
  - >> timer_stop_op_schedule
  - >> timer_start_op_schedule

  user_op_alloc (Thumb, 44 bytes, Stack size 16 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = user_op_alloc
  [Called By]
  - >> timer_stop_all_op_schedule
  - >> timer_stop_op_schedule
  - >> timer_start_op_schedule

  timer_start_op_schedule (Thumb, 80 bytes, Stack size 40 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> rtc1_counter_get
  - >> user_op_alloc
  - >> user_op_enque
  - >> timer_list_handler_sched
  [Called By]
  - >> app_timer_start

  timer_stop_op_schedule (Thumb, 58 bytes, Stack size 24 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = timer_stop_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> user_op_alloc
  - >> user_op_enque
  - >> timer_list_handler_sched
  [Called By]
  - >> app_timer_stop

  timer_stop_all_op_schedule (Thumb, 58 bytes, Stack size 16 bytes, app_timer.o(.text), UNUSED)
  [Calls]

  - >> user_op_alloc
  - >> user_op_enque
  - >> timer_list_handler_sched
  [Called By]
  - >> app_timer_stop_all

  user_id_get (Thumb, 34 bytes, Stack size 8 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = user_id_get ⇒ current_int_priority_get
  [Calls]
  - >> current_int_priority_get
  [Called By]
  - >> app_timer_stop_all
  - >> app_timer_stop
  - >> app_timer_start

  NVIC_EnableIRQ (Thumb, 14 bytes, Stack size 0 bytes, app_timer.o(.text))
  [Called By]

  - >> rtc1_start
  - >> app_timer_init

  NVIC_SetPendingIRQ (Thumb, 14 bytes, Stack size 0 bytes, app_timer.o(.text))
  [Called By]

  - >> timer_list_handler_sched
  - >> timer_timeouts_check_sched

  NVIC_ClearPendingIRQ (Thumb, 16 bytes, Stack size 0 bytes, app_timer.o(.text))
  [Called By]

  - >> rtc1_start
  - >> app_timer_init

  current_int_priority_get (Thumb, 84 bytes, Stack size 8 bytes, app_timer.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = current_int_priority_get
  [Called By]
  - >> user_id_get

  rtc1_counter_get (Thumb, 6 bytes, Stack size 0 bytes, app_timer.o(.text))
  [Called By]

  - >> app_timer_cnt_get
  - >> timer_start_op_schedule
  - >> compare_reg_update
  - >> timer_timeouts_check
  - >> app_timer_init

  ticks_diff_get (Thumb, 10 bytes, Stack size 0 bytes, app_timer.o(.text))
  [Called By]

  - >> app_timer_cnt_diff_compute
  - >> compare_reg_update
  - >> list_insertions_handler
  - >> timer_timeouts_check

  crc_extract (Thumb, 30 bytes, Stack size 0 bytes, ble_bondmngr.o(.text))
  [Called By]

  - >> sys_attr_load_from_flash
  - >> bonding_info_load_from_flash

  bond_info_store (Thumb, 178 bytes, Stack size 24 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = bond_info_store ⇒ pstorage_store ⇒ cmd_queue_enqueue ⇒ process_cmd
  [Calls]
  - >> pstorage_store
  - >> pstorage_block_identifier_get
  - >> crc16_compute
  [Called By]
  - >> ble_bondmngr_bonded_centrals_store
  - >> ble_bondmngr_bonded_central_delete
  - >> auth_status_update
  - >> on_auth_status_from_new_central

  sys_attr_store (Thumb, 156 bytes, Stack size 24 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = sys_attr_store ⇒ pstorage_store ⇒ cmd_queue_enqueue ⇒ process_cmd
  [Calls]
  - >> pstorage_store
  - >> pstorage_block_identifier_get
  - >> crc16_compute
  [Called By]
  - >> ble_bondmngr_bonded_centrals_store
  - >> ble_bondmngr_bonded_central_delete
  - >> ble_bondmngr_sys_attr_store

  bonding_info_load_from_flash (Thumb, 200 bytes, Stack size 32 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = bonding_info_load_from_flash ⇒ pstorage_load ⇒ __aeabi_memcpy
  [Calls]
  - >> pstorage_load
  - >> pstorage_block_identifier_get
  - >> crc16_compute
  - >> crc_extract
  [Called By]
  - >> load_all_from_flash

  sys_attr_load_from_flash (Thumb, 222 bytes, Stack size 32 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = sys_attr_load_from_flash ⇒ pstorage_load ⇒ __aeabi_memcpy
  [Calls]
  - >> pstorage_load
  - >> pstorage_block_identifier_get
  - >> crc16_compute
  - >> crc_extract
  [Called By]
  - >> load_all_from_flash

  flash_pages_erase (Thumb, 30 bytes, Stack size 8 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = flash_pages_erase ⇒ pstorage_clear ⇒ cmd_queue_enqueue ⇒ process_cmd
  [Calls]
  - >> pstorage_clear
  [Called By]
  - >> ble_bondmngr_init
  - >> ble_bondmngr_bonded_central_delete
  - >> ble_bondmngr_bonded_centrals_delete

  bond_info_changed (Thumb, 66 bytes, Stack size 16 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = bond_info_changed ⇒ crc16_compute
  [Calls]
  - >> crc16_compute
  [Called By]
  - >> ble_bondmngr_bonded_centrals_store

  sys_attr_changed (Thumb, 70 bytes, Stack size 16 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = sys_attr_changed ⇒ crc16_compute
  [Calls]
  - >> crc16_compute
  [Called By]
  - >> ble_bondmngr_bonded_centrals_store

  central_sys_attr_set (Thumb, 104 bytes, Stack size 16 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = central_sys_attr_set
  [Called By]
  - >> on_sec_update
  - >> on_sys_attr_missing

  update_whitelist (Thumb, 128 bytes, Stack size 8 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = update_whitelist
  [Called By]
  - >> ble_bondmngr_bonded_central_delete
  - >> load_all_from_flash
  - >> central_update
  - >> on_auth_status_from_new_central

  on_auth_status_from_new_central (Thumb, 224 bytes, Stack size 24 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = on_auth_status_from_new_central ⇒ bond_info_store ⇒ pstorage_store ⇒ cmd_queue_enqueue ⇒ process_cmd
  [Calls]
  - >> __aeabi_memcpy
  - >> __aeabi_memcpy4
  - >> update_whitelist
  - >> bond_info_store
  [Called By]
  - >> on_auth_status

  central_update (Thumb, 90 bytes, Stack size 16 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = central_update ⇒ update_whitelist
  [Calls]
  - >> __aeabi_memcpy4
  - >> update_whitelist
  [Called By]
  - >> ble_bondmngr_bonded_centrals_store

  central_find_in_db (Thumb, 58 bytes, Stack size 16 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = central_find_in_db
  [Calls]
  - >> __aeabi_memcpy4
  [Called By]
  - >> on_sec_info_request
  - >> on_auth_status

  load_all_from_flash (Thumb, 244 bytes, Stack size 96 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 176
  - Call Chain = load_all_from_flash ⇒ sys_attr_load_from_flash ⇒ pstorage_load ⇒ __aeabi_memcpy
  [Calls]
  - >> __aeabi_memcpy4
  - >> update_whitelist
  - >> sys_attr_load_from_flash
  - >> bonding_info_load_from_flash
  [Called By]
  - >> ble_bondmngr_init

  on_connect (Thumb, 236 bytes, Stack size 24 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = on_connect ⇒ __aeabi_memcpy
  [Calls]
  - >> __aeabi_memcpy
  - >> __aeabi_memcpy4
  - >> memcmp
  [Called By]
  - >> ble_bondmngr_on_ble_evt

  on_sys_attr_missing (Thumb, 132 bytes, Stack size 16 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = on_sys_attr_missing ⇒ central_sys_attr_set
  [Calls]
  - >> central_sys_attr_set
  [Called By]
  - >> ble_bondmngr_on_ble_evt

  auth_status_update (Thumb, 166 bytes, Stack size 24 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = auth_status_update ⇒ bond_info_store ⇒ pstorage_store ⇒ cmd_queue_enqueue ⇒ process_cmd
  [Calls]
  - >> __aeabi_memclr4
  - >> __aeabi_memcpy
  - >> __aeabi_memcpy4
  - >> bond_info_store
  [Called By]
  - >> on_auth_status

  on_auth_status (Thumb, 86 bytes, Stack size 16 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = on_auth_status ⇒ auth_status_update ⇒ bond_info_store ⇒ pstorage_store ⇒ cmd_queue_enqueue ⇒ process_cmd
  [Calls]
  - >> auth_status_update
  - >> central_find_in_db
  - >> on_auth_status_from_new_central
  [Called By]
  - >> ble_bondmngr_on_ble_evt

  on_sec_info_request (Thumb, 116 bytes, Stack size 16 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = on_sec_info_request ⇒ __aeabi_memcpy
  [Calls]
  - >> __aeabi_memcpy
  - >> central_find_in_db
  [Called By]
  - >> ble_bondmngr_on_ble_evt

  on_sec_update (Thumb, 118 bytes, Stack size 32 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = on_sec_update ⇒ central_sys_attr_set
  [Calls]
  - >> central_sys_attr_set
  [Called By]
  - >> ble_bondmngr_on_ble_evt

  on_sec_param_request (Thumb, 52 bytes, Stack size 8 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = on_sec_param_request
  [Calls]
  - >> __aeabi_memclr4
  [Called By]
  - >> ble_bondmngr_on_ble_evt

  bm_pstorage_cb_handler (Thumb, 24 bytes, Stack size 24 bytes, ble_bondmngr.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = bm_pstorage_cb_handler
  [Address Reference Count : 1]
  - ble_bondmngr.o(.text)

  cmd_queue_init_element (Thumb, 64 bytes, Stack size 0 bytes, pstorage.o(.text))
  [Called By]

  - >> cmd_queue_dequeue
  - >> cmd_queue_init

  cmd_queue_init (Thumb, 32 bytes, Stack size 8 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = cmd_queue_init
  [Calls]
  - >> cmd_queue_init_element
  [Called By]
  - >> pstorage_init

  process_cmd (Thumb, 156 bytes, Stack size 24 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = process_cmd
  [Calls]
  - >> __aeabi_uidivmod
  [Called By]
  - >> cmd_queue_dequeue
  - >> cmd_queue_enqueue

  cmd_queue_enqueue (Thumb, 278 bytes, Stack size 40 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = cmd_queue_enqueue ⇒ process_cmd
  [Calls]
  - >> process_cmd
  [Called By]
  - >> pstorage_store
  - >> pstorage_clear

  app_notify (Thumb, 104 bytes, Stack size 24 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = app_notify
  [Called By]
  - >> pstorage_sys_event_handler
  - >> cmd_queue_dequeue

  cmd_queue_dequeue (Thumb, 92 bytes, Stack size 16 bytes, pstorage.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = cmd_queue_dequeue ⇒ app_notify
  [Calls]
  - >> app_notify
  - >> process_cmd
  - >> cmd_queue_init_element
  [Called By]
  - >> pstorage_sys_event_handler

  is_word_aligned (Thumb, 16 bytes, Stack size 0 bytes, pstorage.o(.text))
  [Called By]

  - >> pstorage_store
  - >> pstorage_load

  button_handler_execute (Thumb, 58 bytes, Stack size 16 bytes, app_button.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = button_handler_execute
  [Calls]
  - >> app_error_handler
  [Called By]
  - >> detection_delay_timeout_handler

  detection_delay_timeout_handler (Thumb, 112 bytes, Stack size 32 bytes, app_button.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = detection_delay_timeout_handler ⇒ button_handler_execute
  [Calls]
  - >> app_gpiote_pins_state_get
  - >> button_handler_execute
  [Address Reference Count : 1]
  - app_button.o(.text)

  gpiote_event_handler (Thumb, 46 bytes, Stack size 16 bytes, app_button.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = gpiote_event_handler ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> app_timer_stop
  - >> app_timer_start
  [Address Reference Count : 1]
  - app_button.o(.text)

  sense_level_toggle (Thumb, 124 bytes, Stack size 20 bytes, app_gpiote.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = sense_level_toggle
  [Called By]
  - >> GPIOTE_IRQHandler

  pins_sense_disable (Thumb, 96 bytes, Stack size 8 bytes, app_gpiote.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = pins_sense_disable
  [Called By]
  - >> app_gpiote_user_register
  - >> app_gpiote_user_disable

  NVIC_SetPriority (Thumb, 110 bytes, Stack size 8 bytes, app_gpiote.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = NVIC_SetPriority
  [Called By]
  - >> app_gpiote_init

  ### Undefined Global Symbols

  _call_atexit_fns (ARM, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> exit