# Static Call Graph for image .\_build\nrf52832_xxaa.axf

#<CALLGRAPH># ARM Linker, 5060528: Last Updated: Thu Aug 08 15:05:29 2019

### Maximum Stack Usage = 20 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

SystemInit

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemoryManagement_Handler ⇒ MemoryManagement_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- CCM_AAR_IRQHandler ⇒ CCM_AAR_IRQHandler

  ### Function Pointers

  - BusFault_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - CCM_AAR_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - COMP_LPCOMP_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - DebugMon_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - ECB_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - FPU_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - GPIOTE_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - HardFault_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - I2S_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - MWU_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - MemoryManagement_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - NFCT_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - NMI_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - PDM_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - POWER_CLOCK_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - PWM0_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - PWM1_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - PWM2_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - PendSV_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - QDEC_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - RADIO_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - RNG_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - RTC0_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - RTC1_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - RTC2_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - Reset_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SAADC_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SPIM1_SPIS1_TWIM1_TWIS1_SPI1_TWI1_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SPIM2_SPIS2_SPI2_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SVC_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SWI0_EGU0_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SWI1_EGU1_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SWI2_EGU2_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SWI3_EGU3_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SWI4_EGU4_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SWI5_EGU5_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SysTick_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SystemInit from system_nrf52.o(i.SystemInit) referenced from arm_startup_nrf52.o(.text)
  - TEMP_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - TIMER0_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - TIMER1_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - TIMER2_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - TIMER3_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - TIMER4_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - UARTE0_UART0_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - UsageFault_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - WDT_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from arm_startup_nrf52.o(.text)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  MemoryManagement_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> MemoryManagement_Handler
  [Called By]
  - >> MemoryManagement_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  CCM_AAR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> CCM_AAR_IRQHandler
  [Called By]
  - >> CCM_AAR_IRQHandler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  COMP_LPCOMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  ECB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  GPIOTE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  I2S_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  MWU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  NFCT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  PDM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  POWER_CLOCK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  PWM0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  PWM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  PWM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  QDEC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  RADIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  RTC0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  RTC1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  RTC2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  SAADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  SPIM1_SPIS1_TWIM1_TWIS1_SPI1_TWI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  SPIM2_SPIS2_SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  SWI0_EGU0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  SWI1_EGU1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  SWI2_EGU2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  SWI3_EGU3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  SWI4_EGU4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  SWI5_EGU5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  TEMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  TIMER0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  TIMER1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  TIMER2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  TIMER3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  TIMER4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  UARTE0_UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  Delay (Thumb, 24 bytes, Stack size 0 bytes, main.o(i.Delay))
  [Called By]

  - >> main

  SystemInit (Thumb, 726 bytes, Stack size 20 bytes, system_nrf52.o(i.SystemInit))
  [Stack]

  - Max Depth = 20
  - Call Chain = SystemInit
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(.text)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  main (Thumb, 48 bytes, Stack size 0 bytes, main.o(i.main))
  [Calls]

  - >> Delay
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  ### Undefined Global Symbols