Tool Versions:
Toolchain:       MDK-Lite  Version: 5.14.0.0
Toolchain Path:  C:\Keil_v5\ARM\ARMCC\Bin
C Compiler:      Armcc.exe V5.05 update 1 (build 106)
Assembler:       Armasm.exe V5.05 update 1 (build 106)
Linker/Locator:  ArmLink.exe V5.05 update 1 (build 106)
Library Manager: ArmAr.exe V5.05 update 1 (build 106)
Hex Converter:   FromElf.exe V5.05 update 1 (build 106)
CPU DLL:         SARMCM3.DLL V5.14.0.0
Dialog DLL:      DARMCM1.DLL V1.12.0.0
Target DLL:      UL2CM3.DLL V1.155.0.0
Dialog DLL:      TARMCM1.DLL V1.9.0.0

<H2>Project:</H2>
D:\Wearable\Sample_APP\Sample.uvprojx
Project File Date:  05/17/2015

<H2>Output:</H2>
Rebuild target 'Target 1'
compiling main.c...
compiling bsp.c...
compiling RTX_Conf_CM.c...
assembling arm_startup_nrf51.s...
compiling system_nrf51.c...
compiling ble_ancs_c.c...
compiling ble_bas.c...
C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.0\ble_services\ble_bas\ble_bas.c(254): error:  #20: identifier "ble_gatts_value_t" is undefined
      ble_gatts_value_t gatts_value;
C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.0\ble_services\ble_bas\ble_bas.c(271): error:  #165: too few arguments in function call
                                            &amp;gatts_value);
C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.0\ble_services\ble_bas\ble_bas.c: 0 warnings, 2 errors
compiling ble_bas_c.c...
compiling ble_cts_c.c...
compiling ble_srv_common.c...
compiling ble_db_discovery.c...
compiling nrf_drv_common.c...
compiling nrf_drv_gpiote.c...
compiling nrf_delay.c...
compiling app_uart.c...
compiling spi_master.c...
compiling app_button.c...
compiling app_error.c...
compiling app_timer.c...
compiling app_trace.c...
compiling nrf_assert.c...
compiling retarget.c...
".\Objects\Sample.axf" - 2 Error(s), 0 Warning(s).

<H2>Software Packages used:</H2>

Package Vendor: ARM
                http://www.keil.com/pack/ARM.CMSIS.4.3.0.pack
                ::CMSIS:RTOS:1.0 (API)
                CMSIS (Cortex Microcontroller Software Interface Standard)
   * Component: RTOS Version: 1.0
   * Component: CORE Version: 4.1.0
   * Component: Keil RTX Version: 4.78.0

Package Vendor: NordicSemiconductor
                http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_BLE/NordicSemiconductor.nRF_BLE.3.0.0.pack
                NordicSemiconductor::nRF_BLE:BLE_Services:ble_cts_c:3.0.0
                Bluetooth Low Energy (Bluetooth Smart) services and software modules for Nordic Semiconductor nRF family.
   * Component: ble_cts_c Version: 3.0.0
   * Component: ble_service_common Version: 3.0.0
   * Component: ble_bas Version: 3.0.0
   * Component: ble_bas_c Version: 3.0.0
   * Component: ble_db_discovery Version: 3.0.0
   * Component: ble_ancs_c Version: 3.0.0

Package Vendor: NordicSemiconductor
                http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_DeviceFamilyPack/NordicSemiconductor.nRF_DeviceFamilyPack.7.2.1.pack
                NordicSemiconductor::Device:Startup:7.2.1
                Nordic Semiconductor nRF ARM devices Device Family Pack.
   * Component: Startup Version: 7.2.1

Package Vendor: NordicSemiconductor
                http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_Drivers/NordicSemiconductor.nRF_Drivers.3.0.0.pack
                NordicSemiconductor::nRF_Drivers:nrf_delay:3.0.0
                Drivers for Nordic Semiconductor nRF family.
   * Component: nrf_delay Version: 3.0.0
   * Component: nrf_gpio Version: 3.0.0
   * Component: spi_master Version: 3.0.0
   * Component: nrf_gpiote Version: 3.0.0
   * Component: nrf_error Variant: default Version: 3.0.0
   * Component: nrf_soc Variant: default Version: 3.0.0
   * Component: nrf_drv_gpiote Version: 3.0.0
   * Component: nrf_drv_common Version: 3.0.0
   * Component: app_uart Variant: default Version: 3.0.0

Package Vendor: NordicSemiconductor
                http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_Examples/NordicSemiconductor.nRF_Examples.8.1.0.pack
                NordicSemiconductor::Board Support:bsp:default:8.1.0
                Examples and BSP for Nordic Semiconductor nRF family.
   * Component: bsp Variant: default Version: 8.1.0

Package Vendor: NordicSemiconductor
                http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_Libraries/NordicSemiconductor.nRF_Libraries.3.0.0.pack
                NordicSemiconductor::nRF_Libraries:app_button:3.0.0
                Software modules for Nordic Semiconductor nRF family.
   * Component: app_button Version: 3.0.0
   * Component: app_error Version: 3.0.0
   * Component: retarget Version: 3.0.0
   * Component: app_trace Variant: default Version: 3.0.0
   * Component: nrf_assert Version: 3.0.0
   * Component: app_timer Variant: default Version: 3.0.0
   * Component: app_util Variant: default Version: 3.0.0

Package Vendor: NordicSemiconductor
                http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_SoftDevice_Common/NordicSemiconductor.nRF_SoftDevice_Common.1.1.3.pack
                NordicSemiconductor::nRF_SoftDevice:Internal:softdevice_present:1.1.3
                Common components for Nordic Semiconductor nRF family SoftDevices.
   * Component: softdevice_present Version: 1.1.3

Package Vendor: NordicSemiconductor
                http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_SoftDevice_S310/NordicSemiconductor.nRF_SoftDevice_S310.2.0.0.pack
                NordicSemiconductor::nRF_SoftDevice:s310:default:2.0.0
                Components for combined ANT/ANT+ and BLE S310 SoftDevice for Nordic Semiconductor nRF family.
   * Component: s310 Variant: default Version: 2.0.0

<H2>Collection of Component include folders:</H2>
  D:\Wearable\Sample_APP\RTE
  D:\Wearable\Sample_APP\RTE\nRF_BLE\nRF51422_xxAC
  D:\Wearable\Sample_APP\RTE\nRF_Drivers\nRF51422_xxAC
  D:\Wearable\Sample_APP\RTE\nRF_Libraries\nRF51422_xxAC
  C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.3.0\CMSIS\Include
  C:\Keil_v5\ARM\PACK\ARM\CMSIS\4.3.0\CMSIS\RTOS\RTX\INC
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.0\ble_db_discovery
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.0\ble_services\ble_ancs_c
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.0\ble_services\ble_bas
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.0\ble_services\ble_bas_c
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.0\ble_services\ble_cts_c
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_BLE\3.0.0\common
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\7.2.1\Device\Include
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.0\common
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.0\config
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.0\gpiote
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.0\hal
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.0\spi_master
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\3.0.0\uart
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\8.1.0\bsp
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.0\button
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.0\timer
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.0\trace
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\3.0.0\util
  C:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_SoftDevice_S310\2.0.0\headers

<H2>Collection of Component Files used:</H2>

   * Component: ::CMSIS:RTOS:1.0 (API)

   * Component: ARM::CMSIS:CORE:4.1.0

   * Component: ARM::CMSIS:RTOS:Keil RTX:4.78.0
      Include file:  CMSIS\RTOS\RTX\INC\cmsis_os.h
      Source file:   CMSIS\RTOS\RTX\Templates\RTX_Conf_CM.c
      Include file:  CMSIS\RTOS\RTX\UserCodeTemplates\osObjects.h
      Source file:   CMSIS\RTOS\RTX\UserCodeTemplates\main.c
      Source file:   CMSIS\RTOS\RTX\UserCodeTemplates\MailQueue.c
      Source file:   CMSIS\RTOS\RTX\UserCodeTemplates\MemPool.c
      Source file:   CMSIS\RTOS\RTX\UserCodeTemplates\MsgQueue.c
      Source file:   CMSIS\RTOS\RTX\UserCodeTemplates\Mutex.c
      Source file:   CMSIS\RTOS\RTX\UserCodeTemplates\Semaphore.c
      Source file:   CMSIS\RTOS\RTX\UserCodeTemplates\Thread.c
      Source file:   CMSIS\RTOS\RTX\UserCodeTemplates\Timer.c
      Source file:   CMSIS\RTOS\RTX\SRC\ARM\SVC_Table.s
      Library file:  CMSIS\RTOS\RTX\LIB\ARM\RTX_CM0.lib

   * Component: NordicSemiconductor::nRF_BLE:BLE_Services:ble_cts_c:3.0.0
      Source file:   ble_services\ble_cts_c\ble_cts_c.c
      Include file:  ble_services\ble_cts_c\ble_cts_c.h

   * Component: NordicSemiconductor::nRF_BLE:BLE_Modules:ble_service_common:3.0.0
      Source file:   common\ble_srv_common.c
      Include file:  common\ble_srv_common.h

   * Component: NordicSemiconductor::nRF_BLE:BLE_Services:ble_bas:3.0.0
      Source file:   ble_services\ble_bas\ble_bas.c
      Include file:  ble_services\ble_bas\ble_bas.h

   * Component: NordicSemiconductor::nRF_BLE:BLE_Services:ble_bas_c:3.0.0
      Source file:   ble_services\ble_bas_c\ble_bas_c.c
      Include file:  ble_services\ble_bas_c\ble_bas_c.h

   * Component: NordicSemiconductor::nRF_BLE:BLE_Modules:ble_db_discovery:3.0.0
      Source file:   ble_db_discovery\ble_db_discovery.c
      Include file:  ble_db_discovery\ble_db_discovery.h

   * Component: NordicSemiconductor::nRF_BLE:BLE_Services:ble_ancs_c:3.0.0
      Source file:   ble_services\ble_ancs_c\ble_ancs_c.c
      Include file:  ble_services\ble_ancs_c\ble_ancs_c.h

   * Component: NordicSemiconductor::Device:Startup:7.2.1
      Source file:   Device\Source\arm\arm_startup_nrf51.s
      Source file:   Device\Source\system_nrf51.c
      Include file:  Device\Include\system_nrf51.h

   * Component: NordicSemiconductor::nRF_Drivers:nrf_delay:3.0.0
      Source file:   hal\nrf_delay.c
      Include file:  hal\nrf_delay.h

   * Component: NordicSemiconductor::nRF_Drivers:nrf_gpio:3.0.0
      Include file:  hal\nrf_gpio.h

   * Component: NordicSemiconductor::nRF_Drivers:spi_master:3.0.0
      Source file:   spi_master\spi_master.c
      Include file:  spi_master\spi_master.h

   * Component: NordicSemiconductor::nRF_Drivers:nrf_gpiote:3.0.0
      Include file:  hal\nrf_gpiote.h

   * Component: NordicSemiconductor::nRF_Drivers:nrf_error:default:3.0.0

   * Component: NordicSemiconductor::nRF_Drivers:nrf_soc:default:3.0.0

   * Component: NordicSemiconductor::nRF_Drivers:nrf_drv_gpiote:3.0.0
      Source file:   gpiote\nrf_drv_gpiote.c
      Include file:  gpiote\nrf_drv_gpiote.h
      Include file:  config\nrf_drv_config.h

   * Component: NordicSemiconductor::nRF_Drivers:nrf_drv_common:3.0.0
      Source file:   common\nrf_drv_common.c
      Include file:  common\nrf_drv_common.h

   * Component: NordicSemiconductor::nRF_Drivers:app_uart:default:3.0.0
      Source file:   uart\app_uart.c
      Include file:  uart\app_uart.h

   * Component: NordicSemiconductor::Board Support:bsp:default:8.1.0
      Source file:   bsp\bsp.c

   * Component: NordicSemiconductor::nRF_Libraries:app_button:3.0.0
      Source file:   button\app_button.c
      Include file:  button\app_button.h

   * Component: NordicSemiconductor::nRF_Libraries:app_error:3.0.0
      Source file:   util\app_error.c
      Include file:  util\app_error.h

   * Component: NordicSemiconductor::nRF_Libraries:retarget:3.0.0
      Source file:   uart\retarget.c

   * Component: NordicSemiconductor::nRF_Libraries:app_trace:default:3.0.0
      Source file:   trace\app_trace.c
      Include file:  trace\app_trace.h

   * Component: NordicSemiconductor::nRF_Libraries:nrf_assert:3.0.0
      Source file:   util\nrf_assert.c
      Include file:  util\nrf_assert.h

   * Component: NordicSemiconductor::nRF_Libraries:app_timer:default:3.0.0
      Source file:   timer\app_timer.c
      Include file:  timer\app_timer.h

   * Component: NordicSemiconductor::nRF_Libraries:app_util:default:3.0.0

   * Component: NordicSemiconductor::nRF_SoftDevice:Internal:softdevice_present:1.1.3

   * Component: NordicSemiconductor::nRF_SoftDevice:s310:default:2.0.0
      Include file:  headers\ant_error.h
      Include file:  headers\ant_interface.h
      Include file:  headers\ant_parameters.h
      Include file:  headers\ble.h
      Include file:  headers\ble_err.h
      Include file:  headers\ble_gap.h
      Include file:  headers\ble_gatt.h
      Include file:  headers\ble_gattc.h
      Include file:  headers\ble_gatts.h
      Include file:  headers\ble_hci.h
      Include file:  headers\ble_l2cap.h
      Include file:  headers\ble_ranges.h
      Include file:  headers\ble_types.h
      Include file:  headers\nrf_error.h
      Include file:  headers\nrf_error_sdm.h
      Include file:  headers\nrf_error_soc.h
      Include file:  headers\nrf_mbr.h
      Include file:  headers\nrf_sdm.h
      Include file:  headers\nrf_soc.h
      Include file:  headers\nrf_svc.h
      Include file:  headers\softdevice_assert.h
Target not created.
</PRE>