ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x25e9
  Start of program headers:          52 (bytes into file)
  Start of section headers:          1440348 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         5
  Size of section headers:           40 (bytes)
  Number of section headers:         35
  Section header string table index: 34

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        00000000 0000e0 0004c8 00  AX  0   0  4
  [ 2] text              PROGBITS        000004c8 0005a8 009648 00  AX  0   0  8
  [ 3] .ARM.exidx        ARM_EXIDX       00009b10 009bf0 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        00009b18 009bf8 000078 00   A  0   0  4
  [ 5] device_area       PROGBITS        00009b90 009c70 0000c4 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        00009c54 009d34 000910 00   A  0   0  4
  [ 7] flash_driver[...] PROGBITS        0000a564 00a644 000018 00   A  0   0  4
  [ 8] gpio_driver_[...] PROGBITS        0000a57c 00a65c 000024 00   A  0   0  4
  [ 9] clock_contro[...] PROGBITS        0000a5a0 00a680 00001c 00   A  0   0  4
  [10] uart_driver_[...] PROGBITS        0000a5bc 00a69c 00000c 00   A  0   0  4
  [11] log_const_area    PROGBITS        0000a5c8 00a6a8 000010 00   A  0   0  4
  [12] log_backend_area  PROGBITS        0000a5d8 00a6b8 000010 00   A  0   0  4
  [13] rodata            PROGBITS        0000a5f0 00a6d0 000c2c 00   A  0   0 16
  [14] NRF_KMU_RESE[...] NOBITS          20000000 00b5d8 000060 00  WA  0   0  1
  [15] .ramfunc          PROGBITS        20000060 00b300 000040 00  AX  0   0  4
  [16] datas             PROGBITS        200000a0 00b340 00027e 00  WA  0   0  8
  [17] device_states     PROGBITS        2000031e 00b5be 000012 00  WA  0   0  1
  [18] log_msg_ptr_area  PROGBITS        20000330 00b5d0 000004 00  WA  0   0  4
  [19] .comment          PROGBITS        00000000 00b5d8 000020 01  MS  0   0  1
  [20] .debug_aranges    PROGBITS        00000000 00b5f8 002d08 00      0   0  8
  [21] .debug_info       PROGBITS        00000000 00e300 08005e 00      0   0  1
  [22] .debug_abbrev     PROGBITS        00000000 08e35e 01784b 00      0   0  1
  [23] .debug_line       PROGBITS        00000000 0a5ba9 03b2d4 00      0   0  1
  [24] .debug_frame      PROGBITS        00000000 0e0e80 007080 00      0   0  4
  [25] .debug_str        PROGBITS        00000000 0e7f00 0171da 01  MS  0   0  1
  [26] .debug_loc        PROGBITS        00000000 0ff0da 0417b6 00      0   0  1
  [27] .debug_ranges     PROGBITS        00000000 140890 0081e8 00      0   0  8
  [28] .ARM.attributes   ARM_ATTRIBUTES  00000000 148a78 000038 00      0   0  1
  [29] .last_section     PROGBITS        0000b4f0 00b5d4 000004 00  WA  0   0  4
  [30] bss               NOBITS          20000338 00b5d8 00366f 00  WA  0   0  8
  [31] noinit            NOBITS          200039a8 00b5d8 003000 00  WA  0   0  8
  [32] .symtab           SYMTAB          00000000 148ab0 00bb60 10     33 1529  4
  [33] .strtab           STRTAB          00000000 154610 00b289 00      0   0  1
  [34] .shstrtab         STRTAB          00000000 15f899 0001c1 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  D (mbind), y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x009bf0 0x00009b10 0x00009b10 0x00008 0x00008 R   0x4
  LOAD           0x0000e0 0x00000000 0x00000000 0x0b21c 0x0b21c R E 0x10
  LOAD           0x00b300 0x20000060 0x0000b21c 0x002d4 0x002d4 RWE 0x8
  LOAD           0x00b5d4 0x0000b4f0 0x0000b4f0 0x00004 0x00004 RW  0x4
  LOAD           0x000000 0x20000000 0x20000000 0x00000 0x069a8 RW  0x8

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel device_area sw_isr_table flash_driver_api_area gpio_driver_api_area clock_control_driver_api_area uart_driver_api_area log_const_area log_backend_area rodata 
   02     .ramfunc datas device_states log_msg_ptr_area 
   03     .last_section 
   04     NRF_KMU_RESERVED_PUSH_SECTION bss noinit 
