3;13:10:11.4120 [MainThread] Master Control Panel 3.7.1.8567
4;13:10:11.8850 [MainThread] nrfjprog.dll 5.2.0.45231
5;13:10:11.8860 [MainThread] JLinkARM.dll 4.97d
6;13:10:11.8880 [MainThread] 480104015 - COM5
7;13:10:11.8880 [MainThread] ftd2xx not used.
8;13:10:11.8960 [MainThread] nrfjprog.dll 5.2.0.45231
9;13:10:11.9320 [MainThread] HciJLinkDriver opened (COM5, 115200-8-None-1-RequestToSend)
10;13:10:11.9390 [480104015][MainThread] JLinkARM.dll 4.97d
11;13:10:11.9410 [480104015][MainThread] 480104015 - COM5
12;13:10:13.0582 [480104015][MainThread] HCI command: BTLE_CMD_READ_BD_ADDR
13;13:10:13.0602 [480104015][MainThread] Serial port write: 01-09-10-00
14;13:10:13.0632 [480104015][MainThread] Waiting for event packet. Timeout is 500ms
15;13:10:13.0642 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-0A-01-09-10-00-56-FF-99-00-CD-29
16;13:10:13.0762 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: BTLE_CMD_READ_BD_ADDR, Status: BTLE_STATUS_CODE_SUCCESS, BdAddress: 0x29CD0099FF56
17;13:10:13.0762 [480104015][MainThread] Finished waiting for event packet. PacketReceived:True
18;13:10:13.0802 [480104015][MainThread] HCI command: NRF_CMD_SET_BD_ADDR, Address: 0x4E-25-87-A6-B7-8A
19;13:10:13.0802 [480104015][MainThread] Serial port write: 01-03-FC-06-4E-25-87-A6-B7-8A
20;13:10:13.0802 [480104015][MainThread] Waiting for event packet. Timeout is 500ms
21;13:10:13.0832 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-04-01-03-FC-00
22;13:10:13.0832 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: NRF_CMD_SET_BD_ADDR, Status: BTLE_STATUS_CODE_SUCCESS
23;13:10:13.0842 [480104015][MainThread] Finished waiting for event packet. PacketReceived:True
24;13:10:13.0852 [480104015][MainThread] HCI command: NRF_CMD_GET_VERSION_INFO
25;13:10:13.0852 [480104015][MainThread] Serial port write: 01-06-FC-00
26;13:10:13.0852 [480104015][MainThread] Waiting for event packet. Timeout is 500ms
27;13:10:13.0912 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-2C-01-06-FC-00-6D-65-66-77-5F-6E-72-66-35-31-38-32-32-5F-30-2E-39-2E-30-2E-31-30-30-32-32-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00
28;13:10:13.0912 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: NRF_CMD_GET_VERSION_INFO, Status: BTLE_STATUS_CODE_SUCCESS, VersionInfo: mefw_nrf51822_0.9.0.10022
29;13:10:13.0912 [480104015][MainThread] Finished waiting for event packet. PacketReceived:True
30;13:10:15.9973 [480104015][ScriptThread]  - - Start of script: (2015-03-18 20:10:15) - - 
31;13:10:16.0073 [480104015][ScriptThread] 
32;13:10:16.1384 [480104015][ScriptThread] HCI command: BTLE_CMD_READ_BD_ADDR
33;13:10:16.1434 [480104015][ScriptThread] Serial port write: 01-09-10-00
34;13:10:16.1454 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-0A-01-09-10-00-4E-25-87-A6-B7-8A
35;13:10:16.1454 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: BTLE_CMD_READ_BD_ADDR, Status: BTLE_STATUS_CODE_SUCCESS, BdAddress: 0x8AB7A687254E
36;13:10:16.3914 [480104015][ScriptThread] Device address: 0x8AB7A687254E
37;13:10:16.3984 [480104015][ScriptThread] Ready
38;13:10:16.4774 [480104015][] Successfully parsed the server setup: 
1: R_PERM:yes NOTIFY:no UUID:0x2800 W_PERM:no INDICATE:no DATA:0x[0, 18]
2: R_PERM:yes NOTIFY:no UUID:0x2803 W_PERM:no INDICATE:no DATA:0x[6, 3, 0, 0, 2A]
3: R_PERM:yes NOTIFY:no UUID:0x2A00 W_PERM:yes INDICATE:no DATA:0x[4D, 61, 73, 74, 65, 72, 20, 43, 6F, 6E, 74, 72, 6F, 6C, 20, 50, 61, 6E, 65, 6C]
4: R_PERM:yes NOTIFY:no UUID:0x2800 W_PERM:no INDICATE:no DATA:0x[1, 18]
39;13:10:16.4784 [480104015][] CreateServerFromObject()
40;13:10:16.4804 [480104015][] Starting Server
41;13:10:16.6254 [480104015][MainThread] ServerStartupWorker completed
42;13:10:16.6274 [480104015][] SERVER: Server has started
43;13:10:48.1040 [480104015][MainThread] HciH4Driver closed
44;13:10:49.1073 [480104015][MainThread] nrfjprog.dll 5.2.0.45231
45;13:10:49.1113 [480104015][MainThread] HciJLinkDriver opened (COM5, 115200-8-None-1-RequestToSend)
46;13:10:49.1133 [480104015][MainThread] JLinkARM.dll 4.97d
47;13:10:49.1413 [480104015][MainThread] 480104015 - COM5
48;13:10:50.1030 [480104015][MainThread] HCI command: BTLE_CMD_READ_BD_ADDR
49;13:10:50.1030 [480104015][MainThread] Serial port write: 01-09-10-00
50;13:10:50.1030 [480104015][MainThread] Waiting for event packet. Timeout is 500ms
51;13:10:50.1060 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-0A-01-09-10-00-56-FF-99-00-CD-29
52;13:10:50.1060 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: BTLE_CMD_READ_BD_ADDR, Status: BTLE_STATUS_CODE_SUCCESS, BdAddress: 0x29CD0099FF56
53;13:10:50.1060 [480104015][MainThread] Finished waiting for event packet. PacketReceived:True
54;13:10:50.1060 [480104015][MainThread] HCI command: NRF_CMD_SET_BD_ADDR, Address: 0x4E-25-87-A6-B7-8A
55;13:10:50.1060 [480104015][MainThread] Serial port write: 01-03-FC-06-4E-25-87-A6-B7-8A
56;13:10:50.1070 [480104015][MainThread] Waiting for event packet. Timeout is 500ms
57;13:10:50.1090 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-04-01-03-FC-00
58;13:10:50.1090 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: NRF_CMD_SET_BD_ADDR, Status: BTLE_STATUS_CODE_SUCCESS
59;13:10:50.1090 [480104015][MainThread] Finished waiting for event packet. PacketReceived:True
60;13:10:50.1090 [480104015][MainThread] HCI command: NRF_CMD_GET_VERSION_INFO
61;13:10:50.1090 [480104015][MainThread] Serial port write: 01-06-FC-00
62;13:10:50.1099 [480104015][MainThread] Waiting for event packet. Timeout is 500ms
63;13:10:50.1150 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-2C-01-06-FC-00-6D-65-66-77-5F-6E-72-66-35-31-38-32-32-5F-30-2E-39-2E-30-2E-31-30-30-32-32-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00
64;13:10:50.1150 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: NRF_CMD_GET_VERSION_INFO, Status: BTLE_STATUS_CODE_SUCCESS, VersionInfo: mefw_nrf51822_0.9.0.10022
65;13:10:50.1150 [480104015][MainThread] Finished waiting for event packet. PacketReceived:True
66;13:10:50.2440 [480104015][ScriptThread]  - - Start of script: (2015-03-18 20:10:50) - - 
67;13:10:50.2500 [480104015][ScriptThread] 
68;13:10:50.2820 [480104015][ScriptThread] HCI command: BTLE_CMD_READ_BD_ADDR
69;13:10:50.2830 [480104015][ScriptThread] Serial port write: 01-09-10-00
70;13:10:50.2860 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-0A-01-09-10-00-4E-25-87-A6-B7-8A
71;13:10:50.2860 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: BTLE_CMD_READ_BD_ADDR, Status: BTLE_STATUS_CODE_SUCCESS, BdAddress: 0x8AB7A687254E
72;13:10:50.3610 [480104015][ScriptThread] Device address: 0x8AB7A687254E
73;13:10:50.3630 [480104015][ScriptThread] Ready
74;13:10:50.4645 [480104015][] Successfully parsed the server setup: 
1: R_PERM:yes NOTIFY:no UUID:0x2800 W_PERM:no INDICATE:no DATA:0x[0, 18]
2: R_PERM:yes NOTIFY:no UUID:0x2803 W_PERM:no INDICATE:no DATA:0x[6, 3, 0, 0, 2A]
3: R_PERM:yes NOTIFY:no UUID:0x2A00 W_PERM:yes INDICATE:no DATA:0x[4D, 61, 73, 74, 65, 72, 20, 43, 6F, 6E, 74, 72, 6F, 6C, 20, 50, 61, 6E, 65, 6C]
4: R_PERM:yes NOTIFY:no UUID:0x2800 W_PERM:no INDICATE:no DATA:0x[1, 18]
75;13:10:50.4655 [480104015][] CreateServerFromObject()
76;13:10:50.4665 [480104015][] Starting Server
77;13:10:50.5155 [480104015][MainThread] ServerStartupWorker completed
78;13:10:50.5175 [480104015][] SERVER: Server has started
79;13:11:22.4002 [480104015][ScriptMethodCallThread] SERVER: Stopping server
80;13:11:22.4012 [480104015][ScriptMethodCallThread] Waiting for server to terminate
81;13:11:22.6279 [480104015][] SERVER: Server has stopped
82;13:11:30.3715 [480104015][MainThread] Successfully parsed the server setup: 
1: R_PERM:yes NOTIFY:no UUID:0x2800 W_PERM:no INDICATE:no DATA:0x[D0, 0, 2D, 12, 1E, 4B, F, A4, 99, 4E, CE, B5, 31, F4, 5, 79]
2: R_PERM:yes NOTIFY:no UUID:0x2803 W_PERM:no INDICATE:no DATA:0x[10, 3, 0, BD, 1D, A2, 99, E6, 25, 58, 8C, D9, 42, 1, 63, D, 12, BF, 9F]
3: R_PERM:no NOTIFY:yes UUID:0x9FBF120D630142D98C5825E699A21DBD W_PERM:no INDICATE:no DATA:0x[0]
4: R_PERM:yes NOTIFY:no UUID:0x2902 W_PERM:yes INDICATE:no DATA:0x[0]
5: R_PERM:yes NOTIFY:no UUID:0x2803 W_PERM:no INDICATE:no DATA:0x[4, 6, 0, D9, D9, AA, FD, BD, 9B, 21, 98, A8, 49, E1, 45, F3, D8, D1, 69]
6: R_PERM:no NOTIFY:no UUID:0x69D1D8F345E149A898219BBDFDAAD9D9 W_PERM:yes INDICATE:no DATA:0x[0]
7: R_PERM:yes NOTIFY:no UUID:0x2803 W_PERM:no INDICATE:no DATA:0x[10, 8, 0, FB, 7B, 7C, CE, 6A, B3, 44, BE, B5, 4B, D6, 24, E9, C6, EA, 22]
8: R_PERM:no NOTIFY:yes UUID:0x22EAC6E924D64BB5BE44B36ACE7C7BFB W_PERM:no INDICATE:no DATA:0x[0]
9: R_PERM:yes NOTIFY:no UUID:0x2902 W_PERM:yes INDICATE:no DATA:0x[0]
83;13:11:30.3725 [480104015][MainThread] Starting Server
84;13:11:30.3795 [480104015][] SERVER: Server has started
85;13:11:42.0847 [480104015][MainThread] HCI command: BTLE_CMD_LE_READ_BUFFER_SIZE
86;13:11:42.0858 [480104015][MainThread] Serial port write: 01-02-20-00
87;13:11:42.0858 [480104015][MainThread] Waiting for event packet. Timeout is 500ms
88;13:11:42.0881 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-07-01-02-20-00-1B-00-02
89;13:11:42.0881 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: BTLE_CMD_LE_READ_BUFFER_SIZE, Status: BTLE_STATUS_CODE_SUCCESS, PacketLength: 27, PacketBufferDepth: 2
90;13:11:42.0891 [480104015][MainThread] Finished waiting for event packet. PacketReceived:True
91;13:11:42.0931 [480104015][MainThread] HCI command: BTLE_CMD_LE_WRITE_SCAN_PARAMETERS, ScanType: BTLE_SCAN_TYPE_ACTIVE, ScanInterval: 250ms, ScanWindow: 50ms, OwnAddressType: BTLE_ADDR_TYPE_PUBLIC, FilterPolicy: BTLE_SCAN_FILTER_ACCEPT_ANY
92;13:11:42.0941 [480104015][MainThread] Serial port write: 01-0B-20-07-01-90-01-50-00-00-00
93;13:11:42.0941 [480104015][MainThread] Waiting for event packet. Timeout is 500ms
94;13:11:42.1061 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-04-01-0B-20-00
95;13:11:42.1061 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: BTLE_CMD_LE_WRITE_SCAN_PARAMETERS, Status: BTLE_STATUS_CODE_SUCCESS
96;13:11:42.1061 [480104015][MainThread] Finished waiting for event packet. PacketReceived:True
97;13:11:42.1071 [480104015][MainThread] HCI command: BTLE_CMD_LE_WRITE_SCAN_ENABLE, ScanMode: BTLE_SCAN_MODE_ENABLE, FilterMode: BTLE_SCAN_DUPLICATE_FILTER_DISABLE
98;13:11:42.1071 [480104015][MainThread] Serial port write: 01-0C-20-02-01-00
99;13:11:42.1071 [480104015][MainThread] Waiting for event packet. Timeout is 500ms
100;13:11:42.1111 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-04-01-0C-20-00
101;13:11:42.1121 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: BTLE_CMD_LE_WRITE_SCAN_ENABLE, Status: BTLE_STATUS_CODE_SUCCESS
102;13:11:42.1121 [480104015][MainThread] Finished waiting for event packet. PacketReceived:True
103;13:12:04.1621 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-CB
104;13:12:04.1841 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -53dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
105;13:12:04.2211 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-CC
106;13:12:04.2211 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -52dBm, DataLength: 0, Data: 
107;13:12:04.4122 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-CE
108;13:12:04.4132 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -50dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
109;13:12:04.4262 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-CE
110;13:12:04.4262 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -50dBm, DataLength: 0, Data: 
111;13:12:04.6626 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-D4
112;13:12:04.6626 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -44dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
113;13:12:04.6726 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D3
114;13:12:04.6726 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -45dBm, DataLength: 0, Data: 
115;13:12:04.9126 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-D3
116;13:12:04.9126 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -45dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
117;13:12:04.9166 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D4
118;13:12:04.9166 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -44dBm, DataLength: 0, Data: 
119;13:12:05.1626 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-D4
120;13:12:05.1626 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -44dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
121;13:12:05.1656 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D4
122;13:12:05.1666 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -44dBm, DataLength: 0, Data: 
123;13:12:05.4126 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-D4
124;13:12:05.4126 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -44dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
125;13:12:05.4266 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D3
126;13:12:05.4276 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -45dBm, DataLength: 0, Data: 
127;13:12:05.6627 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-D2
128;13:12:05.6627 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -46dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
129;13:12:05.6846 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D3
130;13:12:05.6846 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -45dBm, DataLength: 0, Data: 
131;13:12:05.9126 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-D4
132;13:12:05.9126 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -44dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
133;13:12:05.9227 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D3
134;13:12:05.9227 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -45dBm, DataLength: 0, Data: 
135;13:12:06.1621 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-D4
136;13:12:06.1631 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -44dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
137;13:12:06.1751 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D3
138;13:12:06.1761 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -45dBm, DataLength: 0, Data: 
139;13:12:06.4126 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-D2
140;13:12:06.4126 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -46dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
141;13:12:06.4156 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D3
142;13:12:06.4156 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -45dBm, DataLength: 0, Data: 
143;13:12:06.6622 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-D3
144;13:12:06.6632 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -45dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
145;13:12:06.6682 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D3
146;13:12:06.6682 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -45dBm, DataLength: 0, Data: 
147;13:12:06.9127 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-D4
148;13:12:06.9127 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -44dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
149;13:12:06.9227 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D4
150;13:12:06.9227 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -44dBm, DataLength: 0, Data: 
151;13:12:07.1866 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-D2
152;13:12:07.1866 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -46dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
153;13:12:07.1906 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D3
154;13:12:07.1906 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -45dBm, DataLength: 0, Data: 
155;13:12:07.4092 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-CF
156;13:12:07.4102 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -49dBm, DataLength: 0, Data: 
157;13:12:07.4142 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-CF
158;13:12:07.4152 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -49dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
159;13:12:07.6627 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-C6
160;13:12:07.6627 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -58dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
161;13:12:07.6927 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-C5
162;13:12:07.6927 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -59dBm, DataLength: 0, Data: 
163;13:12:07.9220 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-CD
164;13:12:07.9220 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -51dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
165;13:12:07.9280 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-CE
166;13:12:07.9280 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -50dBm, DataLength: 0, Data: 
167;13:12:08.1628 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-D2
168;13:12:08.1628 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -46dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
169;13:12:08.1698 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D2
170;13:12:08.1698 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -46dBm, DataLength: 0, Data: 
171;13:12:08.4124 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-D1
172;13:12:08.4134 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -47dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
173;13:12:08.4193 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D0
174;13:12:08.4193 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -48dBm, DataLength: 0, Data: 
175;13:12:08.6623 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-D1
176;13:12:08.6633 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -47dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
177;13:12:08.6773 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D2
178;13:12:08.6773 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -46dBm, DataLength: 0, Data: 
179;13:12:08.9129 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-CF
180;13:12:08.9129 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -49dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
181;13:12:08.9139 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-CF
182;13:12:08.9149 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -49dBm, DataLength: 0, Data: 
183;13:12:09.1620 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-CF
184;13:12:09.1630 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -49dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
185;13:12:09.1640 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-CF
186;13:12:09.1650 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -49dBm, DataLength: 0, Data: 
187;13:12:09.4120 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-CF
188;13:12:09.4130 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -49dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
189;13:12:09.4140 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D0
190;13:12:09.4150 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -48dBm, DataLength: 0, Data: 
191;13:12:09.6620 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-CF
192;13:12:09.6630 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -49dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
193;13:12:09.6640 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-CF
194;13:12:09.6640 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -49dBm, DataLength: 0, Data: 
195;13:12:09.9128 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-CE
196;13:12:09.9128 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -50dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
197;13:12:09.9207 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-CE
198;13:12:09.9207 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -50dBm, DataLength: 0, Data: 
199;13:12:10.1628 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-CF
200;13:12:10.1628 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -49dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
201;13:12:10.1648 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D1
202;13:12:10.1648 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -47dBm, DataLength: 0, Data: 
203;13:12:10.4127 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-CD
204;13:12:10.4127 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -51dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
205;13:12:10.4197 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-CD
206;13:12:10.4207 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -51dBm, DataLength: 0, Data: 
207;13:12:10.6631 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-CE
208;13:12:10.6631 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -50dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
209;13:12:10.6651 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-CE
210;13:12:10.6661 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -50dBm, DataLength: 0, Data: 
211;13:12:10.9125 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-D0
212;13:12:10.9125 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -48dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
213;13:12:10.9145 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D1
214;13:12:10.9145 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -47dBm, DataLength: 0, Data: 
215;13:12:11.1629 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-CD
216;13:12:11.1629 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -51dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
217;13:12:11.1649 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-CD
218;13:12:11.1649 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -51dBm, DataLength: 0, Data: 
219;13:12:11.4127 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-CE
220;13:12:11.4127 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -50dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
221;13:12:11.4147 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-CE
222;13:12:11.4147 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -50dBm, DataLength: 0, Data: 
223;13:12:11.6630 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-CF
224;13:12:11.6630 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -49dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
225;13:12:11.6650 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-D1
226;13:12:11.6650 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -47dBm, DataLength: 0, Data: 
227;13:12:11.9116 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-CD
228;13:12:11.9116 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -51dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
229;13:12:11.9186 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-CD
230;13:12:11.9196 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -51dBm, DataLength: 0, Data: 
231;13:12:12.0303 [480104015][MainThread] HCI command: BTLE_CMD_LE_WRITE_SCAN_ENABLE, ScanMode: BTLE_SCAN_MODE_DISABLE, FilterMode: BTLE_SCAN_DUPLICATE_FILTER_DISABLE
232;13:12:12.0313 [480104015][MainThread] Serial port write: 01-0C-20-02-00-00
233;13:12:12.0313 [480104015][MainThread] Waiting for event packet. Timeout is 500ms
234;13:12:12.1593 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-04-01-0C-20-00
235;13:12:12.1603 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: BTLE_CMD_LE_WRITE_SCAN_ENABLE, Status: BTLE_STATUS_CODE_SUCCESS
236;13:12:12.1603 [480104015][MainThread] Finished waiting for event packet. PacketReceived:True
237;13:12:12.1673 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-2B-02-01-00-01-D6-C2-86-74-1B-E6-1F-05-09-41-4E-43-43-03-19-00-00-02-01-05-11-15-D0-00-2D-12-1E-4B-0F-A4-99-4E-CE-B5-31-F4-05-79-CE
238;13:12:12.1683 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_ADV_IND, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -50dBm, DataLength: 31, Data: CompleteLocalName:ANCC Appearance:0x0000 Flags:LimitedDiscoverable, BrEdrNotSupported SolicitedServicesUuid128:0x7905F431B5CE4E99A40F4B1E122D00D0 
239;13:12:12.1693 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0C-02-01-04-01-D6-C2-86-74-1B-E6-00-CE
240;13:12:12.1693 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_ADVERTISING_REPORT, EventType: BTLE_REPORT_TYPE_SCAN_RSP, AddressType: BTLE_ADDR_TYPE_RANDOM, DeviceAddress: 0xE61B7486C2D6, RSSI: -50dBm, DataLength: 0, Data: 
241;13:12:15.6611 [480104015][MainThread] ConnectToDevice(peerAddress="D6C286741BE6",addressTypePeer=1,scanInterval=400,scanWindow=320,connIntervalMin=16,connIntervalMax=16,connLatency=0,connTimeout=300)
242;13:12:15.7651 [480104015][ScriptMethodCallThread] Enter Connect
243;13:12:15.7771 [480104015][ScriptMethodCallThread] TST-Client: Sending Create LL connection to E61B7486C2D6
244;13:12:15.9411 [480104015][ScriptMethodCallThread] HCI command: BTLE_CMD_LE_CREATE_CONNECTION, ConnIntervalMin: 20ms, ConnIntervalMax: 20ms, SupervisionTimeout: 3000ms, PeerAddress: 0xD6-C2-86-74-1B-E6, PeerAddressType: BTLE_ADDR_TYPE_RANDOM, OwnAddressType: BTLE_ADDR_TYPE_PUBLIC, ConnLatency: 0, ScanInterval: 250ms, ScanWindow: 200ms, FilterPolicy: BTLE_INITIATOR_FILTER_SKIP_WHITELIST, MinCeLength: 160, MaxCeLength: 160
245;13:12:15.9421 [480104015][ScriptMethodCallThread] Serial port write: 01-0D-20-19-90-01-40-01-00-01-D6-C2-86-74-1B-E6-00-10-00-10-00-00-00-2C-01-A0-00-A0-00
246;13:12:15.9581 [480104015][ReadPacketQueueThread] Serial port read: 04-0F-04-00-01-0D-20
247;13:12:15.9581 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_STATUS, OpCode: BTLE_CMD_LE_CREATE_CONNECTION, Status: BTLE_STATUS_CODE_SUCCESS
248;13:12:15.9951 [480104015][ScriptMethodCallThread] TST-Client: Waiting for LL Connection Created Event
249;13:12:16.2081 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-13-01-00-00-00-00-01-D6-C2-86-74-1B-E6-10-00-00-00-2C-01-01
250;13:12:16.2101 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_CONNECTION_COMPLETE, Status: BTLE_STATUS_CODE_SUCCESS, ConnectionHandle: 0x0000, Role: BTLE_CONNECTION_ROLE_MASTER, AddressType: BTLE_ADDR_TYPE_RANDOM, PeerAddress: 0xE61B7486C2D6, ConnectionInterval: 20ms, Latency: 0, Timeout: 3000ms, ClockAccuracy: BTLE_CLOCK_ACCURACY_250_PPM
251;13:12:16.2662 [480104015][ScriptMethodCallThread] TST-Client: Connection created successful. ConnectionId: 0
252;13:12:16.2711 [480104015][ScriptMethodCallThread] ----------------------------
253;13:12:16.2711 [480104015][ScriptMethodCallThread] Connected to device
254;13:12:16.2711 [480104015][ScriptMethodCallThread] Role: 0
255;13:12:16.2711 [480104015][ScriptMethodCallThread] PeerAddressType: 1
256;13:12:16.2721 [480104015][ScriptMethodCallThread] PeerAddress (MSB): E61B7486C2D6
257;13:12:16.2881 [480104015][ScriptMethodCallThread] Connection Interval: 20.0ms
258;13:12:16.2881 [480104015][ScriptMethodCallThread] Connection Latency: 0
259;13:12:16.2891 [480104015][ScriptMethodCallThread] Supervision Timeout: 3000ms
260;13:12:16.2891 [480104015][ScriptMethodCallThread] Clock Accuracy: (1)
261;13:12:16.2891 [480104015][ScriptMethodCallThread] ----------------------------
262;13:12:16.2901 [480104015][ScriptMethodCallThread] Connected to E61B7486C2D6
263;13:12:16.2931 [480104015][] SERVER: Received packet <HciEvent: eventCode=0x05> - <HciEvent: eventCode=0x05>
264;13:12:21.2300 [480104015][ReadPacketQueueThread] Serial port read: 02-00-20-10-00-0C-00-05-00-12-02-08-00-90-01-20-03-00-00-90-01
265;13:12:21.2830 [480104015][ReadPacketQueueThread] Received packet: L2capConnectionParameterUpdateRequest, 12-02-08-00-90-01-20-03-00-00-90-01, IntervalMin: 500ms, IntervalMax: 1000ms, SlaveLatency: 0, Timeout: 4000ms
266;13:12:21.3500 [480104015][ScriptThread] Received Connection Parameter Update Request
267;13:12:21.4380 [480104015][ScriptThread] launching connection update worker
268;13:12:21.5060 [480104015][] BackgroundWorker completed
269;13:12:21.5160 [480104015][ScriptMethodCallThread] WRITE DATA PACKET:06-00-05-00-13-02-02-00-00-00
270;13:12:21.5170 [480104015][ScriptMethodCallThread] Sending packet: L2capConnectionParameterUpdateResponse, 13-02-02-00-00-00, Result: ConnectionParametersAccepted
271;13:12:21.5170 [480104015][ScriptMethodCallThread] Serial port write: 02-00-00-0A-00-06-00-05-00-13-02-02-00-00-00
272;13:12:21.5170 [480104015][ScriptMethodCallThread] Data buffer queue length (+1): 1 
273;13:12:21.5170 [480104015][ScriptMethodCallThread] Number of data packets sent: 1
274;13:12:21.5210 [480104015][ScriptMethodCallThread] ConnectionParameterUpdateResponse sent
275;13:12:21.5290 [480104015][ReadPacketQueueThread] Serial port read: 04-13-05-01-00-00-01-00
276;13:12:21.5300 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_NUMBER_OF_COMPLETED_PACKETS, NumberOfHandles: 1, ConnectionHandle: 0x0000, NumberOfPackets: 1
277;13:12:21.5300 [480104015][ReadPacketQueueThread] Data buffer queue length: 0
278;13:12:21.5460 [480104015][ScriptMethodCallThread] HCI command: BTLE_CMD_LE_CONNECTION_UPDATE, ConnectionHandle: 0x0000, ConnIntervalMin: 500ms, ConnIntervalMax: 500ms, ConnLatency: 0, SupervisionTimeout: 4000ms, MinCeLength: 2, MaxCeLength: 2
279;13:12:21.5470 [480104015][ScriptMethodCallThread] Serial port write: 01-13-20-0E-00-00-90-01-90-01-00-00-90-01-02-00-02-00
280;13:12:21.5510 [480104015][ReadPacketQueueThread] Serial port read: 04-0F-04-00-01-13-20
281;13:12:21.5510 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_STATUS, OpCode: BTLE_CMD_LE_CONNECTION_UPDATE, Status: BTLE_STATUS_CODE_SUCCESS
282;13:12:21.7090 [480104015][ReadPacketQueueThread] Serial port read: 04-3E-0A-03-00-00-00-90-01-00-00-90-01
283;13:12:21.7100 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_LE_CONNECTION_UPDATE_COMPLETE, ConnectionHandle: 0x0, ConnectionInterval: 500ms, Latency: 0, SupervisionTimeout: 4000ms
284;13:12:21.7330 [480104015][ScriptMethodCallThread] Connection Parameters Updated. ConnInterval:500ms, SlaveLatency:0, SupervisionTimeout:4000ms
285;13:12:36.1654 [480104015][MainThread] BondToDevice(peerAddress="D6C286741BE6",addressTypePeer=1,scanInterval=400,scanWindow=320,connIntervalMin=16,connIntervalMax=16,connLatency=0,connTimeout=300)
286;13:12:36.2215 [480104015][ScriptMethodCallThread] TST-Client: Generating MRandom
287;13:12:36.2225 [480104015][ScriptMethodCallThread] TST-Client: calling rand function
288;13:12:36.2235 [480104015][ScriptMethodCallThread] HCI command: BTLE_CMD_LE_RAND
289;13:12:36.2255 [480104015][ScriptMethodCallThread] Serial port write: 01-18-20-00
290;13:12:36.2285 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-0C-01-18-20-00-CD-1C-B3-35-10-69-7B-90
291;13:12:36.2285 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: BTLE_CMD_LE_RAND, Status: BTLE_STATUS_CODE_SUCCESS, RandomNumber: CD-1C-B3-35-10-69-7B-90
292;13:12:36.2405 [480104015][ScriptMethodCallThread] TST-Client: Received random number: 0x907B691035B31CCD
293;13:12:36.2685 [480104015][ScriptMethodCallThread] TST-Client: calling rand function
294;13:12:36.2685 [480104015][ScriptMethodCallThread] HCI command: BTLE_CMD_LE_RAND
295;13:12:36.2685 [480104015][ScriptMethodCallThread] Serial port write: 01-18-20-00
296;13:12:36.2715 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-0C-01-18-20-00-D6-9D-7A-66-B3-85-43-9C
297;13:12:36.2715 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: BTLE_CMD_LE_RAND, Status: BTLE_STATUS_CODE_SUCCESS, RandomNumber: D6-9D-7A-66-B3-85-43-9C
298;13:12:36.2746 [480104015][ScriptMethodCallThread] TST-Client: Received random number: 0x9C4385B3667A9DD6
299;13:12:36.3115 [480104015][ScriptMethodCallThread] TST-Client: MRandom - 0X907B691035B31CCD9C4385B3667A9DD6
300;13:12:36.3125 [480104015][ScriptMethodCallThread] TST-Client: Sending Get Device Address
301;13:12:36.3125 [480104015][ScriptMethodCallThread] TST-Client: calling read public device address
302;13:12:36.3135 [480104015][ScriptMethodCallThread] HCI command: BTLE_CMD_READ_BD_ADDR
303;13:12:36.3135 [480104015][ScriptMethodCallThread] Serial port write: 01-09-10-00
304;13:12:36.3205 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-0A-01-09-10-00-4E-25-87-A6-B7-8A
305;13:12:36.3205 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: BTLE_CMD_READ_BD_ADDR, Status: BTLE_STATUS_CODE_SUCCESS, BdAddress: 0x8AB7A687254E
306;13:12:36.3255 [480104015][ScriptMethodCallThread] TST-Client: Received device address: 0x8AB7A687254E
307;13:12:36.3265 [480104015][ScriptMethodCallThread] TST-Client: Tester Address - 0X8AB7A687254E
308;13:12:36.3535 [480104015][ScriptMethodCallThread] TST-Client: Sending <class 'protocol.Smp.SmpPairingRequest'> - [0x01, 0x04, 0x00, 0x01, 0x10, 0x00, 0x01]
309;13:12:36.3555 [480104015][ScriptMethodCallThread] WRITE DATA PACKET:07-00-06-00-01-04-00-01-10-00-01
310;13:12:36.3595 [480104015][ScriptMethodCallThread] Sending packet: SmpPairingRequest, 01-04-00-01-10-00-01, IoCapability: KeyboardDisplay, OobDataPresent: OobAuthDataNotPresent, AuthRequirements: Bonding, MaxEnryptionSize: 16, InitiatorKeyDistribution: 0, ResponderKeyDistribution: EncKey
311;13:12:36.3595 [480104015][ScriptMethodCallThread] Serial port write: 02-00-00-0B-00-07-00-06-00-01-04-00-01-10-00-01
312;13:12:36.3595 [480104015][ScriptMethodCallThread] Data buffer queue length (+1): 1 
313;13:12:36.3595 [480104015][ScriptMethodCallThread] Number of data packets sent: 2
314;13:12:36.7280 [480104015][ReadPacketQueueThread] Serial port read: 04-13-05-01-00-00-01-00
315;13:12:36.7280 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_NUMBER_OF_COMPLETED_PACKETS, NumberOfHandles: 1, ConnectionHandle: 0x0000, NumberOfPackets: 1
316;13:12:36.7290 [480104015][ReadPacketQueueThread] Data buffer queue length: 0
317;13:12:36.7830 [480104015][ScriptMethodCallThread] TST-Client: Discarded <HciEvent: eventCode=0x0D> - <HciEvent: eventCode=0x0D>
318;13:12:37.2290 [480104015][ReadPacketQueueThread] Serial port read: 02-00-20-0B-00-07-00-06-00-02-03-00-01-10-00-01
319;13:12:37.2290 [480104015][ReadPacketQueueThread] Received packet: SmpPairingResponse, 02-03-00-01-10-00-01, IoCapability: NoInputNoOutput, OobDataPresent: OobAuthDataNotPresent, AuthRequirements: Bonding, MaxEnryptionSize: 16, InitiatorKeyDistribution: 0, ResponderKeyDistribution: EncKey
320;13:12:37.2640 [480104015][ScriptMethodCallThread] TST-Client: Received <class 'protocol.Smp.SmpPairingResponse'> - [0x02, 0x03, 0x00, 0x01, 0x10, 0x00, 0x01]
321;13:12:37.2750 [480104015][ScriptMethodCallThread] TST-Client: Creating MConfirm
322;13:12:37.3000 [480104015][ScriptMethodCallThread] TST-Client: P1 - 0X01001001000302010010010004010100
323;13:12:37.3020 [480104015][ScriptMethodCallThread] TST-Client: P2 - 0X000000008AB7A687254EE61B7486C2D6
324;13:12:37.3220 [480104015][ScriptMethodCallThread] TST-Client: MRandom XOR p1 - 0X917B791135B01ECC9C5384B3627B9CD6
325;13:12:37.3440 [480104015][ScriptMethodCallThread] TST-Client: calling encrypt function, with key 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 and plaintextdata 0x91 0x7b 0x79 0x11 0x35 0xb0 0x1e 0xcc 0x9c 0x53 0x84 0xb3 0x62 0x7b 0x9c 0xd6
326;13:12:37.3460 [480104015][ScriptMethodCallThread] HCI command: BTLE_CMD_LE_ENCRYPT, Key: 0x00-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00, PlaintextData: 0xD6-9C-7B-62-B3-84-53-9C-CC-1E-B0-35-11-79-7B-91
327;13:12:37.3470 [480104015][ScriptMethodCallThread] Serial port write: 01-17-20-20-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00-D6-9C-7B-62-B3-84-53-9C-CC-1E-B0-35-11-79-7B-91
328;13:12:37.3530 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-14-01-17-20-00-E1-80-9E-3E-03-62-6A-33-F0-4E-C2-30-4F-00-19-63
329;13:12:37.3540 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: BTLE_CMD_LE_ENCRYPT, Status: BTLE_STATUS_CODE_SUCCESS, EncryptedData: E1-80-9E-3E-03-62-6A-33-F0-4E-C2-30-4F-00-19-63
330;13:12:37.3700 [480104015][ScriptMethodCallThread] TST-Client: Received encrypted data: 0x6319004F30C24EF0336A62033E9E80E1
331;13:12:37.3700 [480104015][ScriptMethodCallThread] TST-Client: Encrypt(MRandom XOR p1) XOR p2 - 0X6319004FBA75E877162484184A184237
332;13:12:37.3710 [480104015][ScriptMethodCallThread] TST-Client: calling encrypt function, with key 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 and plaintextdata 0x63 0x19 0x0 0x4f 0xba 0x75 0xe8 0x77 0x16 0x24 0x84 0x18 0x4a 0x18 0x42 0x37
333;13:12:37.3710 [480104015][ScriptMethodCallThread] HCI command: BTLE_CMD_LE_ENCRYPT, Key: 0x00-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00, PlaintextData: 0x37-42-18-4A-18-84-24-16-77-E8-75-BA-4F-00-19-63
334;13:12:37.3710 [480104015][ScriptMethodCallThread] Serial port write: 01-17-20-20-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00-37-42-18-4A-18-84-24-16-77-E8-75-BA-4F-00-19-63
335;13:12:37.3780 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-14-01-17-20-00-2E-F4-84-67-0C-B8-25-35-89-AB-53-53-43-10-2A-5B
336;13:12:37.3780 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: BTLE_CMD_LE_ENCRYPT, Status: BTLE_STATUS_CODE_SUCCESS, EncryptedData: 2E-F4-84-67-0C-B8-25-35-89-AB-53-53-43-10-2A-5B
337;13:12:37.3820 [480104015][ScriptMethodCallThread] TST-Client: Received encrypted data: 0x5B2A10435353AB893525B80C6784F42E
338;13:12:37.3830 [480104015][ScriptMethodCallThread] TST-Client: MConfirm - 0X5B2A10435353AB893525B80C6784F42E
339;13:12:37.3900 [480104015][ScriptMethodCallThread] TST-Client: Sending <class 'protocol.Smp.SmpPairingConfirm'> - [0x03, 0x2E, 0xF4, 0x84, 0x67, 0x0C, 0xB8, 0x25, 0x35, 0x89, 0xAB, 0x53, 0x53, 0x43, 0x10, 0x2A, 0x5B]
340;13:12:37.3940 [480104015][ScriptMethodCallThread] WRITE DATA PACKET:11-00-06-00-03-2E-F4-84-67-0C-B8-25-35-89-AB-53-53-43-10-2A-5B
341;13:12:37.3951 [480104015][ScriptMethodCallThread] Sending packet: SmpPairingConfirm, 03-2E-F4-84-67-0C-B8-25-35-89-AB-53-53-43-10-2A-5B, ConfirmValue: 2E-F4-84-67-0C-B8-25-35-89-AB-53-53-43-10-2A-5B
342;13:12:37.3951 [480104015][ScriptMethodCallThread] Serial port write: 02-00-00-15-00-11-00-06-00-03-2E-F4-84-67-0C-B8-25-35-89-AB-53-53-43-10-2A-5B
343;13:12:37.3951 [480104015][ScriptMethodCallThread] Data buffer queue length (+1): 1 
344;13:12:37.3951 [480104015][ScriptMethodCallThread] Number of data packets sent: 3
345;13:12:37.7280 [480104015][ReadPacketQueueThread] Serial port read: 04-13-05-01-00-00-01-00
346;13:12:37.7280 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_NUMBER_OF_COMPLETED_PACKETS, NumberOfHandles: 1, ConnectionHandle: 0x0000, NumberOfPackets: 1
347;13:12:37.7280 [480104015][ReadPacketQueueThread] Data buffer queue length: 0
348;13:12:37.7700 [480104015][ScriptMethodCallThread] TST-Client: Discarded <HciEvent: eventCode=0x0D> - <HciEvent: eventCode=0x0D>
349;13:12:38.2301 [480104015][ReadPacketQueueThread] Serial port read: 02-00-20-15-00-11-00-06-00-03-E5-EF-90-5B-04-B4-43-04-DF-BF-01-0C-A6-AF-2E-04
350;13:12:38.2301 [480104015][ReadPacketQueueThread] Received packet: SmpPairingConfirm, 03-E5-EF-90-5B-04-B4-43-04-DF-BF-01-0C-A6-AF-2E-04, ConfirmValue: E5-EF-90-5B-04-B4-43-04-DF-BF-01-0C-A6-AF-2E-04
351;13:12:38.2501 [480104015][ScriptMethodCallThread] TST-Client: Received <class 'protocol.Smp.SmpPairingConfirm'> - [0x03, 0xE5, 0xEF, 0x90, 0x5B, 0x04, 0xB4, 0x43, 0x04, 0xDF, 0xBF, 0x01, 0x0C, 0xA6, 0xAF, 0x2E, 0x04]
352;13:12:38.2531 [480104015][ScriptMethodCallThread] TST-Client: Sending <class 'protocol.Smp.SmpPairingRandom'> - [0x04, 0xD6, 0x9D, 0x7A, 0x66, 0xB3, 0x85, 0x43, 0x9C, 0xCD, 0x1C, 0xB3, 0x35, 0x10, 0x69, 0x7B, 0x90]
353;13:12:38.2561 [480104015][ScriptMethodCallThread] WRITE DATA PACKET:11-00-06-00-04-D6-9D-7A-66-B3-85-43-9C-CD-1C-B3-35-10-69-7B-90
354;13:12:38.2571 [480104015][ScriptMethodCallThread] Sending packet: SmpPairingRandom, 04-D6-9D-7A-66-B3-85-43-9C-CD-1C-B3-35-10-69-7B-90, RandomValue: D6-9D-7A-66-B3-85-43-9C-CD-1C-B3-35-10-69-7B-90
355;13:12:38.2571 [480104015][ScriptMethodCallThread] Serial port write: 02-00-00-15-00-11-00-06-00-04-D6-9D-7A-66-B3-85-43-9C-CD-1C-B3-35-10-69-7B-90
356;13:12:38.2571 [480104015][ScriptMethodCallThread] Data buffer queue length (+1): 1 
357;13:12:38.2571 [480104015][ScriptMethodCallThread] Number of data packets sent: 4
358;13:12:38.7284 [480104015][ReadPacketQueueThread] Serial port read: 04-13-05-01-00-00-01-00
359;13:12:38.7294 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_NUMBER_OF_COMPLETED_PACKETS, NumberOfHandles: 1, ConnectionHandle: 0x0000, NumberOfPackets: 1
360;13:12:38.7294 [480104015][ReadPacketQueueThread] Data buffer queue length: 0
361;13:12:38.7826 [480104015][ScriptMethodCallThread] TST-Client: Discarded <HciEvent: eventCode=0x0D> - <HciEvent: eventCode=0x0D>
362;13:12:39.2300 [480104015][ReadPacketQueueThread] Serial port read: 02-00-20-15-00-11-00-06-00-04-38-73-20-B5-F9-35-F1-9D-0C-7B-52-47-02-48-7B-71
363;13:12:39.2300 [480104015][ReadPacketQueueThread] Received packet: SmpPairingRandom, 04-38-73-20-B5-F9-35-F1-9D-0C-7B-52-47-02-48-7B-71, RandomValue: 38-73-20-B5-F9-35-F1-9D-0C-7B-52-47-02-48-7B-71
364;13:12:39.2571 [480104015][ScriptMethodCallThread] TST-Client: Received <class 'protocol.Smp.SmpPairingRandom'> - [0x04, 0x38, 0x73, 0x20, 0xB5, 0xF9, 0x35, 0xF1, 0x9D, 0x0C, 0x7B, 0x52, 0x47, 0x02, 0x48, 0x7B, 0x71]
365;13:12:39.2872 [480104015][ScriptMethodCallThread] TST-Client: Creating SConfirm
366;13:12:39.2882 [480104015][ScriptMethodCallThread] TST-Client: P1 - 0X01001001000302010010010004010100
367;13:12:39.2892 [480104015][ScriptMethodCallThread] TST-Client: P2 - 0X000000008AB7A687254EE61B7486C2D6
368;13:12:39.2892 [480104015][ScriptMethodCallThread] TST-Client: SRandom XOR p1 - 0X707B58034751790D9DE134F9B1217238
369;13:12:39.2892 [480104015][ScriptMethodCallThread] TST-Client: calling encrypt function, with key 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 and plaintextdata 0x70 0x7b 0x58 0x3 0x47 0x51 0x79 0xd 0x9d 0xe1 0x34 0xf9 0xb1 0x21 0x72 0x38
370;13:12:39.2902 [480104015][ScriptMethodCallThread] HCI command: BTLE_CMD_LE_ENCRYPT, Key: 0x00-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00, PlaintextData: 0x38-72-21-B1-F9-34-E1-9D-0D-79-51-47-03-58-7B-70
371;13:12:39.2902 [480104015][ScriptMethodCallThread] Serial port write: 01-17-20-20-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00-38-72-21-B1-F9-34-E1-9D-0D-79-51-47-03-58-7B-70
372;13:12:39.2965 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-14-01-17-20-00-61-77-C4-AC-BD-90-D5-2A-75-CA-EC-CE-49-11-8B-48
373;13:12:39.2965 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: BTLE_CMD_LE_ENCRYPT, Status: BTLE_STATUS_CODE_SUCCESS, EncryptedData: 61-77-C4-AC-BD-90-D5-2A-75-CA-EC-CE-49-11-8B-48
374;13:12:39.3132 [480104015][ScriptMethodCallThread] TST-Client: Received encrypted data: 0x488B1149CEECCA752AD590BDACC47761
375;13:12:39.3132 [480104015][ScriptMethodCallThread] TST-Client: Encrypt(SRandom XOR p1) XOR p2 - 0X488B1149445B6CF20F9B76A6D842B5B7
376;13:12:39.3132 [480104015][ScriptMethodCallThread] TST-Client: calling encrypt function, with key 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 and plaintextdata 0x48 0x8b 0x11 0x49 0x44 0x5b 0x6c 0xf2 0xf 0x9b 0x76 0xa6 0xd8 0x42 0xb5 0xb7
377;13:12:39.3142 [480104015][ScriptMethodCallThread] HCI command: BTLE_CMD_LE_ENCRYPT, Key: 0x00-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00, PlaintextData: 0xB7-B5-42-D8-A6-76-9B-0F-F2-6C-5B-44-49-11-8B-48
378;13:12:39.3142 [480104015][ScriptMethodCallThread] Serial port write: 01-17-20-20-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00-B7-B5-42-D8-A6-76-9B-0F-F2-6C-5B-44-49-11-8B-48
379;13:12:39.3232 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-14-01-17-20-00-E5-EF-90-5B-04-B4-43-04-DF-BF-01-0C-A6-AF-2E-04
380;13:12:39.3232 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: BTLE_CMD_LE_ENCRYPT, Status: BTLE_STATUS_CODE_SUCCESS, EncryptedData: E5-EF-90-5B-04-B4-43-04-DF-BF-01-0C-A6-AF-2E-04
381;13:12:39.3336 [480104015][ScriptMethodCallThread] TST-Client: Received encrypted data: 0x042EAFA60C01BFDF0443B4045B90EFE5
382;13:12:39.3336 [480104015][ScriptMethodCallThread] TST-Client: SConfirm - 0X042EAFA60C01BFDF0443B4045B90EFE5
383;13:12:39.3416 [480104015][ScriptMethodCallThread] TST-Client: calling encrypt function, with key 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 and plaintextdata 0x9d 0xf1 0x35 0xf9 0xb5 0x20 0x73 0x38 0x9c 0x43 0x85 0xb3 0x66 0x7a 0x9d 0xd6
384;13:12:39.3416 [480104015][ScriptMethodCallThread] HCI command: BTLE_CMD_LE_ENCRYPT, Key: 0x00-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00, PlaintextData: 0xD6-9D-7A-66-B3-85-43-9C-38-73-20-B5-F9-35-F1-9D
385;13:12:39.3416 [480104015][ScriptMethodCallThread] Serial port write: 01-17-20-20-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00-D6-9D-7A-66-B3-85-43-9C-38-73-20-B5-F9-35-F1-9D
386;13:12:39.3484 [480104015][ReadPacketQueueThread] Serial port read: 04-0E-14-01-17-20-00-40-2D-31-52-41-B4-A5-FF-8E-5C-29-FF-A9-E3-ED-4D
387;13:12:39.3484 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_COMPLETE, OpCode: BTLE_CMD_LE_ENCRYPT, Status: BTLE_STATUS_CODE_SUCCESS, EncryptedData: 40-2D-31-52-41-B4-A5-FF-8E-5C-29-FF-A9-E3-ED-4D
388;13:12:39.3503 [480104015][ScriptMethodCallThread] TST-Client: Received encrypted data: 0x4DEDE3A9FF295C8EFFA5B44152312D40
389;13:12:39.3503 [480104015][ScriptMethodCallThread] TST-Client: Encrypting the link with STK
390;13:12:39.3542 [480104015][ScriptMethodCallThread] TST-Client: Starting Encryption
391;13:12:39.3582 [480104015][ScriptMethodCallThread] HCI command: BTLE_CMD_LE_START_ENCRYPTION, ConnectionHandle: 0x0000, Diversifier: 0x00-00, RandomNumber: 0x00-00-00-00-00-00-00-00, LongTermKey: 0x40-2D-31-52-41-B4-A5-FF-8E-5C-29-FF-A9-E3-ED-4D
392;13:12:39.3582 [480104015][ScriptMethodCallThread] Serial port write: 01-19-20-1C-00-00-00-00-00-00-00-00-00-00-00-00-40-2D-31-52-41-B4-A5-FF-8E-5C-29-FF-A9-E3-ED-4D
393;13:12:39.3638 [480104015][ReadPacketQueueThread] Serial port read: 04-0F-04-00-01-19-20
394;13:12:39.3638 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_COMMAND_STATUS, OpCode: BTLE_CMD_LE_START_ENCRYPTION, Status: BTLE_STATUS_CODE_SUCCESS
395;13:12:39.3679 [480104015][ScriptMethodCallThread] TST-Client: Start Encryption command returned success
396;13:12:42.7289 [480104015][ReadPacketQueueThread] Serial port read: 04-08-04-00-00-00-01
397;13:12:42.7289 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_ENCRYPTION_CHANGE, ConnectionHandle: 0x0000, Status: BTLE_STATUS_CODE_SUCCESS, EncryptionMode: BTLE_ENCRYPTION_ON
398;13:12:42.7419 [480104015][ScriptThread] Encryption change: Link encryption is ON
399;13:12:42.7470 [480104015][ScriptMethodCallThread] TST-Client: Encryption Event returned success
400;13:12:42.7530 [480104015][] SERVER: Received packet <HciEvent: eventCode=0x0B> - <HciEvent: eventCode=0x0B>
401;13:12:42.7530 [480104015][] SERVER: Received Encryption Change Event
402;13:12:43.2306 [480104015][ReadPacketQueueThread] Serial port read: 02-00-20-15-00-11-00-06-00-06-E4-30-63-F1-EA-A2-70-DC-1D-3C-E2-DD-6C-6E-83-FA
403;13:12:43.2316 [480104015][ReadPacketQueueThread] Received packet: SmpEncryptionInformation, 06-E4-30-63-F1-EA-A2-70-DC-1D-3C-E2-DD-6C-6E-83-FA, LongTermKey: E4-30-63-F1-EA-A2-70-DC-1D-3C-E2-DD-6C-6E-83-FA
404;13:12:43.2827 [480104015][ScriptMethodCallThread] TST-Client: Received <class 'protocol.Smp.SmpEncryptionInformation'> - [0x06, 0xE4, 0x30, 0x63, 0xF1, 0xEA, 0xA2, 0x70, 0xDC, 0x1D, 0x3C, 0xE2, 0xDD, 0x6C, 0x6E, 0x83, 0xFA]
405;13:12:44.2297 [480104015][ReadPacketQueueThread] Serial port read: 02-00-20-0F-00-0B-00-06-00-07-94-DB-63-F9-D7-9D-AC-09-7B-A6
406;13:12:44.2317 [480104015][ReadPacketQueueThread] Received packet: SmpMasterIdentification, 07-94-DB-63-F9-D7-9D-AC-09-7B-A6, Ediv: 0xDB94, Rand: 0xA67B09AC9DD7F963
407;13:12:44.3160 [480104015][ScriptMethodCallThread] TST-Client: Received <class 'protocol.Smp.SmpMasterIdentification'> - [0x07, 0x94, 0xDB, 0x63, 0xF9, 0xD7, 0x9D, 0xAC, 0x09, 0x7B, 0xA6]
408;13:12:49.2286 [480104015][ReadPacketQueueThread] Serial port read: 04-05-04-00-00-00-08
409;13:12:49.2297 [480104015][ReadPacketQueueThread] HCI event: BTLE_EVENT_DISCONNECTION_COMPLETE ConnectionHandle: 0x0000, Reason: BTLE_CONNECTION_TIMEOUT
410;13:12:49.2496 [480104015][ReadPacketQueueThread] Received LL Connection Termination Event, reason 08
411;13:12:49.2506 [480104015][ScriptThread] Lost connection to device. Reason: BTLE_CONNECTION_TIMEOUT
412;13:12:49.2879 [480104015][] SERVER: Received packet <HciEvent: eventCode=0x0A> - <HciEvent: eventCode=0x0A>
413;13:12:49.2909 [480104015][] SERVER: Received Link Loss