# Static Call Graph for image .\_build\nrf52832_xxaa_s132.axf

#<CALLGRAPH># ARM Linker, 5060422: Last Updated: Wed Sep 06 15:05:35 2017

### Maximum Stack Usage = 392 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ advertising_init ⇒ ble_advertising_init ⇒ ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemoryManagement_Handler ⇒ MemoryManagement_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- CCM_AAR_IRQHandler ⇒ CCM_AAR_IRQHandler
- __asm___11_app_timer_c_cd27f9c3__nrf_delay_us ⇒ __asm___11_app_timer_c_cd27f9c3__nrf_delay_us
- __asm___13_nrf_drv_twi_c_a9bcf68d__nrf_delay_us ⇒ __asm___13_nrf_drv_twi_c_a9bcf68d__nrf_delay_us
- app_notify_error_state_transit ⇒ sm_state_change
- cmd_queue_dequeue ⇒ cmd_process

  ### Function Pointers

  - BusFault_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - CCM_AAR_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - COMP_LPCOMP_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - DebugMon_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - ECB_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - FPU_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - GPIOTE_IRQHandler from nrf_drv_gpiote.o(i.GPIOTE_IRQHandler) referenced from arm_startup_nrf52.o(RESET)
  - HardFault_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - I2S_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - MWU_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - MemoryManagement_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - NFCT_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - NMI_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - PDM_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - POWER_CLOCK_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - PWM0_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - PWM1_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - PWM2_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - PendSV_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - QDEC_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - RADIO_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - RNG_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - RTC0_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - RTC1_IRQHandler from app_timer.o(i.RTC1_IRQHandler) referenced from arm_startup_nrf52.o(RESET)
  - RTC2_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - Reset_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SAADC_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler from nrf_drv_twi.o(i.SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler) referenced from arm_startup_nrf52.o(RESET)
  - SPIM1_SPIS1_TWIM1_TWIS1_SPI1_TWI1_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SPIM2_SPIS2_SPI2_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SVC_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SWI0_EGU0_IRQHandler from app_timer.o(i.SWI0_EGU0_IRQHandler) referenced from arm_startup_nrf52.o(RESET)
  - SWI1_EGU1_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SWI2_EGU2_IRQHandler from softdevice_handler.o(i.SWI2_EGU2_IRQHandler) referenced from arm_startup_nrf52.o(RESET)
  - SWI3_EGU3_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SWI4_EGU4_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SWI5_EGU5_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SysTick_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - SystemInit from system_nrf52.o(i.SystemInit) referenced from arm_startup_nrf52.o(.text)
  - TEMP_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - TIMER0_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - TIMER1_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - TIMER2_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - TIMER3_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - TIMER4_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - UARTE0_UART0_IRQHandler from nrf_drv_uart.o(i.UARTE0_UART0_IRQHandler) referenced from arm_startup_nrf52.o(RESET)
  - UsageFault_Handler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - WDT_IRQHandler from arm_startup_nrf52.o(.text) referenced from arm_startup_nrf52.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from arm_startup_nrf52.o(.text)
  - ble_evt_dispatch from main.o(i.ble_evt_dispatch) referenced from main.o(i.ble_stack_init)
  - conn_params_error_handler from main.o(i.conn_params_error_handler) referenced from main.o(i.conn_params_init)
  - data_page_erase_state_run from pstorage.o(i.data_page_erase_state_run) referenced from pstorage.o(.constdata)
  - data_to_swap_write_state_run from pstorage.o(i.data_to_swap_write_state_run) referenced from pstorage.o(.constdata)
  - device_manager_evt_handler from main.o(i.device_manager_evt_handler) referenced from main.o(i.device_manager_init)
  - dm_pstorage_cb_handler from device_manager_peripheral.o(i.dm_pstorage_cb_handler) referenced from device_manager_peripheral.o(i.dm_init)
  - fputc from retarget.o(i.fputc) referenced from printf8.o(i.__0printf$8)
  - gattc_context_apply from device_manager_peripheral.o(i.gattc_context_apply) referenced from device_manager_peripheral.o(.constdata)
  - gattc_context_load from device_manager_peripheral.o(i.gattc_context_load) referenced from device_manager_peripheral.o(.constdata)
  - gattc_context_store from device_manager_peripheral.o(i.gattc_context_store) referenced from device_manager_peripheral.o(.constdata)
  - gatts_context_apply from device_manager_peripheral.o(i.gatts_context_apply) referenced from device_manager_peripheral.o(.constdata)
  - gatts_context_load from device_manager_peripheral.o(i.gatts_context_load) referenced from device_manager_peripheral.o(.constdata)
  - gatts_context_store from device_manager_peripheral.o(i.gatts_context_store) referenced from device_manager_peripheral.o(.constdata)
  - gattsc_context_apply from device_manager_peripheral.o(i.gattsc_context_apply) referenced from device_manager_peripheral.o(.constdata)
  - gattsc_context_load from device_manager_peripheral.o(i.gattsc_context_load) referenced from device_manager_peripheral.o(.constdata)
  - gattsc_context_store from device_manager_peripheral.o(i.gattsc_context_store) referenced from device_manager_peripheral.o(.constdata)
  - head_restore_state_run from pstorage.o(i.head_restore_state_run) referenced from pstorage.o(.constdata)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)
  - no_service_context_apply from device_manager_peripheral.o(i.no_service_context_apply) referenced from device_manager_peripheral.o(.constdata)
  - no_service_context_load from device_manager_peripheral.o(i.no_service_context_load) referenced from device_manager_peripheral.o(.constdata)
  - no_service_context_store from device_manager_peripheral.o(i.no_service_context_store) referenced from device_manager_peripheral.o(.constdata)
  - nrf_drv_mpu_twi_event_handler from nrf_drv_mpu_twi.o(i.nrf_drv_mpu_twi_event_handler) referenced from nrf_drv_mpu_twi.o(i.nrf_drv_mpu_init)
  - on_adv_evt from main.o(i.on_adv_evt) referenced from main.o(i.advertising_init)
  - on_conn_params_evt from main.o(i.on_conn_params_evt) referenced from main.o(i.conn_params_init)
  - pstorage_store from pstorage.o(i.pstorage_store) referenced from device_manager_peripheral.o(i.device_context_store)
  - pstorage_store from pstorage.o(i.pstorage_store) referenced from device_manager_peripheral.o(i.gatts_context_store)
  - pstorage_update from pstorage.o(i.pstorage_update) referenced from device_manager_peripheral.o(i.device_context_store)
  - pstorage_update from pstorage.o(i.pstorage_update) referenced from device_manager_peripheral.o(i.gatts_context_store)
  - softdevice_fault_handler from softdevice_handler.o(i.softdevice_fault_handler) referenced from softdevice_handler.o(i.softdevice_handler_init)
  - state_erase_data_page_entry_run from pstorage.o(i.state_erase_data_page_entry_run) referenced from pstorage.o(.constdata)
  - state_restore_head_entry_run from pstorage.o(i.state_restore_head_entry_run) referenced from pstorage.o(.constdata)
  - state_restore_tail_entry_run from pstorage.o(i.state_restore_tail_entry_run) referenced from pstorage.o(.constdata)
  - state_swap_erase_entry_run from pstorage.o(i.state_swap_erase_entry_run) referenced from pstorage.o(.constdata)
  - state_write_data_swap_entry_run from pstorage.o(i.state_write_data_swap_entry_run) referenced from pstorage.o(.constdata)
  - storage_operation_dummy_handler from device_manager_peripheral.o(i.storage_operation_dummy_handler) referenced from device_manager_peripheral.o(i.device_context_store)
  - swap_erase_state_run from pstorage.o(i.swap_erase_state_run) referenced from pstorage.o(.constdata)
  - sys_evt_dispatch from main.o(i.sys_evt_dispatch) referenced from main.o(i.ble_stack_init)
  - tail_restore_state_run from pstorage.o(i.tail_restore_state_run) referenced from pstorage.o(.constdata)
  - timer_accel_update_handler from main.o(i.timer_accel_update_handler) referenced from main.o(i.timers_init)
  - uart_event_handler from app_uart_fifo.o(i.uart_event_handler) referenced from app_uart_fifo.o(i.app_uart_init)
  - uart_events_handler from main.o(i.uart_events_handler) referenced from main.o(i.uart_config)
  - update_timeout_handler from ble_conn_params.o(i.update_timeout_handler) referenced from ble_conn_params.o(i.ble_conn_params_init)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  __asm___13_nrf_drv_twi_c_a9bcf68d__nrf_delay_us (Thumb, 118 bytes, Stack size 0 bytes, nrf_drv_twi.o(.emb_text))
  [Calls]

  - >> __asm___13_nrf_drv_twi_c_a9bcf68d__nrf_delay_us
  [Called By]
  - >> __asm___13_nrf_drv_twi_c_a9bcf68d__nrf_delay_us
  - >> twi_clear_bus

  __asm___11_app_timer_c_cd27f9c3__nrf_delay_us (Thumb, 118 bytes, Stack size 0 bytes, app_timer.o(.emb_text))
  [Calls]

  - >> __asm___11_app_timer_c_cd27f9c3__nrf_delay_us
  [Called By]
  - >> __asm___11_app_timer_c_cd27f9c3__nrf_delay_us
  - >> rtc1_stop
  - >> rtc1_start
  - >> compare_reg_update

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  MemoryManagement_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> MemoryManagement_Handler
  [Called By]
  - >> MemoryManagement_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  CCM_AAR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Calls]

  - >> CCM_AAR_IRQHandler
  [Called By]
  - >> CCM_AAR_IRQHandler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  COMP_LPCOMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  ECB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  I2S_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  MWU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  NFCT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  PDM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  POWER_CLOCK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  PWM0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  PWM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  PWM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  QDEC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  RADIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  RTC0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  RTC2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  SAADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  SPIM1_SPIS1_TWIM1_TWIS1_SPI1_TWI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  SPIM2_SPIS2_SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  SWI1_EGU1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  SWI3_EGU3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  SWI4_EGU4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  SWI5_EGU5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  TEMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  TIMER0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  TIMER1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  TIMER2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  TIMER3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  TIMER4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52.o(RESET)

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> merge_register_and_data
  - >> pstorage_load
  - >> service_data_encode
  - >> manuf_specific_data_encode

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> ble_conn_params_init
  - >> ble_advertising_init
  - >> app_uart_init
  - >> gatts_context_store

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text))
  [Calls]

  - >> __aeabi_memset
  [Called By]
  - >> peer_instance_init

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> ble_char_accel_add
  - >> softdevice_enable_get_default_config
  - >> dm_init
  - >> dm_ble_evt_handler
  - >> ble_advertising_start
  - >> ble_advertising_init
  - >> conn_params_init
  - >> advertising_init
  - >> gatts_context_store
  - >> dm_pstorage_cb_handler

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  memcmp (Thumb, 26 bytes, Stack size 12 bytes, memcmp.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = memcmp
  [Called By]
  - >> gatts_context_store
  - >> dm_pstorage_cb_handler
  - >> device_instance_find

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  GPIOTE_IRQHandler (Thumb, 420 bytes, Stack size 64 bytes, nrf_drv_gpiote.o(i.GPIOTE_IRQHandler))
  [Stack]

  - Max Depth = 80
  - Call Chain = GPIOTE_IRQHandler ⇒ nrf_gpiote_event_clear
  [Calls]
  - >> nrf_gpiote_event_is_set
  - >> nrf_gpiote_event_clear
  - >> nrf_gpio_cfg_sense_set
  - >> channel_port_get
  - >> channel_handler_get
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  RTC1_IRQHandler (Thumb, 44 bytes, Stack size 8 bytes, app_timer.o(i.RTC1_IRQHandler))
  [Stack]

  - Max Depth = 108
  - Call Chain = RTC1_IRQHandler ⇒ timer_timeouts_check ⇒ timeout_handler_exec ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> timer_timeouts_check
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler (Thumb, 12 bytes, Stack size 8 bytes, nrf_drv_twi.o(i.SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler))
  [Stack]

  - Max Depth = 144
  - Call Chain = SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler ⇒ irq_handler_twi ⇒ twi_tx_start_transfer ⇒ twi_transfer ⇒ twi_send_byte
  [Calls]
  - >> irq_handler_twi
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  SWI0_EGU0_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, app_timer.o(i.SWI0_EGU0_IRQHandler))
  [Stack]

  - Max Depth = 80
  - Call Chain = SWI0_EGU0_IRQHandler ⇒ timer_list_handler ⇒ list_insertions_handler ⇒ timer_list_insert
  [Calls]
  - >> timer_list_handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  SWI2_EGU2_IRQHandler (Thumb, 48 bytes, Stack size 16 bytes, softdevice_handler.o(i.SWI2_EGU2_IRQHandler))
  [Stack]

  - Max Depth = 100
  - Call Chain = SWI2_EGU2_IRQHandler ⇒ intern_softdevice_events_execute ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> app_error_handler
  - >> intern_softdevice_events_execute
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  SystemCoreClockUpdate (Thumb, 8 bytes, Stack size 0 bytes, system_nrf52.o(i.SystemCoreClockUpdate))
  [Called By]

  - >> SystemInit

  SystemInit (Thumb, 554 bytes, Stack size 8 bytes, system_nrf52.o(i.SystemInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = SystemInit
  [Calls]
  - >> SystemCoreClockUpdate
  - >> errata_66
  - >> errata_57
  - >> errata_37
  - >> errata_36
  - >> errata_32
  - >> errata_31
  - >> errata_16
  - >> errata_12
  - >> errata_108
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(.text)

  UARTE0_UART0_IRQHandler (Thumb, 20 bytes, Stack size 8 bytes, nrf_drv_uart.o(i.UARTE0_UART0_IRQHandler))
  [Stack]

  - Max Depth = 72
  - Call Chain = UARTE0_UART0_IRQHandler ⇒ uarte_irq_handler ⇒ rx_done_event
  [Calls]
  - >> uarte_irq_handler
  - >> uart_irq_handler
  [Address Reference Count : 1]
  - arm_startup_nrf52.o(RESET)

  __0printf$8 (Thumb, 22 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf$8 (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> main

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  adv_data_encode (Thumb, 454 bytes, Stack size 32 bytes, ble_advdata.o(i.adv_data_encode))
  [Stack]

  - Max Depth = 128
  - Call Chain = adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> flags_encode
  - >> conn_int_encode
  - >> ble_device_addr_encode
  - >> appearance_encode
  - >> uuid_list_encode
  - >> tx_power_level_encode
  - >> tk_value_encode
  - >> service_data_encode
  - >> sec_mgr_oob_flags_encode
  - >> name_encode
  - >> manuf_specific_data_encode
  - >> le_role_encode
  [Called By]
  - >> ble_advdata_set

  app_error_fault_handler (Thumb, 26 bytes, Stack size 16 bytes, app_error_weak.o(i.app_error_fault_handler))
  [Stack]

  - Max Depth = 28
  - Call Chain = app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> bsp_indication_set
  - >> app_error_save_and_stop
  [Called By]
  - >> app_error_handler
  - >> softdevice_fault_handler

  app_error_handler (Thumb, 32 bytes, Stack size 32 bytes, app_error.o(i.app_error_handler))
  [Stack]

  - Max Depth = 60
  - Call Chain = app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> app_error_fault_handler
  [Called By]
  - >> ble_char_accel_add
  - >> dm_ble_evt_handler
  - >> ble_mpu_service_init
  - >> mpu_setup
  - >> main
  - >> uart_events_handler
  - >> uart_config
  - >> timers_init
  - >> sleep_mode_enter
  - >> power_manage
  - >> on_conn_params_evt
  - >> on_ble_evt
  - >> on_adv_evt
  - >> gap_params_init
  - >> device_manager_init
  - >> device_manager_evt_handler
  - >> conn_params_init
  - >> conn_params_error_handler
  - >> ble_stack_init
  - >> advertising_init
  - >> dm_pstorage_cb_handler
  - >> timeout_handler_exec
  - >> intern_softdevice_events_execute
  - >> SWI2_EGU2_IRQHandler

  app_error_save_and_stop (Thumb, 132 bytes, Stack size 12 bytes, app_error.o(i.app_error_save_and_stop))
  [Stack]

  - Max Depth = 12
  - Call Chain = app_error_save_and_stop
  [Called By]
  - >> app_error_fault_handler

  app_fifo_get (Thumb, 30 bytes, Stack size 16 bytes, app_fifo.o(i.app_fifo_get))
  [Stack]

  - Max Depth = 40
  - Call Chain = app_fifo_get ⇒ fifo_get ⇒ fifo_peek
  [Calls]
  - >> fifo_length
  - >> fifo_get
  [Called By]
  - >> app_uart_put
  - >> uart_event_handler

  app_fifo_init (Thumb, 36 bytes, Stack size 0 bytes, app_fifo.o(i.app_fifo_init))
  [Called By]

  - >> app_uart_init

  app_fifo_put (Thumb, 34 bytes, Stack size 16 bytes, app_fifo.o(i.app_fifo_put))
  [Stack]

  - Max Depth = 16
  - Call Chain = app_fifo_put
  [Calls]
  - >> fifo_put
  - >> fifo_length
  [Called By]
  - >> app_uart_put
  - >> uart_event_handler

  app_timer_create (Thumb, 56 bytes, Stack size 8 bytes, app_timer.o(i.app_timer_create))
  [Stack]

  - Max Depth = 8
  - Call Chain = app_timer_create
  [Called By]
  - >> ble_conn_params_init
  - >> timers_init

  app_timer_init (Thumb, 154 bytes, Stack size 24 bytes, app_timer.o(i.app_timer_init))
  [Stack]

  - Max Depth = 40
  - Call Chain = app_timer_init ⇒ rtc1_init ⇒ NVIC_SetPriority
  [Calls]
  - >> rtc1_stop
  - >> rtc1_init
  - >> rtc1_counter_get
  - >> NVIC_SetPriority
  - >> NVIC_EnableIRQ
  - >> NVIC_ClearPendingIRQ
  [Called By]
  - >> timers_init

  app_timer_start (Thumb, 84 bytes, Stack size 32 bytes, app_timer.o(i.app_timer_start))
  [Stack]

  - Max Depth = 76
  - Call Chain = app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> user_id_get
  - >> timer_start_op_schedule
  [Called By]
  - >> on_ble_evt
  - >> conn_params_negotiation

  app_timer_stop (Thumb, 48 bytes, Stack size 16 bytes, app_timer.o(i.app_timer_stop))
  [Stack]

  - Max Depth = 52
  - Call Chain = app_timer_stop ⇒ timer_stop_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> user_id_get
  - >> timer_stop_op_schedule
  [Called By]
  - >> on_ble_evt
  - >> on_write
  - >> on_disconnect

  app_uart_init (Thumb, 178 bytes, Stack size 56 bytes, app_uart_fifo.o(i.app_uart_init))
  [Stack]

  - Max Depth = 124
  - Call Chain = app_uart_init ⇒ nrf_drv_uart_init ⇒ apply_config ⇒ nrf_gpio_cfg_input ⇒ nrf_gpio_cfg
  [Calls]
  - >> nrf_drv_uart_rx_enable
  - >> nrf_drv_uart_rx
  - >> nrf_drv_uart_init
  - >> app_fifo_init
  - >> __aeabi_memcpy4
  [Called By]
  - >> uart_config

  app_uart_put (Thumb, 46 bytes, Stack size 16 bytes, app_uart_fifo.o(i.app_uart_put))
  [Stack]

  - Max Depth = 56
  - Call Chain = app_uart_put ⇒ app_fifo_get ⇒ fifo_get ⇒ fifo_peek
  [Calls]
  - >> nrf_drv_uart_tx_in_progress
  - >> nrf_drv_uart_tx
  - >> app_fifo_put
  - >> app_fifo_get
  [Called By]
  - >> fputc

  ble_advdata_set (Thumb, 148 bytes, Stack size 96 bytes, ble_advdata.o(i.ble_advdata_set))
  [Stack]

  - Max Depth = 224
  - Call Chain = ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> advdata_check
  - >> adv_data_encode
  - >> srdata_check
  [Called By]
  - >> ble_advertising_start
  - >> ble_advertising_init

  ble_advertising_init (Thumb, 324 bytes, Stack size 32 bytes, ble_advertising.o(i.ble_advertising_init))
  [Stack]

  - Max Depth = 256
  - Call Chain = ble_advertising_init ⇒ ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> ble_advertising_peer_address_clear
  - >> ble_advdata_set
  - >> __aeabi_memclr4
  - >> __aeabi_memcpy4
  [Called By]
  - >> advertising_init

  ble_advertising_on_ble_evt (Thumb, 224 bytes, Stack size 16 bytes, ble_advertising.o(i.ble_advertising_on_ble_evt))
  [Stack]

  - Max Depth = 280
  - Call Chain = ble_advertising_on_ble_evt ⇒ ble_advertising_start ⇒ ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> ble_advertising_start
  [Called By]
  - >> ble_evt_dispatch

  ble_advertising_on_sys_evt (Thumb, 64 bytes, Stack size 16 bytes, ble_advertising.o(i.ble_advertising_on_sys_evt))
  [Stack]

  - Max Depth = 280
  - Call Chain = ble_advertising_on_sys_evt ⇒ ble_advertising_start ⇒ ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> ble_advertising_start
  [Called By]
  - >> sys_evt_dispatch

  ble_advertising_start (Thumb, 604 bytes, Stack size 40 bytes, ble_advertising.o(i.ble_advertising_start))
  [Stack]

  - Max Depth = 264
  - Call Chain = ble_advertising_start ⇒ ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> whitelist_has_entries
  - >> peer_address_exists
  - >> flash_access_in_progress
  - >> ble_advertising_peer_address_clear
  - >> ble_advdata_set
  - >> __aeabi_memclr4
  [Called By]
  - >> ble_advertising_on_sys_evt
  - >> ble_advertising_on_ble_evt
  - >> main

  ble_conn_params_init (Thumb, 84 bytes, Stack size 16 bytes, ble_conn_params.o(i.ble_conn_params_init))
  [Stack]

  - Max Depth = 24
  - Call Chain = ble_conn_params_init ⇒ app_timer_create
  [Calls]
  - >> app_timer_create
  - >> __aeabi_memcpy4
  [Called By]
  - >> conn_params_init

  ble_conn_params_on_ble_evt (Thumb, 62 bytes, Stack size 8 bytes, ble_conn_params.o(i.ble_conn_params_on_ble_evt))
  [Stack]

  - Max Depth = 116
  - Call Chain = ble_conn_params_on_ble_evt ⇒ on_write ⇒ conn_params_negotiation ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> on_write
  - >> on_disconnect
  - >> on_connect
  - >> on_conn_params_update
  [Called By]
  - >> ble_evt_dispatch

  ble_mpu_on_ble_evt (Thumb, 32 bytes, Stack size 0 bytes, ble_mpu.o(i.ble_mpu_on_ble_evt))
  [Called By]

  - >> ble_evt_dispatch

  ble_mpu_service_init (Thumb, 100 bytes, Stack size 40 bytes, ble_mpu.o(i.ble_mpu_service_init))
  [Stack]

  - Max Depth = 188
  - Call Chain = ble_mpu_service_init ⇒ ble_char_accel_add ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> ble_char_accel_add
  - >> app_error_handler
  [Called By]
  - >> services_init

  ble_mpu_update (Thumb, 68 bytes, Stack size 32 bytes, ble_mpu.o(i.ble_mpu_update))
  [Stack]

  - Max Depth = 32
  - Call Chain = ble_mpu_update
  [Called By]
  - >> main

  bond_data_load (Thumb, 64 bytes, Stack size 24 bytes, device_manager_peripheral.o(i.bond_data_load))
  [Stack]

  - Max Depth = 48
  - Call Chain = bond_data_load ⇒ pstorage_load
  [Calls]
  - >> pstorage_load
  - >> pstorage_block_identifier_get
  [Called By]
  - >> dm_ble_evt_handler

  bsp_indication_set (Thumb, 6 bytes, Stack size 0 bytes, bsp.o(i.bsp_indication_set))
  [Called By]

  - >> on_ble_evt
  - >> on_adv_evt
  - >> app_error_fault_handler

  dm_ble_evt_handler (Thumb, 1696 bytes, Stack size 88 bytes, device_manager_peripheral.o(i.dm_ble_evt_handler))
  [Stack]

  - Max Depth = 336
  - Call Chain = dm_ble_evt_handler ⇒ device_instance_free ⇒ pstorage_clear ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ update_operation_execute ⇒ clear_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> app_error_handler
  - >> dm_handle_initialize
  - >> bond_data_load
  - >> peer_instance_init
  - >> device_instance_free
  - >> device_instance_find
  - >> device_instance_allocate
  - >> device_context_store
  - >> connection_instance_init
  - >> connection_instance_find
  - >> app_evt_notify
  - >> __aeabi_memclr4
  [Called By]
  - >> ble_evt_dispatch

  dm_handle_initialize (Thumb, 24 bytes, Stack size 0 bytes, device_manager_peripheral.o(i.dm_handle_initialize))
  [Called By]

  - >> dm_ble_evt_handler
  - >> dm_pstorage_cb_handler

  dm_init (Thumb, 234 bytes, Stack size 32 bytes, device_manager_peripheral.o(i.dm_init))
  [Stack]

  - Max Depth = 256
  - Call Chain = dm_init ⇒ pstorage_clear ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ update_operation_execute ⇒ clear_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> pstorage_register
  - >> pstorage_load
  - >> pstorage_clear
  - >> pstorage_block_identifier_get
  - >> peer_instance_init
  - >> connection_instance_init
  - >> __aeabi_memclr4
  [Called By]
  - >> device_manager_init

  dm_register (Thumb, 166 bytes, Stack size 8 bytes, device_manager_peripheral.o(i.dm_register))
  [Stack]

  - Max Depth = 8
  - Call Chain = dm_register
  [Called By]
  - >> device_manager_init

  fputc (Thumb, 16 bytes, Stack size 16 bytes, retarget.o(i.fputc))
  [Stack]

  - Max Depth = 72
  - Call Chain = fputc ⇒ app_uart_put ⇒ app_fifo_get ⇒ fifo_get ⇒ fifo_peek
  [Calls]
  - >> app_uart_put
  [Address Reference Count : 1]
  - printf8.o(i.__0printf$8)

  fs_queued_op_count_get (Thumb, 18 bytes, Stack size 0 bytes, fstorage.o(i.fs_queued_op_count_get))
  [Called By]

  - >> flash_access_in_progress

  intern_softdevice_events_execute (Thumb, 150 bytes, Stack size 24 bytes, softdevice_handler.o(i.intern_softdevice_events_execute))
  [Stack]

  - Max Depth = 84
  - Call Chain = intern_softdevice_events_execute ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> app_error_handler
  [Called By]
  - >> SWI2_EGU2_IRQHandler

  main (Thumb, 306 bytes, Stack size 24 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 392
  - Call Chain = main ⇒ advertising_init ⇒ ble_advertising_init ⇒ ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> mpu_read_accel
  - >> ble_mpu_update
  - >> ble_advertising_start
  - >> app_error_handler
  - >> mpu_setup
  - >> uart_config
  - >> timers_init
  - >> services_init
  - >> power_manage
  - >> gap_params_init
  - >> device_manager_init
  - >> conn_params_init
  - >> ble_stack_init
  - >> application_timers_start
  - >> advertising_init
  - >> __2printf
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  mpu_config (Thumb, 18 bytes, Stack size 16 bytes, app_mpu.o(i.mpu_config))
  [Stack]

  - Max Depth = 216
  - Call Chain = mpu_config ⇒ nrf_drv_mpu_write_registers ⇒ nrf_drv_twi_xfer ⇒ twi_xfer ⇒ twi_tx_start_transfer ⇒ twi_transfer ⇒ twi_send_byte
  [Calls]
  - >> nrf_drv_mpu_write_registers
  [Called By]
  - >> mpu_setup

  mpu_init (Thumb, 52 bytes, Stack size 16 bytes, app_mpu.o(i.mpu_init))
  [Stack]

  - Max Depth = 248
  - Call Chain = mpu_init ⇒ nrf_drv_mpu_write_single_register ⇒ nrf_drv_twi_tx ⇒ nrf_drv_twi_xfer ⇒ twi_xfer ⇒ twi_tx_start_transfer ⇒ twi_transfer ⇒ twi_send_byte
  [Calls]
  - >> nrf_drv_mpu_write_single_register
  - >> nrf_drv_mpu_init
  [Called By]
  - >> mpu_setup

  mpu_read_accel (Thumb, 52 bytes, Stack size 24 bytes, app_mpu.o(i.mpu_read_accel))
  [Stack]

  - Max Depth = 264
  - Call Chain = mpu_read_accel ⇒ nrf_drv_mpu_read_registers ⇒ nrf_drv_twi_tx ⇒ nrf_drv_twi_xfer ⇒ twi_xfer ⇒ twi_tx_start_transfer ⇒ twi_transfer ⇒ twi_send_byte
  [Calls]
  - >> nrf_drv_mpu_read_registers
  [Called By]
  - >> main

  mpu_setup (Thumb, 90 bytes, Stack size 16 bytes, main.o(i.mpu_setup))
  [Stack]

  - Max Depth = 264
  - Call Chain = mpu_setup ⇒ mpu_init ⇒ nrf_drv_mpu_write_single_register ⇒ nrf_drv_twi_tx ⇒ nrf_drv_twi_xfer ⇒ twi_xfer ⇒ twi_tx_start_transfer ⇒ twi_transfer ⇒ twi_send_byte
  [Calls]
  - >> mpu_init
  - >> mpu_config
  - >> app_error_handler
  [Called By]
  - >> main

  nrf_drv_common_irq_enable (Thumb, 84 bytes, Stack size 16 bytes, nrf_drv_common.o(i.nrf_drv_common_irq_enable))
  [Stack]

  - Max Depth = 16
  - Call Chain = nrf_drv_common_irq_enable
  [Called By]
  - >> nrf_drv_twi_init
  - >> nrf_drv_uart_init

  nrf_drv_mpu_init (Thumb, 42 bytes, Stack size 24 bytes, nrf_drv_mpu_twi.o(i.nrf_drv_mpu_init))
  [Stack]

  - Max Depth = 72
  - Call Chain = nrf_drv_mpu_init ⇒ nrf_drv_twi_init ⇒ nrf_drv_common_irq_enable
  [Calls]
  - >> nrf_drv_twi_init
  - >> nrf_drv_twi_enable
  [Called By]
  - >> mpu_init

  nrf_drv_mpu_read_registers (Thumb, 118 bytes, Stack size 40 bytes, nrf_drv_mpu_twi.o(i.nrf_drv_mpu_read_registers))
  [Stack]

  - Max Depth = 240
  - Call Chain = nrf_drv_mpu_read_registers ⇒ nrf_drv_twi_tx ⇒ nrf_drv_twi_xfer ⇒ twi_xfer ⇒ twi_tx_start_transfer ⇒ twi_transfer ⇒ twi_send_byte
  [Calls]
  - >> nrf_drv_twi_tx
  - >> nrf_drv_twi_rx
  [Called By]
  - >> mpu_read_accel

  nrf_drv_mpu_write_registers (Thumb, 94 bytes, Stack size 40 bytes, nrf_drv_mpu_twi.o(i.nrf_drv_mpu_write_registers))
  [Stack]

  - Max Depth = 200
  - Call Chain = nrf_drv_mpu_write_registers ⇒ nrf_drv_twi_xfer ⇒ twi_xfer ⇒ twi_tx_start_transfer ⇒ twi_transfer ⇒ twi_send_byte
  [Calls]
  - >> nrf_drv_twi_xfer
  - >> merge_register_and_data
  [Called By]
  - >> mpu_config

  nrf_drv_mpu_write_single_register (Thumb, 76 bytes, Stack size 32 bytes, nrf_drv_mpu_twi.o(i.nrf_drv_mpu_write_single_register))
  [Stack]

  - Max Depth = 232
  - Call Chain = nrf_drv_mpu_write_single_register ⇒ nrf_drv_twi_tx ⇒ nrf_drv_twi_xfer ⇒ twi_xfer ⇒ twi_tx_start_transfer ⇒ twi_transfer ⇒ twi_send_byte
  [Calls]
  - >> nrf_drv_twi_tx
  [Called By]
  - >> mpu_init

  nrf_drv_twi_enable (Thumb, 32 bytes, Stack size 0 bytes, nrf_drv_twi.o(i.nrf_drv_twi_enable))
  [Called By]

  - >> nrf_drv_mpu_init

  nrf_drv_twi_init (Thumb, 142 bytes, Stack size 32 bytes, nrf_drv_twi.o(i.nrf_drv_twi_init))
  [Stack]

  - Max Depth = 48
  - Call Chain = nrf_drv_twi_init ⇒ nrf_drv_common_irq_enable
  [Calls]
  - >> nrf_drv_common_irq_enable
  - >> nrf_drv_get_IRQn
  - >> twi_clear_bus
  [Called By]
  - >> nrf_drv_mpu_init

  nrf_drv_twi_rx (Thumb, 40 bytes, Stack size 32 bytes, nrf_drv_twi.o(i.nrf_drv_twi_rx))
  [Stack]

  - Max Depth = 192
  - Call Chain = nrf_drv_twi_rx ⇒ nrf_drv_twi_xfer ⇒ twi_xfer ⇒ twi_tx_start_transfer ⇒ twi_transfer ⇒ twi_send_byte
  [Calls]
  - >> nrf_drv_twi_xfer
  [Called By]
  - >> nrf_drv_mpu_read_registers

  nrf_drv_twi_tx (Thumb, 60 bytes, Stack size 40 bytes, nrf_drv_twi.o(i.nrf_drv_twi_tx))
  [Stack]

  - Max Depth = 200
  - Call Chain = nrf_drv_twi_tx ⇒ nrf_drv_twi_xfer ⇒ twi_xfer ⇒ twi_tx_start_transfer ⇒ twi_transfer ⇒ twi_send_byte
  [Calls]
  - >> nrf_drv_twi_xfer
  [Called By]
  - >> nrf_drv_mpu_write_single_register
  - >> nrf_drv_mpu_read_registers

  nrf_drv_twi_xfer (Thumb, 54 bytes, Stack size 24 bytes, nrf_drv_twi.o(i.nrf_drv_twi_xfer))
  [Stack]

  - Max Depth = 160
  - Call Chain = nrf_drv_twi_xfer ⇒ twi_xfer ⇒ twi_tx_start_transfer ⇒ twi_transfer ⇒ twi_send_byte
  [Calls]
  - >> twi_xfer
  [Called By]
  - >> nrf_drv_twi_tx
  - >> nrf_drv_twi_rx
  - >> nrf_drv_mpu_write_registers

  nrf_drv_uart_init (Thumb, 202 bytes, Stack size 16 bytes, nrf_drv_uart.o(i.nrf_drv_uart_init))
  [Stack]

  - Max Depth = 68
  - Call Chain = nrf_drv_uart_init ⇒ apply_config ⇒ nrf_gpio_cfg_input ⇒ nrf_gpio_cfg
  [Calls]
  - >> nrf_drv_common_irq_enable
  - >> nrf_uarte_int_enable
  - >> nrf_uarte_event_clear
  - >> nrf_uart_int_enable
  - >> nrf_uart_event_clear
  - >> apply_config
  [Called By]
  - >> app_uart_init

  nrf_drv_uart_rx (Thumb, 168 bytes, Stack size 16 bytes, nrf_drv_uart.o(i.nrf_drv_uart_rx))
  [Stack]

  - Max Depth = 56
  - Call Chain = nrf_drv_uart_rx ⇒ nrf_drv_uart_rx_for_uart ⇒ rx_enable
  [Calls]
  - >> nrf_uarte_int_enable
  - >> nrf_uarte_int_disable
  - >> nrf_uart_int_enable
  - >> nrf_uart_int_disable
  - >> nrf_drv_uart_rx_for_uarte
  - >> nrf_drv_uart_rx_for_uart
  [Called By]
  - >> app_uart_init
  - >> uart_event_handler

  nrf_drv_uart_rx_enable (Thumb, 26 bytes, Stack size 8 bytes, nrf_drv_uart.o(i.nrf_drv_uart_rx_enable))
  [Stack]

  - Max Depth = 16
  - Call Chain = nrf_drv_uart_rx_enable ⇒ rx_enable
  [Calls]
  - >> rx_enable
  [Called By]
  - >> app_uart_init

  nrf_drv_uart_tx (Thumb, 66 bytes, Stack size 16 bytes, nrf_drv_uart.o(i.nrf_drv_uart_tx))
  [Stack]

  - Max Depth = 32
  - Call Chain = nrf_drv_uart_tx ⇒ nrf_drv_uart_tx_for_uarte
  [Calls]
  - >> nrf_drv_uart_tx_in_progress
  - >> nrf_drv_uart_tx_for_uarte
  - >> nrf_drv_uart_tx_for_uart
  [Called By]
  - >> app_uart_put
  - >> uart_event_handler

  nrf_drv_uart_tx_in_progress (Thumb, 14 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_drv_uart_tx_in_progress))
  [Called By]

  - >> nrf_drv_uart_tx
  - >> app_uart_put

  pstorage_access_status_get (Thumb, 36 bytes, Stack size 0 bytes, pstorage.o(i.pstorage_access_status_get))
  [Called By]

  - >> flash_access_in_progress

  pstorage_block_identifier_get (Thumb, 154 bytes, Stack size 24 bytes, pstorage.o(i.pstorage_block_identifier_get))
  [Stack]

  - Max Depth = 24
  - Call Chain = pstorage_block_identifier_get
  [Called By]
  - >> dm_init
  - >> bond_data_load
  - >> dm_pstorage_cb_handler
  - >> device_instance_free
  - >> device_context_store

  pstorage_clear (Thumb, 280 bytes, Stack size 32 bytes, pstorage.o(i.pstorage_clear))
  [Stack]

  - Max Depth = 224
  - Call Chain = pstorage_clear ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ update_operation_execute ⇒ clear_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> is_word_aligned
  - >> cmd_queue_enqueue
  [Called By]
  - >> dm_init
  - >> device_instance_free

  pstorage_init (Thumb, 110 bytes, Stack size 8 bytes, pstorage.o(i.pstorage_init))
  [Stack]

  - Max Depth = 16
  - Call Chain = pstorage_init ⇒ pstorage_flash_page_end
  [Calls]
  - >> pstorage_flash_page_size
  - >> pstorage_flash_page_end
  - >> cmd_queue_init
  [Called By]
  - >> device_manager_init

  pstorage_load (Thumb, 236 bytes, Stack size 24 bytes, pstorage.o(i.pstorage_load))
  [Stack]

  - Max Depth = 24
  - Call Chain = pstorage_load
  [Calls]
  - >> is_word_aligned
  - >> __aeabi_memcpy
  [Called By]
  - >> dm_init
  - >> bond_data_load
  - >> gatts_context_load

  pstorage_register (Thumb, 256 bytes, Stack size 24 bytes, pstorage.o(i.pstorage_register))
  [Stack]

  - Max Depth = 32
  - Call Chain = pstorage_register ⇒ pstorage_flash_page_end
  [Calls]
  - >> pstorage_flash_page_size
  - >> pstorage_flash_page_end
  [Called By]
  - >> dm_init

  pstorage_store (Thumb, 212 bytes, Stack size 24 bytes, pstorage.o(i.pstorage_store))
  [Stack]

  - Max Depth = 216
  - Call Chain = pstorage_store ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ update_operation_execute ⇒ clear_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> is_word_aligned
  - >> cmd_queue_enqueue
  [Address Reference Count : 2]
  - device_manager_peripheral.o(i.gatts_context_store)
  - device_manager_peripheral.o(i.device_context_store)

  pstorage_sys_event_handler (Thumb, 62 bytes, Stack size 8 bytes, pstorage.o(i.pstorage_sys_event_handler))
  [Stack]

  - Max Depth = 144
  - Call Chain = pstorage_sys_event_handler ⇒ flash_operation_success_run ⇒ erase_sub_state_sm_run ⇒ clear_post_processing_run ⇒ store_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> flash_operation_success_run
  - >> flash_operation_failure_run
  [Called By]
  - >> sys_evt_dispatch

  pstorage_update (Thumb, 212 bytes, Stack size 24 bytes, pstorage.o(i.pstorage_update))
  [Stack]

  - Max Depth = 216
  - Call Chain = pstorage_update ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ update_operation_execute ⇒ clear_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> is_word_aligned
  - >> cmd_queue_enqueue
  [Address Reference Count : 2]
  - device_manager_peripheral.o(i.gatts_context_store)
  - device_manager_peripheral.o(i.device_context_store)

  sd_check_ram_start (Thumb, 22 bytes, Stack size 8 bytes, softdevice_handler.o(i.sd_check_ram_start))
  [Stack]

  - Max Depth = 8
  - Call Chain = sd_check_ram_start
  [Called By]
  - >> ble_stack_init

  softdevice_ble_evt_handler_set (Thumb, 20 bytes, Stack size 0 bytes, softdevice_handler.o(i.softdevice_ble_evt_handler_set))
  [Called By]

  - >> ble_stack_init

  softdevice_enable (Thumb, 24 bytes, Stack size 24 bytes, softdevice_handler.o(i.softdevice_enable))
  [Stack]

  - Max Depth = 24
  - Call Chain = softdevice_enable
  [Called By]
  - >> ble_stack_init

  softdevice_enable_get_default_config (Thumb, 44 bytes, Stack size 16 bytes, softdevice_handler.o(i.softdevice_enable_get_default_config))
  [Stack]

  - Max Depth = 16
  - Call Chain = softdevice_enable_get_default_config
  [Calls]
  - >> __aeabi_memclr4
  [Called By]
  - >> ble_stack_init

  softdevice_fault_handler (Thumb, 20 bytes, Stack size 16 bytes, softdevice_handler.o(i.softdevice_fault_handler))
  [Stack]

  - Max Depth = 44
  - Call Chain = softdevice_fault_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> app_error_fault_handler
  [Address Reference Count : 1]
  - softdevice_handler.o(i.softdevice_handler_init)

  softdevice_handler_init (Thumb, 80 bytes, Stack size 24 bytes, softdevice_handler.o(i.softdevice_handler_init))
  [Stack]

  - Max Depth = 32
  - Call Chain = softdevice_handler_init ⇒ sd_nvic_EnableIRQ
  [Calls]
  - >> sd_nvic_EnableIRQ
  [Called By]
  - >> ble_stack_init

  softdevice_sys_evt_handler_set (Thumb, 20 bytes, Stack size 0 bytes, softdevice_handler.o(i.softdevice_sys_evt_handler_set))
  [Called By]

  - >> ble_stack_init

  timer_accel_update_handler (Thumb, 8 bytes, Stack size 0 bytes, main.o(i.timer_accel_update_handler))
  [Address Reference Count : 1]

  - main.o(i.timers_init)

  ### Local Symbols

  advertising_init (Thumb, 94 bytes, Stack size 112 bytes, main.o(i.advertising_init))
  [Stack]

  - Max Depth = 368
  - Call Chain = advertising_init ⇒ ble_advertising_init ⇒ ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> ble_advertising_init
  - >> app_error_handler
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  application_timers_start (Thumb, 2 bytes, Stack size 0 bytes, main.o(i.application_timers_start))
  [Called By]

  - >> main

  ble_evt_dispatch (Thumb, 38 bytes, Stack size 8 bytes, main.o(i.ble_evt_dispatch))
  [Stack]

  - Max Depth = 344
  - Call Chain = ble_evt_dispatch ⇒ dm_ble_evt_handler ⇒ device_instance_free ⇒ pstorage_clear ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ update_operation_execute ⇒ clear_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> dm_ble_evt_handler
  - >> ble_mpu_on_ble_evt
  - >> ble_conn_params_on_ble_evt
  - >> ble_advertising_on_ble_evt
  - >> on_ble_evt
  [Address Reference Count : 1]
  - main.o(i.ble_stack_init)

  ble_stack_init (Thumb, 226 bytes, Stack size 40 bytes, main.o(i.ble_stack_init))
  [Stack]

  - Max Depth = 100
  - Call Chain = ble_stack_init ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> softdevice_sys_evt_handler_set
  - >> softdevice_handler_init
  - >> softdevice_enable_get_default_config
  - >> softdevice_enable
  - >> softdevice_ble_evt_handler_set
  - >> sd_check_ram_start
  - >> app_error_handler
  [Called By]
  - >> main

  conn_params_error_handler (Thumb, 20 bytes, Stack size 8 bytes, main.o(i.conn_params_error_handler))
  [Stack]

  - Max Depth = 68
  - Call Chain = conn_params_error_handler ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> app_error_handler
  [Address Reference Count : 1]
  - main.o(i.conn_params_init)

  conn_params_init (Thumb, 86 bytes, Stack size 40 bytes, main.o(i.conn_params_init))
  [Stack]

  - Max Depth = 100
  - Call Chain = conn_params_init ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> ble_conn_params_init
  - >> app_error_handler
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  device_manager_evt_handler (Thumb, 40 bytes, Stack size 24 bytes, main.o(i.device_manager_evt_handler))
  [Stack]

  - Max Depth = 84
  - Call Chain = device_manager_evt_handler ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> app_error_handler
  [Address Reference Count : 1]
  - main.o(i.device_manager_init)

  device_manager_init (Thumb, 188 bytes, Stack size 32 bytes, main.o(i.device_manager_init))
  [Stack]

  - Max Depth = 288
  - Call Chain = device_manager_init ⇒ dm_init ⇒ pstorage_clear ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ update_operation_execute ⇒ clear_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> pstorage_init
  - >> dm_register
  - >> dm_init
  - >> app_error_handler
  [Called By]
  - >> main

  gap_params_init (Thumb, 124 bytes, Stack size 24 bytes, main.o(i.gap_params_init))
  [Stack]

  - Max Depth = 84
  - Call Chain = gap_params_init ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> app_error_handler
  [Called By]
  - >> main

  on_adv_evt (Thumb, 54 bytes, Stack size 16 bytes, main.o(i.on_adv_evt))
  [Stack]

  - Max Depth = 92
  - Call Chain = on_adv_evt ⇒ sleep_mode_enter ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> bsp_indication_set
  - >> app_error_handler
  - >> sleep_mode_enter
  [Address Reference Count : 1]
  - main.o(i.advertising_init)

  on_ble_evt (Thumb, 120 bytes, Stack size 16 bytes, main.o(i.on_ble_evt))
  [Stack]

  - Max Depth = 92
  - Call Chain = on_ble_evt ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> bsp_indication_set
  - >> app_timer_stop
  - >> app_timer_start
  - >> app_error_handler
  [Called By]
  - >> ble_evt_dispatch

  on_conn_params_evt (Thumb, 42 bytes, Stack size 16 bytes, main.o(i.on_conn_params_evt))
  [Stack]

  - Max Depth = 76
  - Call Chain = on_conn_params_evt ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> app_error_handler
  [Address Reference Count : 1]
  - main.o(i.conn_params_init)

  power_manage (Thumb, 32 bytes, Stack size 16 bytes, main.o(i.power_manage))
  [Stack]

  - Max Depth = 76
  - Call Chain = power_manage ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> app_error_handler
  [Called By]
  - >> main

  services_init (Thumb, 10 bytes, Stack size 8 bytes, main.o(i.services_init))
  [Stack]

  - Max Depth = 196
  - Call Chain = services_init ⇒ ble_mpu_service_init ⇒ ble_char_accel_add ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> ble_mpu_service_init
  [Called By]
  - >> main

  sleep_mode_enter (Thumb, 30 bytes, Stack size 16 bytes, main.o(i.sleep_mode_enter))
  [Stack]

  - Max Depth = 76
  - Call Chain = sleep_mode_enter ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> app_error_handler
  [Called By]
  - >> on_adv_evt

  sys_evt_dispatch (Thumb, 18 bytes, Stack size 8 bytes, main.o(i.sys_evt_dispatch))
  [Stack]

  - Max Depth = 288
  - Call Chain = sys_evt_dispatch ⇒ ble_advertising_on_sys_evt ⇒ ble_advertising_start ⇒ ble_advdata_set ⇒ adv_data_encode ⇒ uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> pstorage_sys_event_handler
  - >> ble_advertising_on_sys_evt
  [Address Reference Count : 1]
  - main.o(i.ble_stack_init)

  timers_init (Thumb, 78 bytes, Stack size 16 bytes, main.o(i.timers_init))
  [Stack]

  - Max Depth = 76
  - Call Chain = timers_init ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> app_timer_init
  - >> app_timer_create
  - >> app_error_handler
  [Called By]
  - >> main

  uart_config (Thumb, 76 bytes, Stack size 40 bytes, main.o(i.uart_config))
  [Stack]

  - Max Depth = 164
  - Call Chain = uart_config ⇒ app_uart_init ⇒ nrf_drv_uart_init ⇒ apply_config ⇒ nrf_gpio_cfg_input ⇒ nrf_gpio_cfg
  [Calls]
  - >> app_uart_init
  - >> app_error_handler
  [Called By]
  - >> main

  uart_events_handler (Thumb, 56 bytes, Stack size 8 bytes, main.o(i.uart_events_handler))
  [Stack]

  - Max Depth = 68
  - Call Chain = uart_events_handler ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> app_error_handler
  [Address Reference Count : 1]
  - main.o(i.uart_config)

  ble_char_accel_add (Thumb, 316 bytes, Stack size 88 bytes, ble_mpu.o(i.ble_char_accel_add))
  [Stack]

  - Max Depth = 148
  - Call Chain = ble_char_accel_add ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> app_error_handler
  - >> __aeabi_memclr4
  [Called By]
  - >> ble_mpu_service_init

  merge_register_and_data (Thumb, 28 bytes, Stack size 24 bytes, nrf_drv_mpu_twi.o(i.merge_register_and_data))
  [Stack]

  - Max Depth = 24
  - Call Chain = merge_register_and_data
  [Calls]
  - >> __aeabi_memcpy
  [Called By]
  - >> nrf_drv_mpu_write_registers

  nrf_drv_mpu_twi_event_handler (Thumb, 80 bytes, Stack size 0 bytes, nrf_drv_mpu_twi.o(i.nrf_drv_mpu_twi_event_handler))
  [Address Reference Count : 1]

  - nrf_drv_mpu_twi.o(i.nrf_drv_mpu_init)

  advdata_check (Thumb, 18 bytes, Stack size 0 bytes, ble_advdata.o(i.advdata_check))
  [Called By]

  - >> ble_advdata_set

  appearance_encode (Thumb, 82 bytes, Stack size 24 bytes, ble_advdata.o(i.appearance_encode))
  [Stack]

  - Max Depth = 24
  - Call Chain = appearance_encode
  [Calls]
  - >> uint16_encode
  [Called By]
  - >> adv_data_encode

  ble_device_addr_encode (Thumb, 116 bytes, Stack size 32 bytes, ble_advdata.o(i.ble_device_addr_encode))
  [Stack]

  - Max Depth = 32
  - Call Chain = ble_device_addr_encode
  [Called By]
  - >> adv_data_encode

  conn_int_check (Thumb, 90 bytes, Stack size 0 bytes, ble_advdata.o(i.conn_int_check))
  [Called By]

  - >> conn_int_encode

  conn_int_encode (Thumb, 104 bytes, Stack size 24 bytes, ble_advdata.o(i.conn_int_encode))
  [Stack]

  - Max Depth = 24
  - Call Chain = conn_int_encode
  [Calls]
  - >> conn_int_check
  - >> uint16_encode
  [Called By]
  - >> adv_data_encode

  flags_encode (Thumb, 54 bytes, Stack size 12 bytes, ble_advdata.o(i.flags_encode))
  [Stack]

  - Max Depth = 12
  - Call Chain = flags_encode
  [Called By]
  - >> adv_data_encode

  le_role_encode (Thumb, 106 bytes, Stack size 12 bytes, ble_advdata.o(i.le_role_encode))
  [Stack]

  - Max Depth = 12
  - Call Chain = le_role_encode
  [Called By]
  - >> adv_data_encode

  manuf_specific_data_encode (Thumb, 118 bytes, Stack size 24 bytes, ble_advdata.o(i.manuf_specific_data_encode))
  [Stack]

  - Max Depth = 24
  - Call Chain = manuf_specific_data_encode
  [Calls]
  - >> uint16_encode
  - >> __aeabi_memcpy
  [Called By]
  - >> adv_data_encode

  name_encode (Thumb, 194 bytes, Stack size 40 bytes, ble_advdata.o(i.name_encode))
  [Stack]

  - Max Depth = 40
  - Call Chain = name_encode
  [Called By]
  - >> adv_data_encode

  sec_mgr_oob_flags_encode (Thumb, 54 bytes, Stack size 12 bytes, ble_advdata.o(i.sec_mgr_oob_flags_encode))
  [Stack]

  - Max Depth = 12
  - Call Chain = sec_mgr_oob_flags_encode
  [Called By]
  - >> adv_data_encode

  service_data_encode (Thumb, 150 bytes, Stack size 32 bytes, ble_advdata.o(i.service_data_encode))
  [Stack]

  - Max Depth = 32
  - Call Chain = service_data_encode
  [Calls]
  - >> uint16_encode
  - >> __aeabi_memcpy
  [Called By]
  - >> adv_data_encode

  srdata_check (Thumb, 14 bytes, Stack size 0 bytes, ble_advdata.o(i.srdata_check))
  [Called By]

  - >> ble_advdata_set

  tk_value_encode (Thumb, 70 bytes, Stack size 16 bytes, ble_advdata.o(i.tk_value_encode))
  [Stack]

  - Max Depth = 16
  - Call Chain = tk_value_encode
  [Called By]
  - >> adv_data_encode

  tx_power_level_encode (Thumb, 54 bytes, Stack size 12 bytes, ble_advdata.o(i.tx_power_level_encode))
  [Stack]

  - Max Depth = 12
  - Call Chain = tx_power_level_encode
  [Called By]
  - >> adv_data_encode

  uint16_encode (Thumb, 12 bytes, Stack size 0 bytes, ble_advdata.o(i.uint16_encode))
  [Called By]

  - >> conn_int_encode
  - >> appearance_encode
  - >> service_data_encode
  - >> manuf_specific_data_encode

  uuid_list_encode (Thumb, 78 bytes, Stack size 40 bytes, ble_advdata.o(i.uuid_list_encode))
  [Stack]

  - Max Depth = 96
  - Call Chain = uuid_list_encode ⇒ uuid_list_sized_encode
  [Calls]
  - >> uuid_list_sized_encode
  [Called By]
  - >> adv_data_encode

  uuid_list_sized_encode (Thumb, 220 bytes, Stack size 56 bytes, ble_advdata.o(i.uuid_list_sized_encode))
  [Stack]

  - Max Depth = 56
  - Call Chain = uuid_list_sized_encode
  [Called By]
  - >> uuid_list_encode

  ble_advertising_peer_address_clear (Thumb, 12 bytes, Stack size 0 bytes, ble_advertising.o(i.ble_advertising_peer_address_clear))
  [Called By]

  - >> ble_advertising_start
  - >> ble_advertising_init

  flash_access_in_progress (Thumb, 54 bytes, Stack size 16 bytes, ble_advertising.o(i.flash_access_in_progress))
  [Stack]

  - Max Depth = 16
  - Call Chain = flash_access_in_progress
  [Calls]
  - >> pstorage_access_status_get
  - >> fs_queued_op_count_get
  [Called By]
  - >> ble_advertising_start

  peer_address_exists (Thumb, 24 bytes, Stack size 0 bytes, ble_advertising.o(i.peer_address_exists))
  [Called By]

  - >> ble_advertising_start

  whitelist_has_entries (Thumb, 18 bytes, Stack size 0 bytes, ble_advertising.o(i.whitelist_has_entries))
  [Called By]

  - >> ble_advertising_start

  conn_params_negotiation (Thumb, 112 bytes, Stack size 16 bytes, ble_conn_params.o(i.conn_params_negotiation))
  [Stack]

  - Max Depth = 92
  - Call Chain = conn_params_negotiation ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> app_timer_start
  - >> is_conn_params_ok
  [Called By]
  - >> on_write
  - >> on_connect
  - >> on_conn_params_update

  is_conn_params_ok (Thumb, 30 bytes, Stack size 0 bytes, ble_conn_params.o(i.is_conn_params_ok))
  [Called By]

  - >> conn_params_negotiation

  on_conn_params_update (Thumb, 20 bytes, Stack size 8 bytes, ble_conn_params.o(i.on_conn_params_update))
  [Stack]

  - Max Depth = 100
  - Call Chain = on_conn_params_update ⇒ conn_params_negotiation ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> conn_params_negotiation
  [Called By]
  - >> ble_conn_params_on_ble_evt

  on_connect (Thumb, 38 bytes, Stack size 8 bytes, ble_conn_params.o(i.on_connect))
  [Stack]

  - Max Depth = 100
  - Call Chain = on_connect ⇒ conn_params_negotiation ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> conn_params_negotiation
  [Called By]
  - >> ble_conn_params_on_ble_evt

  on_disconnect (Thumb, 46 bytes, Stack size 16 bytes, ble_conn_params.o(i.on_disconnect))
  [Stack]

  - Max Depth = 68
  - Call Chain = on_disconnect ⇒ app_timer_stop ⇒ timer_stop_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> app_timer_stop
  [Called By]
  - >> ble_conn_params_on_ble_evt

  on_write (Thumb, 78 bytes, Stack size 16 bytes, ble_conn_params.o(i.on_write))
  [Stack]

  - Max Depth = 108
  - Call Chain = on_write ⇒ conn_params_negotiation ⇒ app_timer_start ⇒ timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> app_timer_stop
  - >> conn_params_negotiation
  [Called By]
  - >> ble_conn_params_on_ble_evt

  update_timeout_handler (Thumb, 126 bytes, Stack size 16 bytes, ble_conn_params.o(i.update_timeout_handler))
  [Stack]

  - Max Depth = 16
  - Call Chain = update_timeout_handler
  [Address Reference Count : 1]
  - ble_conn_params.o(i.ble_conn_params_init)

  app_evt_notify (Thumb, 26 bytes, Stack size 24 bytes, device_manager_peripheral.o(i.app_evt_notify))
  [Stack]

  - Max Depth = 24
  - Call Chain = app_evt_notify
  [Called By]
  - >> dm_ble_evt_handler
  - >> dm_pstorage_cb_handler

  connection_instance_find (Thumb, 68 bytes, Stack size 16 bytes, device_manager_peripheral.o(i.connection_instance_find))
  [Stack]

  - Max Depth = 16
  - Call Chain = connection_instance_find
  [Called By]
  - >> dm_ble_evt_handler

  connection_instance_init (Thumb, 60 bytes, Stack size 0 bytes, device_manager_peripheral.o(i.connection_instance_init))
  [Called By]

  - >> dm_init
  - >> dm_ble_evt_handler

  device_context_store (Thumb, 186 bytes, Stack size 32 bytes, device_manager_peripheral.o(i.device_context_store))
  [Stack]

  - Max Depth = 56
  - Call Chain = device_context_store ⇒ pstorage_block_identifier_get
  [Calls]
  - >> pstorage_block_identifier_get
  [Called By]
  - >> dm_ble_evt_handler

  device_instance_allocate (Thumb, 130 bytes, Stack size 16 bytes, device_manager_peripheral.o(i.device_instance_allocate))
  [Stack]

  - Max Depth = 16
  - Call Chain = device_instance_allocate
  [Called By]
  - >> dm_ble_evt_handler

  device_instance_find (Thumb, 84 bytes, Stack size 24 bytes, device_manager_peripheral.o(i.device_instance_find))
  [Stack]

  - Max Depth = 36
  - Call Chain = device_instance_find ⇒ memcmp
  [Calls]
  - >> memcmp
  [Called By]
  - >> dm_ble_evt_handler

  device_instance_free (Thumb, 40 bytes, Stack size 24 bytes, device_manager_peripheral.o(i.device_instance_free))
  [Stack]

  - Max Depth = 248
  - Call Chain = device_instance_free ⇒ pstorage_clear ⇒ cmd_queue_enqueue ⇒ cmd_process ⇒ update_operation_execute ⇒ clear_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> pstorage_clear
  - >> pstorage_block_identifier_get
  - >> peer_instance_init
  [Called By]
  - >> dm_ble_evt_handler

  dm_pstorage_cb_handler (Thumb, 560 bytes, Stack size 120 bytes, device_manager_peripheral.o(i.dm_pstorage_cb_handler))
  [Stack]

  - Max Depth = 180
  - Call Chain = dm_pstorage_cb_handler ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> app_error_handler
  - >> pstorage_block_identifier_get
  - >> dm_handle_initialize
  - >> update_status_bit_reset
  - >> app_evt_notify
  - >> memcmp
  - >> __aeabi_memclr4
  [Address Reference Count : 1]
  - device_manager_peripheral.o(i.dm_init)

  gattc_context_apply (Thumb, 6 bytes, Stack size 0 bytes, device_manager_peripheral.o(i.gattc_context_apply))
  [Address Reference Count : 1]

  - device_manager_peripheral.o(.constdata)

  gattc_context_load (Thumb, 6 bytes, Stack size 0 bytes, device_manager_peripheral.o(i.gattc_context_load))
  [Address Reference Count : 1]

  - device_manager_peripheral.o(.constdata)

  gattc_context_store (Thumb, 6 bytes, Stack size 0 bytes, device_manager_peripheral.o(i.gattc_context_store))
  [Address Reference Count : 1]

  - device_manager_peripheral.o(.constdata)

  gatts_context_apply (Thumb, 238 bytes, Stack size 24 bytes, device_manager_peripheral.o(i.gatts_context_apply))
  [Stack]

  - Max Depth = 24
  - Call Chain = gatts_context_apply
  [Called By]
  - >> gattsc_context_apply
  [Address Reference Count : 1]
  - device_manager_peripheral.o(.constdata)

  gatts_context_load (Thumb, 70 bytes, Stack size 16 bytes, device_manager_peripheral.o(i.gatts_context_load))
  [Stack]

  - Max Depth = 40
  - Call Chain = gatts_context_load ⇒ pstorage_load
  [Calls]
  - >> pstorage_load
  [Called By]
  - >> gattsc_context_load
  [Address Reference Count : 1]
  - device_manager_peripheral.o(.constdata)

  gatts_context_store (Thumb, 224 bytes, Stack size 56 bytes, device_manager_peripheral.o(i.gatts_context_store))
  [Stack]

  - Max Depth = 68
  - Call Chain = gatts_context_store ⇒ memcmp
  [Calls]
  - >> memcmp
  - >> __aeabi_memclr4
  - >> __aeabi_memcpy4
  [Called By]
  - >> gattsc_context_store
  [Address Reference Count : 1]
  - device_manager_peripheral.o(.constdata)

  gattsc_context_apply (Thumb, 24 bytes, Stack size 16 bytes, device_manager_peripheral.o(i.gattsc_context_apply))
  [Stack]

  - Max Depth = 40
  - Call Chain = gattsc_context_apply ⇒ gatts_context_apply
  [Calls]
  - >> gatts_context_apply
  [Address Reference Count : 1]
  - device_manager_peripheral.o(.constdata)

  gattsc_context_load (Thumb, 28 bytes, Stack size 16 bytes, device_manager_peripheral.o(i.gattsc_context_load))
  [Stack]

  - Max Depth = 56
  - Call Chain = gattsc_context_load ⇒ gatts_context_load ⇒ pstorage_load
  [Calls]
  - >> gatts_context_load
  [Address Reference Count : 1]
  - device_manager_peripheral.o(.constdata)

  gattsc_context_store (Thumb, 28 bytes, Stack size 16 bytes, device_manager_peripheral.o(i.gattsc_context_store))
  [Stack]

  - Max Depth = 84
  - Call Chain = gattsc_context_store ⇒ gatts_context_store ⇒ memcmp
  [Calls]
  - >> gatts_context_store
  [Address Reference Count : 1]
  - device_manager_peripheral.o(.constdata)

  no_service_context_apply (Thumb, 6 bytes, Stack size 0 bytes, device_manager_peripheral.o(i.no_service_context_apply))
  [Address Reference Count : 1]

  - device_manager_peripheral.o(.constdata)

  no_service_context_load (Thumb, 6 bytes, Stack size 0 bytes, device_manager_peripheral.o(i.no_service_context_load))
  [Address Reference Count : 1]

  - device_manager_peripheral.o(.constdata)

  no_service_context_store (Thumb, 6 bytes, Stack size 0 bytes, device_manager_peripheral.o(i.no_service_context_store))
  [Address Reference Count : 1]

  - device_manager_peripheral.o(.constdata)

  peer_instance_init (Thumb, 92 bytes, Stack size 8 bytes, device_manager_peripheral.o(i.peer_instance_init))
  [Stack]

  - Max Depth = 8
  - Call Chain = peer_instance_init
  [Calls]
  - >> update_status_bit_reset
  - >> __aeabi_memclr
  [Called By]
  - >> dm_init
  - >> dm_ble_evt_handler
  - >> device_instance_free

  storage_operation_dummy_handler (Thumb, 8 bytes, Stack size 8 bytes, device_manager_peripheral.o(i.storage_operation_dummy_handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = storage_operation_dummy_handler
  [Address Reference Count : 1]
  - device_manager_peripheral.o(i.device_context_store)

  update_status_bit_reset (Thumb, 16 bytes, Stack size 0 bytes, device_manager_peripheral.o(i.update_status_bit_reset))
  [Called By]

  - >> peer_instance_init
  - >> dm_pstorage_cb_handler

  channel_handler_get (Thumb, 10 bytes, Stack size 0 bytes, nrf_drv_gpiote.o(i.channel_handler_get))
  [Called By]

  - >> GPIOTE_IRQHandler

  channel_port_get (Thumb, 8 bytes, Stack size 0 bytes, nrf_drv_gpiote.o(i.channel_port_get))
  [Called By]

  - >> GPIOTE_IRQHandler

  nrf_gpio_cfg_sense_set (Thumb, 32 bytes, Stack size 0 bytes, nrf_drv_gpiote.o(i.nrf_gpio_cfg_sense_set))
  [Called By]

  - >> GPIOTE_IRQHandler

  nrf_gpiote_event_addr_get (Thumb, 8 bytes, Stack size 0 bytes, nrf_drv_gpiote.o(i.nrf_gpiote_event_addr_get))
  [Called By]

  - >> nrf_gpiote_event_is_set
  - >> nrf_gpiote_event_clear

  nrf_gpiote_event_clear (Thumb, 28 bytes, Stack size 16 bytes, nrf_drv_gpiote.o(i.nrf_gpiote_event_clear))
  [Stack]

  - Max Depth = 16
  - Call Chain = nrf_gpiote_event_clear
  [Calls]
  - >> nrf_gpiote_event_addr_get
  [Called By]
  - >> GPIOTE_IRQHandler

  nrf_gpiote_event_is_set (Thumb, 22 bytes, Stack size 8 bytes, nrf_drv_gpiote.o(i.nrf_gpiote_event_is_set))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_gpiote_event_is_set
  [Calls]
  - >> nrf_gpiote_event_addr_get
  [Called By]
  - >> GPIOTE_IRQHandler

  apply_config (Thumb, 174 bytes, Stack size 8 bytes, nrf_drv_uart.o(i.apply_config))
  [Stack]

  - Max Depth = 52
  - Call Chain = apply_config ⇒ nrf_gpio_cfg_input ⇒ nrf_gpio_cfg
  [Calls]
  - >> nrf_uarte_txrx_pins_set
  - >> nrf_uarte_hwfc_pins_set
  - >> nrf_uart_txrx_pins_set
  - >> nrf_uart_hwfc_pins_set
  - >> nrf_gpio_pin_set
  - >> nrf_gpio_cfg_output
  - >> nrf_gpio_cfg_input
  [Called By]
  - >> nrf_drv_uart_init

  nrf_drv_uart_rx_for_uart (Thumb, 172 bytes, Stack size 32 bytes, nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uart))
  [Stack]

  - Max Depth = 40
  - Call Chain = nrf_drv_uart_rx_for_uart ⇒ rx_enable
  [Calls]
  - >> rx_enable
  - >> rx_byte
  - >> nrf_uart_task_trigger
  - >> nrf_uart_int_enable
  - >> nrf_uart_event_clear
  - >> nrf_uart_event_check
  [Called By]
  - >> nrf_drv_uart_rx

  nrf_drv_uart_rx_for_uarte (Thumb, 168 bytes, Stack size 32 bytes, nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uarte))
  [Stack]

  - Max Depth = 32
  - Call Chain = nrf_drv_uart_rx_for_uarte
  [Calls]
  - >> nrf_uarte_task_trigger
  - >> nrf_uarte_int_enable
  - >> nrf_uarte_event_clear
  - >> nrf_uarte_event_check
  [Called By]
  - >> nrf_drv_uart_rx

  nrf_drv_uart_tx_for_uart (Thumb, 132 bytes, Stack size 8 bytes, nrf_drv_uart.o(i.nrf_drv_uart_tx_for_uart))
  [Stack]

  - Max Depth = 16
  - Call Chain = nrf_drv_uart_tx_for_uart ⇒ tx_byte
  [Calls]
  - >> tx_byte
  - >> nrf_uart_task_trigger
  - >> nrf_uart_event_clear
  - >> nrf_uart_event_check
  [Called By]
  - >> nrf_drv_uart_tx

  nrf_drv_uart_tx_for_uarte (Thumb, 104 bytes, Stack size 16 bytes, nrf_drv_uart.o(i.nrf_drv_uart_tx_for_uarte))
  [Stack]

  - Max Depth = 16
  - Call Chain = nrf_drv_uart_tx_for_uarte
  [Calls]
  - >> nrf_uarte_task_trigger
  - >> nrf_uarte_event_clear
  - >> nrf_uarte_event_check
  [Called By]
  - >> nrf_drv_uart_tx

  nrf_gpio_cfg (Thumb, 30 bytes, Stack size 20 bytes, nrf_drv_uart.o(i.nrf_gpio_cfg))
  [Stack]

  - Max Depth = 20
  - Call Chain = nrf_gpio_cfg
  [Called By]
  - >> nrf_gpio_cfg_output
  - >> nrf_gpio_cfg_input

  nrf_gpio_cfg_input (Thumb, 26 bytes, Stack size 24 bytes, nrf_drv_uart.o(i.nrf_gpio_cfg_input))
  [Stack]

  - Max Depth = 44
  - Call Chain = nrf_gpio_cfg_input ⇒ nrf_gpio_cfg
  [Calls]
  - >> nrf_gpio_cfg
  [Called By]
  - >> apply_config

  nrf_gpio_cfg_output (Thumb, 24 bytes, Stack size 16 bytes, nrf_drv_uart.o(i.nrf_gpio_cfg_output))
  [Stack]

  - Max Depth = 36
  - Call Chain = nrf_gpio_cfg_output ⇒ nrf_gpio_cfg
  [Calls]
  - >> nrf_gpio_cfg
  [Called By]
  - >> apply_config

  nrf_gpio_pin_set (Thumb, 10 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_gpio_pin_set))
  [Called By]

  - >> apply_config

  nrf_uart_errorsrc_get_and_clear (Thumb, 12 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uart_errorsrc_get_and_clear))
  [Called By]

  - >> uart_irq_handler

  nrf_uart_event_check (Thumb, 14 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uart_event_check))
  [Called By]

  - >> uart_irq_handler
  - >> nrf_drv_uart_tx_for_uart
  - >> nrf_drv_uart_rx_for_uart

  nrf_uart_event_clear (Thumb, 6 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uart_event_clear))
  [Called By]

  - >> nrf_drv_uart_init
  - >> uart_irq_handler
  - >> tx_byte
  - >> rx_enable
  - >> rx_byte
  - >> nrf_drv_uart_tx_for_uart
  - >> nrf_drv_uart_rx_for_uart

  nrf_uart_hwfc_pins_set (Thumb, 10 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uart_hwfc_pins_set))
  [Called By]

  - >> apply_config

  nrf_uart_int_disable (Thumb, 6 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uart_int_disable))
  [Called By]

  - >> nrf_drv_uart_rx
  - >> uart_irq_handler

  nrf_uart_int_enable (Thumb, 6 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uart_int_enable))
  [Called By]

  - >> nrf_drv_uart_rx
  - >> nrf_drv_uart_init
  - >> nrf_drv_uart_rx_for_uart

  nrf_uart_int_enable_check (Thumb, 18 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uart_int_enable_check))
  [Called By]

  - >> uart_irq_handler

  nrf_uart_task_trigger (Thumb, 6 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uart_task_trigger))
  [Called By]

  - >> uart_irq_handler
  - >> rx_enable
  - >> nrf_drv_uart_tx_for_uart
  - >> nrf_drv_uart_rx_for_uart

  nrf_uart_txrx_pins_set (Thumb, 10 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uart_txrx_pins_set))
  [Called By]

  - >> apply_config

  nrf_uarte_errorsrc_get_and_clear (Thumb, 12 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uarte_errorsrc_get_and_clear))
  [Called By]

  - >> uarte_irq_handler

  nrf_uarte_event_check (Thumb, 14 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uarte_event_check))
  [Called By]

  - >> uarte_irq_handler
  - >> nrf_drv_uart_tx_for_uarte
  - >> nrf_drv_uart_rx_for_uarte

  nrf_uarte_event_clear (Thumb, 6 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uarte_event_clear))
  [Called By]

  - >> nrf_drv_uart_init
  - >> uarte_irq_handler
  - >> nrf_drv_uart_tx_for_uarte
  - >> nrf_drv_uart_rx_for_uarte

  nrf_uarte_hwfc_pins_set (Thumb, 12 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uarte_hwfc_pins_set))
  [Called By]

  - >> apply_config

  nrf_uarte_int_disable (Thumb, 6 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uarte_int_disable))
  [Called By]

  - >> nrf_drv_uart_rx

  nrf_uarte_int_enable (Thumb, 6 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uarte_int_enable))
  [Called By]

  - >> nrf_drv_uart_rx
  - >> nrf_drv_uart_init
  - >> nrf_drv_uart_rx_for_uarte

  nrf_uarte_rx_amount_get (Thumb, 10 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uarte_rx_amount_get))
  [Called By]

  - >> uarte_irq_handler

  nrf_uarte_task_trigger (Thumb, 6 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uarte_task_trigger))
  [Called By]

  - >> nrf_drv_uart_tx_for_uarte
  - >> nrf_drv_uart_rx_for_uarte

  nrf_uarte_txrx_pins_set (Thumb, 14 bytes, Stack size 0 bytes, nrf_drv_uart.o(i.nrf_uarte_txrx_pins_set))
  [Called By]

  - >> apply_config

  rx_byte (Thumb, 68 bytes, Stack size 8 bytes, nrf_drv_uart.o(i.rx_byte))
  [Stack]

  - Max Depth = 8
  - Call Chain = rx_byte
  [Calls]
  - >> nrf_uart_event_clear
  [Called By]
  - >> uart_irq_handler
  - >> nrf_drv_uart_rx_for_uart

  rx_done_event (Thumb, 30 bytes, Stack size 32 bytes, nrf_drv_uart.o(i.rx_done_event))
  [Stack]

  - Max Depth = 32
  - Call Chain = rx_done_event
  [Called By]
  - >> uarte_irq_handler
  - >> uart_irq_handler

  rx_enable (Thumb, 32 bytes, Stack size 8 bytes, nrf_drv_uart.o(i.rx_enable))
  [Stack]

  - Max Depth = 8
  - Call Chain = rx_enable
  [Calls]
  - >> nrf_uart_task_trigger
  - >> nrf_uart_event_clear
  [Called By]
  - >> nrf_drv_uart_rx_enable
  - >> nrf_drv_uart_rx_for_uart

  tx_byte (Thumb, 42 bytes, Stack size 8 bytes, nrf_drv_uart.o(i.tx_byte))
  [Stack]

  - Max Depth = 8
  - Call Chain = tx_byte
  [Calls]
  - >> nrf_uart_event_clear
  [Called By]
  - >> uart_irq_handler
  - >> nrf_drv_uart_tx_for_uart

  tx_done_event (Thumb, 38 bytes, Stack size 24 bytes, nrf_drv_uart.o(i.tx_done_event))
  [Stack]

  - Max Depth = 24
  - Call Chain = tx_done_event
  [Called By]
  - >> uarte_irq_handler
  - >> uart_irq_handler

  uart_irq_handler (Thumb, 342 bytes, Stack size 32 bytes, nrf_drv_uart.o(i.uart_irq_handler))
  [Stack]

  - Max Depth = 64
  - Call Chain = uart_irq_handler ⇒ rx_done_event
  [Calls]
  - >> tx_done_event
  - >> tx_byte
  - >> rx_done_event
  - >> rx_byte
  - >> nrf_uart_task_trigger
  - >> nrf_uart_int_enable_check
  - >> nrf_uart_int_disable
  - >> nrf_uart_event_clear
  - >> nrf_uart_event_check
  - >> nrf_uart_errorsrc_get_and_clear
  [Called By]
  - >> UARTE0_UART0_IRQHandler

  uarte_irq_handler (Thumb, 286 bytes, Stack size 32 bytes, nrf_drv_uart.o(i.uarte_irq_handler))
  [Stack]

  - Max Depth = 64
  - Call Chain = uarte_irq_handler ⇒ rx_done_event
  [Calls]
  - >> tx_done_event
  - >> rx_done_event
  - >> nrf_uarte_rx_amount_get
  - >> nrf_uarte_event_clear
  - >> nrf_uarte_event_check
  - >> nrf_uarte_errorsrc_get_and_clear
  [Called By]
  - >> UARTE0_UART0_IRQHandler

  app_notify (Thumb, 40 bytes, Stack size 24 bytes, pstorage.o(i.app_notify))
  [Stack]

  - Max Depth = 24
  - Call Chain = app_notify
  [Called By]
  - >> command_end_procedure_run
  - >> app_notify_error_state_transit

  app_notify_error_state_transit (Thumb, 34 bytes, Stack size 8 bytes, pstorage.o(i.app_notify_error_state_transit))
  [Stack]

  - Max Depth = 32 + In Cycle
  - Call Chain = app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> sm_state_change
  - >> app_notify
  [Called By]
  - >> flash_operation_failure_run
  - >> flash_api_err_code_process

  clear_operation_execute (Thumb, 238 bytes, Stack size 40 bytes, pstorage.o(i.clear_operation_execute))
  [Stack]

  - Max Depth = 144
  - Call Chain = clear_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> tail_word_size_calculate
  - >> sm_state_change
  - >> pstorage_flash_page_size
  [Called By]
  - >> update_operation_execute
  - >> cmd_process

  clear_post_processing_run (Thumb, 36 bytes, Stack size 8 bytes, pstorage.o(i.clear_post_processing_run))
  [Stack]

  - Max Depth = 120
  - Call Chain = clear_post_processing_run ⇒ store_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> store_operation_execute
  - >> command_end_procedure_run
  [Called By]
  - >> swap_sub_sm_exit_action_run
  - >> erase_sub_state_sm_run

  cmd_process (Thumb, 64 bytes, Stack size 8 bytes, pstorage.o(i.cmd_process))
  [Stack]

  - Max Depth = 160
  - Call Chain = cmd_process ⇒ update_operation_execute ⇒ clear_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> update_operation_execute
  - >> store_operation_execute
  - >> clear_operation_execute
  [Called By]
  - >> cmd_queue_enqueue
  - >> cmd_queue_dequeue

  cmd_queue_dequeue (Thumb, 14 bytes, Stack size 8 bytes, pstorage.o(i.cmd_queue_dequeue))
  [Stack]

  - Max Depth = 8 + In Cycle
  - Call Chain = cmd_queue_dequeue ⇒ cmd_process (Cycle)
  [Calls]
  - >> cmd_process
  [Called By]
  - >> state_idle_entry_run

  cmd_queue_element_init (Thumb, 76 bytes, Stack size 0 bytes, pstorage.o(i.cmd_queue_element_init))
  [Called By]

  - >> command_queue_element_consume
  - >> cmd_queue_init

  cmd_queue_enqueue (Thumb, 148 bytes, Stack size 32 bytes, pstorage.o(i.cmd_queue_enqueue))
  [Stack]

  - Max Depth = 192
  - Call Chain = cmd_queue_enqueue ⇒ cmd_process ⇒ update_operation_execute ⇒ clear_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> cmd_process
  [Called By]
  - >> pstorage_update
  - >> pstorage_store
  - >> pstorage_clear

  cmd_queue_init (Thumb, 28 bytes, Stack size 8 bytes, pstorage.o(i.cmd_queue_init))
  [Stack]

  - Max Depth = 8
  - Call Chain = cmd_queue_init
  [Calls]
  - >> cmd_queue_element_init
  [Called By]
  - >> pstorage_init

  command_end_procedure_run (Thumb, 36 bytes, Stack size 8 bytes, pstorage.o(i.command_end_procedure_run))
  [Stack]

  - Max Depth = 112
  - Call Chain = command_end_procedure_run ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> sm_state_change
  - >> command_queue_element_consume
  - >> app_notify
  [Called By]
  - >> store_sub_state_sm_run
  - >> clear_post_processing_run

  command_queue_element_consume (Thumb, 40 bytes, Stack size 8 bytes, pstorage.o(i.command_queue_element_consume))
  [Stack]

  - Max Depth = 8
  - Call Chain = command_queue_element_consume
  [Calls]
  - >> cmd_queue_element_init
  [Called By]
  - >> command_end_procedure_run

  data_page_erase_state_run (Thumb, 106 bytes, Stack size 8 bytes, pstorage.o(i.data_page_erase_state_run))
  [Stack]

  - Max Depth = 136
  - Call Chain = data_page_erase_state_run ⇒ swap_sub_sm_exit_action_run ⇒ clear_post_processing_run ⇒ store_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> swap_sub_state_state_change
  - >> swap_sub_state_err_busy_process
  - >> swap_sub_sm_exit_action_run
  - >> is_page_erase_required
  [Address Reference Count : 1]
  - pstorage.o(.constdata)

  data_to_swap_write_state_run (Thumb, 48 bytes, Stack size 8 bytes, pstorage.o(i.data_to_swap_write_state_run))
  [Stack]

  - Max Depth = 32
  - Call Chain = data_to_swap_write_state_run ⇒ swap_sub_state_err_busy_process ⇒ swap_sub_state_state_change ⇒ swap_sub_state_entry_action_run
  [Calls]
  - >> swap_sub_state_state_change
  - >> swap_sub_state_err_busy_process
  [Address Reference Count : 1]
  - pstorage.o(.constdata)

  erase_sub_state_sm_run (Thumb, 50 bytes, Stack size 8 bytes, pstorage.o(i.erase_sub_state_sm_run))
  [Stack]

  - Max Depth = 128
  - Call Chain = erase_sub_state_sm_run ⇒ clear_post_processing_run ⇒ store_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> sm_state_change
  - >> main_state_err_busy_process
  - >> is_page_erase_required
  - >> clear_post_processing_run
  [Called By]
  - >> flash_operation_success_run

  flash_api_err_code_process (Thumb, 40 bytes, Stack size 8 bytes, pstorage.o(i.flash_api_err_code_process))
  [Stack]

  - Max Depth = 40
  - Call Chain = flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> app_notify_error_state_transit
  [Called By]
  - >> flash_write
  - >> flash_page_erase

  flash_operation_failure_run (Thumb, 54 bytes, Stack size 8 bytes, pstorage.o(i.flash_operation_failure_run))
  [Stack]

  - Max Depth = 112
  - Call Chain = flash_operation_failure_run ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> swap_sub_state_state_change
  - >> sm_state_change
  - >> app_notify_error_state_transit
  [Called By]
  - >> pstorage_sys_event_handler

  flash_operation_success_run (Thumb, 44 bytes, Stack size 8 bytes, pstorage.o(i.flash_operation_success_run))
  [Stack]

  - Max Depth = 136
  - Call Chain = flash_operation_success_run ⇒ erase_sub_state_sm_run ⇒ clear_post_processing_run ⇒ store_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> swap_sub_state_sm_run
  - >> store_sub_state_sm_run
  - >> erase_sub_state_sm_run
  [Called By]
  - >> pstorage_sys_event_handler

  flash_page_erase (Thumb, 16 bytes, Stack size 16 bytes, pstorage.o(i.flash_page_erase))
  [Stack]

  - Max Depth = 56
  - Call Chain = flash_page_erase ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> flash_api_err_code_process
  [Called By]
  - >> state_swap_erase_entry_run
  - >> state_erase_data_page_entry_run
  - >> state_data_erase_entry_run

  flash_write (Thumb, 28 bytes, Stack size 24 bytes, pstorage.o(i.flash_write))
  [Stack]

  - Max Depth = 64
  - Call Chain = flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> flash_api_err_code_process
  [Called By]
  - >> store_cmd_flash_write_execute
  - >> state_write_data_swap_entry_run
  - >> state_restore_tail_entry_run
  - >> state_restore_head_entry_run

  head_restore_state_run (Thumb, 90 bytes, Stack size 8 bytes, pstorage.o(i.head_restore_state_run))
  [Stack]

  - Max Depth = 136
  - Call Chain = head_restore_state_run ⇒ swap_sub_sm_exit_action_run ⇒ clear_post_processing_run ⇒ store_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> swap_sub_state_state_change
  - >> swap_sub_state_err_busy_process
  - >> swap_sub_sm_exit_action_run
  - >> is_tail_data_page_swap_required
  - >> is_page_erase_required
  [Address Reference Count : 1]
  - pstorage.o(.constdata)

  is_page_erase_required (Thumb, 74 bytes, Stack size 24 bytes, pstorage.o(i.is_page_erase_required))
  [Stack]

  - Max Depth = 24
  - Call Chain = is_page_erase_required
  [Calls]
  - >> pstorage_flash_page_size
  [Called By]
  - >> head_restore_state_run
  - >> erase_sub_state_sm_run
  - >> data_page_erase_state_run

  is_tail_data_page_swap_required (Thumb, 66 bytes, Stack size 24 bytes, pstorage.o(i.is_tail_data_page_swap_required))
  [Stack]

  - Max Depth = 24
  - Call Chain = is_tail_data_page_swap_required
  [Calls]
  - >> pstorage_flash_page_size
  [Called By]
  - >> head_restore_state_run

  is_word_aligned (Thumb, 16 bytes, Stack size 0 bytes, pstorage.o(i.is_word_aligned))
  [Called By]

  - >> pstorage_update
  - >> pstorage_store
  - >> pstorage_load
  - >> pstorage_clear

  main_state_err_busy_process (Thumb, 24 bytes, Stack size 8 bytes, pstorage.o(i.main_state_err_busy_process))
  [Stack]

  - Max Depth = 112
  - Call Chain = main_state_err_busy_process ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> sm_state_change
  [Called By]
  - >> store_sub_state_sm_run
  - >> erase_sub_state_sm_run

  pstorage_flash_page_end (Thumb, 30 bytes, Stack size 8 bytes, pstorage.o(i.pstorage_flash_page_end))
  [Stack]

  - Max Depth = 8
  - Call Chain = pstorage_flash_page_end
  [Calls]
  - >> pstorage_flash_page_size
  [Called By]
  - >> pstorage_init
  - >> pstorage_register
  - >> state_write_data_swap_entry_run
  - >> state_swap_erase_entry_run
  - >> state_restore_tail_entry_run
  - >> state_restore_head_entry_run

  pstorage_flash_page_size (Thumb, 10 bytes, Stack size 0 bytes, pstorage.o(i.pstorage_flash_page_size))
  [Called By]

  - >> pstorage_init
  - >> pstorage_register
  - >> tail_word_size_calculate
  - >> store_cmd_flash_write_execute
  - >> state_write_data_swap_entry_run
  - >> state_swap_erase_entry_run
  - >> state_restore_tail_entry_run
  - >> state_restore_head_entry_run
  - >> state_data_erase_swap_entry_run
  - >> pstorage_flash_page_end
  - >> is_tail_data_page_swap_required
  - >> is_page_erase_required
  - >> clear_operation_execute

  sm_state_change (Thumb, 14 bytes, Stack size 8 bytes, pstorage.o(i.sm_state_change))
  [Stack]

  - Max Depth = 104
  - Call Chain = sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> state_entry_action_run
  [Called By]
  - >> store_operation_execute
  - >> main_state_err_busy_process
  - >> flash_operation_failure_run
  - >> erase_sub_state_sm_run
  - >> command_end_procedure_run
  - >> clear_operation_execute
  - >> app_notify_error_state_transit

  state_data_erase_entry_run (Thumb, 12 bytes, Stack size 8 bytes, pstorage.o(i.state_data_erase_entry_run))
  [Stack]

  - Max Depth = 64
  - Call Chain = state_data_erase_entry_run ⇒ flash_page_erase ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> flash_page_erase
  [Called By]
  - >> state_entry_action_run

  state_data_erase_swap_entry_run (Thumb, 124 bytes, Stack size 24 bytes, pstorage.o(i.state_data_erase_swap_entry_run))
  [Stack]

  - Max Depth = 40
  - Call Chain = state_data_erase_swap_entry_run ⇒ swap_sub_state_state_change ⇒ swap_sub_state_entry_action_run
  [Calls]
  - >> swap_sub_state_state_change
  - >> pstorage_flash_page_size
  [Called By]
  - >> state_entry_action_run

  state_entry_action_run (Thumb, 52 bytes, Stack size 8 bytes, pstorage.o(i.state_entry_action_run))
  [Stack]

  - Max Depth = 96
  - Call Chain = state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> state_store_entry_run
  - >> state_idle_entry_run
  - >> state_data_erase_swap_entry_run
  - >> state_data_erase_entry_run
  [Called By]
  - >> sm_state_change

  state_erase_data_page_entry_run (Thumb, 12 bytes, Stack size 8 bytes, pstorage.o(i.state_erase_data_page_entry_run))
  [Stack]

  - Max Depth = 64
  - Call Chain = state_erase_data_page_entry_run ⇒ flash_page_erase ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> flash_page_erase
  [Address Reference Count : 1]
  - pstorage.o(.constdata)

  state_idle_entry_run (Thumb, 18 bytes, Stack size 8 bytes, pstorage.o(i.state_idle_entry_run))
  [Stack]

  - Max Depth = 16
  - Call Chain = state_idle_entry_run ⇒ cmd_queue_dequeue ⇒ cmd_process (Cycle)
  [Calls]
  - >> cmd_queue_dequeue
  [Called By]
  - >> state_entry_action_run

  state_restore_head_entry_run (Thumb, 44 bytes, Stack size 16 bytes, pstorage.o(i.state_restore_head_entry_run))
  [Stack]

  - Max Depth = 80
  - Call Chain = state_restore_head_entry_run ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> pstorage_flash_page_size
  - >> pstorage_flash_page_end
  - >> flash_write
  [Address Reference Count : 1]
  - pstorage.o(.constdata)

  state_restore_tail_entry_run (Thumb, 80 bytes, Stack size 24 bytes, pstorage.o(i.state_restore_tail_entry_run))
  [Stack]

  - Max Depth = 88
  - Call Chain = state_restore_tail_entry_run ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> pstorage_flash_page_size
  - >> pstorage_flash_page_end
  - >> flash_write
  [Address Reference Count : 1]
  - pstorage.o(.constdata)

  state_store_entry_run (Thumb, 8 bytes, Stack size 8 bytes, pstorage.o(i.state_store_entry_run))
  [Stack]

  - Max Depth = 88
  - Call Chain = state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> store_cmd_flash_write_execute
  [Called By]
  - >> state_entry_action_run

  state_swap_erase_entry_run (Thumb, 30 bytes, Stack size 16 bytes, pstorage.o(i.state_swap_erase_entry_run))
  [Stack]

  - Max Depth = 72
  - Call Chain = state_swap_erase_entry_run ⇒ flash_page_erase ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> pstorage_flash_page_size
  - >> pstorage_flash_page_end
  - >> flash_page_erase
  [Address Reference Count : 1]
  - pstorage.o(.constdata)

  state_write_data_swap_entry_run (Thumb, 50 bytes, Stack size 24 bytes, pstorage.o(i.state_write_data_swap_entry_run))
  [Stack]

  - Max Depth = 88
  - Call Chain = state_write_data_swap_entry_run ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> pstorage_flash_page_size
  - >> pstorage_flash_page_end
  - >> flash_write
  [Address Reference Count : 1]
  - pstorage.o(.constdata)

  store_cmd_flash_write_execute (Thumb, 94 bytes, Stack size 16 bytes, pstorage.o(i.store_cmd_flash_write_execute))
  [Stack]

  - Max Depth = 80
  - Call Chain = store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> pstorage_flash_page_size
  - >> flash_write
  [Called By]
  - >> store_sub_state_sm_run
  - >> state_store_entry_run

  store_operation_execute (Thumb, 10 bytes, Stack size 8 bytes, pstorage.o(i.store_operation_execute))
  [Stack]

  - Max Depth = 112
  - Call Chain = store_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> sm_state_change
  [Called By]
  - >> cmd_process
  - >> clear_post_processing_run

  store_sub_state_sm_run (Thumb, 60 bytes, Stack size 8 bytes, pstorage.o(i.store_sub_state_sm_run))
  [Stack]

  - Max Depth = 120
  - Call Chain = store_sub_state_sm_run ⇒ main_state_err_busy_process ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> store_cmd_flash_write_execute
  - >> main_state_err_busy_process
  - >> command_end_procedure_run
  [Called By]
  - >> flash_operation_success_run

  swap_erase_state_run (Thumb, 26 bytes, Stack size 8 bytes, pstorage.o(i.swap_erase_state_run))
  [Stack]

  - Max Depth = 32
  - Call Chain = swap_erase_state_run ⇒ swap_sub_state_err_busy_process ⇒ swap_sub_state_state_change ⇒ swap_sub_state_entry_action_run
  [Calls]
  - >> swap_sub_state_state_change
  - >> swap_sub_state_err_busy_process
  [Address Reference Count : 1]
  - pstorage.o(.constdata)

  swap_sub_sm_exit_action_run (Thumb, 8 bytes, Stack size 8 bytes, pstorage.o(i.swap_sub_sm_exit_action_run))
  [Stack]

  - Max Depth = 128
  - Call Chain = swap_sub_sm_exit_action_run ⇒ clear_post_processing_run ⇒ store_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> clear_post_processing_run
  [Called By]
  - >> tail_restore_state_run
  - >> head_restore_state_run
  - >> data_page_erase_state_run

  swap_sub_state_entry_action_run (Thumb, 16 bytes, Stack size 8 bytes, pstorage.o(i.swap_sub_state_entry_action_run))
  [Stack]

  - Max Depth = 8
  - Call Chain = swap_sub_state_entry_action_run
  [Called By]
  - >> swap_sub_state_state_change

  swap_sub_state_err_busy_process (Thumb, 24 bytes, Stack size 8 bytes, pstorage.o(i.swap_sub_state_err_busy_process))
  [Stack]

  - Max Depth = 24
  - Call Chain = swap_sub_state_err_busy_process ⇒ swap_sub_state_state_change ⇒ swap_sub_state_entry_action_run
  [Calls]
  - >> swap_sub_state_state_change
  [Called By]
  - >> tail_restore_state_run
  - >> swap_erase_state_run
  - >> head_restore_state_run
  - >> data_to_swap_write_state_run
  - >> data_page_erase_state_run

  swap_sub_state_sm_run (Thumb, 16 bytes, Stack size 8 bytes, pstorage.o(i.swap_sub_state_sm_run))
  [Stack]

  - Max Depth = 8
  - Call Chain = swap_sub_state_sm_run
  [Called By]
  - >> flash_operation_success_run

  swap_sub_state_state_change (Thumb, 14 bytes, Stack size 8 bytes, pstorage.o(i.swap_sub_state_state_change))
  [Stack]

  - Max Depth = 16
  - Call Chain = swap_sub_state_state_change ⇒ swap_sub_state_entry_action_run
  [Calls]
  - >> swap_sub_state_entry_action_run
  [Called By]
  - >> swap_sub_state_err_busy_process
  - >> swap_erase_state_run
  - >> state_data_erase_swap_entry_run
  - >> head_restore_state_run
  - >> flash_operation_failure_run
  - >> data_to_swap_write_state_run
  - >> data_page_erase_state_run

  tail_restore_state_run (Thumb, 24 bytes, Stack size 8 bytes, pstorage.o(i.tail_restore_state_run))
  [Stack]

  - Max Depth = 136
  - Call Chain = tail_restore_state_run ⇒ swap_sub_sm_exit_action_run ⇒ clear_post_processing_run ⇒ store_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> swap_sub_state_err_busy_process
  - >> swap_sub_sm_exit_action_run
  [Address Reference Count : 1]
  - pstorage.o(.constdata)

  tail_word_size_calculate (Thumb, 70 bytes, Stack size 24 bytes, pstorage.o(i.tail_word_size_calculate))
  [Stack]

  - Max Depth = 24
  - Call Chain = tail_word_size_calculate
  [Calls]
  - >> pstorage_flash_page_size
  [Called By]
  - >> clear_operation_execute

  update_operation_execute (Thumb, 8 bytes, Stack size 8 bytes, pstorage.o(i.update_operation_execute))
  [Stack]

  - Max Depth = 152
  - Call Chain = update_operation_execute ⇒ clear_operation_execute ⇒ sm_state_change ⇒ state_entry_action_run ⇒ state_store_entry_run ⇒ store_cmd_flash_write_execute ⇒ flash_write ⇒ flash_api_err_code_process ⇒ app_notify_error_state_transit ⇒ sm_state_change (Cycle)
  [Calls]
  - >> clear_operation_execute
  [Called By]
  - >> cmd_process

  irq_handler_twi (Thumb, 218 bytes, Stack size 32 bytes, nrf_drv_twi.o(i.irq_handler_twi))
  [Stack]

  - Max Depth = 136
  - Call Chain = irq_handler_twi ⇒ twi_tx_start_transfer ⇒ twi_transfer ⇒ twi_send_byte
  [Calls]
  - >> twi_tx_start_transfer
  - >> twi_transfer
  - >> twi_rx_start_transfer
  [Called By]
  - >> SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler

  nrf_drv_get_IRQn (Thumb, 10 bytes, Stack size 0 bytes, nrf_drv_twi.o(i.nrf_drv_get_IRQn))
  [Called By]

  - >> nrf_drv_twi_init

  nrf_gpio_pin_clear (Thumb, 10 bytes, Stack size 0 bytes, nrf_drv_twi.o(i.nrf_gpio_pin_clear))
  [Called By]

  - >> twi_clear_bus

  nrf_gpio_pin_set (Thumb, 10 bytes, Stack size 0 bytes, nrf_drv_twi.o(i.nrf_gpio_pin_set))
  [Called By]

  - >> twi_clear_bus

  nrf_twi_event_check (Thumb, 14 bytes, Stack size 0 bytes, nrf_drv_twi.o(i.nrf_twi_event_check))
  [Called By]

  - >> twi_transfer

  nrf_twi_event_clear (Thumb, 6 bytes, Stack size 0 bytes, nrf_drv_twi.o(i.nrf_twi_event_clear))
  [Called By]

  - >> twi_tx_start_transfer
  - >> twi_transfer
  - >> twi_rx_start_transfer

  nrf_twi_int_disable (Thumb, 6 bytes, Stack size 0 bytes, nrf_drv_twi.o(i.nrf_twi_int_disable))
  [Called By]

  - >> twi_xfer

  nrf_twi_int_enable (Thumb, 6 bytes, Stack size 0 bytes, nrf_drv_twi.o(i.nrf_twi_int_enable))
  [Called By]

  - >> twi_xfer
  - >> twi_tx_start_transfer
  - >> twi_rx_start_transfer

  nrf_twi_shorts_set (Thumb, 6 bytes, Stack size 0 bytes, nrf_drv_twi.o(i.nrf_twi_shorts_set))
  [Called By]

  - >> twi_tx_start_transfer
  - >> twi_rx_start_transfer
  - >> twi_receive_byte

  nrf_twi_task_trigger (Thumb, 6 bytes, Stack size 0 bytes, nrf_drv_twi.o(i.nrf_twi_task_trigger))
  [Called By]

  - >> twi_tx_start_transfer
  - >> twi_transfer
  - >> twi_send_byte
  - >> twi_rx_start_transfer
  - >> twi_receive_byte

  twi_clear_bus (Thumb, 138 bytes, Stack size 16 bytes, nrf_drv_twi.o(i.twi_clear_bus))
  [Stack]

  - Max Depth = 16
  - Call Chain = twi_clear_bus
  [Calls]
  - >> __asm___13_nrf_drv_twi_c_a9bcf68d__nrf_delay_us
  - >> nrf_gpio_pin_set
  - >> nrf_gpio_pin_clear
  [Called By]
  - >> nrf_drv_twi_init

  twi_receive_byte (Thumb, 76 bytes, Stack size 24 bytes, nrf_drv_twi.o(i.twi_receive_byte))
  [Stack]

  - Max Depth = 24
  - Call Chain = twi_receive_byte
  [Calls]
  - >> nrf_twi_task_trigger
  - >> nrf_twi_shorts_set
  [Called By]
  - >> twi_transfer

  twi_rx_start_transfer (Thumb, 166 bytes, Stack size 32 bytes, nrf_drv_twi.o(i.twi_rx_start_transfer))
  [Stack]

  - Max Depth = 96
  - Call Chain = twi_rx_start_transfer ⇒ twi_transfer ⇒ twi_send_byte
  [Calls]
  - >> twi_transfer
  - >> nrf_twi_task_trigger
  - >> nrf_twi_shorts_set
  - >> nrf_twi_int_enable
  - >> nrf_twi_event_clear
  [Called By]
  - >> irq_handler_twi
  - >> twi_xfer

  twi_send_byte (Thumb, 72 bytes, Stack size 24 bytes, nrf_drv_twi.o(i.twi_send_byte))
  [Stack]

  - Max Depth = 24
  - Call Chain = twi_send_byte
  [Calls]
  - >> nrf_twi_task_trigger
  [Called By]
  - >> twi_tx_start_transfer
  - >> twi_transfer

  twi_transfer (Thumb, 290 bytes, Stack size 40 bytes, nrf_drv_twi.o(i.twi_transfer))
  [Stack]

  - Max Depth = 64
  - Call Chain = twi_transfer ⇒ twi_send_byte
  [Calls]
  - >> twi_send_byte
  - >> twi_receive_byte
  - >> nrf_twi_task_trigger
  - >> nrf_twi_event_clear
  - >> nrf_twi_event_check
  [Called By]
  - >> irq_handler_twi
  - >> twi_tx_start_transfer
  - >> twi_rx_start_transfer

  twi_tx_start_transfer (Thumb, 172 bytes, Stack size 40 bytes, nrf_drv_twi.o(i.twi_tx_start_transfer))
  [Stack]

  - Max Depth = 104
  - Call Chain = twi_tx_start_transfer ⇒ twi_transfer ⇒ twi_send_byte
  [Calls]
  - >> twi_transfer
  - >> twi_send_byte
  - >> nrf_twi_task_trigger
  - >> nrf_twi_shorts_set
  - >> nrf_twi_int_enable
  - >> nrf_twi_event_clear
  [Called By]
  - >> irq_handler_twi
  - >> twi_xfer

  twi_xfer (Thumb, 184 bytes, Stack size 32 bytes, nrf_drv_twi.o(i.twi_xfer))
  [Stack]

  - Max Depth = 136
  - Call Chain = twi_xfer ⇒ twi_tx_start_transfer ⇒ twi_transfer ⇒ twi_send_byte
  [Calls]
  - >> twi_tx_start_transfer
  - >> twi_rx_start_transfer
  - >> nrf_twi_int_enable
  - >> nrf_twi_int_disable
  [Called By]
  - >> nrf_drv_twi_xfer

  NVIC_ClearPendingIRQ (Thumb, 18 bytes, Stack size 0 bytes, app_timer.o(i.NVIC_ClearPendingIRQ))
  [Called By]

  - >> app_timer_init
  - >> rtc1_start

  NVIC_EnableIRQ (Thumb, 22 bytes, Stack size 0 bytes, app_timer.o(i.NVIC_EnableIRQ))
  [Called By]

  - >> app_timer_init
  - >> rtc1_start

  NVIC_SetPendingIRQ (Thumb, 18 bytes, Stack size 0 bytes, app_timer.o(i.NVIC_SetPendingIRQ))
  [Called By]

  - >> timer_timeouts_check_sched
  - >> timer_list_handler_sched

  NVIC_SetPriority (Thumb, 32 bytes, Stack size 8 bytes, app_timer.o(i.NVIC_SetPriority))
  [Stack]

  - Max Depth = 8
  - Call Chain = NVIC_SetPriority
  [Called By]
  - >> app_timer_init
  - >> rtc1_init

  compare_reg_update (Thumb, 132 bytes, Stack size 32 bytes, app_timer.o(i.compare_reg_update))
  [Stack]

  - Max Depth = 40
  - Call Chain = compare_reg_update ⇒ timer_timeouts_check_sched
  [Calls]
  - >> __asm___11_app_timer_c_cd27f9c3__nrf_delay_us
  - >> timer_timeouts_check_sched
  - >> ticks_diff_get
  - >> rtc1_stop
  - >> rtc1_start
  - >> rtc1_counter_get
  - >> rtc1_compare0_set
  [Called By]
  - >> timer_list_handler

  elapsed_ticks_acquire (Thumb, 82 bytes, Stack size 0 bytes, app_timer.o(i.elapsed_ticks_acquire))
  [Called By]

  - >> timer_list_handler

  expired_timers_handler (Thumb, 84 bytes, Stack size 20 bytes, app_timer.o(i.expired_timers_handler))
  [Stack]

  - Max Depth = 20
  - Call Chain = expired_timers_handler
  [Called By]
  - >> timer_list_handler

  list_deletions_handler (Thumb, 140 bytes, Stack size 24 bytes, app_timer.o(i.list_deletions_handler))
  [Stack]

  - Max Depth = 36
  - Call Chain = list_deletions_handler ⇒ timer_list_remove
  [Calls]
  - >> timer_list_remove
  [Called By]
  - >> timer_list_handler

  list_insertions_handler (Thumb, 242 bytes, Stack size 32 bytes, app_timer.o(i.list_insertions_handler))
  [Stack]

  - Max Depth = 40
  - Call Chain = list_insertions_handler ⇒ timer_list_insert
  [Calls]
  - >> timer_list_insert
  - >> ticks_diff_get
  [Called By]
  - >> timer_list_handler

  rtc1_compare0_set (Thumb, 6 bytes, Stack size 0 bytes, app_timer.o(i.rtc1_compare0_set))
  [Called By]

  - >> compare_reg_update

  rtc1_counter_get (Thumb, 6 bytes, Stack size 0 bytes, app_timer.o(i.rtc1_counter_get))
  [Called By]

  - >> app_timer_init
  - >> timer_timeouts_check
  - >> timer_start_op_schedule
  - >> compare_reg_update

  rtc1_init (Thumb, 18 bytes, Stack size 8 bytes, app_timer.o(i.rtc1_init))
  [Stack]

  - Max Depth = 16
  - Call Chain = rtc1_init ⇒ NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> app_timer_init

  rtc1_start (Thumb, 48 bytes, Stack size 8 bytes, app_timer.o(i.rtc1_start))
  [Stack]

  - Max Depth = 8
  - Call Chain = rtc1_start
  [Calls]
  - >> __asm___11_app_timer_c_cd27f9c3__nrf_delay_us
  - >> NVIC_EnableIRQ
  - >> NVIC_ClearPendingIRQ
  [Called By]
  - >> compare_reg_update

  rtc1_stop (Thumb, 68 bytes, Stack size 8 bytes, app_timer.o(i.rtc1_stop))
  [Stack]

  - Max Depth = 8
  - Call Chain = rtc1_stop
  [Calls]
  - >> __asm___11_app_timer_c_cd27f9c3__nrf_delay_us
  [Called By]
  - >> app_timer_init
  - >> compare_reg_update

  ticks_diff_get (Thumb, 10 bytes, Stack size 0 bytes, app_timer.o(i.ticks_diff_get))
  [Called By]

  - >> timer_timeouts_check
  - >> list_insertions_handler
  - >> compare_reg_update

  timeout_handler_exec (Thumb, 56 bytes, Stack size 16 bytes, app_timer.o(i.timeout_handler_exec))
  [Stack]

  - Max Depth = 76
  - Call Chain = timeout_handler_exec ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> app_error_handler
  [Called By]
  - >> timer_timeouts_check

  timer_list_handler (Thumb, 72 bytes, Stack size 32 bytes, app_timer.o(i.timer_list_handler))
  [Stack]

  - Max Depth = 72
  - Call Chain = timer_list_handler ⇒ list_insertions_handler ⇒ timer_list_insert
  [Calls]
  - >> list_insertions_handler
  - >> list_deletions_handler
  - >> expired_timers_handler
  - >> elapsed_ticks_acquire
  - >> compare_reg_update
  [Called By]
  - >> SWI0_EGU0_IRQHandler

  timer_list_handler_sched (Thumb, 10 bytes, Stack size 8 bytes, app_timer.o(i.timer_list_handler_sched))
  [Stack]

  - Max Depth = 8
  - Call Chain = timer_list_handler_sched
  [Calls]
  - >> NVIC_SetPendingIRQ
  [Called By]
  - >> timer_timeouts_check
  - >> timer_stop_op_schedule
  - >> timer_start_op_schedule

  timer_list_insert (Thumb, 98 bytes, Stack size 8 bytes, app_timer.o(i.timer_list_insert))
  [Stack]

  - Max Depth = 8
  - Call Chain = timer_list_insert
  [Called By]
  - >> list_insertions_handler

  timer_list_remove (Thumb, 90 bytes, Stack size 12 bytes, app_timer.o(i.timer_list_remove))
  [Stack]

  - Max Depth = 12
  - Call Chain = timer_list_remove
  [Called By]
  - >> list_deletions_handler

  timer_start_op_schedule (Thumb, 86 bytes, Stack size 32 bytes, app_timer.o(i.timer_start_op_schedule))
  [Stack]

  - Max Depth = 44
  - Call Chain = timer_start_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> user_op_enque
  - >> user_op_alloc
  - >> timer_list_handler_sched
  - >> rtc1_counter_get
  [Called By]
  - >> app_timer_start

  timer_stop_op_schedule (Thumb, 58 bytes, Stack size 24 bytes, app_timer.o(i.timer_stop_op_schedule))
  [Stack]

  - Max Depth = 36
  - Call Chain = timer_stop_op_schedule ⇒ user_op_alloc
  [Calls]
  - >> user_op_enque
  - >> user_op_alloc
  - >> timer_list_handler_sched
  [Called By]
  - >> app_timer_stop

  timer_timeouts_check (Thumb, 130 bytes, Stack size 24 bytes, app_timer.o(i.timer_timeouts_check))
  [Stack]

  - Max Depth = 100
  - Call Chain = timer_timeouts_check ⇒ timeout_handler_exec ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ app_error_save_and_stop
  [Calls]
  - >> timer_list_handler_sched
  - >> timeout_handler_exec
  - >> ticks_diff_get
  - >> rtc1_counter_get
  [Called By]
  - >> RTC1_IRQHandler

  timer_timeouts_check_sched (Thumb, 10 bytes, Stack size 8 bytes, app_timer.o(i.timer_timeouts_check_sched))
  [Stack]

  - Max Depth = 8
  - Call Chain = timer_timeouts_check_sched
  [Calls]
  - >> NVIC_SetPendingIRQ
  [Called By]
  - >> compare_reg_update

  user_id_get (Thumb, 78 bytes, Stack size 12 bytes, app_timer.o(i.user_id_get))
  [Stack]

  - Max Depth = 12
  - Call Chain = user_id_get
  [Called By]
  - >> app_timer_stop
  - >> app_timer_start

  user_op_alloc (Thumb, 48 bytes, Stack size 12 bytes, app_timer.o(i.user_op_alloc))
  [Stack]

  - Max Depth = 12
  - Call Chain = user_op_alloc
  [Called By]
  - >> timer_stop_op_schedule
  - >> timer_start_op_schedule

  user_op_enque (Thumb, 4 bytes, Stack size 0 bytes, app_timer.o(i.user_op_enque))
  [Called By]

  - >> timer_stop_op_schedule
  - >> timer_start_op_schedule

  fifo_get (Thumb, 24 bytes, Stack size 16 bytes, app_fifo.o(i.fifo_get))
  [Stack]

  - Max Depth = 24
  - Call Chain = fifo_get ⇒ fifo_peek
  [Calls]
  - >> fifo_peek
  [Called By]
  - >> app_fifo_get

  fifo_length (Thumb, 10 bytes, Stack size 0 bytes, app_fifo.o(i.fifo_length))
  [Called By]

  - >> app_fifo_put
  - >> app_fifo_get

  fifo_peek (Thumb, 18 bytes, Stack size 8 bytes, app_fifo.o(i.fifo_peek))
  [Stack]

  - Max Depth = 8
  - Call Chain = fifo_peek
  [Called By]
  - >> fifo_get

  fifo_put (Thumb, 18 bytes, Stack size 0 bytes, app_fifo.o(i.fifo_put))
  [Called By]

  - >> app_fifo_put

  fifo_length (Thumb, 10 bytes, Stack size 0 bytes, app_uart_fifo.o(i.fifo_length))
  [Called By]

  - >> uart_event_handler

  uart_event_handler (Thumb, 170 bytes, Stack size 24 bytes, app_uart_fifo.o(i.uart_event_handler))
  [Stack]

  - Max Depth = 80
  - Call Chain = uart_event_handler ⇒ nrf_drv_uart_rx ⇒ nrf_drv_uart_rx_for_uart ⇒ rx_enable
  [Calls]
  - >> nrf_drv_uart_tx
  - >> nrf_drv_uart_rx
  - >> app_fifo_put
  - >> app_fifo_get
  - >> fifo_length
  [Address Reference Count : 1]
  - app_uart_fifo.o(i.app_uart_init)

  sd_nvic_EnableIRQ (Thumb, 190 bytes, Stack size 8 bytes, softdevice_handler.o(i.sd_nvic_EnableIRQ))
  [Stack]

  - Max Depth = 8
  - Call Chain = sd_nvic_EnableIRQ
  [Called By]
  - >> softdevice_handler_init

  errata_108 (Thumb, 78 bytes, Stack size 0 bytes, system_nrf52.o(i.errata_108))
  [Called By]

  - >> SystemInit

  errata_12 (Thumb, 78 bytes, Stack size 0 bytes, system_nrf52.o(i.errata_12))
  [Called By]

  - >> SystemInit

  errata_16 (Thumb, 42 bytes, Stack size 0 bytes, system_nrf52.o(i.errata_16))
  [Called By]

  - >> SystemInit

  errata_31 (Thumb, 78 bytes, Stack size 0 bytes, system_nrf52.o(i.errata_31))
  [Called By]

  - >> SystemInit

  errata_32 (Thumb, 42 bytes, Stack size 0 bytes, system_nrf52.o(i.errata_32))
  [Called By]

  - >> SystemInit

  errata_36 (Thumb, 78 bytes, Stack size 0 bytes, system_nrf52.o(i.errata_36))
  [Called By]

  - >> SystemInit

  errata_37 (Thumb, 42 bytes, Stack size 0 bytes, system_nrf52.o(i.errata_37))
  [Called By]

  - >> SystemInit

  errata_57 (Thumb, 42 bytes, Stack size 0 bytes, system_nrf52.o(i.errata_57))
  [Called By]

  - >> SystemInit

  errata_66 (Thumb, 42 bytes, Stack size 0 bytes, system_nrf52.o(i.errata_66))
  [Called By]

  - >> SystemInit

  _printf_core (Thumb, 996 bytes, Stack size 104 bytes, printf8.o(i._printf_core), UNUSED)
  [Calls]

  - >> _printf_pre_padding
  - >> _printf_post_padding
  - >> __aeabi_uldivmod
  [Called By]
  - >> __0printf$8

  _printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printf8.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printf8.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  ### Undefined Global Symbols