nrf/
commit e0d62535662ed6e04730b53f5c7b92fa58cedabf (HEAD -> master, origin/master)
Author: Rubin Gerritsen <rubin.gerritsen@nordicsemi.no>
Date:   Mon Nov 2 15:03:26 2020 +0100

    manifest: SoftDevice Controller with configurable ext. scanning

    See CHANGELOG for additional details.

    Signed-off-by: Rubin Gerritsen <rubin.gerritsen@nordicsemi.no>

zephyr/
commit 105a1b9e2bc48acdd1f1173ad2ef43a90c120fbe (HEAD, tag: v2.4.0-ncs1-rc2, tag: v2.4.0-ncs1, manifest-rev)
Author: Andrzej Głąbek <andrzej.glabek@nordicsemi.no>
Date:   Wed Oct 21 17:51:42 2020 +0200

    [nrf fromlist] modules: hal_nordic: Fix workaround for nRF52 [...]

    anomaly 197 in nrf_power

    Upstream PR: https://github.com/zephyrproject-rtos/zephyr/pull/29409

    Update the hal_nordic module revision to get the following commit:

    nrf_power: Fix implementation of workaround for nRF52 anomaly 197

    Since the workaround increases power consumption in System ON IDLE,
    it should be applied only when the DC/DC converter for REG0 stage is
    to be enabled, not regardless of the applied setting as it was done
    so far.

    Signed-off-by: Andrzej Głąbek <andrzej.glabek@nordicsemi.no>
    (cherry picked from commit 457b290e26d53df9b3be5d74142c15ec636a1764)

