/*
 * Copyright (c) 2019-2020 Nordic Semiconductor ASA
 *
 * SPDX-License-Identifier: Apache-2.0
 */

/*
 * Default Flash planning for nrf5340dk_nrf5340 CPUAPP (Application MCU).
 *
 * Zephyr build for nRF5340 with ARM TrustZone-M support,
 * implies building Secure and Non-Secure Zephyr images.
 *
 * Secure image will be placed, by default, in flash0
 * (or in slot0, if MCUboot is present).
 * Secure image will use sram0 for system memory.
 *
 * Non-Secure image will be placed in slot0_ns, and use
 * sram0_ns for system memory.
 *
 * Note that the Secure image only requires knowledge of
 * the beginning of the Non-Secure image (not its size).
 */

&slot0_partition {
	reg = <0x00010000 0x40000>;
};

&slot0_ns_partition {
	reg = <0x00050000 0x30000>;
};

&slot1_partition {
	reg = <0x00080000 0x40000>;
};

&slot1_ns_partition {
	reg = <0x000c0000 0x30000>;
};

/* Default SRAM planning when building for nRF5340 with
 * ARM TrustZone-M support
 * - Lowest 256 kB SRAM allocated to Secure image (sram0_s)
 * - Middle 192 kB allocated to Non-Secure image (sram0_ns)
 * - Upper 64 kB SRAM allocated as Shared memory (sram0_shared)
 *   (see nrf5340_shared_sram_planning_conf.dtsi)
 */
&sram0_image {
	reg = <0x20000000 DT_SIZE_K(448)>;
};

&sram0_s {
	reg = <0x20000000 0x40000>;
};

&sram0_ns {
	reg = <0x20040000 0x30000>;
};

/* Include shared RAM configuration file */
#include "nrf5340_shared_sram_planning_conf.dtsi"
