ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x15bc1
  Start of program headers:          52 (bytes into file)
  Start of section headers:          5646808 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         7
  Size of section headers:           40 (bytes)
  Number of section headers:         52
  Section header string table index: 51

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        00000000 000120 00047c 00 WAX  0   0  4
  [ 2] text              PROGBITS        00000480 0005a0 034518 00  AX  0   0  8
  [ 3] .ARM.exidx        ARM_EXIDX       00034998 034ab8 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        000349a0 034ac0 0000d8 00   A  0   0  4
  [ 5] device_area       PROGBITS        00034a78 034b98 0000dc 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        00034b54 034c74 000878 00  WA  0   0  4
  [ 7] _static_thre[...] PROGBITS        000353d0 0354f0 000030 00  WA  0   0  8
  [ 8] entropy_driv[...] PROGBITS        00035400 035520 000010 00   A  0   0  4
  [ 9] flash_driver[...] PROGBITS        00035410 035530 000030 00   A  0   0  4
  [10] gpio_driver_[...] PROGBITS        00035440 035560 000024 00   A  0   0  4
  [11] spi_driver_a[...] PROGBITS        00035464 035584 000008 00   A  0   0  4
  [12] clock_contro[...] PROGBITS        0003546c 03558c 00001c 00   A  0   0  4
  [13] uart_driver_[...] PROGBITS        00035488 0355a8 000024 00   A  0   0  4
  [14] bt_l2cap_fix[...] PROGBITS        000354ac 0355cc 000024 00   A  0   0  4
  [15] bt_conn_cb_area   PROGBITS        000354d0 0355f0 000020 00   A  0   0  4
  [16] bt_gatt_serv[...] PROGBITS        000354f0 035610 000018 00   A  0   0  4
  [17] log_const_area    PROGBITS        00035508 035628 000148 00   A  0   0  4
  [18] log_backend_area  PROGBITS        00035650 035770 000020 00   A  0   0  4
  [19] settings_han[...] PROGBITS        00035670 035790 000090 00   A  0   0  4
  [20] tbss              NOBITS          00035700 035820 000008 00 WAT  0   0  4
  [21] rodata            PROGBITS        00035700 035820 009434 00   A  0   0 16
  [22] NRF_KMU_RESE[...] NOBITS          20000000 03faa0 000040 00  WA  0   0  1
  [23] _RTT_SECTION_NAME NOBITS          20000040 03faa0 0004b8 00  WA  0   0  4
  [24] .ramfunc          NOBITS          200004f8 03ec54 000008 00  WA  0   0  1
  [25] datas             PROGBITS        20000500 03ec58 000a0f 00  WA  0   0  8
  [26] device_states     PROGBITS        20000f0f 03f667 000016 00  WA  0   0  1
  [27] log_mpsc_pbu[...] PROGBITS        20000f28 03f680 000044 00  WA  0   0  4
  [28] log_msg_ptr_area  PROGBITS        20000f6c 03f6c4 000004 00  WA  0   0  4
  [29] k_mem_slab_area   PROGBITS        20000f70 03f6c8 000060 00  WA  0   0  4
  [30] k_heap_area       PROGBITS        20000fd0 03f728 000018 00  WA  0   0  4
  [31] k_mutex_area      PROGBITS        20000fe8 03f740 0000c8 00  WA  0   0  4
  [32] k_sem_area        PROGBITS        200010b0 03f808 000048 00  WA  0   0  4
  [33] k_event_area      PROGBITS        200010f8 03f850 000020 00  WA  0   0  4
  [34] k_fifo_area       PROGBITS        20001118 03f870 000054 00  WA  0   0  4
  [35] net_buf_pool_area PROGBITS        2000116c 03f8c4 0001d4 00  WA  0   0  4
  [36] .comment          PROGBITS        00000000 03fa9c 000020 01  MS  0   0  1
  [37] .debug_aranges    PROGBITS        00000000 03fac0 0055a8 00      0   0  8
  [38] .debug_info       PROGBITS        00000000 045068 30f1c5 00      0   0  1
  [39] .debug_abbrev     PROGBITS        00000000 35422d 02ba8e 00      0   0  1
  [40] .debug_line       PROGBITS        00000000 37fcbb 098307 00      0   0  1
  [41] .debug_frame      PROGBITS        00000000 417fc4 00fc44 00      0   0  4
  [42] .debug_str        PROGBITS        00000000 427c08 02e65e 01  MS  0   0  1
  [43] .debug_loc        PROGBITS        00000000 456266 0b036e 00      0   0  1
  [44] .debug_ranges     PROGBITS        00000000 5065d8 0199a0 00      0   0  8
  [45] .ARM.attributes   ARM_ATTRIBUTES  00000000 51ff78 000038 00      0   0  1
  [46] .last_section     PROGBITS        0003f97c 03fa98 000004 00  WA  0   0  4
  [47] bss               NOBITS          20001340 03faa0 003f23 00  WA  0   0  8
  [48] noinit            NOBITS          20005268 03faa0 0093e4 00  WA  0   0  8
  [49] .symtab           SYMTAB          00000000 51ffb0 025e90 10     50 6713  4
  [50] .strtab           STRTAB          00000000 545e40 01c8ab 00      0   0  1
  [51] .shstrtab         STRTAB          00000000 5626eb 0002ed 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  D (mbind), y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x034ab8 0x00034998 0x00034998 0x00008 0x00008 R   0x4
  LOAD           0x000120 0x00000000 0x00000000 0x3eb34 0x3eb34 RWE 0x10
  LOAD           0x000000 0x200004f8 0x0003eb34 0x00000 0x00008 RW  0x1
  LOAD           0x03ec58 0x20000500 0x0003eb3c 0x00e40 0x00e40 RW  0x8
  LOAD           0x03fa98 0x0003f97c 0x0003f97c 0x00004 0x00004 RW  0x4
  LOAD           0x000000 0x20000000 0x20000000 0x00000 0x0e64c RW  0x8
  TLS            0x035820 0x00035700 0x00035700 0x00000 0x00008 R   0x4

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel device_area sw_isr_table _static_thread_data_area entropy_driver_api_area flash_driver_api_area gpio_driver_api_area spi_driver_api_area clock_control_driver_api_area uart_driver_api_area bt_l2cap_fixed_chan_area bt_conn_cb_area bt_gatt_service_static_area log_const_area log_backend_area settings_handler_static_area rodata 
   02     .ramfunc 
   03     datas device_states log_mpsc_pbuf_area log_msg_ptr_area k_mem_slab_area k_heap_area k_mutex_area k_sem_area k_event_area k_fifo_area net_buf_pool_area 
   04     .last_section 
   05     NRF_KMU_RESERVED_PUSH_SECTION _RTT_SECTION_NAME .ramfunc bss noinit 
   06     tbss 
