# In nRF54L15 we place the TF-M non-secure storage partitions after the
# TF-M non-secure application to avoid splitting the secure/non-secure
# partitions more than necessary.
settings_storage:
  placement:
    after: [app]
    before: [end]
  inside: [nonsecure_storage]
  size: 0x2000
