Advertising interval is 500ms
0 dbm TX output

Current power conusmption using nrf52840dk: average->744 microamps peak->11.69 ma peak current

Current power conusmption using nrf7002dk: average-> peak->