#

##

##

##

##

##

##

    µVision Build Log
    Tool Versions:
    IDE-Version: ¦ÌVision V5.14.0.0
    Copyright (C) 2015 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: Kai Liu, NXP, LIC=FQQGK-ZQ3AN-ZDEK6-DKBSD-6XJR2-QFUL4

    Tool Versions:
    Toolchain:       MDK-ARM Professional  Version: 5.14.0.0
    Toolchain Path:  D:\Keil_v5\ARM\ARMCC\Bin
    C Compiler:      Armcc.exe V5.05 update 1 (build 106)
    Assembler:       Armasm.exe V5.05 update 1 (build 106)
    Linker/Locator:  ArmLink.exe V5.05 update 1 (build 106)
    Library Manager: ArmAr.exe V5.05 update 1 (build 106)
    Hex Converter:   FromElf.exe V5.05 update 1 (build 106)
    CPU DLL:
    Dialog DLL:
    Target DLL:      STLink\ST-LINKIII-KEIL_SWO.dll V2.0.14.0_KEIL
    Dialog DLL:      TARMCM1.DLL V1.9.0.0

    Project:
    F:\BLE_Labs\peripheral\uart\pca10028\arm5\uart_pca10028.uvprojx
    Project File Date:  12/18/2015

    Output:
    Build target 'nrf51422_xxac'
    compiling main.c...
    linking...
    Program Size: Code=2568 RO-data=300 RW-data=20 ZI-data=2364
    FromELF: creating hex file...
    ".\_build\nrf51422_xxac.axf" - 0 Error(s), 0 Warning(s).

    Software Packages used:

    Package Vendor: ARM
                    http://www.keil.com/pack/ARM.CMSIS.4.5.0.pack
                    ARM::CMSIS:CORE:4.3.0
                    CMSIS (Cortex Microcontroller Software Interface Standard)
       * Component: CORE Version: 4.3.0

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_DeviceFamilyPack/NordicSemiconductor.nRF_DeviceFamilyPack.8.3.1.pack
                    NordicSemiconductor::Device:Startup:8.3.1
                    Nordic Semiconductor nRF ARM devices Device Family Pack.
       * Component: Startup Version: 8.3.1

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_Drivers/NordicSemiconductor.nRF_Drivers.4.0.0-2.alpha.pack
                    NordicSemiconductor::nRF_Drivers:nrf_delay:4.0.0-2.alpha
                    Drivers for Nordic Semiconductor nRF family.
       * Component: nrf_delay Version: 4.0.0-2.alpha
       * Component: nrf_gpio Version: 4.0.0-2.alpha
       * Component: nrf_uart Version: 4.0.0-2.alpha
       * Component: nrf_error Variant: No_softdevice Version: 4.0.0-2.alpha
       * Component: nrf_uarte Version: 4.0.0-2.alpha
       * Component: nrf_drv_uart Version: 4.0.0-2.alpha
       * Component: nrf_drv_common Version: 4.0.0-2.alpha

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_Examples/NordicSemiconductor.nRF_Examples.11.0.0-2.alpha.pack
                    NordicSemiconductor::Board Support:bsp:Defines:11.0.0-2.alpha
                    Examples and BSP for Nordic Semiconductor nRF family.
       * Component: bsp Variant: Defines Version: 11.0.0-2.alpha

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF51_SDK/pieces/nRF_Libraries/NordicSemiconductor.nRF_Libraries.4.0.0-2.alpha.pack
                    NordicSemiconductor::nRF_Libraries:app_error:4.0.0-2.alpha
                    Software modules for Nordic Semiconductor nRF family.
       * Component: app_error Version: 4.0.0-2.alpha
       * Component: nrf_assert Version: 4.0.0-2.alpha
       * Component: retarget Version: 4.0.0-2.alpha
       * Component: app_fifo Version: 4.0.0-2.alpha
       * Component: app_util Variant: No_softdevice Version: 4.0.0-2.alpha
       * Component: nordic_common Version: 4.0.0-2.alpha
       * Component: app_uart Variant: Fifo Version: 4.0.0-2.alpha

    Collection of Component include folders:
      F:\BLE_Labs\peripheral\uart\pca10028\arm5\RTE
      F:\BLE_Labs\peripheral\uart\pca10028\arm5\RTE\nRF_Drivers\nRF51422_xxAC
      F:\BLE_Labs\peripheral\uart\pca10028\arm5\RTE\nRF_Libraries\nRF51422_xxAC
      D:\Keil_v5\ARM\PACK\ARM\CMSIS\4.5.0\CMSIS\Include
      D:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.14.1\Device\Include
      D:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_DeviceFamilyPack\8.3.1\Device\Include
      D:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\4.0.0-2.alpha\common
      D:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\4.0.0-2.alpha\config
      D:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\4.0.0-2.alpha\delay
      D:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\4.0.0-2.alpha\hal
      D:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\4.0.0-2.alpha\nrf_soc_nosd
      D:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Drivers\4.0.0-2.alpha\uart
      D:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Examples\11.0.0-2.alpha\bsp
      D:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\4.0.0-2.alpha\fifo
      D:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\4.0.0-2.alpha\uart
      D:\Keil_v5\ARM\PACK\NordicSemiconductor\nRF_Libraries\4.0.0-2.alpha\util

    Collection of Component Files used:

       * Component: ARM::CMSIS:CORE:4.3.0

       * Component: NordicSemiconductor::Device:Startup:8.3.1
          Source file:   Device\Source\arm\arm_startup_nrf51.s
          Source file:   Device\Source\system_nrf51.c
          Include file:  Device\Include\system_nrf51.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_delay:4.0.0-2.alpha
          Source file:   delay\nrf_delay.c
          Include file:  delay\nrf_delay.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_gpio:4.0.0-2.alpha
          Include file:  hal\nrf_gpio.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_uart:4.0.0-2.alpha
          Include file:  hal\nrf_uart.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_error:No_softdevice:4.0.0-2.alpha

       * Component: NordicSemiconductor::nRF_Drivers:nrf_uarte:4.0.0-2.alpha
          Include file:  hal\nrf_uarte.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_drv_uart:4.0.0-2.alpha
          Source file:   uart\nrf_drv_uart.c
          Include file:  uart\nrf_drv_uart.h
          Include file:  config\nrf_drv_config.h

       * Component: NordicSemiconductor::nRF_Drivers:nrf_drv_common:4.0.0-2.alpha
          Source file:   common\nrf_drv_common.c
          Include file:  common\nrf_drv_common.h
          Include file:  config\nrf_drv_config.h

       * Component: NordicSemiconductor::Board Support:bsp:Defines:11.0.0-2.alpha

       * Component: NordicSemiconductor::nRF_Libraries:app_error:4.0.0-2.alpha
          Source file:   util\app_error.c
          Include file:  util\app_error.h

       * Component: NordicSemiconductor::nRF_Libraries:nrf_assert:4.0.0-2.alpha
          Source file:   util\nrf_assert.c
          Include file:  util\nrf_assert.h

       * Component: NordicSemiconductor::nRF_Libraries:retarget:4.0.0-2.alpha
          Source file:   uart\retarget.c

       * Component: NordicSemiconductor::nRF_Libraries:app_fifo:4.0.0-2.alpha
          Source file:   fifo\app_fifo.c
          Include file:  fifo\app_fifo.h

       * Component: NordicSemiconductor::nRF_Libraries:app_util:No_softdevice:4.0.0-2.alpha
          Source file:   util\app_util_platform.c

       * Component: NordicSemiconductor::nRF_Libraries:nordic_common:4.0.0-2.alpha

       * Component: NordicSemiconductor::nRF_Drivers:app_uart:Fifo:4.0.0-2.alpha
          Source file:   uart\app_uart_fifo.c
          Include file:  uart\app_uart.h