/* champ2.0 overlay file for bl653 */

/* console uses uart0 port and pins are re routed to 15 and 24 */
&uart0 {
  compatible = "nordic,nrf-uart";
  current-speed = <115200>;
  status = "okay";
  tx-pin = <15>;
  rx-pin = <24>;
  label = "UART_0";
};
