This sample extends the same-named Zephyr sample to verify it
with Nordic development kits.

Source code and basic configuration files can be found in the corresponding folder structure in zephyr/samples/subsys/usb/cdc_acm.
