# Static Call Graph for image .\_build\nrf52840_xxaa.axf

#<CALLGRAPH># ARM Linker, 5050106: Last Updated: Mon Aug 26 14:07:00 2019

### Maximum Stack Usage = 768 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ nrf_cli_process ⇒ cli_state_collect ⇒ cli_tab_handle ⇒ option_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- MemoryManagement_Handler ⇒ MemoryManagement_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- CCM_AAR_IRQHandler ⇒ CCM_AAR_IRQHandler
- nrf_log_frontend_dequeue ⇒ nrf_log_frontend_std_0
- app_util_critical_region_exit ⇒ assert_nrf_callback
- app_util_critical_region_enter ⇒ assert_nrf_callback
- nrf_memobj_write ⇒ assert_nrf_callback
- memobj_op ⇒ assert_nrf_callback
- nrf_balloc_free ⇒ assert_nrf_callback
- nrf_balloc_alloc ⇒ assert_nrf_callback
- std_n ⇒ assert_nrf_callback
- log_skip ⇒ assert_nrf_callback
- app_usbd_event_execute ⇒ app_usbd_event_execute
- buffer_add ⇒ buffer_add
- qsort ⇒ qsort

  ### Function Pointers

  - BusFault_Handler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - CCM_AAR_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - COMP_LPCOMP_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - CRYPTOCELL_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - DebugMon_Handler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - ECB_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - FPU_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - GPIOTE_IRQHandler from nrfx_gpiote.o(i.GPIOTE_IRQHandler) referenced from arm_startup_nrf52840.o(RESET)
  - HardFault_Handler from hardfault_handler_keil.o(.emb_text) referenced from arm_startup_nrf52840.o(RESET)
  - HardFault_c_handler from hardfault_implementation.o(i.HardFault_c_handler) referenced from hardfault_handler_keil.o(.emb_text)
  - I2S_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - MWU_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - MemoryManagement_Handler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - NFCT_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - NMI_Handler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - PDM_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - POWER_CLOCK_IRQHandler from nrfx_power.o(i.POWER_CLOCK_IRQHandler) referenced from arm_startup_nrf52840.o(RESET)
  - PWM0_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - PWM1_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - PWM2_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - PWM3_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - PendSV_Handler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - QDEC_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - QSPI_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - RADIO_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - RNG_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - RTC0_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - RTC1_IRQHandler from app_timer.o(i.RTC1_IRQHandler) referenced from arm_startup_nrf52840.o(RESET)
  - RTC2_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - Reset_Handler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - SAADC_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - SPIM1_SPIS1_TWIM1_TWIS1_SPI1_TWI1_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - SPIM2_SPIS2_SPI2_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - SPIM3_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - SVC_Handler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - SWI0_EGU0_IRQHandler from app_timer.o(i.SWI0_EGU0_IRQHandler) referenced from arm_startup_nrf52840.o(RESET)
  - SWI1_EGU1_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - SWI2_EGU2_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - SWI3_EGU3_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - SWI4_EGU4_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - SWI5_EGU5_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - SysTick_Handler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - SystemInit from system_nrf52840.o(i.SystemInit) referenced from arm_startup_nrf52840.o(.text)
  - TEMP_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - TIMER0_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - TIMER1_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - TIMER2_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - TIMER3_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - TIMER4_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - UARTE0_UART0_IRQHandler from nrfx_prs.o(i.UARTE0_UART0_IRQHandler) referenced from arm_startup_nrf52840.o(RESET)
  - UARTE1_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - USBD_IRQHandler from nrfx_usbd.o(i.USBD_IRQHandler) referenced from arm_startup_nrf52840.o(RESET)
  - UsageFault_Handler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - WDT_IRQHandler from arm_startup_nrf52840.o(.text) referenced from arm_startup_nrf52840.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from arm_startup_nrf52840.o(.text)
  - _sbackspace from _sgetc.o(.text) referenced from __0sscanf.o(.text)
  - _scanf_char_input from scanf_char.o(.text) referenced from scanf_char.o(.text)
  - _sgetc from _sgetc.o(.text) referenced from __0sscanf.o(.text)
  - alert_timer_handler from bsp.o(i.alert_timer_handler) referenced from bsp.o(i.bsp_init)
  - app_usbd_core_event_handler from app_usbd_core.o(i.app_usbd_core_event_handler) referenced from app_usbd_core.o(.constdata)
  - app_usbd_event_execute from app_usbd.o(i.app_usbd_event_execute) referenced from app_usbd.o(.constdata)
  - app_usbd_event_execute from app_usbd.o(i.app_usbd_event_execute) referenced from app_usbd.o(i.app_usbd_init)
  - app_usbd_event_handler from app_usbd.o(i.app_usbd_event_handler) referenced from app_usbd.o(i.app_usbd_init)
  - app_usbd_hfclk_ready from app_usbd.o(i.app_usbd_hfclk_ready) referenced 2 times from app_usbd.o(.data)
  - app_usbd_power_event_handler from app_usbd.o(i.app_usbd_power_event_handler) referenced from app_usbd.o(.constdata)
  - backend_name_get from nrf_log_frontend.o(i.backend_name_get) referenced from nrf_log_frontend.o(.constdata)
  - bsp_button_event_handler from bsp.o(i.bsp_button_event_handler) referenced 4 times from bsp.o(.constdata)
  - bsp_event_callback from main.o(i.bsp_event_callback) referenced from main.o(i.init_bsp)
  - bsp_event_callback from main.o(i.bsp_event_callback) referenced from main.o(i.init_cli)
  - button_timer_handler from bsp.o(i.button_timer_handler) referenced from bsp.o(i.bsp_init)
  - cli_transport_evt_handler from nrf_cli.o(i.cli_transport_evt_handler) referenced from nrf_cli.o(i.nrf_cli_instance_init)
  - cli_uart_enable from nrf_cli_uart.o(i.cli_uart_enable) referenced from nrf_cli_uart.o(.constdata)
  - cli_uart_init from nrf_cli_uart.o(i.cli_uart_init) referenced from nrf_cli_uart.o(.constdata)
  - cli_uart_read from nrf_cli_uart.o(i.cli_uart_read) referenced from nrf_cli_uart.o(.constdata)
  - cli_uart_uninit from nrf_cli_uart.o(i.cli_uart_uninit) referenced from nrf_cli_uart.o(.constdata)
  - cli_uart_write from nrf_cli_uart.o(i.cli_uart_write) referenced from nrf_cli_uart.o(.constdata)
  - clock_irq_handler from nrf_drv_clock.o(i.clock_irq_handler) referenced from nrf_drv_clock.o(i.nrf_drv_clock_init)
  - cmd_btn from bsp_cli.o(i.cmd_btn) referenced from bsp_cli.o(.constdata)
  - cmd_evt from bsp_cli.o(i.cmd_evt) referenced from bsp_cli.o(.constdata)
  - detection_delay_timeout_handler from app_button.o(i.detection_delay_timeout_handler) referenced from app_button.o(i.app_button_init)
  - ev_dma_epin0_handler from nrfx_usbd.o(i.ev_dma_epin0_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_dma_epin1_handler from nrfx_usbd.o(i.ev_dma_epin1_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_dma_epin2_handler from nrfx_usbd.o(i.ev_dma_epin2_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_dma_epin3_handler from nrfx_usbd.o(i.ev_dma_epin3_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_dma_epin4_handler from nrfx_usbd.o(i.ev_dma_epin4_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_dma_epin5_handler from nrfx_usbd.o(i.ev_dma_epin5_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_dma_epin6_handler from nrfx_usbd.o(i.ev_dma_epin6_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_dma_epin7_handler from nrfx_usbd.o(i.ev_dma_epin7_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_dma_epin8_handler from nrfx_usbd.o(i.ev_dma_epin8_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_dma_epout0_handler from nrfx_usbd.o(i.ev_dma_epout0_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_dma_epout1_handler from nrfx_usbd.o(i.ev_dma_epout1_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_dma_epout2_handler from nrfx_usbd.o(i.ev_dma_epout2_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_dma_epout3_handler from nrfx_usbd.o(i.ev_dma_epout3_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_dma_epout4_handler from nrfx_usbd.o(i.ev_dma_epout4_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_dma_epout5_handler from nrfx_usbd.o(i.ev_dma_epout5_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_dma_epout6_handler from nrfx_usbd.o(i.ev_dma_epout6_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_dma_epout7_handler from nrfx_usbd.o(i.ev_dma_epout7_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_dma_epout8_handler from nrfx_usbd.o(i.ev_dma_epout8_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_epdata_handler from nrfx_usbd.o(i.ev_epdata_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_setup_data_handler from nrfx_usbd.o(i.ev_setup_data_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_setup_handler from nrfx_usbd.o(i.ev_setup_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_sof_handler from nrfx_usbd.o(i.ev_sof_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_started_handler from nrfx_usbd.o(i.ev_started_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_usbevent_handler from nrfx_usbd.o(i.ev_usbevent_handler) referenced from nrfx_usbd.o(.constdata)
  - ev_usbreset_handler from nrfx_usbd.o(i.ev_usbreset_handler) referenced from nrfx_usbd.o(.constdata)
  - gpiote_event_handler from app_button.o(i.gpiote_event_handler) referenced from app_button.o(i.app_button_init)
  - hid_generic_ep_transfer_in from app_usbd_hid_generic.o(i.hid_generic_ep_transfer_in) referenced from app_usbd_hid_generic.o(.constdata)
  - hid_generic_ep_transfer_out from app_usbd_hid_generic.o(i.hid_generic_ep_transfer_out) referenced from app_usbd_hid_generic.o(.constdata)
  - hid_generic_event_handler from app_usbd_hid_generic.o(i.hid_generic_event_handler) referenced from app_usbd_hid_generic.o(.constdata)
  - hid_generic_feed_descriptors from app_usbd_hid_generic.o(i.hid_generic_feed_descriptors) referenced from app_usbd_hid_generic.o(.constdata)
  - hid_generic_get_class_descriptors_data from app_usbd_hid_generic.o(i.hid_generic_get_class_descriptors_data) referenced from app_usbd_hid_generic.o(.constdata)
  - hid_generic_get_class_descriptors_length from app_usbd_hid_generic.o(i.hid_generic_get_class_descriptors_length) referenced from app_usbd_hid_generic.o(.constdata)
  - hid_generic_idle_handler_set from app_usbd_hid_generic.o(i.hid_generic_idle_handler_set) referenced from app_usbd_hid_generic.o(.constdata)
  - hid_generic_on_get_report from app_usbd_hid_generic.o(i.hid_generic_on_get_report) referenced from app_usbd_hid_generic.o(.constdata)
  - hid_generic_on_idle from app_usbd_hid_generic.o(i.hid_generic_on_idle) referenced from app_usbd_hid_generic.o(.constdata)
  - hid_generic_on_set_report from app_usbd_hid_generic.o(i.hid_generic_on_set_report) referenced from app_usbd_hid_generic.o(.constdata)
  - hid_generic_on_set_report_data_cb from app_usbd_hid_generic.o(i.hid_generic_on_set_report_data_cb) referenced from app_usbd_hid_generic.o(.constdata)
  - hid_user_ev_handler from main.o(i.hid_user_ev_handler) referenced from main.o(.constdata)
  - idle_handle from main.o(i.idle_handle) referenced from main.o(i.main)
  - isspace from isspace_o.o(.text) referenced from scanf_char.o(.text)
  - leds_timer_handler from bsp.o(i.leds_timer_handler) referenced from bsp.o(i.bsp_init)
  - log_backend_ctrl from nrf_log_frontend.o(i.log_backend_ctrl) referenced 2 times from nrf_log_frontend.o(.constdata)
  - log_backend_go from nrf_log_frontend.o(i.log_backend_go) referenced from nrf_log_frontend.o(.constdata)
  - log_backend_halt from nrf_log_frontend.o(i.log_backend_halt) referenced from nrf_log_frontend.o(.constdata)
  - log_backend_status from nrf_log_frontend.o(i.log_backend_status) referenced from nrf_log_frontend.o(.constdata)
  - log_cmd from nrf_log_frontend.o(i.log_cmd) referenced from nrf_log_frontend.o(.constdata)
  - log_cmd_backends_list from nrf_log_frontend.o(i.log_cmd_backends_list) referenced from nrf_log_frontend.o(.constdata)
  - log_config_load_cmd from nrf_log_frontend.o(i.log_config_load_cmd) referenced from nrf_log_frontend.o(.constdata)
  - log_config_store_cmd from nrf_log_frontend.o(i.log_config_store_cmd) referenced from nrf_log_frontend.o(.constdata)
  - log_ctrl from nrf_log_frontend.o(i.log_ctrl) referenced from nrf_log_frontend.o(i.log_backend_ctrl)
  - log_go from nrf_log_frontend.o(i.log_go) referenced from nrf_log_frontend.o(i.log_backend_go)
  - log_halt from nrf_log_frontend.o(i.log_halt) referenced from nrf_log_frontend.o(i.log_backend_halt)
  - log_self_ctrl from nrf_log_frontend.o(i.log_self_ctrl) referenced 2 times from nrf_log_frontend.o(.constdata)
  - log_self_go from nrf_log_frontend.o(i.log_self_go) referenced from nrf_log_frontend.o(.constdata)
  - log_self_halt from nrf_log_frontend.o(i.log_self_halt) referenced from nrf_log_frontend.o(.constdata)
  - log_self_status from nrf_log_frontend.o(i.log_self_status) referenced from nrf_log_frontend.o(.constdata)
  - log_status from nrf_log_frontend.o(i.log_status) referenced from nrf_log_frontend.o(i.log_backend_status)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)
  - module_name_get from nrf_log_frontend.o(i.module_name_get) referenced from nrf_log_frontend.o(.constdata)
  - mouse_move_timer_handler from main.o(i.mouse_move_timer_handler) referenced from main.o(i.main)
  - nrf_balloc_status from nrf_balloc.o(i.nrf_balloc_status) referenced 2 times from nrf_balloc.o(.constdata)
  - nrf_cli_cmd_clear from nrf_cli.o(i.nrf_cli_cmd_clear) referenced from nrf_cli.o(.constdata)
  - nrf_cli_cmd_cli from nrf_cli.o(i.nrf_cli_cmd_cli) referenced from nrf_cli.o(.constdata)
  - nrf_cli_cmd_cli_stats from nrf_cli.o(i.nrf_cli_cmd_cli_stats) referenced from nrf_cli.o(.constdata)
  - nrf_cli_cmd_cli_stats_reset from nrf_cli.o(i.nrf_cli_cmd_cli_stats_reset) referenced from nrf_cli.o(.constdata)
  - nrf_cli_cmd_cli_stats_show from nrf_cli.o(i.nrf_cli_cmd_cli_stats_show) referenced from nrf_cli.o(.constdata)
  - nrf_cli_cmd_colors from nrf_cli.o(i.nrf_cli_cmd_colors) referenced from nrf_cli.o(.constdata)
  - nrf_cli_cmd_colors_off from nrf_cli.o(i.nrf_cli_cmd_colors_off) referenced from nrf_cli.o(.constdata)
  - nrf_cli_cmd_colors_on from nrf_cli.o(i.nrf_cli_cmd_colors_on) referenced from nrf_cli.o(.constdata)
  - nrf_cli_cmd_echo from nrf_cli.o(i.nrf_cli_cmd_echo) referenced from nrf_cli.o(.constdata)
  - nrf_cli_cmd_echo_off from nrf_cli.o(i.nrf_cli_cmd_echo_off) referenced from nrf_cli.o(.constdata)
  - nrf_cli_cmd_echo_on from nrf_cli.o(i.nrf_cli_cmd_echo_on) referenced from nrf_cli.o(.constdata)
  - nrf_cli_cmd_history from nrf_cli.o(i.nrf_cli_cmd_history) referenced from nrf_cli.o(.constdata)
  - nrf_cli_cmd_resize from nrf_cli.o(i.nrf_cli_cmd_resize) referenced from nrf_cli.o(.constdata)
  - nrf_cli_cmd_resize_default from nrf_cli.o(i.nrf_cli_cmd_resize_default) referenced from nrf_cli.o(.constdata)
  - nrf_cli_print_stream from nrf_cli.o(i.nrf_cli_print_stream) referenced 2 times from main.o(.data)
  - nrf_log_backend_cli_flush from nrf_cli.o(i.nrf_log_backend_cli_flush) referenced from nrf_cli.o(.constdata)
  - nrf_log_backend_cli_panic_set from nrf_cli.o(i.nrf_log_backend_cli_panic_set) referenced from nrf_cli.o(.constdata)
  - nrf_log_backend_cli_put from nrf_cli.o(i.nrf_log_backend_cli_put) referenced from nrf_cli.o(.constdata)
  - nrf_log_backend_uart_flush from nrf_log_backend_uart.o(i.nrf_log_backend_uart_flush) referenced from nrf_log_backend_uart.o(.constdata)
  - nrf_log_backend_uart_panic_set from nrf_log_backend_uart.o(i.nrf_log_backend_uart_panic_set) referenced from nrf_log_backend_uart.o(.constdata)
  - nrf_log_backend_uart_put from nrf_log_backend_uart.o(i.nrf_log_backend_uart_put) referenced from nrf_log_backend_uart.o(.constdata)
  - nrf_queue_status from nrf_queue.o(i.nrf_queue_status) referenced 2 times from nrf_queue.o(.constdata)
  - nrfx_uart_0_irq_handler from nrfx_uart.o(i.nrfx_uart_0_irq_handler) referenced from nrfx_uart.o(.constdata)
  - nrfx_uarte_0_irq_handler from nrfx_uarte.o(i.nrfx_uarte_0_irq_handler) referenced from nrfx_uarte.o(.constdata)
  - nrfx_usbd_consumer from nrfx_usbd.o(i.nrfx_usbd_consumer) referenced from nrfx_usbd.o(i.nrfx_usbd_ep_transfer)
  - nrfx_usbd_feeder_flash from nrfx_usbd.o(i.nrfx_usbd_feeder_flash) referenced from nrfx_usbd.o(i.nrfx_usbd_ep_transfer)
  - nrfx_usbd_feeder_flash_zlp from nrfx_usbd.o(i.nrfx_usbd_feeder_flash_zlp) referenced from nrfx_usbd.o(i.nrfx_usbd_ep_transfer)
  - nrfx_usbd_feeder_ram from nrfx_usbd.o(i.nrfx_usbd_feeder_ram) referenced from nrfx_usbd.o(i.nrfx_usbd_ep_transfer)
  - nrfx_usbd_feeder_ram_zlp from nrfx_usbd.o(i.nrfx_usbd_feeder_ram_zlp) referenced from nrfx_usbd.o(i.nrfx_usbd_ep_transfer)
  - serial_tx from nrf_log_backend_uart.o(i.serial_tx) referenced from nrf_log_backend_uart.o(i.nrf_log_backend_uart_put)
  - setup_data_handler_empty from app_usbd_core.o(i.setup_data_handler_empty) referenced from app_usbd_core.o(.constdata)
  - severity_lvl_get from nrf_log_frontend.o(i.severity_lvl_get) referenced from nrf_log_frontend.o(.constdata)
  - string_cmp from nrf_cli.o(i.string_cmp) referenced from nrf_cli.o(i.nrf_cli_instance_init)
  - timer_handler from nrf_cli_uart.o(i.timer_handler) referenced from nrf_cli_uart.o(i.cli_uart_enable)
  - uart_event_handler from nrf_cli_uart.o(i.uart_event_handler) referenced from nrf_cli_uart.o(i.cli_uart_init)
  - uart_evt_handler from nrf_drv_uart.o(i.uart_evt_handler) referenced from nrf_drv_uart.o(i.nrf_drv_uart_init)
  - uart_evt_handler from nrf_log_backend_uart.o(i.uart_evt_handler) referenced from nrf_log_backend_uart.o(i.uart_init)
  - uarte_evt_handler from nrf_drv_uart.o(i.uarte_evt_handler) referenced from nrf_drv_uart.o(i.nrf_drv_uart_init)
  - usbd_descriptor_conf_feeder from app_usbd_core.o(i.usbd_descriptor_conf_feeder) referenced from app_usbd_core.o(.constdata)
  - usbd_user_ev_handler from main.o(i.usbd_user_ev_handler) referenced from main.o(.constdata)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_mov (Thumb, 24 bytes, Stack size 0 bytes, nrfx_atomic.o(.emb_text), UNUSED)

  __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_orr (Thumb, 26 bytes, Stack size 0 bytes, nrfx_atomic.o(.emb_text), UNUSED)

  __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_and (Thumb, 26 bytes, Stack size 0 bytes, nrfx_atomic.o(.emb_text))
  [Called By]

  - >> nrfx_atomic_u32_fetch_and

  __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_eor (Thumb, 26 bytes, Stack size 0 bytes, nrfx_atomic.o(.emb_text), UNUSED)

  __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_add (Thumb, 26 bytes, Stack size 0 bytes, nrfx_atomic.o(.emb_text), UNUSED)

  __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_sub (Thumb, 26 bytes, Stack size 0 bytes, nrfx_atomic.o(.emb_text), UNUSED)

  __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_cmp_exch (Thumb, 42 bytes, Stack size 0 bytes, nrfx_atomic.o(.emb_text), UNUSED)

  __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_sub_hs (Thumb, 30 bytes, Stack size 0 bytes, nrfx_atomic.o(.emb_text), UNUSED)

  app_error_handler (Thumb, 26 bytes, Stack size 0 bytes, app_error_handler_keil.o(.emb_text))
  [Stack]

  - Max Depth = 248
  - Call Chain = app_error_handler ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_error_fault_handler
  [Called By]
  - >> app_usbd_power_events_enable
  - >> app_usbd_init
  - >> main
  - >> init_cli
  - >> init_bsp
  - >> uart_init
  - >> serial_tx

  HardFault_Handler (Thumb, 40 bytes, Stack size 0 bytes, hardfault_handler_keil.o(.emb_text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_mov (Thumb, 24 bytes, Stack size 0 bytes, nrf_atomic.o(.emb_text))
  [Called By]

  - >> nrf_atomic_u32_fetch_store

  __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_orr (Thumb, 26 bytes, Stack size 0 bytes, nrf_atomic.o(.emb_text))
  [Called By]

  - >> nrf_atomic_u32_or
  - >> nrf_atomic_u32_fetch_or

  __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_and (Thumb, 26 bytes, Stack size 0 bytes, nrf_atomic.o(.emb_text))
  [Called By]

  - >> nrf_atomic_u32_and
  - >> nrf_atomic_u32_fetch_and

  __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_eor (Thumb, 26 bytes, Stack size 0 bytes, nrf_atomic.o(.emb_text), UNUSED)

  __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_add (Thumb, 26 bytes, Stack size 0 bytes, nrf_atomic.o(.emb_text))
  [Called By]

  - >> nrf_atomic_u32_add

  __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_sub (Thumb, 26 bytes, Stack size 0 bytes, nrf_atomic.o(.emb_text))
  [Called By]

  - >> nrf_atomic_u32_sub

  __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_cmp_exch (Thumb, 42 bytes, Stack size 0 bytes, nrf_atomic.o(.emb_text), UNUSED)

  __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_sub_hs (Thumb, 30 bytes, Stack size 0 bytes, nrf_atomic.o(.emb_text), UNUSED)

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52840.o(RESET)

  MemoryManagement_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Calls]

  - >> MemoryManagement_Handler
  [Called By]
  - >> MemoryManagement_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52840.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52840.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52840.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52840.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52840.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52840.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - arm_startup_nrf52840.o(RESET)

  CCM_AAR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Calls]

  - >> CCM_AAR_IRQHandler
  [Called By]
  - >> CCM_AAR_IRQHandler
  [Address Reference Count : 1]
  - arm_startup_nrf52840.o(RESET)

  COMP_LPCOMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  CRYPTOCELL_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  ECB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  I2S_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  MWU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  NFCT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  PDM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  PWM0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  PWM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  PWM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  PWM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  QDEC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  QSPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  RADIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  RTC0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  RTC2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  SAADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  SPIM1_SPIS1_TWIM1_TWIS1_SPI1_TWI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  SPIM2_SPIS2_SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  SPIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  SWI1_EGU1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  SWI2_EGU2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  SWI3_EGU3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  SWI4_EGU4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  SWI5_EGU5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  TEMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  TIMER0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  TIMER1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  TIMER2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  TIMER3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  TIMER4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  UARTE1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, arm_startup_nrf52840.o(.text))
  [Address Reference Count : 1]

  - arm_startup_nrf52840.o(RESET)

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_uldivmod
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> bsp_led_indication

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> gpiote_event_handler
  - >> detection_delay_timeout_handler
  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __rt_ctype_table (Thumb, 4 bytes, Stack size 0 bytes, ctype_o.o(.text))
  [Called By]

  - >> cmd_trim
  - >> cli_tab_handle
  - >> cli_state_collect
  - >> nrf_log_hexdump_entry_process
  - >> make_argv
  - >> format_offset_string_print
  - >> isspace

  isspace (Thumb, 18 bytes, Stack size 8 bytes, isspace_o.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = isspace
  [Calls]
  - >> __rt_ctype_table
  [Address Reference Count : 1]
  - scanf_char.o(.text)

  qsort (Thumb, 156 bytes, Stack size 40 bytes, qsort.o(.text))
  [Stack]

  - Max Depth = 40 + In Cycle
  - Call Chain = qsort ⇒ qsort (Cycle)
  [Calls]
  - >> qsort
  [Called By]
  - >> nrf_cli_instance_init
  - >> qsort

  ___aeabi_memcpy8$move (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text), UNUSED)

  __aeabi_memcpy (Thumb, 64 bytes, Stack size 8 bytes, memmovea.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_memcpy
  [Called By]
  - >> nrfx_usbd_feeder_flash_zlp
  - >> nrfx_usbd_feeder_flash
  - >> nrf_queue_push
  - >> nrf_queue_generic_pop
  - >> usbd_descriptor_conf_feeder
  - >> setup_device_req_get_descriptor
  - >> memobj_op
  - >> nrf_ringbuf_cpy_put
  - >> nrf_ringbuf_cpy_get

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_memcpy4
  [Called By]
  - >> nrf_drv_uart_init
  - >> init_cli
  - >> cli_tab_handle
  - >> uart_init
  - >> cli_uart_init

  __aeabi_memmove (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_memmove
  [Called By]
  - >> completion_insert
  - >> cmd_trim
  - >> char_insert
  - >> char_delete
  - >> char_backspace
  - >> make_argv

  __aeabi_memmove4 (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text), UNUSED)

  __aeabi_memmove8 (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> app_usbd_init
  - >> nrf_log_backend_serial_put
  - >> nrf_cli_instance_init
  - >> cursor_position_get

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
  [Called By]

  - >> cli_strlen
  - >> nrf_fprintf_fmt

  strcmp (Thumb, 28 bytes, Stack size 8 bytes, strcmp.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = strcmp
  [Called By]
  - >> cmd_get
  - >> cli_tab_handle
  - >> cli_execute
  - >> nrf_cli_backend_cmd_execute
  - >> string_cmp
  - >> history_save

  strcpy (Thumb, 18 bytes, Stack size 0 bytes, strcpy.o(.text))
  [Called By]

  - >> history_handle

  strncmp (Thumb, 30 bytes, Stack size 12 bytes, strncmp.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = strncmp
  [Called By]
  - >> nrf_log_init
  - >> log_ctrl
  - >> is_completion_candidate

  __0sscanf (Thumb, 48 bytes, Stack size 72 bytes, __0sscanf.o(.text))
  [Stack]

  - Max Depth = 216
  - Call Chain = __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_int
  [Calls]
  - >> __vfscanf_char
  [Called By]
  - >> cmd_evt
  - >> cmd_btn

  _scanf_int (Thumb, 332 bytes, Stack size 56 bytes, _scanf_int.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _scanf_int
  [Calls]
  - >> _chval
  [Called By]
  - >> __vfscanf

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  _chval (Thumb, 28 bytes, Stack size 0 bytes, _chval.o(.text))
  [Called By]

  - >> _scanf_int

  __vfscanf_char (Thumb, 20 bytes, Stack size 0 bytes, scanf_char.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = __vfscanf_char ⇒ __vfscanf ⇒ _scanf_int
  [Calls]
  - >> __vfscanf
  [Called By]
  - >> __0sscanf

  _sgetc (Thumb, 30 bytes, Stack size 0 bytes, _sgetc.o(.text))
  [Address Reference Count : 1]

  - __0sscanf.o(.text)

  _sbackspace (Thumb, 34 bytes, Stack size 0 bytes, _sgetc.o(.text))
  [Address Reference Count : 1]

  - __0sscanf.o(.text)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __vfscanf (Thumb, 808 bytes, Stack size 88 bytes, _scanf.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = __vfscanf ⇒ _scanf_int
  [Calls]
  - >> _scanf_int
  [Called By]
  - >> __vfscanf_char

  __decompress (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  __decompress1 (Thumb, 86 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  GPIOTE_IRQHandler (Thumb, 428 bytes, Stack size 88 bytes, nrfx_gpiote.o(i.GPIOTE_IRQHandler))
  [Stack]

  - Max Depth = 376
  - Call Chain = GPIOTE_IRQHandler ⇒ nrf_gpio_ports_read ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpiote_event_is_set
  - >> nrf_gpiote_event_clear
  - >> nrf_gpio_ports_read
  - >> nrf_gpio_pin_port_decode
  - >> nrf_gpio_cfg_sense_set
  - >> nrf_bitmask_bit_set
  - >> nrf_bitmask_bit_is_set
  - >> channel_port_get
  [Address Reference Count : 1]
  - arm_startup_nrf52840.o(RESET)

  HardFault_c_handler (Thumb, 246 bytes, Stack size 16 bytes, hardfault_implementation.o(i.HardFault_c_handler))
  [Stack]

  - Max Depth = 216
  - Call Chain = HardFault_c_handler ⇒ nrf_log_frontend_std_4 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_log_frontend_std_0
  - >> nrf_log_frontend_dequeue
  - >> nrf_log_panic
  - >> nrf_log_frontend_std_1
  - >> HardFault_process
  - >> nrf_log_frontend_std_4
  - >> nrf_log_frontend_std_3
  [Address Reference Count : 1]
  - hardfault_handler_keil.o(.emb_text)

  HardFault_process (Thumb, 26 bytes, Stack size 0 bytes, hardfault_implementation.o(i.HardFault_process))
  [Called By]

  - >> HardFault_c_handler

  POWER_CLOCK_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, nrfx_power.o(i.POWER_CLOCK_IRQHandler))
  [Stack]

  - Max Depth = 288
  - Call Chain = POWER_CLOCK_IRQHandler ⇒ nrfx_power_irq_handler ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_power_irq_handler
  - >> nrfx_clock_irq_handler
  [Address Reference Count : 1]
  - arm_startup_nrf52840.o(RESET)

  RTC1_IRQHandler (Thumb, 32 bytes, Stack size 0 bytes, app_timer.o(i.RTC1_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = RTC1_IRQHandler ⇒ timer_timeouts_check
  [Calls]
  - >> timer_timeouts_check
  [Address Reference Count : 1]
  - arm_startup_nrf52840.o(RESET)

  SWI0_EGU0_IRQHandler (Thumb, 4 bytes, Stack size 0 bytes, app_timer.o(i.SWI0_EGU0_IRQHandler))
  [Stack]

  - Max Depth = 96
  - Call Chain = SWI0_EGU0_IRQHandler ⇒ timer_list_handler ⇒ list_insertions_handler ⇒ timer_list_remove
  [Calls]
  - >> timer_list_handler
  [Address Reference Count : 1]
  - arm_startup_nrf52840.o(RESET)

  SystemInit (Thumb, 416 bytes, Stack size 12 bytes, system_nrf52840.o(i.SystemInit))
  [Stack]

  - Max Depth = 12
  - Call Chain = SystemInit
  [Address Reference Count : 1]
  - arm_startup_nrf52840.o(.text)

  UARTE0_UART0_IRQHandler (Thumb, 24 bytes, Stack size 8 bytes, nrfx_prs.o(i.UARTE0_UART0_IRQHandler))
  [Stack]

  - Max Depth = 272
  - Call Chain = UARTE0_UART0_IRQHandler ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Address Reference Count : 1]
  - arm_startup_nrf52840.o(RESET)

  USBD_IRQHandler (Thumb, 344 bytes, Stack size 40 bytes, nrfx_usbd.o(i.USBD_IRQHandler))
  [Stack]

  - Max Depth = 400
  - Call Chain = USBD_IRQHandler ⇒ usbd_dmareq_process ⇒ nrfx_systick_delay_us ⇒ nrfx_systick_delay_ticks ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> usbd_dmareq_process
  - >> nrfx_usbd_errata_104
  - >> nrf_usbd_event_clear
  - >> nrf_usbd_event_check
  - >> ev_setup_handler
  [Address Reference Count : 1]
  - arm_startup_nrf52840.o(RESET)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  app_button_enable (Thumb, 44 bytes, Stack size 16 bytes, app_button.o(i.app_button_enable))
  [Stack]

  - Max Depth = 328
  - Call Chain = app_button_enable ⇒ nrfx_gpiote_in_event_enable ⇒ nrf_gpio_cfg_sense_set ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_gpiote_in_event_enable
  [Called By]
  - >> bsp_init

  app_button_init (Thumb, 102 bytes, Stack size 24 bytes, app_button.o(i.app_button_init))
  [Stack]

  - Max Depth = 368
  - Call Chain = app_button_init ⇒ nrfx_gpiote_in_init ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_timer_create
  - >> nrfx_gpiote_is_init
  - >> nrfx_gpiote_init
  - >> nrfx_gpiote_in_init
  [Called By]
  - >> bsp_init

  app_error_fault_handler (Thumb, 168 bytes, Stack size 40 bytes, app_error_weak.o(i.app_error_fault_handler))
  [Stack]

  - Max Depth = 248
  - Call Chain = app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_log_frontend_std_0
  - >> nrf_log_frontend_dequeue
  - >> nrf_strerror_get
  - >> nrf_log_panic
  - >> nrf_log_frontend_std_5
  - >> nrf_log_frontend_std_2
  - >> nrf_log_frontend_std_1
  - >> app_error_save_and_stop
  [Called By]
  - >> assert_nrf_callback
  - >> app_error_handler

  app_error_save_and_stop (Thumb, 96 bytes, Stack size 8 bytes, app_error.o(i.app_error_save_and_stop))
  [Stack]

  - Max Depth = 8
  - Call Chain = app_error_save_and_stop
  [Called By]
  - >> app_error_fault_handler

  app_timer_create (Thumb, 32 bytes, Stack size 0 bytes, app_timer.o(i.app_timer_create))
  [Called By]

  - >> app_button_init
  - >> bsp_init
  - >> main
  - >> cli_uart_enable

  app_timer_init (Thumb, 70 bytes, Stack size 16 bytes, app_timer.o(i.app_timer_init))
  [Stack]

  - Max Depth = 32
  - Call Chain = app_timer_init ⇒ rtc1_stop
  [Calls]
  - >> rtc1_stop
  - >> NVIC_SetPriority
  - >> NVIC_EnableIRQ
  - >> NVIC_ClearPendingIRQ
  [Called By]
  - >> main

  app_timer_start (Thumb, 120 bytes, Stack size 32 bytes, app_timer.o(i.app_timer_start))
  [Stack]

  - Max Depth = 40
  - Call Chain = app_timer_start ⇒ app_util_critical_region_exit ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> user_op_alloc
  - >> NVIC_SetPendingIRQ
  [Called By]
  - >> bsp_led_indication
  - >> bsp_button_event_handler
  - >> bsp_event_callback
  - >> gpiote_event_handler
  - >> rx_try

  app_timer_stop (Thumb, 26 bytes, Stack size 0 bytes, app_timer.o(i.app_timer_stop))
  [Stack]

  - Max Depth = 32
  - Call Chain = app_timer_stop ⇒ timer_stop_op_schedule ⇒ app_util_critical_region_exit ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> timer_stop_op_schedule
  [Called By]
  - >> bsp_led_indication
  - >> bsp_button_event_handler
  - >> mouse_move_timer_handler
  - >> gpiote_event_handler
  - >> cli_uart_uninit
  - >> cli_uart_enable

  app_usbd_all_call (Thumb, 32 bytes, Stack size 16 bytes, app_usbd.o(i.app_usbd_all_call))
  [Stack]

  - Max Depth = 296
  - Call Chain = app_usbd_all_call ⇒ class_event_handler ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> class_event_handler
  - >> app_usbd_class_next_get
  [Called By]
  - >> app_usbd_event_execute

  app_usbd_all_iface_deselect (Thumb, 44 bytes, Stack size 16 bytes, app_usbd.o(i.app_usbd_all_iface_deselect))
  [Stack]

  - Max Depth = 376
  - Call Chain = app_usbd_all_iface_deselect ⇒ app_usbd_iface_deselect ⇒ nrfx_usbd_ep_disable ⇒ usbd_ep_abort ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_usbd_class_next_get
  - >> app_usbd_iface_deselect
  [Called By]
  - >> setup_device_req_std_handler
  - >> app_usbd_event_execute

  app_usbd_all_iface_select_0 (Thumb, 64 bytes, Stack size 24 bytes, app_usbd.o(i.app_usbd_all_iface_select_0))
  [Stack]

  - Max Depth = 360
  - Call Chain = app_usbd_all_iface_select_0 ⇒ app_usbd_iface_select ⇒ app_usbd_ep_enable ⇒ nrfx_usbd_ep_enable ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_usbd_class_next_get
  - >> app_usbd_iface_select
  [Called By]
  - >> setup_device_req_std_handler

  app_usbd_all_until_served_call (Thumb, 42 bytes, Stack size 16 bytes, app_usbd.o(i.app_usbd_all_until_served_call))
  [Stack]

  - Max Depth = 296
  - Call Chain = app_usbd_all_until_served_call ⇒ class_event_handler ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> class_event_handler
  - >> app_usbd_class_next_get
  [Called By]
  - >> app_usbd_core_setup_req_handler

  app_usbd_class_append (Thumb, 232 bytes, Stack size 24 bytes, app_usbd.o(i.app_usbd_class_append))
  [Stack]

  - Max Depth = 312
  - Call Chain = app_usbd_class_append ⇒ app_usbd_ep_instance_set ⇒ app_usbd_ep_conf_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_usbd_is_enabled
  - >> assert_nrf_callback
  - >> nrfx_usbd_is_initialized
  - >> class_event_handler
  - >> app_usbd_ep_instance_set
  - >> app_usbd_ep_instance_get
  - >> app_usbd_class_iface_get
  - >> app_usbd_class_iface_ep_get
  [Called By]
  - >> main

  app_usbd_class_descriptor_find (Thumb, 192 bytes, Stack size 64 bytes, app_usbd.o(i.app_usbd_class_descriptor_find))
  [Stack]

  - Max Depth = 64
  - Call Chain = app_usbd_class_descriptor_find
  [Called By]
  - >> setup_req_std_in

  app_usbd_class_first_get (Thumb, 6 bytes, Stack size 0 bytes, app_usbd.o(i.app_usbd_class_first_get))
  [Called By]

  - >> setup_device_req_get_descriptor

  app_usbd_class_rwu_enabled_check (Thumb, 12 bytes, Stack size 0 bytes, app_usbd.o(i.app_usbd_class_rwu_enabled_check))
  [Called By]

  - >> setup_device_req_std_handler
  - >> setup_device_req_get_descriptor
  - >> app_usbd_wakeup_req

  app_usbd_class_rwu_register (Thumb, 42 bytes, Stack size 8 bytes, app_usbd.o(i.app_usbd_class_rwu_register))
  [Stack]

  - Max Depth = 272
  - Call Chain = app_usbd_class_rwu_register ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> app_usbd_hid_event_handler

  app_usbd_class_rwu_unregister (Thumb, 40 bytes, Stack size 8 bytes, app_usbd.o(i.app_usbd_class_rwu_unregister))
  [Stack]

  - Max Depth = 272
  - Call Chain = app_usbd_class_rwu_unregister ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> app_usbd_hid_event_handler

  app_usbd_class_sof_register (Thumb, 154 bytes, Stack size 16 bytes, app_usbd.o(i.app_usbd_class_sof_register))
  [Stack]

  - Max Depth = 280
  - Call Chain = app_usbd_class_sof_register ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_usbd_is_enabled
  - >> assert_nrf_callback
  - >> nrfx_usbd_is_initialized
  [Called By]
  - >> app_usbd_hid_event_handler

  app_usbd_class_sof_unregister (Thumb, 76 bytes, Stack size 8 bytes, app_usbd.o(i.app_usbd_class_sof_unregister))
  [Stack]

  - Max Depth = 272
  - Call Chain = app_usbd_class_sof_unregister ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_usbd_is_enabled
  - >> assert_nrf_callback
  - >> nrfx_usbd_is_initialized
  [Called By]
  - >> app_usbd_hid_event_handler

  app_usbd_core_ep0_disable (Thumb, 18 bytes, Stack size 8 bytes, app_usbd_core.o(i.app_usbd_core_ep0_disable))
  [Stack]

  - Max Depth = 352
  - Call Chain = app_usbd_core_ep0_disable ⇒ app_usbd_ep_disable ⇒ nrfx_usbd_ep_disable ⇒ usbd_ep_abort ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_usbd_ep_disable
  [Called By]
  - >> app_usbd_event_execute

  app_usbd_core_ep0_enable (Thumb, 18 bytes, Stack size 8 bytes, app_usbd_core.o(i.app_usbd_core_ep0_enable))
  [Stack]

  - Max Depth = 328
  - Call Chain = app_usbd_core_ep0_enable ⇒ app_usbd_ep_enable ⇒ nrfx_usbd_ep_enable ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_usbd_ep_enable
  [Called By]
  - >> app_usbd_event_execute

  app_usbd_core_feature_state_get (Thumb, 12 bytes, Stack size 0 bytes, app_usbd_core.o(i.app_usbd_core_feature_state_get))
  [Called By]

  - >> app_usbd_wakeup_req

  app_usbd_core_setup_data_handler_set (Thumb, 32 bytes, Stack size 16 bytes, app_usbd_core.o(i.app_usbd_core_setup_data_handler_set))
  [Stack]

  - Max Depth = 16
  - Call Chain = app_usbd_core_setup_data_handler_set
  [Calls]
  - >> nrfx_usbd_last_setup_dir_get
  [Called By]
  - >> hid_generic_on_set_report
  - >> app_usbd_core_setup_rsp
  - >> setup_device_req_get_descriptor

  app_usbd_core_setup_rsp (Thumb, 90 bytes, Stack size 32 bytes, app_usbd_core.o(i.app_usbd_core_setup_rsp))
  [Stack]

  - Max Depth = 352
  - Call Chain = app_usbd_core_setup_rsp ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> nrfx_usbd_ep_max_packet_size_get
  - >> app_usbd_core_setup_data_handler_set
  - >> app_usbd_ep_transfer
  [Called By]
  - >> hid_generic_on_get_report
  - >> setup_req_std_in
  - >> setup_event_handler
  - >> setup_interface_req_std_handle
  - >> setup_endpoint_req_std
  - >> setup_device_req_std_handler
  - >> setup_device_req_get_status
  - >> setup_device_req_get_descriptor

  app_usbd_core_setup_transfer_buff_get (Thumb, 10 bytes, Stack size 0 bytes, app_usbd_core.o(i.app_usbd_core_setup_transfer_buff_get))
  [Called By]

  - >> setup_req_std_in
  - >> setup_interface_req_std_handle
  - >> setup_endpoint_req_std
  - >> setup_device_req_std_handler
  - >> setup_device_req_get_status
  - >> setup_device_req_get_descriptor
  - >> app_usbd_prepare_string

  app_usbd_disable (Thumb, 26 bytes, Stack size 8 bytes, app_usbd.o(i.app_usbd_disable))
  [Stack]

  - Max Depth = 384
  - Call Chain = app_usbd_disable ⇒ nrfx_usbd_disable ⇒ nrfx_usbd_stop ⇒ usbd_ep_abort_all ⇒ usbd_ep_abort ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_usbd_is_started
  - >> nrfx_usbd_disable
  [Called By]
  - >> usbd_user_ev_handler

  app_usbd_enable (Thumb, 4 bytes, Stack size 0 bytes, app_usbd.o(i.app_usbd_enable))
  [Stack]

  - Max Depth = 296
  - Call Chain = app_usbd_enable ⇒ nrfx_usbd_enable ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_usbd_enable
  [Called By]
  - >> usbd_user_ev_handler

  app_usbd_ep_call (Thumb, 36 bytes, Stack size 8 bytes, app_usbd.o(i.app_usbd_ep_call))
  [Stack]

  - Max Depth = 288
  - Call Chain = app_usbd_ep_call ⇒ class_event_handler ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> class_event_handler
  - >> app_usbd_ep_conf_access
  [Called By]
  - >> app_usbd_core_setup_req_handler

  app_usbd_ep_disable (Thumb, 4 bytes, Stack size 0 bytes, app_usbd.o(i.app_usbd_ep_disable))
  [Stack]

  - Max Depth = 344
  - Call Chain = app_usbd_ep_disable ⇒ nrfx_usbd_ep_disable ⇒ usbd_ep_abort ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_usbd_ep_disable
  [Called By]
  - >> app_usbd_core_ep0_disable

  app_usbd_ep_enable (Thumb, 34 bytes, Stack size 8 bytes, app_usbd.o(i.app_usbd_ep_enable))
  [Stack]

  - Max Depth = 320
  - Call Chain = app_usbd_ep_enable ⇒ nrfx_usbd_ep_enable ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_usbd_ep_stall_clear
  - >> nrfx_usbd_ep_enable
  - >> nrfx_usbd_ep_dtoggle_clear
  [Called By]
  - >> app_usbd_core_ep0_enable
  - >> app_usbd_iface_select

  app_usbd_ep_handled_transfer (Thumb, 36 bytes, Stack size 16 bytes, app_usbd.o(i.app_usbd_ep_handled_transfer))
  [Stack]

  - Max Depth = 320
  - Call Chain = app_usbd_ep_handled_transfer ⇒ nrfx_usbd_ep_handled_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_usbd_ep_handled_transfer
  - >> nrfx_usbd_ep_enable_check
  [Called By]
  - >> setup_device_req_get_descriptor

  app_usbd_ep_transfer (Thumb, 36 bytes, Stack size 16 bytes, app_usbd.o(i.app_usbd_ep_transfer))
  [Stack]

  - Max Depth = 320
  - Call Chain = app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_usbd_ep_transfer
  - >> nrfx_usbd_ep_enable_check
  [Called By]
  - >> app_usbd_hid_generic_idle_report_set
  - >> hid_generic_transfer_set
  - >> hid_generic_on_set_report
  - >> hid_generic_ep_transfer_out
  - >> app_usbd_core_setup_rsp

  app_usbd_event_execute (Thumb, 556 bytes, Stack size 16 bytes, app_usbd.o(i.app_usbd_event_execute))
  [Stack]

  - Max Depth = 392 + In Cycle
  - Call Chain = app_usbd_event_execute ⇒ app_usbd_event_execute (Cycle)
  [Calls]
  - >> nrf_drv_clock_hfclk_release
  - >> assert_nrf_callback
  - >> nrfx_usbd_wakeup_req
  - >> nrfx_usbd_suspend
  - >> nrfx_usbd_stop
  - >> nrfx_usbd_start
  - >> nrfx_usbd_force_bus_wakeup
  - >> nrfx_usbd_ep_stall
  - >> user_event_state_proc
  - >> sustate_set
  - >> class_event_handler
  - >> app_usbd_sustate_with_requested_hfclk
  - >> app_usbd_ep_conf_access
  - >> app_usbd_core_handler_call
  - >> current_int_priority_get
  - >> app_usbd_core_ep0_enable
  - >> app_usbd_core_ep0_disable
  - >> app_usbd_event_execute
  - >> app_usbd_all_iface_deselect
  - >> app_usbd_all_call
  [Called By]
  - >> usbd_core_state_set
  - >> app_usbd_event_execute
  [Address Reference Count : 2]
  - app_usbd.o(i.app_usbd_init)
  - app_usbd.o(.constdata)

  app_usbd_hid_event_handler (Thumb, 318 bytes, Stack size 24 bytes, app_usbd_hid.o(i.app_usbd_hid_event_handler))
  [Stack]

  - Max Depth = 432
  - Call Chain = app_usbd_hid_event_handler ⇒ setup_event_handler ⇒ setup_req_std_in ⇒ app_usbd_core_setup_rsp ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> user_event_handler
  - >> setup_event_handler
  - >> hid_sof_required
  - >> endpoint_in_event_handler
  - >> app_usbd_hid_state_flag_set
  - >> app_usbd_hid_state_flag_clr
  - >> app_usbd_clear_idle_ctx
  - >> app_usbd_class_sof_unregister
  - >> app_usbd_class_sof_register
  - >> app_usbd_class_rwu_unregister
  - >> app_usbd_class_rwu_register
  [Called By]
  - >> hid_generic_event_handler

  app_usbd_hid_generic_idle_report_set (Thumb, 72 bytes, Stack size 32 bytes, app_usbd_hid_generic.o(i.app_usbd_hid_generic_idle_report_set))
  [Stack]

  - Max Depth = 352
  - Call Chain = app_usbd_hid_generic_idle_report_set ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> hid_generic_ctx_get
  - >> app_usbd_hid_state_flag_set
  - >> app_usbd_hid_state_flag_clr
  - >> app_usbd_hid_epin_addr_get
  - >> app_usbd_ep_transfer
  [Called By]
  - >> idle_handle

  app_usbd_hid_generic_in_report_get (Thumb, 12 bytes, Stack size 0 bytes, app_usbd_hid_generic.o(i.app_usbd_hid_generic_in_report_get))
  [Called By]

  - >> hid_generic_on_get_report

  app_usbd_hid_generic_in_report_set (Thumb, 94 bytes, Stack size 32 bytes, app_usbd_hid_generic.o(i.app_usbd_hid_generic_in_report_set))
  [Stack]

  - Max Depth = 384
  - Call Chain = app_usbd_hid_generic_in_report_set ⇒ hid_generic_transfer_set ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_queue_push
  - >> hid_generic_transfer_set
  - >> hid_generic_ctx_get
  - >> app_usbd_wakeup_req
  [Called By]
  - >> hid_generic_mouse_process_state

  app_usbd_hid_generic_out_report_get (Thumb, 12 bytes, Stack size 0 bytes, app_usbd_hid_generic.o(i.app_usbd_hid_generic_out_report_get))
  [Called By]

  - >> hid_generic_on_get_report

  app_usbd_hid_rep_buff_in_get (Thumb, 20 bytes, Stack size 8 bytes, app_usbd_hid.o(i.app_usbd_hid_rep_buff_in_get))
  [Stack]

  - Max Depth = 272
  - Call Chain = app_usbd_hid_rep_buff_in_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> hid_generic_rep_buffer_get

  app_usbd_iface_call (Thumb, 6 bytes, Stack size 0 bytes, app_usbd.o(i.app_usbd_iface_call))
  [Stack]

  - Max Depth = 280
  - Call Chain = app_usbd_iface_call ⇒ class_event_handler ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> class_event_handler
  [Called By]
  - >> app_usbd_core_setup_req_handler

  app_usbd_iface_deselect (Thumb, 72 bytes, Stack size 16 bytes, app_usbd.o(i.app_usbd_iface_deselect))
  [Stack]

  - Max Depth = 360
  - Call Chain = app_usbd_iface_deselect ⇒ nrfx_usbd_ep_disable ⇒ usbd_ep_abort ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_usbd_ep_disable
  - >> app_usbd_class_iface_get
  - >> app_usbd_class_iface_ep_get
  [Called By]
  - >> app_usbd_all_iface_deselect

  app_usbd_iface_find (Thumb, 68 bytes, Stack size 24 bytes, app_usbd.o(i.app_usbd_iface_find))
  [Stack]

  - Max Depth = 304
  - Call Chain = app_usbd_iface_find ⇒ app_usbd_class_iface_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_usbd_class_next_get
  - >> app_usbd_class_iface_get
  [Called By]
  - >> app_usbd_core_setup_req_handler

  app_usbd_iface_select (Thumb, 86 bytes, Stack size 16 bytes, app_usbd.o(i.app_usbd_iface_select))
  [Stack]

  - Max Depth = 336
  - Call Chain = app_usbd_iface_select ⇒ app_usbd_ep_enable ⇒ nrfx_usbd_ep_enable ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_usbd_class_iface_get
  - >> app_usbd_class_iface_ep_get
  - >> app_usbd_ep_enable
  [Called By]
  - >> setup_interface_req_std_handle
  - >> app_usbd_all_iface_select_0

  app_usbd_iface_selection_get (Thumb, 18 bytes, Stack size 0 bytes, app_usbd.o(i.app_usbd_iface_selection_get))
  [Called By]

  - >> setup_interface_req_std_handle

  app_usbd_init (Thumb, 202 bytes, Stack size 32 bytes, app_usbd.o(i.app_usbd_init))
  [Stack]

  - Max Depth = 352
  - Call Chain = app_usbd_init ⇒ nrfx_usbd_init ⇒ nrfx_usbd_ep_max_packet_size_set ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_drv_power_init
  - >> nrf_drv_clock_init_check
  - >> assert_nrf_callback
  - >> app_error_handler
  - >> nrfx_usbd_uninit
  - >> nrfx_usbd_init
  - >> class_event_handler
  - >> app_usbd_ep_instance_set
  - >> app_usbd_class_iface_get
  - >> app_usbd_class_iface_ep_get
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  app_usbd_power_events_enable (Thumb, 40 bytes, Stack size 8 bytes, app_usbd.o(i.app_usbd_power_events_enable))
  [Stack]

  - Max Depth = 256
  - Call Chain = app_usbd_power_events_enable ⇒ app_error_handler ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_drv_power_usbevt_init
  - >> nrfx_usbd_is_enabled
  - >> app_error_handler
  - >> nrfx_usbd_is_initialized
  [Called By]
  - >> main

  app_usbd_start (Thumb, 48 bytes, Stack size 8 bytes, app_usbd.o(i.app_usbd_start))
  [Stack]

  - Max Depth = 272
  - Call Chain = app_usbd_start ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_usbd_is_enabled
  - >> assert_nrf_callback
  - >> app_usbd_event_add
  [Called By]
  - >> usbd_user_ev_handler

  app_usbd_stop (Thumb, 16 bytes, Stack size 8 bytes, app_usbd.o(i.app_usbd_stop))
  [Stack]

  - Max Depth = 8
  - Call Chain = app_usbd_stop
  [Calls]
  - >> app_usbd_event_add
  [Called By]
  - >> usbd_user_ev_handler

  app_usbd_string_desc_get (Thumb, 38 bytes, Stack size 0 bytes, app_usbd_string_desc.o(i.app_usbd_string_desc_get))
  [Stack]

  - Max Depth = 288
  - Call Chain = app_usbd_string_desc_get ⇒ app_usbd_prepare_string ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_usbd_prepare_string
  [Called By]
  - >> setup_device_req_get_descriptor

  app_usbd_suspend_req (Thumb, 16 bytes, Stack size 8 bytes, app_usbd.o(i.app_usbd_suspend_req))
  [Stack]

  - Max Depth = 8
  - Call Chain = app_usbd_suspend_req
  [Calls]
  - >> app_usbd_event_add
  [Called By]
  - >> usbd_user_ev_handler

  app_usbd_wakeup_req (Thumb, 44 bytes, Stack size 8 bytes, app_usbd.o(i.app_usbd_wakeup_req))
  [Stack]

  - Max Depth = 272
  - Call Chain = app_usbd_wakeup_req ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_usbd_event_add
  - >> app_usbd_core_feature_state_get
  - >> app_usbd_class_rwu_enabled_check
  [Called By]
  - >> app_usbd_hid_generic_in_report_set

  app_util_critical_region_enter (Thumb, 26 bytes, Stack size 8 bytes, app_util_platform.o(i.app_util_critical_region_enter))
  [Stack]

  - Max Depth = 8 + In Cycle
  - Call Chain = app_util_critical_region_enter ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> privilege_level_get
  - >> app_util_disable_irq
  [Called By]
  - >> nrf_drv_clock_hfclk_release
  - >> nrf_log_frontend_dequeue
  - >> nrf_drv_clock_lfclk_request
  - >> nrf_drv_clock_hfclk_request
  - >> hid_generic_clear_buffer
  - >> app_usbd_hid_generic_idle_report_set
  - >> app_timer_start
  - >> hid_generic_mouse_process_state
  - >> hid_generic_mouse_action
  - >> nrfx_prs_acquire
  - >> nrfx_usbd_wakeup_req
  - >> nrfx_usbd_transfer_out_drop
  - >> nrfx_usbd_suspend
  - >> nrfx_usbd_ep_transfer
  - >> nrfx_usbd_ep_handled_transfer
  - >> nrfx_usbd_ep_enable
  - >> nrfx_usbd_enable
  - >> usbd_ep_abort
  - >> timer_stop_op_schedule
  - >> nrf_queue_push
  - >> nrf_queue_generic_pop
  - >> hid_generic_transfer_set
  - >> hid_generic_on_set_report
  - >> app_usbd_core_setup_rsp
  - >> setup_device_req_get_descriptor
  - >> nrf_balloc_free
  - >> nrf_balloc_alloc
  - >> buf_prealloc
  - >> nrf_queue_utilization_get

  app_util_critical_region_exit (Thumb, 26 bytes, Stack size 8 bytes, app_util_platform.o(i.app_util_critical_region_exit))
  [Stack]

  - Max Depth = 8 + In Cycle
  - Call Chain = app_util_critical_region_exit ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> privilege_level_get
  - >> app_util_enable_irq
  [Called By]
  - >> nrf_drv_clock_hfclk_release
  - >> nrf_log_frontend_dequeue
  - >> nrf_drv_clock_lfclk_request
  - >> nrf_drv_clock_hfclk_request
  - >> hid_generic_clear_buffer
  - >> app_usbd_hid_generic_idle_report_set
  - >> app_timer_start
  - >> hid_generic_mouse_process_state
  - >> hid_generic_mouse_action
  - >> nrfx_prs_acquire
  - >> nrfx_usbd_wakeup_req
  - >> nrfx_usbd_transfer_out_drop
  - >> nrfx_usbd_suspend
  - >> nrfx_usbd_ep_transfer
  - >> nrfx_usbd_ep_handled_transfer
  - >> nrfx_usbd_ep_enable
  - >> nrfx_usbd_enable
  - >> usbd_ep_abort
  - >> timer_stop_op_schedule
  - >> nrf_queue_push
  - >> nrf_queue_generic_pop
  - >> hid_generic_transfer_set
  - >> hid_generic_on_set_report
  - >> app_usbd_core_setup_rsp
  - >> setup_device_req_get_descriptor
  - >> nrf_balloc_free
  - >> nrf_balloc_alloc
  - >> buf_prealloc
  - >> nrf_queue_utilization_get

  app_util_disable_irq (Thumb, 12 bytes, Stack size 0 bytes, app_util_platform.o(i.app_util_disable_irq))
  [Called By]

  - >> app_util_critical_region_enter

  app_util_enable_irq (Thumb, 14 bytes, Stack size 0 bytes, app_util_platform.o(i.app_util_enable_irq))
  [Called By]

  - >> app_util_critical_region_exit

  assert_nrf_callback (Thumb, 22 bytes, Stack size 16 bytes, nrf_assert.o(i.assert_nrf_callback))
  [Stack]

  - Max Depth = 264
  - Call Chain = assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_error_fault_handler
  [Called By]
  - >> nrfx_uarte_init
  - >> nrfx_uart_init
  - >> nrf_drv_uart_init
  - >> nrfx_power_init
  - >> nrfx_clock_lfclk_start
  - >> nrfx_clock_init
  - >> nrfx_clock_hfclk_stop
  - >> nrfx_clock_hfclk_start
  - >> nrfx_clock_enable
  - >> nrf_drv_clock_hfclk_release
  - >> cmd_evt
  - >> cmd_btn
  - >> app_button_enable
  - >> bsp_board_led_state_get
  - >> bsp_board_led_off
  - >> bsp_board_button_state_get
  - >> nrf_gpio_pin_port_decode
  - >> nrf_drv_clock_lfclk_request
  - >> nrf_drv_clock_lfclk_is_running
  - >> nrf_drv_clock_hfclk_request
  - >> nrf_cli_start
  - >> nrf_cli_process
  - >> nrf_cli_init
  - >> hid_generic_idle_handler_set
  - >> hid_generic_clear_buffer
  - >> bsp_board_led_on
  - >> bsp_board_led_invert
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> app_usbd_start
  - >> app_usbd_init
  - >> app_usbd_disable
  - >> app_usbd_class_append
  - >> hid_user_ev_handler
  - >> nrf_gpio_pin_port_decode
  - >> interrupts_enable
  - >> nrfx_systick_delay_us
  - >> nrfx_systick_delay_ticks
  - >> nrfx_prs_release
  - >> nrfx_prs_acquire
  - >> UARTE0_UART0_IRQHandler
  - >> nrfx_power_irq_handler
  - >> nrfx_gpiote_in_is_set
  - >> nrfx_gpiote_in_init
  - >> nrfx_gpiote_in_event_enable
  - >> nrf_gpio_ports_read
  - >> nrf_gpio_pin_port_decode
  - >> nrfx_usbd_uninit
  - >> nrfx_usbd_transfer_out_drop
  - >> nrfx_usbd_stop
  - >> nrfx_usbd_start
  - >> nrfx_usbd_init
  - >> nrfx_usbd_feeder_ram_zlp
  - >> nrfx_usbd_feeder_ram
  - >> nrfx_usbd_feeder_flash_zlp
  - >> nrfx_usbd_feeder_flash
  - >> nrfx_usbd_ep_transfer
  - >> nrfx_usbd_ep_stall_clear
  - >> nrfx_usbd_ep_stall
  - >> nrfx_usbd_ep_max_packet_size_set
  - >> nrfx_usbd_ep_handled_transfer
  - >> nrfx_usbd_ep_enable
  - >> nrfx_usbd_ep_dtoggle_clear
  - >> nrfx_usbd_ep_disable
  - >> nrfx_usbd_enable
  - >> nrfx_usbd_disable
  - >> nrfx_usbd_consumer
  - >> usbd_dmareq_process
  - >> usbd_dma_start
  - >> nrfx_usbd_ep_to_int
  - >> nrfx_usbd_ep_to_endevent
  - >> nrf_usbd_epout_size_get
  - >> nrf_usbd_epout_dma_handler
  - >> nrf_usbd_episoout_size_get
  - >> nrf_usbd_epiniso_dma_handler
  - >> nrf_usbd_epin_dma_handler
  - >> nrf_usbd_ep_enable_check
  - >> ev_usbevent_handler
  - >> ep_to_hal
  - >> ep_state_access
  - >> ep2bit
  - >> nrfx_uarte_tx
  - >> nrfx_uarte_rx
  - >> nrf_gpio_pin_port_decode
  - >> interrupts_enable
  - >> nrfx_uart_tx
  - >> nrfx_uart_rx
  - >> class_event_handler
  - >> app_usbd_power_event_handler
  - >> app_usbd_hfclk_ready
  - >> app_usbd_ep_instance_set
  - >> app_usbd_ep_conf_access
  - >> app_usbd_class_next_get
  - >> app_usbd_class_iface_get
  - >> app_usbd_class_iface_ep_get
  - >> nrf_queue_push
  - >> nrf_queue_is_empty
  - >> nrf_queue_generic_pop
  - >> hid_generic_transfer_set
  - >> hid_generic_rep_buffer_get
  - >> hid_generic_get
  - >> hid_generic_feed_descriptors
  - >> hid_generic_event_handler
  - >> hid_generic_ctx_get
  - >> app_usbd_hid_rep_buff_out_get
  - >> app_usbd_class_iface_get
  - >> app_usbd_class_iface_ep_get
  - >> app_usbd_hid_rep_buff_in_get
  - >> app_usbd_hid_event_handler
  - >> setup_req_std_in
  - >> setup_event_handler
  - >> usbd_descriptor_conf_feeder
  - >> setup_device_req_std_handler
  - >> setup_device_req_get_status
  - >> setup_device_req_get_descriptor
  - >> app_usbd_core_event_handler
  - >> app_usbd_class_next_get
  - >> app_usbd_wakeup_req
  - >> app_usbd_iface_select
  - >> app_usbd_iface_deselect
  - >> app_usbd_event_execute
  - >> app_usbd_class_sof_unregister
  - >> app_usbd_class_sof_register
  - >> app_usbd_class_rwu_unregister
  - >> app_usbd_class_rwu_register
  - >> app_usbd_all_iface_select_0
  - >> completion_insert
  - >> cmd_get
  - >> cli_write
  - >> cli_transport_evt_handler
  - >> cli_read
  - >> cli_execute
  - >> cli_cursor_save
  - >> cli_cursor_restore
  - >> cli_clear_eos
  - >> char_delete
  - >> nrf_cli_help_print
  - >> nrf_cli_fprintf
  - >> nrf_balloc_init
  - >> nrf_balloc_free
  - >> nrf_balloc_alloc
  - >> nrf_balloc_status
  - >> app_usbd_prepare_string
  - >> std_n
  - >> log_skip
  - >> nrf_queue_utilization_get
  - >> nrf_queue_is_full
  - >> nrf_queue_next_idx
  - >> memobj_op
  - >> nrf_ringbuf_get
  - >> nrf_ringbuf_cpy_put
  - >> nrf_ringbuf_cpy_get
  - >> nrf_ringbuf_alloc
  - >> uart_event_handler
  - >> rx_try
  - >> cli_uart_write
  - >> cli_uart_read
  - >> nrf_queue_max_utilization_reset
  - >> nrf_queue_max_utilization_get
  - >> nrf_memobj_write
  - >> nrf_memobj_read
  - >> nrf_fprintf_fmt
  - >> nrf_fprintf_buffer_flush
  - >> nrf_fprintf
  - >> terminal_size_get
  - >> string_cmp
  - >> nrf_cli_instance_init
  - >> nrf_cli_cmd_resize_default
  - >> nrf_cli_cmd_resize
  - >> nrf_cli_cmd_history
  - >> nrf_cli_cmd_colors
  - >> nrf_cli_cmd_cli
  - >> nrf_cli_cmd_clear
  - >> make_argv
  - >> history_list_element_add

  bsp_board_button_state_get (Thumb, 50 bytes, Stack size 16 bytes, boards.o(i.bsp_board_button_state_get))
  [Stack]

  - Max Depth = 288
  - Call Chain = bsp_board_button_state_get ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_pin_port_decode
  - >> assert_nrf_callback
  [Called By]
  - >> bsp_button_is_pressed

  bsp_board_init (Thumb, 80 bytes, Stack size 32 bytes, boards.o(i.bsp_board_init))
  [Stack]

  - Max Depth = 344
  - Call Chain = bsp_board_init ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_cfg
  - >> bsp_board_leds_off
  [Called By]
  - >> bsp_init
  - >> init_bsp

  bsp_board_led_invert (Thumb, 54 bytes, Stack size 16 bytes, boards.o(i.bsp_board_led_invert))
  [Stack]

  - Max Depth = 288
  - Call Chain = bsp_board_led_invert ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_pin_port_decode
  - >> assert_nrf_callback
  [Called By]
  - >> bsp_led_indication
  - >> alert_timer_handler
  - >> hid_user_ev_handler

  bsp_board_led_off (Thumb, 30 bytes, Stack size 8 bytes, boards.o(i.bsp_board_led_off))
  [Stack]

  - Max Depth = 296
  - Call Chain = bsp_board_led_off ⇒ nrf_gpio_pin_write ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_pin_write
  - >> assert_nrf_callback
  [Called By]
  - >> leds_off
  - >> bsp_led_indication
  - >> bsp_board_leds_off

  bsp_board_led_on (Thumb, 30 bytes, Stack size 8 bytes, boards.o(i.bsp_board_led_on))
  [Stack]

  - Max Depth = 296
  - Call Chain = bsp_board_led_on ⇒ nrf_gpio_pin_write ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_pin_write
  - >> assert_nrf_callback
  [Called By]
  - >> bsp_led_indication
  - >> bsp_board_leds_on
  - >> usbd_user_ev_handler

  bsp_board_led_state_get (Thumb, 50 bytes, Stack size 16 bytes, boards.o(i.bsp_board_led_state_get))
  [Stack]

  - Max Depth = 288
  - Call Chain = bsp_board_led_state_get ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_pin_port_decode
  - >> assert_nrf_callback
  [Called By]
  - >> bsp_led_indication

  bsp_board_leds_off (Thumb, 18 bytes, Stack size 8 bytes, boards.o(i.bsp_board_leds_off))
  [Stack]

  - Max Depth = 304
  - Call Chain = bsp_board_leds_off ⇒ bsp_board_led_off ⇒ nrf_gpio_pin_write ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> bsp_board_led_off
  [Called By]
  - >> leds_off
  - >> bsp_board_init
  - >> usbd_user_ev_handler

  bsp_board_leds_on (Thumb, 18 bytes, Stack size 8 bytes, boards.o(i.bsp_board_leds_on))
  [Stack]

  - Max Depth = 304
  - Call Chain = bsp_board_leds_on ⇒ bsp_board_led_on ⇒ nrf_gpio_pin_write ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> bsp_board_led_on
  [Called By]
  - >> bsp_led_indication

  bsp_board_pin_to_button_idx (Thumb, 30 bytes, Stack size 8 bytes, boards.o(i.bsp_board_pin_to_button_idx))
  [Stack]

  - Max Depth = 8
  - Call Chain = bsp_board_pin_to_button_idx
  [Called By]
  - >> bsp_button_event_handler

  bsp_button_is_pressed (Thumb, 12 bytes, Stack size 0 bytes, bsp.o(i.bsp_button_is_pressed))
  [Stack]

  - Max Depth = 288
  - Call Chain = bsp_button_is_pressed ⇒ bsp_board_button_state_get ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> bsp_board_button_state_get
  [Called By]
  - >> mouse_move_timer_handler

  bsp_cli_init (Thumb, 8 bytes, Stack size 0 bytes, bsp_cli.o(i.bsp_cli_init))
  [Called By]

  - >> init_cli

  bsp_event_to_button_action_assign (Thumb, 64 bytes, Stack size 16 bytes, bsp.o(i.bsp_event_to_button_action_assign))
  [Stack]

  - Max Depth = 16
  - Call Chain = bsp_event_to_button_action_assign
  [Called By]
  - >> bsp_init
  - >> init_bsp

  bsp_init (Thumb, 128 bytes, Stack size 16 bytes, bsp.o(i.bsp_init))
  [Stack]

  - Max Depth = 384
  - Call Chain = bsp_init ⇒ app_button_init ⇒ nrfx_gpiote_in_init ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_button_init
  - >> app_button_enable
  - >> bsp_event_to_button_action_assign
  - >> bsp_board_init
  - >> app_timer_create
  [Called By]
  - >> init_bsp

  buffer_is_empty (Thumb, 16 bytes, Stack size 0 bytes, nrf_log_frontend.o(i.buffer_is_empty))
  [Called By]

  - >> nrf_log_frontend_dequeue

  current_int_priority_get (Thumb, 48 bytes, Stack size 0 bytes, app_util_platform.o(i.current_int_priority_get))
  [Called By]

  - >> app_usbd_event_execute

  hid_generic_clear_buffer (Thumb, 164 bytes, Stack size 40 bytes, app_usbd_hid_generic.o(i.hid_generic_clear_buffer))
  [Stack]

  - Max Depth = 368
  - Call Chain = hid_generic_clear_buffer ⇒ nrfx_usbd_ep_abort ⇒ usbd_ep_abort ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> nrfx_usbd_ep_abort
  - >> nrf_queue_generic_pop
  - >> hid_generic_rep_buffer_get
  - >> hid_generic_get
  - >> hid_generic_ctx_get
  - >> app_usbd_hid_state_flag_clr
  - >> app_usbd_class_iface_get
  - >> app_usbd_class_iface_ep_get
  [Called By]
  - >> hid_user_ev_handler

  hid_generic_idle_handler_set (Thumb, 34 bytes, Stack size 16 bytes, app_usbd_hid_generic.o(i.hid_generic_idle_handler_set))
  [Stack]

  - Max Depth = 288
  - Call Chain = hid_generic_idle_handler_set ⇒ hid_generic_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> hid_generic_get
  - >> hid_generic_ctx_get
  [Called By]
  - >> main
  [Address Reference Count : 1]
  - app_usbd_hid_generic.o(.constdata)

  main (Thumb, 246 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 768
  - Call Chain = main ⇒ nrf_cli_process ⇒ cli_state_collect ⇒ cli_tab_handle ⇒ option_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_log_init
  - >> nrf_log_frontend_std_0
  - >> nrf_log_frontend_dequeue
  - >> nrf_drv_clock_lfclk_request
  - >> nrf_drv_clock_lfclk_is_running
  - >> nrf_drv_clock_init
  - >> nrf_drv_clock_hfclk_request
  - >> nrf_cli_process
  - >> hid_generic_idle_handler_set
  - >> app_usbd_power_events_enable
  - >> app_usbd_init
  - >> app_usbd_class_append
  - >> app_timer_init
  - >> app_timer_create
  - >> app_error_handler
  - >> init_cli
  - >> init_bsp
  - >> hid_generic_mouse_process_state
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  nrf_atomic_flag_clear (Thumb, 6 bytes, Stack size 0 bytes, nrf_atomic.o(i.nrf_atomic_flag_clear))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_atomic_flag_clear ⇒ nrf_atomic_u32_and
  [Calls]
  - >> nrf_atomic_u32_and
  [Called By]
  - >> nrf_ringbuf_get
  - >> nrf_ringbuf_free
  - >> nrf_ringbuf_cpy_put
  - >> nrf_ringbuf_cpy_get
  - >> nrf_ringbuf_alloc

  nrf_atomic_flag_clear_fetch (Thumb, 6 bytes, Stack size 0 bytes, nrf_atomic.o(i.nrf_atomic_flag_clear_fetch))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_atomic_flag_clear_fetch ⇒ nrf_atomic_u32_fetch_and
  [Calls]
  - >> nrf_atomic_u32_fetch_and
  [Called By]
  - >> app_usbd_core_event_handler
  - >> log_skip
  - >> nrf_ringbuf_put

  nrf_atomic_flag_set (Thumb, 6 bytes, Stack size 0 bytes, nrf_atomic.o(i.nrf_atomic_flag_set))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_atomic_flag_set ⇒ nrf_atomic_u32_or
  [Calls]
  - >> nrf_atomic_u32_or
  [Called By]
  - >> log_skip

  nrf_atomic_flag_set_fetch (Thumb, 6 bytes, Stack size 0 bytes, nrf_atomic.o(i.nrf_atomic_flag_set_fetch))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_atomic_flag_set_fetch ⇒ nrf_atomic_u32_fetch_or
  [Calls]
  - >> nrf_atomic_u32_fetch_or
  [Called By]
  - >> nrf_ringbuf_get
  - >> nrf_ringbuf_cpy_put
  - >> nrf_ringbuf_cpy_get
  - >> nrf_ringbuf_alloc

  nrf_atomic_u32_add (Thumb, 12 bytes, Stack size 8 bytes, nrf_atomic.o(i.nrf_atomic_u32_add))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_atomic_u32_add
  [Calls]
  - >> __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_add
  [Called By]
  - >> buf_prealloc
  - >> nrf_memobj_get

  nrf_atomic_u32_and (Thumb, 12 bytes, Stack size 8 bytes, nrf_atomic.o(i.nrf_atomic_u32_and))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_atomic_u32_and
  [Calls]
  - >> __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_and
  [Called By]
  - >> nrf_cli_process
  - >> nrf_atomic_flag_clear
  - >> app_usbd_hid_state_flag_clr
  - >> app_usbd_hid_state_flag_clr

  nrf_atomic_u32_fetch_and (Thumb, 10 bytes, Stack size 8 bytes, nrf_atomic.o(i.nrf_atomic_u32_fetch_and))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_atomic_u32_fetch_and
  [Calls]
  - >> __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_and
  [Called By]
  - >> nrf_atomic_flag_clear_fetch

  nrf_atomic_u32_fetch_or (Thumb, 10 bytes, Stack size 8 bytes, nrf_atomic.o(i.nrf_atomic_u32_fetch_or))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_atomic_u32_fetch_or
  [Calls]
  - >> __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_orr
  [Called By]
  - >> nrf_atomic_flag_set_fetch

  nrf_atomic_u32_fetch_store (Thumb, 10 bytes, Stack size 8 bytes, nrf_atomic.o(i.nrf_atomic_u32_fetch_store))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_atomic_u32_fetch_store
  [Calls]
  - >> __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_mov
  [Called By]
  - >> dropped_sat16_get

  nrf_atomic_u32_or (Thumb, 12 bytes, Stack size 8 bytes, nrf_atomic.o(i.nrf_atomic_u32_or))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_atomic_u32_or
  [Calls]
  - >> __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_orr
  [Called By]
  - >> nrf_cli_process
  - >> nrf_atomic_flag_set
  - >> app_usbd_hid_state_flag_set
  - >> app_usbd_hid_state_flag_set

  nrf_atomic_u32_sub (Thumb, 12 bytes, Stack size 8 bytes, nrf_atomic.o(i.nrf_atomic_u32_sub))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_atomic_u32_sub
  [Calls]
  - >> __asm___12_nrf_atomic_c_85ca2469__nrf_atomic_internal_sub
  [Called By]
  - >> nrf_memobj_put

  nrf_balloc_alloc (Thumb, 86 bytes, Stack size 16 bytes, nrf_balloc.o(i.nrf_balloc_alloc))
  [Stack]

  - Max Depth = 24 + In Cycle
  - Call Chain = nrf_balloc_alloc ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  [Called By]
  - >> nrf_memobj_alloc

  nrf_balloc_free (Thumb, 76 bytes, Stack size 16 bytes, nrf_balloc.o(i.nrf_balloc_free))
  [Stack]

  - Max Depth = 24 + In Cycle
  - Call Chain = nrf_balloc_free ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  [Called By]
  - >> nrf_memobj_free

  nrf_balloc_init (Thumb, 118 bytes, Stack size 8 bytes, nrf_balloc.o(i.nrf_balloc_init))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrf_balloc_init ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrf_memobj_pool_init

  nrf_cli_cmd_cli_stats (Thumb, 70 bytes, Stack size 16 bytes, nrf_cli.o(i.nrf_cli_cmd_cli_stats))
  [Stack]

  - Max Depth = 608
  - Call Chain = nrf_cli_cmd_cli_stats ⇒ nrf_cli_build_in_cmd_common_executed ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_help_print
  - >> nrf_cli_fprintf
  - >> nrf_cli_build_in_cmd_common_executed
  [Address Reference Count : 1]
  - nrf_cli.o(.constdata)

  nrf_cli_cmd_cli_stats_reset (Thumb, 48 bytes, Stack size 8 bytes, nrf_cli.o(i.nrf_cli_cmd_cli_stats_reset))
  [Stack]

  - Max Depth = 600
  - Call Chain = nrf_cli_cmd_cli_stats_reset ⇒ nrf_cli_build_in_cmd_common_executed ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_queue_max_utilization_reset
  - >> nrf_cli_build_in_cmd_common_executed
  [Address Reference Count : 1]
  - nrf_cli.o(.constdata)

  nrf_cli_cmd_cli_stats_show (Thumb, 78 bytes, Stack size 24 bytes, nrf_cli.o(i.nrf_cli_cmd_cli_stats_show))
  [Stack]

  - Max Depth = 616
  - Call Chain = nrf_cli_cmd_cli_stats_show ⇒ nrf_cli_build_in_cmd_common_executed ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_fprintf
  - >> nrf_queue_max_utilization_get
  - >> nrf_cli_build_in_cmd_common_executed
  [Address Reference Count : 1]
  - nrf_cli.o(.constdata)

  nrf_cli_fprintf (Thumb, 132 bytes, Stack size 40 bytes, nrf_cli.o(i.nrf_cli_fprintf))
  [Stack]

  - Max Depth = 504
  - Call Chain = nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_fprintf_fmt
  - >> vt100_color_set
  - >> vt100_bgcolor_set
  [Called By]
  - >> nrf_cli_process
  - >> completion_insert
  - >> cli_tab_handle
  - >> cli_state_set
  - >> cli_log_entry_process
  - >> cli_execute
  - >> char_insert
  - >> char_delete
  - >> char_backspace
  - >> nrf_cli_help_print
  - >> nrf_balloc_status
  - >> nrf_cli_backend_cmd_execute
  - >> log_status
  - >> log_ctrl
  - >> log_config_store_cmd
  - >> log_config_load_cmd
  - >> log_cmd_backends_list
  - >> log_cmd
  - >> nrf_queue_status
  - >> nrf_cli_cmd_cli_stats_show
  - >> nrf_cli_cmd_cli_stats
  - >> option_print
  - >> nrf_cli_cmd_resize
  - >> nrf_cli_cmd_history
  - >> nrf_cli_cmd_echo
  - >> nrf_cli_cmd_colors
  - >> nrf_cli_cmd_cli
  - >> nrf_cli_build_in_cmd_common_executed
  - >> history_handle

  nrf_cli_help_print (Thumb, 584 bytes, Stack size 72 bytes, nrf_cli.o(i.nrf_cli_help_print))
  [Stack]

  - Max Depth = 576
  - Call Chain = nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> cmd_get
  - >> cli_strlen
  - >> nrf_cli_fprintf
  - >> nrf_fprintf
  - >> format_offset_string_print
  - >> cursor_right_move
  - >> cursor_next_line_move
  [Called By]
  - >> nrf_balloc_status
  - >> log_config_store_cmd
  - >> log_config_load_cmd
  - >> log_cmd_backends_list
  - >> log_cmd
  - >> nrf_queue_status
  - >> nrf_cli_cmd_cli_stats
  - >> nrf_cli_cmd_colors
  - >> nrf_cli_cmd_cli
  - >> nrf_cli_cmd_clear
  - >> nrf_cli_build_in_cmd_common_executed

  nrf_cli_init (Thumb, 74 bytes, Stack size 24 bytes, nrf_cli.o(i.nrf_cli_init))
  [Stack]

  - Max Depth = 328
  - Call Chain = nrf_cli_init ⇒ nrf_cli_instance_init ⇒ nrf_memobj_pool_init ⇒ nrf_balloc_init ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_log_backend_add
  - >> nrf_cli_instance_init
  [Called By]
  - >> init_cli

  nrf_cli_print_stream (Thumb, 6 bytes, Stack size 0 bytes, nrf_cli.o(i.nrf_cli_print_stream))
  [Stack]

  - Max Depth = 296
  - Call Chain = nrf_cli_print_stream ⇒ cli_write ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> cli_write
  [Address Reference Count : 1]
  - main.o(.data)

  nrf_cli_process (Thumb, 144 bytes, Stack size 8 bytes, nrf_cli.o(i.nrf_cli_process))
  [Stack]

  - Max Depth = 768
  - Call Chain = nrf_cli_process ⇒ cli_state_collect ⇒ cli_tab_handle ⇒ option_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_atomic_u32_or
  - >> nrf_atomic_u32_and
  - >> cli_state_collect
  - >> cli_log_entry_process
  - >> cli_flag_echo_is_set
  - >> nrf_cli_fprintf
  - >> nrf_fprintf_buffer_flush
  - >> cursor_position_synchronize
  [Called By]
  - >> main

  nrf_cli_start (Thumb, 100 bytes, Stack size 16 bytes, nrf_cli.o(i.nrf_cli_start))
  [Stack]

  - Max Depth = 520
  - Call Chain = nrf_cli_start ⇒ cli_state_set ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> cli_state_set
  - >> nrf_fprintf
  - >> vt100_color_set
  - >> vt100_bgcolor_set
  [Called By]
  - >> init_cli

  nrf_drv_clock_hfclk_release (Thumb, 66 bytes, Stack size 8 bytes, nrf_drv_clock.o(i.nrf_drv_clock_hfclk_release))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrf_drv_clock_hfclk_release ⇒ nrfx_clock_hfclk_stop ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_clock_hfclk_stop
  - >> assert_nrf_callback
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  [Called By]
  - >> sustate_set
  - >> app_usbd_event_execute

  nrf_drv_clock_hfclk_request (Thumb, 100 bytes, Stack size 16 bytes, nrf_drv_clock.o(i.nrf_drv_clock_hfclk_request))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrf_drv_clock_hfclk_request ⇒ nrfx_clock_hfclk_start ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_clock_hfclk_start
  - >> item_enqueue
  - >> assert_nrf_callback
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  [Called By]
  - >> main
  - >> sustate_set

  nrf_drv_clock_init (Thumb, 42 bytes, Stack size 16 bytes, nrf_drv_clock.o(i.nrf_drv_clock_init))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrf_drv_clock_init ⇒ nrfx_clock_init ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_clock_init
  - >> nrfx_clock_enable
  [Called By]
  - >> main

  nrf_drv_clock_init_check (Thumb, 6 bytes, Stack size 0 bytes, nrf_drv_clock.o(i.nrf_drv_clock_init_check))
  [Called By]

  - >> app_usbd_init

  nrf_drv_clock_lfclk_is_running (Thumb, 28 bytes, Stack size 8 bytes, nrf_drv_clock.o(i.nrf_drv_clock_lfclk_is_running))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrf_drv_clock_lfclk_is_running ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> main

  nrf_drv_clock_lfclk_request (Thumb, 98 bytes, Stack size 16 bytes, nrf_drv_clock.o(i.nrf_drv_clock_lfclk_request))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrf_drv_clock_lfclk_request ⇒ nrfx_clock_lfclk_start ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_clock_lfclk_start
  - >> item_enqueue
  - >> assert_nrf_callback
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  [Called By]
  - >> main

  nrf_drv_power_init (Thumb, 30 bytes, Stack size 8 bytes, nrf_drv_power.o(i.nrf_drv_power_init))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrf_drv_power_init ⇒ nrfx_power_init ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_power_init
  [Called By]
  - >> app_usbd_init

  nrf_drv_power_usbevt_init (Thumb, 22 bytes, Stack size 8 bytes, nrf_drv_power.o(i.nrf_drv_power_usbevt_init))
  [Stack]

  - Max Depth = 16
  - Call Chain = nrf_drv_power_usbevt_init ⇒ nrf_drv_power_usbevt_uninit
  [Calls]
  - >> nrfx_power_usbevt_init
  - >> nrfx_power_usbevt_enable
  - >> nrf_drv_power_usbevt_uninit
  [Called By]
  - >> app_usbd_power_events_enable

  nrf_drv_power_usbevt_uninit (Thumb, 14 bytes, Stack size 8 bytes, nrf_drv_power.o(i.nrf_drv_power_usbevt_uninit))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_drv_power_usbevt_uninit
  [Calls]
  - >> nrfx_power_usbevt_uninit
  - >> nrfx_power_usbevt_disable
  [Called By]
  - >> nrf_drv_power_usbevt_init

  nrf_drv_uart_init (Thumb, 122 bytes, Stack size 56 bytes, nrf_drv_uart.o(i.nrf_drv_uart_init))
  [Stack]

  - Max Depth = 424
  - Call Chain = nrf_drv_uart_init ⇒ nrfx_uarte_init ⇒ apply_config ⇒ nrf_gpio_cfg_output ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_uarte_init
  - >> nrfx_uart_init
  - >> assert_nrf_callback
  - >> __aeabi_memcpy4
  [Called By]
  - >> uart_init
  - >> cli_uart_init
  - >> cli_uart_enable

  nrf_fprintf (Thumb, 76 bytes, Stack size 32 bytes, nrf_fprintf.o(i.nrf_fprintf))
  [Stack]

  - Max Depth = 448
  - Call Chain = nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_fprintf_fmt
  [Called By]
  - >> nrf_cli_start
  - >> cursor_down_move
  - >> cli_cursor_save
  - >> cli_cursor_restore
  - >> cli_clear_eos
  - >> char_insert
  - >> char_delete
  - >> char_backspace
  - >> nrf_cli_help_print
  - >> prefix_process
  - >> postfix_process
  - >> nrf_log_std_entry_process
  - >> nrf_log_hexdump_entry_process
  - >> vt100_color_set
  - >> vt100_bgcolor_set
  - >> nrf_cli_cmd_resize_default
  - >> nrf_cli_cmd_clear
  - >> format_offset_string_print
  - >> cursor_up_move
  - >> cursor_right_move
  - >> cursor_position_get
  - >> cursor_next_line_move
  - >> cursor_left_move

  nrf_fprintf_buffer_flush (Thumb, 34 bytes, Stack size 8 bytes, nrf_fprintf.o(i.nrf_fprintf_buffer_flush))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrf_fprintf_buffer_flush ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrf_cli_process
  - >> postfix_process
  - >> buffer_add
  - >> nrf_fprintf_fmt
  - >> format_offset_string_print
  - >> cursor_position_get

  nrf_fprintf_fmt (Thumb, 538 bytes, Stack size 40 bytes, nrf_fprintf_format.o(i.nrf_fprintf_fmt))
  [Stack]

  - Max Depth = 416
  - Call Chain = nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> unsigned_print
  - >> int_print
  - >> buffer_add
  - >> nrf_fprintf_buffer_flush
  - >> strlen
  [Called By]
  - >> nrf_cli_fprintf
  - >> nrf_fprintf

  nrf_log_backend_add (Thumb, 134 bytes, Stack size 24 bytes, nrf_log_frontend.o(i.nrf_log_backend_add))
  [Stack]

  - Max Depth = 40
  - Call Chain = nrf_log_backend_add ⇒ nrf_log_module_filter_set
  [Calls]
  - >> nrf_log_module_filter_set
  - >> nrf_log_module_cnt_get
  [Called By]
  - >> nrf_cli_init

  nrf_log_backend_serial_put (Thumb, 200 bytes, Stack size 104 bytes, nrf_log_backend_serial.o(i.nrf_log_backend_serial_put))
  [Stack]

  - Max Depth = 616
  - Call Chain = nrf_log_backend_serial_put ⇒ nrf_log_std_entry_process ⇒ prefix_process ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_memobj_read
  - >> nrf_memobj_put
  - >> nrf_memobj_get
  - >> nrf_log_std_entry_process
  - >> nrf_log_hexdump_entry_process
  - >> __aeabi_memclr4
  [Called By]
  - >> nrf_log_backend_uart_put

  nrf_log_color_id_get (Thumb, 42 bytes, Stack size 0 bytes, nrf_log_frontend.o(i.nrf_log_color_id_get))
  [Called By]

  - >> prefix_process

  nrf_log_frontend_dequeue (Thumb, 574 bytes, Stack size 56 bytes, nrf_log_frontend.o(i.nrf_log_frontend_dequeue))
  [Stack]

  - Max Depth = 128 + In Cycle
  - Call Chain = nrf_log_frontend_dequeue ⇒ nrf_log_frontend_std_0 (Cycle)
  [Calls]
  - >> nrf_log_frontend_std_0
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> buffer_is_empty
  - >> invalid_packets_omit
  - >> nrf_memobj_write
  - >> nrf_memobj_put
  - >> nrf_memobj_get
  - >> nrf_memobj_alloc
  [Called By]
  - >> main
  - >> app_error_fault_handler
  - >> HardFault_c_handler
  - >> std_n

  nrf_log_frontend_std_0 (Thumb, 8 bytes, Stack size 0 bytes, nrf_log_frontend.o(i.nrf_log_frontend_std_0))
  [Stack]

  - Max Depth = 168
  - Call Chain = nrf_log_frontend_std_0 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> std_n
  [Called By]
  - >> nrf_log_frontend_dequeue
  - >> main
  - >> usbd_user_ev_handler
  - >> hid_user_ev_handler
  - >> app_error_fault_handler
  - >> HardFault_c_handler

  nrf_log_frontend_std_1 (Thumb, 14 bytes, Stack size 8 bytes, nrf_log_frontend.o(i.nrf_log_frontend_std_1))
  [Stack]

  - Max Depth = 176
  - Call Chain = nrf_log_frontend_std_1 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> std_n
  [Called By]
  - >> app_error_fault_handler
  - >> HardFault_c_handler

  nrf_log_frontend_std_2 (Thumb, 16 bytes, Stack size 16 bytes, nrf_log_frontend.o(i.nrf_log_frontend_std_2))
  [Stack]

  - Max Depth = 184
  - Call Chain = nrf_log_frontend_std_2 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> std_n
  [Called By]
  - >> app_error_fault_handler

  nrf_log_frontend_std_3 (Thumb, 18 bytes, Stack size 24 bytes, nrf_log_frontend.o(i.nrf_log_frontend_std_3))
  [Stack]

  - Max Depth = 192
  - Call Chain = nrf_log_frontend_std_3 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> std_n
  [Called By]
  - >> HardFault_c_handler

  nrf_log_frontend_std_4 (Thumb, 20 bytes, Stack size 32 bytes, nrf_log_frontend.o(i.nrf_log_frontend_std_4))
  [Stack]

  - Max Depth = 200
  - Call Chain = nrf_log_frontend_std_4 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> std_n
  [Called By]
  - >> HardFault_c_handler

  nrf_log_frontend_std_5 (Thumb, 28 bytes, Stack size 40 bytes, nrf_log_frontend.o(i.nrf_log_frontend_std_5))
  [Stack]

  - Max Depth = 208
  - Call Chain = nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> std_n
  [Called By]
  - >> app_error_fault_handler

  nrf_log_hexdump_entry_process (Thumb, 150 bytes, Stack size 32 bytes, nrf_log_str_formatter.o(i.nrf_log_hexdump_entry_process))
  [Stack]

  - Max Depth = 496
  - Call Chain = nrf_log_hexdump_entry_process ⇒ prefix_process ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> prefix_process
  - >> postfix_process
  - >> nrf_fprintf
  - >> __rt_ctype_table
  [Called By]
  - >> cli_log_entry_process
  - >> nrf_log_backend_serial_put

  nrf_log_init (Thumb, 146 bytes, Stack size 32 bytes, nrf_log_frontend.o(i.nrf_log_init))
  [Stack]

  - Max Depth = 304
  - Call Chain = nrf_log_init ⇒ nrf_memobj_pool_init ⇒ nrf_balloc_init ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_ringbuf_init
  - >> nrf_memobj_pool_init
  - >> strncmp
  [Called By]
  - >> main

  nrf_log_module_cnt_get (Thumb, 10 bytes, Stack size 0 bytes, nrf_log_frontend.o(i.nrf_log_module_cnt_get))
  [Called By]

  - >> std_n
  - >> module_idx_get
  - >> log_status
  - >> log_ctrl
  - >> nrf_log_backend_add

  nrf_log_module_filter_get (Thumb, 64 bytes, Stack size 32 bytes, nrf_log_frontend.o(i.nrf_log_module_filter_get))
  [Stack]

  - Max Depth = 44
  - Call Chain = nrf_log_module_filter_get ⇒ module_idx_get
  [Calls]
  - >> module_idx_get
  [Called By]
  - >> module_id_filter_set
  - >> log_status

  nrf_log_module_filter_set (Thumb, 70 bytes, Stack size 16 bytes, nrf_log_frontend.o(i.nrf_log_module_filter_set))
  [Stack]

  - Max Depth = 16
  - Call Chain = nrf_log_module_filter_set
  [Called By]
  - >> module_id_filter_set
  - >> nrf_log_backend_add

  nrf_log_module_name_get (Thumb, 24 bytes, Stack size 16 bytes, nrf_log_frontend.o(i.nrf_log_module_name_get))
  [Stack]

  - Max Depth = 28
  - Call Chain = nrf_log_module_name_get ⇒ module_idx_get
  [Calls]
  - >> module_idx_get
  [Called By]
  - >> prefix_process
  - >> module_name_get
  - >> log_status
  - >> log_ctrl

  nrf_log_panic (Thumb, 38 bytes, Stack size 16 bytes, nrf_log_frontend.o(i.nrf_log_panic))
  [Stack]

  - Max Depth = 16
  - Call Chain = nrf_log_panic
  [Called By]
  - >> app_error_fault_handler
  - >> HardFault_c_handler

  nrf_log_std_entry_process (Thumb, 182 bytes, Stack size 48 bytes, nrf_log_str_formatter.o(i.nrf_log_std_entry_process))
  [Stack]

  - Max Depth = 512
  - Call Chain = nrf_log_std_entry_process ⇒ prefix_process ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> prefix_process
  - >> postfix_process
  - >> nrf_fprintf
  [Called By]
  - >> cli_log_entry_process
  - >> nrf_log_backend_serial_put

  nrf_memobj_alloc (Thumb, 96 bytes, Stack size 24 bytes, nrf_memobj.o(i.nrf_memobj_alloc))
  [Stack]

  - Max Depth = 72
  - Call Chain = nrf_memobj_alloc ⇒ nrf_memobj_free ⇒ nrf_balloc_free ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_balloc_alloc
  - >> nrf_memobj_free
  [Called By]
  - >> nrf_log_frontend_dequeue
  - >> history_save

  nrf_memobj_free (Thumb, 50 bytes, Stack size 24 bytes, nrf_memobj.o(i.nrf_memobj_free))
  [Stack]

  - Max Depth = 48
  - Call Chain = nrf_memobj_free ⇒ nrf_balloc_free ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_balloc_free
  [Called By]
  - >> nrf_memobj_put
  - >> nrf_memobj_alloc
  - >> history_list_element_oldest_remove

  nrf_memobj_get (Thumb, 8 bytes, Stack size 0 bytes, nrf_memobj.o(i.nrf_memobj_get))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_memobj_get ⇒ nrf_atomic_u32_add
  [Calls]
  - >> nrf_atomic_u32_add
  [Called By]
  - >> nrf_log_frontend_dequeue
  - >> nrf_log_backend_serial_put
  - >> nrf_log_backend_cli_put

  nrf_memobj_pool_init (Thumb, 4 bytes, Stack size 0 bytes, nrf_memobj.o(i.nrf_memobj_pool_init))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrf_memobj_pool_init ⇒ nrf_balloc_init ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_balloc_init
  [Called By]
  - >> nrf_log_init
  - >> nrf_cli_instance_init

  nrf_memobj_put (Thumb, 30 bytes, Stack size 8 bytes, nrf_memobj.o(i.nrf_memobj_put))
  [Stack]

  - Max Depth = 56
  - Call Chain = nrf_memobj_put ⇒ nrf_memobj_free ⇒ nrf_balloc_free ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_atomic_u32_sub
  - >> nrf_memobj_free
  [Called By]
  - >> nrf_log_frontend_dequeue
  - >> cli_log_entry_process
  - >> nrf_log_backend_serial_put

  nrf_memobj_read (Thumb, 34 bytes, Stack size 16 bytes, nrf_memobj.o(i.nrf_memobj_read))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrf_memobj_read ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> memobj_op
  [Called By]
  - >> cli_log_entry_process
  - >> nrf_log_backend_serial_put
  - >> nrf_cli_cmd_history
  - >> history_save
  - >> history_list_element_oldest_remove
  - >> history_list_element_add
  - >> history_handle

  nrf_memobj_write (Thumb, 32 bytes, Stack size 16 bytes, nrf_memobj.o(i.nrf_memobj_write))
  [Stack]

  - Max Depth = 64 + In Cycle
  - Call Chain = nrf_memobj_write ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> memobj_op
  [Called By]
  - >> nrf_log_frontend_dequeue
  - >> history_list_element_oldest_remove
  - >> history_list_element_add

  nrf_pwr_mgmt_feed (Thumb, 2 bytes, Stack size 0 bytes, nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_feed))
  [Called By]

  - >> cli_state_collect

  nrf_queue_generic_pop (Thumb, 158 bytes, Stack size 24 bytes, nrf_queue.o(i.nrf_queue_generic_pop))
  [Stack]

  - Max Depth = 304
  - Call Chain = nrf_queue_generic_pop ⇒ nrf_queue_next_idx ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> nrf_queue_is_empty
  - >> nrf_queue_next_idx
  - >> __aeabi_memcpy
  [Called By]
  - >> hid_generic_clear_buffer
  - >> hid_generic_transfer_set
  - >> cli_log_entry_process
  - >> nrf_log_backend_cli_flush

  nrf_queue_is_empty (Thumb, 34 bytes, Stack size 8 bytes, nrf_queue.o(i.nrf_queue_is_empty))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrf_queue_is_empty ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrf_queue_generic_pop
  - >> hid_generic_transfer_set
  - >> hid_generic_ep_transfer_in

  nrf_queue_is_full (Thumb, 38 bytes, Stack size 16 bytes, nrf_queue.o(i.nrf_queue_is_full))
  [Stack]

  - Max Depth = 296
  - Call Chain = nrf_queue_is_full ⇒ nrf_queue_next_idx ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_queue_next_idx
  [Called By]
  - >> nrf_queue_push

  nrf_queue_max_utilization_get (Thumb, 22 bytes, Stack size 8 bytes, nrf_queue.o(i.nrf_queue_max_utilization_get))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrf_queue_max_utilization_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrf_queue_status
  - >> nrf_cli_cmd_cli_stats_show

  nrf_queue_max_utilization_reset (Thumb, 24 bytes, Stack size 8 bytes, nrf_queue.o(i.nrf_queue_max_utilization_reset))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrf_queue_max_utilization_reset ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrf_cli_cmd_cli_stats_reset

  nrf_queue_push (Thumb, 192 bytes, Stack size 24 bytes, nrf_queue.o(i.nrf_queue_push))
  [Stack]

  - Max Depth = 320
  - Call Chain = nrf_queue_push ⇒ nrf_queue_is_full ⇒ nrf_queue_next_idx ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> nrf_queue_is_full
  - >> queue_utilization_get
  - >> nrf_queue_next_idx
  - >> __aeabi_memcpy
  [Called By]
  - >> app_usbd_hid_generic_in_report_set
  - >> nrf_log_backend_cli_put

  nrf_queue_utilization_get (Thumb, 40 bytes, Stack size 8 bytes, nrf_queue.o(i.nrf_queue_utilization_get))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrf_queue_utilization_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> queue_utilization_get
  [Called By]
  - >> nrf_queue_status

  nrf_ringbuf_alloc (Thumb, 132 bytes, Stack size 24 bytes, nrf_ringbuf.o(i.nrf_ringbuf_alloc))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrf_ringbuf_alloc ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_atomic_flag_clear
  - >> nrf_atomic_flag_set_fetch
  [Called By]
  - >> rx_try

  nrf_ringbuf_cpy_get (Thumb, 146 bytes, Stack size 24 bytes, nrf_ringbuf.o(i.nrf_ringbuf_cpy_get))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrf_ringbuf_cpy_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_atomic_flag_clear
  - >> nrf_atomic_flag_set_fetch
  - >> __aeabi_memcpy
  [Called By]
  - >> cli_uart_read

  nrf_ringbuf_cpy_put (Thumb, 136 bytes, Stack size 24 bytes, nrf_ringbuf.o(i.nrf_ringbuf_cpy_put))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrf_ringbuf_cpy_put ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_atomic_flag_clear
  - >> nrf_atomic_flag_set_fetch
  - >> __aeabi_memcpy
  [Called By]
  - >> cli_uart_write

  nrf_ringbuf_free (Thumb, 38 bytes, Stack size 8 bytes, nrf_ringbuf.o(i.nrf_ringbuf_free))
  [Stack]

  - Max Depth = 16
  - Call Chain = nrf_ringbuf_free ⇒ nrf_atomic_flag_clear ⇒ nrf_atomic_u32_and
  [Calls]
  - >> nrf_atomic_flag_clear
  [Called By]
  - >> uart_event_handler
  - >> cli_uart_write

  nrf_ringbuf_get (Thumb, 132 bytes, Stack size 24 bytes, nrf_ringbuf.o(i.nrf_ringbuf_get))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrf_ringbuf_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_atomic_flag_clear
  - >> nrf_atomic_flag_set_fetch
  [Called By]
  - >> uart_event_handler
  - >> cli_uart_write

  nrf_ringbuf_init (Thumb, 28 bytes, Stack size 0 bytes, nrf_ringbuf.o(i.nrf_ringbuf_init))
  [Called By]

  - >> nrf_log_init
  - >> cli_uart_init

  nrf_ringbuf_put (Thumb, 48 bytes, Stack size 16 bytes, nrf_ringbuf.o(i.nrf_ringbuf_put))
  [Stack]

  - Max Depth = 24
  - Call Chain = nrf_ringbuf_put ⇒ nrf_atomic_flag_clear_fetch ⇒ nrf_atomic_u32_fetch_and
  [Calls]
  - >> nrf_atomic_flag_clear_fetch
  [Called By]
  - >> uart_event_handler

  nrf_strerror_find (Thumb, 52 bytes, Stack size 8 bytes, nrf_strerror.o(i.nrf_strerror_find))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_strerror_find
  [Called By]
  - >> nrf_strerror_get

  nrf_strerror_get (Thumb, 14 bytes, Stack size 4 bytes, nrf_strerror.o(i.nrf_strerror_get))
  [Stack]

  - Max Depth = 12
  - Call Chain = nrf_strerror_get ⇒ nrf_strerror_find
  [Calls]
  - >> nrf_strerror_find
  [Called By]
  - >> app_error_fault_handler

  nrfx_atomic_u32_fetch_and (Thumb, 10 bytes, Stack size 8 bytes, nrfx_atomic.o(i.nrfx_atomic_u32_fetch_and))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrfx_atomic_u32_fetch_and
  [Calls]
  - >> __asm___13_nrfx_atomic_c_3bd32246__nrfx_atomic_internal_and
  [Called By]
  - >> usbd_dmareq_process
  - >> nrf_usbd_epout_dma_handler
  - >> nrf_usbd_epiniso_dma_handler
  - >> nrf_usbd_epin_dma_handler
  - >> ev_setup_handler
  - >> ev_dma_epout8_handler
  - >> ev_dma_epout0_handler
  - >> ev_dma_epin0_handler

  nrfx_clock_enable (Thumb, 34 bytes, Stack size 8 bytes, nrfx_clock.o(i.nrfx_clock_enable))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrfx_clock_enable ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_power_clock_irq_init
  - >> assert_nrf_callback
  [Called By]
  - >> nrf_drv_clock_init

  nrfx_clock_hfclk_start (Thumb, 36 bytes, Stack size 8 bytes, nrfx_clock.o(i.nrfx_clock_hfclk_start))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrfx_clock_hfclk_start ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_clock_event_clear
  - >> assert_nrf_callback
  [Called By]
  - >> nrf_drv_clock_hfclk_request

  nrfx_clock_hfclk_stop (Thumb, 46 bytes, Stack size 8 bytes, nrfx_clock.o(i.nrfx_clock_hfclk_stop))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrfx_clock_hfclk_stop ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrf_drv_clock_hfclk_release

  nrfx_clock_init (Thumb, 38 bytes, Stack size 8 bytes, nrfx_clock.o(i.nrfx_clock_init))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrfx_clock_init ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrf_drv_clock_init

  nrfx_clock_irq_handler (Thumb, 82 bytes, Stack size 16 bytes, nrfx_clock.o(i.nrfx_clock_irq_handler))
  [Stack]

  - Max Depth = 24
  - Call Chain = nrfx_clock_irq_handler ⇒ nrf_clock_event_clear
  [Calls]
  - >> nrf_clock_event_clear
  - >> nrf_clock_event_check
  [Called By]
  - >> POWER_CLOCK_IRQHandler

  nrfx_clock_lfclk_start (Thumb, 40 bytes, Stack size 8 bytes, nrfx_clock.o(i.nrfx_clock_lfclk_start))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrfx_clock_lfclk_start ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_clock_event_clear
  - >> assert_nrf_callback
  [Called By]
  - >> nrf_drv_clock_lfclk_request

  nrfx_gpiote_in_event_enable (Thumb, 178 bytes, Stack size 24 bytes, nrfx_gpiote.o(i.nrfx_gpiote_in_event_enable))
  [Stack]

  - Max Depth = 312
  - Call Chain = nrfx_gpiote_in_event_enable ⇒ nrf_gpio_cfg_sense_set ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> pin_in_use_by_te
  - >> pin_in_use_by_port
  - >> pin_in_use_by_gpiote
  - >> nrf_gpiote_event_clear
  - >> nrf_gpio_pin_read
  - >> nrf_gpio_cfg_sense_set
  - >> channel_port_get
  [Called By]
  - >> app_button_enable

  nrfx_gpiote_in_init (Thumb, 204 bytes, Stack size 32 bytes, nrfx_gpiote.o(i.nrfx_gpiote_in_init))
  [Stack]

  - Max Depth = 344
  - Call Chain = nrfx_gpiote_in_init ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> pin_in_use_by_gpiote
  - >> nrf_gpio_pin_port_decode
  - >> nrf_gpio_cfg
  - >> nrf_bitmask_bit_set
  - >> channel_port_alloc
  [Called By]
  - >> app_button_init

  nrfx_gpiote_in_is_set (Thumb, 32 bytes, Stack size 8 bytes, nrfx_gpiote.o(i.nrfx_gpiote_in_is_set))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrfx_gpiote_in_is_set ⇒ nrf_gpio_pin_read ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_gpio_pin_read
  [Called By]
  - >> gpiote_event_handler
  - >> detection_delay_timeout_handler

  nrfx_gpiote_init (Thumb, 100 bytes, Stack size 16 bytes, nrfx_gpiote.o(i.nrfx_gpiote_init))
  [Stack]

  - Max Depth = 24
  - Call Chain = nrfx_gpiote_init ⇒ nrf_gpiote_event_clear
  [Calls]
  - >> nrf_gpiote_event_clear
  - >> channel_free
  [Called By]
  - >> app_button_init

  nrfx_gpiote_is_init (Thumb, 14 bytes, Stack size 0 bytes, nrfx_gpiote.o(i.nrfx_gpiote_is_init))
  [Called By]

  - >> app_button_init

  nrfx_power_init (Thumb, 58 bytes, Stack size 16 bytes, nrfx_power.o(i.nrfx_power_init))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrfx_power_init ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_power_clock_irq_init
  [Called By]
  - >> nrf_drv_power_init

  nrfx_power_irq_handler (Thumb, 222 bytes, Stack size 16 bytes, nrfx_power.o(i.nrfx_power_irq_handler))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrfx_power_irq_handler ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_power_event_get_and_clear
  [Called By]
  - >> POWER_CLOCK_IRQHandler

  nrfx_power_usbevt_disable (Thumb, 14 bytes, Stack size 0 bytes, nrfx_power.o(i.nrfx_power_usbevt_disable))
  [Called By]

  - >> nrf_drv_power_usbevt_uninit

  nrfx_power_usbevt_enable (Thumb, 14 bytes, Stack size 0 bytes, nrfx_power.o(i.nrfx_power_usbevt_enable))
  [Called By]

  - >> nrf_drv_power_usbevt_init

  nrfx_power_usbevt_init (Thumb, 16 bytes, Stack size 0 bytes, nrfx_power.o(i.nrfx_power_usbevt_init))
  [Called By]

  - >> nrf_drv_power_usbevt_init

  nrfx_power_usbevt_uninit (Thumb, 8 bytes, Stack size 0 bytes, nrfx_power.o(i.nrfx_power_usbevt_uninit))
  [Called By]

  - >> nrf_drv_power_usbevt_uninit

  nrfx_prs_acquire (Thumb, 62 bytes, Stack size 16 bytes, nrfx_prs.o(i.nrfx_prs_acquire))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrfx_prs_acquire ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> prs_box_get
  [Called By]
  - >> nrfx_uarte_init
  - >> nrfx_uart_init

  nrfx_prs_release (Thumb, 32 bytes, Stack size 8 bytes, nrfx_prs.o(i.nrfx_prs_release))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrfx_prs_release ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> prs_box_get
  [Called By]
  - >> nrfx_uarte_uninit
  - >> nrfx_uart_uninit

  nrfx_systick_delay_ticks (Thumb, 38 bytes, Stack size 8 bytes, nrfx_systick.o(i.nrfx_systick_delay_ticks))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrfx_systick_delay_ticks ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrfx_systick_delay_us

  nrfx_systick_delay_us (Thumb, 48 bytes, Stack size 16 bytes, nrfx_systick.o(i.nrfx_systick_delay_us))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrfx_systick_delay_us ⇒ nrfx_systick_delay_ticks ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_systick_delay_ticks
  [Called By]
  - >> usbd_dmareq_process

  nrfx_uart_0_irq_handler (Thumb, 8 bytes, Stack size 0 bytes, nrfx_uart.o(i.nrfx_uart_0_irq_handler))
  [Stack]

  - Max Depth = 72
  - Call Chain = nrfx_uart_0_irq_handler ⇒ uart_irq_handler ⇒ tx_done_event
  [Calls]
  - >> uart_irq_handler
  [Address Reference Count : 1]
  - nrfx_uart.o(.constdata)

  nrfx_uart_init (Thumb, 118 bytes, Stack size 24 bytes, nrfx_uart.o(i.nrfx_uart_init))
  [Stack]

  - Max Depth = 368
  - Call Chain = nrfx_uart_init ⇒ apply_config ⇒ nrf_gpio_cfg_output ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> interrupts_enable
  - >> apply_config
  - >> nrfx_prs_acquire
  [Called By]
  - >> nrf_drv_uart_init

  nrfx_uart_rx (Thumb, 276 bytes, Stack size 40 bytes, nrfx_uart.o(i.nrfx_uart_rx))
  [Stack]

  - Max Depth = 304
  - Call Chain = nrfx_uart_rx ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> rx_enable
  - >> rx_byte
  - >> nrf_uart_event_clear
  - >> nrf_uart_event_check
  [Called By]
  - >> rx_try

  nrfx_uart_rx_abort (Thumb, 18 bytes, Stack size 0 bytes, nrfx_uart.o(i.nrfx_uart_rx_abort))
  [Called By]

  - >> timer_handler

  nrfx_uart_tx (Thumb, 204 bytes, Stack size 32 bytes, nrfx_uart.o(i.nrfx_uart_tx))
  [Stack]

  - Max Depth = 296
  - Call Chain = nrfx_uart_tx ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> tx_byte
  - >> nrf_uart_event_clear
  - >> nrf_uart_event_check
  - >> nrfx_uart_tx_in_progress
  [Called By]
  - >> serial_tx
  - >> nrf_drv_uart_tx

  nrfx_uart_tx_in_progress (Thumb, 26 bytes, Stack size 0 bytes, nrfx_uart.o(i.nrfx_uart_tx_in_progress))
  [Called By]

  - >> nrfx_uart_tx
  - >> cli_uart_write

  nrfx_uart_uninit (Thumb, 170 bytes, Stack size 32 bytes, nrfx_uart.o(i.nrfx_uart_uninit))
  [Stack]

  - Max Depth = 360
  - Call Chain = nrfx_uart_uninit ⇒ nrf_gpio_cfg_default ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_cfg_default
  - >> nrfx_prs_release
  [Called By]
  - >> nrf_log_backend_uart_panic_set
  - >> nrf_drv_uart_uninit

  nrfx_uarte_0_irq_handler (Thumb, 8 bytes, Stack size 0 bytes, nrfx_uarte.o(i.nrfx_uarte_0_irq_handler))
  [Stack]

  - Max Depth = 64
  - Call Chain = nrfx_uarte_0_irq_handler ⇒ uarte_irq_handler ⇒ rx_done_event
  [Calls]
  - >> uarte_irq_handler
  [Address Reference Count : 1]
  - nrfx_uarte.o(.constdata)

  nrfx_uarte_init (Thumb, 110 bytes, Stack size 24 bytes, nrfx_uarte.o(i.nrfx_uarte_init))
  [Stack]

  - Max Depth = 368
  - Call Chain = nrfx_uarte_init ⇒ apply_config ⇒ nrf_gpio_cfg_output ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_prs_acquire
  - >> interrupts_enable
  - >> apply_config
  [Called By]
  - >> nrf_drv_uart_init

  nrfx_uarte_rx (Thumb, 318 bytes, Stack size 40 bytes, nrfx_uarte.o(i.nrfx_uarte_rx))
  [Stack]

  - Max Depth = 304
  - Call Chain = nrfx_uarte_rx ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_is_in_ram
  - >> nrf_uarte_event_clear
  - >> nrf_uarte_event_check
  [Called By]
  - >> rx_try

  nrfx_uarte_rx_abort (Thumb, 38 bytes, Stack size 0 bytes, nrfx_uarte.o(i.nrfx_uarte_rx_abort))
  [Called By]

  - >> timer_handler

  nrfx_uarte_tx (Thumb, 200 bytes, Stack size 32 bytes, nrfx_uarte.o(i.nrfx_uarte_tx))
  [Stack]

  - Max Depth = 296
  - Call Chain = nrfx_uarte_tx ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_uarte_tx_in_progress
  - >> nrfx_is_in_ram
  - >> nrf_uarte_event_clear
  - >> nrf_uarte_event_check
  [Called By]
  - >> serial_tx
  - >> nrf_drv_uart_tx

  nrfx_uarte_tx_in_progress (Thumb, 22 bytes, Stack size 0 bytes, nrfx_uarte.o(i.nrfx_uarte_tx_in_progress))
  [Called By]

  - >> nrfx_uarte_tx
  - >> cli_uart_write

  nrfx_uarte_uninit (Thumb, 166 bytes, Stack size 32 bytes, nrfx_uarte.o(i.nrfx_uarte_uninit))
  [Stack]

  - Max Depth = 360
  - Call Chain = nrfx_uarte_uninit ⇒ nrf_gpio_cfg_default ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_prs_release
  - >> nrf_gpio_cfg_default
  [Called By]
  - >> nrf_log_backend_uart_panic_set
  - >> nrf_drv_uart_uninit

  nrfx_usbd_active_irq_config (Thumb, 10 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrfx_usbd_active_irq_config))
  [Called By]

  - >> sustate_set

  nrfx_usbd_consumer (Thumb, 94 bytes, Stack size 24 bytes, nrfx_usbd.o(i.nrfx_usbd_consumer))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrfx_usbd_consumer ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_is_in_ram
  [Address Reference Count : 1]
  - nrfx_usbd.o(i.nrfx_usbd_ep_transfer)

  nrfx_usbd_disable (Thumb, 56 bytes, Stack size 8 bytes, nrfx_usbd.o(i.nrfx_usbd_disable))
  [Stack]

  - Max Depth = 376
  - Call Chain = nrfx_usbd_disable ⇒ nrfx_usbd_stop ⇒ usbd_ep_abort_all ⇒ usbd_ep_abort ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_usbd_stop
  - >> usbd_dma_pending_clear
  [Called By]
  - >> app_usbd_disable

  nrfx_usbd_enable (Thumb, 284 bytes, Stack size 32 bytes, nrfx_usbd.o(i.nrfx_usbd_enable))
  [Stack]

  - Max Depth = 296
  - Call Chain = nrfx_usbd_enable ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> usbd_dma_pending_clear
  - >> nrfx_usbd_errata_type_52840_eng_b
  - >> nrf_usbd_eventcause_clear
  [Called By]
  - >> app_usbd_enable

  nrfx_usbd_ep_abort (Thumb, 4 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrfx_usbd_ep_abort))
  [Stack]

  - Max Depth = 328
  - Call Chain = nrfx_usbd_ep_abort ⇒ usbd_ep_abort ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> usbd_ep_abort
  [Called By]
  - >> hid_generic_clear_buffer

  nrfx_usbd_ep_disable (Thumb, 84 bytes, Stack size 16 bytes, nrfx_usbd.o(i.nrfx_usbd_ep_disable))
  [Stack]

  - Max Depth = 344
  - Call Chain = nrfx_usbd_ep_disable ⇒ usbd_ep_abort ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> usbd_ep_abort
  - >> nrfx_usbd_ep_to_int
  - >> ep_to_hal
  [Called By]
  - >> app_usbd_iface_deselect
  - >> app_usbd_ep_disable

  nrfx_usbd_ep_dtoggle_clear (Thumb, 62 bytes, Stack size 16 bytes, nrfx_usbd.o(i.nrfx_usbd_ep_dtoggle_clear))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrfx_usbd_ep_dtoggle_clear ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> setup_endpoint_req_std
  - >> app_usbd_ep_enable

  nrfx_usbd_ep_enable (Thumb, 144 bytes, Stack size 16 bytes, nrfx_usbd.o(i.nrfx_usbd_ep_enable))
  [Stack]

  - Max Depth = 312
  - Call Chain = nrfx_usbd_ep_enable ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> nrfx_usbd_transfer_out_drop
  - >> nrfx_usbd_ep_to_int
  - >> nrf_usbd_ep_enable_check
  - >> ep_to_hal
  - >> ep2bit
  [Called By]
  - >> app_usbd_ep_enable

  nrfx_usbd_ep_enable_check (Thumb, 14 bytes, Stack size 8 bytes, nrfx_usbd.o(i.nrfx_usbd_ep_enable_check))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrfx_usbd_ep_enable_check ⇒ nrf_usbd_ep_enable_check ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_ep_enable_check
  - >> ep_to_hal
  [Called By]
  - >> app_usbd_ep_transfer
  - >> app_usbd_ep_handled_transfer

  nrfx_usbd_ep_handled_transfer (Thumb, 116 bytes, Stack size 24 bytes, nrfx_usbd.o(i.nrfx_usbd_ep_handled_transfer))
  [Stack]

  - Max Depth = 304
  - Call Chain = nrfx_usbd_ep_handled_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> usbd_int_rise
  - >> ep_state_access
  - >> ep2bit
  [Called By]
  - >> app_usbd_ep_handled_transfer

  nrfx_usbd_ep_max_packet_size_get (Thumb, 10 bytes, Stack size 8 bytes, nrfx_usbd.o(i.nrfx_usbd_ep_max_packet_size_get))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrfx_usbd_ep_max_packet_size_get ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> ep_state_access
  [Called By]
  - >> app_usbd_core_setup_rsp

  nrfx_usbd_ep_max_packet_size_set (Thumb, 82 bytes, Stack size 16 bytes, nrfx_usbd.o(i.nrfx_usbd_ep_max_packet_size_set))
  [Stack]

  - Max Depth = 296
  - Call Chain = nrfx_usbd_ep_max_packet_size_set ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> ep_state_access
  [Called By]
  - >> nrfx_usbd_init

  nrfx_usbd_ep_stall (Thumb, 44 bytes, Stack size 8 bytes, nrfx_usbd.o(i.nrfx_usbd_ep_stall))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrfx_usbd_ep_stall ⇒ ep_to_hal ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> ep_to_hal
  [Called By]
  - >> setup_endpoint_req_std
  - >> app_usbd_event_execute

  nrfx_usbd_ep_stall_check (Thumb, 44 bytes, Stack size 8 bytes, nrfx_usbd.o(i.nrfx_usbd_ep_stall_check))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrfx_usbd_ep_stall_check ⇒ ep_to_hal ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> ep_to_hal
  [Called By]
  - >> nrfx_usbd_ep_stall_clear
  - >> setup_endpoint_req_std

  nrfx_usbd_ep_stall_clear (Thumb, 62 bytes, Stack size 8 bytes, nrfx_usbd.o(i.nrfx_usbd_ep_stall_clear))
  [Stack]

  - Max Depth = 304
  - Call Chain = nrfx_usbd_ep_stall_clear ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_usbd_transfer_out_drop
  - >> nrfx_usbd_ep_stall_check
  - >> ep_to_hal
  [Called By]
  - >> setup_endpoint_req_std
  - >> app_usbd_ep_enable

  nrfx_usbd_ep_transfer (Thumb, 210 bytes, Stack size 24 bytes, nrfx_usbd.o(i.nrfx_usbd_ep_transfer))
  [Stack]

  - Max Depth = 304
  - Call Chain = nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> usbd_int_rise
  - >> nrfx_is_in_ram
  - >> ep_state_access
  - >> ep2bit
  [Called By]
  - >> app_usbd_ep_transfer

  nrfx_usbd_epout_size_get (Thumb, 14 bytes, Stack size 8 bytes, nrfx_usbd.o(i.nrfx_usbd_epout_size_get))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrfx_usbd_epout_size_get ⇒ nrf_usbd_epout_size_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_epout_size_get
  - >> ep_to_hal
  [Called By]
  - >> usbd_dmareq_process

  nrfx_usbd_feeder_buffer_get (Thumb, 4 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrfx_usbd_feeder_buffer_get))
  [Called By]

  - >> usbd_descriptor_conf_feeder

  nrfx_usbd_feeder_flash (Thumb, 90 bytes, Stack size 24 bytes, nrfx_usbd.o(i.nrfx_usbd_feeder_flash))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrfx_usbd_feeder_flash ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_is_in_ram
  - >> __aeabi_memcpy
  [Address Reference Count : 1]
  - nrfx_usbd.o(i.nrfx_usbd_ep_transfer)

  nrfx_usbd_feeder_flash_zlp (Thumb, 100 bytes, Stack size 24 bytes, nrfx_usbd.o(i.nrfx_usbd_feeder_flash_zlp))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrfx_usbd_feeder_flash_zlp ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_is_in_ram
  - >> __aeabi_memcpy
  [Address Reference Count : 1]
  - nrfx_usbd.o(i.nrfx_usbd_ep_transfer)

  nrfx_usbd_feeder_ram (Thumb, 66 bytes, Stack size 24 bytes, nrfx_usbd.o(i.nrfx_usbd_feeder_ram))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrfx_usbd_feeder_ram ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_is_in_ram
  [Address Reference Count : 1]
  - nrfx_usbd.o(i.nrfx_usbd_ep_transfer)

  nrfx_usbd_feeder_ram_zlp (Thumb, 84 bytes, Stack size 24 bytes, nrfx_usbd.o(i.nrfx_usbd_feeder_ram_zlp))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrfx_usbd_feeder_ram_zlp ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_is_in_ram
  [Address Reference Count : 1]
  - nrfx_usbd.o(i.nrfx_usbd_ep_transfer)

  nrfx_usbd_force_bus_wakeup (Thumb, 8 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrfx_usbd_force_bus_wakeup))
  [Called By]

  - >> app_usbd_event_execute

  nrfx_usbd_init (Thumb, 136 bytes, Stack size 24 bytes, nrfx_usbd.o(i.nrfx_usbd_init))
  [Stack]

  - Max Depth = 320
  - Call Chain = nrfx_usbd_init ⇒ nrfx_usbd_ep_max_packet_size_set ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_usbd_ep_max_packet_size_set
  - >> ep_state_access
  [Called By]
  - >> app_usbd_init

  nrfx_usbd_is_enabled (Thumb, 16 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrfx_usbd_is_enabled))
  [Called By]

  - >> app_usbd_start
  - >> app_usbd_power_events_enable
  - >> app_usbd_class_append
  - >> usbd_user_ev_handler
  - >> nrfx_usbd_is_started
  - >> app_usbd_class_sof_unregister
  - >> app_usbd_class_sof_register

  nrfx_usbd_is_initialized (Thumb, 12 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrfx_usbd_is_initialized))
  [Called By]

  - >> app_usbd_power_events_enable
  - >> app_usbd_class_append
  - >> app_usbd_class_sof_unregister
  - >> app_usbd_class_sof_register

  nrfx_usbd_is_started (Thumb, 24 bytes, Stack size 8 bytes, nrfx_usbd.o(i.nrfx_usbd_is_started))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrfx_usbd_is_started
  [Calls]
  - >> nrfx_usbd_is_enabled
  - >> _NRFX_IRQ_IS_ENABLED
  [Called By]
  - >> app_usbd_disable

  nrfx_usbd_last_setup_dir_get (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrfx_usbd_last_setup_dir_get))
  [Called By]

  - >> app_usbd_core_setup_data_handler_set
  - >> app_usbd_core_setup_req_handler

  nrfx_usbd_setup_clear (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrfx_usbd_setup_clear))
  [Calls]

  - >> nrf_usbd_task_trigger
  [Called By]
  - >> app_usbd_core_setup_req_handler
  - >> app_usbd_core_event_handler

  nrfx_usbd_setup_data_clear (Thumb, 42 bytes, Stack size 8 bytes, nrfx_usbd.o(i.nrfx_usbd_setup_data_clear))
  [Stack]

  - Max Depth = 16
  - Call Chain = nrfx_usbd_setup_data_clear ⇒ nrfx_usbd_errata_104
  [Calls]
  - >> nrfx_usbd_errata_104
  - >> nrf_usbd_task_trigger
  [Called By]
  - >> ev_dma_epout0_handler
  - >> app_usbd_core_setup_req_handler
  - >> app_usbd_core_event_handler

  nrfx_usbd_setup_get (Thumb, 76 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrfx_usbd_setup_get))
  [Called By]

  - >> app_usbd_core_setup_req_handler

  nrfx_usbd_setup_stall (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrfx_usbd_setup_stall))
  [Calls]

  - >> nrf_usbd_task_trigger
  [Called By]
  - >> app_usbd_core_setup_req_handler
  - >> app_usbd_core_event_handler

  nrfx_usbd_start (Thumb, 78 bytes, Stack size 16 bytes, nrfx_usbd.o(i.nrfx_usbd_start))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrfx_usbd_start ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_usbd_errata_104
  [Called By]
  - >> app_usbd_event_execute

  nrfx_usbd_stop (Thumb, 70 bytes, Stack size 16 bytes, nrfx_usbd.o(i.nrfx_usbd_stop))
  [Stack]

  - Max Depth = 368
  - Call Chain = nrfx_usbd_stop ⇒ usbd_ep_abort_all ⇒ usbd_ep_abort ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> usbd_ep_abort_all
  - >> _NRFX_IRQ_IS_ENABLED
  [Called By]
  - >> nrfx_usbd_disable
  - >> app_usbd_event_execute

  nrfx_usbd_suspend (Thumb, 58 bytes, Stack size 8 bytes, nrfx_usbd.o(i.nrfx_usbd_suspend))
  [Stack]

  - Max Depth = 360
  - Call Chain = nrfx_usbd_suspend ⇒ usbd_ep_abort_all ⇒ usbd_ep_abort ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> usbd_ep_abort_all
  [Called By]
  - >> app_usbd_event_execute

  nrfx_usbd_suspend_irq_config (Thumb, 10 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrfx_usbd_suspend_irq_config))
  [Called By]

  - >> sustate_set

  nrfx_usbd_transfer_out_drop (Thumb, 150 bytes, Stack size 24 bytes, nrfx_usbd.o(i.nrfx_usbd_transfer_out_drop))
  [Stack]

  - Max Depth = 296
  - Call Chain = nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> nrfx_usbd_errata_type_52840_eng_b
  - >> ep2bit
  [Called By]
  - >> nrfx_usbd_ep_stall_clear
  - >> nrfx_usbd_ep_enable
  - >> usbd_ep_abort

  nrfx_usbd_uninit (Thumb, 28 bytes, Stack size 8 bytes, nrfx_usbd.o(i.nrfx_usbd_uninit))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrfx_usbd_uninit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> app_usbd_init

  nrfx_usbd_wakeup_req (Thumb, 66 bytes, Stack size 8 bytes, nrfx_usbd.o(i.nrfx_usbd_wakeup_req))
  [Stack]

  - Max Depth = 16
  - Call Chain = nrfx_usbd_wakeup_req ⇒ app_util_critical_region_exit ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> nrf_usbd_lowpower_check
  [Called By]
  - >> app_usbd_event_execute

  privilege_level_get (Thumb, 26 bytes, Stack size 0 bytes, app_util_platform.o(i.privilege_level_get))
  [Called By]

  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter

  ### Local Symbols

  bsp_event_callback (Thumb, 78 bytes, Stack size 8 bytes, main.o(i.bsp_event_callback))
  [Stack]

  - Max Depth = 48
  - Call Chain = bsp_event_callback ⇒ app_timer_start ⇒ app_util_critical_region_exit ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_timer_start
  - >> hid_generic_mouse_action
  [Address Reference Count : 2]
  - main.o(i.init_bsp)
  - main.o(i.init_cli)

  hid_acc_for_report_get (Thumb, 24 bytes, Stack size 0 bytes, main.o(i.hid_acc_for_report_get))
  [Called By]

  - >> hid_generic_mouse_process_state

  hid_generic_mouse_action (Thumb, 92 bytes, Stack size 16 bytes, main.o(i.hid_generic_mouse_action))
  [Stack]

  - Max Depth = 24
  - Call Chain = hid_generic_mouse_action ⇒ app_util_critical_region_exit ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  [Called By]
  - >> mouse_move_timer_handler
  - >> bsp_event_callback

  hid_generic_mouse_process_state (Thumb, 114 bytes, Stack size 16 bytes, main.o(i.hid_generic_mouse_process_state))
  [Stack]

  - Max Depth = 400
  - Call Chain = hid_generic_mouse_process_state ⇒ app_usbd_hid_generic_in_report_set ⇒ hid_generic_transfer_set ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> app_usbd_hid_generic_in_report_set
  - >> hid_acc_for_report_get
  [Called By]
  - >> main
  - >> hid_user_ev_handler

  hid_user_ev_handler (Thumb, 106 bytes, Stack size 16 bytes, main.o(i.hid_user_ev_handler))
  [Stack]

  - Max Depth = 416
  - Call Chain = hid_user_ev_handler ⇒ hid_generic_mouse_process_state ⇒ app_usbd_hid_generic_in_report_set ⇒ hid_generic_transfer_set ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_log_frontend_std_0
  - >> hid_generic_clear_buffer
  - >> bsp_board_led_invert
  - >> assert_nrf_callback
  - >> hid_generic_mouse_process_state
  [Address Reference Count : 1]
  - main.o(.constdata)

  idle_handle (Thumb, 26 bytes, Stack size 8 bytes, main.o(i.idle_handle))
  [Stack]

  - Max Depth = 360
  - Call Chain = idle_handle ⇒ app_usbd_hid_generic_idle_report_set ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_usbd_hid_generic_idle_report_set
  [Address Reference Count : 1]
  - main.o(i.main)

  init_bsp (Thumb, 76 bytes, Stack size 8 bytes, main.o(i.init_bsp))
  [Stack]

  - Max Depth = 392
  - Call Chain = init_bsp ⇒ bsp_init ⇒ app_button_init ⇒ nrfx_gpiote_in_init ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> bsp_init
  - >> bsp_event_to_button_action_assign
  - >> bsp_board_init
  - >> app_error_handler
  [Called By]
  - >> main

  init_cli (Thumb, 102 bytes, Stack size 40 bytes, main.o(i.init_cli))
  [Stack]

  - Max Depth = 560
  - Call Chain = init_cli ⇒ nrf_cli_start ⇒ cli_state_set ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_start
  - >> nrf_cli_init
  - >> bsp_cli_init
  - >> app_error_handler
  - >> __aeabi_memcpy4
  [Called By]
  - >> main

  mouse_move_timer_handler (Thumb, 60 bytes, Stack size 8 bytes, main.o(i.mouse_move_timer_handler))
  [Stack]

  - Max Depth = 296
  - Call Chain = mouse_move_timer_handler ⇒ bsp_button_is_pressed ⇒ bsp_board_button_state_get ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> bsp_button_is_pressed
  - >> app_timer_stop
  - >> hid_generic_mouse_action
  [Address Reference Count : 1]
  - main.o(i.main)

  usbd_user_ev_handler (Thumb, 152 bytes, Stack size 16 bytes, main.o(i.usbd_user_ev_handler))
  [Stack]

  - Max Depth = 400
  - Call Chain = usbd_user_ev_handler ⇒ app_usbd_disable ⇒ nrfx_usbd_disable ⇒ nrfx_usbd_stop ⇒ usbd_ep_abort_all ⇒ usbd_ep_abort ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_usbd_is_enabled
  - >> nrf_log_frontend_std_0
  - >> bsp_board_leds_off
  - >> bsp_board_led_on
  - >> app_usbd_suspend_req
  - >> app_usbd_stop
  - >> app_usbd_start
  - >> app_usbd_enable
  - >> app_usbd_disable
  [Address Reference Count : 1]
  - main.o(.constdata)

  nrf_gpio_cfg (Thumb, 50 bytes, Stack size 40 bytes, boards.o(i.nrf_gpio_cfg))
  [Stack]

  - Max Depth = 312
  - Call Chain = nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_pin_port_decode
  [Called By]
  - >> bsp_board_init

  nrf_gpio_pin_port_decode (Thumb, 42 bytes, Stack size 8 bytes, boards.o(i.nrf_gpio_pin_port_decode))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> bsp_board_led_state_get
  - >> bsp_board_button_state_get
  - >> nrf_gpio_pin_write
  - >> nrf_gpio_cfg
  - >> bsp_board_led_invert

  nrf_gpio_pin_write (Thumb, 38 bytes, Stack size 16 bytes, boards.o(i.nrf_gpio_pin_write))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrf_gpio_pin_write ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_pin_port_decode
  [Called By]
  - >> bsp_board_led_off
  - >> bsp_board_led_on

  alert_timer_handler (Thumb, 6 bytes, Stack size 0 bytes, bsp.o(i.alert_timer_handler))
  [Stack]

  - Max Depth = 288
  - Call Chain = alert_timer_handler ⇒ bsp_board_led_invert ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> bsp_board_led_invert
  [Address Reference Count : 1]
  - bsp.o(i.bsp_init)

  bsp_button_event_handler (Thumb, 132 bytes, Stack size 32 bytes, bsp.o(i.bsp_button_event_handler))
  [Stack]

  - Max Depth = 72
  - Call Chain = bsp_button_event_handler ⇒ app_timer_start ⇒ app_util_critical_region_exit ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> bsp_board_pin_to_button_idx
  - >> app_timer_stop
  - >> app_timer_start
  [Called By]
  - >> button_timer_handler
  [Address Reference Count : 1]
  - bsp.o(.constdata)

  bsp_led_indication (Thumb, 446 bytes, Stack size 40 bytes, bsp.o(i.bsp_led_indication))
  [Stack]

  - Max Depth = 352
  - Call Chain = bsp_led_indication ⇒ leds_off ⇒ bsp_board_leds_off ⇒ bsp_board_led_off ⇒ nrf_gpio_pin_write ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> leds_off
  - >> bsp_board_leds_on
  - >> bsp_board_led_state_get
  - >> bsp_board_led_off
  - >> bsp_board_led_on
  - >> bsp_board_led_invert
  - >> app_timer_stop
  - >> app_timer_start
  - >> __aeabi_uldivmod
  [Called By]
  - >> leds_timer_handler

  button_timer_handler (Thumb, 8 bytes, Stack size 0 bytes, bsp.o(i.button_timer_handler))
  [Stack]

  - Max Depth = 72
  - Call Chain = button_timer_handler ⇒ bsp_button_event_handler ⇒ app_timer_start ⇒ app_util_critical_region_exit ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> bsp_button_event_handler
  [Address Reference Count : 1]
  - bsp.o(i.bsp_init)

  leds_off (Thumb, 42 bytes, Stack size 8 bytes, bsp.o(i.leds_off))
  [Stack]

  - Max Depth = 312
  - Call Chain = leds_off ⇒ bsp_board_leds_off ⇒ bsp_board_led_off ⇒ nrf_gpio_pin_write ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> bsp_board_led_off
  - >> bsp_board_leds_off
  [Called By]
  - >> bsp_led_indication

  leds_timer_handler (Thumb, 16 bytes, Stack size 0 bytes, bsp.o(i.leds_timer_handler))
  [Stack]

  - Max Depth = 352
  - Call Chain = leds_timer_handler ⇒ bsp_led_indication ⇒ leds_off ⇒ bsp_board_leds_off ⇒ bsp_board_led_off ⇒ nrf_gpio_pin_write ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> bsp_led_indication
  [Address Reference Count : 1]
  - bsp.o(i.bsp_init)

  cmd_btn (Thumb, 40 bytes, Stack size 16 bytes, bsp_cli.o(i.cmd_btn))
  [Stack]

  - Max Depth = 280
  - Call Chain = cmd_btn ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> __0sscanf
  [Address Reference Count : 1]
  - bsp_cli.o(.constdata)

  cmd_evt (Thumb, 38 bytes, Stack size 16 bytes, bsp_cli.o(i.cmd_evt))
  [Stack]

  - Max Depth = 280
  - Call Chain = cmd_evt ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> __0sscanf
  [Address Reference Count : 1]
  - bsp_cli.o(.constdata)

  clock_clk_started_notify (Thumb, 34 bytes, Stack size 16 bytes, nrf_drv_clock.o(i.clock_clk_started_notify))
  [Stack]

  - Max Depth = 16
  - Call Chain = clock_clk_started_notify
  [Called By]
  - >> clock_irq_handler

  clock_irq_handler (Thumb, 24 bytes, Stack size 0 bytes, nrf_drv_clock.o(i.clock_irq_handler))
  [Stack]

  - Max Depth = 16
  - Call Chain = clock_irq_handler ⇒ clock_clk_started_notify
  [Calls]
  - >> clock_clk_started_notify
  [Address Reference Count : 1]
  - nrf_drv_clock.o(i.nrf_drv_clock_init)

  item_enqueue (Thumb, 22 bytes, Stack size 0 bytes, nrf_drv_clock.o(i.item_enqueue))
  [Called By]

  - >> nrf_drv_clock_lfclk_request
  - >> nrf_drv_clock_hfclk_request

  uart_evt_handler (Thumb, 42 bytes, Stack size 24 bytes, nrf_drv_uart.o(i.uart_evt_handler))
  [Stack]

  - Max Depth = 24
  - Call Chain = uart_evt_handler
  [Address Reference Count : 1]
  - nrf_drv_uart.o(i.nrf_drv_uart_init)

  uarte_evt_handler (Thumb, 42 bytes, Stack size 24 bytes, nrf_drv_uart.o(i.uarte_evt_handler))
  [Stack]

  - Max Depth = 24
  - Call Chain = uarte_evt_handler
  [Address Reference Count : 1]
  - nrf_drv_uart.o(i.nrf_drv_uart_init)

  nrf_clock_event_check (Thumb, 14 bytes, Stack size 0 bytes, nrfx_clock.o(i.nrf_clock_event_check))
  [Called By]

  - >> nrfx_clock_irq_handler

  nrf_clock_event_clear (Thumb, 16 bytes, Stack size 8 bytes, nrfx_clock.o(i.nrf_clock_event_clear))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_clock_event_clear
  [Called By]
  - >> nrfx_clock_lfclk_start
  - >> nrfx_clock_hfclk_start
  - >> nrfx_clock_irq_handler

  nrfx_power_clock_irq_init (Thumb, 28 bytes, Stack size 0 bytes, nrfx_clock.o(i.nrfx_power_clock_irq_init))
  [Called By]

  - >> nrfx_clock_enable

  channel_free (Thumb, 22 bytes, Stack size 0 bytes, nrfx_gpiote.o(i.channel_free))
  [Called By]

  - >> nrfx_gpiote_init

  channel_port_alloc (Thumb, 66 bytes, Stack size 20 bytes, nrfx_gpiote.o(i.channel_port_alloc))
  [Stack]

  - Max Depth = 20
  - Call Chain = channel_port_alloc
  [Called By]
  - >> nrfx_gpiote_in_init

  channel_port_get (Thumb, 10 bytes, Stack size 0 bytes, nrfx_gpiote.o(i.channel_port_get))
  [Called By]

  - >> nrfx_gpiote_in_event_enable
  - >> GPIOTE_IRQHandler

  nrf_bitmask_bit_is_set (Thumb, 16 bytes, Stack size 0 bytes, nrfx_gpiote.o(i.nrf_bitmask_bit_is_set))
  [Called By]

  - >> GPIOTE_IRQHandler

  nrf_bitmask_bit_set (Thumb, 20 bytes, Stack size 8 bytes, nrfx_gpiote.o(i.nrf_bitmask_bit_set))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_bitmask_bit_set
  [Called By]
  - >> nrfx_gpiote_in_init
  - >> GPIOTE_IRQHandler

  nrf_gpio_cfg (Thumb, 50 bytes, Stack size 40 bytes, nrfx_gpiote.o(i.nrf_gpio_cfg))
  [Stack]

  - Max Depth = 312
  - Call Chain = nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_pin_port_decode
  [Called By]
  - >> nrfx_gpiote_in_init

  nrf_gpio_cfg_sense_set (Thumb, 48 bytes, Stack size 16 bytes, nrfx_gpiote.o(i.nrf_gpio_cfg_sense_set))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrf_gpio_cfg_sense_set ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_pin_port_decode
  [Called By]
  - >> nrfx_gpiote_in_event_enable
  - >> GPIOTE_IRQHandler

  nrf_gpio_pin_port_decode (Thumb, 42 bytes, Stack size 8 bytes, nrfx_gpiote.o(i.nrf_gpio_pin_port_decode))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrfx_gpiote_in_init
  - >> GPIOTE_IRQHandler
  - >> nrf_gpio_pin_read
  - >> nrf_gpio_cfg_sense_set
  - >> nrf_gpio_cfg

  nrf_gpio_pin_read (Thumb, 22 bytes, Stack size 8 bytes, nrfx_gpiote.o(i.nrf_gpio_pin_read))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrf_gpio_pin_read ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_pin_port_decode
  [Called By]
  - >> nrfx_gpiote_in_is_set
  - >> nrfx_gpiote_in_event_enable

  nrf_gpio_ports_read (Thumb, 54 bytes, Stack size 24 bytes, nrfx_gpiote.o(i.nrf_gpio_ports_read))
  [Stack]

  - Max Depth = 288
  - Call Chain = nrf_gpio_ports_read ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> GPIOTE_IRQHandler

  nrf_gpiote_event_clear (Thumb, 16 bytes, Stack size 8 bytes, nrfx_gpiote.o(i.nrf_gpiote_event_clear))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_gpiote_event_clear
  [Called By]
  - >> nrfx_gpiote_init
  - >> nrfx_gpiote_in_event_enable
  - >> GPIOTE_IRQHandler

  nrf_gpiote_event_is_set (Thumb, 12 bytes, Stack size 0 bytes, nrfx_gpiote.o(i.nrf_gpiote_event_is_set))
  [Called By]

  - >> GPIOTE_IRQHandler

  pin_in_use_by_gpiote (Thumb, 14 bytes, Stack size 0 bytes, nrfx_gpiote.o(i.pin_in_use_by_gpiote))
  [Called By]

  - >> nrfx_gpiote_in_init
  - >> nrfx_gpiote_in_event_enable

  pin_in_use_by_port (Thumb, 20 bytes, Stack size 0 bytes, nrfx_gpiote.o(i.pin_in_use_by_port))
  [Called By]

  - >> nrfx_gpiote_in_event_enable

  pin_in_use_by_te (Thumb, 20 bytes, Stack size 0 bytes, nrfx_gpiote.o(i.pin_in_use_by_te))
  [Called By]

  - >> nrfx_gpiote_in_event_enable

  nrf_power_event_get_and_clear (Thumb, 28 bytes, Stack size 8 bytes, nrfx_power.o(i.nrf_power_event_get_and_clear))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_power_event_get_and_clear
  [Called By]
  - >> nrfx_power_irq_handler

  nrfx_power_clock_irq_init (Thumb, 28 bytes, Stack size 0 bytes, nrfx_power.o(i.nrfx_power_clock_irq_init))
  [Called By]

  - >> nrfx_power_init

  prs_box_get (Thumb, 14 bytes, Stack size 0 bytes, nrfx_prs.o(i.prs_box_get))
  [Called By]

  - >> nrfx_prs_release
  - >> nrfx_prs_acquire

  apply_config (Thumb, 118 bytes, Stack size 16 bytes, nrfx_uart.o(i.apply_config))
  [Stack]

  - Max Depth = 344
  - Call Chain = apply_config ⇒ nrf_gpio_cfg_output ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_pin_set
  - >> nrf_gpio_cfg_output
  - >> nrf_gpio_cfg_input
  [Called By]
  - >> nrfx_uart_init

  interrupts_enable (Thumb, 110 bytes, Stack size 16 bytes, nrfx_uart.o(i.interrupts_enable))
  [Stack]

  - Max Depth = 280
  - Call Chain = interrupts_enable ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_uart_event_clear
  [Called By]
  - >> nrfx_uart_init

  nrf_gpio_cfg (Thumb, 50 bytes, Stack size 40 bytes, nrfx_uart.o(i.nrf_gpio_cfg))
  [Stack]

  - Max Depth = 312
  - Call Chain = nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_pin_port_decode
  [Called By]
  - >> nrf_gpio_cfg_output
  - >> nrf_gpio_cfg_input
  - >> nrf_gpio_cfg_default

  nrf_gpio_cfg_default (Thumb, 18 bytes, Stack size 16 bytes, nrfx_uart.o(i.nrf_gpio_cfg_default))
  [Stack]

  - Max Depth = 328
  - Call Chain = nrf_gpio_cfg_default ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_cfg
  [Called By]
  - >> nrfx_uart_uninit

  nrf_gpio_cfg_input (Thumb, 18 bytes, Stack size 16 bytes, nrfx_uart.o(i.nrf_gpio_cfg_input))
  [Stack]

  - Max Depth = 328
  - Call Chain = nrf_gpio_cfg_input ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_cfg
  [Called By]
  - >> apply_config

  nrf_gpio_cfg_output (Thumb, 20 bytes, Stack size 16 bytes, nrfx_uart.o(i.nrf_gpio_cfg_output))
  [Stack]

  - Max Depth = 328
  - Call Chain = nrf_gpio_cfg_output ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_cfg
  [Called By]
  - >> apply_config

  nrf_gpio_pin_port_decode (Thumb, 42 bytes, Stack size 8 bytes, nrfx_uart.o(i.nrf_gpio_pin_port_decode))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrf_gpio_pin_set
  - >> nrf_gpio_cfg

  nrf_gpio_pin_set (Thumb, 20 bytes, Stack size 8 bytes, nrfx_uart.o(i.nrf_gpio_pin_set))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrf_gpio_pin_set ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_pin_port_decode
  [Called By]
  - >> apply_config

  nrf_uart_event_check (Thumb, 10 bytes, Stack size 0 bytes, nrfx_uart.o(i.nrf_uart_event_check))
  [Called By]

  - >> uart_irq_handler
  - >> nrfx_uart_tx
  - >> nrfx_uart_rx

  nrf_uart_event_clear (Thumb, 12 bytes, Stack size 8 bytes, nrfx_uart.o(i.nrf_uart_event_clear))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_uart_event_clear
  [Called By]
  - >> uart_irq_handler
  - >> tx_byte
  - >> rx_enable
  - >> rx_byte
  - >> interrupts_enable
  - >> nrfx_uart_tx
  - >> nrfx_uart_rx

  nrf_uart_int_enable_check (Thumb, 12 bytes, Stack size 0 bytes, nrfx_uart.o(i.nrf_uart_int_enable_check))
  [Called By]

  - >> uart_irq_handler

  rx_byte (Thumb, 50 bytes, Stack size 16 bytes, nrfx_uart.o(i.rx_byte))
  [Stack]

  - Max Depth = 24
  - Call Chain = rx_byte ⇒ nrf_uart_event_clear
  [Calls]
  - >> nrf_uart_event_clear
  [Called By]
  - >> uart_irq_handler
  - >> nrfx_uart_rx

  rx_done_event (Thumb, 22 bytes, Stack size 24 bytes, nrfx_uart.o(i.rx_done_event))
  [Stack]

  - Max Depth = 24
  - Call Chain = rx_done_event
  [Called By]
  - >> uart_irq_handler

  rx_enable (Thumb, 32 bytes, Stack size 8 bytes, nrfx_uart.o(i.rx_enable))
  [Stack]

  - Max Depth = 16
  - Call Chain = rx_enable ⇒ nrf_uart_event_clear
  [Calls]
  - >> nrf_uart_event_clear
  [Called By]
  - >> nrfx_uart_rx

  tx_byte (Thumb, 32 bytes, Stack size 16 bytes, nrfx_uart.o(i.tx_byte))
  [Stack]

  - Max Depth = 24
  - Call Chain = tx_byte ⇒ nrf_uart_event_clear
  [Calls]
  - >> nrf_uart_event_clear
  [Called By]
  - >> uart_irq_handler
  - >> nrfx_uart_tx

  tx_done_event (Thumb, 26 bytes, Stack size 24 bytes, nrfx_uart.o(i.tx_done_event))
  [Stack]

  - Max Depth = 24
  - Call Chain = tx_done_event
  [Called By]
  - >> uart_irq_handler

  uart_irq_handler (Thumb, 296 bytes, Stack size 48 bytes, nrfx_uart.o(i.uart_irq_handler))
  [Stack]

  - Max Depth = 72
  - Call Chain = uart_irq_handler ⇒ tx_done_event
  [Calls]
  - >> tx_done_event
  - >> tx_byte
  - >> rx_done_event
  - >> rx_byte
  - >> nrf_uart_int_enable_check
  - >> nrf_uart_event_clear
  - >> nrf_uart_event_check
  [Called By]
  - >> nrfx_uart_0_irq_handler

  apply_config (Thumb, 118 bytes, Stack size 16 bytes, nrfx_uarte.o(i.apply_config))
  [Stack]

  - Max Depth = 344
  - Call Chain = apply_config ⇒ nrf_gpio_cfg_output ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_pin_set
  - >> nrf_gpio_cfg_output
  - >> nrf_gpio_cfg_input
  [Called By]
  - >> nrfx_uarte_init

  interrupts_enable (Thumb, 130 bytes, Stack size 16 bytes, nrfx_uarte.o(i.interrupts_enable))
  [Stack]

  - Max Depth = 280
  - Call Chain = interrupts_enable ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_uarte_event_clear
  [Called By]
  - >> nrfx_uarte_init

  nrf_gpio_cfg (Thumb, 50 bytes, Stack size 40 bytes, nrfx_uarte.o(i.nrf_gpio_cfg))
  [Stack]

  - Max Depth = 312
  - Call Chain = nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_pin_port_decode
  [Called By]
  - >> nrf_gpio_cfg_output
  - >> nrf_gpio_cfg_input
  - >> nrf_gpio_cfg_default

  nrf_gpio_cfg_default (Thumb, 18 bytes, Stack size 16 bytes, nrfx_uarte.o(i.nrf_gpio_cfg_default))
  [Stack]

  - Max Depth = 328
  - Call Chain = nrf_gpio_cfg_default ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_cfg
  [Called By]
  - >> nrfx_uarte_uninit

  nrf_gpio_cfg_input (Thumb, 18 bytes, Stack size 16 bytes, nrfx_uarte.o(i.nrf_gpio_cfg_input))
  [Stack]

  - Max Depth = 328
  - Call Chain = nrf_gpio_cfg_input ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_cfg
  [Called By]
  - >> apply_config

  nrf_gpio_cfg_output (Thumb, 20 bytes, Stack size 16 bytes, nrfx_uarte.o(i.nrf_gpio_cfg_output))
  [Stack]

  - Max Depth = 328
  - Call Chain = nrf_gpio_cfg_output ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_cfg
  [Called By]
  - >> apply_config

  nrf_gpio_pin_port_decode (Thumb, 42 bytes, Stack size 8 bytes, nrfx_uarte.o(i.nrf_gpio_pin_port_decode))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrf_gpio_pin_set
  - >> nrf_gpio_cfg

  nrf_gpio_pin_set (Thumb, 20 bytes, Stack size 8 bytes, nrfx_uarte.o(i.nrf_gpio_pin_set))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrf_gpio_pin_set ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_gpio_pin_port_decode
  [Called By]
  - >> apply_config

  nrf_uarte_event_check (Thumb, 10 bytes, Stack size 0 bytes, nrfx_uarte.o(i.nrf_uarte_event_check))
  [Called By]

  - >> nrfx_uarte_tx
  - >> nrfx_uarte_rx
  - >> uarte_irq_handler

  nrf_uarte_event_clear (Thumb, 12 bytes, Stack size 8 bytes, nrfx_uarte.o(i.nrf_uarte_event_clear))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_uarte_event_clear
  [Called By]
  - >> nrfx_uarte_tx
  - >> nrfx_uarte_rx
  - >> uarte_irq_handler
  - >> interrupts_enable

  nrfx_is_in_ram (Thumb, 16 bytes, Stack size 0 bytes, nrfx_uarte.o(i.nrfx_is_in_ram))
  [Called By]

  - >> nrfx_uarte_tx
  - >> nrfx_uarte_rx

  rx_done_event (Thumb, 22 bytes, Stack size 24 bytes, nrfx_uarte.o(i.rx_done_event))
  [Stack]

  - Max Depth = 24
  - Call Chain = rx_done_event
  [Called By]
  - >> uarte_irq_handler

  uarte_irq_handler (Thumb, 242 bytes, Stack size 40 bytes, nrfx_uarte.o(i.uarte_irq_handler))
  [Stack]

  - Max Depth = 64
  - Call Chain = uarte_irq_handler ⇒ rx_done_event
  [Calls]
  - >> rx_done_event
  - >> nrf_uarte_event_clear
  - >> nrf_uarte_event_check
  [Called By]
  - >> nrfx_uarte_0_irq_handler

  _NRFX_IRQ_IS_ENABLED (Thumb, 36 bytes, Stack size 0 bytes, nrfx_usbd.o(i._NRFX_IRQ_IS_ENABLED))
  [Called By]

  - >> nrfx_usbd_stop
  - >> nrfx_usbd_is_started

  bit2ep (Thumb, 16 bytes, Stack size 0 bytes, nrfx_usbd.o(i.bit2ep))
  [Called By]

  - >> usbd_ep_abort_all
  - >> usbd_dmareq_process
  - >> ev_epdata_handler

  ep2bit (Thumb, 38 bytes, Stack size 8 bytes, nrfx_usbd.o(i.ep2bit))
  [Stack]

  - Max Depth = 272
  - Call Chain = ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrfx_usbd_transfer_out_drop
  - >> nrfx_usbd_ep_transfer
  - >> nrfx_usbd_ep_handled_transfer
  - >> nrfx_usbd_ep_enable
  - >> usbd_ep_abort
  - >> nrf_usbd_epout_dma_handler
  - >> nrf_usbd_epiniso_dma_handler
  - >> nrf_usbd_epin_dma_handler
  - >> ev_sof_handler
  - >> ev_setup_handler
  - >> ev_setup_data_handler
  - >> ev_dma_epout8_handler
  - >> ev_dma_epout0_handler
  - >> ev_dma_epin0_handler

  ep_state_access (Thumb, 50 bytes, Stack size 16 bytes, nrfx_usbd.o(i.ep_state_access))
  [Stack]

  - Max Depth = 280
  - Call Chain = ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrfx_usbd_init
  - >> nrfx_usbd_ep_transfer
  - >> nrfx_usbd_ep_max_packet_size_set
  - >> nrfx_usbd_ep_max_packet_size_get
  - >> nrfx_usbd_ep_handled_transfer
  - >> usbd_ep_abort
  - >> usbd_dmareq_process
  - >> nrf_usbd_epout_dma_handler
  - >> nrf_usbd_epiniso_dma_handler
  - >> nrf_usbd_epin_dma_handler
  - >> ev_dma_epout8_handler
  - >> ev_dma_epout0_handler
  - >> ev_dma_epin0_handler

  ep_to_hal (Thumb, 28 bytes, Stack size 8 bytes, nrfx_usbd.o(i.ep_to_hal))
  [Stack]

  - Max Depth = 272
  - Call Chain = ep_to_hal ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrfx_usbd_epout_size_get
  - >> nrfx_usbd_ep_stall_clear
  - >> nrfx_usbd_ep_stall_check
  - >> nrfx_usbd_ep_stall
  - >> nrfx_usbd_ep_enable_check
  - >> nrfx_usbd_ep_enable
  - >> nrfx_usbd_ep_disable

  ev_dma_epin0_handler (Thumb, 48 bytes, Stack size 8 bytes, nrfx_usbd.o(i.ev_dma_epin0_handler))
  [Stack]

  - Max Depth = 288
  - Call Chain = ev_dma_epin0_handler ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_atomic_u32_fetch_and
  - >> usbd_dma_pending_clear
  - >> ep_state_access
  - >> ep2bit
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_dma_epin1_handler (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.ev_dma_epin1_handler))
  [Stack]

  - Max Depth = 296
  - Call Chain = ev_dma_epin1_handler ⇒ nrf_usbd_epin_dma_handler ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_epin_dma_handler
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_dma_epin2_handler (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.ev_dma_epin2_handler))
  [Stack]

  - Max Depth = 296
  - Call Chain = ev_dma_epin2_handler ⇒ nrf_usbd_epin_dma_handler ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_epin_dma_handler
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_dma_epin3_handler (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.ev_dma_epin3_handler))
  [Stack]

  - Max Depth = 296
  - Call Chain = ev_dma_epin3_handler ⇒ nrf_usbd_epin_dma_handler ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_epin_dma_handler
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_dma_epin4_handler (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.ev_dma_epin4_handler))
  [Stack]

  - Max Depth = 296
  - Call Chain = ev_dma_epin4_handler ⇒ nrf_usbd_epin_dma_handler ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_epin_dma_handler
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_dma_epin5_handler (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.ev_dma_epin5_handler))
  [Stack]

  - Max Depth = 296
  - Call Chain = ev_dma_epin5_handler ⇒ nrf_usbd_epin_dma_handler ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_epin_dma_handler
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_dma_epin6_handler (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.ev_dma_epin6_handler))
  [Stack]

  - Max Depth = 296
  - Call Chain = ev_dma_epin6_handler ⇒ nrf_usbd_epin_dma_handler ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_epin_dma_handler
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_dma_epin7_handler (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.ev_dma_epin7_handler))
  [Stack]

  - Max Depth = 296
  - Call Chain = ev_dma_epin7_handler ⇒ nrf_usbd_epin_dma_handler ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_epin_dma_handler
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_dma_epin8_handler (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.ev_dma_epin8_handler))
  [Stack]

  - Max Depth = 296
  - Call Chain = ev_dma_epin8_handler ⇒ nrf_usbd_epiniso_dma_handler ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_epiniso_dma_handler
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_dma_epout0_handler (Thumb, 86 bytes, Stack size 16 bytes, nrfx_usbd.o(i.ev_dma_epout0_handler))
  [Stack]

  - Max Depth = 296
  - Call Chain = ev_dma_epout0_handler ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_atomic_u32_fetch_and
  - >> nrfx_usbd_setup_data_clear
  - >> usbd_dma_pending_clear
  - >> ep_state_access
  - >> ep2bit
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_dma_epout1_handler (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.ev_dma_epout1_handler))
  [Stack]

  - Max Depth = 376
  - Call Chain = ev_dma_epout1_handler ⇒ nrf_usbd_epout_dma_handler ⇒ usbd_dmareq_process ⇒ nrfx_systick_delay_us ⇒ nrfx_systick_delay_ticks ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_epout_dma_handler
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_dma_epout2_handler (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.ev_dma_epout2_handler))
  [Stack]

  - Max Depth = 376
  - Call Chain = ev_dma_epout2_handler ⇒ nrf_usbd_epout_dma_handler ⇒ usbd_dmareq_process ⇒ nrfx_systick_delay_us ⇒ nrfx_systick_delay_ticks ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_epout_dma_handler
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_dma_epout3_handler (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.ev_dma_epout3_handler))
  [Stack]

  - Max Depth = 376
  - Call Chain = ev_dma_epout3_handler ⇒ nrf_usbd_epout_dma_handler ⇒ usbd_dmareq_process ⇒ nrfx_systick_delay_us ⇒ nrfx_systick_delay_ticks ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_epout_dma_handler
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_dma_epout4_handler (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.ev_dma_epout4_handler))
  [Stack]

  - Max Depth = 376
  - Call Chain = ev_dma_epout4_handler ⇒ nrf_usbd_epout_dma_handler ⇒ usbd_dmareq_process ⇒ nrfx_systick_delay_us ⇒ nrfx_systick_delay_ticks ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_epout_dma_handler
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_dma_epout5_handler (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.ev_dma_epout5_handler))
  [Stack]

  - Max Depth = 376
  - Call Chain = ev_dma_epout5_handler ⇒ nrf_usbd_epout_dma_handler ⇒ usbd_dmareq_process ⇒ nrfx_systick_delay_us ⇒ nrfx_systick_delay_ticks ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_epout_dma_handler
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_dma_epout6_handler (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.ev_dma_epout6_handler))
  [Stack]

  - Max Depth = 376
  - Call Chain = ev_dma_epout6_handler ⇒ nrf_usbd_epout_dma_handler ⇒ usbd_dmareq_process ⇒ nrfx_systick_delay_us ⇒ nrfx_systick_delay_ticks ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_epout_dma_handler
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_dma_epout7_handler (Thumb, 6 bytes, Stack size 0 bytes, nrfx_usbd.o(i.ev_dma_epout7_handler))
  [Stack]

  - Max Depth = 376
  - Call Chain = ev_dma_epout7_handler ⇒ nrf_usbd_epout_dma_handler ⇒ usbd_dmareq_process ⇒ nrfx_systick_delay_us ⇒ nrfx_systick_delay_ticks ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_epout_dma_handler
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_dma_epout8_handler (Thumb, 66 bytes, Stack size 16 bytes, nrfx_usbd.o(i.ev_dma_epout8_handler))
  [Stack]

  - Max Depth = 296
  - Call Chain = ev_dma_epout8_handler ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_atomic_u32_fetch_and
  - >> usbd_dma_pending_clear
  - >> ep_state_access
  - >> ep2bit
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_epdata_handler (Thumb, 78 bytes, Stack size 16 bytes, nrfx_usbd.o(i.ev_epdata_handler))
  [Stack]

  - Max Depth = 376
  - Call Chain = ev_epdata_handler ⇒ usbd_dmareq_process ⇒ nrfx_systick_delay_us ⇒ nrfx_systick_delay_ticks ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> usbd_ep_data_handler
  - >> usbd_dmareq_process
  - >> nrfx_usbd_errata_104
  - >> bit2ep
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_setup_data_handler (Thumb, 22 bytes, Stack size 8 bytes, nrfx_usbd.o(i.ev_setup_data_handler))
  [Stack]

  - Max Depth = 280
  - Call Chain = ev_setup_data_handler ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> usbd_ep_data_handler
  - >> ep2bit
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_setup_handler (Thumb, 108 bytes, Stack size 24 bytes, nrfx_usbd.o(i.ev_setup_handler))
  [Stack]

  - Max Depth = 352
  - Call Chain = ev_setup_handler ⇒ usbd_ep_abort ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_atomic_u32_fetch_and
  - >> usbd_ep_abort
  - >> ep2bit
  [Called By]
  - >> USBD_IRQHandler
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_sof_handler (Thumb, 62 bytes, Stack size 16 bytes, nrfx_usbd.o(i.ev_sof_handler))
  [Stack]

  - Max Depth = 296
  - Call Chain = ev_sof_handler ⇒ nrf_usbd_episoout_size_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_usbd_episoout_size_get
  - >> ep2bit
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_started_handler (Thumb, 2 bytes, Stack size 0 bytes, nrfx_usbd.o(i.ev_started_handler))
  [Address Reference Count : 1]

  - nrfx_usbd.o(.constdata)

  ev_usbevent_handler (Thumb, 114 bytes, Stack size 24 bytes, nrfx_usbd.o(i.ev_usbevent_handler))
  [Stack]

  - Max Depth = 288
  - Call Chain = ev_usbevent_handler ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_usbd_task_trigger
  - >> nrf_usbd_lowpower_check
  - >> nrf_usbd_eventcause_clear
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  ev_usbreset_handler (Thumb, 24 bytes, Stack size 8 bytes, nrfx_usbd.o(i.ev_usbreset_handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = ev_usbreset_handler
  [Address Reference Count : 1]
  - nrfx_usbd.o(.constdata)

  nrf_usbd_ep_easydma_set (Thumb, 66 bytes, Stack size 12 bytes, nrfx_usbd.o(i.nrf_usbd_ep_easydma_set))
  [Stack]

  - Max Depth = 12
  - Call Chain = nrf_usbd_ep_easydma_set
  [Called By]
  - >> usbd_dmareq_process

  nrf_usbd_ep_enable_check (Thumb, 60 bytes, Stack size 8 bytes, nrfx_usbd.o(i.nrf_usbd_ep_enable_check))
  [Stack]

  - Max Depth = 272
  - Call Chain = nrf_usbd_ep_enable_check ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrfx_usbd_ep_enable_check
  - >> nrfx_usbd_ep_enable

  nrf_usbd_epin_dma_handler (Thumb, 96 bytes, Stack size 16 bytes, nrfx_usbd.o(i.nrf_usbd_epin_dma_handler))
  [Stack]

  - Max Depth = 296
  - Call Chain = nrf_usbd_epin_dma_handler ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_atomic_u32_fetch_and
  - >> assert_nrf_callback
  - >> usbd_dma_pending_clear
  - >> ep_state_access
  - >> ep2bit
  [Called By]
  - >> ev_dma_epin7_handler
  - >> ev_dma_epin6_handler
  - >> ev_dma_epin5_handler
  - >> ev_dma_epin4_handler
  - >> ev_dma_epin3_handler
  - >> ev_dma_epin2_handler
  - >> ev_dma_epin1_handler

  nrf_usbd_epiniso_dma_handler (Thumb, 118 bytes, Stack size 16 bytes, nrfx_usbd.o(i.nrf_usbd_epiniso_dma_handler))
  [Stack]

  - Max Depth = 296
  - Call Chain = nrf_usbd_epiniso_dma_handler ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_atomic_u32_fetch_and
  - >> assert_nrf_callback
  - >> usbd_dma_pending_clear
  - >> ep_state_access
  - >> ep2bit
  [Called By]
  - >> ev_dma_epin8_handler

  nrf_usbd_episoout_size_get (Thumb, 80 bytes, Stack size 16 bytes, nrfx_usbd.o(i.nrf_usbd_episoout_size_get))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrf_usbd_episoout_size_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> ev_sof_handler

  nrf_usbd_epout_dma_handler (Thumb, 136 bytes, Stack size 16 bytes, nrfx_usbd.o(i.nrf_usbd_epout_dma_handler))
  [Stack]

  - Max Depth = 376
  - Call Chain = nrf_usbd_epout_dma_handler ⇒ usbd_dmareq_process ⇒ nrfx_systick_delay_us ⇒ nrfx_systick_delay_ticks ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_atomic_u32_fetch_and
  - >> assert_nrf_callback
  - >> usbd_dmareq_process
  - >> usbd_dma_pending_clear
  - >> ep_state_access
  - >> ep2bit
  [Called By]
  - >> ev_dma_epout7_handler
  - >> ev_dma_epout6_handler
  - >> ev_dma_epout5_handler
  - >> ev_dma_epout4_handler
  - >> ev_dma_epout3_handler
  - >> ev_dma_epout2_handler
  - >> ev_dma_epout1_handler

  nrf_usbd_epout_size_get (Thumb, 74 bytes, Stack size 16 bytes, nrfx_usbd.o(i.nrf_usbd_epout_size_get))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrf_usbd_epout_size_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrfx_usbd_epout_size_get

  nrf_usbd_event_check (Thumb, 12 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrf_usbd_event_check))
  [Called By]

  - >> USBD_IRQHandler
  - >> usbd_dmareq_process

  nrf_usbd_event_clear (Thumb, 18 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrf_usbd_event_clear))
  [Called By]

  - >> USBD_IRQHandler
  - >> usbd_dmareq_process

  nrf_usbd_eventcause_clear (Thumb, 14 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrf_usbd_eventcause_clear))
  [Called By]

  - >> nrfx_usbd_enable
  - >> ev_usbevent_handler

  nrf_usbd_lowpower_check (Thumb, 12 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrf_usbd_lowpower_check))
  [Called By]

  - >> nrfx_usbd_wakeup_req
  - >> ev_usbevent_handler

  nrf_usbd_task_trigger (Thumb, 18 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrf_usbd_task_trigger))
  [Called By]

  - >> nrfx_usbd_setup_stall
  - >> nrfx_usbd_setup_data_clear
  - >> nrfx_usbd_setup_clear
  - >> usbd_dma_start
  - >> ev_usbevent_handler

  nrfx_is_in_ram (Thumb, 16 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrfx_is_in_ram))
  [Called By]

  - >> nrfx_usbd_feeder_ram_zlp
  - >> nrfx_usbd_feeder_ram
  - >> nrfx_usbd_feeder_flash_zlp
  - >> nrfx_usbd_feeder_flash
  - >> nrfx_usbd_ep_transfer
  - >> nrfx_usbd_consumer

  nrfx_usbd_ep_to_endevent (Thumb, 50 bytes, Stack size 16 bytes, nrfx_usbd.o(i.nrfx_usbd_ep_to_endevent))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrfx_usbd_ep_to_endevent ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> usbd_dmareq_process

  nrfx_usbd_ep_to_int (Thumb, 52 bytes, Stack size 16 bytes, nrfx_usbd.o(i.nrfx_usbd_ep_to_int))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrfx_usbd_ep_to_int ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrfx_usbd_ep_enable
  - >> nrfx_usbd_ep_disable

  nrfx_usbd_errata_104 (Thumb, 12 bytes, Stack size 8 bytes, nrfx_usbd.o(i.nrfx_usbd_errata_104))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrfx_usbd_errata_104
  [Calls]
  - >> nrfx_usbd_errata_type_52840_eng_b
  [Called By]
  - >> nrfx_usbd_start
  - >> nrfx_usbd_setup_data_clear
  - >> USBD_IRQHandler
  - >> usbd_dmareq_process
  - >> ev_epdata_handler

  nrfx_usbd_errata_type_52840_eng_b (Thumb, 26 bytes, Stack size 0 bytes, nrfx_usbd.o(i.nrfx_usbd_errata_type_52840_eng_b))
  [Called By]

  - >> nrfx_usbd_transfer_out_drop
  - >> nrfx_usbd_enable
  - >> nrfx_usbd_errata_104

  usbd_dma_pending_clear (Thumb, 12 bytes, Stack size 0 bytes, nrfx_usbd.o(i.usbd_dma_pending_clear))
  [Called By]

  - >> nrfx_usbd_enable
  - >> nrfx_usbd_disable
  - >> nrf_usbd_epout_dma_handler
  - >> nrf_usbd_epiniso_dma_handler
  - >> nrf_usbd_epin_dma_handler
  - >> ev_dma_epout8_handler
  - >> ev_dma_epout0_handler
  - >> ev_dma_epin0_handler

  usbd_dma_start (Thumb, 54 bytes, Stack size 16 bytes, nrfx_usbd.o(i.usbd_dma_start))
  [Stack]

  - Max Depth = 280
  - Call Chain = usbd_dma_start ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_usbd_task_trigger
  [Called By]
  - >> usbd_dmareq_process

  usbd_dmareq_process (Thumb, 342 bytes, Stack size 72 bytes, nrfx_usbd.o(i.usbd_dmareq_process))
  [Stack]

  - Max Depth = 360
  - Call Chain = usbd_dmareq_process ⇒ nrfx_systick_delay_us ⇒ nrfx_systick_delay_ticks ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_atomic_u32_fetch_and
  - >> assert_nrf_callback
  - >> nrfx_systick_delay_us
  - >> nrfx_usbd_epout_size_get
  - >> usbd_dma_start
  - >> nrfx_usbd_errata_104
  - >> nrfx_usbd_ep_to_endevent
  - >> nrf_usbd_event_clear
  - >> nrf_usbd_event_check
  - >> nrf_usbd_ep_easydma_set
  - >> ep_state_access
  - >> bit2ep
  [Called By]
  - >> USBD_IRQHandler
  - >> nrf_usbd_epout_dma_handler
  - >> ev_epdata_handler

  usbd_ep_abort (Thumb, 242 bytes, Stack size 32 bytes, nrfx_usbd.o(i.usbd_ep_abort))
  [Stack]

  - Max Depth = 328
  - Call Chain = usbd_ep_abort ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> nrfx_usbd_transfer_out_drop
  - >> ep_state_access
  - >> ep2bit
  [Called By]
  - >> nrfx_usbd_ep_disable
  - >> nrfx_usbd_ep_abort
  - >> usbd_ep_abort_all
  - >> ev_setup_handler

  usbd_ep_abort_all (Thumb, 72 bytes, Stack size 24 bytes, nrfx_usbd.o(i.usbd_ep_abort_all))
  [Stack]

  - Max Depth = 352
  - Call Chain = usbd_ep_abort_all ⇒ usbd_ep_abort ⇒ nrfx_usbd_transfer_out_drop ⇒ ep2bit ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> usbd_ep_abort
  - >> bit2ep
  [Called By]
  - >> nrfx_usbd_suspend
  - >> nrfx_usbd_stop

  usbd_ep_data_handler (Thumb, 56 bytes, Stack size 16 bytes, nrfx_usbd.o(i.usbd_ep_data_handler))
  [Stack]

  - Max Depth = 16
  - Call Chain = usbd_ep_data_handler
  [Called By]
  - >> ev_setup_data_handler
  - >> ev_epdata_handler

  usbd_int_rise (Thumb, 10 bytes, Stack size 0 bytes, nrfx_usbd.o(i.usbd_int_rise))
  [Called By]

  - >> nrfx_usbd_ep_transfer
  - >> nrfx_usbd_ep_handled_transfer

  detection_delay_timeout_handler (Thumb, 150 bytes, Stack size 32 bytes, app_button.o(i.detection_delay_timeout_handler))
  [Stack]

  - Max Depth = 320
  - Call Chain = detection_delay_timeout_handler ⇒ nrfx_gpiote_in_is_set ⇒ nrf_gpio_pin_read ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_gpiote_in_is_set
  - >> __aeabi_llsl
  [Address Reference Count : 1]
  - app_button.o(i.app_button_init)

  gpiote_event_handler (Thumb, 122 bytes, Stack size 24 bytes, app_button.o(i.gpiote_event_handler))
  [Stack]

  - Max Depth = 312
  - Call Chain = gpiote_event_handler ⇒ nrfx_gpiote_in_is_set ⇒ nrf_gpio_pin_read ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_timer_stop
  - >> app_timer_start
  - >> nrfx_gpiote_in_is_set
  - >> __aeabi_llsl
  [Address Reference Count : 1]
  - app_button.o(i.app_button_init)

  NVIC_ClearPendingIRQ (Thumb, 22 bytes, Stack size 0 bytes, app_timer.o(i.NVIC_ClearPendingIRQ))
  [Called By]

  - >> app_timer_init
  - >> compare_reg_update

  NVIC_EnableIRQ (Thumb, 22 bytes, Stack size 0 bytes, app_timer.o(i.NVIC_EnableIRQ))
  [Called By]

  - >> app_timer_init
  - >> compare_reg_update

  NVIC_SetPendingIRQ (Thumb, 22 bytes, Stack size 0 bytes, app_timer.o(i.NVIC_SetPendingIRQ))
  [Called By]

  - >> app_timer_start
  - >> timer_timeouts_check
  - >> timer_stop_op_schedule
  - >> compare_reg_update

  NVIC_SetPriority (Thumb, 32 bytes, Stack size 0 bytes, app_timer.o(i.NVIC_SetPriority))
  [Called By]

  - >> app_timer_init

  compare_reg_update (Thumb, 160 bytes, Stack size 40 bytes, app_timer.o(i.compare_reg_update))
  [Stack]

  - Max Depth = 56
  - Call Chain = compare_reg_update ⇒ rtc1_stop
  [Calls]
  - >> rtc1_stop
  - >> nrfx_coredep_delay_us
  - >> NVIC_SetPendingIRQ
  - >> NVIC_EnableIRQ
  - >> NVIC_ClearPendingIRQ
  [Called By]
  - >> timer_list_handler

  elapsed_ticks_acquire (Thumb, 58 bytes, Stack size 8 bytes, app_timer.o(i.elapsed_ticks_acquire))
  [Stack]

  - Max Depth = 8
  - Call Chain = elapsed_ticks_acquire
  [Called By]
  - >> timer_list_handler

  list_insertions_handler (Thumb, 234 bytes, Stack size 32 bytes, app_timer.o(i.list_insertions_handler))
  [Stack]

  - Max Depth = 56
  - Call Chain = list_insertions_handler ⇒ timer_list_remove
  [Calls]
  - >> timer_list_remove
  - >> timer_list_insert
  [Called By]
  - >> timer_list_handler

  nrfx_coredep_delay_us (Thumb, 12 bytes, Stack size 0 bytes, app_timer.o(i.nrfx_coredep_delay_us))
  [Called By]

  - >> timer_list_remove
  - >> rtc1_stop
  - >> compare_reg_update

  rtc1_stop (Thumb, 52 bytes, Stack size 16 bytes, app_timer.o(i.rtc1_stop))
  [Stack]

  - Max Depth = 16
  - Call Chain = rtc1_stop
  [Calls]
  - >> nrfx_coredep_delay_us
  [Called By]
  - >> app_timer_init
  - >> compare_reg_update

  timer_list_handler (Thumb, 122 bytes, Stack size 40 bytes, app_timer.o(i.timer_list_handler))
  [Stack]

  - Max Depth = 96
  - Call Chain = timer_list_handler ⇒ list_insertions_handler ⇒ timer_list_remove
  [Calls]
  - >> list_insertions_handler
  - >> elapsed_ticks_acquire
  - >> compare_reg_update
  [Called By]
  - >> SWI0_EGU0_IRQHandler

  timer_list_insert (Thumb, 56 bytes, Stack size 8 bytes, app_timer.o(i.timer_list_insert))
  [Stack]

  - Max Depth = 8
  - Call Chain = timer_list_insert
  [Called By]
  - >> list_insertions_handler

  timer_list_remove (Thumb, 88 bytes, Stack size 24 bytes, app_timer.o(i.timer_list_remove))
  [Stack]

  - Max Depth = 24
  - Call Chain = timer_list_remove
  [Calls]
  - >> nrfx_coredep_delay_us
  [Called By]
  - >> list_insertions_handler

  timer_stop_op_schedule (Thumb, 60 bytes, Stack size 24 bytes, app_timer.o(i.timer_stop_op_schedule))
  [Stack]

  - Max Depth = 32
  - Call Chain = timer_stop_op_schedule ⇒ app_util_critical_region_exit ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> user_op_alloc
  - >> NVIC_SetPendingIRQ
  [Called By]
  - >> app_timer_stop

  timer_timeouts_check (Thumb, 106 bytes, Stack size 24 bytes, app_timer.o(i.timer_timeouts_check))
  [Stack]

  - Max Depth = 24
  - Call Chain = timer_timeouts_check
  [Calls]
  - >> NVIC_SetPendingIRQ
  [Called By]
  - >> RTC1_IRQHandler

  user_op_alloc (Thumb, 42 bytes, Stack size 0 bytes, app_timer.o(i.user_op_alloc))
  [Called By]

  - >> app_timer_start
  - >> timer_stop_op_schedule

  app_usbd_class_iface_ep_get (Thumb, 36 bytes, Stack size 16 bytes, app_usbd.o(i.app_usbd_class_iface_ep_get))
  [Stack]

  - Max Depth = 280
  - Call Chain = app_usbd_class_iface_ep_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> app_usbd_init
  - >> app_usbd_class_append
  - >> app_usbd_iface_select
  - >> app_usbd_iface_deselect

  app_usbd_class_iface_get (Thumb, 38 bytes, Stack size 16 bytes, app_usbd.o(i.app_usbd_class_iface_get))
  [Stack]

  - Max Depth = 280
  - Call Chain = app_usbd_class_iface_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> app_usbd_init
  - >> app_usbd_class_append
  - >> app_usbd_iface_select
  - >> app_usbd_iface_find
  - >> app_usbd_iface_deselect

  app_usbd_class_next_get (Thumb, 22 bytes, Stack size 8 bytes, app_usbd.o(i.app_usbd_class_next_get))
  [Stack]

  - Max Depth = 272
  - Call Chain = app_usbd_class_next_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> app_usbd_iface_find
  - >> app_usbd_all_until_served_call
  - >> app_usbd_all_iface_select_0
  - >> app_usbd_all_iface_deselect
  - >> app_usbd_all_call

  app_usbd_core_handler_call (Thumb, 10 bytes, Stack size 0 bytes, app_usbd.o(i.app_usbd_core_handler_call))
  [Called By]

  - >> app_usbd_event_execute

  app_usbd_ep_conf_access (Thumb, 52 bytes, Stack size 8 bytes, app_usbd.o(i.app_usbd_ep_conf_access))
  [Stack]

  - Max Depth = 272
  - Call Chain = app_usbd_ep_conf_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> app_usbd_ep_instance_set
  - >> app_usbd_ep_instance_get
  - >> app_usbd_event_execute
  - >> app_usbd_ep_call

  app_usbd_ep_instance_get (Thumb, 10 bytes, Stack size 8 bytes, app_usbd.o(i.app_usbd_ep_instance_get))
  [Stack]

  - Max Depth = 280
  - Call Chain = app_usbd_ep_instance_get ⇒ app_usbd_ep_conf_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_usbd_ep_conf_access
  [Called By]
  - >> app_usbd_class_append

  app_usbd_ep_instance_set (Thumb, 44 bytes, Stack size 16 bytes, app_usbd.o(i.app_usbd_ep_instance_set))
  [Stack]

  - Max Depth = 288
  - Call Chain = app_usbd_ep_instance_set ⇒ app_usbd_ep_conf_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_usbd_ep_conf_access
  [Called By]
  - >> app_usbd_init
  - >> app_usbd_class_append

  app_usbd_event_add (Thumb, 36 bytes, Stack size 0 bytes, app_usbd.o(i.app_usbd_event_add))
  [Called By]

  - >> app_usbd_suspend_req
  - >> app_usbd_stop
  - >> app_usbd_start
  - >> app_usbd_power_event_handler
  - >> app_usbd_hfclk_ready
  - >> app_usbd_event_handler
  - >> app_usbd_wakeup_req

  app_usbd_event_handler (Thumb, 4 bytes, Stack size 0 bytes, app_usbd.o(i.app_usbd_event_handler))
  [Calls]

  - >> app_usbd_event_add
  [Address Reference Count : 1]
  - app_usbd.o(i.app_usbd_init)

  app_usbd_hfclk_ready (Thumb, 24 bytes, Stack size 8 bytes, app_usbd.o(i.app_usbd_hfclk_ready))
  [Stack]

  - Max Depth = 272
  - Call Chain = app_usbd_hfclk_ready ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_usbd_event_add
  [Address Reference Count : 1]
  - app_usbd.o(.data)

  app_usbd_power_event_handler (Thumb, 38 bytes, Stack size 0 bytes, app_usbd.o(i.app_usbd_power_event_handler))
  [Stack]

  - Max Depth = 264
  - Call Chain = app_usbd_power_event_handler ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_usbd_event_add
  [Address Reference Count : 1]
  - app_usbd.o(.constdata)

  app_usbd_sustate_with_requested_hfclk (Thumb, 26 bytes, Stack size 0 bytes, app_usbd.o(i.app_usbd_sustate_with_requested_hfclk))
  [Called By]

  - >> sustate_set
  - >> app_usbd_event_execute

  app_usbd_sustate_with_running_hfclk (Thumb, 26 bytes, Stack size 0 bytes, app_usbd.o(i.app_usbd_sustate_with_running_hfclk))
  [Called By]

  - >> sustate_set

  class_event_handler (Thumb, 62 bytes, Stack size 16 bytes, app_usbd.o(i.class_event_handler))
  [Stack]

  - Max Depth = 280
  - Call Chain = class_event_handler ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> app_usbd_init
  - >> app_usbd_class_append
  - >> app_usbd_iface_call
  - >> app_usbd_event_execute
  - >> app_usbd_ep_call
  - >> app_usbd_all_until_served_call
  - >> app_usbd_all_call

  sustate_set (Thumb, 84 bytes, Stack size 16 bytes, app_usbd.o(i.sustate_set))
  [Stack]

  - Max Depth = 304
  - Call Chain = sustate_set ⇒ nrf_drv_clock_hfclk_request ⇒ nrfx_clock_hfclk_start ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_drv_clock_hfclk_release
  - >> nrf_drv_clock_hfclk_request
  - >> nrfx_usbd_suspend_irq_config
  - >> nrfx_usbd_active_irq_config
  - >> app_usbd_sustate_with_running_hfclk
  - >> app_usbd_sustate_with_requested_hfclk
  [Called By]
  - >> app_usbd_event_execute

  user_event_state_proc (Thumb, 12 bytes, Stack size 0 bytes, app_usbd.o(i.user_event_state_proc))
  [Called By]

  - >> app_usbd_event_execute

  app_usbd_class_next_get (Thumb, 22 bytes, Stack size 8 bytes, app_usbd_core.o(i.app_usbd_class_next_get))
  [Stack]

  - Max Depth = 272
  - Call Chain = app_usbd_class_next_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> usbd_descriptor_conf_feeder
  - >> setup_device_req_get_descriptor

  app_usbd_core_event_handler (Thumb, 310 bytes, Stack size 24 bytes, app_usbd_core.o(i.app_usbd_core_event_handler))
  [Stack]

  - Max Depth = 472
  - Call Chain = app_usbd_core_event_handler ⇒ app_usbd_core_setup_req_handler ⇒ setup_device_req_std_handler ⇒ usbd_core_state_set ⇒ app_usbd_event_execute ⇒ app_usbd_event_execute (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_usbd_setup_stall
  - >> nrfx_usbd_setup_data_clear
  - >> nrfx_usbd_setup_clear
  - >> nrf_atomic_flag_clear_fetch
  - >> usbd_core_state_set
  - >> usb_core_ep0_handler_check
  - >> app_usbd_core_setup_req_handler
  [Address Reference Count : 1]
  - app_usbd_core.o(.constdata)

  app_usbd_core_setup_req_handler (Thumb, 192 bytes, Stack size 32 bytes, app_usbd_core.o(i.app_usbd_core_setup_req_handler))
  [Stack]

  - Max Depth = 448
  - Call Chain = app_usbd_core_setup_req_handler ⇒ setup_device_req_std_handler ⇒ usbd_core_state_set ⇒ app_usbd_event_execute ⇒ app_usbd_event_execute (Cycle)
  [Calls]
  - >> nrfx_usbd_setup_stall
  - >> nrfx_usbd_setup_get
  - >> nrfx_usbd_setup_data_clear
  - >> nrfx_usbd_setup_clear
  - >> nrfx_usbd_last_setup_dir_get
  - >> usb_core_ep0_handler_check
  - >> setup_interface_req_std_handle
  - >> setup_endpoint_req_std
  - >> setup_device_req_std_handler
  - >> app_usbd_iface_find
  - >> app_usbd_iface_call
  - >> app_usbd_ep_call
  - >> app_usbd_all_until_served_call
  [Called By]
  - >> app_usbd_core_event_handler

  setup_data_handler_empty (Thumb, 4 bytes, Stack size 0 bytes, app_usbd_core.o(i.setup_data_handler_empty))
  [Address Reference Count : 1]

  - app_usbd_core.o(.constdata)

  setup_device_req_get_descriptor (Thumb, 304 bytes, Stack size 40 bytes, app_usbd_core.o(i.setup_device_req_get_descriptor))
  [Stack]

  - Max Depth = 392
  - Call Chain = setup_device_req_get_descriptor ⇒ app_usbd_core_setup_rsp ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> app_usbd_string_desc_get
  - >> app_usbd_core_setup_transfer_buff_get
  - >> app_usbd_core_setup_rsp
  - >> app_usbd_core_setup_data_handler_set
  - >> app_usbd_class_next_get
  - >> app_usbd_ep_handled_transfer
  - >> app_usbd_class_rwu_enabled_check
  - >> app_usbd_class_first_get
  - >> __aeabi_memcpy
  [Called By]
  - >> setup_device_req_std_handler

  setup_device_req_get_status (Thumb, 68 bytes, Stack size 16 bytes, app_usbd_core.o(i.setup_device_req_get_status))
  [Stack]

  - Max Depth = 368
  - Call Chain = setup_device_req_get_status ⇒ app_usbd_core_setup_rsp ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_usbd_core_setup_transfer_buff_get
  - >> app_usbd_core_setup_rsp
  [Called By]
  - >> setup_device_req_std_handler

  setup_device_req_std_handler (Thumb, 260 bytes, Stack size 24 bytes, app_usbd_core.o(i.setup_device_req_std_handler))
  [Stack]

  - Max Depth = 416
  - Call Chain = setup_device_req_std_handler ⇒ usbd_core_state_set ⇒ app_usbd_event_execute ⇒ app_usbd_event_execute (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_usbd_core_setup_transfer_buff_get
  - >> app_usbd_core_setup_rsp
  - >> usbd_core_state_set
  - >> setup_device_req_get_status
  - >> setup_device_req_get_descriptor
  - >> app_usbd_class_rwu_enabled_check
  - >> app_usbd_all_iface_select_0
  - >> app_usbd_all_iface_deselect
  [Called By]
  - >> app_usbd_core_setup_req_handler

  setup_endpoint_req_std (Thumb, 144 bytes, Stack size 24 bytes, app_usbd_core.o(i.setup_endpoint_req_std))
  [Stack]

  - Max Depth = 376
  - Call Chain = setup_endpoint_req_std ⇒ app_usbd_core_setup_rsp ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_usbd_ep_stall_clear
  - >> nrfx_usbd_ep_stall_check
  - >> nrfx_usbd_ep_stall
  - >> nrfx_usbd_ep_dtoggle_clear
  - >> app_usbd_core_setup_transfer_buff_get
  - >> app_usbd_core_setup_rsp
  [Called By]
  - >> app_usbd_core_setup_req_handler

  setup_interface_req_std_handle (Thumb, 130 bytes, Stack size 24 bytes, app_usbd_core.o(i.setup_interface_req_std_handle))
  [Stack]

  - Max Depth = 376
  - Call Chain = setup_interface_req_std_handle ⇒ app_usbd_core_setup_rsp ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_usbd_core_setup_transfer_buff_get
  - >> app_usbd_core_setup_rsp
  - >> app_usbd_iface_selection_get
  - >> app_usbd_iface_select
  [Called By]
  - >> app_usbd_core_setup_req_handler

  usb_core_ep0_handler_check (Thumb, 12 bytes, Stack size 0 bytes, app_usbd_core.o(i.usb_core_ep0_handler_check))
  [Called By]

  - >> app_usbd_core_setup_req_handler
  - >> app_usbd_core_event_handler

  usbd_core_state_set (Thumb, 30 bytes, Stack size 0 bytes, app_usbd_core.o(i.usbd_core_state_set))
  [Stack]

  - Max Depth = 392
  - Call Chain = usbd_core_state_set ⇒ app_usbd_event_execute ⇒ app_usbd_event_execute (Cycle)
  [Calls]
  - >> app_usbd_event_execute
  [Called By]
  - >> setup_device_req_std_handler
  - >> app_usbd_core_event_handler

  usbd_descriptor_conf_feeder (Thumb, 258 bytes, Stack size 48 bytes, app_usbd_core.o(i.usbd_descriptor_conf_feeder))
  [Stack]

  - Max Depth = 320
  - Call Chain = usbd_descriptor_conf_feeder ⇒ app_usbd_class_next_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_usbd_feeder_buffer_get
  - >> app_usbd_class_next_get
  - >> __aeabi_memcpy
  [Address Reference Count : 1]
  - app_usbd_core.o(.constdata)

  app_usbd_clear_idle_ctx (Thumb, 38 bytes, Stack size 8 bytes, app_usbd_hid.o(i.app_usbd_clear_idle_ctx))
  [Stack]

  - Max Depth = 8
  - Call Chain = app_usbd_clear_idle_ctx
  [Called By]
  - >> app_usbd_hid_event_handler

  app_usbd_hid_state_flag_clr (Thumb, 10 bytes, Stack size 0 bytes, app_usbd_hid.o(i.app_usbd_hid_state_flag_clr))
  [Stack]

  - Max Depth = 8
  - Call Chain = app_usbd_hid_state_flag_clr ⇒ nrf_atomic_u32_and
  [Calls]
  - >> nrf_atomic_u32_and
  [Called By]
  - >> app_usbd_hid_event_handler
  - >> hid_sof_required
  - >> endpoint_in_event_handler

  app_usbd_hid_state_flag_set (Thumb, 10 bytes, Stack size 0 bytes, app_usbd_hid.o(i.app_usbd_hid_state_flag_set))
  [Stack]

  - Max Depth = 8
  - Call Chain = app_usbd_hid_state_flag_set ⇒ nrf_atomic_u32_or
  [Calls]
  - >> nrf_atomic_u32_or
  [Called By]
  - >> app_usbd_hid_event_handler

  endpoint_in_event_handler (Thumb, 94 bytes, Stack size 16 bytes, app_usbd_hid.o(i.endpoint_in_event_handler))
  [Stack]

  - Max Depth = 24
  - Call Chain = endpoint_in_event_handler ⇒ app_usbd_hid_state_flag_clr ⇒ nrf_atomic_u32_and
  [Calls]
  - >> user_event_handler
  - >> app_usbd_hid_state_flag_clr
  [Called By]
  - >> app_usbd_hid_event_handler

  hid_sof_required (Thumb, 132 bytes, Stack size 32 bytes, app_usbd_hid.o(i.hid_sof_required))
  [Stack]

  - Max Depth = 40
  - Call Chain = hid_sof_required ⇒ app_usbd_hid_state_flag_clr ⇒ nrf_atomic_u32_and
  [Calls]
  - >> app_usbd_hid_state_flag_clr
  [Called By]
  - >> app_usbd_hid_event_handler

  setup_event_handler (Thumb, 182 bytes, Stack size 24 bytes, app_usbd_hid.o(i.setup_event_handler))
  [Stack]

  - Max Depth = 408
  - Call Chain = setup_event_handler ⇒ setup_req_std_in ⇒ app_usbd_core_setup_rsp ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> setup_req_std_in
  - >> setup_req_class_out
  - >> app_usbd_core_setup_rsp
  [Called By]
  - >> app_usbd_hid_event_handler

  setup_req_class_out (Thumb, 152 bytes, Stack size 16 bytes, app_usbd_hid.o(i.setup_req_class_out))
  [Stack]

  - Max Depth = 16
  - Call Chain = setup_req_class_out
  [Calls]
  - >> user_event_handler
  [Called By]
  - >> setup_event_handler

  setup_req_std_in (Thumb, 116 bytes, Stack size 32 bytes, app_usbd_hid.o(i.setup_req_std_in))
  [Stack]

  - Max Depth = 384
  - Call Chain = setup_req_std_in ⇒ app_usbd_core_setup_rsp ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_usbd_core_setup_transfer_buff_get
  - >> app_usbd_core_setup_rsp
  - >> app_usbd_class_descriptor_find
  [Called By]
  - >> setup_event_handler

  user_event_handler (Thumb, 12 bytes, Stack size 0 bytes, app_usbd_hid.o(i.user_event_handler))
  [Called By]

  - >> app_usbd_hid_event_handler
  - >> setup_req_class_out
  - >> endpoint_in_event_handler

  app_usbd_class_iface_ep_get (Thumb, 36 bytes, Stack size 16 bytes, app_usbd_hid_generic.o(i.app_usbd_class_iface_ep_get))
  [Stack]

  - Max Depth = 280
  - Call Chain = app_usbd_class_iface_ep_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> hid_generic_clear_buffer
  - >> hid_generic_feed_descriptors
  - >> hid_generic_ep_transfer_out
  - >> app_usbd_hid_epin_addr_get

  app_usbd_class_iface_get (Thumb, 38 bytes, Stack size 16 bytes, app_usbd_hid_generic.o(i.app_usbd_class_iface_get))
  [Stack]

  - Max Depth = 280
  - Call Chain = app_usbd_class_iface_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> hid_generic_clear_buffer
  - >> hid_generic_feed_descriptors
  - >> hid_generic_ep_transfer_out
  - >> app_usbd_hid_epin_addr_get

  app_usbd_hid_epin_addr_get (Thumb, 18 bytes, Stack size 8 bytes, app_usbd_hid_generic.o(i.app_usbd_hid_epin_addr_get))
  [Stack]

  - Max Depth = 288
  - Call Chain = app_usbd_hid_epin_addr_get ⇒ app_usbd_class_iface_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_usbd_class_iface_get
  - >> app_usbd_class_iface_ep_get
  [Called By]
  - >> app_usbd_hid_generic_idle_report_set
  - >> hid_generic_transfer_set

  app_usbd_hid_rep_buff_out_get (Thumb, 20 bytes, Stack size 8 bytes, app_usbd_hid_generic.o(i.app_usbd_hid_rep_buff_out_get))
  [Stack]

  - Max Depth = 272
  - Call Chain = app_usbd_hid_rep_buff_out_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> hid_generic_on_set_report
  - >> hid_generic_ep_transfer_out

  app_usbd_hid_state_flag_clr (Thumb, 10 bytes, Stack size 0 bytes, app_usbd_hid_generic.o(i.app_usbd_hid_state_flag_clr))
  [Stack]

  - Max Depth = 8
  - Call Chain = app_usbd_hid_state_flag_clr ⇒ nrf_atomic_u32_and
  [Calls]
  - >> nrf_atomic_u32_and
  [Called By]
  - >> hid_generic_clear_buffer
  - >> app_usbd_hid_generic_idle_report_set
  - >> hid_generic_transfer_set
  - >> hid_generic_ep_transfer_in

  app_usbd_hid_state_flag_set (Thumb, 10 bytes, Stack size 0 bytes, app_usbd_hid_generic.o(i.app_usbd_hid_state_flag_set))
  [Stack]

  - Max Depth = 8
  - Call Chain = app_usbd_hid_state_flag_set ⇒ nrf_atomic_u32_or
  [Calls]
  - >> nrf_atomic_u32_or
  [Called By]
  - >> app_usbd_hid_generic_idle_report_set
  - >> hid_generic_transfer_set

  hid_generic_ctx_get (Thumb, 32 bytes, Stack size 8 bytes, app_usbd_hid_generic.o(i.hid_generic_ctx_get))
  [Stack]

  - Max Depth = 272
  - Call Chain = hid_generic_ctx_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> hid_generic_idle_handler_set
  - >> hid_generic_clear_buffer
  - >> app_usbd_hid_generic_in_report_set
  - >> app_usbd_hid_generic_idle_report_set
  - >> hid_generic_transfer_set
  - >> hid_generic_on_idle
  - >> hid_generic_event_handler
  - >> hid_generic_ep_transfer_in

  hid_generic_ep_transfer_in (Thumb, 46 bytes, Stack size 16 bytes, app_usbd_hid_generic.o(i.hid_generic_ep_transfer_in))
  [Stack]

  - Max Depth = 368
  - Call Chain = hid_generic_ep_transfer_in ⇒ hid_generic_transfer_set ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_queue_is_empty
  - >> hid_generic_transfer_set
  - >> hid_generic_get
  - >> hid_generic_ctx_get
  - >> app_usbd_hid_state_flag_clr
  [Address Reference Count : 1]
  - app_usbd_hid_generic.o(.constdata)

  hid_generic_ep_transfer_out (Thumb, 60 bytes, Stack size 24 bytes, app_usbd_hid_generic.o(i.hid_generic_ep_transfer_out))
  [Stack]

  - Max Depth = 344
  - Call Chain = hid_generic_ep_transfer_out ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> hid_generic_get
  - >> app_usbd_hid_rep_buff_out_get
  - >> app_usbd_class_iface_get
  - >> app_usbd_class_iface_ep_get
  - >> app_usbd_ep_transfer
  [Address Reference Count : 1]
  - app_usbd_hid_generic.o(.constdata)

  hid_generic_event_handler (Thumb, 60 bytes, Stack size 16 bytes, app_usbd_hid_generic.o(i.hid_generic_event_handler))
  [Stack]

  - Max Depth = 448
  - Call Chain = hid_generic_event_handler ⇒ app_usbd_hid_event_handler ⇒ setup_event_handler ⇒ setup_req_std_in ⇒ app_usbd_core_setup_rsp ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> hid_generic_get
  - >> hid_generic_ctx_get
  - >> app_usbd_hid_event_handler
  [Address Reference Count : 1]
  - app_usbd_hid_generic.o(.constdata)

  hid_generic_feed_descriptors (Thumb, 976 bytes, Stack size 40 bytes, app_usbd_hid_generic.o(i.hid_generic_feed_descriptors))
  [Stack]

  - Max Depth = 320
  - Call Chain = hid_generic_feed_descriptors ⇒ hid_generic_get_class_descriptors_length ⇒ hid_generic_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> hid_generic_get_class_descriptors_length
  - >> hid_generic_get_class_descriptors_count
  - >> hid_generic_get
  - >> app_usbd_class_iface_get
  - >> app_usbd_class_iface_ep_get
  [Address Reference Count : 1]
  - app_usbd_hid_generic.o(.constdata)

  hid_generic_get (Thumb, 18 bytes, Stack size 8 bytes, app_usbd_hid_generic.o(i.hid_generic_get))
  [Stack]

  - Max Depth = 272
  - Call Chain = hid_generic_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> hid_generic_idle_handler_set
  - >> hid_generic_clear_buffer
  - >> hid_generic_on_set_report
  - >> hid_generic_on_idle
  - >> hid_generic_on_get_report
  - >> hid_generic_get_class_descriptors_length
  - >> hid_generic_get_class_descriptors_data
  - >> hid_generic_get_class_descriptors_count
  - >> hid_generic_feed_descriptors
  - >> hid_generic_event_handler
  - >> hid_generic_ep_transfer_out
  - >> hid_generic_ep_transfer_in

  hid_generic_get_class_descriptors_count (Thumb, 10 bytes, Stack size 8 bytes, app_usbd_hid_generic.o(i.hid_generic_get_class_descriptors_count))
  [Stack]

  - Max Depth = 280
  - Call Chain = hid_generic_get_class_descriptors_count ⇒ hid_generic_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> hid_generic_get
  [Called By]
  - >> hid_generic_feed_descriptors

  hid_generic_get_class_descriptors_data (Thumb, 22 bytes, Stack size 16 bytes, app_usbd_hid_generic.o(i.hid_generic_get_class_descriptors_data))
  [Stack]

  - Max Depth = 288
  - Call Chain = hid_generic_get_class_descriptors_data ⇒ hid_generic_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> hid_generic_get
  [Address Reference Count : 1]
  - app_usbd_hid_generic.o(.constdata)

  hid_generic_get_class_descriptors_length (Thumb, 18 bytes, Stack size 8 bytes, app_usbd_hid_generic.o(i.hid_generic_get_class_descriptors_length))
  [Stack]

  - Max Depth = 280
  - Call Chain = hid_generic_get_class_descriptors_length ⇒ hid_generic_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> hid_generic_get
  [Called By]
  - >> hid_generic_feed_descriptors
  [Address Reference Count : 1]
  - app_usbd_hid_generic.o(.constdata)

  hid_generic_on_get_report (Thumb, 52 bytes, Stack size 16 bytes, app_usbd_hid_generic.o(i.hid_generic_on_get_report))
  [Stack]

  - Max Depth = 368
  - Call Chain = hid_generic_on_get_report ⇒ app_usbd_core_setup_rsp ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_usbd_hid_generic_out_report_get
  - >> app_usbd_hid_generic_in_report_get
  - >> hid_generic_get
  - >> app_usbd_core_setup_rsp
  [Address Reference Count : 1]
  - app_usbd_hid_generic.o(.constdata)

  hid_generic_on_idle (Thumb, 32 bytes, Stack size 16 bytes, app_usbd_hid_generic.o(i.hid_generic_on_idle))
  [Stack]

  - Max Depth = 288
  - Call Chain = hid_generic_on_idle ⇒ hid_generic_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> hid_generic_get
  - >> hid_generic_ctx_get
  [Address Reference Count : 1]
  - app_usbd_hid_generic.o(.constdata)

  hid_generic_on_set_report (Thumb, 92 bytes, Stack size 32 bytes, app_usbd_hid_generic.o(i.hid_generic_on_set_report))
  [Stack]

  - Max Depth = 352
  - Call Chain = hid_generic_on_set_report ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> hid_generic_get
  - >> app_usbd_hid_rep_buff_out_get
  - >> app_usbd_core_setup_data_handler_set
  - >> app_usbd_ep_transfer
  [Address Reference Count : 1]
  - app_usbd_hid_generic.o(.constdata)

  hid_generic_on_set_report_data_cb (Thumb, 22 bytes, Stack size 8 bytes, app_usbd_hid_generic.o(i.hid_generic_on_set_report_data_cb))
  [Stack]

  - Max Depth = 8
  - Call Chain = hid_generic_on_set_report_data_cb
  [Address Reference Count : 1]
  - app_usbd_hid_generic.o(.constdata)

  hid_generic_rep_buffer_get (Thumb, 26 bytes, Stack size 8 bytes, app_usbd_hid_generic.o(i.hid_generic_rep_buffer_get))
  [Stack]

  - Max Depth = 280
  - Call Chain = hid_generic_rep_buffer_get ⇒ app_usbd_hid_rep_buff_in_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_usbd_hid_rep_buff_in_get
  [Called By]
  - >> hid_generic_clear_buffer
  - >> hid_generic_transfer_set

  hid_generic_transfer_set (Thumb, 118 bytes, Stack size 32 bytes, app_usbd_hid_generic.o(i.hid_generic_transfer_set))
  [Stack]

  - Max Depth = 352
  - Call Chain = hid_generic_transfer_set ⇒ app_usbd_ep_transfer ⇒ nrfx_usbd_ep_transfer ⇒ ep_state_access ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> nrf_queue_is_empty
  - >> nrf_queue_generic_pop
  - >> hid_generic_rep_buffer_get
  - >> hid_generic_ctx_get
  - >> app_usbd_hid_state_flag_set
  - >> app_usbd_hid_state_flag_clr
  - >> app_usbd_hid_epin_addr_get
  - >> app_usbd_ep_transfer
  [Called By]
  - >> app_usbd_hid_generic_in_report_set
  - >> hid_generic_ep_transfer_in

  app_usbd_prepare_string (Thumb, 94 bytes, Stack size 24 bytes, app_usbd_string_desc.o(i.app_usbd_prepare_string))
  [Stack]

  - Max Depth = 288
  - Call Chain = app_usbd_prepare_string ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_usbd_core_setup_transfer_buff_get
  [Called By]
  - >> app_usbd_string_desc_get

  nrf_balloc_status (Thumb, 196 bytes, Stack size 72 bytes, nrf_balloc.o(i.nrf_balloc_status))
  [Stack]

  - Max Depth = 648
  - Call Chain = nrf_balloc_status ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_cli_help_print
  - >> nrf_cli_fprintf
  [Address Reference Count : 2]
  - nrf_balloc.o(.constdata)
  - nrf_balloc.o(.constdata)

  char_backspace (Thumb, 170 bytes, Stack size 16 bytes, nrf_cli.o(i.char_backspace))
  [Stack]

  - Max Depth = 520
  - Call Chain = char_backspace ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> cli_cursor_save
  - >> cli_cursor_restore
  - >> cli_clear_eos
  - >> nrf_cli_fprintf
  - >> nrf_fprintf
  - >> multiline_console_data_check
  - >> cursor_left_move
  - >> __aeabi_memmove
  [Called By]
  - >> cli_state_collect

  char_delete (Thumb, 166 bytes, Stack size 16 bytes, nrf_cli.o(i.char_delete))
  [Stack]

  - Max Depth = 520
  - Call Chain = char_delete ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> cli_cursor_save
  - >> cli_cursor_restore
  - >> cli_clear_eos
  - >> nrf_cli_fprintf
  - >> nrf_fprintf
  - >> multiline_console_data_check
  - >> cursor_left_move
  - >> __aeabi_memmove
  [Called By]
  - >> cli_state_collect

  char_insert (Thumb, 312 bytes, Stack size 24 bytes, nrf_cli.o(i.char_insert))
  [Stack]

  - Max Depth = 528
  - Call Chain = char_insert ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> cursor_down_move
  - >> cli_cursor_save
  - >> cli_cursor_restore
  - >> nrf_cli_fprintf
  - >> nrf_fprintf
  - >> multiline_console_data_check
  - >> full_line_cmd
  - >> cursor_up_move
  - >> cursor_right_move
  - >> cursor_next_line_move
  - >> cursor_left_move
  - >> cursor_in_empty_line
  - >> __aeabi_memmove
  [Called By]
  - >> cli_tab_handle
  - >> cli_state_collect

  cli_clear_eos (Thumb, 44 bytes, Stack size 16 bytes, nrf_cli.o(i.cli_clear_eos))
  [Stack]

  - Max Depth = 464
  - Call Chain = cli_clear_eos ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_fprintf
  [Called By]
  - >> cli_log_entry_process
  - >> char_delete
  - >> char_backspace
  - >> history_handle

  cli_cursor_restore (Thumb, 44 bytes, Stack size 16 bytes, nrf_cli.o(i.cli_cursor_restore))
  [Stack]

  - Max Depth = 464
  - Call Chain = cli_cursor_restore ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_fprintf
  [Called By]
  - >> char_insert
  - >> char_delete
  - >> char_backspace

  cli_cursor_save (Thumb, 44 bytes, Stack size 16 bytes, nrf_cli.o(i.cli_cursor_save))
  [Stack]

  - Max Depth = 464
  - Call Chain = cli_cursor_save ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_fprintf
  [Called By]
  - >> char_insert
  - >> char_delete
  - >> char_backspace

  cli_execute (Thumb, 374 bytes, Stack size 120 bytes, nrf_cli.o(i.cli_execute))
  [Stack]

  - Max Depth = 624
  - Call Chain = cli_execute ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> cursor_end_position_move
  - >> cmd_trim
  - >> cmd_get
  - >> nrf_cli_fprintf
  - >> make_argv
  - >> history_save
  - >> cursor_next_line_move
  - >> cursor_in_empty_line
  - >> strcmp
  [Called By]
  - >> cli_state_collect

  cli_flag_echo_is_set (Thumb, 12 bytes, Stack size 0 bytes, nrf_cli.o(i.cli_flag_echo_is_set))
  [Called By]

  - >> nrf_cli_process
  - >> cli_state_collect
  - >> nrf_cli_cmd_echo

  cli_log_entry_process (Thumb, 314 bytes, Stack size 80 bytes, nrf_cli.o(i.cli_log_entry_process))
  [Stack]

  - Max Depth = 592
  - Call Chain = cli_log_entry_process ⇒ nrf_log_std_entry_process ⇒ prefix_process ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_queue_generic_pop
  - >> cli_clear_eos
  - >> nrf_cli_fprintf
  - >> nrf_memobj_read
  - >> nrf_memobj_put
  - >> nrf_log_std_entry_process
  - >> nrf_log_hexdump_entry_process
  - >> multiline_console_data_check
  - >> cursor_up_move
  - >> cursor_left_move
  [Called By]
  - >> nrf_cli_process
  - >> nrf_log_backend_cli_put
  - >> nrf_log_backend_cli_flush

  cli_read (Thumb, 60 bytes, Stack size 24 bytes, nrf_cli.o(i.cli_read))
  [Stack]

  - Max Depth = 288
  - Call Chain = cli_read ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> cli_state_collect
  - >> cursor_position_get

  cli_state_collect (Thumb, 628 bytes, Stack size 32 bytes, nrf_cli.o(i.cli_state_collect))
  [Stack]

  - Max Depth = 760
  - Call Chain = cli_state_collect ⇒ cli_tab_handle ⇒ option_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> cursor_home_position_move
  - >> cursor_end_position_move
  - >> cursor_down_move
  - >> cli_tab_handle
  - >> cli_state_set
  - >> cli_read
  - >> cli_flag_echo_is_set
  - >> cli_execute
  - >> char_insert
  - >> char_delete
  - >> char_backspace
  - >> nrf_pwr_mgmt_feed
  - >> multiline_console_data_check
  - >> history_handle
  - >> cursor_up_move
  - >> cursor_right_move
  - >> cursor_next_line_move
  - >> cursor_left_move
  - >> __rt_ctype_table
  [Called By]
  - >> nrf_cli_process

  cli_state_set (Thumb, 36 bytes, Stack size 0 bytes, nrf_cli.o(i.cli_state_set))
  [Stack]

  - Max Depth = 504
  - Call Chain = cli_state_set ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_fprintf
  [Called By]
  - >> nrf_cli_start
  - >> cli_state_collect

  cli_strlen (Thumb, 10 bytes, Stack size 0 bytes, nrf_cli.o(i.cli_strlen))
  [Calls]

  - >> strlen
  [Called By]
  - >> completion_insert
  - >> cli_tab_handle
  - >> nrf_cli_help_print
  - >> option_print
  - >> multiline_console_data_check
  - >> make_argv
  - >> history_save
  - >> history_handle
  - >> full_line_cmd
  - >> format_offset_string_print
  - >> cursor_in_empty_line

  cli_tab_handle (Thumb, 740 bytes, Stack size 192 bytes, nrf_cli.o(i.cli_tab_handle))
  [Stack]

  - Max Depth = 728
  - Call Chain = cli_tab_handle ⇒ option_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> completion_insert
  - >> cmd_get
  - >> cli_strlen
  - >> char_insert
  - >> nrf_cli_fprintf
  - >> option_print
  - >> multiline_console_data_check
  - >> make_argv
  - >> is_completion_candidate
  - >> cursor_right_move
  - >> cursor_position_synchronize
  - >> cursor_next_line_move
  - >> strcmp
  - >> __aeabi_memcpy4
  - >> __rt_ctype_table
  [Called By]
  - >> cli_state_collect

  cli_transport_evt_handler (Thumb, 38 bytes, Stack size 16 bytes, nrf_cli.o(i.cli_transport_evt_handler))
  [Stack]

  - Max Depth = 280
  - Call Chain = cli_transport_evt_handler ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Address Reference Count : 1]
  - nrf_cli.o(i.nrf_cli_instance_init)

  cli_write (Thumb, 144 bytes, Stack size 32 bytes, nrf_cli.o(i.cli_write))
  [Stack]

  - Max Depth = 296
  - Call Chain = cli_write ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrf_cli_print_stream
  - >> format_offset_string_print

  cmd_get (Thumb, 150 bytes, Stack size 40 bytes, nrf_cli.o(i.cmd_get))
  [Stack]

  - Max Depth = 304
  - Call Chain = cmd_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> strcmp
  [Called By]
  - >> cli_tab_handle
  - >> cli_execute
  - >> nrf_cli_help_print

  cmd_trim (Thumb, 154 bytes, Stack size 24 bytes, nrf_cli.o(i.cmd_trim))
  [Stack]

  - Max Depth = 32
  - Call Chain = cmd_trim ⇒ __aeabi_memmove
  [Calls]
  - >> __aeabi_memmove
  - >> __rt_ctype_table
  [Called By]
  - >> cli_execute

  completion_insert (Thumb, 154 bytes, Stack size 24 bytes, nrf_cli.o(i.completion_insert))
  [Stack]

  - Max Depth = 528
  - Call Chain = completion_insert ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> cli_strlen
  - >> nrf_cli_fprintf
  - >> full_line_cmd
  - >> cursor_position_synchronize
  - >> cursor_next_line_move
  - >> cursor_in_empty_line
  - >> __aeabi_memmove
  [Called By]
  - >> cli_tab_handle

  cursor_down_move (Thumb, 16 bytes, Stack size 0 bytes, nrf_cli.o(i.cursor_down_move))
  [Stack]

  - Max Depth = 448
  - Call Chain = cursor_down_move ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_fprintf
  [Called By]
  - >> cursor_end_position_move
  - >> cli_state_collect
  - >> char_insert
  - >> terminal_size_get

  cursor_end_position_move (Thumb, 82 bytes, Stack size 16 bytes, nrf_cli.o(i.cursor_end_position_move))
  [Stack]

  - Max Depth = 464
  - Call Chain = cursor_end_position_move ⇒ cursor_down_move ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> cursor_down_move
  - >> multiline_console_data_check
  - >> cursor_right_move
  - >> cursor_left_move
  [Called By]
  - >> cli_state_collect
  - >> cli_execute

  cursor_home_position_move (Thumb, 84 bytes, Stack size 16 bytes, nrf_cli.o(i.cursor_home_position_move))
  [Stack]

  - Max Depth = 464
  - Call Chain = cursor_home_position_move ⇒ cursor_up_move ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> multiline_console_data_check
  - >> cursor_up_move
  - >> cursor_right_move
  - >> cursor_left_move
  [Called By]
  - >> cli_state_collect
  - >> history_handle

  cursor_in_empty_line (Thumb, 38 bytes, Stack size 8 bytes, nrf_cli.o(i.cursor_in_empty_line))
  [Stack]

  - Max Depth = 8
  - Call Chain = cursor_in_empty_line
  [Calls]
  - >> cli_strlen
  [Called By]
  - >> completion_insert
  - >> cli_execute
  - >> char_insert
  - >> history_handle
  - >> cursor_position_synchronize

  cursor_left_move (Thumb, 16 bytes, Stack size 0 bytes, nrf_cli.o(i.cursor_left_move))
  [Stack]

  - Max Depth = 448
  - Call Chain = cursor_left_move ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_fprintf
  [Called By]
  - >> cursor_home_position_move
  - >> cursor_end_position_move
  - >> cli_state_collect
  - >> cli_log_entry_process
  - >> char_insert
  - >> char_delete
  - >> char_backspace
  - >> terminal_size_get
  - >> cursor_position_synchronize

  cursor_next_line_move (Thumb, 8 bytes, Stack size 0 bytes, nrf_cli.o(i.cursor_next_line_move))
  [Stack]

  - Max Depth = 448
  - Call Chain = cursor_next_line_move ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_fprintf
  [Called By]
  - >> completion_insert
  - >> cli_tab_handle
  - >> cli_state_collect
  - >> cli_execute
  - >> char_insert
  - >> nrf_cli_help_print
  - >> history_handle
  - >> format_offset_string_print
  - >> cursor_position_synchronize

  cursor_position_get (Thumb, 288 bytes, Stack size 40 bytes, nrf_cli.o(i.cursor_position_get))
  [Stack]

  - Max Depth = 488
  - Call Chain = cursor_position_get ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> cli_read
  - >> nrf_fprintf_buffer_flush
  - >> nrf_fprintf
  - >> __aeabi_memclr4
  [Called By]
  - >> terminal_size_get

  cursor_position_synchronize (Thumb, 106 bytes, Stack size 16 bytes, nrf_cli.o(i.cursor_position_synchronize))
  [Stack]

  - Max Depth = 464
  - Call Chain = cursor_position_synchronize ⇒ cursor_up_move ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> multiline_console_data_check
  - >> full_line_cmd
  - >> cursor_up_move
  - >> cursor_right_move
  - >> cursor_next_line_move
  - >> cursor_left_move
  - >> cursor_in_empty_line
  [Called By]
  - >> nrf_cli_process
  - >> completion_insert
  - >> cli_tab_handle

  cursor_right_move (Thumb, 16 bytes, Stack size 0 bytes, nrf_cli.o(i.cursor_right_move))
  [Stack]

  - Max Depth = 448
  - Call Chain = cursor_right_move ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_fprintf
  [Called By]
  - >> cursor_home_position_move
  - >> cursor_end_position_move
  - >> cli_tab_handle
  - >> cli_state_collect
  - >> char_insert
  - >> nrf_cli_help_print
  - >> terminal_size_get
  - >> option_print
  - >> format_offset_string_print
  - >> cursor_position_synchronize

  cursor_up_move (Thumb, 16 bytes, Stack size 0 bytes, nrf_cli.o(i.cursor_up_move))
  [Stack]

  - Max Depth = 448
  - Call Chain = cursor_up_move ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_fprintf
  [Called By]
  - >> cursor_home_position_move
  - >> cli_state_collect
  - >> cli_log_entry_process
  - >> char_insert
  - >> terminal_size_get
  - >> cursor_position_synchronize

  format_offset_string_print (Thumb, 242 bytes, Stack size 40 bytes, nrf_cli.o(i.format_offset_string_print))
  [Stack]

  - Max Depth = 488
  - Call Chain = format_offset_string_print ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> cli_write
  - >> cli_strlen
  - >> nrf_fprintf_buffer_flush
  - >> nrf_fprintf
  - >> cursor_right_move
  - >> cursor_next_line_move
  - >> __rt_ctype_table
  [Called By]
  - >> nrf_cli_help_print

  full_line_cmd (Thumb, 38 bytes, Stack size 8 bytes, nrf_cli.o(i.full_line_cmd))
  [Stack]

  - Max Depth = 8
  - Call Chain = full_line_cmd
  [Calls]
  - >> cli_strlen
  [Called By]
  - >> completion_insert
  - >> char_insert
  - >> history_handle
  - >> cursor_position_synchronize

  history_handle (Thumb, 320 bytes, Stack size 32 bytes, nrf_cli.o(i.history_handle))
  [Stack]

  - Max Depth = 536
  - Call Chain = history_handle ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> cursor_home_position_move
  - >> cli_strlen
  - >> cli_clear_eos
  - >> nrf_cli_fprintf
  - >> nrf_memobj_read
  - >> full_line_cmd
  - >> cursor_next_line_move
  - >> cursor_in_empty_line
  - >> strcpy
  [Called By]
  - >> cli_state_collect

  history_list_element_add (Thumb, 132 bytes, Stack size 32 bytes, nrf_cli.o(i.history_list_element_add))
  [Stack]

  - Max Depth = 312
  - Call Chain = history_list_element_add ⇒ nrf_memobj_read ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_memobj_write
  - >> nrf_memobj_read
  [Called By]
  - >> history_save

  history_list_element_oldest_remove (Thumb, 104 bytes, Stack size 32 bytes, nrf_cli.o(i.history_list_element_oldest_remove))
  [Stack]

  - Max Depth = 312
  - Call Chain = history_list_element_oldest_remove ⇒ nrf_memobj_read ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_memobj_write
  - >> nrf_memobj_read
  - >> nrf_memobj_free
  [Called By]
  - >> history_save

  history_save (Thumb, 134 bytes, Stack size 32 bytes, nrf_cli.o(i.history_save))
  [Stack]

  - Max Depth = 344
  - Call Chain = history_save ⇒ history_list_element_oldest_remove ⇒ nrf_memobj_read ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> cli_strlen
  - >> nrf_memobj_read
  - >> nrf_memobj_alloc
  - >> history_list_element_oldest_remove
  - >> history_list_element_add
  - >> strcmp
  [Called By]
  - >> cli_execute

  is_completion_candidate (Thumb, 16 bytes, Stack size 8 bytes, nrf_cli.o(i.is_completion_candidate))
  [Stack]

  - Max Depth = 20
  - Call Chain = is_completion_candidate ⇒ strncmp
  [Calls]
  - >> strncmp
  [Called By]
  - >> cli_tab_handle

  make_argv (Thumb, 364 bytes, Stack size 56 bytes, nrf_cli.o(i.make_argv))
  [Stack]

  - Max Depth = 320
  - Call Chain = make_argv ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> cli_strlen
  - >> __aeabi_memmove
  - >> __rt_ctype_table
  [Called By]
  - >> cli_tab_handle
  - >> cli_execute

  multiline_console_data_check (Thumb, 80 bytes, Stack size 16 bytes, nrf_cli.o(i.multiline_console_data_check))
  [Stack]

  - Max Depth = 16
  - Call Chain = multiline_console_data_check
  [Calls]
  - >> cli_strlen
  [Called By]
  - >> cursor_home_position_move
  - >> cursor_end_position_move
  - >> cli_tab_handle
  - >> cli_state_collect
  - >> cli_log_entry_process
  - >> char_insert
  - >> char_delete
  - >> char_backspace
  - >> cursor_position_synchronize

  nrf_cli_build_in_cmd_common_executed (Thumb, 46 bytes, Stack size 16 bytes, nrf_cli.o(i.nrf_cli_build_in_cmd_common_executed))
  [Stack]

  - Max Depth = 592
  - Call Chain = nrf_cli_build_in_cmd_common_executed ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_help_print
  - >> nrf_cli_fprintf
  [Called By]
  - >> nrf_cli_cmd_cli_stats_show
  - >> nrf_cli_cmd_cli_stats_reset
  - >> nrf_cli_cmd_cli_stats
  - >> nrf_cli_cmd_resize_default
  - >> nrf_cli_cmd_resize
  - >> nrf_cli_cmd_history
  - >> nrf_cli_cmd_echo_on
  - >> nrf_cli_cmd_echo_off
  - >> nrf_cli_cmd_echo
  - >> nrf_cli_cmd_colors_on
  - >> nrf_cli_cmd_colors_off
  - >> nrf_cli_cmd_colors

  nrf_cli_cmd_clear (Thumb, 148 bytes, Stack size 16 bytes, nrf_cli.o(i.nrf_cli_cmd_clear))
  [Stack]

  - Max Depth = 592
  - Call Chain = nrf_cli_cmd_clear ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_cli_help_print
  - >> nrf_fprintf
  [Address Reference Count : 1]
  - nrf_cli.o(.constdata)

  nrf_cli_cmd_cli (Thumb, 88 bytes, Stack size 16 bytes, nrf_cli.o(i.nrf_cli_cmd_cli))
  [Stack]

  - Max Depth = 592
  - Call Chain = nrf_cli_cmd_cli ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_cli_help_print
  - >> nrf_cli_fprintf
  [Address Reference Count : 1]
  - nrf_cli.o(.constdata)

  nrf_cli_cmd_colors (Thumb, 108 bytes, Stack size 24 bytes, nrf_cli.o(i.nrf_cli_cmd_colors))
  [Stack]

  - Max Depth = 616
  - Call Chain = nrf_cli_cmd_colors ⇒ nrf_cli_build_in_cmd_common_executed ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_cli_help_print
  - >> nrf_cli_fprintf
  - >> nrf_cli_build_in_cmd_common_executed
  [Address Reference Count : 1]
  - nrf_cli.o(.constdata)

  nrf_cli_cmd_colors_off (Thumb, 42 bytes, Stack size 8 bytes, nrf_cli.o(i.nrf_cli_cmd_colors_off))
  [Stack]

  - Max Depth = 600
  - Call Chain = nrf_cli_cmd_colors_off ⇒ nrf_cli_build_in_cmd_common_executed ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_build_in_cmd_common_executed
  [Address Reference Count : 1]
  - nrf_cli.o(.constdata)

  nrf_cli_cmd_colors_on (Thumb, 42 bytes, Stack size 8 bytes, nrf_cli.o(i.nrf_cli_cmd_colors_on))
  [Stack]

  - Max Depth = 600
  - Call Chain = nrf_cli_cmd_colors_on ⇒ nrf_cli_build_in_cmd_common_executed ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_build_in_cmd_common_executed
  [Address Reference Count : 1]
  - nrf_cli.o(.constdata)

  nrf_cli_cmd_echo (Thumb, 86 bytes, Stack size 24 bytes, nrf_cli.o(i.nrf_cli_cmd_echo))
  [Stack]

  - Max Depth = 616
  - Call Chain = nrf_cli_cmd_echo ⇒ nrf_cli_build_in_cmd_common_executed ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> cli_flag_echo_is_set
  - >> nrf_cli_fprintf
  - >> nrf_cli_build_in_cmd_common_executed
  [Address Reference Count : 1]
  - nrf_cli.o(.constdata)

  nrf_cli_cmd_echo_off (Thumb, 42 bytes, Stack size 8 bytes, nrf_cli.o(i.nrf_cli_cmd_echo_off))
  [Stack]

  - Max Depth = 600
  - Call Chain = nrf_cli_cmd_echo_off ⇒ nrf_cli_build_in_cmd_common_executed ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_build_in_cmd_common_executed
  [Address Reference Count : 1]
  - nrf_cli.o(.constdata)

  nrf_cli_cmd_echo_on (Thumb, 42 bytes, Stack size 8 bytes, nrf_cli.o(i.nrf_cli_cmd_echo_on))
  [Stack]

  - Max Depth = 600
  - Call Chain = nrf_cli_cmd_echo_on ⇒ nrf_cli_build_in_cmd_common_executed ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_build_in_cmd_common_executed
  [Address Reference Count : 1]
  - nrf_cli.o(.constdata)

  nrf_cli_cmd_history (Thumb, 146 bytes, Stack size 32 bytes, nrf_cli.o(i.nrf_cli_cmd_history))
  [Stack]

  - Max Depth = 624
  - Call Chain = nrf_cli_cmd_history ⇒ nrf_cli_build_in_cmd_common_executed ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_cli_fprintf
  - >> nrf_memobj_read
  - >> nrf_cli_build_in_cmd_common_executed
  [Address Reference Count : 1]
  - nrf_cli.o(.constdata)

  nrf_cli_cmd_resize (Thumb, 138 bytes, Stack size 24 bytes, nrf_cli.o(i.nrf_cli_cmd_resize))
  [Stack]

  - Max Depth = 616
  - Call Chain = nrf_cli_cmd_resize ⇒ nrf_cli_build_in_cmd_common_executed ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_cli_fprintf
  - >> terminal_size_get
  - >> nrf_cli_build_in_cmd_common_executed
  [Address Reference Count : 1]
  - nrf_cli.o(.constdata)

  nrf_cli_cmd_resize_default (Thumb, 76 bytes, Stack size 16 bytes, nrf_cli.o(i.nrf_cli_cmd_resize_default))
  [Stack]

  - Max Depth = 608
  - Call Chain = nrf_cli_cmd_resize_default ⇒ nrf_cli_build_in_cmd_common_executed ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_fprintf
  - >> nrf_cli_build_in_cmd_common_executed
  [Address Reference Count : 1]
  - nrf_cli.o(.constdata)

  nrf_cli_instance_init (Thumb, 262 bytes, Stack size 32 bytes, nrf_cli.o(i.nrf_cli_instance_init))
  [Stack]

  - Max Depth = 304
  - Call Chain = nrf_cli_instance_init ⇒ nrf_memobj_pool_init ⇒ nrf_balloc_init ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_memobj_pool_init
  - >> __aeabi_memclr4
  - >> qsort
  [Called By]
  - >> nrf_cli_init

  nrf_log_backend_cli_flush (Thumb, 30 bytes, Stack size 16 bytes, nrf_cli.o(i.nrf_log_backend_cli_flush))
  [Stack]

  - Max Depth = 608
  - Call Chain = nrf_log_backend_cli_flush ⇒ cli_log_entry_process ⇒ nrf_log_std_entry_process ⇒ prefix_process ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_queue_generic_pop
  - >> cli_log_entry_process
  [Address Reference Count : 1]
  - nrf_cli.o(.constdata)

  nrf_log_backend_cli_panic_set (Thumb, 30 bytes, Stack size 8 bytes, nrf_cli.o(i.nrf_log_backend_cli_panic_set))
  [Stack]

  - Max Depth = 8
  - Call Chain = nrf_log_backend_cli_panic_set
  [Address Reference Count : 1]
  - nrf_cli.o(.constdata)

  nrf_log_backend_cli_put (Thumb, 82 bytes, Stack size 32 bytes, nrf_cli.o(i.nrf_log_backend_cli_put))
  [Stack]

  - Max Depth = 624
  - Call Chain = nrf_log_backend_cli_put ⇒ cli_log_entry_process ⇒ nrf_log_std_entry_process ⇒ prefix_process ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_queue_push
  - >> cli_log_entry_process
  - >> nrf_memobj_get
  [Address Reference Count : 1]
  - nrf_cli.o(.constdata)

  option_print (Thumb, 128 bytes, Stack size 32 bytes, nrf_cli.o(i.option_print))
  [Stack]

  - Max Depth = 536
  - Call Chain = option_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> cli_strlen
  - >> nrf_cli_fprintf
  - >> cursor_right_move
  [Called By]
  - >> cli_tab_handle

  string_cmp (Thumb, 42 bytes, Stack size 16 bytes, nrf_cli.o(i.string_cmp))
  [Stack]

  - Max Depth = 280
  - Call Chain = string_cmp ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> strcmp
  [Address Reference Count : 1]
  - nrf_cli.o(i.nrf_cli_instance_init)

  terminal_size_get (Thumb, 122 bytes, Stack size 24 bytes, nrf_cli.o(i.terminal_size_get))
  [Stack]

  - Max Depth = 512
  - Call Chain = terminal_size_get ⇒ cursor_position_get ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> cursor_down_move
  - >> cursor_up_move
  - >> cursor_right_move
  - >> cursor_position_get
  - >> cursor_left_move
  [Called By]
  - >> nrf_cli_cmd_resize

  vt100_bgcolor_set (Thumb, 48 bytes, Stack size 16 bytes, nrf_cli.o(i.vt100_bgcolor_set))
  [Stack]

  - Max Depth = 464
  - Call Chain = vt100_bgcolor_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_fprintf
  [Called By]
  - >> nrf_cli_start
  - >> nrf_cli_fprintf

  vt100_color_set (Thumb, 64 bytes, Stack size 16 bytes, nrf_cli.o(i.vt100_color_set))
  [Stack]

  - Max Depth = 464
  - Call Chain = vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_fprintf
  [Called By]
  - >> nrf_cli_start
  - >> nrf_cli_fprintf

  cli_uart_enable (Thumb, 104 bytes, Stack size 16 bytes, nrf_cli_uart.o(i.cli_uart_enable))
  [Stack]

  - Max Depth = 440
  - Call Chain = cli_uart_enable ⇒ nrf_drv_uart_init ⇒ nrfx_uarte_init ⇒ apply_config ⇒ nrf_gpio_cfg_output ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_drv_uart_init
  - >> app_timer_stop
  - >> app_timer_create
  - >> rx_try
  - >> nrf_drv_uart_uninit
  [Address Reference Count : 1]
  - nrf_cli_uart.o(.constdata)

  cli_uart_init (Thumb, 70 bytes, Stack size 16 bytes, nrf_cli_uart.o(i.cli_uart_init))
  [Stack]

  - Max Depth = 440
  - Call Chain = cli_uart_init ⇒ nrf_drv_uart_init ⇒ nrfx_uarte_init ⇒ apply_config ⇒ nrf_gpio_cfg_output ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_drv_uart_init
  - >> nrf_ringbuf_init
  - >> __aeabi_memcpy4
  [Address Reference Count : 1]
  - nrf_cli_uart.o(.constdata)

  cli_uart_read (Thumb, 38 bytes, Stack size 24 bytes, nrf_cli_uart.o(i.cli_uart_read))
  [Stack]

  - Max Depth = 312
  - Call Chain = cli_uart_read ⇒ nrf_ringbuf_cpy_get ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_ringbuf_cpy_get
  [Address Reference Count : 1]
  - nrf_cli_uart.o(.constdata)

  cli_uart_uninit (Thumb, 22 bytes, Stack size 8 bytes, nrf_cli_uart.o(i.cli_uart_uninit))
  [Stack]

  - Max Depth = 368
  - Call Chain = cli_uart_uninit ⇒ nrf_drv_uart_uninit ⇒ nrfx_uarte_uninit ⇒ nrf_gpio_cfg_default ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_timer_stop
  - >> nrf_drv_uart_uninit
  [Address Reference Count : 1]
  - nrf_cli_uart.o(.constdata)

  cli_uart_write (Thumb, 122 bytes, Stack size 32 bytes, nrf_cli_uart.o(i.cli_uart_write))
  [Stack]

  - Max Depth = 336
  - Call Chain = cli_uart_write ⇒ nrf_drv_uart_tx ⇒ nrfx_uarte_tx ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrfx_uarte_tx_in_progress
  - >> nrfx_uart_tx_in_progress
  - >> nrf_ringbuf_get
  - >> nrf_ringbuf_free
  - >> nrf_ringbuf_cpy_put
  - >> nrf_drv_uart_tx
  [Address Reference Count : 1]
  - nrf_cli_uart.o(.constdata)

  nrf_drv_uart_tx (Thumb, 26 bytes, Stack size 8 bytes, nrf_cli_uart.o(i.nrf_drv_uart_tx))
  [Stack]

  - Max Depth = 304
  - Call Chain = nrf_drv_uart_tx ⇒ nrfx_uarte_tx ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_uarte_tx
  - >> nrfx_uart_tx
  [Called By]
  - >> uart_event_handler
  - >> cli_uart_write

  nrf_drv_uart_uninit (Thumb, 20 bytes, Stack size 0 bytes, nrf_cli_uart.o(i.nrf_drv_uart_uninit))
  [Stack]

  - Max Depth = 360
  - Call Chain = nrf_drv_uart_uninit ⇒ nrfx_uarte_uninit ⇒ nrf_gpio_cfg_default ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_uarte_uninit
  - >> nrfx_uart_uninit
  [Called By]
  - >> cli_uart_uninit
  - >> cli_uart_enable

  rx_try (Thumb, 90 bytes, Stack size 24 bytes, nrf_cli_uart.o(i.rx_try))
  [Stack]

  - Max Depth = 328
  - Call Chain = rx_try ⇒ nrfx_uarte_rx ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> app_timer_start
  - >> nrfx_uarte_rx
  - >> nrfx_uart_rx
  - >> nrf_ringbuf_alloc
  [Called By]
  - >> uart_event_handler
  - >> cli_uart_enable

  timer_handler (Thumb, 22 bytes, Stack size 0 bytes, nrf_cli_uart.o(i.timer_handler))
  [Calls]

  - >> nrfx_uarte_rx_abort
  - >> nrfx_uart_rx_abort
  [Address Reference Count : 1]
  - nrf_cli_uart.o(i.cli_uart_enable)

  uart_event_handler (Thumb, 202 bytes, Stack size 24 bytes, nrf_cli_uart.o(i.uart_event_handler))
  [Stack]

  - Max Depth = 352
  - Call Chain = uart_event_handler ⇒ rx_try ⇒ nrfx_uarte_rx ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_ringbuf_put
  - >> nrf_ringbuf_get
  - >> nrf_ringbuf_free
  - >> rx_try
  - >> nrf_drv_uart_tx
  [Address Reference Count : 1]
  - nrf_cli_uart.o(i.cli_uart_init)

  buffer_add (Thumb, 46 bytes, Stack size 16 bytes, nrf_fprintf_format.o(i.buffer_add))
  [Stack]

  - Max Depth = 288 + In Cycle
  - Call Chain = buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> buffer_add
  - >> nrf_fprintf_buffer_flush
  [Called By]
  - >> unsigned_print
  - >> int_print
  - >> buffer_add
  - >> nrf_fprintf_fmt

  int_print (Thumb, 166 bytes, Stack size 48 bytes, nrf_fprintf_format.o(i.int_print))
  [Stack]

  - Max Depth = 376
  - Call Chain = int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> unsigned_print
  - >> buffer_add
  [Called By]
  - >> nrf_fprintf_fmt

  unsigned_print (Thumb, 176 bytes, Stack size 40 bytes, nrf_fprintf_format.o(i.unsigned_print))
  [Stack]

  - Max Depth = 328
  - Call Chain = unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> buffer_add
  [Called By]
  - >> int_print
  - >> nrf_fprintf_fmt

  memobj_op (Thumb, 162 bytes, Stack size 40 bytes, nrf_memobj.o(i.memobj_op))
  [Stack]

  - Max Depth = 48 + In Cycle
  - Call Chain = memobj_op ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> __aeabi_memcpy
  [Called By]
  - >> nrf_memobj_write
  - >> nrf_memobj_read

  nrf_queue_next_idx (Thumb, 30 bytes, Stack size 16 bytes, nrf_queue.o(i.nrf_queue_next_idx))
  [Stack]

  - Max Depth = 280
  - Call Chain = nrf_queue_next_idx ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  [Called By]
  - >> nrf_queue_push
  - >> nrf_queue_generic_pop
  - >> nrf_queue_is_full

  nrf_queue_status (Thumb, 176 bytes, Stack size 72 bytes, nrf_queue.o(i.nrf_queue_status))
  [Stack]

  - Max Depth = 648
  - Call Chain = nrf_queue_status ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_help_print
  - >> nrf_cli_fprintf
  - >> nrf_queue_utilization_get
  - >> nrf_queue_max_utilization_get
  [Address Reference Count : 2]
  - nrf_queue.o(.constdata)
  - nrf_queue.o(.constdata)

  queue_utilization_get (Thumb, 24 bytes, Stack size 0 bytes, nrf_queue.o(i.queue_utilization_get))
  [Called By]

  - >> nrf_queue_push
  - >> nrf_queue_utilization_get

  nrf_log_backend_uart_flush (Thumb, 2 bytes, Stack size 0 bytes, nrf_log_backend_uart.o(i.nrf_log_backend_uart_flush))
  [Address Reference Count : 1]

  - nrf_log_backend_uart.o(.constdata)

  nrf_log_backend_uart_panic_set (Thumb, 36 bytes, Stack size 8 bytes, nrf_log_backend_uart.o(i.nrf_log_backend_uart_panic_set))
  [Stack]

  - Max Depth = 472
  - Call Chain = nrf_log_backend_uart_panic_set ⇒ uart_init ⇒ nrf_drv_uart_init ⇒ nrfx_uarte_init ⇒ apply_config ⇒ nrf_gpio_cfg_output ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrfx_uarte_uninit
  - >> nrfx_uart_uninit
  - >> uart_init
  [Address Reference Count : 1]
  - nrf_log_backend_uart.o(.constdata)

  nrf_log_backend_uart_put (Thumb, 16 bytes, Stack size 8 bytes, nrf_log_backend_uart.o(i.nrf_log_backend_uart_put))
  [Stack]

  - Max Depth = 624
  - Call Chain = nrf_log_backend_uart_put ⇒ nrf_log_backend_serial_put ⇒ nrf_log_std_entry_process ⇒ prefix_process ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_log_backend_serial_put
  [Address Reference Count : 1]
  - nrf_log_backend_uart.o(.constdata)

  serial_tx (Thumb, 58 bytes, Stack size 16 bytes, nrf_log_backend_uart.o(i.serial_tx))
  [Stack]

  - Max Depth = 312
  - Call Chain = serial_tx ⇒ nrfx_uarte_tx ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_error_handler
  - >> nrfx_uarte_tx
  - >> nrfx_uart_tx
  [Address Reference Count : 1]
  - nrf_log_backend_uart.o(i.nrf_log_backend_uart_put)

  uart_evt_handler (Thumb, 8 bytes, Stack size 0 bytes, nrf_log_backend_uart.o(i.uart_evt_handler))
  [Address Reference Count : 1]

  - nrf_log_backend_uart.o(i.uart_init)

  uart_init (Thumb, 70 bytes, Stack size 40 bytes, nrf_log_backend_uart.o(i.uart_init))
  [Stack]

  - Max Depth = 464
  - Call Chain = uart_init ⇒ nrf_drv_uart_init ⇒ nrfx_uarte_init ⇒ apply_config ⇒ nrf_gpio_cfg_output ⇒ nrf_gpio_cfg ⇒ nrf_gpio_pin_port_decode ⇒ assert_nrf_callback ⇒ app_error_fault_handler ⇒ nrf_log_frontend_std_5 ⇒ std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_drv_uart_init
  - >> app_error_handler
  - >> __aeabi_memcpy4
  [Called By]
  - >> nrf_log_backend_uart_panic_set

  backend_name_get (Thumb, 58 bytes, Stack size 20 bytes, nrf_log_frontend.o(i.backend_name_get))
  [Stack]

  - Max Depth = 20
  - Call Chain = backend_name_get
  [Address Reference Count : 1]
  - nrf_log_frontend.o(.constdata)

  buf_prealloc (Thumb, 130 bytes, Stack size 32 bytes, nrf_log_frontend.o(i.buf_prealloc))
  [Stack]

  - Max Depth = 80
  - Call Chain = buf_prealloc ⇒ log_skip ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> app_util_critical_region_exit
  - >> app_util_critical_region_enter
  - >> nrf_atomic_u32_add
  - >> log_skip
  [Called By]
  - >> std_n

  dropped_sat16_get (Thumb, 16 bytes, Stack size 8 bytes, nrf_log_frontend.o(i.dropped_sat16_get))
  [Stack]

  - Max Depth = 16
  - Call Chain = dropped_sat16_get ⇒ nrf_atomic_u32_fetch_store
  [Calls]
  - >> nrf_atomic_u32_fetch_store
  [Called By]
  - >> std_n

  invalid_packets_omit (Thumb, 52 bytes, Stack size 0 bytes, nrf_log_frontend.o(i.invalid_packets_omit))
  [Called By]

  - >> nrf_log_frontend_dequeue
  - >> log_skip

  log_backend_ctrl (Thumb, 6 bytes, Stack size 0 bytes, nrf_log_frontend.o(i.log_backend_ctrl))
  [Stack]

  - Max Depth = 560
  - Call Chain = log_backend_ctrl ⇒ nrf_cli_backend_cmd_execute ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_backend_cmd_execute
  [Address Reference Count : 1]
  - nrf_log_frontend.o(.constdata)

  log_backend_go (Thumb, 6 bytes, Stack size 0 bytes, nrf_log_frontend.o(i.log_backend_go))
  [Stack]

  - Max Depth = 560
  - Call Chain = log_backend_go ⇒ nrf_cli_backend_cmd_execute ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_backend_cmd_execute
  [Address Reference Count : 1]
  - nrf_log_frontend.o(.constdata)

  log_backend_halt (Thumb, 6 bytes, Stack size 0 bytes, nrf_log_frontend.o(i.log_backend_halt))
  [Stack]

  - Max Depth = 560
  - Call Chain = log_backend_halt ⇒ nrf_cli_backend_cmd_execute ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_backend_cmd_execute
  [Address Reference Count : 1]
  - nrf_log_frontend.o(.constdata)

  log_backend_status (Thumb, 6 bytes, Stack size 0 bytes, nrf_log_frontend.o(i.log_backend_status))
  [Stack]

  - Max Depth = 560
  - Call Chain = log_backend_status ⇒ nrf_cli_backend_cmd_execute ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_backend_cmd_execute
  [Address Reference Count : 1]
  - nrf_log_frontend.o(.constdata)

  log_cmd (Thumb, 54 bytes, Stack size 24 bytes, nrf_log_frontend.o(i.log_cmd))
  [Stack]

  - Max Depth = 600
  - Call Chain = log_cmd ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_help_print
  - >> nrf_cli_fprintf
  - >> nrf_cli_help_requested
  [Address Reference Count : 1]
  - nrf_log_frontend.o(.constdata)

  log_cmd_backends_list (Thumb, 102 bytes, Stack size 32 bytes, nrf_log_frontend.o(i.log_cmd_backends_list))
  [Stack]

  - Max Depth = 608
  - Call Chain = log_cmd_backends_list ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_help_print
  - >> nrf_cli_fprintf
  - >> nrf_cli_help_requested
  [Address Reference Count : 1]
  - nrf_log_frontend.o(.constdata)

  log_config_load_cmd (Thumb, 38 bytes, Stack size 8 bytes, nrf_log_frontend.o(i.log_config_load_cmd))
  [Stack]

  - Max Depth = 584
  - Call Chain = log_config_load_cmd ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_help_print
  - >> nrf_cli_fprintf
  - >> nrf_cli_help_requested
  [Address Reference Count : 1]
  - nrf_log_frontend.o(.constdata)

  log_config_store_cmd (Thumb, 38 bytes, Stack size 8 bytes, nrf_log_frontend.o(i.log_config_store_cmd))
  [Stack]

  - Max Depth = 584
  - Call Chain = log_config_store_cmd ⇒ nrf_cli_help_print ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_help_print
  - >> nrf_cli_fprintf
  - >> nrf_cli_help_requested
  [Address Reference Count : 1]
  - nrf_log_frontend.o(.constdata)

  log_ctrl (Thumb, 304 bytes, Stack size 56 bytes, nrf_log_frontend.o(i.log_ctrl))
  [Stack]

  - Max Depth = 560
  - Call Chain = log_ctrl ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_fprintf
  - >> nrf_log_module_name_get
  - >> nrf_log_module_cnt_get
  - >> module_id_filter_set
  - >> strncmp
  [Called By]
  - >> log_self_ctrl
  [Address Reference Count : 1]
  - nrf_log_frontend.o(i.log_backend_ctrl)

  log_go (Thumb, 8 bytes, Stack size 0 bytes, nrf_log_frontend.o(i.log_go))
  [Address Reference Count : 1]

  - nrf_log_frontend.o(i.log_backend_go)

  log_halt (Thumb, 8 bytes, Stack size 0 bytes, nrf_log_frontend.o(i.log_halt))
  [Address Reference Count : 1]

  - nrf_log_frontend.o(i.log_backend_halt)

  log_self_ctrl (Thumb, 16 bytes, Stack size 8 bytes, nrf_log_frontend.o(i.log_self_ctrl))
  [Stack]

  - Max Depth = 568
  - Call Chain = log_self_ctrl ⇒ log_ctrl ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> log_ctrl
  [Address Reference Count : 1]
  - nrf_log_frontend.o(.constdata)

  log_self_go (Thumb, 10 bytes, Stack size 0 bytes, nrf_log_frontend.o(i.log_self_go))
  [Address Reference Count : 1]

  - nrf_log_frontend.o(.constdata)

  log_self_halt (Thumb, 10 bytes, Stack size 0 bytes, nrf_log_frontend.o(i.log_self_halt))
  [Address Reference Count : 1]

  - nrf_log_frontend.o(.constdata)

  log_self_status (Thumb, 16 bytes, Stack size 8 bytes, nrf_log_frontend.o(i.log_self_status))
  [Stack]

  - Max Depth = 560
  - Call Chain = log_self_status ⇒ log_status ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> log_status
  [Address Reference Count : 1]
  - nrf_log_frontend.o(.constdata)

  log_skip (Thumb, 160 bytes, Stack size 40 bytes, nrf_log_frontend.o(i.log_skip))
  [Stack]

  - Max Depth = 48 + In Cycle
  - Call Chain = log_skip ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> assert_nrf_callback
  - >> nrf_atomic_flag_set
  - >> nrf_atomic_flag_clear_fetch
  - >> invalid_packets_omit
  [Called By]
  - >> buf_prealloc

  log_status (Thumb, 158 bytes, Stack size 48 bytes, nrf_log_frontend.o(i.log_status))
  [Stack]

  - Max Depth = 552
  - Call Chain = log_status ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_fprintf
  - >> nrf_log_module_name_get
  - >> nrf_log_module_filter_get
  - >> nrf_log_module_cnt_get
  [Called By]
  - >> log_self_status
  [Address Reference Count : 1]
  - nrf_log_frontend.o(i.log_backend_status)

  module_id_filter_set (Thumb, 38 bytes, Stack size 16 bytes, nrf_log_frontend.o(i.module_id_filter_set))
  [Stack]

  - Max Depth = 60
  - Call Chain = module_id_filter_set ⇒ nrf_log_module_filter_get ⇒ module_idx_get
  [Calls]
  - >> nrf_log_module_filter_set
  - >> nrf_log_module_filter_get
  [Called By]
  - >> log_ctrl

  module_idx_get (Thumb, 42 bytes, Stack size 12 bytes, nrf_log_frontend.o(i.module_idx_get))
  [Stack]

  - Max Depth = 12
  - Call Chain = module_idx_get
  [Calls]
  - >> nrf_log_module_cnt_get
  [Called By]
  - >> nrf_log_module_name_get
  - >> nrf_log_module_filter_get

  module_name_get (Thumb, 24 bytes, Stack size 8 bytes, nrf_log_frontend.o(i.module_name_get))
  [Stack]

  - Max Depth = 36
  - Call Chain = module_name_get ⇒ nrf_log_module_name_get ⇒ module_idx_get
  [Calls]
  - >> nrf_log_module_name_get
  [Address Reference Count : 1]
  - nrf_log_frontend.o(.constdata)

  nrf_cli_backend_cmd_execute (Thumb, 92 bytes, Stack size 56 bytes, nrf_log_frontend.o(i.nrf_cli_backend_cmd_execute))
  [Stack]

  - Max Depth = 560
  - Call Chain = nrf_cli_backend_cmd_execute ⇒ nrf_cli_fprintf ⇒ vt100_color_set ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_cli_fprintf
  - >> strcmp
  [Called By]
  - >> log_backend_status
  - >> log_backend_halt
  - >> log_backend_go
  - >> log_backend_ctrl

  nrf_cli_help_requested (Thumb, 12 bytes, Stack size 0 bytes, nrf_log_frontend.o(i.nrf_cli_help_requested))
  [Called By]

  - >> log_config_store_cmd
  - >> log_config_load_cmd
  - >> log_cmd_backends_list
  - >> log_cmd

  severity_lvl_get (Thumb, 28 bytes, Stack size 0 bytes, nrf_log_frontend.o(i.severity_lvl_get))
  [Address Reference Count : 1]

  - nrf_log_frontend.o(.constdata)

  std_n (Thumb, 160 bytes, Stack size 40 bytes, nrf_log_frontend.o(i.std_n))
  [Stack]

  - Max Depth = 168 + In Cycle
  - Call Chain = std_n ⇒ assert_nrf_callback (Cycle)
  [Calls]
  - >> nrf_log_frontend_dequeue
  - >> assert_nrf_callback
  - >> nrf_log_module_cnt_get
  - >> dropped_sat16_get
  - >> buf_prealloc
  [Called By]
  - >> nrf_log_frontend_std_0
  - >> nrf_log_frontend_std_5
  - >> nrf_log_frontend_std_2
  - >> nrf_log_frontend_std_1
  - >> nrf_log_frontend_std_4
  - >> nrf_log_frontend_std_3

  postfix_process (Thumb, 48 bytes, Stack size 8 bytes, nrf_log_str_formatter.o(i.postfix_process))
  [Stack]

  - Max Depth = 456
  - Call Chain = postfix_process ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_fprintf_buffer_flush
  - >> nrf_fprintf
  [Called By]
  - >> nrf_log_std_entry_process
  - >> nrf_log_hexdump_entry_process

  prefix_process (Thumb, 90 bytes, Stack size 16 bytes, nrf_log_str_formatter.o(i.prefix_process))
  [Stack]

  - Max Depth = 464
  - Call Chain = prefix_process ⇒ nrf_fprintf ⇒ nrf_fprintf_fmt ⇒ int_print ⇒ unsigned_print ⇒ buffer_add ⇒ buffer_add (Cycle)
  [Calls]
  - >> nrf_log_module_name_get
  - >> nrf_log_color_id_get
  - >> nrf_fprintf
  [Called By]
  - >> nrf_log_std_entry_process
  - >> nrf_log_hexdump_entry_process

  _scanf_char_input (Thumb, 12 bytes, Stack size 0 bytes, scanf_char.o(.text))
  [Address Reference Count : 1]

  - scanf_char.o(.text)

  ### Undefined Global Symbols