 *  Executing task: nRF Connect: Build [pristine]: DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build (active) 

Building DL02_S2MB_KPD_Small
cmd.exe /d /s /c "west build --build-dir c:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build c:/nordic/DL02_S2MB_KPD_Small --pristine --board dl02_s2mb_kpd_small_cpuapp -- -DNCS_TOOLCHAIN_VERSION=NONE -DBOARD_ROOT=c:/nordic/dl02_s2mb_kpd_small"

-- west build: generating a build system
Loading Zephyr default modules (Zephyr base).
-- Application: C:/nordic/DL02_S2MB_KPD_Small
-- CMake version: 3.21.0
-- Found Python3: C:/ncs/toolchains/cf2149caf2/opt/bin/python.exe (found suitable version "3.9.13", minimum required is "3.8") found components: Interpreter 
-- Cache files will be written to: C:/ncs/v2.6.1/zephyr/.cache
-- Zephyr version: 3.5.99 (C:/ncs/v2.6.1/zephyr)
-- Found west (found suitable version "1.2.0", minimum required is "0.14.0")
-- Board: dl02_s2mb_kpd_small_cpuapp
-- Found host-tools: zephyr 0.16.5 (C:/ncs/toolchains/cf2149caf2/opt/zephyr-sdk)
-- Found toolchain: zephyr 0.16.5 (C:/ncs/toolchains/cf2149caf2/opt/zephyr-sdk)
-- Found Dtc: C:/ncs/toolchains/cf2149caf2/opt/bin/dtc.exe (found suitable version "1.4.7", minimum required is "1.4.6") 
-- Found BOARD.dts: C:/nordic/DL02_S2MB_KPD_Small/boards/arm/dl02_s2mb_kpd_small/dl02_s2mb_kpd_small_cpuapp.dts
-- Found devicetree overlay: C:/nordic/DL02_S2MB_KPD_Small/boards/dl02_s2mb_kpd_small_cpuapp.overlay
'label' is marked as deprecated in 'properties:' in C:/ncs/v2.6.1/zephyr/dts/bindings\mtd\jedec,spi-nor.yaml for node /soc/peripheral@50000000/spi@c000/mx25r6435f@0.
node '/soc/peripheral@50000000/i2c@9000/outside@5B' compatible 'sunion,outside' has unknown vendor prefix 'sunion'
node '/soc/peripheral@50000000/i2c@9000/store@50' compatible 'sunion,eeprom' has unknown vendor prefix 'sunion'
node '/soc/peripheral@50000000/i2c@9000/timer@32' compatible 'sunion,rtc' has unknown vendor prefix 'sunion'
-- Generated zephyr.dts: C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/zephyr/zephyr.dts
-- Generated devicetree_generated.h: C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/zephyr/include/generated/devicetree_generated.h
-- Including generated dts.cmake file: C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/zephyr/dts.cmake

warning: MBEDTLS (defined at soc/arm/nxp_imx\rt5xx\Kconfig.defconfig.series:63,
soc/arm/nxp_imx\rt6xx\Kconfig.defconfig.series:64, soc/arm/nxp_imx\rt\Kconfig.defconfig.series:117,
C:/ncs/v2.6.1/nrf\modules/trusted-firmware-m/Kconfig.mbedtls_minimal.defconfig:7,
C:/ncs/v2.6.1/nrf\modules/trusted-firmware-m/Kconfig.psa.defconfig:1,
C:/ncs/v2.6.1/zephyr/modules/mbedtls/Kconfig:17, modules\mbedtls\Kconfig:17) was assigned the value
'y' but got the value 'n'. See http://docs.zephyrproject.org/latest/kconfig.html#CONFIG_MBEDTLS
and/or look up MBEDTLS in the menuconfig/guiconfig interface. The Application Development Primer,
Setting Configuration Values, and Kconfig - Tips and Best Practices sections of the manual might be
helpful too.


warning: PM (defined at soc/arm/silabs_exx32\efr32bg22\Kconfig.defconfig.series:18,
soc/arm/silabs_exx32\efr32bg27\Kconfig.defconfig.series:18,
soc/arm/silabs_exx32\efr32mg24\Kconfig.defconfig.series:19,
soc/arm/st_stm32\stm32f4\Kconfig.defconfig.series:20, subsys/pm/Kconfig:13) was assigned the value
'y' but got the value 'n'. Check these unsatisfied dependencies: ((SOC_SERIES_EFR32BG22 &&
SOC_FAMILY_EXX32) || (SOC_SERIES_EFR32BG27 && SOC_FAMILY_EXX32) || (SOC_SERIES_EFR32MG24 &&
SOC_FAMILY_EXX32) || SOC_SERIES_STM32F4X || (SYS_CLOCK_EXISTS && HAS_PM)) (=n). See
http://docs.zephyrproject.org/latest/kconfig.html#CONFIG_PM and/or look up PM in the
menuconfig/guiconfig interface. The Application Development Primer, Setting Configuration Values,
and Kconfig - Tips and Best Practices sections of the manual might be helpful too.


warning: BT_CTLR_SDC_PERIPHERAL_COUNT (defined at
C:/ncs/v2.6.1/nrf\subsys\bluetooth\controller/Kconfig:123) was assigned the value '3' but got the
value ''. Check these unsatisfied dependencies: BT_LL_SOFTDEVICE (=n), BT_CTLR (=n). See
http://docs.zephyrproject.org/latest/kconfig.html#CONFIG_BT_CTLR_SDC_PERIPHERAL_COUNT and/or look up
BT_CTLR_SDC_PERIPHERAL_COUNT in the menuconfig/guiconfig interface. The Application Development
Primer, Setting Configuration Values, and Kconfig - Tips and Best Practices sections of the manual
might be helpful too.


warning: Experimental symbol GPIO_ENABLE_DISABLE_INTERRUPT is enabled.

Parsing C:/nordic/DL02_S2MB_KPD_Small/Kconfig
Loaded configuration 'C:/nordic/DL02_S2MB_KPD_Small/boards/arm/dl02_s2mb_kpd_small/dl02_s2mb_kpd_small_cpuapp_defconfig'
Merged configuration 'C:/nordic/DL02_S2MB_KPD_Small/prj.conf'
Configuration saved to 'C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/zephyr/.config'
Kconfig header saved to 'C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/zephyr/include/generated/autoconf.h'
-- Found GnuLd: c:/ncs/toolchains/cf2149caf2/opt/zephyr-sdk/arm-zephyr-eabi/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/bin/ld.bfd.exe (found version "2.38") 
-- The C compiler identification is GNU 12.2.0
-- The CXX compiler identification is GNU 12.2.0
-- The ASM compiler identification is GNU
-- Found assembler: C:/ncs/toolchains/cf2149caf2/opt/zephyr-sdk/arm-zephyr-eabi/bin/arm-zephyr-eabi-gcc.exe

=== child image multiprotocol_rpmsg - CPUNET begin ===
loading initial cache file C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/multiprotocol_rpmsg/child_image_preload.cmake
Loading Zephyr default modules (Zephyr base).
-- Application: C:/ncs/v2.6.1/nrf/samples/nrf5340/multiprotocol_rpmsg
-- CMake version: 3.21.0
-- Found Python3: C:/ncs/toolchains/cf2149caf2/opt/bin/python.exe (found suitable version "3.9.13", minimum required is "3.8") found components: Interpreter 
-- Cache files will be written to: C:/ncs/v2.6.1/zephyr/.cache
-- Zephyr version: 3.5.99 (C:/ncs/v2.6.1/zephyr)
-- Found west (found suitable version "1.2.0", minimum required is "0.14.0")
-- Board: dl02_s2mb_kpd_small_cpunet
-- Found host-tools: zephyr 0.16.5 (C:/ncs/toolchains/cf2149caf2/opt/zephyr-sdk)
-- Found toolchain: zephyr 0.16.5 (C:/ncs/toolchains/cf2149caf2/opt/zephyr-sdk)
-- Found Dtc: C:/ncs/toolchains/cf2149caf2/opt/bin/dtc.exe (found suitable version "1.4.7", minimum required is "1.4.6") 
-- Found BOARD.dts: C:/nordic/DL02_S2MB_KPD_Small/boards/arm/dl02_s2mb_kpd_small/dl02_s2mb_kpd_small_cpunet.dts
-- Generated zephyr.dts: C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/multiprotocol_rpmsg/zephyr/zephyr.dts
-- Generated devicetree_generated.h: C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/multiprotocol_rpmsg/zephyr/include/generated/devicetree_generated.h
-- Including generated dts.cmake file: C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/multiprotocol_rpmsg/zephyr/dts.cmake
Parsing C:/ncs/v2.6.1/modules/lib/matter/config/nrfconnect/chip-module/Kconfig.multiprotocol_rpmsg.root
Loaded configuration 'C:/nordic/DL02_S2MB_KPD_Small/boards/arm/dl02_s2mb_kpd_small/dl02_s2mb_kpd_small_cpunet_defconfig'
Merged configuration 'C:/nordic/DL02_S2MB_KPD_Small/child_image/multiprotocol_rpmsg/prj.conf'
Merged configuration 'C:/ncs/v2.6.1/nrf/subsys/bootloader/image/secure_boot.conf'
Merged configuration 'C:/ncs/v2.6.1/nrf/subsys/partition_manager/partition_manager_enabled.conf'
Merged configuration 'C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/multiprotocol_rpmsg/zephyr/misc/generated/extra_kconfig_options.conf'
Configuration saved to 'C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/multiprotocol_rpmsg/zephyr/.config'
Kconfig header saved to 'C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/multiprotocol_rpmsg/zephyr/include/generated/autoconf.h'
-- Found GnuLd: c:/ncs/toolchains/cf2149caf2/opt/zephyr-sdk/arm-zephyr-eabi/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/bin/ld.bfd.exe (found version "2.38") 
-- The C compiler identification is GNU 12.2.0
-- The CXX compiler identification is GNU 12.2.0
-- The ASM compiler identification is GNU
-- Found assembler: C:/ncs/toolchains/cf2149caf2/opt/zephyr-sdk/arm-zephyr-eabi/bin/arm-zephyr-eabi-gcc.exe

=== child image b0n - CPUNET (inherited) begin ===
loading initial cache file C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/multiprotocol_rpmsg/b0n/child_image_preload.cmake
Loading Zephyr default modules (Zephyr base).
-- Application: C:/ncs/v2.6.1/nrf/samples/nrf5340/netboot
-- CMake version: 3.21.0
-- Found Python3: C:/ncs/toolchains/cf2149caf2/opt/bin/python.exe (found suitable version "3.9.13", minimum required is "3.8") found components: Interpreter 
-- Cache files will be written to: C:/ncs/v2.6.1/zephyr/.cache
-- Zephyr version: 3.5.99 (C:/ncs/v2.6.1/zephyr)
-- Found west (found suitable version "1.2.0", minimum required is "0.14.0")
-- Board: dl02_s2mb_kpd_small_cpunet
-- Found host-tools: zephyr 0.16.5 (C:/ncs/toolchains/cf2149caf2/opt/zephyr-sdk)
-- Found toolchain: zephyr 0.16.5 (C:/ncs/toolchains/cf2149caf2/opt/zephyr-sdk)
-- Found Dtc: C:/ncs/toolchains/cf2149caf2/opt/bin/dtc.exe (found suitable version "1.4.7", minimum required is "1.4.6") 
-- Found BOARD.dts: C:/nordic/DL02_S2MB_KPD_Small/boards/arm/dl02_s2mb_kpd_small/dl02_s2mb_kpd_small_cpunet.dts
-- Generated zephyr.dts: C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/multiprotocol_rpmsg/b0n/zephyr/zephyr.dts
-- Generated devicetree_generated.h: C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/multiprotocol_rpmsg/b0n/zephyr/include/generated/devicetree_generated.h
-- Including generated dts.cmake file: C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/multiprotocol_rpmsg/b0n/zephyr/dts.cmake
Parsing C:/ncs/v2.6.1/nrf/samples/nrf5340/netboot/Kconfig
Loaded configuration 'C:/nordic/DL02_S2MB_KPD_Small/boards/arm/dl02_s2mb_kpd_small/dl02_s2mb_kpd_small_cpunet_defconfig'
Merged configuration 'C:/ncs/v2.6.1/nrf/samples/nrf5340/netboot/prj.conf'
Merged configuration 'C:/ncs/v2.6.1/nrf/subsys/partition_manager/partition_manager_enabled.conf'
Configuration saved to 'C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/multiprotocol_rpmsg/b0n/zephyr/.config'
Kconfig header saved to 'C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/multiprotocol_rpmsg/b0n/zephyr/include/generated/autoconf.h'
-- Found GnuLd: c:/ncs/toolchains/cf2149caf2/opt/zephyr-sdk/arm-zephyr-eabi/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/bin/ld.bfd.exe (found version "2.38") 
-- The C compiler identification is GNU 12.2.0
-- The CXX compiler identification is GNU 12.2.0
-- The ASM compiler identification is GNU
-- Found assembler: C:/ncs/toolchains/cf2149caf2/opt/zephyr-sdk/arm-zephyr-eabi/bin/arm-zephyr-eabi-gcc.exe
CMake Warning at C:/ncs/v2.6.1/zephyr/CMakeLists.txt:1957 (message):
  __ASSERT() statements are globally ENABLED


-- Configuring done
-- Generating done
-- Build files have been written to: C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/multiprotocol_rpmsg/b0n
=== child image b0n - CPUNET (inherited) end ===

CMake Warning at C:/ncs/v2.6.1/nrf/subsys/bootloader/cmake/debug_keys.cmake:36 (message):
  

      --------------------------------------------------------------
      --- WARNING: Using generated NSIB public/private key-pair. ---
      --- It should not be used for production.                  ---
      --- See CONFIG_SB_SIGNING_KEY_FILE                         ---
      --------------------------------------------------------------
      

Call Stack (most recent call first):
  C:/ncs/v2.6.1/nrf/subsys/bootloader/cmake/provision_hex.cmake:47 (include)
  C:/ncs/v2.6.1/nrf/subsys/CMakeLists.txt:20 (include)


-- libmetal version: 1.4.0 (C:/ncs/v2.6.1/nrf/samples/nrf5340/multiprotocol_rpmsg)
-- Build type:  
-- Host:    Windows/AMD64
-- Target:  Generic/arm
-- Machine: arm
-- Looking for include file stdatomic.h
-- Looking for include file stdatomic.h - found
-- open-amp version: 1.4.0 (C:/ncs/v2.6.1/modules/lib/open-amp/open-amp)
-- Host:    Windows/AMD64
-- Target:  Generic/arm
-- Machine: arm
-- C_FLAGS :  -Wall -Wextra
-- Looking for include file fcntl.h
-- Looking for include file fcntl.h - found
CMake Warning at C:/ncs/v2.6.1/zephyr/CMakeLists.txt:862 (message):
  No SOURCES given to Zephyr library: drivers__console

  Excluding target from build.


CMake Warning at C:/ncs/v2.6.1/zephyr/CMakeLists.txt:1957 (message):
  __ASSERT() statements are globally ENABLED


CMake Warning at C:/ncs/v2.6.1/nrf/cmake/partition_manager.cmake:79 (message):
  

          ---------------------------------------------------------------------
          --- WARNING: Using a bootloader without pm_static.yml.            ---
          --- There are cases where a deployed product can consist of       ---
          --- multiple images, and only a subset of these images can be     ---
          --- upgraded through a firmware update mechanism. In such cases,  ---
          --- the upgradable images must have partitions that are static    ---
          --- and are matching the partition map used by the bootloader     ---
          --- programmed onto the device.                                   ---
          ---------------------------------------------------------------------
          

Call Stack (most recent call first):
  C:/ncs/v2.6.1/zephyr/cmake/modules/kernel.cmake:248 (include)
  C:/ncs/v2.6.1/zephyr/cmake/modules/zephyr_default.cmake:138 (include)
  C:/ncs/v2.6.1/zephyr/share/zephyr-package/cmake/ZephyrConfig.cmake:66 (include)
  C:/ncs/v2.6.1/zephyr/share/zephyr-package/cmake/ZephyrConfig.cmake:92 (include_boilerplate)
  CMakeLists.txt:5 (find_package)


-- Configuring done
-- Generating done
-- Build files have been written to: C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/multiprotocol_rpmsg
=== child image multiprotocol_rpmsg - CPUNET end ===

-- Found Python3: C:/ncs/toolchains/cf2149caf2/opt/bin/python.exe (found version "3.9.13") found components: Interpreter 

=== child image mcuboot -  begin ===
loading initial cache file C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/mcuboot/child_image_preload.cmake
Loading Zephyr default modules (Zephyr base).
-- Application: C:/ncs/v2.6.1/bootloader/mcuboot/boot/zephyr
-- CMake version: 3.21.0
-- Found Python3: C:/ncs/toolchains/cf2149caf2/opt/bin/python.exe (found suitable version "3.9.13", minimum required is "3.8") found components: Interpreter 
-- Cache files will be written to: C:/ncs/v2.6.1/zephyr/.cache
-- Zephyr version: 3.5.99 (C:/ncs/v2.6.1/zephyr)
-- Found west (found suitable version "1.2.0", minimum required is "0.14.0")
-- Board: dl02_s2mb_kpd_small_cpuapp
-- Found host-tools: zephyr 0.16.5 (C:/ncs/toolchains/cf2149caf2/opt/zephyr-sdk)
-- Found toolchain: zephyr 0.16.5 (C:/ncs/toolchains/cf2149caf2/opt/zephyr-sdk)
-- Found Dtc: C:/ncs/toolchains/cf2149caf2/opt/bin/dtc.exe (found suitable version "1.4.7", minimum required is "1.4.6") 
-- Found BOARD.dts: C:/nordic/DL02_S2MB_KPD_Small/boards/arm/dl02_s2mb_kpd_small/dl02_s2mb_kpd_small_cpuapp.dts
-- Found devicetree overlay: C:/ncs/v2.6.1/nrf/modules/mcuboot/flash_sim.overlay
-- Found devicetree overlay: C:/nordic/DL02_S2MB_KPD_Small/child_image/mcuboot/boards/dl02_s2mb_kpd_small_cpuapp.overlay
'label' is marked as deprecated in 'properties:' in C:/ncs/v2.6.1/zephyr/dts/bindings\mtd\jedec,spi-nor.yaml for node /soc/peripheral@50000000/spi@c000/mx25r6435f@0.
node '/soc/peripheral@50000000/i2c@9000/outside@5B' compatible 'sunion,outside' has unknown vendor prefix 'sunion'
node '/soc/peripheral@50000000/i2c@9000/store@50' compatible 'sunion,eeprom' has unknown vendor prefix 'sunion'
node '/soc/peripheral@50000000/i2c@9000/timer@32' compatible 'sunion,rtc' has unknown vendor prefix 'sunion'
-- Generated zephyr.dts: C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/mcuboot/zephyr/zephyr.dts
-- Generated devicetree_generated.h: C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/mcuboot/zephyr/include/generated/devicetree_generated.h
-- Including generated dts.cmake file: C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/mcuboot/zephyr/dts.cmake
Parsing C:/nordic/DL02_S2MB_KPD_Small/Kconfig.mcuboot.root
Loaded configuration 'C:/nordic/DL02_S2MB_KPD_Small/boards/arm/dl02_s2mb_kpd_small/dl02_s2mb_kpd_small_cpuapp_defconfig'
Merged configuration 'C:/nordic/DL02_S2MB_KPD_Small/child_image/mcuboot/prj.conf'
Merged configuration 'C:/nordic/DL02_S2MB_KPD_Small/child_image/mcuboot/boards/dl02_s2mb_kpd_small_cpuapp.conf'
Merged configuration 'C:/ncs/v2.6.1/nrf/subsys/pcd/pcd.conf'
Merged configuration 'C:/ncs/v2.6.1/nrf/subsys/bootloader/bl_override/override_external_mcuboot.conf'
Merged configuration 'C:/ncs/v2.6.1/nrf/subsys/partition_manager/ext_flash_mcuboot_secondary.conf'
Merged configuration 'C:/ncs/v2.6.1/nrf/subsys/partition_manager/partition_manager_enabled.conf'
Merged configuration 'C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/mcuboot/zephyr/misc/generated/extra_kconfig_options.conf'
Configuration saved to 'C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/mcuboot/zephyr/.config'
Kconfig header saved to 'C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/mcuboot/zephyr/include/generated/autoconf.h'
-- Found GnuLd: c:/ncs/toolchains/cf2149caf2/opt/zephyr-sdk/arm-zephyr-eabi/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/bin/ld.bfd.exe (found version "2.38") 
-- The C compiler identification is GNU 12.2.0
-- The CXX compiler identification is GNU 12.2.0
-- The ASM compiler identification is GNU
-- Found assembler: C:/ncs/toolchains/cf2149caf2/opt/zephyr-sdk/arm-zephyr-eabi/bin/arm-zephyr-eabi-gcc.exe
MCUBoot bootloader key file: C:/ncs/v2.6.1/bootloader/mcuboot/root-rsa-2048.pem
-- Configuring done
-- Generating done
-- Build files have been written to: C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/mcuboot
=== child image mcuboot -  end ===

CMake Warning at C:/ncs/v2.6.1/nrf/modules/mcuboot/CMakeLists.txt:382 (message):
  

          ---------------------------------------------------------
          --- WARNING: Using default MCUBoot key, it should not ---
          --- be used for production.                           ---
          ---------------------------------------------------------
          



-- Build type:  
-- libmetal version: 1.4.0 (C:/nordic/DL02_S2MB_KPD_Small)
-- Host:    Windows/AMD64
-- Target:  Generic/arm
-- Machine: arm
-- Looking for include file stdatomic.h
-- Looking for include file stdatomic.h - found
-- open-amp version: 1.4.0 (C:/ncs/v2.6.1/modules/lib/open-amp/open-amp)
-- Host:    Windows/AMD64
-- Target:  Generic/arm
-- Machine: arm
-- C_FLAGS :  -Wall -Wextra
-- Looking for include file fcntl.h
-- Looking for include file fcntl.h - found
CMake Warning at C:/ncs/v2.6.1/zephyr/CMakeLists.txt:862 (message):
  No SOURCES given to Zephyr library: drivers__counter

  Excluding target from build.


CMake Warning at C:/ncs/v2.6.1/zephyr/CMakeLists.txt:1957 (message):
  __ASSERT() statements are globally ENABLED


-- Found partition manager static configuration: C:/nordic/DL02_S2MB_KPD_Small/configuration/dl02_s2mb_kpd_small_cpuapp/pm_static_dfu.yml
Partition 'mcuboot' is not included in the dynamic resolving since it is statically defined.
Partition 'mcuboot_pad' is not included in the dynamic resolving since it is statically defined.
Partition 'mcuboot_primary' is not included in the dynamic resolving since it is statically defined.
Partition 'mcuboot_primary_app' is not included in the dynamic resolving since it is statically defined.
Partition 'settings_storage' is not included in the dynamic resolving since it is statically defined.
Partition 'mcuboot_primary_1' is not included in the dynamic resolving since it is statically defined.
Partition 'mcuboot_secondary' is not included in the dynamic resolving since it is statically defined.
Partition 'mcuboot_secondary_1' is not included in the dynamic resolving since it is statically defined.
Partition 'pcd_sram' is not included in the dynamic resolving since it is statically defined.
Dropping partition 'hw_unique_key_partition' since its size is 0.
-- Configuring done
-- Generating done
-- Build files have been written to: C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build
-- west build: building application
[3/579] Generating include/generated/version.h
-- Zephyr version: 3.5.99 (C:/ncs/v2.6.1/zephyr), build: v3.5.99-ncs1-1
[8/579] Generating new Factory Data...
[INFO] Generating SPAKE2+ Verifier...
[WARNING] KEY password has not been provided. It means that DAC key is not encrypted.
[INFO] Validating JSON with schema...
[INFO] Validate OK
[3/280] Generating include/generated/version.h
-- Zephyr version: 3.5.99 (C:/ncs/v2.6.1/zephyr), build: v3.5.99-ncs1-1
[3/137] Generating include/generated/version.h
-- Zephyr version: 3.5.99 (C:/ncs/v2.6.1/zephyr), build: v3.5.99-ncs1-1
[137/137] Linking C executable zephyr\zephyr.elf
Memory region         Used Size  Region Size  %age Used
           FLASH:       23710 B      34176 B     69.38%
             RAM:        3528 B        64 KB      5.38%
           SRAM1:          0 GB        64 KB      0.00%
        IDT_LIST:          0 GB        32 KB      0.00%
[276/280] Linking C executable zephyr\zephyr.elf
Memory region         Used Size  Region Size  %age Used
           FLASH:      196496 B       222 KB     86.44%
             RAM:       61572 B        64 KB     93.95%
           SRAM1:          0 GB        64 KB      0.00%
        IDT_LIST:          0 GB        32 KB      0.00%
[3/292] Generating include/generated/version.h
-- Zephyr version: 3.5.99 (C:/ncs/v2.6.1/zephyr), build: v3.5.99-ncs1-1
[292/292] Linking C executable zephyr\zephyr.elf
Memory region         Used Size  Region Size  %age Used
           FLASH:       41672 B        52 KB     78.26%
             RAM:      293608 B       440 KB     65.17%
        IDT_LIST:          0 GB        32 KB      0.00%
[380/579] Generating ../../zephyr/net_core_app_update.bin
image.py: sign the payload

[381/579] Generating ../../zephyr/net_core_app_signed.hex
image.py: sign the payload

[389/579] Generating ../../zephyr/net_core_app_test_update.hex
image.py: sign the payload

[469/579] Performing build step for 'chip-gn'
Starting Matter library build in C:/nordic/DL02_S2MB_KPD_Small/DL02_S2MB_KPD_Small_build/modules/connectedhomeip
Done. Made 242 targets from 204 files in 238ms
[433/433] stamp obj/ABS_PATH/C/ncs/v2.6.1/modules/lib/matter/config/nrfconnect/chip-gn/default.stamp
Matter library build complete
[568/579] Linking CXX executable zephyr\zephyr.elf
Memory region         Used Size  Region Size  %age Used
           FLASH:      785100 B     957952 B     81.96%
             RAM:      210512 B       440 KB     46.72%
        IDT_LIST:          0 GB        32 KB      0.00%
[571/579] Generating ../../zephyr/app_update.bin
image.py: sign the payload
[573/579] Generating ../../zephyr/app_signed.hex
image.py: sign the payload
[574/579] Generating ../../zephyr/app_test_update.hex
image.py: sign the payload
[579/579] Generating zephyr/merged_domains.hex
 *  Terminal will be reused by tasks, press any key to close it. 