#include <arm/armv7-m.dtsi>
#include <nordic/nrf_common.dtsi>
#include <nordic/nrf52832.dtsi>
#include <zephyr/dt-bindings/adc/nrf-saadc-v2.h>
#include <zephyr/dt-bindings/regulator/nrf5x.h>

&pinctrl {
	i2c0_default: i2c0_default {
		group1 {
			psels = <NRF_PSEL(TWIM_SDA, 0, 6)>,
				<NRF_PSEL(TWIM_SCL, 0, 7)>;
		};
	};

	i2c0_sleep: i2c0_sleep {
		group1 {
			psels = <NRF_PSEL(TWIM_SDA, 0, 6)>,
				<NRF_PSEL(TWIM_SCL, 0, 7)>;
			low-power-enable;
		};
	};

	pwm0_default: pwm0_default {
		group1 {
			psels = <NRF_PSEL(PWM_OUT0, 0, 30)>;
			nordic,invert;
		};
	};

	pwm0_sleep: pwm0_sleep {
		group1 {
			psels = <NRF_PSEL(PWM_OUT0, 0, 30)>;
			low-power-enable;
		};
	};
};
