/dts-v1/;

/ {
	#address-cells = < 0x1 >;
	#size-cells = < 0x1 >;
	model = "Nordic nRF9160 DK NRF9160";
	compatible = "nordic,nrf9160-dk-nrf9160";
	chosen {
		zephyr,entropy = &psa_rng;
		zephyr,flash-controller = &flash_controller;
		zephyr,console = &uart0;
		zephyr,shell-uart = &uart0;
		zephyr,uart-mcumgr = &uart0;
		zephyr,flash = &flash0;
		zephyr,sram = &sram0_ns;
		zephyr,code-partition = &slot0_ns_partition;
	};
	aliases {
		led0 = &led0;
		led1 = &led1;
		led2 = &led2;
		led3 = &led3;
		pwm-led0 = &pwm_led0;
		sw0 = &button0;
		sw1 = &button1;
		sw2 = &button2;
		sw3 = &button3;
		bootloader-led0 = &led0;
		mcuboot-button0 = &button0;
		mcuboot-led0 = &led0;
		watchdog0 = &wdt0;
		spi-flash0 = &mx25r64;
	};
	soc {
		#address-cells = < 0x1 >;
		#size-cells = < 0x1 >;
		compatible = "nordic,nrf9160-sica", "nordic,nrf9160", "nordic,nrf91", "simple-bus";
		interrupt-parent = < &nvic >;
		ranges;
		nvic: interrupt-controller@e000e100 {
			#address-cells = < 0x1 >;
			compatible = "arm,v8m-nvic";
			reg = < 0xe000e100 0xc00 >;
			interrupt-controller;
			#interrupt-cells = < 0x2 >;
			arm,num-irq-priority-bits = < 0x3 >;
			phandle = < 0x1 >;
		};
		systick: timer@e000e010 {
			compatible = "arm,armv8m-systick";
			reg = < 0xe000e010 0x10 >;
			status = "disabled";
		};
		sram0: memory@20000000 {
			compatible = "mmio-sram";
			reg = < 0x20000000 0x40000 >;
		};
		peripheral@40000000 {
			#address-cells = < 0x1 >;
			#size-cells = < 0x1 >;
			ranges = < 0x0 0x40000000 0x10000000 >;
			flash_controller: flash-controller@39000 {
				compatible = "nordic,nrf91-flash-controller";
				reg = < 0x39000 0x1000 >;
				partial-erase;
				#address-cells = < 0x1 >;
				#size-cells = < 0x1 >;
				flash0: flash@0 {
					compatible = "soc-nv-flash";
					erase-block-size = < 0x1000 >;
					write-block-size = < 0x4 >;
					reg = < 0x0 0x100000 >;
					partitions {
						compatible = "fixed-partitions";
						#address-cells = < 0x1 >;
						#size-cells = < 0x1 >;
						boot_partition: partition@0 {
							label = "mcuboot";
							reg = < 0x0 0x10000 >;
						};
						slot0_partition: partition@10000 {
							label = "image-0";
							reg = < 0x10000 0x40000 >;
						};
						slot0_ns_partition: partition@50000 {
							label = "image-0-nonsecure";
							reg = < 0x50000 0x30000 >;
						};
						slot1_partition: partition@80000 {
							label = "image-1";
							reg = < 0x80000 0x40000 >;
						};
						slot1_ns_partition: partition@c0000 {
							label = "image-1-nonsecure";
							reg = < 0xc0000 0x30000 >;
						};
						storage_partition: partition@f8000 {
							label = "storage";
							reg = < 0xf8000 0x8000 >;
						};
					};
				};
			};
			adc: adc@e000 {
				compatible = "nordic,nrf-saadc";
				reg = < 0xe000 0x1000 >;
				interrupts = < 0xe 0x1 >;
				status = "okay";
				#io-channel-cells = < 0x1 >;
				phandle = < 0x13 >;
			};
			dppic: dppic@17000 {
				compatible = "nordic,nrf-dppic";
				reg = < 0x17000 0x1000 >;
				status = "okay";
			};
			egu0: egu@1b000 {
				compatible = "nordic,nrf-egu";
				reg = < 0x1b000 0x1000 >;
				interrupts = < 0x1b 0x1 >;
				status = "okay";
			};
			egu1: egu@1c000 {
				compatible = "nordic,nrf-egu";
				reg = < 0x1c000 0x1000 >;
				interrupts = < 0x1c 0x1 >;
				status = "okay";
			};
			egu2: egu@1d000 {
				compatible = "nordic,nrf-egu";
				reg = < 0x1d000 0x1000 >;
				interrupts = < 0x1d 0x1 >;
				status = "okay";
			};
			egu3: egu@1e000 {
				compatible = "nordic,nrf-egu";
				reg = < 0x1e000 0x1000 >;
				interrupts = < 0x1e 0x1 >;
				status = "okay";
			};
			egu4: egu@1f000 {
				compatible = "nordic,nrf-egu";
				reg = < 0x1f000 0x1000 >;
				interrupts = < 0x1f 0x1 >;
				status = "okay";
			};
			egu5: egu@20000 {
				compatible = "nordic,nrf-egu";
				reg = < 0x20000 0x1000 >;
				interrupts = < 0x20 0x1 >;
				status = "okay";
			};
			ipc: ipc@2a000 {
				compatible = "nordic,nrf-ipc";
				reg = < 0x2a000 0x1000 >;
				interrupts = < 0x2a 0x1 >;
				status = "okay";
			};
			i2s0: i2s@28000 {
				compatible = "nordic,nrf-i2s";
				#address-cells = < 0x1 >;
				#size-cells = < 0x0 >;
				reg = < 0x28000 0x1000 >;
				interrupts = < 0x28 0x1 >;
				status = "disabled";
			};
			kmu: kmu@39000 {
				compatible = "nordic,nrf-kmu";
				reg = < 0x39000 0x1000 >;
				interrupts = < 0x39 0x1 >;
				status = "okay";
			};
			pdm0: pdm@26000 {
				compatible = "nordic,nrf-pdm";
				reg = < 0x26000 0x1000 >;
				interrupts = < 0x26 0x1 >;
				status = "disabled";
			};
			regulators: regulator@4000 {
				compatible = "nordic,nrf-regulators";
				reg = < 0x4000 0x1000 >;
				status = "okay";
			};
			vmc: vmc@3a000 {
				compatible = "nordic,nrf-vmc";
				reg = < 0x3a000 0x1000 >;
				status = "okay";
			};
			uart0: uart@8000 {
				compatible = "nordic,nrf-uarte";
				reg = < 0x8000 0x1000 >;
				interrupts = < 0x8 0x1 >;
				status = "okay";
				current-speed = < 0x1c200 >;
				pinctrl-0 = < &uart0_default >;
				pinctrl-1 = < &uart0_sleep >;
				pinctrl-names = "default", "sleep";
			};
			uart1: arduino_serial: uart@9000 {
				compatible = "nordic,nrf-uarte";
				reg = < 0x9000 0x1000 >;
				interrupts = < 0x9 0x1 >;
				status = "disabled";
				current-speed = < 0x1c200 >;
				pinctrl-0 = < &uart1_default >;
				pinctrl-1 = < &uart1_sleep >;
				pinctrl-names = "default", "sleep";
			};
			uart2: uart@a000 {
				compatible = "nordic,nrf-uarte";
				reg = < 0xa000 0x1000 >;
				interrupts = < 0xa 0x1 >;
				status = "disabled";
				pinctrl-0 = < &uart2_default >;
				pinctrl-1 = < &uart2_sleep >;
				pinctrl-names = "default", "sleep";
			};
			uart3: uart@b000 {
				compatible = "nordic,nrf-uarte";
				reg = < 0xb000 0x1000 >;
				interrupts = < 0xb 0x1 >;
				status = "disabled";
			};
			i2c0: i2c@8000 {
				compatible = "nordic,nrf-twim";
				#address-cells = < 0x1 >;
				#size-cells = < 0x0 >;
				reg = < 0x8000 0x1000 >;
				clock-frequency = < 0x186a0 >;
				interrupts = < 0x8 0x1 >;
				status = "disabled";
			};
			i2c1: i2c@9000 {
				compatible = "nordic,nrf-twim";
				#address-cells = < 0x1 >;
				#size-cells = < 0x0 >;
				reg = < 0x9000 0x1000 >;
				clock-frequency = < 0x186a0 >;
				interrupts = < 0x9 0x1 >;
				status = "disabled";
			};
			i2c2: arduino_i2c: i2c@a000 {
				compatible = "nordic,nrf-twim";
				#address-cells = < 0x1 >;
				#size-cells = < 0x0 >;
				reg = < 0xa000 0x1000 >;
				clock-frequency = < 0x61a80 >;
				interrupts = < 0xa 0x1 >;
				status = "okay";
				pinctrl-0 = < &i2c2_default >;
				pinctrl-1 = < &i2c2_sleep >;
				pinctrl-names = "default", "sleep";
				pcal6408a: pcal6408a@20 {
					compatible = "nxp,pcal6408a";
					status = "disabled";
					reg = < 0x20 >;
					gpio-controller;
					#gpio-cells = < 0x2 >;
					ngpios = < 0x8 >;
					int-gpios = < &gpio0 0x6 0x11 >;
				};
			};
			i2c3: i2c@b000 {
				compatible = "nordic,nrf-twim";
				#address-cells = < 0x1 >;
				#size-cells = < 0x0 >;
				reg = < 0xb000 0x1000 >;
				clock-frequency = < 0x186a0 >;
				interrupts = < 0xb 0x1 >;
				status = "disabled";
			};
			spi0: spi@8000 {
				compatible = "nordic,nrf-spim";
				#address-cells = < 0x1 >;
				#size-cells = < 0x0 >;
				reg = < 0x8000 0x1000 >;
				interrupts = < 0x8 0x1 >;
				max-frequency = < 0x7a1200 >;
				easydma-maxcnt-bits = < 0xd >;
				status = "disabled";
			};
			spi1: spi@9000 {
				compatible = "nordic,nrf-spim";
				#address-cells = < 0x1 >;
				#size-cells = < 0x0 >;
				reg = < 0x9000 0x1000 >;
				interrupts = < 0x9 0x1 >;
				max-frequency = < 0x7a1200 >;
				easydma-maxcnt-bits = < 0xd >;
				status = "disabled";
			};
			spi2: spi@a000 {
				compatible = "nordic,nrf-spim";
				#address-cells = < 0x1 >;
				#size-cells = < 0x0 >;
				reg = < 0xa000 0x1000 >;
				interrupts = < 0xa 0x1 >;
				max-frequency = < 0x7a1200 >;
				easydma-maxcnt-bits = < 0xd >;
				status = "disabled";
			};
			spi3: arduino_spi: spi@b000 {
				compatible = "nordic,nrf-spim";
				#address-cells = < 0x1 >;
				#size-cells = < 0x0 >;
				reg = < 0xb000 0x1000 >;
				interrupts = < 0xb 0x1 >;
				max-frequency = < 0x7a1200 >;
				easydma-maxcnt-bits = < 0xd >;
				status = "okay";
				cs-gpios = < &arduino_header 0x10 0x1 >, < &gpio0 0x19 0x1 >;
				pinctrl-0 = < &spi3_default >;
				pinctrl-1 = < &spi3_sleep >;
				pinctrl-names = "default", "sleep";
				mx25r64: mx25r6435f@1 {
					compatible = "jedec,spi-nor";
					status = "disabled";
					reg = < 0x1 >;
					spi-max-frequency = < 0x7a1200 >;
					jedec-id = [ C2 28 17 ];
					sfdp-bfp = [ E5 20 F1 FF FF FF FF 03 44 EB 08 6B 08 3B 04 BB EE FF FF FF FF FF 00 FF FF FF 00 FF 0C 20 0F 52 10 D8 00 FF 23 72 F5 00 82 ED 04 CC 44 83 48 44 30 B0 30 B0 F7 C4 D5 5C 00 BE 29 FF F0 D0 FF FF ];
					size = < 0x4000000 >;
					has-dpd;
					t-enter-dpd = < 0x2710 >;
					t-exit-dpd = < 0x88b8 >;
				};
				nrf700x: nrf7002@0 {
					compatible = "nordic,nrf700x-spi";
					status = "okay";
					reg = < 0x0 >;
					spi-max-frequency = < 0x7a1200 >;
					iovdd-ctrl-gpios = < &arduino_header 0x6 0x20 >;
					bucken-gpios = < &arduino_header 0x7 0x20 >;
					host-irq-gpios = < &arduino_header 0xd 0x0 >;
				};
			};
			pwm0: pwm@21000 {
				compatible = "nordic,nrf-pwm";
				reg = < 0x21000 0x1000 >;
				interrupts = < 0x21 0x1 >;
				status = "okay";
				#pwm-cells = < 0x3 >;
				pinctrl-0 = < &pwm0_default >;
				pinctrl-1 = < &pwm0_sleep >;
				pinctrl-names = "default", "sleep";
				phandle = < 0x11 >;
			};
			pwm1: pwm@22000 {
				compatible = "nordic,nrf-pwm";
				reg = < 0x22000 0x1000 >;
				interrupts = < 0x22 0x1 >;
				status = "disabled";
				#pwm-cells = < 0x3 >;
			};
			pwm2: pwm@23000 {
				compatible = "nordic,nrf-pwm";
				reg = < 0x23000 0x1000 >;
				interrupts = < 0x23 0x1 >;
				status = "disabled";
				#pwm-cells = < 0x3 >;
			};
			pwm3: pwm@24000 {
				compatible = "nordic,nrf-pwm";
				reg = < 0x24000 0x1000 >;
				interrupts = < 0x24 0x1 >;
				status = "disabled";
				#pwm-cells = < 0x3 >;
			};
			gpio0: gpio@842500 {
				compatible = "nordic,nrf-gpio";
				gpio-controller;
				reg = < 0x842500 0x300 >;
				#gpio-cells = < 0x2 >;
				status = "okay";
				port = < 0x0 >;
				phandle = < 0xa >;
			};
			rtc0: rtc@14000 {
				compatible = "nordic,nrf-rtc";
				reg = < 0x14000 0x1000 >;
				cc-num = < 0x4 >;
				interrupts = < 0x14 0x1 >;
				status = "disabled";
				clock-frequency = < 0x8000 >;
				prescaler = < 0x1 >;
			};
			rtc1: rtc@15000 {
				compatible = "nordic,nrf-rtc";
				reg = < 0x15000 0x1000 >;
				cc-num = < 0x4 >;
				interrupts = < 0x15 0x1 >;
				status = "disabled";
				clock-frequency = < 0x8000 >;
				prescaler = < 0x1 >;
			};
			clock: clock@5000 {
				compatible = "nordic,nrf-clock";
				reg = < 0x5000 0x1000 >;
				interrupts = < 0x5 0x1 >;
				status = "okay";
			};
			power: power@5000 {
				compatible = "nordic,nrf-power";
				reg = < 0x5000 0x1000 >;
				interrupts = < 0x5 0x1 >;
				status = "okay";
				#address-cells = < 0x1 >;
				#size-cells = < 0x1 >;
				gpregret1: gpregret1@551c {
					#address-cells = < 0x1 >;
					#size-cells = < 0x1 >;
					compatible = "nordic,nrf-gpregret";
					reg = < 0x551c 0x1 >;
					status = "okay";
				};
				gpregret2: gpregret2@5520 {
					#address-cells = < 0x1 >;
					#size-cells = < 0x1 >;
					compatible = "nordic,nrf-gpregret";
					reg = < 0x5520 0x1 >;
					status = "okay";
				};
			};
			wdt: wdt0: watchdog@18000 {
				compatible = "nordic,nrf-wdt";
				reg = < 0x18000 0x1000 >;
				interrupts = < 0x18 0x1 >;
				status = "okay";
			};
			timer0: timer@f000 {
				compatible = "nordic,nrf-timer";
				status = "disabled";
				reg = < 0xf000 0x1000 >;
				cc-num = < 0x6 >;
				max-bit-width = < 0x20 >;
				interrupts = < 0xf 0x1 >;
				prescaler = < 0x0 >;
			};
			timer1: timer@10000 {
				compatible = "nordic,nrf-timer";
				status = "disabled";
				reg = < 0x10000 0x1000 >;
				cc-num = < 0x6 >;
				max-bit-width = < 0x20 >;
				interrupts = < 0x10 0x1 >;
				prescaler = < 0x0 >;
				phandle = < 0x10 >;
			};
			timer2: timer@11000 {
				compatible = "nordic,nrf-timer";
				status = "disabled";
				reg = < 0x11000 0x1000 >;
				cc-num = < 0x6 >;
				max-bit-width = < 0x20 >;
				interrupts = < 0x11 0x1 >;
				prescaler = < 0x0 >;
			};
		};
		gpiote: gpiote@40031000 {
			compatible = "nordic,nrf-gpiote";
			reg = < 0x40031000 0x1000 >;
			interrupts = < 0x31 0x5 >;
			status = "okay";
		};
	};
	pinctrl: pin-controller {
		compatible = "nordic,nrf-pinctrl";
		uart0_default: uart0_default {
			phandle = < 0x2 >;
			group1 {
				psels = < 0x1d >, < 0x2001b >;
			};
			group2 {
				psels = < 0x1001c >, < 0x3001a >;
				bias-pull-up;
			};
		};
		uart0_sleep: uart0_sleep {
			phandle = < 0x3 >;
			group1 {
				psels = < 0x1d >, < 0x1001c >, < 0x2001b >, < 0x3001a >;
				low-power-enable;
			};
		};
		uart1_default: uart1_default {
			phandle = < 0x4 >;
			group1 {
				psels = < 0x1 >, < 0x2000e >;
			};
			group2 {
				psels = < 0x10000 >, < 0x3000f >;
				bias-pull-up;
			};
		};
		uart1_sleep: uart1_sleep {
			phandle = < 0x5 >;
			group1 {
				psels = < 0x1 >, < 0x10000 >, < 0x2000e >, < 0x3000f >;
				low-power-enable;
			};
		};
		uart2_default: uart2_default {
			phandle = < 0x6 >;
			group1 {
				psels = < 0x18 >, < 0x10017 >;
			};
		};
		uart2_sleep: uart2_sleep {
			phandle = < 0x7 >;
			group1 {
				psels = < 0x18 >, < 0x10017 >;
				low-power-enable;
			};
		};
		i2c2_default: i2c2_default {
			phandle = < 0x8 >;
			group1 {
				psels = < 0xc001e >, < 0xb001f >;
			};
		};
		i2c2_sleep: i2c2_sleep {
			phandle = < 0x9 >;
			group1 {
				psels = < 0xc001e >, < 0xb001f >;
				low-power-enable;
			};
		};
		pwm0_default: pwm0_default {
			phandle = < 0xe >;
			group1 {
				psels = < 0x160002 >;
			};
		};
		pwm0_sleep: pwm0_sleep {
			phandle = < 0xf >;
			group1 {
				psels = < 0x160002 >;
				low-power-enable;
			};
		};
		spi3_default: spi3_default {
			phandle = < 0xc >;
			group1 {
				psels = < 0x4000d >, < 0x6000c >, < 0x5000b >;
				nordic,drive-mode = < 0x3 >;
			};
		};
		spi3_sleep: spi3_sleep {
			phandle = < 0xd >;
			group1 {
				psels = < 0x4000d >, < 0x6000c >, < 0x5000b >;
				low-power-enable;
			};
		};
	};
	rng_hci: entropy_bt_hci {
		compatible = "zephyr,bt-hci-entropy";
		status = "okay";
	};
	sw_pwm: sw-pwm {
		compatible = "nordic,nrf-sw-pwm";
		status = "disabled";
		generator = < &timer1 >;
		clock-prescaler = < 0x0 >;
		#pwm-cells = < 0x3 >;
	};
	cpus {
		#address-cells = < 0x1 >;
		#size-cells = < 0x0 >;
		cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-m33f";
			reg = < 0x0 >;
			#address-cells = < 0x1 >;
			#size-cells = < 0x1 >;
			mpu: mpu@e000ed90 {
				compatible = "arm,armv8m-mpu";
				reg = < 0xe000ed90 0x40 >;
				arm,num-mpu-regions = < 0x10 >;
			};
		};
	};
	psa_rng: psa-rng {
		compatible = "zephyr,psa-crypto-rng";
		status = "okay";
	};
	leds {
		compatible = "gpio-leds";
		led0: led_0 {
			gpios = < &gpio0 0x2 0x0 >;
			label = "Green LED 1";
			status = "disabled";
		};
		led1: led_1 {
			gpios = < &gpio0 0x3 0x0 >;
			label = "Green LED 2";
			status = "disabled";
		};
		led2: led_2 {
			gpios = < &gpio0 0x4 0x0 >;
			label = "Green LED 3";
			status = "disabled";
		};
		led3: led_3 {
			gpios = < &gpio0 0x5 0x0 >;
			label = "Green LED 4";
			status = "disabled";
		};
	};
	pwmleds {
		compatible = "pwm-leds";
		pwm_led0: pwm_led_0 {
			pwms = < &pwm0 0x0 0x1312d00 0x0 >;
		};
	};
	buttons {
		compatible = "gpio-keys";
		button0: button_0 {
			gpios = < &gpio0 0x6 0x11 >;
			label = "Push button 1";
			zephyr,code = < 0xb >;
			status = "disabled";
		};
		button1: button_1 {
			gpios = < &gpio0 0x7 0x11 >;
			label = "Push button 2";
			zephyr,code = < 0x2 >;
			status = "disabled";
		};
		button2: button_2 {
			gpios = < &gpio0 0x8 0x11 >;
			label = "Switch 1";
			zephyr,code = < 0x3 >;
		};
		button3: button_3 {
			gpios = < &gpio0 0x9 0x11 >;
			label = "Switch 2";
			zephyr,code = < 0x4 >;
		};
	};
	interface_to_nrf52840: gpio-interface {
		compatible = "nordic,nrf9160dk-nrf52840-interface";
		#gpio-cells = < 0x2 >;
		gpio-map-mask = < 0xf 0x0 >;
		gpio-map-pass-thru = < 0x0 0xffffffff >;
		gpio-map = < 0x0 0x0 &gpio0 0x11 0x0 >, < 0x1 0x0 &gpio0 0x12 0x0 >, < 0x2 0x0 &gpio0 0x13 0x0 >, < 0x3 0x0 &gpio0 0x15 0x0 >, < 0x4 0x0 &gpio0 0x16 0x0 >, < 0x5 0x0 &gpio0 0x17 0x0 >, < 0x9 0x0 &gpio0 0x18 0x0 >;
		phandle = < 0x12 >;
	};
	nrf52840_reset: gpio-reset {
		compatible = "nordic,nrf9160dk-nrf52840-reset";
		status = "disabled";
		gpios = < &interface_to_nrf52840 0x9 0x1 >;
	};
	arduino_header: connector {
		compatible = "arduino-header-r3";
		#gpio-cells = < 0x2 >;
		gpio-map-mask = < 0xffffffff 0xffffffc0 >;
		gpio-map-pass-thru = < 0x0 0x3f >;
		gpio-map = < 0x0 0x0 &gpio0 0xe 0x0 >, < 0x1 0x0 &gpio0 0xf 0x0 >, < 0x2 0x0 &gpio0 0x10 0x0 >, < 0x3 0x0 &gpio0 0x11 0x0 >, < 0x4 0x0 &gpio0 0x12 0x0 >, < 0x5 0x0 &gpio0 0x13 0x0 >, < 0x6 0x0 &gpio0 0x0 0x0 >, < 0x7 0x0 &gpio0 0x1 0x0 >, < 0x8 0x0 &gpio0 0x2 0x0 >, < 0x9 0x0 &gpio0 0x3 0x0 >, < 0xa 0x0 &gpio0 0x4 0x0 >, < 0xb 0x0 &gpio0 0x5 0x0 >, < 0xc 0x0 &gpio0 0x6 0x0 >, < 0xd 0x0 &gpio0 0x7 0x0 >, < 0xe 0x0 &gpio0 0x8 0x0 >, < 0xf 0x0 &gpio0 0x9 0x0 >, < 0x10 0x0 &gpio0 0xa 0x0 >, < 0x11 0x0 &gpio0 0xb 0x0 >, < 0x12 0x0 &gpio0 0xc 0x0 >, < 0x13 0x0 &gpio0 0xd 0x0 >, < 0x14 0x0 &gpio0 0x1e 0x0 >, < 0x15 0x0 &gpio0 0x1f 0x0 >;
		phandle = < 0xb >;
	};
	arduino_adc: analog-connector {
		compatible = "arduino,uno-adc";
		#io-channel-cells = < 0x1 >;
		io-channel-map = < 0x0 &adc 0x1 >, < 0x1 &adc 0x2 >, < 0x2 &adc 0x3 >, < 0x3 &adc 0x4 >, < 0x4 &adc 0x5 >, < 0x5 &adc 0x6 >;
	};
	reserved-memory {
		#address-cells = < 0x1 >;
		#size-cells = < 0x1 >;
		ranges;
		sram0_s: image_s@20000000 {
			reg = < 0x20000000 0x16000 >;
		};
		sram0_modem: image_modem@20016000 {
			reg = < 0x20016000 0xa000 >;
		};
		sram0_ns: image_ns@20020000 {
			reg = < 0x20020000 0x20000 >;
		};
	};
	nrf_radio_coex: nrf7002-coex {
		status = "okay";
		compatible = "nordic,nrf700x-coex";
		status0-gpios = < &arduino_header 0x8 0x0 >;
		req-gpios = < &arduino_header 0x9 0x0 >;
		grant-gpios = < &arduino_header 0xa 0x21 >;
		swctrl1-gpios = < &arduino_header 0xc 0x0 >;
	};
};
