#

##

##

    µVision Build Log
    Project:
    C:\Users\zhu\Desktop\nrf51822-flash\nrf51822_application\Board\pca10001\s110\experimental\ble_app_uart\arm\ble_app_uart.uvproj
    Project File Date:  06/01/2016

    Output:
    Rebuild target 'nrf51822_xxaa_s110 (256K)'
    assembling arm_startup_nrf51.s...
    compiling system_nrf51.c...
    compiling main.c...
    ..\main.c(234): warning:  #550-D: variable "sum" was set but never used
        uint8_t val,len,sum;
    ..\main.c: 1 warning, 0 errors
    compiling ble_srv_common.c...
    compiling ble_nus.c...
    compiling ble_advdata.c...
    compiling ble_conn_params.c...
    compiling softdevice_handler.c...
    compiling simple_uart.c...
    compiling app_timer.c...
    compiling pstorage.c...
    linking...
    Program Size: Code=12988 RO-data=244 RW-data=144 ZI-data=3096
    FromELF: creating hex file...
    ".\_build\application.axf" - 0 Error(s), 1 Warning(s).
    Load "C:\\Users\\zhu\\Desktop\\nrf51822-flash\\nrf51822_application\\Board\\pca10001\\s110\\experimental\\ble_app_uart\\arm\\_build\\application.axf"
    Set JLink Project File to "C:\Users\zhu\Desktop\nrf51822-flash\nrf51822_application\Board\pca10001\s110\experimental\ble_app_uart\arm\JLinkSettings.ini"
    * JLink Info: Device "NRF51822_XXAA" selected.

    JLink info:
    ------------
    DLL: V4.98b, compiled Apr 10 2015 20:15:52
    Firmware: J-Link OB-SAM3U128 V1 compiled Nov 28 2014 10:24:11
    Hardware: V1.00
    S/N : 480205921

    * JLink Info: Found SWD-DP with ID 0x0BB11477
    * JLink Info: Found Cortex-M0 r0p0, Little endian.
    * JLink Info: FPUnit: 4 code (BP) slots and 0 literal slots
    * JLink Info: CoreSight components:
    * JLink Info: ROMTbl 0 @ F0000000
    * JLink Info: ROMTbl 0 [0]: F00FF000, CID: B105100D, PID: 000BB471 ROM Table
    * JLink Info: ROMTbl 1 @ E00FF000
    * JLink Info: ROMTbl 1 [0]: FFF0F000, CID: B105E00D, PID: 000BB008 SCS
    * JLink Info: ROMTbl 1 [1]: FFF02000, CID: B105E00D, PID: 000BB00A DWT
    * JLink Info: ROMTbl 1 [2]: FFF03000, CID: B105E00D, PID: 000BB00B FPB
    * JLink Info: ROMTbl 0 [1]: 00002000, CID: B105900D, PID: 000BB9A3 ???
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: nRF51822_xxAA
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 8192
    Watchpoints:          2
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...

AG speed: 2000 kHz Erase Done. Programming Done. Verify OK. Application running ... \\arm\\_build\\application.axf" Set JLink Project File to "C:\Users\zhu\Desktop\nrf51822-flash\nrf51822_application\Board\pca10001\s110\experimental\ble_app_uart\arm\JLinkSettings.ini" * JLink Info: Device "NRF51822_XXAA" selected. JLink info: ------------ DLL: V4.98b, compiled Apr 10 2015 20:15:52 Firmware: J-Link OB-SAM3U128 V1 compiled Nov 28 2014 10:24:11 Hardware: V1.00 S/N : 480205921 * JLink Info: Found SWD-DP with ID 0x0BB11477 * JLink Info: Found Cortex-M0 r0p0, Little endian. * JLink Info: FPUnit: 4 code (BP) slots and 0 literal slots * JLink Info: CoreSight components: * JLink Info: ROMTbl 0 @ F0000000 * JLink Info: ROMTbl 0 [0]: F00FF000, CID: B105100D, PID: 000BB471 ROM Table * JLink Info: ROMTbl 1 @ E00FF000 * JLink Info: ROMTbl 1 [0]: FFF0F000, CID: B105E00D, PID: 000BB008 SCS * JLink Info: ROMTbl 1 [1]: FFF02000, CID: B105E00D, PID: 000BB00A DWT * JLink Info: ROMTbl 1 [2]: FFF03000, CID: B105E00D, PID: 000BB00B FPB * JLink Info: ROMTbl 0 [1]: 00002000, CID: B105900D, PID: 000BB9A3 ??? ROMTableAddr = 0xE00FF003 Target info: ------------ Device: nRF51822_xxAA VTarget = 3.300V State of Pins: TCK: 0, TDI: 0, TDO: 1, TMS: 1, TRES: 1, TRST: 1 Hardware-Breakpoints: 4 Software-Breakpoints: 8192 Watchpoints: 2 JTAG speed: 2000 kHz Erase Done. Programming Done. Verify OK. Application running ...