<!DOCTYPE CrossStudio_Project_File>
<solution Name="nRF51802_test" target="8" version="2">
  <project Name="nRF51802_test">
    <configuration
      Name="Common"
      Placement="Flash"
      Target="nRF51802_xxAA"
      arm_architecture="v6M"
      arm_core_type="Cortex-M0"
      arm_endian="Little"
      arm_fp_abi="None"
      arm_fpu_type="None"
      arm_interwork="No"
      arm_linker_heap_size="512"
      arm_linker_process_stack_size="0"
      arm_linker_stack_size="2048"
      arm_simulator_memory_simulation_parameter="ROM;0x00000000;0x00040000;RAM;0x20000000;0x00004000"
      arm_target_debug_interface_type="ADIv5"
      arm_target_device_name="nRF51802_xxAA"
      arm_target_interface_type="SWD"
      c_preprocessor_definitions="NRF51;__nRF_FAMILY;ARM_MATH_CM0;FLASH_PLACEMENT=1;BLE_STACK_SUPPORT_REQD;NRF51802;NRF_SD_BLE_API_VERSION=2;S130;SOFTDEVICE_PRESENT;SWI_DISABLE0;DEBUG"
      c_user_include_directories="$(ProjectDir);$(ProjectDir)/CMSIS_4/CMSIS/Include;$(ProjectDir)/nRF/CMSIS/Device/Include;$(ProjectDir)/SoftDevice/common;$(ProjectDir)/SoftDevice/common/softdevice_handler;$(ProjectDir)/SoftDevice/s130/headers;$(ProjectDir)/SoftDevice/s130/hex;$(ProjectDir)/libraries/util;$(ProjectDir)/libraries/log;$(ProjectDir)/libraries/log/src;$(ProjectDir)/libraries/fds;$(ProjectDir)/libraries/fstorage;$(ProjectDir)/libraries/timer;$(ProjectDir)/libraries/hardfault;$(ProjectDir)/libraries/experimental_section_vars;$(ProjectDir)/drivers_nrf/clock;$(ProjectDir)/drivers_nrf/common;$(ProjectDir)/drivers_nrf/delay;$(ProjectDir)/drivers_nrf/hal;$(ProjectDir)/drivers_nrf/uart"
      debug_additional_load_file="$(ProjectDir)/SoftDevice/s130/hex/s130_nrf51_2.0.1_softdevice.hex"
      debug_register_definition_file="$(ProjectDir)/nrf51_Registers.xml"
      debug_target_connection="J-Link"
      gcc_entry_point="Reset_Handler"
      linker_memory_map_file=""
      linker_output_format="hex"
      linker_section_placement_file="$(ProjectDir)/flash_placement.xml"
      linker_section_placement_macros="FLASH_PH_START=0x0 ;FLASH_PH_SIZE=0x40000;RAM_PH_START=0x20000000;RAM_PH_SIZE=0x4000;FLASH_START=0x1b000;FLASH_SIZE=0x25000;RAM_START=0x20001508;RAM_SIZE=0x2af8"
      linker_section_placements_segments="FLASH RX 0x0 0x40000 ;RAM RWX 0x20000000 0x4000"
      macros="DeviceHeaderFile=$(PackagesDir)/nRF/CMSIS/Device/Include/nrf.h;DeviceLibraryIdentifier=M0l;DeviceSystemFile=$(PackagesDir)/nRF/CMSIS/Device/Source/system_nrf51.c;DeviceVectorsFile=$(PackagesDir)/nRF/Source/ses_nrf51_Vectors.s;DeviceFamily=nRF;Target=nRF51802_xxAA;Placement=Flash"
      project_directory=""
      project_type="Executable"
      target_reset_script="Reset();"
      target_script_file="$(ProjectDir)/nRF_Target.js"
      target_trace_initialize_script="EnableTrace(&quot;$(TraceInterfaceType)&quot;)" />
    <folder Name="CMSIS Files">
      <file file_name="nrf.h" />
      <file file_name="system_nrf51.c">
        <configuration
          Name="Common"
          default_code_section=".init"
          default_const_section=".init_rodata" />
      </file>
    </folder>
    <folder Name="RTT Files">
      <file file_name="SEGGER_RTT.c" />
      <file file_name="SEGGER_RTT.h" />
      <file file_name="SEGGER_RTT_Conf.h" />
      <file file_name="SEGGER_RTT_SES.c" />
    </folder>
    <folder Name="Script Files">
      <file file_name="nRF_Target.js">
        <configuration Name="Common" file_type="Reset Script" />
      </file>
    </folder>
    <folder Name="Source Files">
      <configuration Name="Common" filter="c;cpp;cxx;cc;h;s;asm;inc" />
      <file file_name="sdk_config.h" />
      <file file_name="main.c" />
    </folder>
    <folder Name="System Files">
      <file file_name="thumb_crt0.s" />
      <file file_name="ses_nRF_Startup.s" />
      <file file_name="ses_nrf51_Vectors.s">
        <configuration Name="Common" file_type="Assembly" />
      </file>
    </folder>
    <configuration
      Name="Debug"
      linker_section_placement_macros="FLASH_PH_START=0x0 ;FLASH_PH_SIZE=0x20000;RAM_PH_START=0x20000000;RAM_PH_SIZE=0x4000;FLASH_START=0x1b000;FLASH_SIZE=0x5000;RAM_START=0x20001fe8;RAM_SIZE=0x2018" />
    <folder Name="nRF_SoftDevice">
      <file file_name="SoftDevice/common/softdevice_handler/softdevice_handler.c" />
    </folder>
    <folder Name="nRF_Drivers">
      <file file_name="drivers_nrf/clock/nrf_drv_clock.c" />
      <file file_name="drivers_nrf/common/nrf_drv_common.c" />
      <file file_name="drivers_nrf/uart/nrf_drv_uart.c" />
    </folder>
    <folder Name="nRF_Log">
      <file file_name="libraries/log/src/nrf_log_backend_serial.c" />
      <file file_name="libraries/log/src/nrf_log_frontend.c" />
    </folder>
    <folder Name="nRF_Libraries">
      <file file_name="libraries/util/app_error.c" />
      <file file_name="libraries/util/app_error_weak.c" />
      <file file_name="libraries/util/app_util_platform.c" />
      <file file_name="libraries/util/nrf_assert.c" />
      <file file_name="libraries/util/sdk_errors.c" />
      <file file_name="libraries/util/sdk_mapped_flags.c" />
      <file file_name="libraries/timer/app_timer.c" />
      <file file_name="libraries/hardfault/hardfault_implementation.c" />
      <file file_name="libraries/fds/fds.c" />
      <file file_name="libraries/fstorage/fstorage.c" />
    </folder>
  </project>
  <configuration
    Name="Debug"
    c_preprocessor_definitions="DEBUG"
    gcc_debugging_level="Level 3"
    gcc_optimization_level="None" />
  <configuration
    Name="Release"
    c_preprocessor_definitions="NDEBUG"
    gcc_debugging_level="None"
    gcc_omit_frame_pointer="Yes"
    gcc_optimization_level="Level 1" />
</solution>
