// To get started, press Ctrl+Space to bring up the completion menu and view the available nodes.

// You can also use the buttons in the sidebar to perform actions on nodes.
// Actions currently available include:

// * Enabling / disabling the node
// * Adding the bus to a bus
// * Removing the node
// * Connecting ADC channels

// For more help, browse the DeviceTree documentation at https://docs.zephyrproject.org/latest/guides/dts/index.html
// You can also visit the nRF DeviceTree extension documentation at https://docs.nordicsemi.com/bundle/nrf-connect-vscode/page/guides/ncs_configure_app.html#devicetree-support-in-the-extension
/{
    chosen {
            zephyr,console = &uart00;
            zephyr,shell-uart = &uart00;
            zephyr,uart-mcumgr = &uart00;
            zephyr,bt-mon-uart = &uart00;
            zephyr,bt-c2h-uart = &uart00;
    };
};


&uart20_default {
		group1 {
			psels = <NRF_PSEL(UART_TX, 1, 4)>,
				<NRF_PSEL(UART_RTS, 1, 6)>;
		};

		group2 {
			psels = <NRF_PSEL(UART_RX, 1, 5)>,
				<NRF_PSEL(UART_CTS, 1, 7)>;
			bias-pull-up;
		};
	};

&uart00 {
	current-speed = <2000000>;
    status = "okay";
	pinctrl-0 = <&uart20_default>;
	pinctrl-1 = <&uart20_sleep>;
	pinctrl-names = "default", "sleep";
    };

&uart20 {
    status = "disabled";
};