.. _nrf53_audio_app_dk_legal:
.. _nrf53_audio_feature_support:

nRF5340 Audio feature support and QDIDs
#######################################

.. contents::
   :local:
   :depth: 2

The following table lists features of the nRF5340 Audio application and their respective limitations and maturity level.
For an explanation of the maturity levels, see :ref:`Software maturity levels <software_maturity>`.

.. note::
   Features not listed are not supported.

.. include:: /releases_and_maturity/software_maturity.rst
   :start-after: software_maturity_application_nrf5340audio_table:
   :end-before: software_maturity_protocol

.. _nrf5340_audio_dns_and_qdids:

nRF5340 Audio DNs and QDIDs
***************************

The following DNs (Design Numbers) and QDIDs (Qualified Design IDs) are related to the nRF5340 LE Audio applications:

nRF5340 Bluetooth DNs/QDIDs
   See `nRF5340 Bluetooth DNs and QDIDs Compatibility Matrix`_ for the DNs/QDIDs for nRF5340 LE Audio applications.

   A full Audio product DN will typically require DNs/QDIDs for Controller component, Host component, Profiles and Services component and LC3 codec component.
   The exact DN/QDID numbers depend on the project configuration and the features used in the application.

   .. note::
      * The DNs/QDIDs listed in the Compatibility Matrix might not cover all use cases or combinations.
        The full details of what is supported by a DN/QDID can be found in the associated ICS (Implementation Conformance Statement).

      * The Audio applications do not demonstrate the full capabilities of the underlying DNs/QDIDs.
        At the same time, the Audio applications may demonstrate features not available in the underlying DNs/QDID.

.. ncs-include:: lc3/README.rst
   :docset: nrfxlib
   :start-after: lc3_qdid_start
   :end-before: lc3_qdid_end
