/*
 * Copyright (c) 2022 IoT.bzh
 *
 * SPDX-License-Identifier: Apache-2.0
 */

/ {
    pwmleds {
        compatible = "pwm-leds";
        pwm_led_0: pwm_led_0 {
            pwms = <&pwm0 0 PWM_MSEC(20) PWM_POLARITY_NORMAL>;
            label = "PWM LED 0";
        };
    };

    aliases {
        pwm-led0 = &pwm_led_0;
        pwm-0 = &pwm0;
    };

};

&pwm0 {
    status = "okay";
};
