/*
 * SPDX-License-Identifier: Apache-2.0
 *
 * Copyright (c) 2022 STMicroelectronics
 */


/ {
	pwmleds: pwmleds {
		compatible = "pwm-leds";
		status = "okay";

		green_pwm_led: green_pwm_led {
			pwms = <&pwm2 1 PWM_MSEC(20) PWM_POLARITY_NORMAL>;
		};
	};

    aliases {
        pwm-led0 = &green_pwm_led;
    };

};

&pwm2 {
	status = "okay";
};
