ivo@system76-pc:~/src/nrf91-1.5.0/ncs/nrf/samples/nrf9160/fmfu_smp_svr$ python3 update_modem.py mfw_nrf9160_1.2.3.zip /dev/ttyACM0 1000000
# modem firmware upgrade over serial port example started.
[Debug   ] [HighLevel ] dll_open
[Info    ] [HighLevel ] default_jlink_path parameter is NULL, latest JLINKARM DLL will be looked for and used.
[Debug   ] [HighLevel ] is_dll_open
[Debug   ] [HighLevel ] mcuboot_dfu_init
[Info    ] [HighLevel ] Creating new probe
[Info    ] [HighLevel ] initializing DFU
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] ModemUARTDFUProbe_initialize
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Dll directory is /home/ivo/.local/lib/python3.8/site-packages/pynrfjprog/lib_x64.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Find and connect to dfu dll
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Using DFU dll at /home/ivo/.local/lib/python3.8/site-packages/pynrfjprog/lib_x64/libnrfdfu.so.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Load library at /home/ivo/.local/lib/python3.8/site-packages/pynrfjprog/lib_x64/libnrfdfu.so.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Library loaded, loading member functions.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Member functions succesfully loaded.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Timeout set to 30000ms
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Initialize new probe.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] initialize
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Successfully opened port: /dev/ttyACM0@1000000,flow_control:none,parity:none.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(127): 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 127 bytes discarded
[Error   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got corrupt data.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:0 flags:0 len:14, group:2, seq:0, id: 0, total size: 36
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(39)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 400ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(38): 0x06 0x09 0x41 0x44 0x30 0x42 0x41 0x41 0x41 0x31 0x41 0x41 0x49 0x41 0x41 0x4c 0x39 0x69 0x63 0x6d 0x4d 0x41 0x5a 0x47 0x35 0x68 0x62 0x57 0x56 0x6e 0x63 0x32 0x31 0x77 0x58 0x32 0x4e 0x76
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x62 0x57 0x5a 0x6d 0x61 0x57 0x56 0x73 0x5a 0x48 0x4f 0x2f 0x61 0x57 0x5a 0x79 0x59 0x57
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(35): 0x31 0x6c 0x58 0x32 0x31 0x68 0x65 0x42 0x6b 0x43 0x41 0x47 0x68 0x77 0x59 0x57 0x4e 0x72 0x58 0x32 0x31 0x68 0x65 0x42 0x6b 0x42 0x2b 0x50 0x2f 0x2f 0x4c 0x34 0x30 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Found max frame length  512 and max package length 504
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Obtained connection parameters. Max frame size: 512, mtu: 504
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Have image upload chunk size of 276 (1st packet) and 328 (proceeding)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Using MTU 504 and frame size 512.
{
    "duration": 407, 
    "error_code": "Ok", 
    "operation": "open_uart", 
    "outcome": "success", 
    "progress_percentage": 100
}
[Info    ] [HighLevel ] Probe initialization complete!
[Debug   ] [HighLevel ] program
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] program
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] program_package
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Check if provided file exists
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Check if provided file can be read
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Unzipping package mfw_nrf9160_1.2.3.zip.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 13416, bytes from 72B3D7C.ipc_dfu.signed_1.1.0.ihex.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 456, bytes from firmware.update.image.digest.txt.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 6510, bytes from firmware.update.image.segments.0.hex.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 5622317, bytes from firmware.update.image.segments.1.hex.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 68782, bytes from mfw_nrf9160_1.2.3_release_notes.txt.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 15722, bytes from mfw_nrf9160_license-agreement.txt.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 219106, bytes from mfw_nrf9160_update_from_1.2.1_to_1.2.3.bin.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 35214, bytes from mfw_nrf9160_update_from_1.2.2_to_1.2.3.bin.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 14166, bytes from mfw_nrf9160_update_from_1.2.3-FOTA-TEST_to_1.2.3.bin.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 14166, bytes from mfw_nrf9160_update_from_1.2.3_to_1.2.3-FOTA-TEST.bin.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 726, bytes from README.txt.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] program files
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Programming bootloader
Programming modem bootloader.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Found bootloader file /tmp/fileA1kYrmnrfjprog/72B3D7C.ipc_dfu.signed_1.1.0.ihex.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] program_file
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Evaluating file /tmp/fileA1kYrmnrfjprog/72B3D7C.ipc_dfu.signed_1.1.0.ihex.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Check if provided file exists
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Check if provided file can be read
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Open provided file
{
    "duration": 0, 
    "message": "Calculating image size", 
    "operation": "upload_image", 
    "progress_percentage": 5
}
{
    "duration": 0, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 10
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 0, len: 276, out of total len 4752, target addr: 536870924
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:345, group:65, seq:1, id: 1, total size: 476
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(479)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x42 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x42 0x46 0x50 0x38 0x42 0x74 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 9ms. Current upload runtime is 0s
{
    "duration": 9, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 15
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 276, len: 328, out of total len 4752, target addr: 536871200
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:2, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x43 0x41 0x62 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x43 0x58 0x50 0x38 0x2f 0x70 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
{
    "duration": 20, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 21
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 604, len: 328, out of total len 4752, target addr: 536871528
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:3, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(8): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(14): 0x41 0x4e 0x41 0x45 0x45 0x44 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x44 0x70 0x50 0x38 0x38 0x41 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
{
    "duration": 31, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 27
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 932, len: 328, out of total len 4752, target addr: 536871856
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:4, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x45 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x39 0x6d 0x5a 0x68 0x6b 0x45 0x37 0x50 0x39 0x46 0x59 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
{
    "duration": 43, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 33
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1260, len: 328, out of total len 4752, target addr: 536872184
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:5, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x46 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x47 0x4e 0x50 0x38 0x5a 0x63 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
{
    "duration": 54, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 40
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1588, len: 328, out of total len 4752, target addr: 536872512
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:6, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x47 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x48 0x66 0x50 0x39 0x4a 0x41 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
{
    "duration": 65, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 46
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1916, len: 328, out of total len 4752, target addr: 536872840
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:7, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x48 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x49 0x78 0x50 0x39 0x63 0x61 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
{
    "duration": 76, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 52
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 2244, len: 328, out of total len 4752, target addr: 536873168
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:8, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(38): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x49 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4b 0x44 0x50 0x2f 0x79 0x4a 0x51 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
{
    "duration": 88, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 58
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 2572, len: 328, out of total len 4752, target addr: 536873496
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:9, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(37): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x4a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4c 0x56 0x50 0x2f 0x73 0x2f 0x77 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
{
    "duration": 99, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 64
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 2900, len: 328, out of total len 4752, target addr: 536873824
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:10, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x4b 0x41 0x62 0x39 0x69 0x63 0x6d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4d 0x6e 0x50 0x38 0x56 0x74 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
{
    "duration": 111, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 71
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 3228, len: 328, out of total len 4752, target addr: 536874152
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:11, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x4c 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4e 0x35 0x50 0x38 0x4e 0x69 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
{
    "duration": 123, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 77
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 3556, len: 328, out of total len 4752, target addr: 536874480
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:12, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x4d 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x50 0x4c 0x50 0x2b 0x45 0x67 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
{
    "duration": 134, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 83
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 3884, len: 328, out of total len 4752, target addr: 536874808
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:13, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x4e 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x51 0x64 0x50 0x2f 0x43 0x4f 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
{
    "duration": 145, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 89
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 4212, len: 328, out of total len 4752, target addr: 536875136
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:14, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(38): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x4f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x52 0x76 0x50 0x2b 0x4a 0x30 0x51 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
{
    "duration": 157, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 95
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 4540, len: 212, out of total len 4752, target addr: 536875464
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:237, group:65, seq:15, id: 1, total size: 332
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(335)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x50 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x53 0x6b 0x50 0x38 0x39 0x39 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 63ms. Current upload runtime is 0s
{
    "duration": 221, 
    "operation": "upload_image", 
    "outcome": "success", 
    "progress_percentage": 100
}
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Program bootloader SUCCESS
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Bootloader programmed
Programming file 1 of 2 files.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] program_file
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Evaluating file /tmp/fileA1kYrmnrfjprog/firmware.update.image.segments.0.hex.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Check if provided file exists
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Check if provided file can be read
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Open provided file
{
    "duration": 0, 
    "message": "Calculating image size", 
    "operation": "upload_image", 
    "progress_percentage": 5
}
{
    "duration": 0, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 10
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 0, len: 276, out of total len 2304, target addr: 1499471872
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:345, group:65, seq:16, id: 1, total size: 476
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(479)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(33): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x51 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x42 0x46 0x50 0x2f
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x68 0x77 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
{
    "duration": 11, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 20
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 276, len: 328, out of total len 2304, target addr: 1499472148
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:17, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x06 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(30): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x52 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x43 0x58 0x50 0x2b 0x53 0x43 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
{
    "duration": 23, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 33
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 604, len: 328, out of total len 2304, target addr: 1499472476
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:18, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x53 0x41 0x62 0x39 0x69
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x44 0x70 0x50 0x2f 0x63 0x64 0x51 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
{
    "duration": 35, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 46
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 932, len: 328, out of total len 2304, target addr: 1499472804
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:19, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(16): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x54 0x41 0x62
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(23): 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x45 0x37 0x50 0x39 0x7a 0x66 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
{
    "duration": 47, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 59
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1260, len: 328, out of total len 2304, target addr: 1499473132
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:20, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x55 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x47 0x4e 0x50 0x2f 0x35 0x42 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
{
    "duration": 58, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 72
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1588, len: 328, out of total len 2304, target addr: 1499473460
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:21, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(16): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x56 0x41 0x62
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(23): 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x48 0x66 0x50 0x2f 0x6b 0x72 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
{
    "duration": 70, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 84
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1916, len: 328, out of total len 2304, target addr: 1499473788
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:22, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(32): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x57 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x49 0x78 0x50
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x2b 0x38 0x48 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
{
    "duration": 81, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 97
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 2244, len: 60, out of total len 2304, target addr: 1499474116
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:85, group:65, seq:23, id: 1, total size: 132
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(135)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(33): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x58 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4a 0x41 0x50 0x2f
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x2f 0x51 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 6ms. Current upload runtime is 0s
{
    "duration": 88, 
    "operation": "upload_image", 
    "outcome": "success", 
    "progress_percentage": 100
}
Finished with file.
Programming file 2 of 2 files.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] program_file
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Evaluating file /tmp/fileA1kYrmnrfjprog/firmware.update.image.segments.1.hex.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Check if provided file exists
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Check if provided file can be read
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Open provided file
{
    "duration": 0, 
    "message": "Calculating image size", 
    "operation": "upload_image", 
    "progress_percentage": 5
}
{
    "duration": 0, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 10
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 0, len: 276, out of total len 1998848, target addr: 24576
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:345, group:65, seq:24, id: 1, total size: 476
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(479)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(26): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x59 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(13): 0x5a 0x68 0x6b 0x42 0x46 0x50 0x2f 0x47 0x68 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 9ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 276, len: 328, out of total len 1998848, target addr: 24852
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:25, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x5a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x39 0x6d 0x5a 0x68 0x6b 0x43 0x58 0x50 0x2b 0x31 0x54 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 604, len: 328, out of total len 1998848, target addr: 25180
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:26, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(12): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x45 0x61 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(9): 0x70 0x50 0x2f 0x37 0x4d 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 932, len: 328, out of total len 1998848, target addr: 25508
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:27, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x62 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x45 0x37 0x50 0x39 0x55 0x4f 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1260, len: 328, out of total len 1998848, target addr: 25836
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:28, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x63 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x39 0x6d 0x5a 0x68 0x6b 0x47 0x4e 0x50 0x2f 0x65 0x51 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1588, len: 328, out of total len 1998848, target addr: 26164
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:29, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x64 0x41 0x62 0x39 0x69 0x63 0x6d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x48 0x66 0x50 0x2f 0x44 0x36 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1916, len: 328, out of total len 1998848, target addr: 26492
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:30, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(34): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x65 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x49 0x78 0x50 0x2b 0x62
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x57 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 2244, len: 328, out of total len 1998848, target addr: 26820
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:31, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(36): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x66 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4b 0x44 0x50 0x2f 0x45 0x4f 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 2572, len: 328, out of total len 1998848, target addr: 27148
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:32, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x67 0x41 0x62 0x39 0x69 0x63 0x6d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4c 0x56 0x50 0x2f 0x34 0x55 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 2900, len: 328, out of total len 1998848, target addr: 27476
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:33, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(37): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x68 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4d 0x6e 0x50 0x39 0x4d 0x77 0x77 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 3228, len: 328, out of total len 1998848, target addr: 27804
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:34, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(23): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x69 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(16): 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4e 0x35 0x50 0x38 0x5a 0x4a 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 3556, len: 328, out of total len 1998848, target addr: 28132
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:35, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x6a 0x41 0x62 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x50 0x4c 0x50 0x39 0x47 0x52 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 3884, len: 328, out of total len 1998848, target addr: 28460
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:36, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(27): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x6b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(12): 0x68 0x6b 0x51 0x64 0x50 0x2f 0x57 0x6c 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 4212, len: 328, out of total len 1998848, target addr: 28788
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:37, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x6c 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x52 0x76 0x50 0x2f 0x51 0x70 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 4540, len: 328, out of total len 1998848, target addr: 29116
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:38, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x6d 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x54 0x42 0x50 0x2f 0x4b 0x52 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 4868, len: 328, out of total len 1998848, target addr: 29444
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:39, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x6e 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x55 0x54 0x50 0x39 0x6c 0x54 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 5196, len: 328, out of total len 1998848, target addr: 29772
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:40, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x6f 0x41 0x62 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x56 0x6c 0x50 0x2b 0x52 0x49 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 5524, len: 328, out of total len 1998848, target addr: 30100
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:41, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(38): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x70 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x57 0x33 0x50 0x2f 0x69 0x36 0x41 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 5852, len: 328, out of total len 1998848, target addr: 30428
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:42, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(35): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x71 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x59 0x4a 0x50 0x2b 0x41 0x70
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 6180, len: 328, out of total len 1998848, target addr: 30756
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:43, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x72 0x41 0x62 0x39 0x69 0x63
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x5a 0x62 0x50 0x2b 0x64 0x44 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 6508, len: 328, out of total len 1998848, target addr: 31084
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:44, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x73 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x61 0x74 0x50 0x38 0x67 0x52 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 6836, len: 328, out of total len 1998848, target addr: 31412
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:45, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x74 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x62 0x2f 0x50 0x38 0x39 0x37 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 7164, len: 328, out of total len 1998848, target addr: 31740
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:46, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x75 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x64 0x52 0x50 0x2f 0x37 0x7a 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 7492, len: 328, out of total len 1998848, target addr: 32068
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:47, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x76 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x65 0x6a 0x50 0x2b 0x54 0x6e 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 7820, len: 328, out of total len 1998848, target addr: 32396
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:48, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x77 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x66 0x31 0x50 0x38 0x79 0x34 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 8148, len: 328, out of total len 1998848, target addr: 32724
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:49, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(36): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x78 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x68 0x48 0x50 0x2f 0x64 0x52 0x67
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 156ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 8476, len: 328, out of total len 1998848, target addr: 33052
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:50, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(38): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x79 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x69 0x5a 0x50 0x2f 0x6d 0x77 0x77 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 8804, len: 328, out of total len 1998848, target addr: 33380
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:51, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(30): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x7a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x6a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(9): 0x72 0x50 0x2f 0x67 0x38 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 9132, len: 328, out of total len 1998848, target addr: 33708
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:52, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(35): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x30 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x6b 0x39 0x50 0x2b 0x61 0x34
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 9460, len: 328, out of total len 1998848, target addr: 34036
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:53, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x31 0x41 0x62 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x6d 0x50 0x50 0x2f 0x46 0x67 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 9788, len: 328, out of total len 1998848, target addr: 34364
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:54, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(26): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x32 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(13): 0x5a 0x68 0x6b 0x6e 0x68 0x50 0x2b 0x47 0x4d 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 10116, len: 328, out of total len 1998848, target addr: 34692
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:55, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(36): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x33 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x6f 0x7a 0x50 0x2b 0x41 0x6d 0x77
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 10444, len: 328, out of total len 1998848, target addr: 35020
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:56, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(11): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(28): 0x45 0x45 0x34 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x71 0x46 0x50 0x38 0x74 0x70 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 10772, len: 328, out of total len 1998848, target addr: 35348
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:57, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x35 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x72 0x58 0x50 0x38 0x77 0x44 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 11100, len: 328, out of total len 1998848, target addr: 35676
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:58, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x36 0x41 0x62 0x39 0x69
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x73 0x70 0x50 0x2f 0x4d 0x30 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 11428, len: 328, out of total len 1998848, target addr: 36004
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:59, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(12): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x45 0x37 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x74 0x37 0x50 0x2f
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x52 0x65 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 11756, len: 328, out of total len 1998848, target addr: 36332
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:60, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(34): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x38 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x76 0x4e 0x50 0x39 0x62
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x41 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 12084, len: 328, out of total len 1998848, target addr: 36660
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:61, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(16): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x39 0x41 0x62
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x77 0x66 0x50 0x38 0x65 0x79 0x41 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 12412, len: 328, out of total len 1998848, target addr: 36988
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:62, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(10): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(26): 0x41 0x45 0x45 0x2b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x78 0x78 0x50 0x39 0x64 0x65 0x51
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 12740, len: 328, out of total len 1998848, target addr: 37316
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:63, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(36): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x2f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x7a 0x44 0x50 0x38 0x43 0x47 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 13068, len: 328, out of total len 1998848, target addr: 37644
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:64, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x41 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x30 0x56 0x50 0x2b 0x6d 0x32 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 13396, len: 328, out of total len 1998848, target addr: 37972
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:65, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x42 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x31 0x6e 0x50 0x2b 0x67 0x36 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 13724, len: 328, out of total len 1998848, target addr: 38300
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:66, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x43 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x32 0x35 0x50 0x2b 0x62 0x62 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 14052, len: 328, out of total len 1998848, target addr: 38628
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:67, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(11): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(28): 0x45 0x46 0x44 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x34 0x4c 0x50 0x2b 0x78 0x62 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 14380, len: 328, out of total len 1998848, target addr: 38956
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:68, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(31): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x45 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x35 0x64
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(8): 0x50 0x39 0x35 0x33 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 14708, len: 328, out of total len 1998848, target addr: 39284
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:69, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x46 0x41 0x62 0x39 0x69 0x63
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x36 0x76 0x50 0x38 0x52 0x6a 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 15036, len: 328, out of total len 1998848, target addr: 39612
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:70, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x47 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x38 0x42 0x50 0x2f 0x58 0x72 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 15364, len: 328, out of total len 1998848, target addr: 39940
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:71, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x48 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x39 0x54 0x50 0x2f 0x4b 0x42 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 15692, len: 328, out of total len 1998848, target addr: 40268
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:72, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x49 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x2b 0x6c 0x50 0x39 0x51 0x43 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 16020, len: 328, out of total len 1998848, target addr: 40596
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:73, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(38): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x4a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x2f 0x33 0x50 0x39 0x4e 0x6f 0x67 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 16348, len: 328, out of total len 1998848, target addr: 40924
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:74, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(25): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x4b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(14): 0x6d 0x5a 0x68 0x6c 0x42 0x4a 0x50 0x2f 0x33 0x35 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 129ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 16676, len: 328, out of total len 1998848, target addr: 41252
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:75, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x4c 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x43 0x62 0x50 0x2b 0x45 0x4c 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 17004, len: 328, out of total len 1998848, target addr: 41580
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:76, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x4d 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x44 0x74 0x50 0x39 0x58 0x42 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 17332, len: 328, out of total len 1998848, target addr: 41908
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:77, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x4e 0x41 0x62 0x39 0x69 0x63 0x6d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x45 0x2f 0x50 0x2f 0x34 0x44 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 17660, len: 328, out of total len 1998848, target addr: 42236
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:78, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x06 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(29): 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x4f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x47 0x52 0x50 0x2f 0x69 0x37
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 17988, len: 328, out of total len 1998848, target addr: 42564
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:79, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(38): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x50 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x48 0x6a 0x50 0x2f 0x6b 0x33 0x77 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 18316, len: 328, out of total len 1998848, target addr: 42892
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:80, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(16): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x51 0x41 0x62
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(23): 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x49 0x31 0x50 0x39 0x65 0x6f 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 18644, len: 328, out of total len 1998848, target addr: 43220
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:81, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x52 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x4b 0x48 0x50 0x38 0x42 0x77 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 18972, len: 328, out of total len 1998848, target addr: 43548
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:82, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x53 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x4c 0x5a 0x50 0x39 0x55 0x4a 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 19300, len: 328, out of total len 1998848, target addr: 43876
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:83, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x54 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x4d 0x72 0x50 0x2f 0x67 0x74 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 19628, len: 328, out of total len 1998848, target addr: 44204
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:84, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x55 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x4e 0x39 0x50 0x38 0x6f 0x42 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 19956, len: 328, out of total len 1998848, target addr: 44532
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:85, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x06 0x09 0x41 0x42 0x55
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x56 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(14): 0x6d 0x5a 0x68 0x6c 0x50 0x50 0x50 0x39 0x33 0x5a 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 20284, len: 328, out of total len 1998848, target addr: 44860
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:86, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(8): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x41 0x4e 0x41 0x45 0x46 0x57 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x51 0x68 0x50
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x39 0x73 0x74 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 20612, len: 328, out of total len 1998848, target addr: 45188
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:87, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x58 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x52 0x7a 0x50 0x39 0x78 0x48 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 20940, len: 328, out of total len 1998848, target addr: 45516
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:88, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x59 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x54 0x46 0x50 0x2f 0x63 0x49 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 21268, len: 328, out of total len 1998848, target addr: 45844
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:89, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x5a 0x41 0x62 0x39 0x69 0x63
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x55 0x58 0x50 0x39 0x7a 0x4b 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 21596, len: 328, out of total len 1998848, target addr: 46172
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:90, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(38): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x61 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x56 0x70 0x50 0x38 0x39 0x56 0x77 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 21924, len: 328, out of total len 1998848, target addr: 46500
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:91, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x62 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x57 0x37 0x50 0x39 0x4f 0x6e 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
{
    "duration": 1030, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 11
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 22252, len: 328, out of total len 1998848, target addr: 46828
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:92, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(35): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x63 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x59 0x4e 0x50 0x2b 0x78 0x68
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 22580, len: 328, out of total len 1998848, target addr: 47156
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:93, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(12): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(27): 0x46 0x64 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x5a 0x66 0x50 0x2b 0x73 0x4c 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 22908, len: 328, out of total len 1998848, target addr: 47484
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:94, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x65 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x61 0x78 0x50 0x2b 0x42 0x2f 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 23236, len: 328, out of total len 1998848, target addr: 47812
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:95, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(38): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x66 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x63 0x44 0x50 0x38 0x43 0x58 0x77 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 23564, len: 328, out of total len 1998848, target addr: 48140
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:96, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(9): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(30): 0x4e 0x41 0x45 0x46 0x67 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x64 0x56 0x50 0x38 0x2b 0x4e 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 23892, len: 328, out of total len 1998848, target addr: 48468
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:97, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(16): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x68 0x41 0x62
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(23): 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x65 0x6e 0x50 0x39 0x57 0x5a 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 24220, len: 328, out of total len 1998848, target addr: 48796
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:98, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(32): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x69 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x66 0x35 0x50
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x38 0x44 0x67 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 24548, len: 328, out of total len 1998848, target addr: 49124
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:99, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x6a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x68 0x4c 0x50 0x2f 0x73 0x4a 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 32ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 24876, len: 328, out of total len 1998848, target addr: 49452
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:100, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x6b 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x69 0x64 0x50 0x39 0x4b 0x39 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 25204, len: 328, out of total len 1998848, target addr: 49780
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:101, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x06 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x6c 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(14): 0x6d 0x5a 0x68 0x6c 0x6a 0x76 0x50 0x39 0x4d 0x78 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 25532, len: 328, out of total len 1998848, target addr: 50108
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:102, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x6d 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x6c 0x42 0x50 0x2b 0x4b 0x35 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 25860, len: 328, out of total len 1998848, target addr: 50436
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:103, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x6e 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x6d 0x54 0x50 0x2f 0x35 0x4c 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 26188, len: 328, out of total len 1998848, target addr: 50764
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:104, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(38): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x6f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x6e 0x6c 0x50 0x38 0x4e 0x51 0x41 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 26516, len: 328, out of total len 1998848, target addr: 51092
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:105, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x70 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x6f 0x33 0x50 0x38 0x4c 0x36 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 26844, len: 328, out of total len 1998848, target addr: 51420
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:106, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x06 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(26): 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x71 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x71 0x4a 0x50
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x38 0x63 0x78 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 27172, len: 328, out of total len 1998848, target addr: 51748
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:107, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x72 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x72 0x62 0x50 0x38 0x42 0x62 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 27500, len: 328, out of total len 1998848, target addr: 52076
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:108, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(37): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x73 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x73 0x74 0x50 0x39 0x67 0x35 0x51 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 27828, len: 328, out of total len 1998848, target addr: 52404
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:109, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x06 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(26): 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x74 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x74 0x2f 0x50
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x39 0x39 0x54 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 28156, len: 328, out of total len 1998848, target addr: 52732
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:110, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x75 0x41 0x62 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x76 0x52 0x50 0x39 0x6e 0x72 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 28484, len: 328, out of total len 1998848, target addr: 53060
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:111, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(13): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(26): 0x76 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x77 0x6a 0x50 0x38 0x35 0x2f 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 28812, len: 328, out of total len 1998848, target addr: 53388
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:112, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(38): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x77 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x78 0x31 0x50 0x2b 0x59 0x67 0x41 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 29140, len: 328, out of total len 1998848, target addr: 53716
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:113, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x78 0x41 0x62 0x39 0x69 0x63 0x6d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x7a 0x48 0x50 0x2f 0x48 0x34 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 29468, len: 328, out of total len 1998848, target addr: 54044
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:114, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(37): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x79 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x30 0x5a 0x50 0x38 0x67 0x70 0x41 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 29796, len: 328, out of total len 1998848, target addr: 54372
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:115, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(14): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x7a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(25): 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x31 0x72 0x50 0x38 0x6d 0x6c 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 30124, len: 328, out of total len 1998848, target addr: 54700
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:116, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(38): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x30 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x32 0x39 0x50 0x2b 0x41 0x52 0x41 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 30452, len: 328, out of total len 1998848, target addr: 55028
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:117, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(23): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x31 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(16): 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x34 0x50 0x50 0x2b 0x71 0x52 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 30780, len: 328, out of total len 1998848, target addr: 55356
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:118, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x06 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(31): 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x32 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x35 0x68 0x50 0x2f 0x70 0x39 0x51 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 31108, len: 328, out of total len 1998848, target addr: 55684
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:119, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x33 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x36 0x7a 0x50 0x2b 0x61 0x50 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 31436, len: 328, out of total len 1998848, target addr: 56012
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:120, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(37): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x34 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x38 0x46 0x50 0x2f 0x72 0x77 0x41 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 31764, len: 328, out of total len 1998848, target addr: 56340
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:121, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x35 0x41 0x62 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x39 0x58 0x50 0x2f 0x32 0x61 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 32092, len: 328, out of total len 1998848, target addr: 56668
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:122, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(33): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x36 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x2b 0x70 0x50 0x2f
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x57 0x64 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 32420, len: 328, out of total len 1998848, target addr: 56996
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:123, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x37 0x41 0x62 0x39 0x69 0x63
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x2f 0x37 0x50 0x2f 0x4c 0x33 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 32748, len: 328, out of total len 1998848, target addr: 57324
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:124, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x38 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x42 0x4e 0x50 0x2f 0x58 0x6c 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 32ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 33076, len: 328, out of total len 1998848, target addr: 57652
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:125, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(16): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x39 0x41 0x62
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(23): 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x43 0x66 0x50 0x2b 0x6b 0x58 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 33404, len: 328, out of total len 1998848, target addr: 57980
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:126, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(35): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x2b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x44 0x78 0x50 0x2f 0x6e 0x37
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 33732, len: 328, out of total len 1998848, target addr: 58308
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:127, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(16): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x2f 0x41 0x62
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(23): 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x46 0x44 0x50 0x39 0x6b 0x54 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 34060, len: 328, out of total len 1998848, target addr: 58636
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:128, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x41 0x41 0x62 0x39 0x69
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x47 0x56 0x50 0x39 0x49 0x58 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 34388, len: 328, out of total len 1998848, target addr: 58964
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:129, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(28): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x42 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(11): 0x6d 0x48 0x6e 0x50 0x39 0x4f 0x62 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 34716, len: 328, out of total len 1998848, target addr: 59292
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:130, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(35): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x43 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x49 0x35 0x50 0x38 0x41 0x69
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 35044, len: 328, out of total len 1998848, target addr: 59620
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:131, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x44 0x41 0x62 0x39 0x69
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x4b 0x4c 0x50 0x39 0x66 0x36 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 35372, len: 328, out of total len 1998848, target addr: 59948
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:132, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(32): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x45 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x4c 0x64 0x50
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x2b 0x58 0x57 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 35700, len: 328, out of total len 1998848, target addr: 60276
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:133, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x06 0x09 0x41 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(23): 0x41 0x41 0x4e 0x41 0x45 0x47 0x46 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(9): 0x76 0x50 0x38 0x6a 0x79 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 36028, len: 328, out of total len 1998848, target addr: 60604
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:134, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(31): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x47 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x4f 0x42
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(8): 0x50 0x38 0x35 0x4b 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 36356, len: 328, out of total len 1998848, target addr: 60932
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:135, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x48 0x41 0x62 0x39 0x69 0x63
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x50 0x54 0x50 0x38 0x6b 0x67 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 36684, len: 328, out of total len 1998848, target addr: 61260
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:136, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(36): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x49 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x51 0x6c 0x50 0x2b 0x49 0x6a 0x51
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 37012, len: 328, out of total len 1998848, target addr: 61588
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:137, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x4a 0x41 0x62 0x39 0x69
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x52 0x33 0x50 0x2b 0x56 0x4a 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 37340, len: 328, out of total len 1998848, target addr: 61916
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:138, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x4b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x54 0x4a 0x50 0x2b 0x43 0x43 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 37668, len: 328, out of total len 1998848, target addr: 62244
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:139, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(32): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x4c 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x55 0x62 0x50
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x38 0x74 0x41 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 37996, len: 328, out of total len 1998848, target addr: 62572
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:140, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x4d 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x56 0x74 0x50 0x2f 0x2b 0x4b 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 38324, len: 328, out of total len 1998848, target addr: 62900
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:141, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(34): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x4e 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x57 0x2f 0x50 0x2b 0x4e
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x34 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 38652, len: 328, out of total len 1998848, target addr: 63228
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:142, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(10): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(29): 0x41 0x45 0x47 0x4f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x59 0x52 0x50 0x2f 0x69 0x59 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 38980, len: 328, out of total len 1998848, target addr: 63556
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:143, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x50 0x41 0x62 0x39 0x69 0x63
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x5a 0x6a 0x50 0x2f 0x6b 0x55 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 39308, len: 328, out of total len 1998848, target addr: 63884
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:144, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x06 0x09 0x41 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(29): 0x41 0x41 0x4e 0x41 0x45 0x47 0x51 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x61 0x31 0x50 0x38 0x72 0x54 0x77
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 39636, len: 328, out of total len 1998848, target addr: 64212
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:145, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x52 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x63 0x48 0x50 0x2b 0x6f 0x37 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 39964, len: 328, out of total len 1998848, target addr: 64540
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:146, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(38): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x53 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x64 0x5a 0x50 0x2f 0x39 0x43 0x77 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 40292, len: 328, out of total len 1998848, target addr: 64868
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:147, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(14): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x54
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(25): 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x65 0x72 0x50 0x2b 0x56 0x57 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 40620, len: 328, out of total len 1998848, target addr: 65196
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:148, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(10): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(27): 0x41 0x45 0x47 0x55 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x66 0x39 0x50 0x39 0x64 0x36 0x77 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 40948, len: 12, out of total len 1998848, target addr: 65524
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:34, group:65, seq:149, id: 1, total size: 64
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(67)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x56 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x67 0x41 0x50 0x2f 0x46 0x68 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 25ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 40960, len: 328, out of total len 1998848, target addr: 327680
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:150, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(26): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x57 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(13): 0x5a 0x68 0x6d 0x68 0x53 0x50 0x2b 0x56 0x39 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 41288, len: 328, out of total len 1998848, target addr: 328008
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:151, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x58 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x69 0x6b 0x50 0x2f 0x2b 0x31 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 41616, len: 328, out of total len 1998848, target addr: 328336
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:152, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x06 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(32): 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x59 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x6a 0x32 0x50 0x38 0x53 0x55 0x77 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 41944, len: 328, out of total len 1998848, target addr: 328664
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:153, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(25): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x5a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(14): 0x6d 0x5a 0x68 0x6d 0x6c 0x49 0x50 0x2b 0x55 0x5a 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 42272, len: 328, out of total len 1998848, target addr: 328992
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:154, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x61 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x6d 0x61 0x50 0x2b 0x71 0x64 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 42600, len: 328, out of total len 1998848, target addr: 329320
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:155, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x62 0x41 0x62 0x39 0x69
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x6e 0x73 0x50 0x2b 0x76 0x4e 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 42928, len: 328, out of total len 1998848, target addr: 329648
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:156, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x63 0x41 0x62 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x6f 0x2b 0x50 0x39 0x2f 0x39 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 43256, len: 328, out of total len 1998848, target addr: 329976
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:157, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x06 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x64 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(12): 0x68 0x6d 0x71 0x51 0x50 0x38 0x6f 0x7a 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 43584, len: 328, out of total len 1998848, target addr: 330304
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:158, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(10): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(29): 0x41 0x45 0x47 0x65 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x72 0x69 0x50 0x39 0x6a 0x4a 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 43912, len: 328, out of total len 1998848, target addr: 330632
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:159, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(38): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x66 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x73 0x30 0x50 0x2f 0x50 0x58 0x41 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 44240, len: 328, out of total len 1998848, target addr: 330960
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:160, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(32): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x67 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x75 0x47 0x50
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x2b 0x79 0x6a 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
{
    "duration": 1872, 
    "message": "Uploading image to device", 
    "operation": "upload_image", 
    "progress_percentage": 12
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 44568, len: 328, out of total len 1998848, target addr: 331288
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:161, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x68 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x76 0x59 0x50 0x2b 0x71 0x73 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 44896, len: 328, out of total len 1998848, target addr: 331616
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:162, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x69 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x77 0x71 0x50 0x2b 0x35 0x4f 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 45224, len: 328, out of total len 1998848, target addr: 331944
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:163, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(31): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x6a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x78 0x38
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(8): 0x50 0x2b 0x6e 0x34 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 45552, len: 328, out of total len 1998848, target addr: 332272
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:164, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x06 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(27): 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x6b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x7a 0x4f 0x50 0x38
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x75 0x36 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 45880, len: 328, out of total len 1998848, target addr: 332600
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:165, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(27): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x6c 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(12): 0x68 0x6d 0x30 0x67 0x50 0x2b 0x53 0x49 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 46208, len: 328, out of total len 1998848, target addr: 332928
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:166, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x6d 0x41 0x62 0x39 0x69 0x63 0x6d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x31 0x79 0x50 0x2f 0x43 0x55 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 46536, len: 328, out of total len 1998848, target addr: 333256
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:167, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x6e 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x33 0x45 0x50 0x2b 0x65 0x51 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 46864, len: 328, out of total len 1998848, target addr: 333584
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:168, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x6f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x34 0x57 0x50 0x39 0x70 0x78 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 47192, len: 328, out of total len 1998848, target addr: 333912
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:169, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x70 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x35 0x6f 0x50 0x39 0x71 0x59 0x77 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 47520, len: 328, out of total len 1998848, target addr: 334240
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:170, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(13): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x71 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x36 0x36 0x50 0x39 0x55 0x63 0x77 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 47848, len: 328, out of total len 1998848, target addr: 334568
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:171, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x72 0x41 0x62 0x39 0x69 0x63 0x6d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x38 0x4d 0x50 0x2f 0x55 0x6f 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 48176, len: 328, out of total len 1998848, target addr: 334896
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:172, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x73 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x39 0x65 0x50 0x38 0x66 0x59 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 48504, len: 328, out of total len 1998848, target addr: 335224
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:173, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x74 0x41 0x62 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6d 0x2b 0x77 0x50 0x39 0x2f 0x61 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 48832, len: 328, out of total len 1998848, target addr: 335552
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:174, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x75 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x41 0x43 0x50 0x2f 0x41 0x75 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 128ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 49160, len: 328, out of total len 1998848, target addr: 335880
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:175, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x06 0x09 0x41 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x41 0x41 0x4e 0x41 0x45 0x47 0x76 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x39 0x6d 0x5a 0x68 0x6e 0x42 0x55 0x50 0x2f 0x65 0x59 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 49488, len: 328, out of total len 1998848, target addr: 336208
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:176, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x77 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x39 0x6d 0x5a 0x68 0x6e 0x43 0x6d 0x50 0x38 0x4a 0x6c 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 49816, len: 328, out of total len 1998848, target addr: 336536
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:177, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x78 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x44 0x34 0x50 0x38 0x52 0x71 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 50144, len: 328, out of total len 1998848, target addr: 336864
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:178, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(13): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x79 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x46 0x4b 0x50
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x2f 0x66 0x30 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 50472, len: 328, out of total len 1998848, target addr: 337192
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:179, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(25): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x7a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(14): 0x6d 0x5a 0x68 0x6e 0x47 0x63 0x50 0x2b 0x76 0x61 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 50800, len: 328, out of total len 1998848, target addr: 337520
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:180, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(33): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x30 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x48 0x75 0x50 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x2f 0x4d 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 51128, len: 328, out of total len 1998848, target addr: 337848
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:181, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x31 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x4a 0x41 0x50 0x39 0x64 0x61 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 51456, len: 328, out of total len 1998848, target addr: 338176
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:182, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x32 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x4b 0x53 0x50 0x39 0x6a 0x65 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 51784, len: 328, out of total len 1998848, target addr: 338504
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:183, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x33 0x41 0x62 0x39 0x69
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x4c 0x6b 0x50 0x39 0x6d 0x4f 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 52112, len: 328, out of total len 1998848, target addr: 338832
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:184, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x34 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x4d 0x32 0x50 0x38 0x34 0x48 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 52440, len: 328, out of total len 1998848, target addr: 339160
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:185, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x35 0x41 0x62 0x39 0x69 0x63 0x6d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x4f 0x49 0x50 0x39 0x69 0x36 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 52768, len: 328, out of total len 1998848, target addr: 339488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:186, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(38): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x36 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x50 0x61 0x50 0x38 0x79 0x6d 0x51 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 53096, len: 328, out of total len 1998848, target addr: 339816
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:187, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x37 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x51 0x73 0x50 0x39 0x76 0x75 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 53424, len: 328, out of total len 1998848, target addr: 340144
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:188, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(30): 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x38 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x52 0x2b 0x50 0x2b
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x6b 0x65 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 53752, len: 328, out of total len 1998848, target addr: 340472
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:189, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x39 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x54 0x51 0x50 0x2f 0x7a 0x51 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 54080, len: 328, out of total len 1998848, target addr: 340800
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:190, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x2b 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x55 0x69 0x50 0x38 0x4b 0x43 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 54408, len: 328, out of total len 1998848, target addr: 341128
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:191, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(38): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x47 0x2f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x56 0x30 0x50 0x38 0x55 0x30 0x51 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 54736, len: 328, out of total len 1998848, target addr: 341456
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:192, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(28): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x41 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(11): 0x6e 0x58 0x47 0x50 0x39 0x44 0x43 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 55064, len: 328, out of total len 1998848, target addr: 341784
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:193, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x42 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x59 0x59 0x50 0x39 0x41 0x4e 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 55392, len: 328, out of total len 1998848, target addr: 342112
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:194, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(32): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x43 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x5a 0x71 0x50
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x38 0x4c 0x33 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 55720, len: 328, out of total len 1998848, target addr: 342440
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:195, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x44 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x39 0x6d 0x5a 0x68 0x6e 0x61 0x38 0x50 0x39 0x37 0x5a 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 56048, len: 328, out of total len 1998848, target addr: 342768
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:196, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(10): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(28): 0x41 0x45 0x48 0x45 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x63 0x4f 0x50 0x38 0x75 0x72 0x41 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 56376, len: 328, out of total len 1998848, target addr: 343096
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:197, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x06 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(29): 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x46 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x64 0x67 0x50 0x38 0x67 0x78
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 56704, len: 328, out of total len 1998848, target addr: 343424
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:198, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(13): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(26): 0x47 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x65 0x79 0x50 0x38 0x65 0x31 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 57032, len: 328, out of total len 1998848, target addr: 343752
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:199, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x48 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x67 0x45 0x50 0x2f 0x79 0x41 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 129ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 57360, len: 328, out of total len 1998848, target addr: 344080
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:200, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x06 0x09 0x41 0x42 0x55
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x49 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(10): 0x68 0x57 0x50 0x38 0x65 0x68 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 57688, len: 328, out of total len 1998848, target addr: 344408
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:201, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x4a 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x69 0x6f 0x50 0x39 0x7a 0x51 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 58016, len: 328, out of total len 1998848, target addr: 344736
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:202, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x4b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x6a 0x36 0x50 0x38 0x6a 0x4d 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 58344, len: 328, out of total len 1998848, target addr: 345064
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:203, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x4c 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x6c 0x4d 0x50 0x2b 0x6a 0x34 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 58672, len: 328, out of total len 1998848, target addr: 345392
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:204, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(33): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x4d 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x6d 0x65 0x50 0x38
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x47 0x51 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 59000, len: 328, out of total len 1998848, target addr: 345720
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:205, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x4e 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x6e 0x77 0x50 0x38 0x49 0x4b 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 59328, len: 328, out of total len 1998848, target addr: 346048
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:206, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x06 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(29): 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x4f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x70 0x43 0x50 0x39 0x76 0x38
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 59656, len: 328, out of total len 1998848, target addr: 346376
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:207, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x50 0x41 0x62 0x39 0x69 0x63 0x6d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x71 0x55 0x50 0x38 0x66 0x53 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 59984, len: 328, out of total len 1998848, target addr: 346704
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:208, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x51 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x72 0x6d 0x50 0x2b 0x6d 0x33 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 60312, len: 328, out of total len 1998848, target addr: 347032
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:209, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(35): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x52 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x73 0x34 0x50 0x38 0x4d 0x51
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 60640, len: 328, out of total len 1998848, target addr: 347360
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:210, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x53 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x75 0x4b 0x50 0x38 0x65 0x2b 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 60968, len: 328, out of total len 1998848, target addr: 347688
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:211, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(16): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x54 0x41 0x62
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(23): 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x76 0x63 0x50 0x38 0x41 0x49 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 61296, len: 328, out of total len 1998848, target addr: 348016
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:212, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x55 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x77 0x75 0x50 0x2b 0x49 0x47 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 61624, len: 328, out of total len 1998848, target addr: 348344
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:213, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x56 0x41 0x62 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x79 0x41 0x50 0x2f 0x66 0x49 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 61952, len: 328, out of total len 1998848, target addr: 348672
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:214, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x57 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x7a 0x53 0x50 0x2b 0x50 0x55 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 62280, len: 328, out of total len 1998848, target addr: 349000
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:215, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(39): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x58 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x30 0x6b 0x50 0x38 0x34 0x73 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 10ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 62608, len: 328, out of total len 1998848, target addr: 349328
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:216, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x06 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x48 0x59 0x41 0x62 0x39 0x69 0x63 0x6d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6e 0x31 0x32 0x50 0x2f 0x55 0x4e 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 11ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 62936, len: 328, out of total len 1998848, target addr: 349656
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:217, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] No time left to wait for data. Timeout
{
    "duration": 32743, 
    "error_code": "Timeout", 
    "message": "Image upload failed. Bad response from device", 
    "operation": "upload_image", 
    "outcome": "fail", 
    "progress_percentage": 100
}
[Error   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Error during image file upload. Upload returned an error.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Failed programming file /tmp/fileA1kYrmnrfjprog/firmware.update.image.segments.1.hex.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Failed while programming files to target.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Failed to program DFU package
[Info    ] [HighLevel ] Failed programming the device.
b'An error was reported by NRFJPROG DLL: -220 TIME_OUT.'
[Debug   ] [HighLevel ] is_dll_open
[Debug   ] [HighLevel ] probe_uninit
[Info    ] [HighLevel ] Deleting probe at location 0x2339900
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] readDeviceInfo
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uninitializing ModemUARTDFU probe at serial port /dev/ttyACM0.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] uninitialize
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Sending device reset request
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Sending reset request to device.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(23)
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Closing connection to mcuboot device
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] serial port read on port /dev/ttyACM0 aborted
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] serial io_context executed 441 handlers.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] serial port /dev/ttyACM0 closed.
{
    "duration": 1, 
    "error_code": "Ok", 
    "operation": "close_uart", 
    "outcome": "success", 
    "progress_percentage": 100
}
[Info    ] [HighLevel ] Done.
[Debug   ] [HighLevel ] dll_close
[Info    ] [HighLevel ] closing and freeing sub dlls.
Traceback (most recent call last):
  File "update_modem.py", line 43, in <module>
    run(args.uart, args.firmware, args.baudrate)
  File "update_modem.py", line 26, in run
    modem_dfu_probe.program(modem_firmware_zip)
  File "/home/ivo/.local/lib/python3.8/site-packages/pynrfjprog/HighLevel.py", line 350, in program
    raise APIError(result, log=self._logger.error)
pynrfjprog.APIError.APIError: An error was reported by NRFJPROG DLL: -220 TIME_OUT.
ivo@system76-pc:~/src/nrf91-1.5.0/ncs/nrf/samples/nrf9160/fmfu_smp_svr$
