[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x43 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x41 0x2b 0x6f 0x2f 0x39 0x33 0x6c 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 127s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 790440, len: 328, out of total len 2023424, target addr: 1077160
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:131, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x44 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x42 0x44 0x77 0x2f 0x79 0x56 0x44 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 127s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 790768, len: 328, out of total len 2023424, target addr: 1077488
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:132, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x45 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x42 0x49 0x34 0x2f 0x36 0x5a 0x77 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 32ms. Current upload runtime is 127s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 791096, len: 328, out of total len 2023424, target addr: 1077816
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:133, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x46 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x42 0x4f 0x41 0x2f 0x78 0x59 0x47 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 127s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 791424, len: 328, out of total len 2023424, target addr: 1078144
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:134, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x47 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x42 0x54 0x49 0x2f 0x79 0x62 0x56 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 127s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 791752, len: 328, out of total len 2023424, target addr: 1078472
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:135, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x48 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x42 0x59 0x51 0x2f 0x38 0x54 0x5a 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 792080, len: 328, out of total len 2023424, target addr: 1078800
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:136, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x49 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x42 0x64 0x59 0x2f 0x34 0x49 0x79 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 792408, len: 328, out of total len 2023424, target addr: 1079128
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:137, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x4a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x42 0x69 0x67 0x2f 0x79 0x53 0x4a 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 61ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 792736, len: 328, out of total len 2023424, target addr: 1079456
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:138, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x4b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x42 0x6e 0x6f 0x2f 0x36 0x62 0x36 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 31ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 793064, len: 328, out of total len 2023424, target addr: 1079784
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:139, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x4c 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x42 0x73 0x77 0x2f 0x30 0x54 0x32 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 793392, len: 328, out of total len 2023424, target addr: 1080112
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:140, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x4d 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x42 0x78 0x34 0x2f 0x7a 0x65 0x74 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 793720, len: 328, out of total len 2023424, target addr: 1080440
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:141, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x4e 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x42 0x33 0x41 0x2f 0x34 0x66 0x62 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 31ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 794048, len: 328, out of total len 2023424, target addr: 1080768
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:142, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x4f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x42 0x38 0x49 0x2f 0x30 0x64 0x67 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 794376, len: 328, out of total len 2023424, target addr: 1081096
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:143, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x50 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x43 0x42 0x51 0x2f 0x7a 0x6b 0x41 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 172ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 794704, len: 328, out of total len 2023424, target addr: 1081424
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:144, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x51 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x43 0x47 0x59 0x2f 0x33 0x70 0x79 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 61ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 795032, len: 328, out of total len 2023424, target addr: 1081752
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:145, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x52 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x43 0x4c 0x67 0x2f 0x37 0x49 0x77 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 795360, len: 328, out of total len 2023424, target addr: 1082080
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:146, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x53 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x43 0x51 0x6f 0x2f 0x36 0x35 0x4c 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 63ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 795688, len: 328, out of total len 2023424, target addr: 1082408
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:147, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x54 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x43 0x56 0x77 0x2f 0x77 0x36 0x50 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 44ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 796016, len: 328, out of total len 2023424, target addr: 1082736
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:148, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x55 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x43 0x61 0x34 0x2f 0x37 0x71 0x4d 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 796344, len: 328, out of total len 2023424, target addr: 1083064
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:149, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x56 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x43 0x67 0x41 0x2f 0x79 0x62 0x4c 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 796672, len: 328, out of total len 2023424, target addr: 1083392
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:150, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x57 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x43 0x6c 0x49 0x2f 0x36 0x53 0x34 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 797000, len: 328, out of total len 2023424, target addr: 1083720
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:151, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x58 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x43 0x71 0x51 0x2f 0x33 0x47 0x45 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 797328, len: 328, out of total len 2023424, target addr: 1084048
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:152, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x59 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x43 0x76 0x59 0x2f 0x7a 0x64 0x76 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 48ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 797656, len: 328, out of total len 2023424, target addr: 1084376
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:153, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x5a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x43 0x30 0x67 0x2f 0x77 0x39 0x46 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 128s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 797984, len: 328, out of total len 2023424, target addr: 1084704
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:154, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x61 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x43 0x35 0x6f 0x2f 0x2b 0x4e 0x57 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 798312, len: 328, out of total len 2023424, target addr: 1085032
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:155, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x62 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x43 0x2b 0x77 0x2f 0x31 0x67 0x4b 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 798640, len: 328, out of total len 2023424, target addr: 1085360
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:156, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x63 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x44 0x44 0x34 0x2f 0x38 0x47 0x54 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 798968, len: 328, out of total len 2023424, target addr: 1085688
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:157, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x64 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x44 0x4a 0x41 0x2f 0x79 0x69 0x31 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 799296, len: 328, out of total len 2023424, target addr: 1086016
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:158, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x65 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x44 0x4f 0x49 0x2f 0x37 0x46 0x65 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 31ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 799624, len: 328, out of total len 2023424, target addr: 1086344
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:159, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x66 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x44 0x54 0x51 0x2f 0x36 0x4d 0x36 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 799952, len: 328, out of total len 2023424, target addr: 1086672
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:160, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x67 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x44 0x59 0x59 0x2f 0x34 0x55 0x61 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 800280, len: 328, out of total len 2023424, target addr: 1087000
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:161, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x68 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x44 0x64 0x67 0x2f 0x79 0x4d 0x34 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 800608, len: 328, out of total len 2023424, target addr: 1087328
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:162, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x69 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x44 0x69 0x6f 0x2f 0x36 0x48 0x53 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 800936, len: 328, out of total len 2023424, target addr: 1087656
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:163, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x6a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x44 0x6e 0x77 0x2f 0x77 0x45 0x57 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 801264, len: 328, out of total len 2023424, target addr: 1087984
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:164, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x6b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x44 0x73 0x34 0x2f 0x34 0x49 0x6c 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 801592, len: 328, out of total len 2023424, target addr: 1088312
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:165, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x6c 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x44 0x79 0x41 0x2f 0x34 0x44 0x7a 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 801920, len: 328, out of total len 2023424, target addr: 1088640
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:166, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x6d 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x44 0x33 0x49 0x2f 0x77 0x4b 0x41 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 61ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 802248, len: 328, out of total len 2023424, target addr: 1088968
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:167, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x6e 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x44 0x38 0x51 0x2f 0x2b 0x43 0x4d 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 802576, len: 328, out of total len 2023424, target addr: 1089296
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:168, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x6f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x45 0x42 0x59 0x2f 0x32 0x56 0x75 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 170ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 802904, len: 328, out of total len 2023424, target addr: 1089624
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:169, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x70 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x45 0x47 0x67 0x2f 0x39 0x6a 0x55 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 49ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 803232, len: 328, out of total len 2023424, target addr: 1089952
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:170, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x71 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x45 0x4c 0x6f 0x2f 0x7a 0x54 0x48 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 44ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 803560, len: 328, out of total len 2023424, target addr: 1090280
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:171, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x72 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x45 0x51 0x77 0x2f 0x77 0x6f 0x4c 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 31ms. Current upload runtime is 129s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 803888, len: 328, out of total len 2023424, target addr: 1090608
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:172, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x73 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x45 0x56 0x34 0x2f 0x38 0x76 0x77 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 804216, len: 328, out of total len 2023424, target addr: 1090936
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:173, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x74 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x45 0x62 0x41 0x2f 0x78 0x58 0x6d 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 804544, len: 328, out of total len 2023424, target addr: 1091264
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:174, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x75 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x45 0x67 0x49 0x2f 0x36 0x41 0x38 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 32ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 804872, len: 328, out of total len 2023424, target addr: 1091592
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:175, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x76 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x45 0x6c 0x51 0x2f 0x77 0x44 0x34 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 805200, len: 328, out of total len 2023424, target addr: 1091920
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:176, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x77 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x45 0x71 0x59 0x2f 0x79 0x33 0x71 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 805528, len: 328, out of total len 2023424, target addr: 1092248
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:177, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x78 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x45 0x76 0x67 0x2f 0x34 0x76 0x49 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 805856, len: 328, out of total len 2023424, target addr: 1092576
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:178, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x79 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x45 0x30 0x6f 0x2f 0x35 0x65 0x7a 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 806184, len: 328, out of total len 2023424, target addr: 1092904
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:179, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x7a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x45 0x35 0x77 0x2f 0x31 0x6b 0x58 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 61ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 806512, len: 328, out of total len 2023424, target addr: 1093232
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:180, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x30 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x45 0x2b 0x34 0x2f 0x34 0x4e 0x30 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 31ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 806840, len: 328, out of total len 2023424, target addr: 1093560
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:181, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x31 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x46 0x45 0x41 0x2f 0x31 0x78 0x51 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 807168, len: 328, out of total len 2023424, target addr: 1093888
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:182, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x32 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x46 0x4a 0x49 0x2f 0x37 0x42 0x44 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 807496, len: 328, out of total len 2023424, target addr: 1094216
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:183, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x33 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x46 0x4f 0x51 0x2f 0x77 0x73 0x66 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 807824, len: 328, out of total len 2023424, target addr: 1094544
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:184, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x34 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x46 0x54 0x59 0x2f 0x2f 0x39 0x55 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 808152, len: 328, out of total len 2023424, target addr: 1094872
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:185, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x35 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x46 0x59 0x67 0x2f 0x78 0x75 0x2b 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 808480, len: 328, out of total len 2023424, target addr: 1095200
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:186, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x36 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x46 0x64 0x6f 0x2f 0x35 0x6e 0x4e 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 61ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 808808, len: 328, out of total len 2023424, target addr: 1095528
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:187, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x37 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x46 0x69 0x77 0x2f 0x7a 0x6d 0x51 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 809136, len: 328, out of total len 2023424, target addr: 1095856
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:188, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x38 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x46 0x6e 0x34 0x2f 0x2f 0x68 0x72 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 130s
{
    "duration": 130820,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 46
}
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 809464, len: 328, out of total len 2023424, target addr: 1096184
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:189, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x39 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x46 0x74 0x41 0x2f 0x78 0x46 0x4e 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 809792, len: 328, out of total len 2023424, target addr: 1096512
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:190, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x2b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x46 0x79 0x49 0x2f 0x7a 0x6f 0x47 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 48ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 810120, len: 328, out of total len 2023424, target addr: 1096840
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:191, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x47 0x2f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x46 0x33 0x51 0x2f 0x35 0x72 0x43 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 130s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 810448, len: 328, out of total len 2023424, target addr: 1097168
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:192, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x41 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x46 0x38 0x59 0x2f 0x38 0x54 0x6d 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 810776, len: 328, out of total len 2023424, target addr: 1097496
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:193, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x42 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x47 0x42 0x67 0x2f 0x37 0x78 0x67 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 156ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 811104, len: 328, out of total len 2023424, target addr: 1097824
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:194, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x43 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x47 0x47 0x6f 0x2f 0x79 0x57 0x4c 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 811432, len: 328, out of total len 2023424, target addr: 1098152
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:195, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x44 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x47 0x4c 0x77 0x2f 0x2b 0x73 0x76 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 63ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 811760, len: 328, out of total len 2023424, target addr: 1098480
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:196, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x45 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x47 0x51 0x34 0x2f 0x37 0x54 0x63 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 812088, len: 328, out of total len 2023424, target addr: 1098808
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:197, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x46 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x47 0x57 0x41 0x2f 0x77 0x53 0x71 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 31ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 812416, len: 328, out of total len 2023424, target addr: 1099136
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:198, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x47 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x47 0x62 0x49 0x2f 0x2b 0x69 0x35 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 812744, len: 328, out of total len 2023424, target addr: 1099464
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:199, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x48 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x47 0x67 0x51 0x2f 0x33 0x2f 0x55 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 813072, len: 328, out of total len 2023424, target addr: 1099792
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:200, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x49 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x47 0x6c 0x59 0x2f 0x7a 0x6b 0x2f 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 813400, len: 328, out of total len 2023424, target addr: 1100120
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:201, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x4a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x47 0x71 0x67 0x2f 0x2b 0x72 0x6c 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 813728, len: 328, out of total len 2023424, target addr: 1100448
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:202, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x4b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x47 0x76 0x6f 0x2f 0x32 0x69 0x57 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 814056, len: 328, out of total len 2023424, target addr: 1100776
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:203, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x4c 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x47 0x30 0x77 0x2f 0x31 0x5a 0x61 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 63ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 814384, len: 328, out of total len 2023424, target addr: 1101104
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:204, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x4d 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x47 0x35 0x34 0x2f 0x2f 0x6e 0x42 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 814712, len: 328, out of total len 2023424, target addr: 1101432
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:205, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x4e 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x47 0x2f 0x41 0x2f 0x30 0x6d 0x33 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 815040, len: 328, out of total len 2023424, target addr: 1101760
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:206, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x4f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x48 0x45 0x49 0x2f 0x37 0x38 0x4f 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 815368, len: 328, out of total len 2023424, target addr: 1102088
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:207, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x50 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x48 0x4a 0x51 0x2f 0x33 0x47 0x71 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 815696, len: 328, out of total len 2023424, target addr: 1102416
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:208, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x51 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x48 0x4f 0x59 0x2f 0x7a 0x4c 0x59 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 816024, len: 328, out of total len 2023424, target addr: 1102744
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:209, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x52 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x48 0x54 0x67 0x2f 0x79 0x5a 0x61 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 131s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 816352, len: 328, out of total len 2023424, target addr: 1103072
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:210, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x53 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x48 0x59 0x6f 0x2f 0x2b 0x62 0x68 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 816680, len: 328, out of total len 2023424, target addr: 1103400
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:211, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x54 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x48 0x64 0x77 0x2f 0x30 0x59 0x6c 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 817008, len: 328, out of total len 2023424, target addr: 1103728
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:212, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x55 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x48 0x69 0x34 0x2f 0x34 0x64 0x48 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 63ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 817336, len: 328, out of total len 2023424, target addr: 1104056
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:213, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x56 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x48 0x6f 0x41 0x2f 0x32 0x35 0x68 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 44ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 817664, len: 328, out of total len 2023424, target addr: 1104384
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:214, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x57 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x48 0x74 0x49 0x2f 0x2b 0x77 0x53 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 817992, len: 328, out of total len 2023424, target addr: 1104712
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:215, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x58 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x48 0x79 0x51 0x2f 0x2b 0x58 0x75 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 818320, len: 328, out of total len 2023424, target addr: 1105040
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:216, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x59 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x48 0x33 0x59 0x2f 0x36 0x4d 0x46 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 818648, len: 328, out of total len 2023424, target addr: 1105368
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:217, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x5a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x48 0x38 0x67 0x2f 0x30 0x66 0x76 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 818976, len: 328, out of total len 2023424, target addr: 1105696
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:218, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x61 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x49 0x42 0x6f 0x2f 0x7a 0x33 0x50 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 172ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 819304, len: 328, out of total len 2023424, target addr: 1106024
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:219, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x62 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x49 0x47 0x77 0x2f 0x34 0x61 0x54 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 819632, len: 328, out of total len 2023424, target addr: 1106352
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:220, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x63 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x49 0x4c 0x34 0x2f 0x79 0x6b 0x49 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 819960, len: 328, out of total len 2023424, target addr: 1106680
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:221, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x64 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x49 0x52 0x41 0x2f 0x78 0x7a 0x75 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 820288, len: 328, out of total len 2023424, target addr: 1107008
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:222, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x65 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x49 0x57 0x49 0x2f 0x34 0x55 0x46 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 820616, len: 328, out of total len 2023424, target addr: 1107336
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:223, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x66 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x49 0x62 0x51 0x2f 0x30 0x75 0x68 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 820944, len: 328, out of total len 2023424, target addr: 1107664
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:224, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x67 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x49 0x67 0x59 0x2f 0x78 0x6a 0x67 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 821272, len: 328, out of total len 2023424, target addr: 1107992
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:225, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x68 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x49 0x6c 0x67 0x2f 0x37 0x37 0x43 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 821600, len: 328, out of total len 2023424, target addr: 1108320
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:226, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x69 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x49 0x71 0x6f 0x2f 0x30 0x6c 0x4a 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 821928, len: 328, out of total len 2023424, target addr: 1108648
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:227, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x6a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x49 0x76 0x77 0x2f 0x2b 0x6d 0x4e 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 32ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 822256, len: 328, out of total len 2023424, target addr: 1108976
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:228, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x6b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x49 0x30 0x34 0x2f 0x37 0x5a 0x2b 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 132s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 822584, len: 328, out of total len 2023424, target addr: 1109304
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:229, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x6c 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x49 0x36 0x41 0x2f 0x32 0x68 0x6f 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 822912, len: 328, out of total len 2023424, target addr: 1109632
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:230, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x6d 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x49 0x2f 0x49 0x2f 0x2b 0x6f 0x62 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 823240, len: 328, out of total len 2023424, target addr: 1109960
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:231, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x6e 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4a 0x45 0x51 0x2f 0x7a 0x34 0x56 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 823568, len: 328, out of total len 2023424, target addr: 1110288
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:232, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x6f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4a 0x4a 0x59 0x2f 0x78 0x61 0x65 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 823896, len: 328, out of total len 2023424, target addr: 1110616
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:233, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x70 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4a 0x4f 0x67 0x2f 0x36 0x73 0x6b 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 824224, len: 328, out of total len 2023424, target addr: 1110944
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:234, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x71 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4a 0x54 0x6f 0x2f 0x35 0x76 0x33 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 824552, len: 328, out of total len 2023424, target addr: 1111272
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:235, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x72 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4a 0x59 0x77 0x2f 0x33 0x6e 0x37 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 48ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 824880, len: 328, out of total len 2023424, target addr: 1111600
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:236, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x73 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4a 0x64 0x34 0x2f 0x37 0x67 0x41 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 825208, len: 328, out of total len 2023424, target addr: 1111928
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:237, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x74 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4a 0x6a 0x41 0x2f 0x78 0x4e 0x33 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 825536, len: 328, out of total len 2023424, target addr: 1112256
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:238, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x75 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4a 0x6f 0x49 0x2f 0x39 0x50 0x4d 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 825864, len: 328, out of total len 2023424, target addr: 1112584
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:239, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x76 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4a 0x74 0x51 0x2f 0x33 0x4d 0x49 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 826192, len: 328, out of total len 2023424, target addr: 1112912
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:240, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x77 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4a 0x79 0x59 0x2f 0x34 0x4c 0x61 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 826520, len: 328, out of total len 2023424, target addr: 1113240
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:241, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x78 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4a 0x33 0x67 0x2f 0x79 0x54 0x34 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 31ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 826848, len: 328, out of total len 2023424, target addr: 1113568
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:242, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x79 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4a 0x38 0x6f 0x2f 0x2b 0x52 0x44 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 827176, len: 328, out of total len 2023424, target addr: 1113896
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:243, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x7a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4b 0x42 0x77 0x2f 0x35 0x6f 0x6a 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 170ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 827504, len: 328, out of total len 2023424, target addr: 1114224
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:244, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x30 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4b 0x47 0x34 0x2f 0x30 0x42 0x41 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 32ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 827832, len: 328, out of total len 2023424, target addr: 1114552
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:245, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x31 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4b 0x4d 0x41 0x2f 0x36 0x6c 0x6d 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 828160, len: 328, out of total len 2023424, target addr: 1114880
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:246, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x32 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4b 0x52 0x49 0x2f 0x35 0x6d 0x31 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 133s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 828488, len: 328, out of total len 2023424, target addr: 1115208
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:247, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x33 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4b 0x57 0x51 0x2f 0x79 0x4c 0x70 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 828816, len: 328, out of total len 2023424, target addr: 1115536
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:248, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x34 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4b 0x62 0x59 0x2f 0x77 0x70 0x69 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 829144, len: 328, out of total len 2023424, target addr: 1115864
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:249, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x35 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4b 0x67 0x67 0x2f 0x35 0x76 0x70 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 829472, len: 328, out of total len 2023424, target addr: 1116192
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:250, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x36 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4b 0x6c 0x6f 0x2f 0x78 0x6d 0x61 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 829800, len: 328, out of total len 2023424, target addr: 1116520
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:251, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x37 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4b 0x71 0x77 0x2f 0x38 0x79 0x6d 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 830128, len: 328, out of total len 2023424, target addr: 1116848
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:252, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x38 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4b 0x76 0x34 0x2f 0x77 0x31 0x64 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 830456, len: 328, out of total len 2023424, target addr: 1117176
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:253, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x39 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4b 0x31 0x41 0x2f 0x7a 0x69 0x37 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 31ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 830784, len: 328, out of total len 2023424, target addr: 1117504
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:254, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x2b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4b 0x36 0x49 0x2f 0x38 0x38 0x77 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 831112, len: 328, out of total len 2023424, target addr: 1117832
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:255, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x48 0x2f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4b 0x2f 0x51 0x2f 0x32 0x2f 0x30 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 61ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 831440, len: 328, out of total len 2023424, target addr: 1118160
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:0, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x41 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4c 0x45 0x59 0x2f 0x2f 0x66 0x61 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 831768, len: 328, out of total len 2023424, target addr: 1118488
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:1, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x42 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4c 0x4a 0x67 0x2f 0x7a 0x2b 0x59 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 134s
{
    "duration": 134493,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 47
}
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 832096, len: 328, out of total len 2023424, target addr: 1118816
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:2, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x43 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4c 0x4f 0x6f 0x2f 0x36 0x5a 0x7a 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 832424, len: 328, out of total len 2023424, target addr: 1119144
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:3, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x44 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4c 0x54 0x77 0x2f 0x37 0x51 0x58 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 832752, len: 328, out of total len 2023424, target addr: 1119472
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:4, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x45 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4c 0x59 0x34 0x2f 0x7a 0x63 0x6b 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 833080, len: 328, out of total len 2023424, target addr: 1119800
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:5, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x46 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4c 0x65 0x41 0x2f 0x34 0x64 0x53 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 63ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 833408, len: 328, out of total len 2023424, target addr: 1120128
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:6, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x47 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4c 0x6a 0x49 0x2f 0x78 0x34 0x67 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 833736, len: 328, out of total len 2023424, target addr: 1120456
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:7, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x48 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4c 0x6f 0x51 0x2f 0x2f 0x77 0x73 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 834064, len: 328, out of total len 2023424, target addr: 1120784
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:8, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x49 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4c 0x74 0x59 0x2f 0x37 0x72 0x48 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 834392, len: 328, out of total len 2023424, target addr: 1121112
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:9, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x4a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4c 0x79 0x67 0x2f 0x37 0x58 0x64 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 834720, len: 328, out of total len 2023424, target addr: 1121440
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:10, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x4b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4c 0x33 0x6f 0x2f 0x7a 0x65 0x75 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 835048, len: 328, out of total len 2023424, target addr: 1121768
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:11, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x4c 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4c 0x38 0x77 0x2f 0x39 0x57 0x69 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 134s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 835376, len: 328, out of total len 2023424, target addr: 1122096
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:12, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x4d 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4d 0x42 0x34 0x2f 0x39 0x64 0x51 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 156ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 835704, len: 328, out of total len 2023424, target addr: 1122424
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:13, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x4e 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4d 0x48 0x41 0x2f 0x32 0x63 0x6d 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 61ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 836032, len: 328, out of total len 2023424, target addr: 1122752
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:14, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x4f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4d 0x4d 0x49 0x2f 0x36 0x65 0x64 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 836360, len: 328, out of total len 2023424, target addr: 1123080
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:15, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x50 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4d 0x52 0x51 0x2f 0x37 0x58 0x35 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 836688, len: 328, out of total len 2023424, target addr: 1123408
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:16, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x51 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4d 0x57 0x59 0x2f 0x2f 0x61 0x4c 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 60ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 837016, len: 328, out of total len 2023424, target addr: 1123736
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:17, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x52 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4d 0x62 0x67 0x2f 0x7a 0x37 0x4a 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 837344, len: 328, out of total len 2023424, target addr: 1124064
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:18, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x53 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4d 0x67 0x6f 0x2f 0x34 0x73 0x54 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 837672, len: 328, out of total len 2023424, target addr: 1124392
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:19, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x54 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4d 0x6c 0x77 0x2f 0x79 0x76 0x58 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 838000, len: 328, out of total len 2023424, target addr: 1124720
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:20, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x55 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4d 0x71 0x34 0x2f 0x35 0x2f 0x55 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 838328, len: 328, out of total len 2023424, target addr: 1125048
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:21, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x56 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4d 0x77 0x41 0x2f 0x36 0x6f 0x79 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 838656, len: 328, out of total len 2023424, target addr: 1125376
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:22, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x57 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4d 0x31 0x49 0x2f 0x79 0x68 0x42 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 838984, len: 328, out of total len 2023424, target addr: 1125704
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:23, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x58 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4d 0x36 0x51 0x2f 0x2f 0x31 0x39 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 839312, len: 328, out of total len 2023424, target addr: 1126032
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:24, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x59 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4d 0x2f 0x59 0x2f 0x37 0x75 0x57 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 32ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 839640, len: 328, out of total len 2023424, target addr: 1126360
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:25, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x5a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4e 0x45 0x67 0x2f 0x32 0x6c 0x2b 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 839968, len: 328, out of total len 2023424, target addr: 1126688
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:26, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x61 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4e 0x4a 0x6f 0x2f 0x34 0x56 0x74 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 840296, len: 328, out of total len 2023424, target addr: 1127016
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:27, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x62 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4e 0x4f 0x77 0x2f 0x7a 0x34 0x78 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 840624, len: 328, out of total len 2023424, target addr: 1127344
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:28, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x63 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4e 0x54 0x34 0x2f 0x30 0x31 0x71 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 840952, len: 328, out of total len 2023424, target addr: 1127672
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:29, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x64 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4e 0x5a 0x41 0x2f 0x36 0x52 0x4d 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 135s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 841280, len: 328, out of total len 2023424, target addr: 1128000
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:30, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x65 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4e 0x65 0x49 0x2f 0x7a 0x32 0x6e 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 136s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 841608, len: 328, out of total len 2023424, target addr: 1128328
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:31, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x66 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4e 0x6a 0x51 0x2f 0x34 0x5a 0x69 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 136s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 841936, len: 328, out of total len 2023424, target addr: 1128656
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:32, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x67 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4e 0x6f 0x59 0x2f 0x36 0x42 0x43 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 63ms. Current upload runtime is 136s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 842264, len: 328, out of total len 2023424, target addr: 1128984
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:33, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x68 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4e 0x74 0x67 0x2f 0x77 0x5a 0x67 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 136s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 842592, len: 328, out of total len 2023424, target addr: 1129312
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:34, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x69 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4e 0x79 0x6f 0x2f 0x79 0x30 0x72 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 136s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 842920, len: 328, out of total len 2023424, target addr: 1129640
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:35, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x6a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4e 0x33 0x77 0x2f 0x34 0x33 0x76 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 136s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 843248, len: 328, out of total len 2023424, target addr: 1129968
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:36, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x6b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4e 0x38 0x34 0x2f 0x77 0x37 0x63 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 136s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 843576, len: 328, out of total len 2023424, target addr: 1130296
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:37, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x6c 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4f 0x43 0x41 0x2f 0x32 0x41 0x4f 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 171ms. Current upload runtime is 136s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 843904, len: 328, out of total len 2023424, target addr: 1130624
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:38, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x6d 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4f 0x48 0x49 0x2f 0x2b 0x4a 0x39 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 47ms. Current upload runtime is 136s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 844232, len: 328, out of total len 2023424, target addr: 1130952
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:39, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x6e 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4f 0x4d 0x51 0x2f 0x77 0x42 0x78 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 45ms. Current upload runtime is 136s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 844560, len: 328, out of total len 2023424, target addr: 1131280
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:40, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x6f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4f 0x52 0x59 0x2f 0x2f 0x51 0x36 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 136s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 844888, len: 328, out of total len 2023424, target addr: 1131608
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:41, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x70 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4f 0x57 0x67 0x2f 0x30 0x6d 0x41 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 136s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 845216, len: 328, out of total len 2023424, target addr: 1131936
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:42, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x71 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4f 0x62 0x6f 0x2f 0x36 0x57 0x54 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 136s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 845544, len: 328, out of total len 2023424, target addr: 1132264
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:43, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x72 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4f 0x67 0x77 0x2f 0x7a 0x4c 0x2b 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 48ms. Current upload runtime is 136s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 845872, len: 328, out of total len 2023424, target addr: 1132592
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:44, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x73 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4f 0x6c 0x34 0x2f 0x2f 0x4d 0x46 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 44ms. Current upload runtime is 136s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 846200, len: 328, out of total len 2023424, target addr: 1132920
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:45, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x74 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4f 0x72 0x41 0x2f 0x79 0x30 0x54 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 136s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 846528, len: 328, out of total len 2023424, target addr: 1133248
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:46, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x75 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4f 0x77 0x49 0x2f 0x7a 0x46 0x6f 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 136s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 846856, len: 328, out of total len 2023424, target addr: 1133576
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:47, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x76 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4f 0x31 0x51 0x2f 0x35 0x47 0x73 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 137s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 847184, len: 328, out of total len 2023424, target addr: 1133904
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:48, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x77 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4f 0x36 0x59 0x2f 0x37 0x79 0x2b 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 46ms. Current upload runtime is 137s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 847512, len: 328, out of total len 2023424, target addr: 1134232
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:49, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x78 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x4f 0x2f 0x67 0x2f 0x78 0x71 0x63 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 137s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 847840, len: 328, out of total len 2023424, target addr: 1134560
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:50, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x79 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x50 0x45 0x6f 0x2f 0x2b 0x77 0x6c 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 50ms. Current upload runtime is 137s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 848168, len: 328, out of total len 2023424, target addr: 1134888
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:51, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x7a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x50 0x4a 0x77 0x2f 0x79 0x4b 0x42 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 55ms. Current upload runtime is 137s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 848496, len: 328, out of total len 2023424, target addr: 1135216
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:52, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x30 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x50 0x4f 0x34 0x2f 0x2f 0x6a 0x69 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 91ms. Current upload runtime is 137s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 848824, len: 328, out of total len 2023424, target addr: 1135544
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:53, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x31 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x50 0x55 0x41 0x2f 0x38 0x30 0x45 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 80ms. Current upload runtime is 137s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 849152, len: 328, out of total len 2023424, target addr: 1135872
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:54, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x32 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x50 0x5a 0x49 0x2f 0x79 0x45 0x58 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 49ms. Current upload runtime is 137s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 849480, len: 328, out of total len 2023424, target addr: 1136200
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:55, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x33 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x50 0x65 0x51 0x2f 0x35 0x70 0x4c 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 40ms. Current upload runtime is 137s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 849808, len: 328, out of total len 2023424, target addr: 1136528
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:56, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x34 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x50 0x6a 0x59 0x2f 0x38 0x65 0x68 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 48ms. Current upload runtime is 137s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 850136, len: 328, out of total len 2023424, target addr: 1136856
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:57, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x35 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x50 0x6f 0x67 0x2f 0x79 0x4e 0x4c 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 44ms. Current upload runtime is 137s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 850464, len: 328, out of total len 2023424, target addr: 1137184
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:58, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x36 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x50 0x74 0x6f 0x2f 0x36 0x45 0x34 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 61ms. Current upload runtime is 137s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 850792, len: 328, out of total len 2023424, target addr: 1137512
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:59, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x37 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x50 0x79 0x77 0x2f 0x36 0x6a 0x45 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 137s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 851120, len: 328, out of total len 2023424, target addr: 1137840
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:60, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(39): 0x06 0x09 0x41 0x42 0x63 0x44 0x41 0x41 0x41 0x50 0x41 0x45 0x45 0x38 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6f 0x41 0x44 0x50 0x33 0x34 0x2f 0x32 0x6b 0x2f 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-COM3] Chunk upload took 62ms. Current upload runtime is 137s
[Debug   ] [ModemUARTDFU-Probe-COM3] Uploading chunk offset: 851448, len: 328, out of total len 2023424, target addr: 1138168
[Debug   ] [ModemUARTDFU-Probe-COM3] TX pkt with header: op:2 flags:0 len:356, group:65, seq:61, id: 1, total size: 492
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 30000ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x41 0x44
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 29948ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 29697ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 29432ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 29181ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 28947ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 28713ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x69 0x63
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 28463ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x41 0x47
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 28213ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x39 0x72
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 27931ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 27696ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 27447ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 27211ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x45 0x39
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 26947ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x41 0x45
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 26697ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 26462ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x41 0x45
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 26228ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 25993ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 25745ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x30 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Error   ] [ModemUARTDFU-Probe-COM3] Exception occured in smp::SmpPacket::decode, parse error: character [6 '♠'] out of bounds
[Error   ] [ModemUARTDFU-Probe-COM3] Got corrupt data.
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT true
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 25490ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 25448ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 25197ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 24962ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x39 0x72
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 24713ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 24464ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x47 0x2f
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 24197ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x63 0x6d
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 23948ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 23697ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 23448ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 23181ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 22916ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 22681ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 22432ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 22197ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 21963ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 21697ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 21447ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 21181ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 20916ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 20666ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x39 0x41
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 20416ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 20166ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 19916ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 19682ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 19432ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(3): 0x06 0x09 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Error   ] [ModemUARTDFU-Probe-COM3] Exception occured in smp::SmpPacket::decode, parse error: character [6 '♠'] out of bounds
[Error   ] [ModemUARTDFU-Probe-COM3] Got corrupt data.
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT true
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 19179ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 19134ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 18868ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 18620ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 18369ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x69 0x63
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 18104ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 17869ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 17588ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 17352ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x45 0x45
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 17103ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 16854ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 16604ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 16368ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 16119ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 15868ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 15634ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 15385ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 15135ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(3): 0x06 0x09 0x0a
[Debug   ] [ModemUARTDFU-Probe-COM3] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-COM3] Attempting to decode frames vector with 1 frames
[Error   ] [ModemUARTDFU-Probe-COM3] Exception occured in smp::SmpPacket::decode, parse error: character [6 '♠'] out of bounds
[Error   ] [ModemUARTDFU-Probe-COM3] Got corrupt data.
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT true
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 14899ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 14853ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x47 0x41
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 14587ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 14352ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x62 0x39
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 14104ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 13869ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 13635ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x4d 0x47
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 13385ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 13135ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x41 0x62
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 12885ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x41 0x62
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 12649ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 12385ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 12120ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 11883ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 11636ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 11400ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x63 0x6d
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 11150ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x41 0x47
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 10901ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 10650ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x41 0x47
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 10400ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 10151ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 9901ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x45 0x45
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 9651ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 9401ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 9151ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 8901ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 8651ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 8416ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 8182ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 7916ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 7667ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 7401ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x39 0x69
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 7150ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 6885ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 6635ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 6384ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 6120ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 5869ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 5620ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 5369ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 5135ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x62 0x39
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 4886ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 4635ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 4385ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 4136ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 3885ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 3635ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x4d 0x47
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 3369ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 3119ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 2884ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 2649ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 2385ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x39 0x69
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 2135ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 1901ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 1634ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 1385ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 1135ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 884ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 635ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(4): 0x06 0x09 0x45 0x39
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 385ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 200ms
[Debug   ] [ModemUARTDFU-Probe-COM3] Re-sending package
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(495)
[Debug   ] [ModemUARTDFU-Probe-COM3] Waiting with timeout 135ms
[Debug   ] [ModemUARTDFU-Probe-COM3] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-COM3] No time left to wait for data. Timeout
{
    "duration": 167914,
    "error_code": "Timeout",
    "message": "Image upload failed. Bad response from device",
    "operation": "upload_image",
    "outcome": "fail",
    "progress_percentage": 100
}
[Error   ] [ModemUARTDFU-Probe-COM3] Error during image file upload. Upload returned an error.
[Info    ] [ModemUARTDFU-Probe-COM3] Failed programming file C:\Users\jerwood\AppData\Local\Temp\s6jo.0nrfjprog\firmware.update.image.segments.1.hex.
[Info    ] [ModemUARTDFU-Probe-COM3] Failed while programming files to target.
[Info    ] [ModemUARTDFU-Probe-COM3] Failed to program DFU package
[Info    ] [HighLevel ] Failed programming the device.
b'An error was reported by NRFJPROG DLL: -220 TIME_OUT.'
[Debug   ] [HighLevel ] is_dll_open
[Debug   ] [HighLevel ] probe_uninit
[Info    ] [HighLevel ] Deleting probe at location 0x20ef3213530
[Debug   ] [ModemUARTDFU-Probe-COM3] readDeviceInfo
[Info    ] [ModemUARTDFU-Probe-COM3] Uninitializing ModemUARTDFU probe at serial port COM3.
[Debug   ] [ModemUARTDFU-Probe-COM3] uninitialize
[Info    ] [ModemUARTDFU-Probe-COM3] Sending device reset request
[Info    ] [ModemUARTDFU-Probe-COM3] Sending reset request to device.
[Debug   ] [ModemUARTDFU-Probe-COM3] UART TX(23)
[Info    ] [ModemUARTDFU-Probe-COM3] Closing connection to mcuboot device
[Debug   ] [ModemUARTDFU-Probe-COM3] serial port read on port COM3 aborted
[Debug   ] [ModemUARTDFU-Probe-COM3] serial io_context executed 2747 handlers.
[Info    ] [ModemUARTDFU-Probe-COM3] serial port COM3 closed.
{
    "duration": 134,
    "error_code": "Ok",
    "operation": "close_uart",
    "outcome": "success",
    "progress_percentage": 100
}
[Info    ] [HighLevel ] Done.
[Debug   ] [HighLevel ] dll_close
[Info    ] [HighLevel ] closing and freeing sub dlls.
Traceback (most recent call last):
  File "\\Mac\Home\Desktop\fmfu_smp_svr\update_modem.py", line 43, in <module>
    run(args.uart, args.firmware, args.baudrate)
  File "\\Mac\Home\Desktop\fmfu_smp_svr\update_modem.py", line 26, in run
    modem_dfu_probe.program(modem_firmware_zip)
  File "C:\Users\jerwood\AppData\Local\Programs\Python\Python39\lib\site-packages\pynrfjprog\HighLevel.py", line 350, in program
    raise APIError(result, log=self._logger.error)
pynrfjprog.APIError.APIError: An error was reported by NRFJPROG DLL: -220 TIME_OUT.
PS Microsoft.PowerShell.Core\FileSystem::\\Mac\Home\Desktop\fmfu_smp_svr>