sudo ./venv/bin/python ./update_modem.py ./mfwnrf9160123.zip /dev/ttyACM0 1000000
[sudo] password for jerwood:
# modem firmware upgrade over serial port example started.
[Debug   ] [HighLevel ] dll_open
[Info    ] [HighLevel ] default_jlink_path parameter is NULL, latest JLINKARM DLL will be looked for and used.
[Debug   ] [HighLevel ] is_dll_open
[Debug   ] [HighLevel ] mcuboot_dfu_init
[Info    ] [HighLevel ] Creating new probe
[Info    ] [HighLevel ] initializing DFU
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] ModemUARTDFUProbe_initialize
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Dll directory is /home/jerwood/projects/nrf9160_modem_update/ncs/nrf/samples/nrf9160/fmfu_smp_svr/pynrfjprog_10_13_0_preview_2sec_timeout/pynrfjprog/lib_x64.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Find and connect to dfu dll
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Using DFU dll at /home/jerwood/projects/nrf9160_modem_update/ncs/nrf/samples/nrf9160/fmfu_smp_svr/pynrfjprog_10_13_0_preview_2sec_timeout/pynrfjprog/lib_x64/libnrfdfu.so.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Load library at /home/jerwood/projects/nrf9160_modem_update/ncs/nrf/samples/nrf9160/fmfu_smp_svr/pynrfjprog_10_13_0_preview_2sec_timeout/pynrfjprog/lib_x64/libnrfdfu.so.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Library loaded, loading member functions.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Member functions succesfully loaded.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Timeout set to 30000ms
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Initialize new probe.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] initialize
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Successfully opened port: /dev/ttyACM0@1000000,flow_control:none,parity:none.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:0 flags:0 len:14, group:2, seq:0, id: 0, total size: 36
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(39)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 400ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] No time left to wait for data. Timeout
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Have image upload chunk size of 272 (1st packet) and 328 (proceeding)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Using MTU 500 and frame size 500.
{
    "duration": 944,
    "error_code": "Ok",
    "operation": "open_uart",
    "outcome": "success",
    "progress_percentage": 100
}
[Info    ] [HighLevel ] Probe initialization complete!
[Debug   ] [HighLevel ] program
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] program
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] program_package
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Check if provided file exists
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Check if provided file can be read
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Unzipping package ./mfwnrf9160123.zip.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 13416, bytes from 72B3D7C.ipc_dfu.signed_1.1.0.ihex.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 456, bytes from firmware.update.image.digest.txt.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 6510, bytes from firmware.update.image.segments.0.hex.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 5622317, bytes from firmware.update.image.segments.1.hex.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 68782, bytes from mfw_nrf9160_1.2.3_release_notes.txt.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 15722, bytes from mfw_nrf9160_license-agreement.txt.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 219106, bytes from mfw_nrf9160_update_from_1.2.1_to_1.2.3.bin.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 35214, bytes from mfw_nrf9160_update_from_1.2.2_to_1.2.3.bin.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 14166, bytes from mfw_nrf9160_update_from_1.2.3-FOTA-TEST_to_1.2.3.bin.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 14166, bytes from mfw_nrf9160_update_from_1.2.3_to_1.2.3-FOTA-TEST.bin.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Extracting 726, bytes from README.txt.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] program files
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Programming bootloader
Programming modem bootloader.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Found bootloader file /tmp/fileXNB59Inrfjprog/72B3D7C.ipc_dfu.signed_1.1.0.ihex.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] program_file
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Evaluating file /tmp/fileXNB59Inrfjprog/72B3D7C.ipc_dfu.signed_1.1.0.ihex.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Check if provided file exists
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Check if provided file can be read
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Open provided file
{
    "duration": 0,
    "message": "Calculating image size",
    "operation": "upload_image",
    "progress_percentage": 5
}
{
    "duration": 1,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 10
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 0, len: 272, out of total len 4752, target addr: 536870924
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:341, group:65, seq:1, id: 1, total size: 472
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(475)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(33): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x42 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x42 0x45 0x50 0x2f 0x4e 0x63 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 45ms. Current upload runtime is 0s
{
    "duration": 47,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 15
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 272, len: 328, out of total len 4752, target addr: 536871196
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:2, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x09 0x41 0x42
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(35): 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x43 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x43 0x57 0x50 0x2f 0x7a 0x59 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 60ms. Current upload runtime is 0s
{
    "duration": 109,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 21
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 600, len: 328, out of total len 4752, target addr: 536871524
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:3, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x41 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(25): 0x41 0x41 0x4e 0x41 0x45 0x45 0x44 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x44 0x6f 0x50
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x2f 0x77 0x78 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 80ms. Current upload runtime is 0s
{
    "duration": 191,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 27
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 928, len: 328, out of total len 4752, target addr: 536871852
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:4, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x41 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x41 0x41 0x4e 0x41 0x45 0x45 0x45 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x45 0x36 0x50 0x2b 0x4a 0x70 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 0s
{
    "duration": 275,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 33
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1256, len: 328, out of total len 4752, target addr: 536872180
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:5, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(23): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x46 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(10): 0x47 0x4d 0x50 0x2f 0x56 0x74 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 80ms. Current upload runtime is 0s
{
    "duration": 357,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 40
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1584, len: 328, out of total len 4752, target addr: 536872508
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:6, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x41 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x41 0x41 0x4e 0x41 0x45 0x45 0x47 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x39 0x6d 0x5a 0x68 0x6b 0x48 0x65 0x50 0x2b 0x46 0x78 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 0s
{
    "duration": 440,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 46
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1912, len: 328, out of total len 4752, target addr: 536872836
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:7, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x41 0x41 0x4e 0x41 0x45 0x45 0x48 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x39 0x6d 0x5a 0x68 0x6b 0x49 0x77 0x50 0x2b 0x51 0x72 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 0s
{
    "duration": 522,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 52
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 2240, len: 328, out of total len 4752, target addr: 536873164
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:8, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(33): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x49 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4b 0x43 0x50 0x38 0x2b 0x34 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 61ms. Current upload runtime is 0s
{
    "duration": 585,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 58
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 2568, len: 328, out of total len 4752, target addr: 536873492
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:9, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(29): 0x41 0x4e 0x41 0x45 0x45 0x4a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4c 0x55 0x50 0x38 0x67 0x4f 0x77 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 80ms. Current upload runtime is 0s
{
    "duration": 668,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 64
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 2896, len: 328, out of total len 4752, target addr: 536873820
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:10, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x41 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(13): 0x41 0x41 0x4e 0x41 0x45 0x45 0x4b 0x41 0x62 0x39 0x69 0x63 0x6d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4d 0x6d 0x50 0x2f 0x5a 0x63 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 0s
{
    "duration": 751,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 71
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 3224, len: 328, out of total len 4752, target addr: 536874148
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:11, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x41 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(14): 0x41 0x41 0x4e 0x41 0x45 0x45 0x4c 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4e 0x34 0x50 0x2f 0x42 0x54 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 80ms. Current upload runtime is 0s
{
    "duration": 833,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 77
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 3552, len: 328, out of total len 4752, target addr: 536874476
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:12, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(32): 0x41 0x41 0x4e 0x41 0x45 0x45 0x4d 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x50 0x4b 0x50 0x39 0x49 0x52 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 61ms. Current upload runtime is 0s
{
    "duration": 896,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 83
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 3880, len: 328, out of total len 4752, target addr: 536874804
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:13, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x41 0x4e 0x41 0x45 0x45 0x4e 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(14): 0x6d 0x5a 0x68 0x6b 0x51 0x63 0x50 0x38 0x4f 0x2f 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 0s
{
    "duration": 980,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 89
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 4208, len: 328, out of total len 4752, target addr: 536875132
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:14, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x09 0x41 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(30): 0x41 0x4e 0x41 0x45 0x45 0x4f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x52 0x75 0x50 0x39 0x46 0x46 0x51 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 80ms. Current upload runtime is 1s
{
    "duration": 1061,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 95
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 4536, len: 216, out of total len 4752, target addr: 536875460
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:241, group:65, seq:15, id: 1, total size: 340
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(343)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(33): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x50 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x53 0x6b 0x50 0x38 0x39 0x39 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 126ms. Current upload runtime is 1s
{
    "duration": 1189,
    "operation": "upload_image",
    "outcome": "success",
    "progress_percentage": 100
}
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Program bootloader SUCCESS
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Bootloader programmed
Programming file 1 of 2 files.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] program_file
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Evaluating file /tmp/fileXNB59Inrfjprog/firmware.update.image.segments.0.hex.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Check if provided file exists
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Check if provided file can be read
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Open provided file
{
    "duration": 0,
    "message": "Calculating image size",
    "operation": "upload_image",
    "progress_percentage": 5
}
{
    "duration": 1,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 10
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 0, len: 272, out of total len 2304, target addr: 1499471872
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:341, group:65, seq:16, id: 1, total size: 472
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(475)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x41 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x41 0x41 0x4e 0x41 0x45 0x45 0x51 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(12): 0x68 0x6b 0x42 0x45 0x50 0x38 0x74 0x42 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 77ms. Current upload runtime is 0s
{
    "duration": 79,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 20
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 272, len: 328, out of total len 2304, target addr: 1499472144
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:17, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(33): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x52 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x43 0x57 0x50 0x39 0x65 0x7a 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 60ms. Current upload runtime is 0s
{
    "duration": 141,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 33
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 600, len: 328, out of total len 2304, target addr: 1499472472
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:18, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(31): 0x41 0x4e 0x41 0x45 0x45 0x53 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x44 0x6f 0x50 0x38 0x51 0x73 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 60ms. Current upload runtime is 0s
{
    "duration": 202,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 46
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 928, len: 328, out of total len 2304, target addr: 1499472800
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:19, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x54 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(12): 0x68 0x6b 0x45 0x36 0x50 0x2b 0x2f 0x75 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 0s
{
    "duration": 284,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 59
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1256, len: 328, out of total len 2304, target addr: 1499473128
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:20, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x41 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(10): 0x41 0x41 0x4e 0x41 0x45 0x45 0x55 0x41 0x62 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x47 0x4d 0x50 0x38 0x31 0x77 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 0s
{
    "duration": 368,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 71
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1584, len: 328, out of total len 2304, target addr: 1499473456
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:21, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(33): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x56 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x48 0x65 0x50 0x38 0x6f 0x61 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 61ms. Current upload runtime is 0s
{
    "duration": 430,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 84
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1912, len: 328, out of total len 2304, target addr: 1499473784
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:354, group:65, seq:22, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(31): 0x41 0x4e 0x41 0x45 0x45 0x57 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x49 0x77 0x50 0x39 0x77 0x32 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 61ms. Current upload runtime is 0s
{
    "duration": 493,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 97
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 2240, len: 64, out of total len 2304, target addr: 1499474112
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:89, group:65, seq:23, id: 1, total size: 136
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(139)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x09 0x41 0x42 0x55
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x58 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4a 0x41 0x50 0x2f 0x2f 0x51 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 79ms. Current upload runtime is 0s
{
    "duration": 574,
    "operation": "upload_image",
    "outcome": "success",
    "progress_percentage": 100
}
Finished with file.
Programming file 2 of 2 files.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] program_file
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Evaluating file /tmp/fileXNB59Inrfjprog/firmware.update.image.segments.1.hex.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Check if provided file exists
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Check if provided file can be read
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Open provided file
{
    "duration": 0,
    "message": "Calculating image size",
    "operation": "upload_image",
    "progress_percentage": 5
}
{
    "duration": 1,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 10
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 0, len: 272, out of total len 1998848, target addr: 24576
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:341, group:65, seq:24, id: 1, total size: 472
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(475)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x59 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x42 0x45 0x50 0x38 0x4b 0x51 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 79ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 272, len: 328, out of total len 1998848, target addr: 24848
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:25, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(16): 0x41 0x4e 0x41 0x45 0x45 0x5a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x39 0x6d 0x5a 0x68 0x6b 0x43 0x57 0x50 0x39 0x35 0x69 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 600, len: 328, out of total len 1998848, target addr: 25176
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:26, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x41 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x41 0x41 0x4e 0x41 0x45 0x45 0x61 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(12): 0x68 0x6b 0x44 0x6f 0x50 0x38 0x33 0x39 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 83ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 928, len: 328, out of total len 1998848, target addr: 25504
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:27, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x41 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x41 0x4e 0x41 0x45 0x45 0x62 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(12): 0x68 0x6b 0x45 0x36 0x50 0x2b 0x59 0x2f 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1256, len: 328, out of total len 1998848, target addr: 25832
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:28, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(26): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x63 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x47 0x4d 0x50
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x38 0x53 0x68 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 83ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1584, len: 328, out of total len 1998848, target addr: 26160
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:29, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(13): 0x41 0x4e 0x41 0x45 0x45 0x64 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x48 0x65 0x50 0x38 0x50 0x4c 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 1912, len: 328, out of total len 1998848, target addr: 26488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:30, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x09 0x41 0x42 0x55
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(34): 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x65 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x49 0x77 0x50 0x39 0x58 0x6e 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 62ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 2240, len: 328, out of total len 1998848, target addr: 26816
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:31, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(33): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x66 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4b 0x43 0x50 0x38 0x49 0x2f 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 62ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 2568, len: 328, out of total len 1998848, target addr: 27144
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:32, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(13): 0x41 0x4e 0x41 0x45 0x45 0x67 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4c 0x55 0x50 0x38 0x30 0x6c 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 2896, len: 328, out of total len 1998848, target addr: 27472
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:33, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x41 0x42 0x55
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(33): 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x68 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4d 0x6d 0x50 0x2b 0x41 0x42 0x77 0x3d 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 3224, len: 328, out of total len 1998848, target addr: 27800
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:34, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(29): 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x69 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x4e 0x34 0x50
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x2f 0x56 0x34 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 83ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 3552, len: 328, out of total len 1998848, target addr: 28128
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:35, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(23): 0x41 0x4e 0x41 0x45 0x45 0x6a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x50 0x4b
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(8): 0x50 0x2b 0x4b 0x67 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 0s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 3880, len: 328, out of total len 1998848, target addr: 28456
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:36, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x09 0x41 0x42 0x55
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(27): 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x6b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x51 0x63 0x50
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x38 0x61 0x55 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 4208, len: 328, out of total len 1998848, target addr: 28784
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:37, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(27): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x6c 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x52 0x75 0x50 0x38
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(6): 0x63 0x59 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 4536, len: 328, out of total len 1998848, target addr: 29112
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:38, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x09 0x41 0x42 0x55
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(14): 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x6d 0x41 0x62 0x39 0x69 0x63
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x54 0x41 0x50 0x38 0x47 0x67 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 4864, len: 328, out of total len 1998848, target addr: 29440
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:39, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x4e 0x41 0x45 0x45 0x6e 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(13): 0x5a 0x68 0x6b 0x55 0x53 0x50 0x2b 0x70 0x69 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 5192, len: 328, out of total len 1998848, target addr: 29768
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:40, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(12): 0x41 0x4e 0x41 0x45 0x45 0x6f 0x41 0x62 0x39 0x69 0x63 0x6d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x56 0x6b 0x50 0x39 0x64 0x35 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 5520, len: 328, out of total len 1998848, target addr: 30096
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:41, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(26): 0x41 0x4e 0x41 0x45 0x45 0x70 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x57 0x32 0x50 0x38 0x75
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x4c 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 5848, len: 328, out of total len 1998848, target addr: 30424
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:42, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x71 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x59 0x49 0x50 0x39 0x4d 0x59 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 83ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 6176, len: 328, out of total len 1998848, target addr: 30752
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:43, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x72 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x5a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(9): 0x61 0x50 0x39 0x52 0x79 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 6504, len: 328, out of total len 1998848, target addr: 31080
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:44, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(26): 0x73 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x61 0x73 0x50 0x2f 0x73 0x67 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 79ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 6832, len: 328, out of total len 1998848, target addr: 31408
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:45, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x41 0x4e 0x41 0x45 0x45 0x74 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(11): 0x6b 0x62 0x2b 0x50 0x2f 0x78 0x4b 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 83ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 7160, len: 328, out of total len 1998848, target addr: 31736
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:46, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(8): 0x09 0x41 0x42 0x55 0x44 0x41 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(16): 0x4e 0x41 0x45 0x45 0x75 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(14): 0x6d 0x5a 0x68 0x6b 0x64 0x51 0x50 0x38 0x33 0x43 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 7488, len: 328, out of total len 1998848, target addr: 32064
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:47, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(29): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x76 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x65 0x69 0x50 0x39 0x66 0x57
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 1s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 7816, len: 328, out of total len 1998848, target addr: 32392
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:48, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x77 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(16): 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x66 0x30 0x50 0x2f 0x2b 0x4a 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 83ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 8144, len: 328, out of total len 1998848, target addr: 32720
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:49, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(33): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x78 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x68 0x47 0x50 0x38 0x52 0x67 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 201ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 8472, len: 328, out of total len 1998848, target addr: 33048
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:50, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(32): 0x41 0x41 0x4e 0x41 0x45 0x45 0x79 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x69 0x59 0x50 0x38 0x71 0x42 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 62ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 8800, len: 328, out of total len 1998848, target addr: 33376
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:51, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(10): 0x41 0x4e 0x41 0x45 0x45 0x7a 0x41 0x62 0x39 0x69
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x6a 0x71 0x50 0x38 0x73 0x4e 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 9128, len: 328, out of total len 1998848, target addr: 33704
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:52, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(16): 0x41 0x4e 0x41 0x45 0x45 0x30 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x39 0x6d 0x5a 0x68 0x6b 0x6b 0x38 0x50 0x39 0x57 0x4a 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 9456, len: 328, out of total len 1998848, target addr: 34032
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:53, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(14): 0x41 0x41 0x4e 0x41 0x45 0x45 0x31 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x6d 0x4f 0x50 0x38 0x4a 0x52 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 9784, len: 328, out of total len 1998848, target addr: 34360
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:54, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(13): 0x41 0x4e 0x41 0x45 0x45 0x32 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x6e 0x67 0x50 0x39 0x4b 0x39 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 84ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 10112, len: 328, out of total len 1998848, target addr: 34688
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:55, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(29): 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x33 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x6f 0x79 0x50 0x39 0x4d 0x58
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 80ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 10440, len: 328, out of total len 1998848, target addr: 35016
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:56, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(13): 0x41 0x4e 0x41 0x45 0x45 0x34 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x71 0x45 0x50 0x2f 0x68 0x59 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 83ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 10768, len: 328, out of total len 1998848, target addr: 35344
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:57, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(31): 0x41 0x4e 0x41 0x45 0x45 0x35 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x72 0x57 0x50 0x2f 0x38 0x79 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 60ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 11096, len: 328, out of total len 1998848, target addr: 35672
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:58, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x09 0x41 0x42 0x55
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(30): 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x36 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x73 0x6f 0x50 0x38 0x41 0x46
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 83ms. Current upload runtime is 2s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 11424, len: 328, out of total len 1998848, target addr: 36000
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:59, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x09 0x41 0x42
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x45 0x37 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(14): 0x6d 0x5a 0x68 0x6b 0x74 0x36 0x50 0x38 0x64 0x76 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 3s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 11752, len: 328, out of total len 1998848, target addr: 36328
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:60, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(32): 0x41 0x41 0x4e 0x41 0x45 0x45 0x38 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x76 0x4d 0x50 0x2b 0x58 0x78 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 62ms. Current upload runtime is 3s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 12080, len: 328, out of total len 1998848, target addr: 36656
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:61, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(32): 0x41 0x41 0x4e 0x41 0x45 0x45 0x39 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x77 0x65 0x50 0x2f 0x53 0x44 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 61ms. Current upload runtime is 3s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 12408, len: 328, out of total len 1998848, target addr: 36984
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:62, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(16): 0x41 0x4e 0x41 0x45 0x45 0x2b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x39 0x6d 0x5a 0x68 0x6b 0x78 0x77 0x50 0x2b 0x52 0x76 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 3s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 12736, len: 328, out of total len 1998848, target addr: 37312
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:63, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x41 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(32): 0x41 0x41 0x4e 0x41 0x45 0x45 0x2f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x7a 0x43 0x50 0x2f 0x4f 0x33 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 63ms. Current upload runtime is 3s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 13064, len: 328, out of total len 1998848, target addr: 37640
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:64, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x41 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(32): 0x41 0x41 0x4e 0x41 0x45 0x46 0x41 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x30 0x55 0x50 0x39 0x71 0x48 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 60ms. Current upload runtime is 3s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 13392, len: 328, out of total len 1998848, target addr: 37968
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:65, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(10): 0x41 0x4e 0x41 0x45 0x46 0x42 0x41 0x62 0x39 0x69
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(21): 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x31 0x6d 0x50 0x39 0x73 0x4c 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 3s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 13720, len: 328, out of total len 1998848, target addr: 38296
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:66, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(30): 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x43 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x32 0x34 0x50 0x39 0x58 0x71 0x77
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 83ms. Current upload runtime is 3s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 14048, len: 328, out of total len 1998848, target addr: 38624
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:67, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x44 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x34 0x4b 0x50 0x39 0x39 0x71 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 3s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 14376, len: 328, out of total len 1998848, target addr: 38952
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:68, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x41 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x41 0x41 0x4e 0x41 0x45 0x46 0x45 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(12): 0x68 0x6b 0x35 0x63 0x50 0x2b 0x31 0x47 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 80ms. Current upload runtime is 3s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 14704, len: 328, out of total len 1998848, target addr: 39280
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:69, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(31): 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x46 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x36 0x75 0x50 0x2f 0x64 0x53 0x77 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 3s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 15032, len: 328, out of total len 1998848, target addr: 39608
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:70, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(19): 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x47 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(14): 0x6d 0x5a 0x68 0x6b 0x38 0x41 0x50 0x38 0x62 0x61 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 3s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 15360, len: 328, out of total len 1998848, target addr: 39936
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:71, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(17): 0x41 0x41 0x4e 0x41 0x45 0x46 0x48 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x39 0x6d 0x5a 0x68 0x6b 0x39 0x53 0x50 0x38 0x47 0x77 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 3s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 15688, len: 328, out of total len 1998848, target addr: 40264
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:72, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x09 0x41 0x42 0x55
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(34): 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x49 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x2b 0x6b 0x50 0x2b 0x63 0x7a 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 62ms. Current upload runtime is 3s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 16016, len: 328, out of total len 1998848, target addr: 40592
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:73, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(29): 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x4a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6b 0x2f 0x32 0x50 0x2b 0x42 0x5a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 80ms. Current upload runtime is 4s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 16344, len: 328, out of total len 1998848, target addr: 40920
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:74, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x09 0x41 0x42 0x55
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(34): 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x4b 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x42 0x49 0x50 0x38 0x37 0x49 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 198ms. Current upload runtime is 4s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 16672, len: 328, out of total len 1998848, target addr: 41248
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:75, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(29): 0x41 0x4e 0x41 0x45 0x46 0x4c 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x43 0x61 0x50 0x39 0x49 0x36 0x77 0x3d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 83ms. Current upload runtime is 4s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 17000, len: 328, out of total len 1998848, target addr: 41576
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:76, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(16): 0x41 0x4e 0x41 0x45 0x46 0x4d 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x39 0x6d 0x5a 0x68 0x6c 0x44 0x73 0x50 0x2b 0x62 0x77 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 4s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 17328, len: 328, out of total len 1998848, target addr: 41904
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:77, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(10): 0x42 0x55 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(26): 0x4e 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x45 0x2b 0x50 0x38 0x30 0x79 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 80ms. Current upload runtime is 4s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 17656, len: 328, out of total len 1998848, target addr: 42232
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:78, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x4f 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(18): 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x47 0x51 0x50 0x38 0x75 0x4b 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 4s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 17984, len: 328, out of total len 1998848, target addr: 42560
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:79, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(10): 0x41 0x41 0x4e 0x41 0x45 0x46 0x50 0x41 0x62 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x48 0x69 0x50 0x38 0x6f 0x47 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 4s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 18312, len: 328, out of total len 1998848, target addr: 42888
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:80, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x41 0x4e 0x41 0x45 0x46 0x51 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(24): 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x49 0x30 0x50 0x2b 0x53 0x5a 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 80ms. Current upload runtime is 4s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 18640, len: 328, out of total len 1998848, target addr: 43216
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:81, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(31): 0x41 0x4e 0x41 0x45 0x46 0x52 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x4b 0x47 0x50 0x2f 0x4e 0x42 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 62ms. Current upload runtime is 4s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 18968, len: 328, out of total len 1998848, target addr: 43544
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:82, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(26): 0x41 0x4e 0x41 0x45 0x46 0x53 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x4c 0x59 0x50 0x2b 0x59
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x34 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 83ms. Current upload runtime is 4s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 19296, len: 328, out of total len 1998848, target addr: 43872
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:83, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(29): 0x41 0x41 0x4e 0x41 0x45 0x46 0x54 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x4d 0x71 0x50 0x38 0x73 0x63 0x51
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 4s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 19624, len: 328, out of total len 1998848, target addr: 44200
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:84, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(11): 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x55 0x41 0x62 0x39
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(22): 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x4e 0x38 0x50 0x2f 0x6b 0x77 0x41 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 80ms. Current upload runtime is 5s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 19952, len: 328, out of total len 1998848, target addr: 44528
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:85, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x41 0x4e 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(28): 0x45 0x46 0x56 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x50 0x4f 0x50 0x2b 0x37 0x6f 0x51 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 5s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 20280, len: 328, out of total len 1998848, target addr: 44856
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:86, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x41 0x4e 0x41 0x45 0x46 0x57 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(11): 0x6c 0x51 0x67 0x50 0x2b 0x67 0x63 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 83ms. Current upload runtime is 5s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 20608, len: 328, out of total len 1998848, target addr: 45184
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:87, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x41 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(32): 0x41 0x41 0x4e 0x41 0x45 0x46 0x58 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x52 0x79 0x50 0x2b 0x39 0x32 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 62ms. Current upload runtime is 5s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 20936, len: 328, out of total len 1998848, target addr: 45512
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:88, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x09 0x41 0x42 0x55 0x44
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(13): 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x59 0x41 0x62 0x39 0x69 0x63
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(20): 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x54 0x45 0x50 0x38 0x51 0x35 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 81ms. Current upload runtime is 5s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 21264, len: 328, out of total len 1998848, target addr: 45840
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:89, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(3): 0x06 0x09 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(16): 0x41 0x4e 0x41 0x45 0x46 0x5a 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(15): 0x39 0x6d 0x5a 0x68 0x6c 0x55 0x57 0x50 0x2b 0x2f 0x37 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 82ms. Current upload runtime is 5s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 21592, len: 328, out of total len 1998848, target addr: 46168
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:90, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x09 0x41 0x42 0x55
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(11): 0x44 0x41 0x41 0x41 0x4e 0x41 0x45 0x46 0x61 0x41 0x62
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(23): 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x56 0x6f 0x50 0x2f 0x78 0x6b 0x77 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 80ms. Current upload runtime is 5s
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 21920, len: 328, out of total len 1998848, target addr: 46496
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:91, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(2): 0x06 0x09
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(5): 0x41 0x42 0x55 0x44 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x41 0x41 0x4e 0x41 0x45 0x46 0x62
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(25): 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x57 0x36 0x50 0x2b 0x43 0x57 0x67 0x3d 0x3d 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Chunk upload took 80ms. Current upload runtime is 5s
{
    "duration": 5614,
    "message": "Uploading image to device",
    "operation": "upload_image",
    "progress_percentage": 11
}
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uploading chunk offset: 22248, len: 328, out of total len 1998848, target addr: 46824
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] TX pkt with header: op:2 flags:0 len:352, group:65, seq:92, id: 1, total size: 488
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(4): 0x41 0x62 0x39 0x69
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 4 bytes discarded
[Error   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got corrupt data.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT true
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Re-sending package. 29982ms left before timeout.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(491)
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(1): 0x06
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] StartOfPacket or ContinuationFrame not found, discarding data received on UART. 0 bytes discarded, retaining 1 byte
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Got uart flags: DATA true, CORRUPT false
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(7): 0x09 0x41 0x42 0x55 0x44 0x41 0x41
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Waiting with timeout 2000ms
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART RX(58): 0x41 0x4e 0x41 0x45 0x46 0x63 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x41 0x59 0x32 0x39 0x6d 0x5a 0x68 0x6c 0x59 0x4d 0x50 0x39 0x39 0x51 0x67 0x3d 0x3d 0x0a 0x06 0x09 0x41 0x41 0x34 0x44 0x41 0x41 0x41 0x47 0x41 0x45 0x46 0x63 0x41 0x62 0x39 0x69 0x63 0x6d 0x4d 0x47 0x2f 0x78 0x43 0x66 0x0a
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Frame type after decode: START
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Start of frame found before previous frame was decoded. Clearing 1 frames from the frame buffer.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Attempting to decode frames vector with 1 frames
[Error   ] [ModemUARTDFU-Probe-/dev/ttyACM0] CBOR response contains non-zero return code, 6
{
    "duration": 5698,
    "error_code": "BadState",
    "message": "Image upload failed. Bad response from device",
    "operation": "upload_image",
    "outcome": "fail",
    "progress_percentage": 100
}
[Error   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Error during image file upload. Upload returned an error.
[Error   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Failed programming file /tmp/fileXNB59Inrfjprog/firmware.update.image.segments.1.hex.
[Error   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Failed while programming files to target.
[Error   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Failed to program DFU package
[Error   ] [HighLevel ] Failed programming the device.
[Debug   ] [HighLevel ] probe_reset
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] get_errors
[Debug   ] [HighLevel ] probe_reset
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] get_errors
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] clear_errors
b'An error was reported by NRFJPROG DLL: -2 INVALID_OPERATION. \n[Error   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Failed to program DFU package'
[Debug   ] [HighLevel ] is_dll_open
[Debug   ] [HighLevel ] probe_uninit
[Info    ] [HighLevel ] Deleting probe at location 0x1cc9530
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] readDeviceInfo
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Uninitializing ModemUARTDFU probe at serial port /dev/ttyACM0.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] uninitialize
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Sending device reset request
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Sending reset request to device.
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] UART TX(23)
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] Closing connection to mcuboot device
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] serial port read on port /dev/ttyACM0 aborted
[Debug   ] [ModemUARTDFU-Probe-/dev/ttyACM0] serial io_context executed 347 handlers.
[Info    ] [ModemUARTDFU-Probe-/dev/ttyACM0] serial port /dev/ttyACM0 closed.
{
    "duration": 141,
    "error_code": "Ok",
    "operation": "close_uart",
    "outcome": "success",
    "progress_percentage": 100
}
[Info    ] [HighLevel ] Done.
[Debug   ] [HighLevel ] dll_close
[Info    ] [HighLevel ] closing and freeing sub dlls.
Traceback (most recent call last):
  File "./update_modem.py", line 44, in <module>
    run(args.uart, args.firmware, args.baudrate)
  File "./update_modem.py", line 27, in run
    modem_dfu_probe.program(modem_firmware_zip)
  File "/home/jerwood/projects/nrf9160_modem_update/ncs/nrf/samples/nrf9160/fmfu_smp_svr/pynrfjprog_10_13_0_preview_2sec_timeout/pynrfjprog/HighLevel.py", line 398, in program
    raise APIError(result, error_data=self.get_errors(), log=self._logger.error)
pynrfjprog_10_13_0_preview_2sec_timeout.pynrfjprog.APIError.APIError: An error was reported by NRFJPROG DLL: -2 INVALID_OPERATION.
[Error   ] [ModemUARTDFU-Probe-/dev/ttyACM0] Failed to program DFU package
