2021-06-08T06:31:23.847Z INFO Application data folder: C:\Users\oysa\AppData\Roaming\nrfconnect\pc-nrfconnect-programmer
2021-06-08T06:31:23.916Z DEBUG App pc-nrfconnect-programmer v1.4.10 official
2021-06-08T06:31:23.916Z DEBUG App path: C:\Users\oysa\.nrfconnect-apps\node_modules\pc-nrfconnect-programmer
2021-06-08T06:31:23.916Z DEBUG nRFConnect 3.6.1 is supported by the app (^3.6.0)
2021-06-08T06:31:23.916Z DEBUG nRFConnect path: C:\Users\oysa\AppData\Local\Programs\nrfconnect\resources\app.asar
2021-06-08T06:31:23.916Z DEBUG HomeDir: C:\Users\oysa
2021-06-08T06:31:23.916Z DEBUG TmpDir: C:\Users\oysa\AppData\Local\Temp
2021-06-08T06:31:23.927Z INFO Using nrfjprog library 10.12.1, pc-nrfjprog-js 1.7.6
2021-06-08T06:31:24.856Z VERBOSE Could not fetch serial number for serial port at COM1
2021-06-08T06:31:24.856Z VERBOSE Could not fetch serial number for serial port at COM3
2021-06-08T06:31:27.138Z INFO Using nrfjprog to communicate with target
2021-06-08T06:31:27.777Z INFO Using J-Link Software version 6.88
2021-06-08T06:31:28.256Z INFO Segger serial:  960075900
2021-06-08T06:31:28.256Z INFO Segger speed:  2000  kHz
2021-06-08T06:31:28.256Z INFO Segger version:  J-Link OB-K22-NordicSemi compiled Jan 21 2020 17:33:01
2021-06-08T06:31:28.256Z INFO Core probed: 960075900
2021-06-08T06:31:28.256Z INFO Core RAM: 256KiB
2021-06-08T06:31:28.256Z INFO Core ROM: 1024KiB in pages of 4KiB
2021-06-08T06:31:28.568Z INFO Model: NRF9160_xxAA_REV1.
2021-06-08T06:31:29.236Z INFO Core0: Reading device non-volatile memory. This may take a few seconds.
2021-06-08T06:31:38.826Z INFO Core0: Non-volatile memory has been read. 5 non-empty memory blocks identified 
2021-06-08T06:31:49.094Z INFO Parsing HEX file:  C:\Temp\Support\271203\2843.nrf9160dk_asset_tracker_nbiot_2021-03-01_8e8c6089.hex
2021-06-08T06:31:49.118Z INFO File was last modified at  6/8/2021, 8:29:49 AM
2021-06-08T06:33:00.857Z INFO Writing image to disable app readback protection
2021-06-08T06:33:00.865Z ERROR Second argument must be a string
2021-06-08T06:33:00.865Z INFO Recovery procedure finished
2021-06-08T06:33:00.873Z INFO Using nrfjprog to communicate with target
2021-06-08T06:33:01.375Z INFO Using J-Link Software version 6.88
2021-06-08T06:33:01.856Z INFO Segger serial:  960075900
2021-06-08T06:33:01.856Z INFO Segger speed:  2000  kHz
2021-06-08T06:33:01.856Z INFO Segger version:  J-Link OB-K22-NordicSemi compiled Jan 21 2020 17:33:01
2021-06-08T06:33:01.856Z INFO Core probed: 960075900
2021-06-08T06:33:01.856Z INFO Core RAM: 256KiB
2021-06-08T06:33:01.856Z INFO Core ROM: 1024KiB in pages of 4KiB
2021-06-08T06:33:02.163Z INFO Model: NRF9160_xxAA_REV1.
2021-06-08T06:33:02.799Z INFO Core0: Reading device non-volatile memory. This may take a few seconds.
2021-06-08T06:33:03.544Z INFO Core0: UICR has been read. Click read button to read full non-volatile memory.
2021-06-08T06:33:03.804Z INFO Writing procedure starts for core0
2021-06-08T06:33:24.199Z INFO Write procedure finished
2021-06-08T06:33:24.201Z INFO Using nrfjprog to communicate with target
2021-06-08T06:33:24.821Z INFO Using J-Link Software version 6.88
2021-06-08T06:33:25.395Z INFO Segger serial:  960075900
2021-06-08T06:33:25.395Z INFO Segger speed:  2000  kHz
2021-06-08T06:33:25.395Z INFO Segger version:  J-Link OB-K22-NordicSemi compiled Jan 21 2020 17:33:01
2021-06-08T06:33:25.395Z INFO Core probed: 960075900
2021-06-08T06:33:25.395Z INFO Core RAM: 256KiB
2021-06-08T06:33:25.395Z INFO Core ROM: 1024KiB in pages of 4KiB
2021-06-08T06:33:25.692Z INFO Model: NRF9160_xxAA_REV1.
2021-06-08T06:33:26.304Z INFO Core0: Reading device non-volatile memory. This may take a few seconds.
2021-06-08T06:33:35.861Z INFO Core0: Non-volatile memory has been read. 6 non-empty memory blocks identified 
