[m

[1;32muart:~$ [mE: wifi_nrf_hal_fw_chk_boot: Boot_sig check failed for RPU(0), Expected: 0x5A5A5A5A, Actual: 0x17

E: wifi_nrf_fmac_fw_load: LMAC ROM boot check failed

E: wifi_nrf_fmac_dev_add_zep: wifi_nrf_fmac_fw_load failed

E: wifi_nrf_drv_main_zep: wifi_nrf_fmac_dev_add_zep failed

E: wifi_nrf_if_init: vif_ctx_zep is NULL

ASSERTION FAIL [net_if_get_link_addr(iface)->addr != ((void *)0)] @ WEST_TOPDIR/zephyr/subsys/net/ip/net_if.c:4185
	
E: r0/a1:  0x00000004  r1/a2:  0x00001059  r2/a3:  0x20008878
E: r3/a4:  0x2000e398 r12/ip:  0x00000000 r14/lr:  0x0002de6b
E:  xpsr:  0x69100000
E: s[ 0]:  0x00000000  s[ 1]:  0x00000000  s[ 2]:  0x00000000  s[ 3]:  0x00000000
E: s[ 4]:  0x00000000  s[ 5]:  0x00000000  s[ 6]:  0x00000000  s[ 7]:  0x00000000
E: s[ 8]:  0x00000000  s[ 9]:  0x00000000  s[10]:  0x00000000  s[11]:  0x00000000
E: s[12]:  0x00000000  s[13]:  0x00000000  s[14]:  0x00000000  s[15]:  0x00000000
E: fpscr:  0x00000000
E: Faulting instruction address (r15/pc): 0x0008e2f6
E: >>> ZEPHYR FATAL ERROR 4: Kernel panic on CPU 0
E: Current thread: 0x20008878 (main)
E: Halting system
