 *  Executing task: nRF Connect: Build [pristine]: NRF_BLETransparentModule_V2/build 

Building NRF_BLETransparentModule_V2
west build --build-dir /Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/build /Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2 --pristine --board ble_trans_board_nrf52810/nrf52810 --sysbuild -- -DNCS_TOOLCHAIN_VERSION=NONE -DCONF_FILE=prj_minimal.conf -DDTC_OVERLAY_FILE=ble_trans_board_nrf52810_nrf52810.overlay -DBOARD_ROOT=/Users/chinmaydixit/Projects/NRF

-- west build: generating a build system
Loading Zephyr module(s) (Zephyr base): sysbuild_default
-- Found Python3: /opt/nordic/ncs/toolchains/b8efef2ad5/opt/python@3.12/bin/python3.12 (found suitable version "3.12.4", minimum required is "3.8") found components: Interpreter 
-- Cache files will be written to: /Users/chinmaydixit/Library/Caches/zephyr
-- Found west (found suitable version "1.2.0", minimum required is "0.14.0")
-- Board: ble_trans_board_nrf52810, qualifiers: nrf52810
Parsing /Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/Kconfig.sysbuild
Loaded configuration '/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/build/_sysbuild/empty.conf'
Merged configuration '/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/build/_sysbuild/empty.conf'
Configuration saved to '/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/build/zephyr/.config'
Kconfig header saved to '/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/build/_sysbuild/autoconf.h'
-- 
   *************************************************
   * Running CMake for NRF_BLETransparentModule_V2 *
   *************************************************

Loading Zephyr default modules (Zephyr base).
-- Application: /Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2
-- CMake version: 3.21.0
-- Found Python3: /opt/nordic/ncs/toolchains/b8efef2ad5/bin/python (found suitable version "3.12.4", minimum required is "3.8") found components: Interpreter 
-- Cache files will be written to: /Users/chinmaydixit/Library/Caches/zephyr
-- Zephyr version: 3.7.99 (/opt/nordic/ncs/v2.9.1/zephyr)
-- Found west (found suitable version "1.2.0", minimum required is "0.14.0")
-- Board: ble_trans_board_nrf52810, qualifiers: nrf52810
-- Found host-tools: zephyr 0.17.0 (/opt/nordic/ncs/toolchains/b8efef2ad5/opt/zephyr-sdk)
-- Found toolchain: zephyr 0.17.0 (/opt/nordic/ncs/toolchains/b8efef2ad5/opt/zephyr-sdk)
-- Found Dtc: /opt/nordic/ncs/toolchains/b8efef2ad5/bin/dtc (found suitable version "1.6.1", minimum required is "1.4.6") 
-- Found BOARD.dts: /Users/chinmaydixit/Projects/NRF/boards/CGC/ble_trans_board_nrf52810/ble_trans_board_nrf52810.dts
-- Found devicetree overlay: ble_trans_board_nrf52810_nrf52810.overlay
-- Generated zephyr.dts: /Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/build/NRF_BLETransparentModule_V2/zephyr/zephyr.dts
-- Generated devicetree_generated.h: /Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/build/NRF_BLETransparentModule_V2/zephyr/include/generated/zephyr/devicetree_generated.h
-- Including generated dts.cmake file: /Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/build/NRF_BLETransparentModule_V2/zephyr/dts.cmake

warning: HW_STACK_PROTECTION (defined at soc/nxp/s32/s32k1/Kconfig.defconfig:20, arch/Kconfig:283)
was assigned the value 'y' but got the value 'n'. Check these unsatisfied dependencies:
((SOC_SERIES_S32K1 && SOC_FAMILY_NXP_S32) || ARCH_HAS_STACK_PROTECTION) (=n). See
http://docs.zephyrproject.org/latest/kconfig.html#CONFIG_HW_STACK_PROTECTION and/or look up
HW_STACK_PROTECTION in the menuconfig/guiconfig interface. The Application Development Primer,
Setting Configuration Values, and Kconfig - Tips and Best Practices sections of the manual might be
helpful too.


warning: LOG_BUFFER_SIZE (defined at
/opt/nordic/ncs/v2.9.1/nrf/subsys/net/openthread/Kconfig.defconfig:51,
subsys/logging/Kconfig.processing:122) was assigned the value '256' but got the value ''. Check
these unsatisfied dependencies: (NET_L2_OPENTHREAD || (LOG_MODE_DEFERRED && !LOG_FRONTEND_ONLY &&
!LOG_MODE_MINIMAL && LOG)) (=n). See
http://docs.zephyrproject.org/latest/kconfig.html#CONFIG_LOG_BUFFER_SIZE and/or look up
LOG_BUFFER_SIZE in the menuconfig/guiconfig interface. The Application Development Primer, Setting
Configuration Values, and Kconfig - Tips and Best Practices sections of the manual might be helpful
too.


warning: UART_CONSOLE (defined at drivers/console/Kconfig:42) was assigned the value 'y' but got the
value 'n'. Check these unsatisfied dependencies: CONSOLE (=n). See
http://docs.zephyrproject.org/latest/kconfig.html#CONFIG_UART_CONSOLE and/or look up UART_CONSOLE in
the menuconfig/guiconfig interface. The Application Development Primer, Setting Configuration
Values, and Kconfig - Tips and Best Practices sections of the manual might be helpful too.


warning: LOG_PRINTK (defined at subsys/logging/Kconfig.processing:8) was assigned the value 'y' but
got the value 'n'. Check these unsatisfied dependencies: LOG (=n). See
http://docs.zephyrproject.org/latest/kconfig.html#CONFIG_LOG_PRINTK and/or look up LOG_PRINTK in the
menuconfig/guiconfig interface. The Application Development Primer, Setting Configuration Values,
and Kconfig - Tips and Best Practices sections of the manual might be helpful too.


warning: LOG_BACKEND_UART (defined at subsys/logging/backends/Kconfig.uart:4) was assigned the value
'y' but got the value 'n'. Check these unsatisfied dependencies: UART_CONSOLE (=n), LOG (=n). See
http://docs.zephyrproject.org/latest/kconfig.html#CONFIG_LOG_BACKEND_UART and/or look up
LOG_BACKEND_UART in the menuconfig/guiconfig interface. The Application Development Primer, Setting
Configuration Values, and Kconfig - Tips and Best Practices sections of the manual might be helpful
too.

Parsing /Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/Kconfig
Loaded configuration '/Users/chinmaydixit/Projects/NRF/boards/CGC/ble_trans_board_nrf52810/ble_trans_board_nrf52810_defconfig'
Merged configuration '/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/prj_minimal.conf'
Merged configuration '/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/build/NRF_BLETransparentModule_V2/zephyr/.config.sysbuild'
Configuration saved to '/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/build/NRF_BLETransparentModule_V2/zephyr/.config'
Kconfig header saved to '/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/build/NRF_BLETransparentModule_V2/zephyr/include/generated/zephyr/autoconf.h'
-- Found GnuLd: /opt/nordic/ncs/toolchains/b8efef2ad5/opt/zephyr-sdk/arm-zephyr-eabi/arm-zephyr-eabi/bin/ld.bfd (found version "2.38") 
-- The C compiler identification is GNU 12.2.0
-- The CXX compiler identification is GNU 12.2.0
-- The ASM compiler identification is GNU
-- Found assembler: /opt/nordic/ncs/toolchains/b8efef2ad5/opt/zephyr-sdk/arm-zephyr-eabi/bin/arm-zephyr-eabi-gcc
CMake Warning at /opt/nordic/ncs/v2.9.1/zephyr/subsys/bluetooth/host/CMakeLists.txt:91 (message):
  CONFIG_BT_FIXED_PASSKEY is enabled

    A fixed passkey is easy to deduce during the pairing procedure, do not use in
    production.


-- Setting build type to 'MinSizeRel' as none was specified.
-- Using ccache: /opt/nordic/ncs/toolchains/b8efef2ad5/bin/ccache
-- Configuring done
-- Generating done
-- Build files have been written to: /Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/build/NRF_BLETransparentModule_V2
-- Found partition manager static configuration : /Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/pm_static.yml
Partition 'nvs_storage' is not included in the dynamic resolving since it is statically defined.
Partition 'settings_storage' is not included in the dynamic resolving since it is statically defined.
-- Configuring done
-- Generating done
-- Build files have been written to: /Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/build
-- west build: building application
[1/216] Preparing syscall dependency handling

[8/216] Generating include/generated/zephyr/version.h
-- Zephyr version: 3.7.99 (/opt/nordic/ncs/v2.9.1/zephyr), build: v3.7.99-ncs2-1
[39/216] Building C object CMakeFiles/app.dir/src/GPIO_handle/GPIO_handle.c.obj
/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/src/GPIO_handle/GPIO_handle.c: In function 'configure_gpio':
/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/src/GPIO_handle/GPIO_handle.c:131:1: warning: control reaches end of non-void function [-Wreturn-type]
  131 | }
      | ^
[49/216] Building C object CMakeFiles/app.dir/src/ble_handle/ble_handle.c.obj
/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/src/ble_handle/ble_handle.c: In function 'bt_receive_cb':
/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/src/ble_handle/ble_handle.c:81:13: warning: unused variable 'err' [-Wunused-variable]
   81 |         int err;
      |             ^~~
/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/src/ble_handle/ble_handle.c: In function 'auth_passkey_entry':
/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/src/ble_handle/ble_handle.c:204:65: warning: implicit declaration of function 'bt_addr_str'; did you mean 'bt_addr_to_str'? [-Wimplicit-function-declaration]
  204 |                 uart_printk("Failed to enter passkey for %s\n", bt_addr_str(bt_conn_get_dst(conn)));
      |                                                                 ^~~~~~~~~~~
      |                                                                 bt_addr_to_str
/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/src/ble_handle/ble_handle.c: In function 'ble_init':
/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/src/ble_handle/ble_handle.c:466:17: warning: implicit declaration of function 'settings_load' [-Wimplicit-function-declaration]
  466 |                 settings_load();
      |                 ^~~~~~~~~~~~~
/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/src/ble_handle/ble_handle.c: At top level:
/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/src/ble_handle/ble_handle.c:199:13: warning: 'auth_passkey_entry' defined but not used [-Wunused-function]
  199 | static void auth_passkey_entry(struct bt_conn *conn)
      |             ^~~~~~~~~~~~~~~~~~
/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/src/ble_handle/ble_handle.c:145:13: warning: 'auth_passkey_confirm' defined but not used [-Wunused-function]
  145 | static void auth_passkey_confirm(struct bt_conn *conn, unsigned int passkey)
      |             ^~~~~~~~~~~~~~~~~~~~
/Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/src/ble_handle/ble_handle.c:40:13: warning: 'num_comp_reply' defined but not used [-Wunused-function]
   40 | static void num_comp_reply(bool accept)
      |             ^~~~~~~~~~~~~~
[216/216] Linking C executable zephyr/zephyr.elf
Memory region         Used Size  Region Size  %age Used
           FLASH:      151060 B       176 KB     83.82%
             RAM:       23064 B        24 KB     93.85%
        IDT_LIST:          0 GB        32 KB      0.00%
Generating files from /Users/chinmaydixit/Projects/NRF/Projects/NRF_BLETransparentModule_V2/build/NRF_BLETransparentModule_V2/zephyr/zephyr.elf for board: ble_trans_board_nrf52810
[10/10] Generating ../merged.hex
 *  Terminal will be reused by tasks, press any key to close it. 
