00> 
00> 
00> mosh:~$ *** Booting nRF Connect SDK v2.7.0-5cb85570ca43 ***
00> *** Using Zephyr OS v3.6.99-100befc70c74 ***
00> 
00> Reset reason: power-on reset
00> 
00> MOSH version:       v2.7.0
00> MOSH build id:      custom
00> MOSH build variant: dev
00> 
00> Network registration status: searching
00> Currently active system mode: LTE-M
00> LTE cell changed: ID: 77332752, Tracking area: 17169
00> RRC mode: Connected
00> PDN event: PDP context 0 activated
00> PDN event: PDP context 0, PDN type IPv4 only allowed
00> Modem domain event: Search done
00> Network registration status: Connected - roaming
00> PSM parameter update: TAU: 3240, Active time: -1 seconds
00> Modem config for system mode: LTE-M - NB-IoT
00> Modem config for LTE preference: No preference, automatically selected by the modem
00> Currently active system mode: LTE-M
00> Modem FW version:      mfw_nrf9160_1.3.6
00> Device ID:             nrf-351901930730670
00> Operator full name:   "AT&T"
00> Operator short name:  "AT&T"
00> Operator PLMN:        "310410"
00> Current cell id:       77332752 (0x049C0110)
00> Current phy cell id:   476
00> Current band:          12
00> Current TAC:           17169 (0x4311)
00> Current rsrp:          39: -101dBm
00> Current snr:           37: 13dB
00> Mobile network time and date: 25/09/12,14:36:48-20
00> PDP context info 1:
00>   CID:                0
00>   PDN ID:             0
00>   PDP context active: yes
00>   PDP type:           IP
00>   APN:                iot.1nce.net
00>   IPv4 address:       10.200.131.159
00>   IPv6 address:       ::
00>   IPv4 DNS address:   8.8.8.8, 8.8.4.4
00>   IPv6 DNS address:   ::, ::
00> RRC mode: Idle
00> Button 1 pressed - raising a kill signal
00> Button 1 released - resetting a kill signal