ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x1006669
  Start of program headers:          52 (bytes into file)
  Start of section headers:          1664896 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         5
  Size of section headers:           40 (bytes)
  Number of section headers:         35
  Section header string table index: 34

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        01000000 0000e0 0000b8 00 WAX  0   0  4
  [ 2] text              PROGBITS        010000b8 000198 0105d0 00  AX  0   0  4
  [ 3] .ARM.exidx        ARM_EXIDX       01010688 010768 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        01010690 010770 000068 00   A  0   0  4
  [ 5] devices           PROGBITS        010106f8 0107d8 000090 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        01010788 010868 0000f0 00  WA  0   0  4
  [ 7] device_handles    PROGBITS        01010878 010958 00002c 00   A  0   0  2
  [ 8] log_const_se[...] PROGBITS        010108a4 010984 000088 00   A  0   0  4
  [ 9] log_backend_area  PROGBITS        0101092c 010a0c 000010 00   A  0   0  4
  [10] zephyr_dbg_info   PROGBITS        0101093c 010a1c 000040 00  WA  0   0  4
  [11] rodata            PROGBITS        01010980 010a60 001ad4 00   A  0   0 16
  [12] .ramfunc          PROGBITS        21000000 012bb4 000000 00   W  0   0  1
  [13] datas             PROGBITS        21000000 012538 000604 00  WA  0   0  8
  [14] device_states     PROGBITS        21000604 012b3c 00000c 00  WA  0   0  1
  [15] log_mpsc_pbu[...] PROGBITS        21000610 012b48 00003c 00  WA  0   0  4
  [16] log_msg_ptr_area  PROGBITS        2100064c 012b84 000004 00  WA  0   0  4
  [17] k_heap_area       PROGBITS        21000650 012b88 000018 00  WA  0   0  4
  [18] k_sem_area        PROGBITS        21000668 012ba0 000010 00  WA  0   0  4
  [19] bss               NOBITS          21000678 012bb8 000d89 00  WA  0   0  8
  [20] noinit            NOBITS          21001408 012bb8 002d80 00  WA  0   0  8
  [21] .comment          PROGBITS        00000000 012bb4 000020 01  MS  0   0  1
  [22] .debug_aranges    PROGBITS        00000000 012bd8 002988 00      0   0  8
  [23] .debug_info       PROGBITS        00000000 015560 0b0dc0 00      0   0  1
  [24] .debug_abbrev     PROGBITS        00000000 0c6320 01228a 00      0   0  1
  [25] .debug_line       PROGBITS        00000000 0d85aa 038efc 00      0   0  1
  [26] .debug_frame      PROGBITS        00000000 1114a8 006f94 00      0   0  4
  [27] .debug_str        PROGBITS        00000000 11843c 0116db 01  MS  0   0  1
  [28] .debug_loc        PROGBITS        00000000 129b17 04ed7b 00      0   0  1
  [29] .debug_ranges     PROGBITS        00000000 178898 007e80 00      0   0  8
  [30] .ARM.attributes   ARM_ATTRIBUTES  00000000 180718 000032 00      0   0  1
  [31] .last_section     PROGBITS        01012acc 012bb0 000004 00   A  0   0  1
  [32] .symtab           SYMTAB          00000000 18074c 00d3f0 10     33 2309  4
  [33] .strtab           STRTAB          00000000 18db3c 008ab3 00      0   0  1
  [34] .shstrtab         STRTAB          00000000 1965ef 00018e 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  D (mbind), y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x010768 0x01010688 0x01010688 0x00008 0x00008 R   0x4
  LOAD           0x0000e0 0x01000000 0x01000000 0x12454 0x12454 RWE 0x10
  LOAD           0x012538 0x21000000 0x01012454 0x00678 0x00678 RW  0x8
  LOAD           0x012bb0 0x01012acc 0x01012acc 0x00004 0x00004 R   0x1
  LOAD           0x000000 0x21000678 0x21000678 0x00000 0x03b10 RW  0x8

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel devices sw_isr_table device_handles log_const_sections log_backend_area zephyr_dbg_info rodata 
   02     datas device_states log_mpsc_pbuf_area log_msg_ptr_area k_heap_area k_sem_area 
   03     .last_section 
   04     bss noinit 
