ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0xd29d
  Start of program headers:          52 (bytes into file)
  Start of section headers:          614588 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         4
  Size of section headers:           40 (bytes)
  Number of section headers:         25
  Section header string table index: 24

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        0000c000 0000c0 00023c 00 WAX  0   0  4
  [ 2] text              PROGBITS        0000c23c 0002fc 003c18 00  AX  0   0  4
  [ 3] .ARM.exidx        ARM_EXIDX       0000fe54 003f14 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        0000fe5c 003f1c 000058 00   A  0   0  4
  [ 5] sw_isr_table      PROGBITS        0000feb4 003f74 000208 00  WA  0   0  4
  [ 6] rodata            PROGBITS        000100c0 004180 000290 00   A  0   0 16
  [ 7] .ramfunc          PROGBITS        20010000 00450c 000000 00   W  0   0  1
  [ 8] datas             PROGBITS        20010000 004410 000098 00  WA  0   0  4
  [ 9] devices           PROGBITS        20010098 0044a8 000064 00   A  0   0  4
  [10] bss               NOBITS          20010100 004510 000221 00  WA  0   0  8
  [11] noinit            NOBITS          20010328 004510 001940 00  WA  0   0  8
  [12] .comment          PROGBITS        00000000 00450c 000079 01  MS  0   0  1
  [13] .debug_aranges    PROGBITS        00000000 004588 000f80 00      0   0  8
  [14] .debug_info       PROGBITS        00000000 005508 03e74c 00      0   0  1
  [15] .debug_abbrev     PROGBITS        00000000 043c54 00add8 00      0   0  1
  [16] .debug_line       PROGBITS        00000000 04ea2c 0188a4 00      0   0  1
  [17] .debug_frame      PROGBITS        00000000 0672d0 002274 00      0   0  4
  [18] .debug_str        PROGBITS        00000000 069544 008bba 01  MS  0   0  1
  [19] .debug_loc        PROGBITS        00000000 0720fe 015ade 00      0   0  1
  [20] .debug_ranges     PROGBITS        00000000 087be0 005690 00      0   0  8
  [21] .ARM.attributes   ARM_ATTRIBUTES  00000000 08d270 000034 00      0   0  1
  [22] .symtab           SYMTAB          00000000 08d2a4 004d20 10     23 645  4
  [23] .strtab           STRTAB          00000000 091fc4 004004 00      0   0  1
  [24] .shstrtab         STRTAB          00000000 095fc8 0000f4 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x003f14 0x0000fe54 0x0000fe54 0x00008 0x00008 R   0x4
  LOAD           0x0000c0 0x0000c000 0x0000c000 0x04350 0x04350 RWE 0x10
  LOAD           0x004410 0x20010000 0x00010350 0x000fc 0x000fc RW  0x4
  LOAD           0x004510 0x20010100 0x20010100 0x00000 0x01b68 RW  0x8

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel sw_isr_table rodata 
   02     datas devices 
   03     bss noinit 
