// To get started, press Ctrl+Space to bring up the completion menu and view the available nodes.
// For more help, browse the DeviceTree documentation at https://docs.zephyrproject.org/latest/guides/dts/index.html
/{

    leds {
            compatible = "gpio-leds";
            led0: led_0 {
                gpios = <&gpio0 6 GPIO_ACTIVE_LOW>;
                label = "Green LED 0";
            };
    };
        
    alias {
            led0 = &led0;
        
    };
};
    &uart0 {
    
        status = "disabled";
        
    };
    
