// To get started, press Ctrl+Space to bring up the completion menu and view the available nodes.

// You can also use the buttons in the sidebar to perform actions on nodes.
// Actions currently available include:

// * Enabling / disabling the node
// * Adding the bus to a bus
// * Removing the node
// * Connecting ADC channels

// For more help, browse the DeviceTree documentation at https://docs.zephyrproject.org/latest/guides/dts/index.html
// You can also visit the nRF DeviceTree extension documentation at https://nrfconnect.github.io/vscode-nrf-connect/devicetree/nrfdevicetree.html
/delete-node/ &storage_partition;

&mx25r64 {
	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		storage_partition: partition@0 {
			label = "storage";
			reg = <0x00000000 DT_SIZE_K(8000)>;
		};
	};
};

/ {
	msc_disk0 {
		compatible = "zephyr,flash-disk";
		partition = <&storage_partition>;
		disk-name = "NAND";
		cache-size = <4096>;
	};

	
};