ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x252b1
  Start of program headers:          52 (bytes into file)
  Start of section headers:          9236912 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         5
  Size of section headers:           40 (bytes)
  Number of section headers:         51
  Section header string table index: 50

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        00000000 0000e0 000100 00 WAX  0   0  4
  [ 2] text              PROGBITS        00000100 0001e0 055b94 00  AX  0   0  4
  [ 3] .ARM.exidx        ARM_EXIDX       00055c94 055d74 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        00055c9c 055d7c 000110 00   A  0   0  4
  [ 5] devices           PROGBITS        00055dac 055e8c 0000f0 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        00055e9c 055f7c 000180 00  WA  0   0  4
  [ 7] device_handles    PROGBITS        0005601c 0560fc 00003c 00   A  0   0  2
  [ 8] bt_l2cap_fix[...] PROGBITS        00056058 056138 000024 00   A  0   0  4
  [ 9] bt_conn_cb_area   PROGBITS        0005607c 05615c 000028 00   A  0   0  4
  [10] bt_gatt_serv[...] PROGBITS        000560a4 056184 000010 00   A  0   0  4
  [11] bt_mesh_subn[...] PROGBITS        000560b4 056194 000010 00   A  0   0  4
  [12] bt_mesh_app_[...] PROGBITS        000560c4 0561a4 000004 00   A  0   0  4
  [13] log_const_se[...] PROGBITS        000560c8 0561a8 000260 00   A  0   0  4
  [14] log_backend_area  PROGBITS        00056328 056408 000020 00   A  0   0  4
  [15] settings_han[...] PROGBITS        00056348 056428 000154 00   A  0   0  4
  [16] shell_area        PROGBITS        0005649c 05657c 000030 00   A  0   0  4
  [17] shell_root_c[...] PROGBITS        000564cc 0565ac 000034 00   A  0   0  4
  [18] shell_subcmd[...] PROGBITS        00056500 0565e0 000014 00   A  0   0  4
  [19] shell_dynami[...] PROGBITS        00056514 0565f4 000010 00   A  0   0  4
  [20] rodata            PROGBITS        00056530 056610 00c5ac 00   A  0   0 16
  [21] .ramfunc          PROGBITS        20000000 0641b4 000000 00   W  0   0  1
  [22] datas             PROGBITS        20000000 062bc0 000f53 00  WA  0   0  8
  [23] bt_mesh_ext_[...] PROGBITS        20000f58 063b18 000060 00  WA  0   0  8
  [24] device_states     PROGBITS        20000fb8 063b78 000014 00  WA  0   0  1
  [25] log_mpsc_pbu[...] PROGBITS        20000fcc 063b8c 000044 00  WA  0   0  4
  [26] log_msg_ptr_area  PROGBITS        20001010 063bd0 000004 00  WA  0   0  4
  [27] log_dynamic_[...] PROGBITS        20001014 063bd4 000130 00  WA  0   0  4
  [28] k_mem_slab_area   PROGBITS        20001144 063d04 000100 00  WA  0   0  4
  [29] k_mutex_area      PROGBITS        20001244 063e04 0000a0 00  WA  0   0  4
  [30] k_sem_area        PROGBITS        200012e4 063ea4 000018 00  WA  0   0  4
  [31] k_queue_area      PROGBITS        200012fc 063ebc 000070 00  WA  0   0  4
  [32] _net_buf_poo[...] PROGBITS        2000136c 063f2c 0001d4 00  WA  0   0  4
  [33] usb_descriptor    PROGBITS        20001540 064100 00008c 00  WA  0   0  1
  [34] usb_cfg_data_area PROGBITS        200015cc 06418c 000024 00  WA  0   0  4
  [35] bss               NOBITS          200015f0 0641f0 01fe5e 00  WA  0   0  8
  [36] noinit            NOBITS          20021480 0641f0 008202 00  WA  0   0 64
  [37] .comment          PROGBITS        00000000 0641b4 000040 01  MS  0   0  1
  [38] .debug_aranges    PROGBITS        00000000 0641f8 006548 00      0   0  8
  [39] .debug_info       PROGBITS        00000000 06a740 505d35 00      0   0  1
  [40] .debug_abbrev     PROGBITS        00000000 570475 037516 00      0   0  1
  [41] .debug_line       PROGBITS        00000000 5a798b 121ac4 00      0   0  1
  [42] .debug_frame      PROGBITS        00000000 6c9450 0138cc 00      0   0  4
  [43] .debug_str        PROGBITS        00000000 6dcd1c 02e2b9 01  MS  0   0  1
  [44] .debug_loc        PROGBITS        00000000 70afd5 13be8c 00      0   0  1
  [45] .debug_ranges     PROGBITS        00000000 846e68 033258 00      0   0  8
  [46] .ARM.attributes   ARM_ATTRIBUTES  00000000 87a0c0 000030 00      0   0  1
  [47] .last_section     PROGBITS        000640cc 0641b0 000004 00   A  0   0  1
  [48] .symtab           SYMTAB          00000000 87a0f0 036580 10     49 10531  4
  [49] .strtab           STRTAB          00000000 8b0670 01e85a 00      0   0  1
  [50] .shstrtab         STRTAB          00000000 8ceeca 0002e5 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  D (mbind), y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x055d74 0x00055c94 0x00055c94 0x00008 0x00008 R   0x4
  LOAD           0x0000e0 0x00000000 0x00000000 0x62adc 0x62adc RWE 0x10
  LOAD           0x062bc0 0x20000000 0x00062adc 0x015f0 0x015f0 RW  0x8
  LOAD           0x0641b0 0x000640cc 0x000640cc 0x00004 0x00004 R   0x1
  LOAD           0x000000 0x200015f0 0x200015f0 0x00000 0x28092 RW  0x40

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel devices sw_isr_table device_handles bt_l2cap_fixed_chan_area bt_conn_cb_area bt_gatt_service_static_area bt_mesh_subnet_cb_area bt_mesh_app_key_cb_area log_const_sections log_backend_area settings_handler_static_area shell_area shell_root_cmds_sections shell_subcmds_sections shell_dynamic_subcmds_sections rodata 
   02     datas bt_mesh_ext_adv_area device_states log_mpsc_pbuf_area log_msg_ptr_area log_dynamic_sections k_mem_slab_area k_mutex_area k_sem_area k_queue_area _net_buf_pool_area usb_descriptor usb_cfg_data_area 
   03     .last_section 
   04     bss noinit 
