//Invoke script with "$jlink -Commandfile execute_from_ram.jlink -autoconnect 1". Select generic m33 when prompted to select a device 
if SWD
speed 4000
r
h
loadfile build\zephyr\zephyr.hex
w4 0xe000ed08 0x20000000
mem32 0x20000000 2 // Reads MSP and Reset vector from vector table. Check if they match with the addresses set below
wreg MSP, 0x20020CD0 
setPC 0x20001319
regs
g